| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
USCI_UART Exported Constants
Standard Driver » USCI_UART Driver

## Macros
#define | UUART_WORD_LEN_6
#define | UUART_WORD_LEN_7
#define | UUART_WORD_LEN_8
#define | UUART_WORD_LEN_9
#define | UUART_PARITY_NONE
#define | UUART_PARITY_ODD
#define | UUART_PARITY_EVEN
#define | UUART_STOP_BIT_1
#define | UUART_STOP_BIT_2
#define | UUART_ABR_INT_MASK
#define | UUART_RLS_INT_MASK
#define | UUART_BUF_RXOV_INT_MASK
#define | UUART_TXST_INT_MASK
#define | UUART_TXEND_INT_MASK
#define | UUART_RXST_INT_MASK
#define | UUART_RXEND_INT_MASK

## Detailed Description

## Macro Definition Documentation

## ◆ UUART_ABR_INT_MASK

#define UUART_ABR_INT_MASK

Auto-baud rate interrupt mask

Definition at line 52 of file usci_uart.h.

## ◆ UUART_BUF_RXOV_INT_MASK

#define UUART_BUF_RXOV_INT_MASK

Buffer RX overrun interrupt mask

Definition at line 54 of file usci_uart.h.

## ◆ UUART_PARITY_EVEN

#define UUART_PARITY_EVEN

UUART_PROTCTL setting to set UART as even parity

Definition at line 44 of file usci_uart.h.

## ◆ UUART_PARITY_NONE

#define UUART_PARITY_NONE

UUART_PROTCTL setting to set UART as no parity

Definition at line 42 of file usci_uart.h.

## ◆ UUART_PARITY_ODD

#define UUART_PARITY_ODD

UUART_PROTCTL setting to set UART as odd parity

Definition at line 43 of file usci_uart.h.

## ◆ UUART_RLS_INT_MASK

#define UUART_RLS_INT_MASK

Receive line status interrupt mask

Definition at line 53 of file usci_uart.h.

## ◆ UUART_RXEND_INT_MASK

#define UUART_RXEND_INT_MASK

RX end interrupt mask

Definition at line 58 of file usci_uart.h.

## ◆ UUART_RXST_INT_MASK

#define UUART_RXST_INT_MASK

RX start interrupt mask

Definition at line 57 of file usci_uart.h.

## ◆ UUART_STOP_BIT_1

#define UUART_STOP_BIT_1

UUART_PROTCTL setting for one stop bit

Definition at line 46 of file usci_uart.h.

## ◆ UUART_STOP_BIT_2

#define UUART_STOP_BIT_2

UUART_PROTCTL setting for two stop bit

Definition at line 47 of file usci_uart.h.

## ◆ UUART_TXEND_INT_MASK

#define UUART_TXEND_INT_MASK

Tx end interrupt mask

Definition at line 56 of file usci_uart.h.

## ◆ UUART_TXST_INT_MASK

#define UUART_TXST_INT_MASK

TX start interrupt mask

Definition at line 55 of file usci_uart.h.

## ◆ UUART_WORD_LEN_6

#define UUART_WORD_LEN_6

UUART_LINECTL setting to set UART word length to 6 bits

Definition at line 34 of file usci_uart.h.

## ◆ UUART_WORD_LEN_7

#define UUART_WORD_LEN_7

UUART_LINECTL setting to set UART word length to 7 bits

Definition at line 35 of file usci_uart.h.

## ◆ UUART_WORD_LEN_8

#define UUART_WORD_LEN_8

UUART_LINECTL setting to set UART word length to 8 bits

Definition at line 36 of file usci_uart.h.

## ◆ UUART_WORD_LEN_9

#define UUART_WORD_LEN_9

UUART_LINECTL setting to set UART word length to 9 bits

Definition at line 37 of file usci_uart.h.