| M480 BSP V3.05.001 The Board Support Package for M480 Series

Data Structures | Macros | Functions
sclib.h File Reference

Smartcard library header file. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Data Structures
struct | SCLIB_CARD_INFO_T
| A structure holds smartcard information. More...

## Macros
#define | SCLIB_MAX_ATR_LEN
#define | SCLIB_MIN_ATR_LEN
#define | SCLIB_PROTOCOL_UNDEFINED
#define | SCLIB_PROTOCOL_T0
#define | SCLIB_PROTOCOL_T1
#define | SCLIB_SUCCESS
#define | SCLIB_ERR_CARD_REMOVED
#define | SCLIB_ERR_OVER_RUN
#define | SCLIB_ERR_PARITY_ERROR
#define | SCLIB_ERR_NO_STOP
#define | SCLIB_ERR_SILENT_BYTE
#define | SCLIB_ERR_READ
#define | SCLIB_ERR_WRITE
#define | SCLIB_ERR_TIME0OUT
#define | SCLIB_ERR_TIME1OUT
#define | SCLIB_ERR_TIME2OUT
#define | SCLIB_ERR_AUTOCONVENTION
#define | SCLIB_ERR_CLOCK
#define | SCLIB_ERR_ATR_UNRECOGNIZED
#define | SCLIB_ERR_ATR_INVALID_PARAM
#define | SCLIB_ERR_ATR_INVALID_TCK
#define | SCLIB_ERR_PPS
#define | SCLIB_ERR_T1_PROTOCOL
#define | SCLIB_ERR_T1_ABORT_RECEIVED
#define | SCLIB_ERR_T1_RESYNCH_RECEIVED
#define | SCLIB_ERR_T1_VPP_ERROR_RECEIVED
#define | SCLIB_ERR_T1_WTXRES_RECEIVED
#define | SCLIB_ERR_T1_IFSRES_RECEIVED
#define | SCLIB_ERR_T1_ABORTRES_RECEIVED
#define | SCLIB_ERR_T1_CHECKSUM
#define | SCLIB_ERR_T0_PROTOCOL
#define | SCLIB_ERR_DEACTIVE
#define | SCLIB_ERR_CARDBUSY

## Functions
int32_t | SCLIB_Activate (uint32_t num, uint32_t u32EMVCheck)
| Activate a smartcard. More...
int32_t | SCLIB_ActivateDelay (uint32_t num, uint32_t u32EMVCheck, uint32_t u32Delay)
| Activate a smartcard with large delay between set VCC high and start CLK output. More...
int32_t | SCLIB_ColdReset (uint32_t num)
| Cold reset a smartcard. More...
int32_t | SCLIB_WarmReset (uint32_t num)
| Warm reset a smartcard. More...
void | SCLIB_Deactivate (uint32_t num)
| Deactivate a smartcard. More...
int32_t | SCLIB_GetCardInfo (uint32_t num, SCLIB_CARD_INFO_T *s_info)
| Get the card information (e.g., protocol selected, ATR...) after activation success. More...
int32_t | SCLIB_StartTransmission (uint32_t num, uint8_t *cmdBuf, uint32_t cmdLen, uint8_t *rspBuf, uint32_t *rspLen)
| Start a smartcard transmission. More...
int32_t | SCLIB_SetIFSD (uint32_t num, uint8_t size)
| Set interface device max information field size (IFSD) More...
__weak void | SCLIB_RequestTimeExtension (uint32_t u32Protocol)
| A callback called by library while smartcard request for a time extension. More...
uint32_t | SCLIB_CheckCDEvent (uint32_t num)
| Process card detect event in IRQ handler. More...
uint32_t | SCLIB_CheckTimeOutEvent (uint32_t num)
| Process time out event in IRQ handler. More...
uint32_t | SCLIB_CheckTxRxEvent (uint32_t num)
| Process card transmission event in IRQ handler. More...
uint32_t | SCLIB_CheckErrorEvent (uint32_t num)
| Process error event in IRQ handler. More...

## Detailed Description

Smartcard library header file.

Version
  V1.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2017-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file sclib.h.