| M480 BSP V3.05.001 The Board Support Package for M480 Series

BootIspLib.h
Go to the documentation of this file.
1 /**************************************************************************/
12 #ifndef __BLISPLIB_H__
13 #define __BLISPLIB_H__
14
15 #include "NuMicro.h"
16
25 #ifdef __cplusplus
26 extern "C"
27 {
28 #endif
29
39 void UART1_ISR(void);
40
46 void UART1_ISP(void);
47
53 void HSUSBD_ISR(void);
54
60 void HSUSBD_ISP(void);
61
62
63 #ifdef __cplusplus
64 }
65 #endif
66
67 #endif /* __BLISPLIB_H__ */
68 /* end of group BLISPLIB_EXPORTED_FUNCTIONS */
70 /* end of group BLISPLIB */
72 /* end of group LIBRARY */
74
75 /*** (C) COPYRIGHT 2017 Nuvoton Technology Corp. ***/
76
NuMicro.h
NuMicro peripheral access layer header file.
HSUSBD_ISP
void HSUSBD_ISP(void)
HSUSBD ISP function This function will connect with MKROM ISP tool. And ISP tool will send command th...
UART1_ISP
void UART1_ISP(void)
UART1 ISP function This function will connect with MKROM ISP tool. And ISP tool will send command thr...
UART1_ISR
void UART1_ISR(void)
UART1 Interrupt Handler Secure boot firmware update need use interrupt, this API is used to remap UAR...
HSUSBD_ISR
void HSUSBD_ISR(void)
HSUSBD Interrupt Handler Secure boot firmware update need use interrupt, this API is used to remap HS...