| M480 BSP V3.05.001 The Board Support Package for M480 Series

Data Fields
BCAPDAT_T Struct Reference
Control Register

`#include <bpwm_reg.h>`

## Data Fields
__IO uint32_t | RCAPDAT
__IO uint32_t | FCAPDAT

## Detailed Description

    @addtogroup BPWM Basic Pulse Width Modulation Controller(BPWM)
    Memory Mapped Structure for BPWM Controller

Definition at line 26 of file bpwm_reg.h.

## Field Documentation

## ◆ FCAPDAT

BCAPDAT_T::FCAPDAT

[0x210/0x218/0x220/0x228/0x230/0x238] BPWM Falling Capture Data Register 0~5

FCAPDAT

Offset: 0x210 BPWM Falling Capture Data Register 0~5

Bits | Field | Descriptions
[15:0] | FCAPDAT | BPWM Falling Capture Data (Read Only) When falling capture condition happened, the BPWM counter value will be saved in this register.

Definition at line 68 of file bpwm_reg.h.

## ◆ RCAPDAT

BCAPDAT_T::RCAPDAT

[0x20C/0x214/0x21C/0x224/0x22C/0x234] BPWM Rising Capture Data Register 0~5

RCAPDAT

Offset: 0x20C BPWM Rising Capture Data Register 0~5

Bits | Field | Descriptions
[15:0] | RCAPDAT | BPWM Rising Capture Data (Read Only) When rising capture condition happened, the BPWM counter value will be saved in this register.

Definition at line 67 of file bpwm_reg.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/M480/Include/bpwm_reg.h