| M480 BSP V3.05.001 The Board Support Package for M480 Series

Data Fields
S_RTC_TIME_DATA_T Struct Reference
Standard Driver » RTC Driver » RTC Exported Structs

`#include <rtc.h>`

## Data Fields
uint32_t | u32Year
uint32_t | u32Month
uint32_t | u32Day
uint32_t | u32DayOfWeek
uint32_t | u32Hour
uint32_t | u32Minute
uint32_t | u32Second
uint32_t | u32TimeScale
uint32_t | u32AmPm

## Detailed Description

RTC define Time Data Struct

Definition at line 115 of file rtc.h.

## Field Documentation

## ◆ u32AmPm

uint32_t S_RTC_TIME_DATA_T::u32AmPm

Only Time Scale select 12-hr used

Definition at line 125 of file rtc.h.

## ◆ u32Day

uint32_t S_RTC_TIME_DATA_T::u32Day

Day value

Definition at line 119 of file rtc.h.

## ◆ u32DayOfWeek

uint32_t S_RTC_TIME_DATA_T::u32DayOfWeek

Day of week value

Definition at line 120 of file rtc.h.

## ◆ u32Hour

uint32_t S_RTC_TIME_DATA_T::u32Hour

Hour value

Definition at line 121 of file rtc.h.

## ◆ u32Minute

uint32_t S_RTC_TIME_DATA_T::u32Minute

Minute value

Definition at line 122 of file rtc.h.

## ◆ u32Month

uint32_t S_RTC_TIME_DATA_T::u32Month

Month value

Definition at line 118 of file rtc.h.

## ◆ u32Second

uint32_t S_RTC_TIME_DATA_T::u32Second

Second value

Definition at line 123 of file rtc.h.

## ◆ u32TimeScale

uint32_t S_RTC_TIME_DATA_T::u32TimeScale

12-Hour, 24-Hour

Definition at line 124 of file rtc.h.

## ◆ u32Year

uint32_t S_RTC_TIME_DATA_T::u32Year

Year value

Definition at line 117 of file rtc.h.

The documentation for this struct was generated from the following file:

- StdDriver/inc/rtc.h