| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
sys.c File Reference

M480 series SYS driver source file. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
void | SYS_ClearResetSrc (uint32_t u32Src)
| Clear reset source. More...
uint32_t | SYS_GetBODStatus (void)
| Get Brown-out detector output status. More...
uint32_t | SYS_GetResetSrc (void)
| Get reset status register value. More...
uint32_t | SYS_IsRegLocked (void)
| Check if register is locked nor not. More...
uint32_t | SYS_ReadPDID (void)
| Get product ID. More...
void | SYS_ResetChip (void)
| Reset chip with chip reset. More...
void | SYS_ResetCPU (void)
| Reset chip with CPU reset. More...
void | SYS_ResetModule (uint32_t u32ModuleIndex)
| Reset selected module. More...
void | SYS_EnableBOD (int32_t i32Mode, uint32_t u32BODLevel)
| Enable and configure Brown-out detector function. More...
void | SYS_DisableBOD (void)
| Disable Brown-out detector function. More...
void | SYS_SetPowerLevel (uint32_t u32PowerLevel)
| Set Power Level. More...
void | SYS_SetVRef (uint32_t u32VRefCTL)
| Set Reference Voltage. More...

## Detailed Description

M480 series SYS driver source file.

Version
  V1.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file sys.c.