| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros | Functions
epwm.h File Reference

M480 series EPWM driver header file. More...

Go to the source code of this file.

## Macros
#define | EPWM_CHANNEL_NUM
#define | EPWM_CH_0_MASK
#define | EPWM_CH_1_MASK
#define | EPWM_CH_2_MASK
#define | EPWM_CH_3_MASK
#define | EPWM_CH_4_MASK
#define | EPWM_CH_5_MASK
#define | EPWM_UP_COUNTER
#define | EPWM_DOWN_COUNTER
#define | EPWM_UP_DOWN_COUNTER
#define | EPWM_EDGE_ALIGNED
#define | EPWM_CENTER_ALIGNED
#define | EPWM_OUTPUT_NOTHING
#define | EPWM_OUTPUT_LOW
#define | EPWM_OUTPUT_HIGH
#define | EPWM_OUTPUT_TOGGLE
#define | EPWM_SSCTL_SSRC_EPWM0
#define | EPWM_SSCTL_SSRC_EPWM1
#define | EPWM_SSCTL_SSRC_BPWM0
#define | EPWM_SSCTL_SSRC_BPWM1
#define | EPWM_TRG_ADC_EVEN_ZERO
#define | EPWM_TRG_ADC_EVEN_PERIOD
#define | EPWM_TRG_ADC_EVEN_ZERO_PERIOD
#define | EPWM_TRG_ADC_EVEN_COMPARE_UP
#define | EPWM_TRG_ADC_EVEN_COMPARE_DOWN
#define | EPWM_TRG_ADC_ODD_ZERO
#define | EPWM_TRG_ADC_ODD_PERIOD
#define | EPWM_TRG_ADC_ODD_ZERO_PERIOD
#define | EPWM_TRG_ADC_ODD_COMPARE_UP
#define | EPWM_TRG_ADC_ODD_COMPARE_DOWN
#define | EPWM_TRG_ADC_CH_0_FREE_CMP_UP
#define | EPWM_TRG_ADC_CH_0_FREE_CMP_DOWN
#define | EPWM_TRG_ADC_CH_2_FREE_CMP_UP
#define | EPWM_TRG_ADC_CH_2_FREE_CMP_DOWN
#define | EPWM_TRG_ADC_CH_4_FREE_CMP_UP
#define | EPWM_TRG_ADC_CH_4_FREE_CMP_DOWN
#define | EPWM_TRIGGER_DAC_ZERO
#define | EPWM_TRIGGER_DAC_PERIOD
#define | EPWM_TRIGGER_DAC_COMPARE_UP
#define | EPWM_TRIGGER_DAC_COMPARE_DOWN
#define | EPWM_FB_EDGE_ACMP0
#define | EPWM_FB_EDGE_ACMP1
#define | EPWM_FB_EDGE_BKP0
#define | EPWM_FB_EDGE_BKP1
#define | EPWM_FB_EDGE_ADCRM
#define | EPWM_FB_EDGE_SYS_CSS
#define | EPWM_FB_EDGE_SYS_BOD
#define | EPWM_FB_EDGE_SYS_RAM
#define | EPWM_FB_EDGE_SYS_COR
#define | EPWM_FB_LEVEL_ACMP0
#define | EPWM_FB_LEVEL_ACMP1
#define | EPWM_FB_LEVEL_BKP0
#define | EPWM_FB_LEVEL_BKP1
#define | EPWM_FB_LEVEL_ADCRM
#define | EPWM_FB_LEVEL_SYS_CSS
#define | EPWM_FB_LEVEL_SYS_BOD
#define | EPWM_FB_LEVEL_SYS_RAM
#define | EPWM_FB_LEVEL_SYS_COR
#define | EPWM_FB_EDGE
#define | EPWM_FB_LEVEL
#define | EPWM_LEBCTL_TRGTYPE_RISING
#define | EPWM_LEBCTL_TRGTYPE_FALLING
#define | EPWM_LEBCTL_TRGTYPE_RISING_OR_FALLING
#define | EPWM_LEBCTL_SRCEN0
#define | EPWM_LEBCTL_SRCEN2
#define | EPWM_LEBCTL_SRCEN4
#define | EPWM_LEBCTL_SRCEN0_2
#define | EPWM_LEBCTL_SRCEN0_4
#define | EPWM_LEBCTL_SRCEN2_4
#define | EPWM_LEBCTL_SRCEN0_2_4
#define | EPWM_CAPTURE_INT_RISING_LATCH
#define | EPWM_CAPTURE_INT_FALLING_LATCH
#define | EPWM_CAPTURE_PDMA_RISING_LATCH
#define | EPWM_CAPTURE_PDMA_FALLING_LATCH
#define | EPWM_CAPTURE_PDMA_RISING_FALLING_LATCH
#define | EPWM_DUTY_INT_DOWN_COUNT_MATCH_CMP
#define | EPWM_DUTY_INT_UP_COUNT_MATCH_CMP
#define | EPWM_IFA_ZERO_POINT
#define | EPWM_IFA_PERIOD_POINT
#define | EPWM_IFA_COMPARE_UP_COUNT_POINT
#define | EPWM_IFA_COMPARE_DOWN_COUNT_POINT
#define | EPWM_LOAD_MODE_IMMEDIATE
#define | EPWM_LOAD_MODE_WINDOW
#define | EPWM_LOAD_MODE_CENTER
#define | EPWM_SYNC_OUT_FROM_SYNCIN_SWSYNC
#define | EPWM_SYNC_OUT_FROM_COUNT_TO_ZERO
#define | EPWM_SYNC_OUT_FROM_COUNT_TO_COMPARATOR
#define | EPWM_SYNC_OUT_DISABLE
#define | EPWM_PHS_DIR_DECREMENT
#define | EPWM_PHS_DIR_INCREMENT
#define | EPWM_NF_CLK_DIV_1
#define | EPWM_NF_CLK_DIV_2
#define | EPWM_NF_CLK_DIV_4
#define | EPWM_NF_CLK_DIV_8
#define | EPWM_NF_CLK_DIV_16
#define | EPWM_NF_CLK_DIV_32
#define | EPWM_NF_CLK_DIV_64
#define | EPWM_NF_CLK_DIV_128
#define | EPWM_CLKSRC_EPWM_CLK
#define | EPWM_CLKSRC_TIMER0
#define | EPWM_CLKSRC_TIMER1
#define | EPWM_CLKSRC_TIMER2
#define | EPWM_CLKSRC_TIMER3
#define | EPWM_FDCTL_FDCKSEL_CLK_DIV_1
#define | EPWM_FDCTL_FDCKSEL_CLK_DIV_2
#define | EPWM_FDCTL_FDCKSEL_CLK_DIV_4
#define | EPWM_FDCTL_FDCKSEL_CLK_DIV_8
#define | EPWM_ENABLE_COMPLEMENTARY_MODE(epwm)
| This macro enable complementary mode. More...
#define | EPWM_DISABLE_COMPLEMENTARY_MODE(epwm)
| This macro disable complementary mode, and enable independent mode. More...
#define | EPWM_ENABLE_GROUP_MODE(epwm)
| This macro enable group mode. More...
#define | EPWM_DISABLE_GROUP_MODE(epwm)
| This macro disable group mode. More...
#define | EPWM_ENABLE_TIMER_SYNC(epwm, u32ChannelMask, u32SyncSrc)
| Enable timer synchronous start counting function of specified channel(s) More...
#define | EPWM_DISABLE_TIMER_SYNC(epwm, u32ChannelMask)
| Disable timer synchronous start counting function of specified channel(s) More...
#define | EPWM_TRIGGER_SYNC_START(epwm)
| This macro enable EPWM counter synchronous start counting function. More...
#define | EPWM_ENABLE_OUTPUT_INVERTER(epwm, u32ChannelMask)
| This macro enable output inverter of specified channel(s) More...
#define | EPWM_GET_CAPTURE_RISING_DATA(epwm, u32ChannelNum)
| This macro get captured rising data. More...
#define | EPWM_GET_CAPTURE_FALLING_DATA(epwm, u32ChannelNum)
| This macro get captured falling data. More...
#define | EPWM_MASK_OUTPUT(epwm, u32ChannelMask, u32LevelMask)
| This macro mask output logic to high or low. More...
#define | EPWM_SET_PRESCALER(epwm, u32ChannelNum, u32Prescaler)
| This macro set the prescaler of the selected channel. More...
#define | EPWM_GET_PRESCALER(epwm, u32ChannelNum)
| This macro get the prescaler of the selected channel. More...
#define | EPWM_SET_CMR(epwm, u32ChannelNum, u32CMR)
| This macro set the comparator of the selected channel. More...
#define | EPWM_GET_CMR(epwm, u32ChannelNum)
| This macro get the comparator of the selected channel. More...
#define | EPWM_SET_FTCMR(epwm, u32ChannelNum, u32FTCMR)
| This macro set the free trigger comparator of the selected channel. More...
#define | EPWM_SET_CNR(epwm, u32ChannelNum, u32CNR)
| This macro set the period of the selected channel. More...
#define | EPWM_GET_CNR(epwm, u32ChannelNum)
| This macro get the period of the selected channel. More...
#define | EPWM_SET_ALIGNED_TYPE(epwm, u32ChannelMask, u32AlignedType)
| This macro set the EPWM aligned type. More...
#define | EPWM_SET_LOAD_WINDOW(epwm, u32ChannelMask)
| Set load window of window loading mode for specified channel(s) More...
#define | EPWM_TRIGGER_SYNC(epwm, u32ChannelNum)
| Trigger synchronous event from specified channel(s) More...
#define | EPWM_CLR_COUNTER(epwm, u32ChannelMask)
| Clear counter of specified channel(s) More...
#define | EPWM_SET_OUTPUT_LEVEL(epwm, u32ChannelMask, u32ZeroLevel, u32CmpUpLevel, u32PeriodLevel, u32CmpDownLevel)
| Set output level at zero, compare up, period(center) and compare down of specified channel(s) More...
#define | EPWM_TRIGGER_BRAKE(epwm, u32ChannelMask, u32BrakeType)
| Trigger brake event from specified channel(s) More...
#define | EPWM_SET_DEADZONE_CLK_SRC(epwm, u32ChannelNum, u32AfterPrescaler)
| Set Dead zone clock source. More...

## Functions
uint32_t | EPWM_ConfigCaptureChannel (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32UnitTimeNsec, uint32_t u32CaptureEdge)
| Configure EPWM capture and get the nearest unit time. More...
uint32_t | EPWM_ConfigOutputChannel (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Frequency, uint32_t u32DutyCycle)
| This function Configure EPWM generator and get the nearest frequency in edge aligned(up counter type) auto-reload mode. More...
void | EPWM_Start (EPWM_T *epwm, uint32_t u32ChannelMask)
| Start EPWM module. More...
void | EPWM_Stop (EPWM_T *epwm, uint32_t u32ChannelMask)
| Stop EPWM module. More...
void | EPWM_ForceStop (EPWM_T *epwm, uint32_t u32ChannelMask)
| Stop EPWM generation immediately by clear channel enable bit. More...
void | EPWM_EnableADCTrigger (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Condition)
| Enable selected channel to trigger ADC. More...
void | EPWM_DisableADCTrigger (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable selected channel to trigger ADC. More...
int32_t | EPWM_EnableADCTriggerPrescale (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Prescale, uint32_t u32PrescaleCnt)
| Enable and configure trigger ADC prescale. More...
void | EPWM_DisableADCTriggerPrescale (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable Trigger ADC prescale function. More...
void | EPWM_ClearADCTriggerFlag (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Condition)
| Clear selected channel trigger ADC flag. More...
uint32_t | EPWM_GetADCTriggerFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get selected channel trigger ADC flag. More...
void | EPWM_EnableDACTrigger (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Condition)
| Enable selected channel to trigger DAC. More...
void | EPWM_DisableDACTrigger (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable selected channel to trigger DAC. More...
void | EPWM_ClearDACTriggerFlag (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Condition)
| Clear selected channel trigger DAC flag. More...
uint32_t | EPWM_GetDACTriggerFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get selected channel trigger DAC flag. More...
void | EPWM_EnableFaultBrake (EPWM_T *epwm, uint32_t u32ChannelMask, uint32_t u32LevelMask, uint32_t u32BrakeSource)
| This function enable fault brake of selected channel(s) More...
void | EPWM_EnableCapture (EPWM_T *epwm, uint32_t u32ChannelMask)
| Enable capture of selected channel(s) More...
void | EPWM_DisableCapture (EPWM_T *epwm, uint32_t u32ChannelMask)
| Disable capture of selected channel(s) More...
void | EPWM_EnableOutput (EPWM_T *epwm, uint32_t u32ChannelMask)
| Enables EPWM output generation of selected channel(s) More...
void | EPWM_DisableOutput (EPWM_T *epwm, uint32_t u32ChannelMask)
| Disables EPWM output generation of selected channel(s) More...
void | EPWM_EnablePDMA (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32RisingFirst, uint32_t u32Mode)
| Enables PDMA transfer of selected channel for EPWM capture. More...
void | EPWM_DisablePDMA (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disables PDMA transfer of selected channel for EPWM capture. More...
void | EPWM_EnableDeadZone (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Duration)
| Enable Dead zone of selected channel. More...
void | EPWM_DisableDeadZone (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable Dead zone of selected channel. More...
void | EPWM_EnableCaptureInt (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Edge)
| Enable capture interrupt of selected channel. More...
void | EPWM_DisableCaptureInt (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Edge)
| Disable capture interrupt of selected channel. More...
void | EPWM_ClearCaptureIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32Edge)
| Clear capture interrupt of selected channel. More...
uint32_t | EPWM_GetCaptureIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get capture interrupt of selected channel. More...
void | EPWM_EnableDutyInt (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32IntDutyType)
| Enable duty interrupt of selected channel. More...
void | EPWM_DisableDutyInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable duty interrupt of selected channel. More...
void | EPWM_ClearDutyIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Clear duty interrupt flag of selected channel. More...
uint32_t | EPWM_GetDutyIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get duty interrupt flag of selected channel. More...
void | EPWM_EnableFaultBrakeInt (EPWM_T *epwm, uint32_t u32BrakeSource)
| This function enable fault brake interrupt. More...
void | EPWM_DisableFaultBrakeInt (EPWM_T *epwm, uint32_t u32BrakeSource)
| This function disable fault brake interrupt. More...
void | EPWM_ClearFaultBrakeIntFlag (EPWM_T *epwm, uint32_t u32BrakeSource)
| This function clear fault brake interrupt of selected source. More...
uint32_t | EPWM_GetFaultBrakeIntFlag (EPWM_T *epwm, uint32_t u32BrakeSource)
| This function get fault brake interrupt flag of selected source. More...
void | EPWM_EnablePeriodInt (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32IntPeriodType)
| Enable period interrupt of selected channel. More...
void | EPWM_DisablePeriodInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable period interrupt of selected channel. More...
void | EPWM_ClearPeriodIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Clear period interrupt of selected channel. More...
uint32_t | EPWM_GetPeriodIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get period interrupt of selected channel. More...
void | EPWM_EnableZeroInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Enable zero interrupt of selected channel. More...
void | EPWM_DisableZeroInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable zero interrupt of selected channel. More...
void | EPWM_ClearZeroIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Clear zero interrupt of selected channel. More...
uint32_t | EPWM_GetZeroIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get zero interrupt of selected channel. More...
void | EPWM_EnableAcc (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32IntFlagCnt, uint32_t u32IntAccSrc)
| Enable interrupt flag accumulator of selected channel. More...
void | EPWM_DisableAcc (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable interrupt flag accumulator of selected channel. More...
void | EPWM_EnableAccInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Enable interrupt flag accumulator interrupt of selected channel. More...
void | EPWM_DisableAccInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable interrupt flag accumulator interrupt of selected channel. More...
void | EPWM_ClearAccInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Clear interrupt flag accumulator interrupt of selected channel. More...
uint32_t | EPWM_GetAccInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get interrupt flag accumulator interrupt of selected channel. More...
void | EPWM_EnableAccPDMA (EPWM_T *epwm, uint32_t u32ChannelNum)
| Enable accumulator PDMA of selected channel. More...
void | EPWM_DisableAccPDMA (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable accumulator PDMA of selected channel. More...
void | EPWM_EnableAccStopMode (EPWM_T *epwm, uint32_t u32ChannelNum)
| Enable interrupt flag accumulator stop mode of selected channel. More...
void | EPWM_DisableAccStopMode (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable interrupt flag accumulator stop mode of selected channel. More...
void | EPWM_ClearFTDutyIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Clear free trigger duty interrupt flag of selected channel. More...
uint32_t | EPWM_GetFTDutyIntFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get free trigger duty interrupt flag of selected channel. More...
void | EPWM_EnableLoadMode (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32LoadMode)
| Enable load mode of selected channel. More...
void | EPWM_DisableLoadMode (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32LoadMode)
| Disable load mode of selected channel. More...
void | EPWM_ConfigSyncPhase (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32SyncSrc, uint32_t u32Direction, uint32_t u32StartPhase)
| Configure synchronization phase of selected channel. More...
void | EPWM_EnableSyncPhase (EPWM_T *epwm, uint32_t u32ChannelMask)
| Enable SYNC phase of selected channel(s) More...
void | EPWM_DisableSyncPhase (EPWM_T *epwm, uint32_t u32ChannelMask)
| Disable SYNC phase of selected channel(s) More...
void | EPWM_EnableSyncNoiseFilter (EPWM_T *epwm, uint32_t u32ClkCnt, uint32_t u32ClkDivSel)
| Enable EPWM SYNC_IN noise filter function. More...
void | EPWM_DisableSyncNoiseFilter (EPWM_T *epwm)
| Disable EPWM SYNC_IN noise filter function. More...
void | EPWM_EnableSyncPinInverse (EPWM_T *epwm)
| Enable EPWM SYNC input pin inverse function. More...
void | EPWM_DisableSyncPinInverse (EPWM_T *epwm)
| Disable EPWM SYNC input pin inverse function. More...
void | EPWM_SetClockSource (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32ClkSrcSel)
| Set EPWM clock source. More...
void | EPWM_EnableBrakeNoiseFilter (EPWM_T *epwm, uint32_t u32BrakePinNum, uint32_t u32ClkCnt, uint32_t u32ClkDivSel)
| Enable EPWM brake noise filter function. More...
void | EPWM_DisableBrakeNoiseFilter (EPWM_T *epwm, uint32_t u32BrakePinNum)
| Disable EPWM brake noise filter function. More...
void | EPWM_EnableBrakePinInverse (EPWM_T *epwm, uint32_t u32BrakePinNum)
| Enable EPWM brake pin inverse function. More...
void | EPWM_DisableBrakePinInverse (EPWM_T *epwm, uint32_t u32BrakePinNum)
| Disable EPWM brake pin inverse function. More...
void | EPWM_SetBrakePinSource (EPWM_T *epwm, uint32_t u32BrakePinNum, uint32_t u32SelAnotherModule)
| Set EPWM brake pin source. More...
void | EPWM_SetLeadingEdgeBlanking (EPWM_T *epwm, uint32_t u32TrigSrcSel, uint32_t u32TrigType, uint32_t u32BlankingCnt, uint32_t u32BlankingEnable)
| Set EPWM leading edge blanking function. More...
uint32_t | EPWM_GetWrapAroundFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get the time-base counter reached its maximum value flag of selected channel. More...
void | EPWM_ClearWrapAroundFlag (EPWM_T *epwm, uint32_t u32ChannelNum)
| Clear the time-base counter reached its maximum value flag of selected channel. More...
void | EPWM_EnableFaultDetect (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32AfterPrescaler, uint32_t u32ClkSel)
| Enable fault detect of selected channel. More...
void | EPWM_DisableFaultDetect (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable fault detect of selected channel. More...
void | EPWM_EnableFaultDetectOutput (EPWM_T *epwm, uint32_t u32ChannelNum)
| Enable fault detect output of selected channel. More...
void | EPWM_DisableFaultDetectOutput (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable fault detect output of selected channel. More...
void | EPWM_EnableFaultDetectDeglitch (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32DeglitchSmpCycle)
| Enable fault detect deglitch function of selected channel. More...
void | EPWM_DisableFaultDetectDeglitch (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable fault detect deglitch function of selected channel. More...
void | EPWM_EnableFaultDetectMask (EPWM_T *epwm, uint32_t u32ChannelNum, uint32_t u32MaskCnt)
| Enable fault detect mask function of selected channel. More...
void | EPWM_DisableFaultDetectMask (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable fault detect mask function of selected channel. More...
void | EPWM_EnableFaultDetectInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Enable fault detect interrupt of selected channel. More...
void | EPWM_DisableFaultDetectInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Disable fault detect interrupt of selected channel. More...
void | EPWM_ClearFaultDetectInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Clear fault detect interrupt of selected channel. More...
uint32_t | EPWM_GetFaultDetectInt (EPWM_T *epwm, uint32_t u32ChannelNum)
| Get fault detect interrupt of selected channel. More...

## Detailed Description

M480 series EPWM driver header file.

Version
  V3.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file epwm.h.