| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
GPIO Exported Constants
Standard Driver » GPIO Driver

## Macros
#define | GPIO_PIN_MAX
#define | GPIO_MODE_INPUT
#define | GPIO_MODE_OUTPUT
#define | GPIO_MODE_OPEN_DRAIN
#define | GPIO_MODE_QUASI
#define | GPIO_INT_RISING
#define | GPIO_INT_FALLING
#define | GPIO_INT_BOTH_EDGE
#define | GPIO_INT_HIGH
#define | GPIO_INT_LOW
#define | GPIO_INTTYPE_EDGE
#define | GPIO_INTTYPE_LEVEL
#define | GPIO_SLEWCTL_NORMAL
#define | GPIO_SLEWCTL_HIGH
#define | GPIO_SLEWCTL_FAST
#define | GPIO_PUSEL_DISABLE
#define | GPIO_PUSEL_PULL_UP
#define | GPIO_PUSEL_PULL_DOWN
#define | GPIO_DBCTL_ICLK_ON
#define | GPIO_DBCTL_ICLK_OFF
#define | GPIO_DBCTL_DBCLKSRC_LIRC
#define | GPIO_DBCTL_DBCLKSRC_HCLK
#define | GPIO_DBCTL_DBCLKSEL_1
#define | GPIO_DBCTL_DBCLKSEL_2
#define | GPIO_DBCTL_DBCLKSEL_4
#define | GPIO_DBCTL_DBCLKSEL_8
#define | GPIO_DBCTL_DBCLKSEL_16
#define | GPIO_DBCTL_DBCLKSEL_32
#define | GPIO_DBCTL_DBCLKSEL_64
#define | GPIO_DBCTL_DBCLKSEL_128
#define | GPIO_DBCTL_DBCLKSEL_256
#define | GPIO_DBCTL_DBCLKSEL_512
#define | GPIO_DBCTL_DBCLKSEL_1024
#define | GPIO_DBCTL_DBCLKSEL_2048
#define | GPIO_DBCTL_DBCLKSEL_4096
#define | GPIO_DBCTL_DBCLKSEL_8192
#define | GPIO_DBCTL_DBCLKSEL_16384
#define | GPIO_DBCTL_DBCLKSEL_32768
#define | GPIO_PIN_DATA(port, pin)
#define | PA0
#define | PA1
#define | PA2
#define | PA3
#define | PA4
#define | PA5
#define | PA6
#define | PA7
#define | PA8
#define | PA9
#define | PA10
#define | PA11
#define | PA12
#define | PA13
#define | PA14
#define | PA15
#define | PB0
#define | PB1
#define | PB2
#define | PB3
#define | PB4
#define | PB5
#define | PB6
#define | PB7
#define | PB8
#define | PB9
#define | PB10
#define | PB11
#define | PB12
#define | PB13
#define | PB14
#define | PB15
#define | PC0
#define | PC1
#define | PC2
#define | PC3
#define | PC4
#define | PC5
#define | PC6
#define | PC7
#define | PC8
#define | PC9
#define | PC10
#define | PC11
#define | PC12
#define | PC13
#define | PC14
#define | PD0
#define | PD1
#define | PD2
#define | PD3
#define | PD4
#define | PD5
#define | PD6
#define | PD7
#define | PD8
#define | PD9
#define | PD10
#define | PD11
#define | PD12
#define | PD13
#define | PD14
#define | PE0
#define | PE1
#define | PE2
#define | PE3
#define | PE4
#define | PE5
#define | PE6
#define | PE7
#define | PE8
#define | PE9
#define | PE10
#define | PE11
#define | PE12
#define | PE13
#define | PE14
#define | PE15
#define | PF0
#define | PF1
#define | PF2
#define | PF3
#define | PF4
#define | PF5
#define | PF6
#define | PF7
#define | PF8
#define | PF9
#define | PF10
#define | PF11
#define | PG0
#define | PG1
#define | PG2
#define | PG3
#define | PG4
#define | PG5
#define | PG6
#define | PG7
#define | PG8
#define | PG9
#define | PG10
#define | PG11
#define | PG12
#define | PG13
#define | PG14
#define | PG15
#define | PH0
#define | PH1
#define | PH2
#define | PH3
#define | PH4
#define | PH5
#define | PH6
#define | PH7
#define | PH8
#define | PH9
#define | PH10
#define | PH11

## Detailed Description

## Macro Definition Documentation

## ◆ GPIO_DBCTL_DBCLKSEL_1

#define GPIO_DBCTL_DBCLKSEL_1

GPIO_DBCTL setting for sampling cycle = 1 clocks

Definition at line 83 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_1024

#define GPIO_DBCTL_DBCLKSEL_1024

GPIO_DBCTL setting for sampling cycle = 1024 clocks

Definition at line 93 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_128

#define GPIO_DBCTL_DBCLKSEL_128

GPIO_DBCTL setting for sampling cycle = 128 clocks

Definition at line 90 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_16

#define GPIO_DBCTL_DBCLKSEL_16

GPIO_DBCTL setting for sampling cycle = 16 clocks

Definition at line 87 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_16384

#define GPIO_DBCTL_DBCLKSEL_16384

GPIO_DBCTL setting for sampling cycle = 16384 clocks

Definition at line 97 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_2

#define GPIO_DBCTL_DBCLKSEL_2

GPIO_DBCTL setting for sampling cycle = 2 clocks

Definition at line 84 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_2048

#define GPIO_DBCTL_DBCLKSEL_2048

GPIO_DBCTL setting for sampling cycle = 2048 clocks

Definition at line 94 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_256

#define GPIO_DBCTL_DBCLKSEL_256

GPIO_DBCTL setting for sampling cycle = 256 clocks

Definition at line 91 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_32

#define GPIO_DBCTL_DBCLKSEL_32

GPIO_DBCTL setting for sampling cycle = 32 clocks

Definition at line 88 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_32768

#define GPIO_DBCTL_DBCLKSEL_32768

GPIO_DBCTL setting for sampling cycle = 32768 clocks

Definition at line 98 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_4

#define GPIO_DBCTL_DBCLKSEL_4

GPIO_DBCTL setting for sampling cycle = 4 clocks

Definition at line 85 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_4096

#define GPIO_DBCTL_DBCLKSEL_4096

GPIO_DBCTL setting for sampling cycle = 4096 clocks

Definition at line 95 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_512

#define GPIO_DBCTL_DBCLKSEL_512

GPIO_DBCTL setting for sampling cycle = 512 clocks

Definition at line 92 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_64

#define GPIO_DBCTL_DBCLKSEL_64

GPIO_DBCTL setting for sampling cycle = 64 clocks

Definition at line 89 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_8

#define GPIO_DBCTL_DBCLKSEL_8

GPIO_DBCTL setting for sampling cycle = 8 clocks

Definition at line 86 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSEL_8192

#define GPIO_DBCTL_DBCLKSEL_8192

GPIO_DBCTL setting for sampling cycle = 8192 clocks

Definition at line 96 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSRC_HCLK

#define GPIO_DBCTL_DBCLKSRC_HCLK

GPIO_DBCTL setting for de-bounce counter clock source is the HCLK

Definition at line 81 of file gpio.h.

## ◆ GPIO_DBCTL_DBCLKSRC_LIRC

#define GPIO_DBCTL_DBCLKSRC_LIRC

GPIO_DBCTL setting for de-bounce counter clock source is the internal 10 kHz

Definition at line 80 of file gpio.h.

## ◆ GPIO_DBCTL_ICLK_OFF

#define GPIO_DBCTL_ICLK_OFF

GPIO_DBCTL setting for edge detection circuit is active only if IO pin corresponding GPIOx_IEN bit is set to 1

Definition at line 78 of file gpio.h.

## ◆ GPIO_DBCTL_ICLK_ON

#define GPIO_DBCTL_ICLK_ON

GPIO_DBCTL setting for all IO pins edge detection circuit is always active after reset

Definition at line 77 of file gpio.h.

## ◆ GPIO_INT_BOTH_EDGE

#define GPIO_INT_BOTH_EDGE

Interrupt enable by both Rising Edge and Falling Edge

Definition at line 48 of file gpio.h.

## ◆ GPIO_INT_FALLING

#define GPIO_INT_FALLING

Interrupt enable by Input Falling Edge

Definition at line 47 of file gpio.h.

## ◆ GPIO_INT_HIGH

#define GPIO_INT_HIGH

Interrupt enable by Level-High

Definition at line 49 of file gpio.h.

## ◆ GPIO_INT_LOW

#define GPIO_INT_LOW

Interrupt enable by Level-Level

Definition at line 50 of file gpio.h.

## ◆ GPIO_INT_RISING

#define GPIO_INT_RISING

Interrupt enable by Input Rising Edge

Definition at line 46 of file gpio.h.

## ◆ GPIO_INTTYPE_EDGE

#define GPIO_INTTYPE_EDGE

GPIO_INTTYPE Setting for Edge Trigger Mode

Definition at line 56 of file gpio.h.

## ◆ GPIO_INTTYPE_LEVEL

#define GPIO_INTTYPE_LEVEL

GPIO_INTTYPE Setting for Edge Level Mode

Definition at line 57 of file gpio.h.

## ◆ GPIO_MODE_INPUT

#define GPIO_MODE_INPUT

Input Mode

Definition at line 37 of file gpio.h.

## ◆ GPIO_MODE_OPEN_DRAIN

#define GPIO_MODE_OPEN_DRAIN

Open-Drain Mode

Definition at line 39 of file gpio.h.

## ◆ GPIO_MODE_OUTPUT

#define GPIO_MODE_OUTPUT

Output Mode

Definition at line 38 of file gpio.h.

## ◆ GPIO_MODE_QUASI

#define GPIO_MODE_QUASI

Quasi-bidirectional Mode

Definition at line 40 of file gpio.h.

## ◆ GPIO_PIN_DATA

#define GPIO_PIN_DATA | ( |  | port,
|  |  | pin
| ) |  |

Pin Data Input/Output

Definition at line 115 of file gpio.h.

## ◆ GPIO_PIN_MAX

#define GPIO_PIN_MAX

Specify Maximum Pins of Each GPIO Port

Definition at line 31 of file gpio.h.

## ◆ GPIO_PUSEL_DISABLE

#define GPIO_PUSEL_DISABLE

GPIO PUSEL setting for Disable Mode

Definition at line 69 of file gpio.h.

## ◆ GPIO_PUSEL_PULL_DOWN

#define GPIO_PUSEL_PULL_DOWN

GPIO PUSEL setting for Pull-down Mode

Definition at line 71 of file gpio.h.

## ◆ GPIO_PUSEL_PULL_UP

#define GPIO_PUSEL_PULL_UP

GPIO PUSEL setting for Pull-up Mode

Definition at line 70 of file gpio.h.

## ◆ GPIO_SLEWCTL_FAST

#define GPIO_SLEWCTL_FAST

GPIO slew setting for fast Mode

Definition at line 64 of file gpio.h.

## ◆ GPIO_SLEWCTL_HIGH

#define GPIO_SLEWCTL_HIGH

GPIO slew setting for high Mode

Definition at line 63 of file gpio.h.

## ◆ GPIO_SLEWCTL_NORMAL

#define GPIO_SLEWCTL_NORMAL

GPIO slew setting for normal Mode

Definition at line 62 of file gpio.h.

## ◆ PA0

#define PA0

Specify PA.0 Pin Data Input/Output

Definition at line 116 of file gpio.h.

## ◆ PA1

#define PA1

Specify PA.1 Pin Data Input/Output

Definition at line 117 of file gpio.h.

## ◆ PA10

#define PA10

Specify PA.10 Pin Data Input/Output

Definition at line 126 of file gpio.h.

## ◆ PA11

#define PA11

Specify PA.11 Pin Data Input/Output

Definition at line 127 of file gpio.h.

## ◆ PA12

#define PA12

Specify PA.12 Pin Data Input/Output

Definition at line 128 of file gpio.h.

## ◆ PA13

#define PA13

Specify PA.13 Pin Data Input/Output

Definition at line 129 of file gpio.h.

## ◆ PA14

#define PA14

Specify PA.14 Pin Data Input/Output

Definition at line 130 of file gpio.h.

## ◆ PA15

#define PA15

Specify PA.15 Pin Data Input/Output

Definition at line 131 of file gpio.h.

## ◆ PA2

#define PA2

Specify PA.2 Pin Data Input/Output

Definition at line 118 of file gpio.h.

## ◆ PA3

#define PA3

Specify PA.3 Pin Data Input/Output

Definition at line 119 of file gpio.h.

## ◆ PA4

#define PA4

Specify PA.4 Pin Data Input/Output

Definition at line 120 of file gpio.h.

## ◆ PA5

#define PA5

Specify PA.5 Pin Data Input/Output

Definition at line 121 of file gpio.h.

## ◆ PA6

#define PA6

Specify PA.6 Pin Data Input/Output

Definition at line 122 of file gpio.h.

## ◆ PA7

#define PA7

Specify PA.7 Pin Data Input/Output

Definition at line 123 of file gpio.h.

## ◆ PA8

#define PA8

Specify PA.8 Pin Data Input/Output

Definition at line 124 of file gpio.h.

## ◆ PA9

#define PA9

Specify PA.9 Pin Data Input/Output

Definition at line 125 of file gpio.h.

## ◆ PB0

#define PB0

Specify PB.0 Pin Data Input/Output

Definition at line 132 of file gpio.h.

## ◆ PB1

#define PB1

Specify PB.1 Pin Data Input/Output

Definition at line 133 of file gpio.h.

## ◆ PB10

#define PB10

Specify PB.10 Pin Data Input/Output

Definition at line 142 of file gpio.h.

## ◆ PB11

#define PB11

Specify PB.11 Pin Data Input/Output

Definition at line 143 of file gpio.h.

## ◆ PB12

#define PB12

Specify PB.12 Pin Data Input/Output

Definition at line 144 of file gpio.h.

## ◆ PB13

#define PB13

Specify PB.13 Pin Data Input/Output

Definition at line 145 of file gpio.h.

## ◆ PB14

#define PB14

Specify PB.14 Pin Data Input/Output

Definition at line 146 of file gpio.h.

## ◆ PB15

#define PB15

Specify PB.15 Pin Data Input/Output

Definition at line 147 of file gpio.h.

## ◆ PB2

#define PB2

Specify PB.2 Pin Data Input/Output

Definition at line 134 of file gpio.h.

## ◆ PB3

#define PB3

Specify PB.3 Pin Data Input/Output

Definition at line 135 of file gpio.h.

## ◆ PB4

#define PB4

Specify PB.4 Pin Data Input/Output

Definition at line 136 of file gpio.h.

## ◆ PB5

#define PB5

Specify PB.5 Pin Data Input/Output

Definition at line 137 of file gpio.h.

## ◆ PB6

#define PB6

Specify PB.6 Pin Data Input/Output

Definition at line 138 of file gpio.h.

## ◆ PB7

#define PB7

Specify PB.7 Pin Data Input/Output

Definition at line 139 of file gpio.h.

## ◆ PB8

#define PB8

Specify PB.8 Pin Data Input/Output

Definition at line 140 of file gpio.h.

## ◆ PB9

#define PB9

Specify PB.9 Pin Data Input/Output

Definition at line 141 of file gpio.h.

## ◆ PC0

#define PC0

Specify PC.0 Pin Data Input/Output

Definition at line 148 of file gpio.h.

## ◆ PC1

#define PC1

Specify PC.1 Pin Data Input/Output

Definition at line 149 of file gpio.h.

## ◆ PC10

#define PC10

Specify PC.10 Pin Data Input/Output

Definition at line 158 of file gpio.h.

## ◆ PC11

#define PC11

Specify PC.11 Pin Data Input/Output

Definition at line 159 of file gpio.h.

## ◆ PC12

#define PC12

Specify PC.12 Pin Data Input/Output

Definition at line 160 of file gpio.h.

## ◆ PC13

#define PC13

Specify PC.13 Pin Data Input/Output

Definition at line 161 of file gpio.h.

## ◆ PC14

#define PC14

Specify PC.14 Pin Data Input/Output

Definition at line 162 of file gpio.h.

## ◆ PC2

#define PC2

Specify PC.2 Pin Data Input/Output

Definition at line 150 of file gpio.h.

## ◆ PC3

#define PC3

Specify PC.3 Pin Data Input/Output

Definition at line 151 of file gpio.h.

## ◆ PC4

#define PC4

Specify PC.4 Pin Data Input/Output

Definition at line 152 of file gpio.h.

## ◆ PC5

#define PC5

Specify PC.5 Pin Data Input/Output

Definition at line 153 of file gpio.h.

## ◆ PC6

#define PC6

Specify PC.6 Pin Data Input/Output

Definition at line 154 of file gpio.h.

## ◆ PC7

#define PC7

Specify PC.7 Pin Data Input/Output

Definition at line 155 of file gpio.h.

## ◆ PC8

#define PC8

Specify PC.8 Pin Data Input/Output

Definition at line 156 of file gpio.h.

## ◆ PC9

#define PC9

Specify PC.9 Pin Data Input/Output

Definition at line 157 of file gpio.h.

## ◆ PD0

#define PD0

Specify PD.0 Pin Data Input/Output

Definition at line 163 of file gpio.h.

## ◆ PD1

#define PD1

Specify PD.1 Pin Data Input/Output

Definition at line 164 of file gpio.h.

## ◆ PD10

#define PD10

Specify PD.10 Pin Data Input/Output

Definition at line 173 of file gpio.h.

## ◆ PD11

#define PD11

Specify PD.11 Pin Data Input/Output

Definition at line 174 of file gpio.h.

## ◆ PD12

#define PD12

Specify PD.12 Pin Data Input/Output

Definition at line 175 of file gpio.h.

## ◆ PD13

#define PD13

Specify PD.13 Pin Data Input/Output

Definition at line 176 of file gpio.h.

## ◆ PD14

#define PD14

Specify PD.14 Pin Data Input/Output

Definition at line 177 of file gpio.h.

## ◆ PD2

#define PD2

Specify PD.2 Pin Data Input/Output

Definition at line 165 of file gpio.h.

## ◆ PD3

#define PD3

Specify PD.3 Pin Data Input/Output

Definition at line 166 of file gpio.h.

## ◆ PD4

#define PD4

Specify PD.4 Pin Data Input/Output

Definition at line 167 of file gpio.h.

## ◆ PD5

#define PD5

Specify PD.5 Pin Data Input/Output

Definition at line 168 of file gpio.h.

## ◆ PD6

#define PD6

Specify PD.6 Pin Data Input/Output

Definition at line 169 of file gpio.h.

## ◆ PD7

#define PD7

Specify PD.7 Pin Data Input/Output

Definition at line 170 of file gpio.h.

## ◆ PD8

#define PD8

Specify PD.8 Pin Data Input/Output

Definition at line 171 of file gpio.h.

## ◆ PD9

#define PD9

Specify PD.9 Pin Data Input/Output

Definition at line 172 of file gpio.h.

## ◆ PE0

#define PE0

Specify PE.0 Pin Data Input/Output

Definition at line 178 of file gpio.h.

## ◆ PE1

#define PE1

Specify PE.1 Pin Data Input/Output

Definition at line 179 of file gpio.h.

## ◆ PE10

#define PE10

Specify PE.10 Pin Data Input/Output

Definition at line 188 of file gpio.h.

## ◆ PE11

#define PE11

Specify PE.11 Pin Data Input/Output

Definition at line 189 of file gpio.h.

## ◆ PE12

#define PE12

Specify PE.12 Pin Data Input/Output

Definition at line 190 of file gpio.h.

## ◆ PE13

#define PE13

Specify PE.13 Pin Data Input/Output

Definition at line 191 of file gpio.h.

## ◆ PE14

#define PE14

Specify PE.14 Pin Data Input/Output

Definition at line 192 of file gpio.h.

## ◆ PE15

#define PE15

Specify PE.15 Pin Data Input/Output

Definition at line 193 of file gpio.h.

## ◆ PE2

#define PE2

Specify PE.2 Pin Data Input/Output

Definition at line 180 of file gpio.h.

## ◆ PE3

#define PE3

Specify PE.3 Pin Data Input/Output

Definition at line 181 of file gpio.h.

## ◆ PE4

#define PE4

Specify PE.4 Pin Data Input/Output

Definition at line 182 of file gpio.h.

## ◆ PE5

#define PE5

Specify PE.5 Pin Data Input/Output

Definition at line 183 of file gpio.h.

## ◆ PE6

#define PE6

Specify PE.6 Pin Data Input/Output

Definition at line 184 of file gpio.h.

## ◆ PE7

#define PE7

Specify PE.7 Pin Data Input/Output

Definition at line 185 of file gpio.h.

## ◆ PE8

#define PE8

Specify PE.8 Pin Data Input/Output

Definition at line 186 of file gpio.h.

## ◆ PE9

#define PE9

Specify PE.9 Pin Data Input/Output

Definition at line 187 of file gpio.h.

## ◆ PF0

#define PF0

Specify PF.0 Pin Data Input/Output

Definition at line 194 of file gpio.h.

## ◆ PF1

#define PF1

Specify PF.1 Pin Data Input/Output

Definition at line 195 of file gpio.h.

## ◆ PF10

#define PF10

Specify PF.10 Pin Data Input/Output

Definition at line 204 of file gpio.h.

## ◆ PF11

#define PF11

Specify PF.11 Pin Data Input/Output

Definition at line 205 of file gpio.h.

## ◆ PF2

#define PF2

Specify PF.2 Pin Data Input/Output

Definition at line 196 of file gpio.h.

## ◆ PF3

#define PF3

Specify PF.3 Pin Data Input/Output

Definition at line 197 of file gpio.h.

## ◆ PF4

#define PF4

Specify PF.4 Pin Data Input/Output

Definition at line 198 of file gpio.h.

## ◆ PF5

#define PF5

Specify PF.5 Pin Data Input/Output

Definition at line 199 of file gpio.h.

## ◆ PF6

#define PF6

Specify PF.6 Pin Data Input/Output

Definition at line 200 of file gpio.h.

## ◆ PF7

#define PF7

Specify PF.7 Pin Data Input/Output

Definition at line 201 of file gpio.h.

## ◆ PF8

#define PF8

Specify PF.8 Pin Data Input/Output

Definition at line 202 of file gpio.h.

## ◆ PF9

#define PF9

Specify PF.9 Pin Data Input/Output

Definition at line 203 of file gpio.h.

## ◆ PG0

#define PG0

Specify PG.0 Pin Data Input/Output

Definition at line 206 of file gpio.h.

## ◆ PG1

#define PG1

Specify PG.1 Pin Data Input/Output

Definition at line 207 of file gpio.h.

## ◆ PG10

#define PG10

Specify PG.10 Pin Data Input/Output

Definition at line 216 of file gpio.h.

## ◆ PG11

#define PG11

Specify PG.11 Pin Data Input/Output

Definition at line 217 of file gpio.h.

## ◆ PG12

#define PG12

Specify PG.12 Pin Data Input/Output

Definition at line 218 of file gpio.h.

## ◆ PG13

#define PG13

Specify PG.13 Pin Data Input/Output

Definition at line 219 of file gpio.h.

## ◆ PG14

#define PG14

Specify PG.14 Pin Data Input/Output

Definition at line 220 of file gpio.h.

## ◆ PG15

#define PG15

Specify PG.15 Pin Data Input/Output

Definition at line 221 of file gpio.h.

## ◆ PG2

#define PG2

Specify PG.2 Pin Data Input/Output

Definition at line 208 of file gpio.h.

## ◆ PG3

#define PG3

Specify PG.3 Pin Data Input/Output

Definition at line 209 of file gpio.h.

## ◆ PG4

#define PG4

Specify PG.4 Pin Data Input/Output

Definition at line 210 of file gpio.h.

## ◆ PG5

#define PG5

Specify PG.5 Pin Data Input/Output

Definition at line 211 of file gpio.h.

## ◆ PG6

#define PG6

Specify PG.6 Pin Data Input/Output

Definition at line 212 of file gpio.h.

## ◆ PG7

#define PG7

Specify PG.7 Pin Data Input/Output

Definition at line 213 of file gpio.h.

## ◆ PG8

#define PG8

Specify PG.8 Pin Data Input/Output

Definition at line 214 of file gpio.h.

## ◆ PG9

#define PG9

Specify PG.9 Pin Data Input/Output

Definition at line 215 of file gpio.h.

## ◆ PH0

#define PH0

Specify PH.0 Pin Data Input/Output

Definition at line 222 of file gpio.h.

## ◆ PH1

#define PH1

Specify PH.1 Pin Data Input/Output

Definition at line 223 of file gpio.h.

## ◆ PH10

#define PH10

Specify PH.10 Pin Data Input/Output

Definition at line 232 of file gpio.h.

## ◆ PH11

#define PH11

Specify PH.11 Pin Data Input/Output

Definition at line 233 of file gpio.h.

## ◆ PH2

#define PH2

Specify PH.2 Pin Data Input/Output

Definition at line 224 of file gpio.h.

## ◆ PH3

#define PH3

Specify PH.3 Pin Data Input/Output

Definition at line 225 of file gpio.h.

## ◆ PH4

#define PH4

Specify PH.4 Pin Data Input/Output

Definition at line 226 of file gpio.h.

## ◆ PH5

#define PH5

Specify PH.5 Pin Data Input/Output

Definition at line 227 of file gpio.h.

## ◆ PH6

#define PH6

Specify PH.6 Pin Data Input/Output

Definition at line 228 of file gpio.h.

## ◆ PH7

#define PH7

Specify PH.7 Pin Data Input/Output

Definition at line 229 of file gpio.h.

## ◆ PH8

#define PH8

Specify PH.8 Pin Data Input/Output

Definition at line 230 of file gpio.h.

## ◆ PH9

#define PH9

Specify PH.9 Pin Data Input/Output

Definition at line 231 of file gpio.h.