| M480 BSP V3.05.001 The Board Support Package for M480 Series

Data Fields
STR_CANMASK_T Struct Reference
Standard Driver » CAN Driver » CAN Exported Structs

`#include <can.h>`

## Data Fields
uint8_t | u8Xtd
uint8_t | u8Dir
uint32_t | u32Id
uint8_t | u8IdType

## Detailed Description

CAN mask message structure

Definition at line 68 of file can.h.

## Field Documentation

## ◆ u32Id

uint32_t STR_CANMASK_T::u32Id

Message ID

Definition at line 72 of file can.h.

## ◆ u8Dir

uint8_t STR_CANMASK_T::u8Dir

Direction

Definition at line 71 of file can.h.

## ◆ u8IdType

uint8_t STR_CANMASK_T::u8IdType

ID type

Definition at line 73 of file can.h.

## ◆ u8Xtd

uint8_t STR_CANMASK_T::u8Xtd

Extended ID

Definition at line 70 of file can.h.

The documentation for this struct was generated from the following file:

- StdDriver/inc/can.h