| M480 BSP V3.05.001 The Board Support Package for M480 Series

Data Fields
SCLIB_CARD_INFO_T Struct Reference
Library » Smartcard Library » Smartcard Library Exported Structs

A structure holds smartcard information. More...

`#include <sclib.h>`

## Data Fields
uint32_t | T
uint32_t | ATR_Len
uint8_t | ATR_Buf [SCLIB_MAX_ATR_LEN]

## Detailed Description

A structure holds smartcard information.

Definition at line 90 of file sclib.h.

## Field Documentation

## ◆ ATR_Buf

uint8_t SCLIB_CARD_INFO_T::ATR_Buf[SCLIB_MAX_ATR_LEN]

Buffer holds ATR answered by smartcard.

Definition at line 94 of file sclib.h.

## ◆ ATR_Len

uint32_t SCLIB_CARD_INFO_T::ATR_Len

ATR length, between SCLIB_MAX_ATR_LEN and SCLIB_MIN_ATR_LEN.

Definition at line 93 of file sclib.h.

## ◆ T

uint32_t SCLIB_CARD_INFO_T::T

Protocol, ether SCLIB_PROTOCOL_T0 or SCLIB_PROTOCOL_T1.

Definition at line 92 of file sclib.h.

The documentation for this struct was generated from the following file:

- SmartcardLib/Include/sclib.h