| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
cdc_core.c File Reference

M480 MCU USB Host CDC library core. More...

`#include <stdio.h>`
`#include <string.h>`
`#include <stdlib.h>`
`#include "NuMicro.h"`
`#include "usb.h"`
`#include "usbh_lib.h"`
`#include "usbh_cdc.h"`

Go to the source code of this file.

## Functions
int32_t | usbh_cdc_get_line_coding (CDC_DEV_T *cdev, LINE_CODING_T *line_code)
| GET_LINE_CODING request. More...
int32_t | usbh_cdc_set_line_coding (CDC_DEV_T *cdev, LINE_CODING_T *line_code)
| SET_LINE_CODING request. More...
HIDDEN_SYMBOLS int32_t | usbh_cdc_set_control_line_state (CDC_DEV_T *cdev, int active_carrier, int DTE_present)
| SET_CONTROL_LINE_STATE request. More...
int32_t | usbh_cdc_start_polling_status (CDC_DEV_T *cdev, CDC_CB_FUNC *func)
| Start purge the CDC device's interrupt-in transfer pipe. More...
int32_t | usbh_cdc_start_to_receive_data (CDC_DEV_T *cdev, CDC_CB_FUNC *func)
| Make CDC device start to receive data from bulk-in transfer pipe. More...
int32_t | usbh_cdc_send_data (CDC_DEV_T *cdev, uint8_t *buff, int buff_len)
| Send a block of data via CDC device's bulk-out transfer pipe. More...

## Detailed Description

M480 MCU USB Host CDC library core.

Version
  V1.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2017-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file cdc_core.c.