| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
BootIspLib.h File Reference

Firmware Update library header file. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
void | UART1_ISR (void)
| UART1 Interrupt Handler Secure boot firmware update need use interrupt, this API is used to remap UART1 IRQHandler to MKROM UART1 IRQHandler. More...
void | UART1_ISP (void)
| UART1 ISP function This function will connect with MKROM ISP tool. And ISP tool will send command through UART1 to this function to do firmware update. More...
void | HSUSBD_ISR (void)
| HSUSBD Interrupt Handler Secure boot firmware update need use interrupt, this API is used to remap HSUSBD IRQHandler to MKROM HSUSBD IRQHandler. More...
void | HSUSBD_ISP (void)
| HSUSBD ISP function This function will connect with MKROM ISP tool. And ISP tool will send command through HSUSBD to this function to do firmware update. More...

## Detailed Description

Firmware Update library header file.

Version
  V1.00

Secure Boot provide four APIs to do firmware update. M480 can connect with a PC executing firmware update tool via ether HSUSBD or UART1 to update firmware.

SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2017-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file BootIspLib.h.