| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
ccap.c File Reference

M480 Series CCAP Driver Source File. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
void | CCAP_Open (uint32_t u32InFormat, uint32_t u32OutFormet)
| Open engine clock and sensor clock. More...
void | CCAP_SetCroppingWindow (uint32_t u32VStart, uint32_t u32HStart, uint32_t u32Height, uint32_t u32Width)
| Set Cropping Window Starting Address and Size. More...
void | CCAP_SetPacketBuf (uint32_t u32Address)
| Set System Memory Packet Base Address0 Register. More...
void | CCAP_Close (void)
| Close Camera Capture Interface. More...
void | CCAP_EnableInt (uint32_t u32IntMask)
| Set CCAP Interrupt. More...
void | CCAP_DisableInt (uint32_t u32IntMask)
| Disable CCAP Interrupt. More...
void | CCAP_EnableMono (uint32_t u32Interface)
| Enable Monochrome CMOS Sensor. More...
void | CCAP_DisableMono (void)
| Disable Monochrome CMOS Sensor. More...
void | CCAP_EnableLumaYOne (uint32_t u32th)
| Enable Luminance 8-bit Y to 1-bit Y Conversion. More...
void | CCAP_DisableLumaYOne (void)
| Disable Luminance 8-bit Y to 1-bit Y Conversion. More...
void | CCAP_Start (void)
| Start Camera Capture Interface. More...
void | CCAP_Stop (uint32_t u32FrameComplete)
| Stop Camera Capture Interface. More...
void | CCAP_SetPacketScaling (uint32_t u32VNumerator, uint32_t u32VDenominator, uint32_t u32HNumerator, uint32_t u32HDenominator)
| Set Packet Scaling Vertical and Horizontal Factor Register. More...
void | CCAP_SetPacketStride (uint32_t u32Stride)
| Set Packet Frame Output Pixel Stride Width. More...

## Detailed Description

M480 Series CCAP Driver Source File.

Version
  V1.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file ccap.c.