| M480 BSP V3.05.001 The Board Support Package for M480 Series

Data Fields
ECAPDAT_T Struct Reference
Control Register

`#include <epwm_reg.h>`

## Data Fields
__IO uint32_t | RCAPDAT
__IO uint32_t | FCAPDAT

## Detailed Description

    @addtogroup EPWM Pulse Width Modulation Controller(EPWM)
    Memory Mapped Structure for EPWM Controller

Definition at line 26 of file epwm_reg.h.

## Field Documentation

## ◆ FCAPDAT

ECAPDAT_T::FCAPDAT

[0x210/0x218/0x220/0x228/0x230/0x238] EPWM Falling Capture Data Register 0~5

FCAPDAT

Offset: 0x210 EPWM Falling Capture Data Register 0~5

Bits | Field | Descriptions
[15:0] | FCAPDAT | EPWM Falling Capture Data (Read Only) When falling capture condition happened, the EPWM counter value will be saved in this register.

Definition at line 68 of file epwm_reg.h.

## ◆ RCAPDAT

ECAPDAT_T::RCAPDAT

[0x20C/0x214/0x21C/0x224/0x22C/0x234] EPWM Rising Capture Data Register 0~5

RCAPDAT

Offset: 0x20C EPWM Rising Capture Data Register 0~5

Bits | Field | Descriptions
[15:0] | RCAPDAT | EPWM Rising Capture Data (Read Only) When rising capture condition happened, the EPWM counter value will be saved in this register.

Definition at line 67 of file epwm_reg.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/M480/Include/epwm_reg.h