| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
scuart.c File Reference

M480 Smartcard UART mode (SCUART) driver source file. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
static uint32_t | SCUART_GetClock (SC_T *sc)
void | SCUART_Close (SC_T *sc)
| The function is used to disable smartcard interface UART mode. More...
uint32_t | SCUART_Open (SC_T *sc, uint32_t u32baudrate)
| This function use to enable smartcard module UART mode and set baudrate. More...
uint32_t | SCUART_Read (SC_T *sc, uint8_t pu8RxBuf[], uint32_t u32ReadBytes)
| The function is used to read Rx data from RX FIFO. More...
uint32_t | SCUART_SetLineConfig (SC_T *sc, uint32_t u32Baudrate, uint32_t u32DataWidth, uint32_t u32Parity, uint32_t u32StopBits)
| This function use to configure smartcard UART mode line setting. More...
void | SCUART_SetTimeoutCnt (SC_T *sc, uint32_t u32TOC)
| This function use to set receive timeout count. More...
void | SCUART_Write (SC_T *sc, uint8_t pu8TxBuf[], uint32_t u32WriteBytes)
| This function is to write data into transmit FIFO to send data out. More...

## Detailed Description

M480 Smartcard UART mode (SCUART) driver source file.

Version
  V3.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file scuart.c.

## Function Documentation

## ◆ SCUART_GetClock()

static uint32_t SCUART_GetClock | ( | SC_T * | sc | ) |
| static