| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
ecap.c File Reference

Enhanced Input Capture Timer (ECAP) driver source file. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
void | ECAP_Open (ECAP_T *ecap, uint32_t u32FuncMask)
| Enable ECAP function. More...
void | ECAP_Close (ECAP_T *ecap)
| Disable ECAP function. More...
void | ECAP_EnableINT (ECAP_T *ecap, uint32_t u32Mask)
| This macro is used to enable input channel interrupt. More...
void | ECAP_DisableINT (ECAP_T *ecap, uint32_t u32Mask)
| This macro is used to disable input channel interrupt. More...

## Detailed Description

Enhanced Input Capture Timer (ECAP) driver source file.

Version
  V3.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file ecap.c.