| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros | Functions
sys.h File Reference

M480 Series SYS Driver Header File. More...

Go to the source code of this file.

## Macros
#define | PDMA_RST
#define | EBI_RST
#define | EMAC_RST
#define | SDH0_RST
#define | CRC_RST
#define | CCAP_RST
#define | HSUSBD_RST
#define | CRPT_RST
#define | SPIM_RST
#define | USBH_RST
#define | SDH1_RST
#define | GPIO_RST
#define | TMR0_RST
#define | TMR1_RST
#define | TMR2_RST
#define | TMR3_RST
#define | ACMP01_RST
#define | I2C0_RST
#define | I2C1_RST
#define | I2C2_RST
#define | QSPI0_RST
#define | SPI0_RST
#define | SPI1_RST
#define | SPI2_RST
#define | UART0_RST
#define | UART1_RST
#define | UART2_RST
#define | UART3_RST
#define | UART4_RST
#define | UART5_RST
#define | UART6_RST
#define | UART7_RST
#define | CAN0_RST
#define | CAN1_RST
#define | OTG_RST
#define | USBD_RST
#define | EADC_RST
#define | I2S0_RST
#define | HSOTG_RST
#define | TRNG_RST
#define | SC0_RST
#define | SC1_RST
#define | SC2_RST
#define | QSPI1_RST
#define | SPI3_RST
#define | USCI0_RST
#define | USCI1_RST
#define | DAC_RST
#define | EPWM0_RST
#define | EPWM1_RST
#define | BPWM0_RST
#define | BPWM1_RST
#define | QEI0_RST
#define | QEI1_RST
#define | ECAP0_RST
#define | ECAP1_RST
#define | CAN2_RST
#define | OPA_RST
#define | EADC1_RST
#define | SYS_BODCTL_BOD_RST_EN
#define | SYS_BODCTL_BOD_INTERRUPT_EN
#define | SYS_BODCTL_BODVL_3_0V
#define | SYS_BODCTL_BODVL_2_8V
#define | SYS_BODCTL_BODVL_2_6V
#define | SYS_BODCTL_BODVL_2_4V
#define | SYS_BODCTL_BODVL_2_2V
#define | SYS_BODCTL_BODVL_2_0V
#define | SYS_BODCTL_BODVL_1_8V
#define | SYS_BODCTL_BODVL_1_6V
#define | SYS_VREFCTL_VREF_PIN
#define | SYS_VREFCTL_VREF_1_6V
#define | SYS_VREFCTL_VREF_2_0V
#define | SYS_VREFCTL_VREF_2_5V
#define | SYS_VREFCTL_VREF_3_0V
#define | SYS_VREFCTL_VREF_AVDD
#define | SYS_USBPHY_USBROLE_STD_USBD
#define | SYS_USBPHY_USBROLE_STD_USBH
#define | SYS_USBPHY_USBROLE_ID_DEPH
#define | SYS_USBPHY_USBROLE_ON_THE_GO
#define | SYS_USBPHY_HSUSBROLE_STD_USBD
#define | SYS_USBPHY_HSUSBROLE_STD_USBH
#define | SYS_USBPHY_HSUSBROLE_ID_DEPH
#define | SYS_PLCTL_PLSEL_PL0 (0x0UL<<SYS_PLCTL_PLSEL_Pos)
#define | SYS_PLCTL_PLSEL_PL1 (0x1UL<<SYS_PLCTL_PLSEL_Pos)
#define | SYS_GPA_MFPL_PA0MFP_GPIO
#define | SYS_GPA_MFPL_PA0MFP_SPIM_MOSI
#define | SYS_GPA_MFPL_PA0MFP_QSPI0_MOSI0
#define | SYS_GPA_MFPL_PA0MFP_SPI0_MOSI
#define | SYS_GPA_MFPL_PA0MFP_SD1_DAT0
#define | SYS_GPA_MFPL_PA0MFP_SC0_CLK
#define | SYS_GPA_MFPL_PA0MFP_UART0_RXD
#define | SYS_GPA_MFPL_PA0MFP_UART1_nRTS
#define | SYS_GPA_MFPL_PA0MFP_I2C2_SDA
#define | SYS_GPA_MFPL_PA0MFP_CCAP_DATA6
#define | SYS_GPA_MFPL_PA0MFP_BPWM0_CH0
#define | SYS_GPA_MFPL_PA0MFP_EPWM0_CH5
#define | SYS_GPA_MFPL_PA0MFP_DAC0_ST
#define | SYS_GPA_MFPL_PA1MFP_GPIO
#define | SYS_GPA_MFPL_PA1MFP_SPIM_MISO
#define | SYS_GPA_MFPL_PA1MFP_QSPI0_MISO0
#define | SYS_GPA_MFPL_PA1MFP_SPI0_MISO
#define | SYS_GPA_MFPL_PA1MFP_SD1_DAT1
#define | SYS_GPA_MFPL_PA1MFP_SC0_DAT
#define | SYS_GPA_MFPL_PA1MFP_UART0_TXD
#define | SYS_GPA_MFPL_PA1MFP_UART1_nCTS
#define | SYS_GPA_MFPL_PA1MFP_I2C2_SCL
#define | SYS_GPA_MFPL_PA1MFP_CCAP_DATA7
#define | SYS_GPA_MFPL_PA1MFP_BPWM0_CH1
#define | SYS_GPA_MFPL_PA1MFP_EPWM0_CH4
#define | SYS_GPA_MFPL_PA1MFP_DAC1_ST
#define | SYS_GPA_MFPL_PA2MFP_GPIO
#define | SYS_GPA_MFPL_PA2MFP_SPIM_CLK
#define | SYS_GPA_MFPL_PA2MFP_QSPI0_CLK
#define | SYS_GPA_MFPL_PA2MFP_SPI0_CLK
#define | SYS_GPA_MFPL_PA2MFP_SD1_DAT2
#define | SYS_GPA_MFPL_PA2MFP_SC0_RST
#define | SYS_GPA_MFPL_PA2MFP_UART4_RXD
#define | SYS_GPA_MFPL_PA2MFP_UART1_RXD
#define | SYS_GPA_MFPL_PA2MFP_I2C1_SDA
#define | SYS_GPA_MFPL_PA2MFP_I2C0_SMBSUS
#define | SYS_GPA_MFPL_PA2MFP_BPWM0_CH2
#define | SYS_GPA_MFPL_PA2MFP_EPWM0_CH3
#define | SYS_GPA_MFPL_PA3MFP_GPIO
#define | SYS_GPA_MFPL_PA3MFP_SPIM_SS
#define | SYS_GPA_MFPL_PA3MFP_QSPI0_SS
#define | SYS_GPA_MFPL_PA3MFP_SPI0_SS
#define | SYS_GPA_MFPL_PA3MFP_SD1_DAT3
#define | SYS_GPA_MFPL_PA3MFP_SC0_PWR
#define | SYS_GPA_MFPL_PA3MFP_UART4_TXD
#define | SYS_GPA_MFPL_PA3MFP_UART1_TXD
#define | SYS_GPA_MFPL_PA3MFP_I2C1_SCL
#define | SYS_GPA_MFPL_PA3MFP_I2C0_SMBAL
#define | SYS_GPA_MFPL_PA3MFP_BPWM0_CH3
#define | SYS_GPA_MFPL_PA3MFP_EPWM0_CH2
#define | SYS_GPA_MFPL_PA3MFP_QEI0_B
#define | SYS_GPA_MFPL_PA3MFP_EPWM1_BRAKE1
#define | SYS_GPA_MFPL_PA4MFP_GPIO
#define | SYS_GPA_MFPL_PA4MFP_SPIM_D3
#define | SYS_GPA_MFPL_PA4MFP_QSPI0_MOSI1
#define | SYS_GPA_MFPL_PA4MFP_SPI0_I2SMCLK
#define | SYS_GPA_MFPL_PA4MFP_SD1_CLK
#define | SYS_GPA_MFPL_PA4MFP_SC0_nCD
#define | SYS_GPA_MFPL_PA4MFP_UART0_nRTS
#define | SYS_GPA_MFPL_PA4MFP_UART5_RXD
#define | SYS_GPA_MFPL_PA4MFP_I2C0_SDA
#define | SYS_GPA_MFPL_PA4MFP_CAN0_RXD
#define | SYS_GPA_MFPL_PA4MFP_UART0_RXD
#define | SYS_GPA_MFPL_PA4MFP_BPWM0_CH4
#define | SYS_GPA_MFPL_PA4MFP_EPWM0_CH1
#define | SYS_GPA_MFPL_PA4MFP_QEI0_A
#define | SYS_GPA_MFPL_PA5MFP_GPIO
#define | SYS_GPA_MFPL_PA5MFP_SPIM_D2
#define | SYS_GPA_MFPL_PA5MFP_QSPI0_MISO1
#define | SYS_GPA_MFPL_PA5MFP_SPI1_I2SMCLK
#define | SYS_GPA_MFPL_PA5MFP_SD1_CMD
#define | SYS_GPA_MFPL_PA5MFP_SC2_nCD
#define | SYS_GPA_MFPL_PA5MFP_UART0_nCTS
#define | SYS_GPA_MFPL_PA5MFP_UART5_TXD
#define | SYS_GPA_MFPL_PA5MFP_I2C0_SCL
#define | SYS_GPA_MFPL_PA5MFP_CAN0_TXD
#define | SYS_GPA_MFPL_PA5MFP_UART0_TXD
#define | SYS_GPA_MFPL_PA5MFP_BPWM0_CH5
#define | SYS_GPA_MFPL_PA5MFP_EPWM0_CH0
#define | SYS_GPA_MFPL_PA5MFP_QEI0_INDEX
#define | SYS_GPA_MFPL_PA6MFP_GPIO
#define | SYS_GPA_MFPL_PA6MFP_EBI_AD6
#define | SYS_GPA_MFPL_PA6MFP_EMAC_RMII_RXERR
#define | SYS_GPA_MFPL_PA6MFP_SPI1_SS
#define | SYS_GPA_MFPL_PA6MFP_SD1_nCD
#define | SYS_GPA_MFPL_PA6MFP_SC2_CLK
#define | SYS_GPA_MFPL_PA6MFP_UART0_RXD
#define | SYS_GPA_MFPL_PA6MFP_I2C1_SDA
#define | SYS_GPA_MFPL_PA6MFP_QSPI1_MOSI1
#define | SYS_GPA_MFPL_PA6MFP_EPWM1_CH5
#define | SYS_GPA_MFPL_PA6MFP_BPWM1_CH3
#define | SYS_GPA_MFPL_PA6MFP_ACMP1_WLAT
#define | SYS_GPA_MFPL_PA6MFP_TM3
#define | SYS_GPA_MFPL_PA6MFP_INT0
#define | SYS_GPA_MFPL_PA7MFP_GPIO
#define | SYS_GPA_MFPL_PA7MFP_EBI_AD7
#define | SYS_GPA_MFPL_PA7MFP_EMAC_RMII_CRSDV
#define | SYS_GPA_MFPL_PA7MFP_SPI1_CLK
#define | SYS_GPA_MFPL_PA7MFP_SC2_DAT
#define | SYS_GPA_MFPL_PA7MFP_UART0_TXD
#define | SYS_GPA_MFPL_PA7MFP_I2C1_SCL
#define | SYS_GPA_MFPL_PA7MFP_QSPI1_MISO1
#define | SYS_GPA_MFPL_PA7MFP_EPWM1_CH4
#define | SYS_GPA_MFPL_PA7MFP_BPWM1_CH2
#define | SYS_GPA_MFPL_PA7MFP_ACMP0_WLAT
#define | SYS_GPA_MFPL_PA7MFP_TM2
#define | SYS_GPA_MFPL_PA7MFP_INT1
#define | SYS_GPA_MFPH_PA8MFP_GPIO
#define | SYS_GPA_MFPH_PA8MFP_OPA1_P
#define | SYS_GPA_MFPH_PA8MFP_EADC1_CH4
#define | SYS_GPA_MFPH_PA8MFP_EBI_ALE
#define | SYS_GPA_MFPH_PA8MFP_SC2_CLK
#define | SYS_GPA_MFPH_PA8MFP_SPI2_MOSI
#define | SYS_GPA_MFPH_PA8MFP_SD1_DAT0
#define | SYS_GPA_MFPH_PA8MFP_USCI0_CTL1
#define | SYS_GPA_MFPH_PA8MFP_UART1_RXD
#define | SYS_GPA_MFPH_PA8MFP_UART7_RXD
#define | SYS_GPA_MFPH_PA8MFP_BPWM0_CH3
#define | SYS_GPA_MFPH_PA8MFP_QEI1_B
#define | SYS_GPA_MFPH_PA8MFP_ECAP0_IC2
#define | SYS_GPA_MFPH_PA8MFP_TM3_EXT
#define | SYS_GPA_MFPH_PA8MFP_INT4
#define | SYS_GPA_MFPH_PA9MFP_GPIO
#define | SYS_GPA_MFPH_PA9MFP_OPA1_N
#define | SYS_GPA_MFPH_PA9MFP_EADC1_CH5
#define | SYS_GPA_MFPH_PA9MFP_EBI_MCLK
#define | SYS_GPA_MFPH_PA9MFP_SC2_DAT
#define | SYS_GPA_MFPH_PA9MFP_SPI2_MISO
#define | SYS_GPA_MFPH_PA9MFP_SD1_DAT1
#define | SYS_GPA_MFPH_PA9MFP_USCI0_DAT1
#define | SYS_GPA_MFPH_PA9MFP_UART1_TXD
#define | SYS_GPA_MFPH_PA9MFP_UART7_TXD
#define | SYS_GPA_MFPH_PA9MFP_BPWM0_CH2
#define | SYS_GPA_MFPH_PA9MFP_QEI1_A
#define | SYS_GPA_MFPH_PA9MFP_ECAP0_IC1
#define | SYS_GPA_MFPH_PA9MFP_TM2_EXT
#define | SYS_GPA_MFPH_PA9MFP_SWDH_DAT
#define | SYS_GPA_MFPH_PA10MFP_GPIO
#define | SYS_GPA_MFPH_PA10MFP_ACMP1_P0
#define | SYS_GPA_MFPH_PA10MFP_OPA1_O
#define | SYS_GPA_MFPH_PA10MFP_EADC1_CH6
#define | SYS_GPA_MFPH_PA10MFP_EBI_nWR
#define | SYS_GPA_MFPH_PA10MFP_SC2_RST
#define | SYS_GPA_MFPH_PA10MFP_SPI2_CLK
#define | SYS_GPA_MFPH_PA10MFP_SD1_DAT2
#define | SYS_GPA_MFPH_PA10MFP_USCI0_DAT0
#define | SYS_GPA_MFPH_PA10MFP_I2C2_SDA
#define | SYS_GPA_MFPH_PA10MFP_UART6_RXD
#define | SYS_GPA_MFPH_PA10MFP_BPWM0_CH1
#define | SYS_GPA_MFPH_PA10MFP_QEI1_INDEX
#define | SYS_GPA_MFPH_PA10MFP_ECAP0_IC0
#define | SYS_GPA_MFPH_PA10MFP_TM1_EXT
#define | SYS_GPA_MFPH_PA10MFP_DAC0_ST
#define | SYS_GPA_MFPH_PA10MFP_SWDH_CLK
#define | SYS_GPA_MFPH_PA11MFP_GPIO
#define | SYS_GPA_MFPH_PA11MFP_ACMP0_P0
#define | SYS_GPA_MFPH_PA11MFP_EADC1_CH7
#define | SYS_GPA_MFPH_PA11MFP_EBI_nRD
#define | SYS_GPA_MFPH_PA11MFP_SC2_PWR
#define | SYS_GPA_MFPH_PA11MFP_SPI2_SS
#define | SYS_GPA_MFPH_PA11MFP_SD1_DAT3
#define | SYS_GPA_MFPH_PA11MFP_USCI0_CLK
#define | SYS_GPA_MFPH_PA11MFP_I2C2_SCL
#define | SYS_GPA_MFPH_PA11MFP_UART6_TXD
#define | SYS_GPA_MFPH_PA11MFP_BPWM0_CH0
#define | SYS_GPA_MFPH_PA11MFP_EPWM0_SYNC_OUT
#define | SYS_GPA_MFPH_PA11MFP_TM0_EXT
#define | SYS_GPA_MFPH_PA11MFP_DAC1_ST
#define | SYS_GPA_MFPH_PA12MFP_GPIO
#define | SYS_GPA_MFPH_PA12MFP_I2S0_BCLK
#define | SYS_GPA_MFPH_PA12MFP_UART4_TXD
#define | SYS_GPA_MFPH_PA12MFP_I2C1_SCL
#define | SYS_GPA_MFPH_PA12MFP_SPI2_SS
#define | SYS_GPA_MFPH_PA12MFP_CAN0_TXD
#define | SYS_GPA_MFPH_PA12MFP_SC2_PWR
#define | SYS_GPA_MFPH_PA12MFP_BPWM1_CH2
#define | SYS_GPA_MFPH_PA12MFP_QEI1_INDEX
#define | SYS_GPA_MFPH_PA12MFP_USB_VBUS
#define | SYS_GPA_MFPH_PA13MFP_GPIO
#define | SYS_GPA_MFPH_PA13MFP_I2S0_MCLK
#define | SYS_GPA_MFPH_PA13MFP_UART4_RXD
#define | SYS_GPA_MFPH_PA13MFP_I2C1_SDA
#define | SYS_GPA_MFPH_PA13MFP_SPI2_CLK
#define | SYS_GPA_MFPH_PA13MFP_CAN0_RXD
#define | SYS_GPA_MFPH_PA13MFP_SC2_RST
#define | SYS_GPA_MFPH_PA13MFP_BPWM1_CH3
#define | SYS_GPA_MFPH_PA13MFP_QEI1_A
#define | SYS_GPA_MFPH_PA13MFP_USB_D_N
#define | SYS_GPA_MFPH_PA14MFP_GPIO
#define | SYS_GPA_MFPH_PA14MFP_I2S0_DI
#define | SYS_GPA_MFPH_PA14MFP_UART0_TXD
#define | SYS_GPA_MFPH_PA14MFP_SPI2_MISO
#define | SYS_GPA_MFPH_PA14MFP_I2C2_SCL
#define | SYS_GPA_MFPH_PA14MFP_SC2_DAT
#define | SYS_GPA_MFPH_PA14MFP_BPWM1_CH4
#define | SYS_GPA_MFPH_PA14MFP_QEI1_B
#define | SYS_GPA_MFPH_PA14MFP_USB_D_P
#define | SYS_GPA_MFPH_PA15MFP_GPIO
#define | SYS_GPA_MFPH_PA15MFP_I2S0_DO
#define | SYS_GPA_MFPH_PA15MFP_UART0_RXD
#define | SYS_GPA_MFPH_PA15MFP_SPI2_MOSI
#define | SYS_GPA_MFPH_PA15MFP_I2C2_SDA
#define | SYS_GPA_MFPH_PA15MFP_SC2_CLK
#define | SYS_GPA_MFPH_PA15MFP_BPWM1_CH5
#define | SYS_GPA_MFPH_PA15MFP_EPWM0_SYNC_IN
#define | SYS_GPA_MFPH_PA15MFP_USB_OTG_ID
#define | SYS_GPB_MFPL_PB0MFP_GPIO
#define | SYS_GPB_MFPL_PB0MFP_EADC0_CH0
#define | SYS_GPB_MFPL_PB0MFP_EADC1_CH8
#define | SYS_GPB_MFPL_PB0MFP_OPA0_P
#define | SYS_GPB_MFPL_PB0MFP_EBI_ADR9
#define | SYS_GPB_MFPL_PB0MFP_SD0_CMD
#define | SYS_GPB_MFPL_PB0MFP_SPI2_I2SMCLK
#define | SYS_GPB_MFPL_PB0MFP_UART2_RXD
#define | SYS_GPB_MFPL_PB0MFP_SPI0_I2SMCLK
#define | SYS_GPB_MFPL_PB0MFP_I2C1_SDA
#define | SYS_GPB_MFPL_PB0MFP_EPWM0_CH5
#define | SYS_GPB_MFPL_PB0MFP_EPWM1_CH5
#define | SYS_GPB_MFPL_PB0MFP_EPWM0_BRAKE1
#define | SYS_GPB_MFPL_PB1MFP_GPIO
#define | SYS_GPB_MFPL_PB1MFP_EADC0_CH1
#define | SYS_GPB_MFPL_PB1MFP_OPA0_N
#define | SYS_GPB_MFPL_PB1MFP_EADC1_CH9
#define | SYS_GPB_MFPL_PB1MFP_EBI_ADR8
#define | SYS_GPB_MFPL_PB1MFP_SD0_CLK
#define | SYS_GPB_MFPL_PB1MFP_EMAC_RMII_RXERR
#define | SYS_GPB_MFPL_PB1MFP_SPI1_I2SMCLK
#define | SYS_GPB_MFPL_PB1MFP_SPI3_I2SMCLK
#define | SYS_GPB_MFPL_PB1MFP_UART2_TXD
#define | SYS_GPB_MFPL_PB1MFP_USCI1_CLK
#define | SYS_GPB_MFPL_PB1MFP_I2C1_SCL
#define | SYS_GPB_MFPL_PB1MFP_I2S0_LRCK
#define | SYS_GPB_MFPL_PB1MFP_EPWM0_CH4
#define | SYS_GPB_MFPL_PB1MFP_EPWM1_CH4
#define | SYS_GPB_MFPL_PB1MFP_EPWM0_BRAKE0
#define | SYS_GPB_MFPL_PB2MFP_GPIO
#define | SYS_GPB_MFPL_PB2MFP_ACMP0_P1
#define | SYS_GPB_MFPL_PB2MFP_EADC0_CH2
#define | SYS_GPB_MFPL_PB2MFP_OPA0_O
#define | SYS_GPB_MFPL_PB2MFP_EADC1_CH10
#define | SYS_GPB_MFPL_PB2MFP_EBI_ADR3
#define | SYS_GPB_MFPL_PB2MFP_SD0_DAT0
#define | SYS_GPB_MFPL_PB2MFP_EMAC_RMII_CRSDV
#define | SYS_GPB_MFPL_PB2MFP_SPI1_SS
#define | SYS_GPB_MFPL_PB2MFP_UART1_RXD
#define | SYS_GPB_MFPL_PB2MFP_UART5_nCTS
#define | SYS_GPB_MFPL_PB2MFP_USCI1_DAT0
#define | SYS_GPB_MFPL_PB2MFP_SC0_PWR
#define | SYS_GPB_MFPL_PB2MFP_I2S0_DO
#define | SYS_GPB_MFPL_PB2MFP_EPWM0_CH3
#define | SYS_GPB_MFPL_PB2MFP_I2C1_SDA (0x0CUL<<SYS_GPB_MFPL_PB2MFP_Pos)
#define | SYS_GPB_MFPL_PB2MFP_TM3
#define | SYS_GPB_MFPL_PB2MFP_INT3
#define | SYS_GPB_MFPL_PB3MFP_GPIO
#define | SYS_GPB_MFPL_PB3MFP_ACMP0_N
#define | SYS_GPB_MFPL_PB3MFP_EADC0_CH3
#define | SYS_GPB_MFPL_PB3MFP_EADC1_CH11
#define | SYS_GPB_MFPL_PB3MFP_EBI_ADR2
#define | SYS_GPB_MFPL_PB3MFP_SD0_DAT1
#define | SYS_GPB_MFPL_PB3MFP_EMAC_RMII_RXD1
#define | SYS_GPB_MFPL_PB3MFP_SPI1_CLK
#define | SYS_GPB_MFPL_PB3MFP_UART1_TXD
#define | SYS_GPB_MFPL_PB3MFP_UART5_nRTS
#define | SYS_GPB_MFPL_PB3MFP_USCI1_DAT1
#define | SYS_GPB_MFPL_PB3MFP_SC0_RST
#define | SYS_GPB_MFPL_PB3MFP_I2S0_DI
#define | SYS_GPB_MFPL_PB3MFP_EPWM0_CH2
#define | SYS_GPB_MFPL_PB3MFP_I2C1_SCL (0x0CUL<<SYS_GPB_MFPL_PB3MFP_Pos)
#define | SYS_GPB_MFPL_PB3MFP_TM2
#define | SYS_GPB_MFPL_PB3MFP_INT2
#define | SYS_GPB_MFPL_PB4MFP_GPIO
#define | SYS_GPB_MFPL_PB4MFP_ACMP1_P1
#define | SYS_GPB_MFPL_PB4MFP_EADC0_CH4
#define | SYS_GPB_MFPL_PB4MFP_EBI_ADR1
#define | SYS_GPB_MFPL_PB4MFP_SD0_DAT2
#define | SYS_GPB_MFPL_PB4MFP_EMAC_RMII_RXD0
#define | SYS_GPB_MFPL_PB4MFP_SPI1_MOSI
#define | SYS_GPB_MFPL_PB4MFP_I2C0_SDA
#define | SYS_GPB_MFPL_PB4MFP_UART5_RXD
#define | SYS_GPB_MFPL_PB4MFP_USCI1_CTL1
#define | SYS_GPB_MFPL_PB4MFP_SC0_DAT
#define | SYS_GPB_MFPL_PB4MFP_I2S0_MCLK
#define | SYS_GPB_MFPL_PB4MFP_EPWM0_CH1
#define | SYS_GPB_MFPL_PB4MFP_UART2_RXD
#define | SYS_GPB_MFPL_PB4MFP_TM1
#define | SYS_GPB_MFPL_PB4MFP_INT1
#define | SYS_GPB_MFPL_PB5MFP_GPIO
#define | SYS_GPB_MFPL_PB5MFP_ACMP1_N
#define | SYS_GPB_MFPL_PB5MFP_EADC0_CH5
#define | SYS_GPB_MFPL_PB5MFP_EBI_ADR0
#define | SYS_GPB_MFPL_PB5MFP_SD0_DAT3
#define | SYS_GPB_MFPL_PB5MFP_EMAC_RMII_REFCLK
#define | SYS_GPB_MFPL_PB5MFP_SPI1_MISO
#define | SYS_GPB_MFPL_PB5MFP_I2C0_SCL
#define | SYS_GPB_MFPL_PB5MFP_UART5_TXD
#define | SYS_GPB_MFPL_PB5MFP_USCI1_CTL0
#define | SYS_GPB_MFPL_PB5MFP_SC0_CLK
#define | SYS_GPB_MFPL_PB5MFP_I2S0_BCLK
#define | SYS_GPB_MFPL_PB5MFP_EPWM0_CH0
#define | SYS_GPB_MFPL_PB5MFP_UART2_TXD
#define | SYS_GPB_MFPL_PB5MFP_TM0
#define | SYS_GPB_MFPL_PB5MFP_INT0
#define | SYS_GPB_MFPL_PB6MFP_GPIO
#define | SYS_GPB_MFPL_PB6MFP_EADC0_CH6
#define | SYS_GPB_MFPL_PB6MFP_EBI_nWRH
#define | SYS_GPB_MFPL_PB6MFP_EMAC_PPS
#define | SYS_GPB_MFPL_PB6MFP_USCI1_DAT1
#define | SYS_GPB_MFPL_PB6MFP_CAN1_RXD
#define | SYS_GPB_MFPL_PB6MFP_UART1_RXD
#define | SYS_GPB_MFPL_PB6MFP_SD1_CLK
#define | SYS_GPB_MFPL_PB6MFP_EBI_nCS1
#define | SYS_GPB_MFPL_PB6MFP_BPWM1_CH5
#define | SYS_GPB_MFPL_PB6MFP_EPWM1_BRAKE1
#define | SYS_GPB_MFPL_PB6MFP_EPWM1_CH5
#define | SYS_GPB_MFPL_PB6MFP_INT4
#define | SYS_GPB_MFPL_PB6MFP_USB_VBUS_EN
#define | SYS_GPB_MFPL_PB6MFP_ACMP1_O
#define | SYS_GPB_MFPL_PB7MFP_GPIO
#define | SYS_GPB_MFPL_PB7MFP_EADC0_CH7
#define | SYS_GPB_MFPL_PB7MFP_EBI_nWRL
#define | SYS_GPB_MFPL_PB7MFP_EMAC_RMII_TXEN
#define | SYS_GPB_MFPL_PB7MFP_USCI1_DAT0
#define | SYS_GPB_MFPL_PB7MFP_CAN1_TXD
#define | SYS_GPB_MFPL_PB7MFP_UART1_TXD
#define | SYS_GPB_MFPL_PB7MFP_SD1_CMD
#define | SYS_GPB_MFPL_PB7MFP_EBI_nCS0
#define | SYS_GPB_MFPL_PB7MFP_BPWM1_CH4
#define | SYS_GPB_MFPL_PB7MFP_EPWM1_BRAKE0
#define | SYS_GPB_MFPL_PB7MFP_EPWM1_CH4
#define | SYS_GPB_MFPL_PB7MFP_INT5
#define | SYS_GPB_MFPL_PB7MFP_USB_VBUS_ST
#define | SYS_GPB_MFPL_PB7MFP_ACMP0_O
#define | SYS_GPB_MFPH_PB8MFP_GPIO
#define | SYS_GPB_MFPH_PB8MFP_EADC0_CH8
#define | SYS_GPB_MFPH_PB8MFP_EBI_ADR19
#define | SYS_GPB_MFPH_PB8MFP_EMAC_RMII_TXD1
#define | SYS_GPB_MFPH_PB8MFP_USCI1_CLK
#define | SYS_GPB_MFPH_PB8MFP_UART0_RXD
#define | SYS_GPB_MFPH_PB8MFP_UART1_nRTS
#define | SYS_GPB_MFPH_PB8MFP_I2C1_SMBSUS
#define | SYS_GPB_MFPH_PB8MFP_UART7_RXD
#define | SYS_GPB_MFPH_PB8MFP_I2C0_SDA
#define | SYS_GPB_MFPH_PB8MFP_BPWM1_CH3
#define | SYS_GPB_MFPH_PB8MFP_SPI3_MOSI
#define | SYS_GPB_MFPH_PB8MFP_CAN2_RXD
#define | SYS_GPB_MFPH_PB8MFP_INT6
#define | SYS_GPB_MFPH_PB9MFP_GPIO
#define | SYS_GPB_MFPH_PB9MFP_EADC0_CH9
#define | SYS_GPB_MFPH_PB9MFP_EBI_ADR18
#define | SYS_GPB_MFPH_PB9MFP_EMAC_RMII_TXD0
#define | SYS_GPB_MFPH_PB9MFP_USCI1_CTL1
#define | SYS_GPB_MFPH_PB9MFP_UART0_TXD
#define | SYS_GPB_MFPH_PB9MFP_UART1_nCTS
#define | SYS_GPB_MFPH_PB9MFP_I2C1_SMBAL
#define | SYS_GPB_MFPH_PB9MFP_UART7_TXD
#define | SYS_GPB_MFPH_PB9MFP_I2C0_SCL
#define | SYS_GPB_MFPH_PB9MFP_BPWM1_CH2
#define | SYS_GPB_MFPH_PB9MFP_SPI3_MISO
#define | SYS_GPB_MFPH_PB9MFP_CAN2_TXD
#define | SYS_GPB_MFPH_PB9MFP_INT7
#define | SYS_GPB_MFPH_PB9MFP_CCAP_HSYNC
#define | SYS_GPB_MFPH_PB10MFP_GPIO
#define | SYS_GPB_MFPH_PB10MFP_EADC0_CH10
#define | SYS_GPB_MFPH_PB10MFP_EBI_ADR17
#define | SYS_GPB_MFPH_PB10MFP_EMAC_RMII_MDIO
#define | SYS_GPB_MFPH_PB10MFP_USCI1_CTL0
#define | SYS_GPB_MFPH_PB10MFP_UART0_nRTS
#define | SYS_GPB_MFPH_PB10MFP_UART4_RXD
#define | SYS_GPB_MFPH_PB10MFP_I2C1_SDA
#define | SYS_GPB_MFPH_PB10MFP_CAN0_RXD
#define | SYS_GPB_MFPH_PB10MFP_BPWM1_CH1
#define | SYS_GPB_MFPH_PB10MFP_SPI3_SS
#define | SYS_GPB_MFPH_PB10MFP_CCAP_VSYNC
#define | SYS_GPB_MFPH_PB10MFP_HSUSB_VBUS_EN
#define | SYS_GPB_MFPH_PB11MFP_GPIO
#define | SYS_GPB_MFPH_PB11MFP_EADC0_CH11
#define | SYS_GPB_MFPH_PB11MFP_EBI_ADR16
#define | SYS_GPB_MFPH_PB11MFP_EMAC_RMII_MDC
#define | SYS_GPB_MFPH_PB11MFP_UART0_nCTS
#define | SYS_GPB_MFPH_PB11MFP_UART4_TXD
#define | SYS_GPB_MFPH_PB11MFP_I2C1_SCL
#define | SYS_GPB_MFPH_PB11MFP_CAN0_TXD
#define | SYS_GPB_MFPH_PB11MFP_SPI0_I2SMCLK
#define | SYS_GPB_MFPH_PB11MFP_BPWM1_CH0
#define | SYS_GPB_MFPH_PB11MFP_SPI3_CLK
#define | SYS_GPB_MFPH_PB11MFP_CCAP_SFIELD
#define | SYS_GPB_MFPH_PB11MFP_HSUSB_VBUS_ST
#define | SYS_GPB_MFPH_PB12MFP_GPIO
#define | SYS_GPB_MFPH_PB12MFP_ACMP0_P2
#define | SYS_GPB_MFPH_PB12MFP_ACMP1_P2
#define | SYS_GPB_MFPH_PB12MFP_DAC0_OUT
#define | SYS_GPB_MFPH_PB12MFP_EADC0_CH12
#define | SYS_GPB_MFPH_PB12MFP_EADC1_CH12
#define | SYS_GPB_MFPH_PB12MFP_EBI_AD15
#define | SYS_GPB_MFPH_PB12MFP_SC1_CLK
#define | SYS_GPB_MFPH_PB12MFP_SPI0_MOSI
#define | SYS_GPB_MFPH_PB12MFP_USCI0_CLK
#define | SYS_GPB_MFPH_PB12MFP_UART0_RXD
#define | SYS_GPB_MFPH_PB12MFP_UART3_nCTS
#define | SYS_GPB_MFPH_PB12MFP_I2C2_SDA
#define | SYS_GPB_MFPH_PB12MFP_SD0_nCD
#define | SYS_GPB_MFPH_PB12MFP_CCAP_SCLK
#define | SYS_GPB_MFPH_PB12MFP_EPWM1_CH3
#define | SYS_GPB_MFPH_PB12MFP_ETM_TRACE_DATA3
#define | SYS_GPB_MFPH_PB12MFP_TM3_EXT
#define | SYS_GPB_MFPH_PB13MFP_GPIO
#define | SYS_GPB_MFPH_PB13MFP_ACMP0_P3
#define | SYS_GPB_MFPH_PB13MFP_ACMP1_P3
#define | SYS_GPB_MFPH_PB13MFP_DAC1_OUT
#define | SYS_GPB_MFPH_PB13MFP_EADC0_CH13
#define | SYS_GPB_MFPH_PB13MFP_EADC1_CH13
#define | SYS_GPB_MFPH_PB13MFP_EBI_AD14
#define | SYS_GPB_MFPH_PB13MFP_SC1_DAT
#define | SYS_GPB_MFPH_PB13MFP_SPI0_MISO
#define | SYS_GPB_MFPH_PB13MFP_USCI0_DAT0
#define | SYS_GPB_MFPH_PB13MFP_UART0_TXD
#define | SYS_GPB_MFPH_PB13MFP_UART3_nRTS
#define | SYS_GPB_MFPH_PB13MFP_I2C2_SCL
#define | SYS_GPB_MFPH_PB13MFP_CCAP_PIXCLK
#define | SYS_GPB_MFPH_PB13MFP_EPWM1_CH2
#define | SYS_GPB_MFPH_PB13MFP_ETM_TRACE_DATA2
#define | SYS_GPB_MFPH_PB13MFP_TM2_EXT
#define | SYS_GPB_MFPH_PB14MFP_GPIO
#define | SYS_GPB_MFPH_PB14MFP_EADC0_CH14
#define | SYS_GPB_MFPH_PB14MFP_EADC1_CH14
#define | SYS_GPB_MFPH_PB14MFP_EBI_AD13
#define | SYS_GPB_MFPH_PB14MFP_SC1_RST
#define | SYS_GPB_MFPH_PB14MFP_SPI0_CLK
#define | SYS_GPB_MFPH_PB14MFP_USCI0_DAT1
#define | SYS_GPB_MFPH_PB14MFP_UART0_nRTS
#define | SYS_GPB_MFPH_PB14MFP_UART3_RXD
#define | SYS_GPB_MFPH_PB14MFP_I2C2_SMBSUS
#define | SYS_GPB_MFPH_PB14MFP_EPWM1_CH1
#define | SYS_GPB_MFPH_PB14MFP_ETM_TRACE_DATA1
#define | SYS_GPB_MFPH_PB14MFP_TM1_EXT
#define | SYS_GPB_MFPH_PB14MFP_CLKO
#define | SYS_GPB_MFPH_PB14MFP_USB_VBUS_ST (0x0FUL<<SYS_GPB_MFPH_PB14MFP_Pos)
#define | SYS_GPB_MFPH_PB15MFP_GPIO
#define | SYS_GPB_MFPH_PB15MFP_EADC0_CH15
#define | SYS_GPB_MFPH_PB15MFP_EADC1_CH15
#define | SYS_GPB_MFPH_PB15MFP_EBI_AD12
#define | SYS_GPB_MFPH_PB15MFP_SC1_PWR
#define | SYS_GPB_MFPH_PB15MFP_SPI0_SS
#define | SYS_GPB_MFPH_PB15MFP_USCI0_CTL1
#define | SYS_GPB_MFPH_PB15MFP_UART0_nCTS
#define | SYS_GPB_MFPH_PB15MFP_UART3_TXD
#define | SYS_GPB_MFPH_PB15MFP_I2C2_SMBAL
#define | SYS_GPB_MFPH_PB15MFP_EPWM0_BRAKE1
#define | SYS_GPB_MFPH_PB15MFP_EPWM1_CH0
#define | SYS_GPB_MFPH_PB15MFP_ETM_TRACE_DATA0
#define | SYS_GPB_MFPH_PB15MFP_TM0_EXT
#define | SYS_GPB_MFPH_PB15MFP_USB_VBUS_EN
#define | SYS_GPB_MFPH_PB15MFP_HSUSB_VBUS_EN
#define | SYS_GPC_MFPL_PC0MFP_GPIO
#define | SYS_GPC_MFPL_PC0MFP_EBI_AD0
#define | SYS_GPC_MFPL_PC0MFP_SPIM_MOSI
#define | SYS_GPC_MFPL_PC0MFP_QSPI0_MOSI0
#define | SYS_GPC_MFPL_PC0MFP_SC1_CLK
#define | SYS_GPC_MFPL_PC0MFP_I2S0_LRCK
#define | SYS_GPC_MFPL_PC0MFP_SPI1_SS
#define | SYS_GPC_MFPL_PC0MFP_UART2_RXD
#define | SYS_GPC_MFPL_PC0MFP_I2C0_SDA
#define | SYS_GPC_MFPL_PC0MFP_CAN2_RXD
#define | SYS_GPC_MFPL_PC0MFP_EPWM1_CH5
#define | SYS_GPC_MFPL_PC0MFP_CCAP_DATA0
#define | SYS_GPC_MFPL_PC0MFP_ACMP1_O
#define | SYS_GPC_MFPL_PC0MFP_EADC1_ST
#define | SYS_GPC_MFPL_PC1MFP_GPIO
#define | SYS_GPC_MFPL_PC1MFP_EBI_AD1
#define | SYS_GPC_MFPL_PC1MFP_SPIM_MISO
#define | SYS_GPC_MFPL_PC1MFP_QSPI0_MISO0
#define | SYS_GPC_MFPL_PC1MFP_SC1_DAT
#define | SYS_GPC_MFPL_PC1MFP_I2S0_DO
#define | SYS_GPC_MFPL_PC1MFP_SPI1_CLK
#define | SYS_GPC_MFPL_PC1MFP_UART2_TXD
#define | SYS_GPC_MFPL_PC1MFP_I2C0_SCL
#define | SYS_GPC_MFPL_PC1MFP_CAN2_TXD
#define | SYS_GPC_MFPL_PC1MFP_EPWM1_CH4
#define | SYS_GPC_MFPL_PC1MFP_CCAP_DATA1
#define | SYS_GPC_MFPL_PC1MFP_ACMP0_O
#define | SYS_GPC_MFPL_PC1MFP_EADC0_ST
#define | SYS_GPC_MFPL_PC2MFP_GPIO
#define | SYS_GPC_MFPL_PC2MFP_EBI_AD2
#define | SYS_GPC_MFPL_PC2MFP_SPIM_CLK
#define | SYS_GPC_MFPL_PC2MFP_QSPI0_CLK
#define | SYS_GPC_MFPL_PC2MFP_SC1_RST
#define | SYS_GPC_MFPL_PC2MFP_I2S0_DI
#define | SYS_GPC_MFPL_PC2MFP_SPI1_MOSI
#define | SYS_GPC_MFPL_PC2MFP_UART2_nCTS
#define | SYS_GPC_MFPL_PC2MFP_I2C0_SMBSUS
#define | SYS_GPC_MFPL_PC2MFP_CAN1_RXD
#define | SYS_GPC_MFPL_PC2MFP_UART3_RXD
#define | SYS_GPC_MFPL_PC2MFP_EPWM1_CH3
#define | SYS_GPC_MFPL_PC2MFP_CCAP_DATA2
#define | SYS_GPC_MFPL_PC2MFP_QSPI1_MOSI0
#define | SYS_GPC_MFPL_PC3MFP_GPIO
#define | SYS_GPC_MFPL_PC3MFP_EBI_AD3
#define | SYS_GPC_MFPL_PC3MFP_SPIM_SS
#define | SYS_GPC_MFPL_PC3MFP_QSPI0_SS
#define | SYS_GPC_MFPL_PC3MFP_SC1_PWR
#define | SYS_GPC_MFPL_PC3MFP_I2S0_MCLK
#define | SYS_GPC_MFPL_PC3MFP_SPI1_MISO
#define | SYS_GPC_MFPL_PC3MFP_UART2_nRTS
#define | SYS_GPC_MFPL_PC3MFP_I2C0_SMBAL
#define | SYS_GPC_MFPL_PC3MFP_CAN1_TXD
#define | SYS_GPC_MFPL_PC3MFP_UART3_TXD
#define | SYS_GPC_MFPL_PC3MFP_EPWM1_CH2
#define | SYS_GPC_MFPL_PC3MFP_CCAP_DATA3
#define | SYS_GPC_MFPL_PC3MFP_QSPI1_MISO0
#define | SYS_GPC_MFPL_PC4MFP_GPIO
#define | SYS_GPC_MFPL_PC4MFP_EBI_AD4
#define | SYS_GPC_MFPL_PC4MFP_SPIM_D3
#define | SYS_GPC_MFPL_PC4MFP_QSPI0_MOSI1
#define | SYS_GPC_MFPL_PC4MFP_SC1_nCD
#define | SYS_GPC_MFPL_PC4MFP_I2S0_BCLK
#define | SYS_GPC_MFPL_PC4MFP_SPI1_I2SMCLK
#define | SYS_GPC_MFPL_PC4MFP_UART2_RXD
#define | SYS_GPC_MFPL_PC4MFP_I2C1_SDA
#define | SYS_GPC_MFPL_PC4MFP_CAN0_RXD
#define | SYS_GPC_MFPL_PC4MFP_UART4_RXD
#define | SYS_GPC_MFPL_PC4MFP_EPWM1_CH1
#define | SYS_GPC_MFPL_PC4MFP_CCAP_DATA4
#define | SYS_GPC_MFPL_PC4MFP_QSPI1_CLK
#define | SYS_GPC_MFPL_PC5MFP_GPIO
#define | SYS_GPC_MFPL_PC5MFP_EBI_AD5
#define | SYS_GPC_MFPL_PC5MFP_SPIM_D2
#define | SYS_GPC_MFPL_PC5MFP_QSPI0_MISO1
#define | SYS_GPC_MFPL_PC5MFP_UART2_TXD
#define | SYS_GPC_MFPL_PC5MFP_I2C1_SCL
#define | SYS_GPC_MFPL_PC5MFP_CAN0_TXD
#define | SYS_GPC_MFPL_PC5MFP_UART4_TXD
#define | SYS_GPC_MFPL_PC5MFP_EPWM1_CH0
#define | SYS_GPC_MFPL_PC5MFP_CCAP_DATA5
#define | SYS_GPC_MFPL_PC5MFP_QSPI1_SS
#define | SYS_GPC_MFPL_PC6MFP_GPIO
#define | SYS_GPC_MFPL_PC6MFP_EBI_AD8
#define | SYS_GPC_MFPL_PC6MFP_EMAC_RMII_RXD1
#define | SYS_GPC_MFPL_PC6MFP_SPI1_MOSI
#define | SYS_GPC_MFPL_PC6MFP_UART4_RXD
#define | SYS_GPC_MFPL_PC6MFP_SC2_RST
#define | SYS_GPC_MFPL_PC6MFP_UART0_nRTS
#define | SYS_GPC_MFPL_PC6MFP_I2C1_SMBSUS
#define | SYS_GPC_MFPL_PC6MFP_UART6_RXD
#define | SYS_GPC_MFPL_PC6MFP_EPWM1_CH3
#define | SYS_GPC_MFPL_PC6MFP_BPWM1_CH1
#define | SYS_GPC_MFPL_PC6MFP_TM1
#define | SYS_GPC_MFPL_PC6MFP_INT2
#define | SYS_GPC_MFPL_PC7MFP_GPIO
#define | SYS_GPC_MFPL_PC7MFP_EBI_AD9
#define | SYS_GPC_MFPL_PC7MFP_EMAC_RMII_RXD0
#define | SYS_GPC_MFPL_PC7MFP_SPI1_MISO
#define | SYS_GPC_MFPL_PC7MFP_UART4_TXD
#define | SYS_GPC_MFPL_PC7MFP_SC2_PWR
#define | SYS_GPC_MFPL_PC7MFP_UART0_nCTS
#define | SYS_GPC_MFPL_PC7MFP_I2C1_SMBAL
#define | SYS_GPC_MFPL_PC7MFP_UART6_TXD
#define | SYS_GPC_MFPL_PC7MFP_EPWM1_CH2
#define | SYS_GPC_MFPL_PC7MFP_BPWM1_CH0
#define | SYS_GPC_MFPL_PC7MFP_TM0
#define | SYS_GPC_MFPL_PC7MFP_INT3
#define | SYS_GPC_MFPH_PC8MFP_GPIO
#define | SYS_GPC_MFPH_PC8MFP_EBI_ADR16
#define | SYS_GPC_MFPH_PC8MFP_EMAC_RMII_REFCLK
#define | SYS_GPC_MFPH_PC8MFP_I2C0_SDA
#define | SYS_GPC_MFPH_PC8MFP_UART4_nCTS
#define | SYS_GPC_MFPH_PC8MFP_UART1_RXD
#define | SYS_GPC_MFPH_PC8MFP_EPWM1_CH1
#define | SYS_GPC_MFPH_PC8MFP_BPWM1_CH4
#define | SYS_GPC_MFPH_PC9MFP_GPIO
#define | SYS_GPC_MFPH_PC9MFP_EBI_ADR7
#define | SYS_GPC_MFPH_PC9MFP_UART6_nCTS
#define | SYS_GPC_MFPH_PC9MFP_SPI3_SS
#define | SYS_GPC_MFPH_PC9MFP_UART3_RXD
#define | SYS_GPC_MFPH_PC9MFP_CAN1_RXD
#define | SYS_GPC_MFPH_PC9MFP_EPWM1_CH3
#define | SYS_GPC_MFPH_PC9MFP_EADC1_ST
#define | SYS_GPC_MFPH_PC10MFP_GPIO
#define | SYS_GPC_MFPH_PC10MFP_EBI_ADR6
#define | SYS_GPC_MFPH_PC10MFP_UART6_nRTS
#define | SYS_GPC_MFPH_PC10MFP_SPI3_CLK
#define | SYS_GPC_MFPH_PC10MFP_UART3_TXD
#define | SYS_GPC_MFPH_PC10MFP_CAN1_TXD
#define | SYS_GPC_MFPH_PC10MFP_ECAP1_IC0
#define | SYS_GPC_MFPH_PC10MFP_EPWM1_CH2
#define | SYS_GPC_MFPH_PC10MFP_EADC1_ST
#define | SYS_GPC_MFPH_PC11MFP_GPIO
#define | SYS_GPC_MFPH_PC11MFP_EBI_ADR5
#define | SYS_GPC_MFPH_PC11MFP_UART0_RXD
#define | SYS_GPC_MFPH_PC11MFP_I2C0_SDA
#define | SYS_GPC_MFPH_PC11MFP_UART6_RXD
#define | SYS_GPC_MFPH_PC11MFP_SPI3_MOSI
#define | SYS_GPC_MFPH_PC11MFP_ECAP1_IC1
#define | SYS_GPC_MFPH_PC11MFP_EPWM1_CH1
#define | SYS_GPC_MFPH_PC11MFP_ACMP1_O
#define | SYS_GPC_MFPH_PC12MFP_GPIO
#define | SYS_GPC_MFPH_PC12MFP_EBI_ADR4
#define | SYS_GPC_MFPH_PC12MFP_UART0_TXD
#define | SYS_GPC_MFPH_PC12MFP_I2C0_SCL
#define | SYS_GPC_MFPH_PC12MFP_UART6_TXD
#define | SYS_GPC_MFPH_PC12MFP_SPI3_MISO
#define | SYS_GPC_MFPH_PC12MFP_SC0_nCD
#define | SYS_GPC_MFPH_PC12MFP_ECAP1_IC2
#define | SYS_GPC_MFPH_PC12MFP_EPWM1_CH0
#define | SYS_GPC_MFPH_PC12MFP_ACMP0_O
#define | SYS_GPC_MFPH_PC13MFP_GPIO
#define | SYS_GPC_MFPH_PC13MFP_EADC1_CH3
#define | SYS_GPC_MFPH_PC13MFP_EBI_ADR10
#define | SYS_GPC_MFPH_PC13MFP_SC2_nCD
#define | SYS_GPC_MFPH_PC13MFP_SPI2_I2SMCLK
#define | SYS_GPC_MFPH_PC13MFP_CAN1_TXD
#define | SYS_GPC_MFPH_PC13MFP_USCI0_CTL0
#define | SYS_GPC_MFPH_PC13MFP_UART2_TXD
#define | SYS_GPC_MFPH_PC13MFP_BPWM0_CH4
#define | SYS_GPC_MFPH_PC13MFP_CLKO
#define | SYS_GPC_MFPH_PC13MFP_EADC0_ST
#define | SYS_GPC_MFPH_PC14MFP_GPIO
#define | SYS_GPC_MFPH_PC14MFP_EBI_AD11
#define | SYS_GPC_MFPH_PC14MFP_SC1_nCD
#define | SYS_GPC_MFPH_PC14MFP_SPI0_I2SMCLK
#define | SYS_GPC_MFPH_PC14MFP_USCI0_CTL0
#define | SYS_GPC_MFPH_PC14MFP_QSPI0_CLK
#define | SYS_GPC_MFPH_PC14MFP_EPWM0_SYNC_IN
#define | SYS_GPC_MFPH_PC14MFP_ETM_TRACE_CLK
#define | SYS_GPC_MFPH_PC14MFP_TM1
#define | SYS_GPC_MFPH_PC14MFP_USB_VBUS_ST
#define | SYS_GPC_MFPH_PC14MFP_HSUSB_VBUS_ST
#define | SYS_GPD_MFPL_PD0MFP_GPIO
#define | SYS_GPD_MFPL_PD0MFP_EBI_AD13
#define | SYS_GPD_MFPL_PD0MFP_USCI0_CLK
#define | SYS_GPD_MFPL_PD0MFP_SPI0_MOSI
#define | SYS_GPD_MFPL_PD0MFP_UART3_RXD
#define | SYS_GPD_MFPL_PD0MFP_I2C2_SDA
#define | SYS_GPD_MFPL_PD0MFP_SC2_CLK
#define | SYS_GPD_MFPL_PD0MFP_TM2
#define | SYS_GPD_MFPL_PD1MFP_GPIO
#define | SYS_GPD_MFPL_PD1MFP_EBI_AD12
#define | SYS_GPD_MFPL_PD1MFP_USCI0_DAT0
#define | SYS_GPD_MFPL_PD1MFP_SPI0_MISO
#define | SYS_GPD_MFPL_PD1MFP_UART3_TXD
#define | SYS_GPD_MFPL_PD1MFP_I2C2_SCL
#define | SYS_GPD_MFPL_PD1MFP_SC2_DAT
#define | SYS_GPD_MFPL_PD2MFP_GPIO
#define | SYS_GPD_MFPL_PD2MFP_EBI_AD11
#define | SYS_GPD_MFPL_PD2MFP_USCI0_DAT1
#define | SYS_GPD_MFPL_PD2MFP_SPI0_CLK
#define | SYS_GPD_MFPL_PD2MFP_UART3_nCTS
#define | SYS_GPD_MFPL_PD2MFP_SC2_RST
#define | SYS_GPD_MFPL_PD2MFP_UART0_RXD
#define | SYS_GPD_MFPL_PD3MFP_GPIO
#define | SYS_GPD_MFPL_PD3MFP_EBI_AD10
#define | SYS_GPD_MFPL_PD3MFP_USCI0_CTL1
#define | SYS_GPD_MFPL_PD3MFP_SPI0_SS
#define | SYS_GPD_MFPL_PD3MFP_UART3_nRTS
#define | SYS_GPD_MFPL_PD3MFP_USCI1_CTL0
#define | SYS_GPD_MFPL_PD3MFP_SC2_PWR
#define | SYS_GPD_MFPL_PD3MFP_SC1_nCD
#define | SYS_GPD_MFPL_PD3MFP_UART0_TXD
#define | SYS_GPD_MFPL_PD4MFP_GPIO
#define | SYS_GPD_MFPL_PD4MFP_USCI0_CTL0
#define | SYS_GPD_MFPL_PD4MFP_I2C1_SDA
#define | SYS_GPD_MFPL_PD4MFP_SPI1_SS
#define | SYS_GPD_MFPL_PD4MFP_USCI1_CTL1
#define | SYS_GPD_MFPL_PD4MFP_SC1_CLK
#define | SYS_GPD_MFPL_PD4MFP_USB_VBUS_ST
#define | SYS_GPD_MFPL_PD5MFP_GPIO
#define | SYS_GPD_MFPL_PD5MFP_I2C1_SCL
#define | SYS_GPD_MFPL_PD5MFP_SPI1_CLK
#define | SYS_GPD_MFPL_PD5MFP_USCI1_DAT0
#define | SYS_GPD_MFPL_PD5MFP_SC1_DAT
#define | SYS_GPD_MFPL_PD6MFP_GPIO
#define | SYS_GPD_MFPL_PD6MFP_UART1_RXD
#define | SYS_GPD_MFPL_PD6MFP_I2C0_SDA
#define | SYS_GPD_MFPL_PD6MFP_SPI1_MOSI
#define | SYS_GPD_MFPL_PD6MFP_USCI1_DAT1
#define | SYS_GPD_MFPL_PD6MFP_SC1_RST
#define | SYS_GPD_MFPL_PD7MFP_GPIO
#define | SYS_GPD_MFPL_PD7MFP_UART1_TXD
#define | SYS_GPD_MFPL_PD7MFP_I2C0_SCL
#define | SYS_GPD_MFPL_PD7MFP_SPI1_MISO
#define | SYS_GPD_MFPL_PD7MFP_USCI1_CLK
#define | SYS_GPD_MFPL_PD7MFP_SC1_PWR
#define | SYS_GPD_MFPH_PD8MFP_GPIO
#define | SYS_GPD_MFPH_PD8MFP_EBI_AD6
#define | SYS_GPD_MFPH_PD8MFP_I2C2_SDA
#define | SYS_GPD_MFPH_PD8MFP_UART2_nRTS
#define | SYS_GPD_MFPH_PD8MFP_UART7_RXD
#define | SYS_GPD_MFPH_PD8MFP_CAN2_RXD
#define | SYS_GPD_MFPH_PD9MFP_GPIO
#define | SYS_GPD_MFPH_PD9MFP_EBI_AD7
#define | SYS_GPD_MFPH_PD9MFP_I2C2_SCL
#define | SYS_GPD_MFPH_PD9MFP_UART2_nCTS
#define | SYS_GPD_MFPH_PD9MFP_UART7_TXD
#define | SYS_GPD_MFPH_PD9MFP_CAN2_TXD
#define | SYS_GPD_MFPH_PD10MFP_GPIO
#define | SYS_GPD_MFPH_PD10MFP_OPA2_P
#define | SYS_GPD_MFPH_PD10MFP_EADC1_CH0
#define | SYS_GPD_MFPH_PD10MFP_EBI_nCS2
#define | SYS_GPD_MFPH_PD10MFP_UART1_RXD
#define | SYS_GPD_MFPH_PD10MFP_CAN0_RXD
#define | SYS_GPD_MFPH_PD10MFP_QEI0_B
#define | SYS_GPD_MFPH_PD10MFP_INT7
#define | SYS_GPD_MFPH_PD11MFP_GPIO
#define | SYS_GPD_MFPH_PD11MFP_EADC1_CH1
#define | SYS_GPD_MFPH_PD11MFP_OPA2_N
#define | SYS_GPD_MFPH_PD11MFP_EBI_nCS1
#define | SYS_GPD_MFPH_PD11MFP_UART1_TXD
#define | SYS_GPD_MFPH_PD11MFP_CAN0_TXD
#define | SYS_GPD_MFPH_PD11MFP_QEI0_A
#define | SYS_GPD_MFPH_PD11MFP_INT6
#define | SYS_GPD_MFPH_PD12MFP_GPIO
#define | SYS_GPD_MFPH_PD12MFP_OPA2_O
#define | SYS_GPD_MFPH_PD12MFP_EADC1_CH2
#define | SYS_GPD_MFPH_PD12MFP_EBI_nCS0
#define | SYS_GPD_MFPH_PD12MFP_CAN1_RXD
#define | SYS_GPD_MFPH_PD12MFP_UART2_RXD
#define | SYS_GPD_MFPH_PD12MFP_BPWM0_CH5
#define | SYS_GPD_MFPH_PD12MFP_QEI0_INDEX
#define | SYS_GPD_MFPH_PD12MFP_CLKO
#define | SYS_GPD_MFPH_PD12MFP_EADC0_ST
#define | SYS_GPD_MFPH_PD12MFP_INT5
#define | SYS_GPD_MFPH_PD13MFP_GPIO
#define | SYS_GPD_MFPH_PD13MFP_EBI_AD10
#define | SYS_GPD_MFPH_PD13MFP_SD0_nCD
#define | SYS_GPD_MFPH_PD13MFP_SPI0_I2SMCLK
#define | SYS_GPD_MFPH_PD13MFP_SPI1_I2SMCLK
#define | SYS_GPD_MFPH_PD13MFP_SC2_nCD
#define | SYS_GPD_MFPH_PD14MFP_GPIO
#define | SYS_GPD_MFPH_PD14MFP_EBI_nCS0
#define | SYS_GPD_MFPH_PD14MFP_SPI3_I2SMCLK
#define | SYS_GPD_MFPH_PD14MFP_SC1_nCD
#define | SYS_GPD_MFPH_PD14MFP_SPI0_I2SMCLK
#define | SYS_GPD_MFPH_PD14MFP_EPWM0_CH4
#define | SYS_GPE_MFPL_PE0MFP_GPIO
#define | SYS_GPE_MFPL_PE0MFP_EBI_AD11
#define | SYS_GPE_MFPL_PE0MFP_QSPI0_MOSI0
#define | SYS_GPE_MFPL_PE0MFP_SC2_CLK
#define | SYS_GPE_MFPL_PE0MFP_I2S0_MCLK
#define | SYS_GPE_MFPL_PE0MFP_SPI1_MOSI
#define | SYS_GPE_MFPL_PE0MFP_UART3_RXD
#define | SYS_GPE_MFPL_PE0MFP_I2C1_SDA
#define | SYS_GPE_MFPL_PE0MFP_UART4_nRTS
#define | SYS_GPE_MFPL_PE1MFP_GPIO
#define | SYS_GPE_MFPL_PE1MFP_EBI_AD10
#define | SYS_GPE_MFPL_PE1MFP_QSPI0_MISO0
#define | SYS_GPE_MFPL_PE1MFP_SC2_DAT
#define | SYS_GPE_MFPL_PE1MFP_I2S0_BCLK
#define | SYS_GPE_MFPL_PE1MFP_SPI1_MISO
#define | SYS_GPE_MFPL_PE1MFP_UART3_TXD
#define | SYS_GPE_MFPL_PE1MFP_I2C1_SCL
#define | SYS_GPE_MFPL_PE1MFP_UART4_nCTS
#define | SYS_GPE_MFPL_PE2MFP_GPIO
#define | SYS_GPE_MFPL_PE2MFP_EBI_ALE
#define | SYS_GPE_MFPL_PE2MFP_SD0_DAT0
#define | SYS_GPE_MFPL_PE2MFP_SPIM_MOSI
#define | SYS_GPE_MFPL_PE2MFP_SPI3_MOSI
#define | SYS_GPE_MFPL_PE2MFP_SC0_CLK
#define | SYS_GPE_MFPL_PE2MFP_USCI0_CLK
#define | SYS_GPE_MFPL_PE2MFP_UART6_nCTS
#define | SYS_GPE_MFPL_PE2MFP_UART7_RXD
#define | SYS_GPE_MFPL_PE2MFP_QEI0_B
#define | SYS_GPE_MFPL_PE2MFP_EPWM0_CH5
#define | SYS_GPE_MFPL_PE2MFP_BPWM0_CH0
#define | SYS_GPE_MFPL_PE3MFP_GPIO
#define | SYS_GPE_MFPL_PE3MFP_EBI_MCLK
#define | SYS_GPE_MFPL_PE3MFP_SD0_DAT1
#define | SYS_GPE_MFPL_PE3MFP_SPIM_MISO
#define | SYS_GPE_MFPL_PE3MFP_SPI3_MISO
#define | SYS_GPE_MFPL_PE3MFP_SC0_DAT
#define | SYS_GPE_MFPL_PE3MFP_USCI0_DAT0
#define | SYS_GPE_MFPL_PE3MFP_UART6_nRTS
#define | SYS_GPE_MFPL_PE3MFP_UART7_TXD
#define | SYS_GPE_MFPL_PE3MFP_QEI0_A
#define | SYS_GPE_MFPL_PE3MFP_EPWM0_CH4
#define | SYS_GPE_MFPL_PE3MFP_BPWM0_CH1
#define | SYS_GPE_MFPL_PE4MFP_GPIO
#define | SYS_GPE_MFPL_PE4MFP_EBI_nWR
#define | SYS_GPE_MFPL_PE4MFP_SD0_DAT2
#define | SYS_GPE_MFPL_PE4MFP_SPIM_CLK
#define | SYS_GPE_MFPL_PE4MFP_SPI3_CLK
#define | SYS_GPE_MFPL_PE4MFP_SC0_RST
#define | SYS_GPE_MFPL_PE4MFP_USCI0_DAT1
#define | SYS_GPE_MFPL_PE4MFP_UART6_RXD
#define | SYS_GPE_MFPL_PE4MFP_UART7_nCTS
#define | SYS_GPE_MFPL_PE4MFP_QEI0_INDEX
#define | SYS_GPE_MFPL_PE4MFP_EPWM0_CH3
#define | SYS_GPE_MFPL_PE4MFP_BPWM0_CH2
#define | SYS_GPE_MFPL_PE5MFP_GPIO
#define | SYS_GPE_MFPL_PE5MFP_EBI_nRD
#define | SYS_GPE_MFPL_PE5MFP_SD0_DAT3
#define | SYS_GPE_MFPL_PE5MFP_SPIM_SS
#define | SYS_GPE_MFPL_PE5MFP_SPI3_SS
#define | SYS_GPE_MFPL_PE5MFP_SC0_PWR
#define | SYS_GPE_MFPL_PE5MFP_USCI0_CTL1
#define | SYS_GPE_MFPL_PE5MFP_UART6_TXD
#define | SYS_GPE_MFPL_PE5MFP_UART7_nRTS
#define | SYS_GPE_MFPL_PE5MFP_QEI1_B
#define | SYS_GPE_MFPL_PE5MFP_EPWM0_CH2
#define | SYS_GPE_MFPL_PE5MFP_BPWM0_CH3
#define | SYS_GPE_MFPL_PE6MFP_GPIO
#define | SYS_GPE_MFPL_PE6MFP_SD0_CLK
#define | SYS_GPE_MFPL_PE6MFP_SPIM_D3
#define | SYS_GPE_MFPL_PE6MFP_SPI3_I2SMCLK
#define | SYS_GPE_MFPL_PE6MFP_SC0_nCD
#define | SYS_GPE_MFPL_PE6MFP_USCI0_CTL0
#define | SYS_GPE_MFPL_PE6MFP_UART5_RXD
#define | SYS_GPE_MFPL_PE6MFP_CAN1_RXD
#define | SYS_GPE_MFPL_PE6MFP_QEI1_A
#define | SYS_GPE_MFPL_PE6MFP_EPWM0_CH1
#define | SYS_GPE_MFPL_PE6MFP_BPWM0_CH4
#define | SYS_GPE_MFPL_PE7MFP_GPIO
#define | SYS_GPE_MFPL_PE7MFP_SD0_CMD
#define | SYS_GPE_MFPL_PE7MFP_SPIM_D2
#define | SYS_GPE_MFPL_PE7MFP_UART5_TXD
#define | SYS_GPE_MFPL_PE7MFP_CAN1_TXD
#define | SYS_GPE_MFPL_PE7MFP_QEI1_INDEX
#define | SYS_GPE_MFPL_PE7MFP_EPWM0_CH0
#define | SYS_GPE_MFPL_PE7MFP_BPWM0_CH5
#define | SYS_GPE_MFPH_PE8MFP_GPIO
#define | SYS_GPE_MFPH_PE8MFP_EBI_ADR10
#define | SYS_GPE_MFPH_PE8MFP_EMAC_RMII_MDC
#define | SYS_GPE_MFPH_PE8MFP_I2S0_BCLK
#define | SYS_GPE_MFPH_PE8MFP_SPI2_CLK
#define | SYS_GPE_MFPH_PE8MFP_USCI1_CTL1
#define | SYS_GPE_MFPH_PE8MFP_UART2_TXD
#define | SYS_GPE_MFPH_PE8MFP_EPWM0_CH0
#define | SYS_GPE_MFPH_PE8MFP_EPWM0_BRAKE0
#define | SYS_GPE_MFPH_PE8MFP_ECAP0_IC0
#define | SYS_GPE_MFPH_PE8MFP_TRACE_DATA3
#define | SYS_GPE_MFPH_PE9MFP_GPIO
#define | SYS_GPE_MFPH_PE9MFP_EBI_ADR11
#define | SYS_GPE_MFPH_PE9MFP_EMAC_RMII_MDIO
#define | SYS_GPE_MFPH_PE9MFP_I2S0_MCLK
#define | SYS_GPE_MFPH_PE9MFP_SPI2_MISO
#define | SYS_GPE_MFPH_PE9MFP_USCI1_CTL0
#define | SYS_GPE_MFPH_PE9MFP_UART2_RXD
#define | SYS_GPE_MFPH_PE9MFP_EPWM0_CH1
#define | SYS_GPE_MFPH_PE9MFP_EPWM0_BRAKE1
#define | SYS_GPE_MFPH_PE9MFP_ECAP0_IC1
#define | SYS_GPE_MFPH_PE9MFP_TRACE_DATA2
#define | SYS_GPE_MFPH_PE10MFP_GPIO
#define | SYS_GPE_MFPH_PE10MFP_EBI_ADR12
#define | SYS_GPE_MFPH_PE10MFP_EMAC_RMII_TXD0
#define | SYS_GPE_MFPH_PE10MFP_I2S0_DI
#define | SYS_GPE_MFPH_PE10MFP_SPI2_MOSI
#define | SYS_GPE_MFPH_PE10MFP_USCI1_DAT0
#define | SYS_GPE_MFPH_PE10MFP_UART3_TXD
#define | SYS_GPE_MFPH_PE10MFP_EPWM0_CH2
#define | SYS_GPE_MFPH_PE10MFP_EPWM1_BRAKE0
#define | SYS_GPE_MFPH_PE10MFP_ECAP0_IC2
#define | SYS_GPE_MFPH_PE10MFP_TRACE_DATA1
#define | SYS_GPE_MFPH_PE11MFP_GPIO
#define | SYS_GPE_MFPH_PE11MFP_EBI_ADR13
#define | SYS_GPE_MFPH_PE11MFP_EMAC_RMII_TXD1
#define | SYS_GPE_MFPH_PE11MFP_I2S0_DO
#define | SYS_GPE_MFPH_PE11MFP_SPI2_SS
#define | SYS_GPE_MFPH_PE11MFP_USCI1_DAT1
#define | SYS_GPE_MFPH_PE11MFP_UART3_RXD
#define | SYS_GPE_MFPH_PE11MFP_UART1_nCTS
#define | SYS_GPE_MFPH_PE11MFP_EPWM0_CH3
#define | SYS_GPE_MFPH_PE11MFP_EPWM1_BRAKE1
#define | SYS_GPE_MFPH_PE11MFP_ECAP1_IC2
#define | SYS_GPE_MFPH_PE11MFP_TRACE_DATA0
#define | SYS_GPE_MFPH_PE12MFP_GPIO
#define | SYS_GPE_MFPH_PE12MFP_EBI_ADR14
#define | SYS_GPE_MFPH_PE12MFP_EMAC_RMII_TXEN
#define | SYS_GPE_MFPH_PE12MFP_I2S0_LRCK
#define | SYS_GPE_MFPH_PE12MFP_SPI2_I2SMCLK
#define | SYS_GPE_MFPH_PE12MFP_USCI1_CLK
#define | SYS_GPE_MFPH_PE12MFP_UART1_nRTS
#define | SYS_GPE_MFPH_PE12MFP_EPWM0_CH4
#define | SYS_GPE_MFPH_PE12MFP_ECAP1_IC1
#define | SYS_GPE_MFPH_PE12MFP_TRACE_CLK
#define | SYS_GPE_MFPH_PE13MFP_GPIO
#define | SYS_GPE_MFPH_PE13MFP_EBI_ADR15
#define | SYS_GPE_MFPH_PE13MFP_EMAC_PPS
#define | SYS_GPE_MFPH_PE13MFP_I2C0_SCL
#define | SYS_GPE_MFPH_PE13MFP_UART4_nRTS
#define | SYS_GPE_MFPH_PE13MFP_UART1_TXD
#define | SYS_GPE_MFPH_PE13MFP_EPWM0_CH5
#define | SYS_GPE_MFPH_PE13MFP_EPWM1_CH0
#define | SYS_GPE_MFPH_PE13MFP_BPWM1_CH5
#define | SYS_GPE_MFPH_PE13MFP_ECAP1_IC0
#define | SYS_GPE_MFPH_PE14MFP_GPIO
#define | SYS_GPE_MFPH_PE14MFP_EBI_AD8
#define | SYS_GPE_MFPH_PE14MFP_UART2_TXD
#define | SYS_GPE_MFPH_PE14MFP_CAN0_TXD
#define | SYS_GPE_MFPH_PE14MFP_SD1_nCD
#define | SYS_GPE_MFPH_PE14MFP_UART6_TXD (0x06UL<<SYS_GPE_MFPH_PE14MFP_Pos)
#define | SYS_GPE_MFPH_PE15MFP_GPIO
#define | SYS_GPE_MFPH_PE15MFP_EBI_AD9
#define | SYS_GPE_MFPH_PE15MFP_UART2_RXD
#define | SYS_GPE_MFPH_PE15MFP_CAN0_RXD
#define | SYS_GPE_MFPH_PE15MFP_UART6_RXD
#define | SYS_GPF_MFPL_PF0MFP_GPIO
#define | SYS_GPF_MFPL_PF0MFP_UART1_TXD
#define | SYS_GPF_MFPL_PF0MFP_I2C1_SCL
#define | SYS_GPF_MFPL_PF0MFP_UART0_TXD
#define | SYS_GPF_MFPL_PF0MFP_BPWM1_CH0
#define | SYS_GPF_MFPL_PF0MFP_ICE_DAT
#define | SYS_GPF_MFPL_PF1MFP_GPIO
#define | SYS_GPF_MFPL_PF1MFP_UART1_RXD
#define | SYS_GPF_MFPL_PF1MFP_I2C1_SDA
#define | SYS_GPF_MFPL_PF1MFP_UART0_RXD
#define | SYS_GPF_MFPL_PF1MFP_BPWM1_CH1
#define | SYS_GPF_MFPL_PF1MFP_ICE_CLK
#define | SYS_GPF_MFPL_PF2MFP_GPIO
#define | SYS_GPF_MFPL_PF2MFP_EBI_nCS1
#define | SYS_GPF_MFPL_PF2MFP_UART0_RXD
#define | SYS_GPF_MFPL_PF2MFP_I2C0_SDA
#define | SYS_GPF_MFPL_PF2MFP_QSPI0_CLK
#define | SYS_GPF_MFPL_PF2MFP_XT1_OUT
#define | SYS_GPF_MFPL_PF2MFP_BPWM1_CH1
#define | SYS_GPF_MFPL_PF3MFP_GPIO
#define | SYS_GPF_MFPL_PF3MFP_EBI_nCS0
#define | SYS_GPF_MFPL_PF3MFP_UART0_TXD
#define | SYS_GPF_MFPL_PF3MFP_I2C0_SCL
#define | SYS_GPF_MFPL_PF3MFP_XT1_IN
#define | SYS_GPF_MFPL_PF3MFP_BPWM1_CH0
#define | SYS_GPF_MFPL_PF4MFP_GPIO
#define | SYS_GPF_MFPL_PF4MFP_UART2_TXD
#define | SYS_GPF_MFPL_PF4MFP_UART2_nRTS
#define | SYS_GPF_MFPL_PF4MFP_EPWM0_CH1
#define | SYS_GPF_MFPL_PF4MFP_BPWM0_CH5
#define | SYS_GPF_MFPL_PF4MFP_X32_OUT
#define | SYS_GPF_MFPL_PF4MFP_EADC1_ST
#define | SYS_GPF_MFPL_PF5MFP_GPIO
#define | SYS_GPF_MFPL_PF5MFP_UART2_RXD
#define | SYS_GPF_MFPL_PF5MFP_UART2_nCTS
#define | SYS_GPF_MFPL_PF5MFP_EPWM0_CH0
#define | SYS_GPF_MFPL_PF5MFP_BPWM0_CH4
#define | SYS_GPF_MFPL_PF5MFP_EPWM0_SYNC_OUT
#define | SYS_GPF_MFPL_PF5MFP_X32_IN
#define | SYS_GPF_MFPL_PF5MFP_EADC0_ST
#define | SYS_GPF_MFPL_PF6MFP_GPIO
#define | SYS_GPF_MFPL_PF6MFP_EBI_ADR19
#define | SYS_GPF_MFPL_PF6MFP_SC0_CLK
#define | SYS_GPF_MFPL_PF6MFP_I2S0_LRCK
#define | SYS_GPF_MFPL_PF6MFP_SPI0_MOSI
#define | SYS_GPF_MFPL_PF6MFP_UART4_RXD
#define | SYS_GPF_MFPL_PF6MFP_EBI_nCS0
#define | SYS_GPF_MFPL_PF6MFP_CAN2_RXD
#define | SYS_GPF_MFPL_PF6MFP_TAMPER0
#define | SYS_GPF_MFPL_PF7MFP_GPIO
#define | SYS_GPF_MFPL_PF7MFP_EBI_ADR18
#define | SYS_GPF_MFPL_PF7MFP_SC0_DAT
#define | SYS_GPF_MFPL_PF7MFP_I2S0_DO
#define | SYS_GPF_MFPL_PF7MFP_SPI0_MISO
#define | SYS_GPF_MFPL_PF7MFP_UART4_TXD
#define | SYS_GPF_MFPL_PF7MFP_CCAP_DATA0 (0x07UL<<SYS_GPF_MFPL_PF7MFP_Pos)
#define | SYS_GPF_MFPL_PF7MFP_CAN2_TXD (0x08UL<<SYS_GPF_MFPL_PF7MFP_Pos)
#define | SYS_GPF_MFPL_PF7MFP_TAMPER1
#define | SYS_GPF_MFPH_PF8MFP_GPIO
#define | SYS_GPF_MFPH_PF8MFP_EBI_ADR17
#define | SYS_GPF_MFPH_PF8MFP_SC0_RST
#define | SYS_GPF_MFPH_PF8MFP_I2S0_DI
#define | SYS_GPF_MFPH_PF8MFP_SPI0_CLK
#define | SYS_GPF_MFPH_PF8MFP_UART5_nCTS
#define | SYS_GPF_MFPH_PF8MFP_CCAP_DATA1
#define | SYS_GPF_MFPH_PF8MFP_CAN1_RXD (0x08UL<<SYS_GPF_MFPH_PF8MFP_Pos)
#define | SYS_GPF_MFPH_PF8MFP_TAMPER2
#define | SYS_GPF_MFPH_PF9MFP_GPIO
#define | SYS_GPF_MFPH_PF9MFP_EBI_ADR16
#define | SYS_GPF_MFPH_PF9MFP_SC0_PWR
#define | SYS_GPF_MFPH_PF9MFP_I2S0_MCLK
#define | SYS_GPF_MFPH_PF9MFP_SPI0_SS
#define | SYS_GPF_MFPH_PF9MFP_UART5_nRTS
#define | SYS_GPF_MFPH_PF9MFP_CCAP_DATA2
#define | SYS_GPF_MFPH_PF9MFP_CAN1_TXD
#define | SYS_GPF_MFPH_PF9MFP_TAMPER3
#define | SYS_GPF_MFPH_PF10MFP_GPIO
#define | SYS_GPF_MFPH_PF10MFP_EBI_ADR15
#define | SYS_GPF_MFPH_PF10MFP_SC0_nCD
#define | SYS_GPF_MFPH_PF10MFP_I2S0_BCLK
#define | SYS_GPF_MFPH_PF10MFP_SPI0_I2SMCLK
#define | SYS_GPF_MFPH_PF10MFP_UART5_RXD
#define | SYS_GPF_MFPH_PF10MFP_CCAP_DATA3
#define | SYS_GPF_MFPH_PF10MFP_TAMPER4
#define | SYS_GPF_MFPH_PF11MFP_GPIO
#define | SYS_GPF_MFPH_PF11MFP_EBI_ADR14
#define | SYS_GPF_MFPH_PF11MFP_SPI2_MOSI
#define | SYS_GPF_MFPH_PF11MFP_UART5_TXD
#define | SYS_GPF_MFPH_PF11MFP_CCAP_DATA4
#define | SYS_GPF_MFPH_PF11MFP_TAMPER5
#define | SYS_GPF_MFPH_PF11MFP_TM3
#define | SYS_GPG_MFPL_PG0MFP_GPIO
#define | SYS_GPG_MFPL_PG0MFP_EBI_ADR8
#define | SYS_GPG_MFPL_PG0MFP_I2C0_SCL
#define | SYS_GPG_MFPL_PG0MFP_I2C1_SMBAL
#define | SYS_GPG_MFPL_PG0MFP_UART2_RXD
#define | SYS_GPG_MFPL_PG0MFP_CAN1_TXD
#define | SYS_GPG_MFPL_PG0MFP_UART1_TXD
#define | SYS_GPG_MFPL_PG1MFP_GPIO
#define | SYS_GPG_MFPL_PG1MFP_EBI_ADR9
#define | SYS_GPG_MFPL_PG1MFP_SPI2_I2SMCLK
#define | SYS_GPG_MFPL_PG1MFP_I2C0_SDA
#define | SYS_GPG_MFPL_PG1MFP_I2C1_SMBSUS
#define | SYS_GPG_MFPL_PG1MFP_UART2_TXD
#define | SYS_GPG_MFPL_PG1MFP_CAN1_RXD
#define | SYS_GPG_MFPL_PG1MFP_UART1_RXD
#define | SYS_GPG_MFPL_PG2MFP_GPIO
#define | SYS_GPG_MFPL_PG2MFP_EBI_ADR11
#define | SYS_GPG_MFPL_PG2MFP_SPI2_SS
#define | SYS_GPG_MFPL_PG2MFP_I2C0_SMBAL
#define | SYS_GPG_MFPL_PG2MFP_I2C1_SCL
#define | SYS_GPG_MFPL_PG2MFP_CCAP_DATA7
#define | SYS_GPG_MFPL_PG2MFP_TM0
#define | SYS_GPG_MFPL_PG3MFP_GPIO
#define | SYS_GPG_MFPL_PG3MFP_EBI_ADR12
#define | SYS_GPG_MFPL_PG3MFP_SPI2_CLK
#define | SYS_GPG_MFPL_PG3MFP_I2C0_SMBSUS
#define | SYS_GPG_MFPL_PG3MFP_I2C1_SDA
#define | SYS_GPG_MFPL_PG3MFP_CCAP_DATA6
#define | SYS_GPG_MFPL_PG3MFP_TM1
#define | SYS_GPG_MFPL_PG4MFP_GPIO
#define | SYS_GPG_MFPL_PG4MFP_EBI_ADR13
#define | SYS_GPG_MFPL_PG4MFP_SPI2_MISO
#define | SYS_GPG_MFPL_PG4MFP_CCAP_DATA5
#define | SYS_GPG_MFPL_PG4MFP_TM2
#define | SYS_GPG_MFPL_PG5MFP_GPIO
#define | SYS_GPG_MFPL_PG5MFP_EBI_nCS1
#define | SYS_GPG_MFPL_PG5MFP_SPI3_SS
#define | SYS_GPG_MFPL_PG5MFP_SC1_PWR
#define | SYS_GPG_MFPL_PG5MFP_EPWM0_CH3
#define | SYS_GPG_MFPL_PG6MFP_GPIO
#define | SYS_GPG_MFPL_PG6MFP_EBI_nCS2
#define | SYS_GPG_MFPL_PG6MFP_SPI3_CLK
#define | SYS_GPG_MFPL_PG6MFP_SC1_RST
#define | SYS_GPG_MFPL_PG6MFP_EPWM0_CH2
#define | SYS_GPG_MFPL_PG7MFP_GPIO
#define | SYS_GPG_MFPL_PG7MFP_EBI_nWRL
#define | SYS_GPG_MFPL_PG7MFP_SPI3_MISO
#define | SYS_GPG_MFPL_PG7MFP_SC1_DAT
#define | SYS_GPG_MFPL_PG7MFP_EPWM0_CH1
#define | SYS_GPG_MFPH_PG8MFP_GPIO
#define | SYS_GPG_MFPH_PG8MFP_EBI_nWRH
#define | SYS_GPG_MFPH_PG8MFP_SPI3_MOSI
#define | SYS_GPG_MFPH_PG8MFP_SC1_CLK
#define | SYS_GPG_MFPH_PG8MFP_EPWM0_CH0
#define | SYS_GPG_MFPH_PG9MFP_GPIO
#define | SYS_GPG_MFPH_PG9MFP_EBI_AD0
#define | SYS_GPG_MFPH_PG9MFP_SD1_DAT3
#define | SYS_GPG_MFPH_PG9MFP_SPIM_D2
#define | SYS_GPG_MFPH_PG9MFP_QSPI1_MISO1
#define | SYS_GPG_MFPH_PG9MFP_CCAP_PIXCLK
#define | SYS_GPG_MFPH_PG9MFP_BPWM0_CH5
#define | SYS_GPG_MFPH_PG10MFP_GPIO
#define | SYS_GPG_MFPH_PG10MFP_EBI_AD1
#define | SYS_GPG_MFPH_PG10MFP_SD1_DAT2
#define | SYS_GPG_MFPH_PG10MFP_SPIM_D3
#define | SYS_GPG_MFPH_PG10MFP_QSPI1_MOSI1
#define | SYS_GPG_MFPH_PG10MFP_CCAP_SCLK
#define | SYS_GPG_MFPH_PG10MFP_BPWM0_CH4
#define | SYS_GPG_MFPH_PG11MFP_GPIO
#define | SYS_GPG_MFPH_PG11MFP_EBI_AD2
#define | SYS_GPG_MFPH_PG11MFP_SD1_DAT1
#define | SYS_GPG_MFPH_PG11MFP_SPIM_SS
#define | SYS_GPG_MFPH_PG11MFP_QSPI1_SS
#define | SYS_GPG_MFPH_PG11MFP_UART7_TXD
#define | SYS_GPG_MFPH_PG11MFP_CCAP_SFIELD
#define | SYS_GPG_MFPH_PG11MFP_BPWM0_CH3
#define | SYS_GPG_MFPH_PG12MFP_GPIO
#define | SYS_GPG_MFPH_PG12MFP_EBI_AD3
#define | SYS_GPG_MFPH_PG12MFP_SD1_DAT0
#define | SYS_GPG_MFPH_PG12MFP_SPIM_CLK
#define | SYS_GPG_MFPH_PG12MFP_QSPI1_CLK
#define | SYS_GPG_MFPH_PG12MFP_UART7_RXD
#define | SYS_GPG_MFPH_PG12MFP_CCAP_VSYNC
#define | SYS_GPG_MFPH_PG12MFP_BPWM0_CH2
#define | SYS_GPG_MFPH_PG13MFP_GPIO
#define | SYS_GPG_MFPH_PG13MFP_EBI_AD4
#define | SYS_GPG_MFPH_PG13MFP_SD1_CMD
#define | SYS_GPG_MFPH_PG13MFP_SPIM_MISO
#define | SYS_GPG_MFPH_PG13MFP_QSPI1_MISO0
#define | SYS_GPG_MFPH_PG13MFP_UART6_TXD
#define | SYS_GPG_MFPH_PG13MFP_CCAP_HSYNC
#define | SYS_GPG_MFPH_PG13MFP_BPWM0_CH1
#define | SYS_GPG_MFPH_PG14MFP_GPIO
#define | SYS_GPG_MFPH_PG14MFP_EBI_AD5
#define | SYS_GPG_MFPH_PG14MFP_SD1_CLK
#define | SYS_GPG_MFPH_PG14MFP_SPIM_MOSI
#define | SYS_GPG_MFPH_PG14MFP_QSPI1_MOSI0
#define | SYS_GPG_MFPH_PG14MFP_UART6_RXD
#define | SYS_GPG_MFPH_PG14MFP_BPWM0_CH0
#define | SYS_GPG_MFPH_PG15MFP_GPIO
#define | SYS_GPG_MFPH_PG15MFP_SD1_nCD
#define | SYS_GPG_MFPH_PG15MFP_CLKO
#define | SYS_GPG_MFPH_PG15MFP_EADC0_ST
#define | SYS_GPH_MFPL_PH0MFP_GPIO
#define | SYS_GPH_MFPL_PH0MFP_EBI_ADR7
#define | SYS_GPH_MFPL_PH0MFP_UART5_TXD
#define | SYS_GPH_MFPL_PH0MFP_TM0_EXT
#define | SYS_GPH_MFPL_PH1MFP_GPIO
#define | SYS_GPH_MFPL_PH1MFP_EBI_ADR6
#define | SYS_GPH_MFPL_PH1MFP_UART5_RXD
#define | SYS_GPH_MFPL_PH1MFP_TM1_EXT
#define | SYS_GPH_MFPL_PH2MFP_GPIO
#define | SYS_GPH_MFPL_PH2MFP_EBI_ADR5
#define | SYS_GPH_MFPL_PH2MFP_UART5_nRTS
#define | SYS_GPH_MFPL_PH2MFP_UART4_TXD
#define | SYS_GPH_MFPL_PH2MFP_I2C0_SCL
#define | SYS_GPH_MFPL_PH2MFP_TM2_EXT
#define | SYS_GPH_MFPL_PH3MFP_GPIO
#define | SYS_GPH_MFPL_PH3MFP_EBI_ADR4
#define | SYS_GPH_MFPL_PH3MFP_SPI1_I2SMCLK
#define | SYS_GPH_MFPL_PH3MFP_UART5_nCTS
#define | SYS_GPH_MFPL_PH3MFP_UART4_RXD
#define | SYS_GPH_MFPL_PH3MFP_I2C0_SDA
#define | SYS_GPH_MFPL_PH3MFP_TM3_EXT
#define | SYS_GPH_MFPL_PH4MFP_GPIO
#define | SYS_GPH_MFPL_PH4MFP_EBI_ADR3
#define | SYS_GPH_MFPL_PH4MFP_SPI1_MISO
#define | SYS_GPH_MFPL_PH4MFP_UART7_nRTS
#define | SYS_GPH_MFPL_PH4MFP_UART6_TXD
#define | SYS_GPH_MFPL_PH5MFP_GPIO
#define | SYS_GPH_MFPL_PH5MFP_EBI_ADR2
#define | SYS_GPH_MFPL_PH5MFP_SPI1_MOSI
#define | SYS_GPH_MFPL_PH5MFP_UART7_nCTS
#define | SYS_GPH_MFPL_PH5MFP_UART6_RXD
#define | SYS_GPH_MFPL_PH6MFP_GPIO
#define | SYS_GPH_MFPL_PH6MFP_EBI_ADR1
#define | SYS_GPH_MFPL_PH6MFP_SPI1_CLK
#define | SYS_GPH_MFPL_PH6MFP_UART7_TXD
#define | SYS_GPH_MFPL_PH7MFP_GPIO
#define | SYS_GPH_MFPL_PH7MFP_EBI_ADR0
#define | SYS_GPH_MFPL_PH7MFP_SPI1_SS
#define | SYS_GPH_MFPL_PH7MFP_UART7_RXD
#define | SYS_GPH_MFPH_PH8MFP_GPIO
#define | SYS_GPH_MFPH_PH8MFP_EBI_AD12
#define | SYS_GPH_MFPH_PH8MFP_QSPI0_CLK
#define | SYS_GPH_MFPH_PH8MFP_SC2_PWR
#define | SYS_GPH_MFPH_PH8MFP_I2S0_DI
#define | SYS_GPH_MFPH_PH8MFP_SPI1_CLK
#define | SYS_GPH_MFPH_PH8MFP_UART3_nRTS
#define | SYS_GPH_MFPH_PH8MFP_I2C1_SMBAL
#define | SYS_GPH_MFPH_PH8MFP_I2C2_SCL
#define | SYS_GPH_MFPH_PH8MFP_UART1_TXD
#define | SYS_GPH_MFPH_PH9MFP_GPIO
#define | SYS_GPH_MFPH_PH9MFP_EBI_AD13
#define | SYS_GPH_MFPH_PH9MFP_QSPI0_SS
#define | SYS_GPH_MFPH_PH9MFP_SC2_RST
#define | SYS_GPH_MFPH_PH9MFP_I2S0_DO
#define | SYS_GPH_MFPH_PH9MFP_SPI1_SS
#define | SYS_GPH_MFPH_PH9MFP_UART3_nCTS
#define | SYS_GPH_MFPH_PH9MFP_I2C1_SMBSUS
#define | SYS_GPH_MFPH_PH9MFP_I2C2_SDA
#define | SYS_GPH_MFPH_PH9MFP_UART1_RXD
#define | SYS_GPH_MFPH_PH10MFP_GPIO
#define | SYS_GPH_MFPH_PH10MFP_EBI_AD14
#define | SYS_GPH_MFPH_PH10MFP_QSPI0_MISO1
#define | SYS_GPH_MFPH_PH10MFP_SC2_nCD
#define | SYS_GPH_MFPH_PH10MFP_I2S0_LRCK
#define | SYS_GPH_MFPH_PH10MFP_SPI1_I2SMCLK
#define | SYS_GPH_MFPH_PH10MFP_UART4_TXD
#define | SYS_GPH_MFPH_PH10MFP_UART0_TXD
#define | SYS_GPH_MFPH_PH11MFP_GPIO
#define | SYS_GPH_MFPH_PH11MFP_EBI_AD15
#define | SYS_GPH_MFPH_PH11MFP_QSPI0_MOSI1
#define | SYS_GPH_MFPH_PH11MFP_UART4_RXD
#define | SYS_GPH_MFPH_PH11MFP_UART0_RXD
#define | SYS_GPH_MFPH_PH11MFP_EPWM0_CH5
#define | SYS_CLEAR_BOD_INT_FLAG()
| Clear Brown-out detector interrupt flag. More...
#define | SYS_CLEAR_BOD_LPM()
| Set Brown-out detector function to normal mode. More...
#define | SYS_DISABLE_BOD()
| Disable Brown-out detector function. More...
#define | SYS_ENABLE_BOD()
| Enable Brown-out detector function. More...
#define | SYS_GET_BOD_INT_FLAG()
| Get Brown-out detector interrupt flag. More...
#define | SYS_GET_BOD_OUTPUT()
| Get Brown-out detector status. More...
#define | SYS_DISABLE_BOD_RST()
| Enable Brown-out detector interrupt function. More...
#define | SYS_ENABLE_BOD_RST()
| Enable Brown-out detector reset function. More...
#define | SYS_SET_BOD_LPM()
| Set Brown-out detector function low power mode. More...
#define | SYS_SET_BOD_LEVEL(u32Level)
| Set Brown-out detector voltage level. More...
#define | SYS_IS_BOD_RST()
| Get reset source is from Brown-out detector reset. More...
#define | SYS_IS_CPU_RST()
| Get reset source is from CPU reset. More...
#define | SYS_IS_LVR_RST()
| Get reset source is from LVR Reset. More...
#define | SYS_IS_POR_RST()
| Get reset source is from Power-on Reset. More...
#define | SYS_IS_RSTPIN_RST()
| Get reset source is from reset pin reset. More...
#define | SYS_IS_SYSTEM_RST()
| Get reset source is from system reset. More...
#define | SYS_IS_WDT_RST()
| Get reset source is from window watch dog reset. More...
#define | SYS_DISABLE_LVR()
| Disable Low-Voltage-Reset function. More...
#define | SYS_ENABLE_LVR()
| Enable Low-Voltage-Reset function. More...
#define | SYS_DISABLE_POR()
| Disable Power-on Reset function. More...
#define | SYS_ENABLE_POR()
| Enable Power-on Reset function. More...
#define | SYS_CLEAR_RST_SOURCE(u32RstSrc)
| Clear reset source flag. More...

## Functions
__STATIC_INLINE void | SYS_UnlockReg (void)
| Disable register write-protection function. More...
__STATIC_INLINE void | SYS_LockReg (void)
| Enable register write-protection function. More...
void | SYS_ClearResetSrc (uint32_t u32Src)
| Clear reset source. More...
uint32_t | SYS_GetBODStatus (void)
| Get Brown-out detector output status. More...
uint32_t | SYS_GetResetSrc (void)
| Get reset status register value. More...
uint32_t | SYS_IsRegLocked (void)
| Check if register is locked nor not. More...
uint32_t | SYS_ReadPDID (void)
| Get product ID. More...
void | SYS_ResetChip (void)
| Reset chip with chip reset. More...
void | SYS_ResetCPU (void)
| Reset chip with CPU reset. More...
void | SYS_ResetModule (uint32_t u32ModuleIndex)
| Reset selected module. More...
void | SYS_EnableBOD (int32_t i32Mode, uint32_t u32BODLevel)
| Enable and configure Brown-out detector function. More...
void | SYS_DisableBOD (void)
| Disable Brown-out detector function. More...
void | SYS_SetPowerLevel (uint32_t u32PowerLevel)
| Set Power Level. More...
void | SYS_SetVRef (uint32_t u32VRefCTL)
| Set Reference Voltage. More...

## Detailed Description

M480 Series SYS Driver Header File.

Version
  V3.0 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file sys.h.