| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
gpio.c File Reference

M480 series GPIO driver source file. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
void | GPIO_SetMode (GPIO_T *port, uint32_t u32PinMask, uint32_t u32Mode)
| Set GPIO operation mode. More...
void | GPIO_EnableInt (GPIO_T *port, uint32_t u32Pin, uint32_t u32IntAttribs)
| Enable GPIO interrupt. More...
void | GPIO_DisableInt (GPIO_T *port, uint32_t u32Pin)
| Disable GPIO interrupt. More...
void | GPIO_SetSlewCtl (GPIO_T *port, uint32_t u32PinMask, uint32_t u32Mode)
| Set GPIO slew rate control. More...
void | GPIO_SetPullCtl (GPIO_T *port, uint32_t u32PinMask, uint32_t u32Mode)
| Set GPIO Pull-up and Pull-down control. More...

## Detailed Description

M480 series GPIO driver source file.

Version
  V3.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file gpio.c.