| M480 BSP V3.05.001 The Board Support Package for M480 Series

Data Structures
Here are the data structures with brief descriptions:

C__FILE |
C ac_if_t |
C ACMP_T |
C as_if_t |
C BCAPDAT_T |
C BPWM_T |
C CAN_IF_T |
C CAN_T |
C CCAP_T |
C cdc_dev_t |
C CLK_T |
C CRC_T |
C CRPT_T |
C DAC_T |
C DSCT_T |
C EADC_T |
C EBI_T |
C ECAP_T |
C ECAPDAT_T |
C EMAC_T |
C EPWM_T |
C FMC_T |
C GPIO_DBCTL_T |
C GPIO_T |
C HSOTG_T |
C HSUSBD_CMD_STRUCT |
C HSUSBD_EP_T |
C HSUSBD_T |
C HSUSBH_T |
C I2C_T |
C I2S_T |
C NMI_T |
C OPA_T |
C OTG_T |
C PDMA_T |
C QEI_T |
C QSPI_T |
C REPEAT_T |
C RTC_T |
C s_hsusbd_info |
C S_RTC_TIME_DATA_T |
C s_usbd_info |
C SC_T |
C SCLIB_CARD_INFO_T | A structure holds smartcard information
C SDH_info_t |
C SDH_T |
C SPI_T |
C SPIM_T |
C STR_CANMASK_T |
C STR_CANMSG_T |
C STRIDE_T |
C SYS_T |
C TIMER_T |
C TRNG_T |
C uac_dev_t |
C UART_T |
C UI2C_T |
C USBD_EP_T |
C USBD_T |
C USBH_T |
C usbhid_dev |
C usbhid_keyboard_event |
C usbhid_mouse_event |
C USPI_T |
C UUART_T |
C WDT_T |
C WWDT_T |