| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros | Functions
usci_uart.h File Reference

M480 series USCI UART (UUART) driver header file. More...

Go to the source code of this file.

## Macros
#define | UUART_WORD_LEN_6
#define | UUART_WORD_LEN_7
#define | UUART_WORD_LEN_8
#define | UUART_WORD_LEN_9
#define | UUART_PARITY_NONE
#define | UUART_PARITY_ODD
#define | UUART_PARITY_EVEN
#define | UUART_STOP_BIT_1
#define | UUART_STOP_BIT_2
#define | UUART_ABR_INT_MASK
#define | UUART_RLS_INT_MASK
#define | UUART_BUF_RXOV_INT_MASK
#define | UUART_TXST_INT_MASK
#define | UUART_TXEND_INT_MASK
#define | UUART_RXST_INT_MASK
#define | UUART_RXEND_INT_MASK
#define | UUART_WRITE(uuart, u8Data)
| Write USCI_UART data. More...
#define | UUART_READ(uuart)
| Read USCI_UART data. More...
#define | UUART_GET_TX_EMPTY(uuart)
| Get Tx empty. More...
#define | UUART_GET_RX_EMPTY(uuart)
| Get Rx empty. More...
#define | UUART_IS_TX_EMPTY(uuart)
| Check specified usci_uart port transmission is over. More...
#define | UUART_IS_RX_EMPTY(uuart)
| Check specified usci_uart port receiver is empty. More...
#define | UUART_WAIT_TX_EMPTY(uuart)
| Wait specified usci_uart port transmission is over. More...
#define | UUART_IS_TX_FULL(uuart)
| Check TX buffer is full or not. More...
#define | UUART_IS_RX_FULL(uuart)
| Check RX buffer is full or not. More...
#define | UUART_GET_TX_FULL(uuart)
| Get Tx full register value. More...
#define | UUART_GET_RX_FULL(uuart)
| Get Rx full register value. More...
#define | UUART_ENABLE_PROT_INT(uuart, u32IntSel)
| Enable specified USCI_UART protocol interrupt. More...
#define | UUART_DISABLE_PROT_INT(uuart, u32IntSel)
| Disable specified USCI_UART protocol interrupt. More...
#define | UUART_ENABLE_BUF_INT(uuart, u32IntSel)
| Enable specified USCI_UART buffer interrupt. More...
#define | UUART_DISABLE_BUF_INT(uuart, u32IntSel)
| Disable specified USCI_UART buffer interrupt. More...
#define | UUART_ENABLE_TRANS_INT(uuart, u32IntSel)
| Enable specified USCI_UART transfer interrupt. More...
#define | UUART_DISABLE_TRANS_INT(uuart, u32IntSel)
| Disable specified USCI_UART transfer interrupt. More...
#define | UUART_GET_PROT_STATUS(uuart)
| Get protocol interrupt flag/status. More...
#define | UUART_CLR_PROT_INT_FLAG(uuart, u32IntTypeFlag)
| Clear specified protocol interrupt flag. More...
#define | UUART_GET_BUF_STATUS(uuart)
| Get transmit/receive buffer interrupt flag/status. More...
#define | UUART_CLR_BUF_INT_FLAG(uuart, u32IntTypeFlag)
| Clear specified buffer interrupt flag. More...
#define | UUART_GET_WAKEUP_FLAG(uuart)
| Get wakeup flag. More...
#define | UUART_CLR_WAKEUP_FLAG(uuart)
| Clear wakeup flag. More...
#define | UUART_TRIGGER_RX_PDMA(uuart)
| Trigger RX PDMA function. More...
#define | UUART_TRIGGER_TX_PDMA(uuart)
| Trigger TX PDMA function. More...
#define | UUART_DISABLE_RX_PDMA(uuart)
| Disable RX PDMA transfer. More...
#define | UUART_DISABLE_TX_PDMA(uuart)
| Disable TX PDMA transfer. More...
#define | UUART_PDMA_ENABLE(uuart, u32FuncSel)
| Enable specified USCI_UART PDMA function. More...
#define | UUART_PDMA_DISABLE(uuart, u32FuncSel)
| Disable specified USCI_UART PDMA function. More...

## Functions
void | UUART_ClearIntFlag (UUART_T *uuart, uint32_t u32Mask)
| Clear USCI_UART specified interrupt flag. More...
uint32_t | UUART_GetIntFlag (UUART_T *uuart, uint32_t u32Mask)
| Get USCI_UART specified interrupt flag. More...
void | UUART_Close (UUART_T *uuart)
| Disable USCI_UART function mode. More...
void | UUART_DisableInt (UUART_T *uuart, uint32_t u32Mask)
| Disable interrupt function. More...
void | UUART_EnableInt (UUART_T *uuart, uint32_t u32Mask)
| Enable interrupt function. More...
uint32_t | UUART_Open (UUART_T *uuart, uint32_t u32baudrate)
| Open and set USCI_UART function. More...
uint32_t | UUART_Read (UUART_T *uuart, uint8_t pu8RxBuf[], uint32_t u32ReadBytes)
| Read USCI_UART data. More...
uint32_t | UUART_SetLine_Config (UUART_T *uuart, uint32_t u32baudrate, uint32_t u32data_width, uint32_t u32parity, uint32_t u32stop_bits)
| Set USCI_UART line configuration. More...
uint32_t | UUART_Write (UUART_T *uuart, uint8_t pu8TxBuf[], uint32_t u32WriteBytes)
| Write USCI_UART data. More...
void | UUART_EnableWakeup (UUART_T *uuart, uint32_t u32WakeupMode)
| Enable USCI_UART Wake-up Function. More...
void | UUART_DisableWakeup (UUART_T *uuart)
| Disable USCI_UART Wake-up Function. More...
void | UUART_EnableFlowCtrl (UUART_T *uuart)
| Enable USCI_UART auto flow control. More...
void | UUART_DisableFlowCtrl (UUART_T *uuart)
| Disable USCI_UART auto flow control. More...

## Detailed Description

M480 series USCI UART (UUART) driver header file.

Version
  V3.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file usci_uart.h.