| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
SCUART Exported Constants
Standard Driver » SCUART Driver

## Macros
#define | SCUART_CHAR_LEN_5
#define | SCUART_CHAR_LEN_6
#define | SCUART_CHAR_LEN_7
#define | SCUART_CHAR_LEN_8
#define | SCUART_PARITY_NONE
#define | SCUART_PARITY_ODD
#define | SCUART_PARITY_EVEN
#define | SCUART_STOP_BIT_1
#define | SCUART_STOP_BIT_2

## Detailed Description

## Macro Definition Documentation

## ◆ SCUART_CHAR_LEN_5

#define SCUART_CHAR_LEN_5

Set SCUART word length to 5 bits

Definition at line 29 of file scuart.h.

## ◆ SCUART_CHAR_LEN_6

#define SCUART_CHAR_LEN_6

Set SCUART word length to 6 bits

Definition at line 30 of file scuart.h.

## ◆ SCUART_CHAR_LEN_7

#define SCUART_CHAR_LEN_7

Set SCUART word length to 7 bits

Definition at line 31 of file scuart.h.

## ◆ SCUART_CHAR_LEN_8

#define SCUART_CHAR_LEN_8

Set SCUART word length to 8 bits

Definition at line 32 of file scuart.h.

## ◆ SCUART_PARITY_EVEN

#define SCUART_PARITY_EVEN

Set SCUART transfer with even parity

Definition at line 36 of file scuart.h.

## ◆ SCUART_PARITY_NONE

#define SCUART_PARITY_NONE

Set SCUART transfer with no parity

Definition at line 34 of file scuart.h.

## ◆ SCUART_PARITY_ODD

#define SCUART_PARITY_ODD

Set SCUART transfer with odd parity

Definition at line 35 of file scuart.h.

## ◆ SCUART_STOP_BIT_1

#define SCUART_STOP_BIT_1

Set SCUART transfer with one stop bit

Definition at line 38 of file scuart.h.

## ◆ SCUART_STOP_BIT_2

#define SCUART_STOP_BIT_2

Set SCUART transfer with two stop bits

Definition at line 39 of file scuart.h.