| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
I2C Exported Constants
Standard Driver » I2C Driver

## Macros
#define | I2C_CTL_STA_SI
#define | I2C_CTL_STA_SI_AA
#define | I2C_CTL_STO_SI
#define | I2C_CTL_STO_SI_AA
#define | I2C_CTL_SI
#define | I2C_CTL_SI_AA
#define | I2C_CTL_STA
#define | I2C_CTL_STO
#define | I2C_CTL_AA
#define | I2C_GCMODE_ENABLE
#define | I2C_GCMODE_DISABLE
#define | I2C_SMBH_ENABLE
#define | I2C_SMBD_ENABLE
#define | I2C_PECTX_ENABLE
#define | I2C_PECTX_DISABLE

## Detailed Description

## Macro Definition Documentation

## ◆ I2C_CTL_AA

#define I2C_CTL_AA

I2C_CTL setting for I2C control bits. It would set AA bit

Definition at line 41 of file i2c.h.

## ◆ I2C_CTL_SI

#define I2C_CTL_SI

I2C_CTL setting for I2C control bits. It would set SI bit

Definition at line 37 of file i2c.h.

## ◆ I2C_CTL_SI_AA

#define I2C_CTL_SI_AA

I2C_CTL setting for I2C control bits. It would set SI and AA bits

Definition at line 38 of file i2c.h.

## ◆ I2C_CTL_STA

#define I2C_CTL_STA

I2C_CTL setting for I2C control bits. It would set STA bit

Definition at line 39 of file i2c.h.

## ◆ I2C_CTL_STA_SI

#define I2C_CTL_STA_SI

I2C_CTL setting for I2C control bits. It would set STA and SI bits

Definition at line 33 of file i2c.h.

## ◆ I2C_CTL_STA_SI_AA

#define I2C_CTL_STA_SI_AA

I2C_CTL setting for I2C control bits. It would set STA, SI and AA bits

Definition at line 34 of file i2c.h.

## ◆ I2C_CTL_STO

#define I2C_CTL_STO

I2C_CTL setting for I2C control bits. It would set STO bit

Definition at line 40 of file i2c.h.

## ◆ I2C_CTL_STO_SI

#define I2C_CTL_STO_SI

I2C_CTL setting for I2C control bits. It would set STO and SI bits

Definition at line 35 of file i2c.h.

## ◆ I2C_CTL_STO_SI_AA

#define I2C_CTL_STO_SI_AA

I2C_CTL setting for I2C control bits. It would set STO, SI and AA bits

Definition at line 36 of file i2c.h.

## ◆ I2C_GCMODE_DISABLE

#define I2C_GCMODE_DISABLE

Disable I2C GC Mode

Definition at line 47 of file i2c.h.

## ◆ I2C_GCMODE_ENABLE

#define I2C_GCMODE_ENABLE

Enable I2C GC Mode

Definition at line 46 of file i2c.h.

## ◆ I2C_PECTX_DISABLE

#define I2C_PECTX_DISABLE

Disable SMBus Packet Error Check Transmit function

Definition at line 55 of file i2c.h.

## ◆ I2C_PECTX_ENABLE

#define I2C_PECTX_ENABLE

Enable SMBus Packet Error Check Transmit function

Definition at line 54 of file i2c.h.

## ◆ I2C_SMBD_ENABLE

#define I2C_SMBD_ENABLE

Enable SMBus Device Mode enable

Definition at line 53 of file i2c.h.

## ◆ I2C_SMBH_ENABLE

#define I2C_SMBH_ENABLE

Enable SMBus Host Mode enable

Definition at line 52 of file i2c.h.