| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
WWDT Exported Constants
Standard Driver » WWDT Driver

## Macros
#define | WWDT_PRESCALER_1
#define | WWDT_PRESCALER_2
#define | WWDT_PRESCALER_4
#define | WWDT_PRESCALER_8
#define | WWDT_PRESCALER_16
#define | WWDT_PRESCALER_32
#define | WWDT_PRESCALER_64
#define | WWDT_PRESCALER_128
#define | WWDT_PRESCALER_192
#define | WWDT_PRESCALER_256
#define | WWDT_PRESCALER_384
#define | WWDT_PRESCALER_512
#define | WWDT_PRESCALER_768
#define | WWDT_PRESCALER_1024
#define | WWDT_PRESCALER_1536
#define | WWDT_PRESCALER_2048
#define | WWDT_RELOAD_WORD

## Detailed Description

## Macro Definition Documentation

## ◆ WWDT_PRESCALER_1

#define WWDT_PRESCALER_1

Select max time-out period to 1 * (64*WWDT_CLK)

Definition at line 32 of file wwdt.h.

## ◆ WWDT_PRESCALER_1024

#define WWDT_PRESCALER_1024

Select max time-out period to 1024 * (64*WWDT_CLK)

Definition at line 45 of file wwdt.h.

## ◆ WWDT_PRESCALER_128

#define WWDT_PRESCALER_128

Select max time-out period to 128 * (64*WWDT_CLK)

Definition at line 39 of file wwdt.h.

## ◆ WWDT_PRESCALER_1536

#define WWDT_PRESCALER_1536

Select max time-out period to 1536 * (64*WWDT_CLK)

Definition at line 46 of file wwdt.h.

## ◆ WWDT_PRESCALER_16

#define WWDT_PRESCALER_16

Select max time-out period to 16 * (64*WWDT_CLK)

Definition at line 36 of file wwdt.h.

## ◆ WWDT_PRESCALER_192

#define WWDT_PRESCALER_192

Select max time-out period to 192 * (64*WWDT_CLK)

Definition at line 40 of file wwdt.h.

## ◆ WWDT_PRESCALER_2

#define WWDT_PRESCALER_2

Select max time-out period to 2 * (64*WWDT_CLK)

Definition at line 33 of file wwdt.h.

## ◆ WWDT_PRESCALER_2048

#define WWDT_PRESCALER_2048

Select max time-out period to 2048 * (64*WWDT_CLK)

Definition at line 47 of file wwdt.h.

## ◆ WWDT_PRESCALER_256

#define WWDT_PRESCALER_256

Select max time-out period to 256 * (64*WWDT_CLK)

Definition at line 41 of file wwdt.h.

## ◆ WWDT_PRESCALER_32

#define WWDT_PRESCALER_32

Select max time-out period to 32 * (64*WWDT_CLK)

Definition at line 37 of file wwdt.h.

## ◆ WWDT_PRESCALER_384

#define WWDT_PRESCALER_384

Select max time-out period to 384 * (64*WWDT_CLK)

Definition at line 42 of file wwdt.h.

## ◆ WWDT_PRESCALER_4

#define WWDT_PRESCALER_4

Select max time-out period to 4 * (64*WWDT_CLK)

Definition at line 34 of file wwdt.h.

## ◆ WWDT_PRESCALER_512

#define WWDT_PRESCALER_512

Select max time-out period to 512 * (64*WWDT_CLK)

Definition at line 43 of file wwdt.h.

## ◆ WWDT_PRESCALER_64

#define WWDT_PRESCALER_64

Select max time-out period to 64 * (64*WWDT_CLK)

Definition at line 38 of file wwdt.h.

## ◆ WWDT_PRESCALER_768

#define WWDT_PRESCALER_768

Select max time-out period to 768 * (64*WWDT_CLK)

Definition at line 44 of file wwdt.h.

## ◆ WWDT_PRESCALER_8

#define WWDT_PRESCALER_8

Select max time-out period to 8 * (64*WWDT_CLK)

Definition at line 35 of file wwdt.h.

## ◆ WWDT_RELOAD_WORD

#define WWDT_RELOAD_WORD

Fill this value to WWDT_RLDCNT register to reload WWDT counter

Definition at line 52 of file wwdt.h.