| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
usci_uart.c File Reference

M480 series USCI UART (UUART) driver source file. More...

`#include <stdio.h>`
`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
void | UUART_ClearIntFlag (UUART_T *uuart, uint32_t u32Mask)
| Clear USCI_UART specified interrupt flag. More...
uint32_t | UUART_GetIntFlag (UUART_T *uuart, uint32_t u32Mask)
| Get USCI_UART specified interrupt flag. More...
void | UUART_Close (UUART_T *uuart)
| Disable USCI_UART function mode. More...
void | UUART_DisableInt (UUART_T *uuart, uint32_t u32Mask)
| Disable interrupt function. More...
void | UUART_EnableInt (UUART_T *uuart, uint32_t u32Mask)
| Enable interrupt function. More...
uint32_t | UUART_Open (UUART_T *uuart, uint32_t u32baudrate)
| Open and set USCI_UART function. More...
uint32_t | UUART_Read (UUART_T *uuart, uint8_t pu8RxBuf[], uint32_t u32ReadBytes)
| Read USCI_UART data. More...
uint32_t | UUART_SetLine_Config (UUART_T *uuart, uint32_t u32baudrate, uint32_t u32data_width, uint32_t u32parity, uint32_t u32stop_bits)
| Set USCI_UART line configuration. More...
uint32_t | UUART_Write (UUART_T *uuart, uint8_t pu8TxBuf[], uint32_t u32WriteBytes)
| Write USCI_UART data. More...
void | UUART_EnableWakeup (UUART_T *uuart, uint32_t u32WakeupMode)
| Enable USCI_UART Wake-up Function. More...
void | UUART_DisableWakeup (UUART_T *uuart)
| Disable USCI_UART Wake-up Function. More...
void | UUART_EnableFlowCtrl (UUART_T *uuart)
| Enable USCI_UART auto flow control. More...
void | UUART_DisableFlowCtrl (UUART_T *uuart)
| Disable USCI_UART auto flow control. More...

## Detailed Description

M480 series USCI UART (UUART) driver source file.

Version
  V3.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file usci_uart.c.