| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
EMAC Exported Constants
Standard Driver » EMAC Driver

## Macros
#define | EMAC_PHY_ADDR
#define | EMAC_RX_DESC_SIZE
#define | EMAC_TX_DESC_SIZE
#define | EMAC_CAMENTRY_NB
#define | EMAC_MAX_PKT_SIZE
#define | EMAC_LINK_DOWN
#define | EMAC_LINK_100F
#define | EMAC_LINK_100H
#define | EMAC_LINK_10F
#define | EMAC_LINK_10H

## Detailed Description

## Macro Definition Documentation

## ◆ EMAC_CAMENTRY_NB

#define EMAC_CAMENTRY_NB

Number of CAM

Definition at line 34 of file emac.h.

## ◆ EMAC_LINK_100F

#define EMAC_LINK_100F

Ethernet link is 100Mbps full duplex

Definition at line 38 of file emac.h.

## ◆ EMAC_LINK_100H

#define EMAC_LINK_100H

Ethernet link is 100Mbps half duplex

Definition at line 39 of file emac.h.

## ◆ EMAC_LINK_10F

#define EMAC_LINK_10F

Ethernet link is 10Mbps full duplex

Definition at line 40 of file emac.h.

## ◆ EMAC_LINK_10H

#define EMAC_LINK_10H

Ethernet link is 10Mbps half duplex

Definition at line 41 of file emac.h.

## ◆ EMAC_LINK_DOWN

#define EMAC_LINK_DOWN

Ethernet link is down

Definition at line 37 of file emac.h.

## ◆ EMAC_MAX_PKT_SIZE

#define EMAC_MAX_PKT_SIZE

Number of HDR + EXTRA + VLAN_TAG + PAYLOAD + CRC

Definition at line 35 of file emac.h.

## ◆ EMAC_PHY_ADDR

#define EMAC_PHY_ADDR

PHY address, this address is board dependent

Definition at line 31 of file emac.h.

## ◆ EMAC_RX_DESC_SIZE

#define EMAC_RX_DESC_SIZE

Number of Rx Descriptors, should be 2 at least

Definition at line 32 of file emac.h.

## ◆ EMAC_TX_DESC_SIZE

#define EMAC_TX_DESC_SIZE

Number of Tx Descriptors, should be 2 at least

Definition at line 33 of file emac.h.