| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
eadc.c File Reference

M480 series EADC driver source file. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
void | EADC_Open (EADC_T *eadc, uint32_t u32InputMode)
| This function make EADC_module be ready to convert. More...
void | EADC_Close (EADC_T *eadc)
| Disable EADC_module. More...
void | EADC_ConfigSampleModule (EADC_T *eadc, uint32_t u32ModuleNum, uint32_t u32TriggerSrc, uint32_t u32Channel)
| Configure the sample control logic module. More...
void | EADC_SetTriggerDelayTime (EADC_T *eadc, uint32_t u32ModuleNum, uint32_t u32TriggerDelayTime, uint32_t u32DelayClockDivider)
| Set trigger delay time. More...
void | EADC_SetExtendSampleTime (EADC_T *eadc, uint32_t u32ModuleNum, uint32_t u32ExtendSampleTime)
| Set ADC extend sample time. More...

## Detailed Description

M480 series EADC driver source file.

Version
  V2.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file eadc.c.