| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
qspi.c File Reference

M480 series QSPI driver source file. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
uint32_t | QSPI_Open (QSPI_T *qspi, uint32_t u32MasterSlave, uint32_t u32QSPIMode, uint32_t u32DataWidth, uint32_t u32BusClock)
| This function make QSPI module be ready to transfer. More...
void | QSPI_Close (QSPI_T *qspi)
| Disable QSPI controller. More...
void | QSPI_ClearRxFIFO (QSPI_T *qspi)
| Clear RX FIFO buffer. More...
void | QSPI_ClearTxFIFO (QSPI_T *qspi)
| Clear TX FIFO buffer. More...
void | QSPI_DisableAutoSS (QSPI_T *qspi)
| Disable the automatic slave selection function. More...
void | QSPI_EnableAutoSS (QSPI_T *qspi, uint32_t u32SSPinMask, uint32_t u32ActiveLevel)
| Enable the automatic slave selection function. More...
uint32_t | QSPI_SetBusClock (QSPI_T *qspi, uint32_t u32BusClock)
| Set the QSPI bus clock. More...
void | QSPI_SetFIFO (QSPI_T *qspi, uint32_t u32TxThreshold, uint32_t u32RxThreshold)
| Configure FIFO threshold setting. More...
uint32_t | QSPI_GetBusClock (QSPI_T *qspi)
| Get the actual frequency of QSPI bus clock. Only available in Master mode. More...
void | QSPI_EnableInt (QSPI_T *qspi, uint32_t u32Mask)
| Enable interrupt function. More...
void | QSPI_DisableInt (QSPI_T *qspi, uint32_t u32Mask)
| Disable interrupt function. More...
uint32_t | QSPI_GetIntFlag (QSPI_T *qspi, uint32_t u32Mask)
| Get interrupt flag. More...
void | QSPI_ClearIntFlag (QSPI_T *qspi, uint32_t u32Mask)
| Clear interrupt flag. More...
uint32_t | QSPI_GetStatus (QSPI_T *qspi, uint32_t u32Mask)
| Get QSPI status. More...

## Detailed Description

M480 series QSPI driver source file.

Version
  V3.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file qspi.c.