| M480 BSP V3.05.001 The Board Support Package for M480 Series

Functions
rtc.c File Reference

M480 series RTC driver source file. More...

`#include "NuMicro.h"`

Go to the source code of this file.

## Functions
void | RTC_Open (S_RTC_TIME_DATA_T *sPt)
| Initialize RTC module and start counting. More...
void | RTC_Close (void)
| Disable RTC Clock. More...
void | RTC_32KCalibration (int32_t i32FrequencyX10000)
| Set Frequency Compensation Data. More...
void | RTC_GetDateAndTime (S_RTC_TIME_DATA_T *sPt)
| Get Current RTC Date and Time. More...
void | RTC_GetAlarmDateAndTime (S_RTC_TIME_DATA_T *sPt)
| Get RTC Alarm Date and Time. More...
void | RTC_SetDateAndTime (S_RTC_TIME_DATA_T *sPt)
| Update Current RTC Date and Time. More...
void | RTC_SetAlarmDateAndTime (S_RTC_TIME_DATA_T *sPt)
| Update RTC Alarm Date and Time. More...
void | RTC_SetDate (uint32_t u32Year, uint32_t u32Month, uint32_t u32Day, uint32_t u32DayOfWeek)
| Update RTC Current Date. More...
void | RTC_SetTime (uint32_t u32Hour, uint32_t u32Minute, uint32_t u32Second, uint32_t u32TimeMode, uint32_t u32AmPm)
| Update RTC Current Time. More...
void | RTC_SetAlarmDate (uint32_t u32Year, uint32_t u32Month, uint32_t u32Day)
| Update RTC Alarm Date. More...
void | RTC_SetAlarmTime (uint32_t u32Hour, uint32_t u32Minute, uint32_t u32Second, uint32_t u32TimeMode, uint32_t u32AmPm)
| Update RTC Alarm Time. More...
void | RTC_SetAlarmDateMask (uint8_t u8IsTenYMsk, uint8_t u8IsYMsk, uint8_t u8IsTenMMsk, uint8_t u8IsMMsk, uint8_t u8IsTenDMsk, uint8_t u8IsDMsk)
| Set RTC Alarm Date Mask Function. More...
void | RTC_SetAlarmTimeMask (uint8_t u8IsTenHMsk, uint8_t u8IsHMsk, uint8_t u8IsTenMMsk, uint8_t u8IsMMsk, uint8_t u8IsTenSMsk, uint8_t u8IsSMsk)
| Set RTC Alarm Time Mask Function. More...
uint32_t | RTC_GetDayOfWeek (void)
| Get Day of the Week. More...
void | RTC_SetTickPeriod (uint32_t u32TickSelection)
| Set RTC Tick Period Time. More...
void | RTC_EnableInt (uint32_t u32IntFlagMask)
| Enable RTC Interrupt. More...
void | RTC_DisableInt (uint32_t u32IntFlagMask)
| Disable RTC Interrupt. More...
void | RTC_EnableSpareAccess (void)
| Enable Spare Registers Access. More...
void | RTC_DisableSpareRegister (void)
| Disable Spare Register. More...
void | RTC_StaticTamperEnable (uint32_t u32TamperSelect, uint32_t u32DetecLevel, uint32_t u32DebounceEn)
| Static Tamper Detect. More...
void | RTC_StaticTamperDisable (uint32_t u32TamperSelect)
| Static Tamper Disable. More...
void | RTC_DynamicTamperEnable (uint32_t u32PairSel, uint32_t u32DebounceEn, uint32_t u32Pair1Source, uint32_t u32Pair2Source)
| Dynamic Tamper Detect. More...
void | RTC_DynamicTamperDisable (uint32_t u32PairSel)
| Dynamic Tamper Disable. More...
void | RTC_DynamicTamperConfig (uint32_t u32ChangeRate, uint32_t u32SeedReload, uint32_t u32RefPattern, uint32_t u32Seed)
| Config dynamic tamper. More...

## Detailed Description

M480 series RTC driver source file.

Version
  V3.00 SPDX-License-Identifier: Apache-2.0

Copyright
  (C) 2016-2020 Nuvoton Technology Corp. All rights reserved.

Definition in file rtc.c.