| M480 BSP V3.05.001 The Board Support Package for M480 Series

Macros
HSOTG Exported Constants
Standard Driver » HSOTG Driver

## Macros
#define | HSOTG_VBUS_EN_ACTIVE_HIGH
#define | HSOTG_VBUS_EN_ACTIVE_LOW
#define | HSOTG_VBUS_ST_VALID_HIGH
#define | HSOTG_VBUS_ST_VALID_LOW

## Detailed Description

## Macro Definition Documentation

## ◆ HSOTG_VBUS_EN_ACTIVE_HIGH

#define HSOTG_VBUS_EN_ACTIVE_HIGH

USB VBUS power switch enable signal is active high.

Definition at line 36 of file hsotg.h.

## ◆ HSOTG_VBUS_EN_ACTIVE_LOW

#define HSOTG_VBUS_EN_ACTIVE_LOW

USB VBUS power switch enable signal is active low.

Definition at line 37 of file hsotg.h.

## ◆ HSOTG_VBUS_ST_VALID_HIGH

#define HSOTG_VBUS_ST_VALID_HIGH

USB VBUS power switch valid status is high.

Definition at line 38 of file hsotg.h.

## ◆ HSOTG_VBUS_ST_VALID_LOW

#define HSOTG_VBUS_ST_VALID_LOW

USB VBUS power switch valid status is low.

Definition at line 39 of file hsotg.h.