CMSIS-Driver: CAN Control Codes

| CMSIS-Driver Version 2.04 Peripheral Interface for Middleware and Application Code

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Content
CAN Control Codes
CAN Interface

Codes to configure the CAN driver. More...

## Content
| CAN Identifier
| Set object to standard or extended.
| CAN Operation Codes
| Set CAN operation modes.
| CAN Bus Communication Mode
| Set or initialize the CAN bus.
| CAN Bit Timing Codes
| Set bit timing.
| CAN Filter Operation Codes
| Set CAN filter manipulation codes.
| CAN Object Configuration Codes
| CAN Object Configuration codes.

## Description

Codes to configure the CAN driver.

The various CAN control codes define:

- CAN Identifier specify CAN identifier. Refer to ARM_CAN_ObjectConfigure.
- CAN Operation Codes control CAN interface operation. Refer to ARM_CAN_Control.
- CAN Bit Timing Codes specify CAN bit rate and timing. Refer to ARM_CAN_SetBitrate.
- CAN Bus Communication Mode specify CAN bus operating mode. Refer to ARM_CAN_SetMode.
- CAN Filter Operation Codes specify CAN filter operations. Refer to ARM_CAN_ObjectSetFilter.
- CAN Object Configuration Codes specify CAN object configuration modes. Refer to ARM_CAN_ObjectConfigure.