CMSIS-RTOS RTX: Revision History

| CMSIS-RTOS RTX Version 4.80 CMSIS-RTOS RTX: Real-Time Operating System for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Revision History

Version | Description
--- | ---
V4.80 | Restored time delay parameter 'millisec' old behavior (before V4.79) for software compatibility. Corrected: implicit mutex release when mutex owner thread is terminated.
V4.79 | Corrected: time delay parameter ‘millisec’ in all functions (osDelay, osSignalWait, …) is now treated as lower bound – wait for at least time given (before it could have been up to 1ms less). Corrected: Lazy Context switching for Cortex-M4 with FPU could lead to a crash when thread which used FPU was terminated. Corrected: osMailCAlloc only cleared the allocated memory block if it was available without waiting. Corrected: osThreadCreate function returns NULL when trying to create more concurrent threads than defined in the configuration. Improved source code MISRA compliance.
V4.78 | Corrected: osTimerStart function accepts full 32-bit range for time delay value in milisec. Added: User Timer Callback Queue overflow reported through os_error(OS_ERROR_TIMER_OVF).
V4.77 | Added: Stack usage watermark.
V4.76 | Optimized Service calls in GCC libraries. Corrected: Stack/Heap regions can be used with scatter loading.
V4.75 | Corrected: Service calls for Cortex-M4 with Floating Point for GCC. Corrected: osSignalClear returns 0x80000000 when called from interrupt service routines. Corrected: C standard library memory functions (malloc, free, ...) can be called between calls to osKernelInitialize and osKernelStart. Corrected: Interrupt Priority Group can be configured between calls to osKernelInitialize and osKernelStart.
V4.74 | Corrected: osKernelInitialize and osKernelStart when called from main which is already a thread.
V4.73 | Corrected: mutex priority inversion when thread owns more than one mutex. Added: RTX extensions os_suspend and os_resume. Added: RTX os_error template.
V4.72 | Corrected: object initialization when defined inside function (allocated on stack and not as static memory).
V4.71 | Corrected: osMailFree behaviour when osMailAlloc timed out.
V4.70 | Added: New control functions for short timeouts in microsecond resolution osKernelSysTick, osKernelSysTickFrequency, osKernelSysTickMicroSec. Removed: osSignalGet.
V4.61 | Enhanced: osTimerCreate can now be called after osKernelInitialize (before only after osKernelStart). Corrected: Initialization of alternative kernel timer for Cortex-M0/M0+/M1 (when SysTick timer is not used). Corrected: Message/Mail Queue behavior when timeout expires.
V4.51 | Corrected: problem with osKernelInitialize when after the call high priority threads are defined.
V4.50 | Based on CMSIS-RTOS API Version 1.01 and the classic RTX V4.50 Kernel. Added: osTimerDelete, osMutexDelete, osSemaphoreDelete. Added: osKernelInitialize that prepares the Kernel for object creation. Added: support for Low Power Cortex-M applications based on new configuration functions: os_suspend, os_resume. Added: support for peripheral timer to be used as OS tick timer instead of Core SysTick timer. Corrected: stack checking did not work for os_tsk_delete_self function Preview Release.
V4.20 | Initial CMSIS-RTOS adaption of the RTX Kernel.