CMSIS-DAP: JTAG Commands

| CMSIS-DAP Version 1.1.0 Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
Content
JTAG Commands
CMSIS-DAP Commands

Detect and configure the JTAG device chain. More...

## Content
| DAP_JTAG_Sequence
| Generate JTAG sequence TMS,TDI and capture TDO.
| DAP_JTAG_Configure
| Configure JTAG Chain.
| DAP_JTAG_IDCODE
| Read JTAG IDCODE.

## Description

Detect and configure the JTAG device chain.

The JTAG Commands allow to:

- Detect the devices connect to the JTAG chain.
- Configure the IR register length of each device on the JTAG chain.
- Read the JTAG IDCODE value of each device on the JTAG chain.