CMSIS-DAP: DAP_JTAG_Configure

| CMSIS-DAP Version 1.1.0 Interface Firmware for CoreSight Debug Access Port

- Main Page
- Usage and Description
- Reference

All Functions Groups Pages
DAP_JTAG_Configure
JTAG Commands

Configure JTAG Chain. More...

Configure JTAG Chain.

The DAP_JTAG_Configure Command sets the JTAG device chain information for communication with Transfer Commands. The JTAG device chain needs to be iterated with DAP_JTAG_Sequence or manually configured by the debugger on the host computer.

DAP_JTAG_Configure Command:

BYTE | BYTE *| BYTE *****|
> 0x15 | Count | IR Length |
******|*******|+++++++++++|

- Count: Number of devices in chain
- IR Length: JTAG IR register length (in bits) for each device.

DAP_JTAG_Configure Response:

BYTE | BYTE **|
< 0x15 | Status |
******|********|

- Status: Response Status