CMSIS-RTOS RTX: Technical Data

| CMSIS-RTOS RTX Version 4.80 CMSIS-RTOS RTX: Real-Time Operating System for Cortex-M processor-based devices

- Main Page
- Usage and Description
- Reference

All Data Structures Files Functions Variables Typedefs Enumerations Enumerator Macros Groups Pages
Technical Data

This section lists the technical data of CMSIS-RTOS RTX.

Description | Limitations
--- | ---
Defined Tasks | Unlimited
Active Threads | 250 max
Mailboxes | Unlimited
Semaphores | Unlimited
Mutexes | Unlimited
Signals | 16 per thread
Timer Callbacks | Unlimited
Code Space | < 5.0 Kbytes
RAM Space for Kernel | 300 bytes + 128 bytes Main Stack
RAM Space for a Thread | StackSize + 52 bytes
RAM Space for a Mailbox | MaxMessages * 4 + 16 bytes
RAM Space for a Semaphore | 8 bytes
RAM Space for a Mutex | 12 bytes
RAM Space for a User Timer | 24 bytes
Hardware Requirements | SysTick timer or other hardware timer
Thread context switch time | < 2.6 usec @ 72 MHz
Interrupt lockout time | Not disabled

Note
  - Unlimited means that the RTX kernel does not impose any limitations on the number. However, the available system memory resources limit the number of items you can create.
  - RAM requirements depend on the number of concurrently running threads.
  - The code and RAM size is calculated for ARMCC Compiler when using the MicroLib runtime library.

# osWait

The generic wait function osWait is currently not supported by CMSIS-RTOS RTX.