| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches
Data Structures
Here are the data structures with brief descriptions:

C ARM_CAN_CAPABILITIES | CAN Device Driver Capabilities
C ARM_CAN_MSG_INFO | CAN Message Information
C ARM_CAN_OBJ_CAPABILITIES | CAN Object Capabilities
C ARM_CAN_STATUS | CAN Status
C ARM_DRIVER_CAN | Access structure of the CAN Driver
C ARM_DRIVER_ETH_MAC | Access structure of the Ethernet MAC Driver
C ARM_DRIVER_ETH_PHY | Access structure of the Ethernet PHY Driver
C ARM_DRIVER_FLASH | Access structure of the Flash Driver
C ARM_DRIVER_GPIO | Access structure of the GPIO Driver
C ARM_DRIVER_I2C | Access structure of the I2C Driver
C ARM_DRIVER_MCI | Access structure of the MCI Driver
C ARM_DRIVER_NAND | Access structure of the NAND Driver
C ARM_DRIVER_SAI | Access structure of the SAI Driver
C ARM_DRIVER_SPI | Access structure of the SPI Driver
C ARM_DRIVER_STORAGE |
C ARM_DRIVER_USART | Access structure of the USART Driver
C ARM_DRIVER_USBD | Access structure of the USB Device Driver
C ARM_DRIVER_USBH | Access structure of USB Host Driver
C ARM_DRIVER_USBH_HCI | Access structure of USB Host HCI (OHCI/EHCI) Driver
C ARM_DRIVER_VERSION | Driver Version
C ARM_DRIVER_WIFI | Access structure of the WiFi Driver
C ARM_ETH_LINK_INFO | Ethernet link information
C ARM_ETH_MAC_ADDR | Ethernet MAC Address
C ARM_ETH_MAC_CAPABILITIES | Ethernet MAC Capabilities
C ARM_ETH_MAC_TIME | Ethernet MAC Time
C ARM_FLASH_CAPABILITIES | Flash Driver Capabilities
C ARM_FLASH_INFO | Flash information
C ARM_FLASH_SECTOR | Flash Sector information
C ARM_FLASH_STATUS | Flash Status
C ARM_I2C_CAPABILITIES | I2C Driver Capabilities
C ARM_I2C_STATUS | I2C Status
C ARM_MCI_CAPABILITIES | MCI Driver Capabilities
C ARM_MCI_STATUS | MCI Status
C ARM_NAND_CAPABILITIES | NAND Driver Capabilities
C ARM_NAND_ECC_INFO | NAND ECC (Error Correction Code) Information
C ARM_NAND_STATUS | NAND Status
C ARM_SAI_CAPABILITIES | SAI Driver Capabilities
C ARM_SAI_STATUS | SAI Status
C ARM_SPI_CAPABILITIES | SPI Driver Capabilities
C ARM_SPI_STATUS | SPI Status
C ARM_STORAGE_BLOCK | A storage block is a range of memory with uniform attributes
C ARM_STORAGE_BLOCK_ATTRIBUTES | Attributes of the storage range within a storage block
C ARM_STORAGE_CAPABILITIES | Storage Driver API Capabilities
C ARM_STORAGE_INFO |
C ARM_STORAGE_SECURITY_FEATURES |
C ARM_STORAGE_STATUS | Operating status of the storage controller
C ARM_USART_CAPABILITIES | USART Device Driver Capabilities
C ARM_USART_MODEM_STATUS | USART Modem Status
C ARM_USART_STATUS | USART Status
C ARM_USBD_CAPABILITIES | USB Device Driver Capabilities
C ARM_USBD_STATE | USB Device State
C ARM_USBH_CAPABILITIES | USB Host Driver Capabilities
C ARM_USBH_HCI_CAPABILITIES | USB Host HCI (OHCI/EHCI) Driver Capabilities
C ARM_USBH_PORT_STATE | USB Host Port State
C ARM_WIFI_CAPABILITIES | WiFi Driver Capabilities
C ARM_WIFI_CONFIG_t | WiFi Configuration
C ARM_WIFI_NET_INFO_t | WiFi Network Information
C ARM_WIFI_SCAN_INFO_t | WiFi Scan Information