| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches

### - d -

- data_lost : ARM_SPI_STATUS
- data_width : ARM_FLASH_CAPABILITIES
- data_width_16 : ARM_NAND_CAPABILITIES
- data_width_4 : ARM_MCI_CAPABILITIES
- data_width_4_ddr : ARM_MCI_CAPABILITIES
- data_width_8 : ARM_MCI_CAPABILITIES
- data_width_8_ddr : ARM_MCI_CAPABILITIES
- dcd : ARM_USART_CAPABILITIES, ARM_USART_MODEM_STATUS
- ddr : ARM_NAND_CAPABILITIES
- ddr2 : ARM_NAND_CAPABILITIES
- ddr2_timing_mode : ARM_NAND_CAPABILITIES
- ddr_timing_mode : ARM_NAND_CAPABILITIES
- Deactivate : ARM_DRIVER_WIFI
- DeviceConnect : ARM_DRIVER_USBD
- DeviceDisconnect : ARM_DRIVER_USBD
- DeviceGetState : ARM_DRIVER_USBD
- DevicePower : ARM_DRIVER_NAND
- DeviceRemoteWakeup : ARM_DRIVER_USBD
- DeviceSetAddress : ARM_DRIVER_USBD
- direction : ARM_I2C_STATUS
- dlc : ARM_CAN_MSG_INFO
- driver_strength_18 : ARM_NAND_CAPABILITIES
- driver_strength_25 : ARM_NAND_CAPABILITIES
- driver_strength_50 : ARM_NAND_CAPABILITIES
- drv : ARM_DRIVER_VERSION
- dsr : ARM_USART_CAPABILITIES, ARM_USART_MODEM_STATUS
- dtr : ARM_USART_CAPABILITIES
- duplex : ARM_ETH_LINK_INFO