| CMSIS-Driver Peripheral Interface for Middleware and Application Code |

Loading...
Searching...
No Matches

### - p -

- page_count : ARM_NAND_ECC_INFO
- page_layout : ARM_NAND_ECC_INFO
- page_size : ARM_FLASH_INFO, ARM_NAND_ECC_INFO
- pass : ARM_WIFI_CONFIG_t, ARM_WIFI_NET_INFO_t
- PHY_Read : ARM_DRIVER_ETH_MAC
- PHY_Write : ARM_DRIVER_ETH_MAC
- Ping : ARM_DRIVER_WIFI
- ping : ARM_WIFI_CAPABILITIES
- PipeCreate : ARM_DRIVER_USBH
- PipeDelete : ARM_DRIVER_USBH
- PipeModify : ARM_DRIVER_USBH
- PipeReset : ARM_DRIVER_USBH
- PipeTransfer : ARM_DRIVER_USBH
- PipeTransferAbort : ARM_DRIVER_USBH
- PipeTransferGetResult : ARM_DRIVER_USBH
- port_mask : ARM_USBH_CAPABILITIES, ARM_USBH_HCI_CAPABILITIES
- PortGetState : ARM_DRIVER_USBH
- PortReset : ARM_DRIVER_USBH
- PortResume : ARM_DRIVER_USBH
- PortSuspend : ARM_DRIVER_USBH
- PortVbusOnOff : ARM_DRIVER_USBH, ARM_DRIVER_USBH_HCI
- PowerControl : ARM_DRIVER_CAN, ARM_DRIVER_ETH_MAC, ARM_DRIVER_ETH_PHY, ARM_DRIVER_FLASH, ARM_DRIVER_I2C, ARM_DRIVER_MCI, ARM_DRIVER_NAND, ARM_DRIVER_SAI, ARM_DRIVER_SPI, ARM_DRIVER_STORAGE, ARM_DRIVER_USART, ARM_DRIVER_USBD, ARM_DRIVER_USBH, ARM_DRIVER_USBH_HCI, ARM_DRIVER_WIFI
- precision_timer : ARM_ETH_MAC_CAPABILITIES
- program_cycles : ARM_STORAGE_INFO
- program_unit : ARM_FLASH_INFO, ARM_STORAGE_INFO
- ProgramData : ARM_DRIVER_FLASH, ARM_DRIVER_STORAGE
- programmability : ARM_STORAGE_INFO
- programmable : ARM_STORAGE_BLOCK_ATTRIBUTES
- protectable : ARM_STORAGE_BLOCK_ATTRIBUTES
- protection_unit : ARM_STORAGE_BLOCK_ATTRIBUTES
- protocol_ac97 : ARM_SAI_CAPABILITIES
- protocol_i2s : ARM_SAI_CAPABILITIES
- protocol_justified : ARM_SAI_CAPABILITIES
- protocol_pcm : ARM_SAI_CAPABILITIES
- protocol_user : ARM_SAI_CAPABILITIES