| MINI51DE_BSP V3.02.004 The Board Support Package for Mini51DE Series MCU

Data Structures | Macros | Typedefs | Enumerations
Mini51Series.h File Reference

Mini51 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Mini51 series MCU. More...

`#include "core_cm0.h"`
`#include "system_Mini51Series.h"`
`#include <stdint.h>`
`#include "sys.h"`
`#include "clk.h"`
`#include "acmp.h"`
`#include "adc.h"`
`#include "fmc.h"`
`#include "gpio.h"`
`#include "i2c.h"`
`#include "pwm.h"`
`#include "spi.h"`
`#include "timer.h"`
`#include "uart.h"`
`#include "wdt.h"`
Include dependency graph for Mini51Series.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | ACMP_T
struct | ADC_T
struct | CLK_T
struct | FMC_T
struct | GCR_T
struct | GPIO_T
struct | GPIO_DBNCECON_T
| GPIO debounce register map. More...
struct | I2C_T
struct | INT_T
struct | PWM_T
struct | SPI_T
struct | TIMER_T
struct | UART_T
struct | WDT_T

## Macros
#define | __CM0_REV 0x0201
#define | __NVIC_PRIO_BITS 2
#define | __Vendor_SysTickConfig 0
#define | __MPU_PRESENT 0
#define | __FPU_PRESENT 0
#define | FLASH_BASE ((uint32_t)0x00000000)
| Flash base address. More...
#define | SRAM_BASE ((uint32_t)0x20000000)
| SRAM base address. More...
#define | APB1PERIPH_BASE ((uint32_t)0x40000000)
| APB1 base address. More...
#define | APB2PERIPH_BASE ((uint32_t)0x40100000)
| APB2 base address. More...
#define | AHBPERIPH_BASE ((uint32_t)0x50000000)
| AHB base address. More...
#define | WDT_BASE (APB1PERIPH_BASE + 0x04000)
| WDT register base address. More...
#define | TIMER0_BASE (APB1PERIPH_BASE + 0x10000)
| TIMER0 register base address. More...
#define | TIMER1_BASE (APB1PERIPH_BASE + 0x10020)
| TIMER1 register base address. More...
#define | I2C_BASE (APB1PERIPH_BASE + 0x20000)
| I2C register base address. More...
#define | SPI_BASE (APB1PERIPH_BASE + 0x30000)
| SPI register base address. More...
#define | PWM_BASE (APB1PERIPH_BASE + 0x40000)
| PWM register base address. More...
#define | UART_BASE (APB1PERIPH_BASE + 0x50000)
| UART register base address. More...
#define | ACMP_BASE (APB1PERIPH_BASE + 0xD0000)
| ACMP register base address. More...
#define | ADC_BASE (APB1PERIPH_BASE + 0xE0000)
| ADC register base address. More...
#define | GCR_BASE (AHBPERIPH_BASE + 0x00000)
| GCR register base address. More...
#define | CLK_BASE (AHBPERIPH_BASE + 0x00200)
| CLK register base address. More...
#define | INT_BASE (AHBPERIPH_BASE + 0x00300)
| INT register base address. More...
#define | P0_BASE (AHBPERIPH_BASE + 0x04000)
| GPIO Port 0 register base address. More...
#define | P1_BASE (AHBPERIPH_BASE + 0x04040)
| GPIO Port 1 register base address. More...
#define | P2_BASE (AHBPERIPH_BASE + 0x04080)
| GPIO Port 2 register base address. More...
#define | P3_BASE (AHBPERIPH_BASE + 0x040C0)
| GPIO Port 3 register base address. More...
#define | P4_BASE (AHBPERIPH_BASE + 0x04100)
| GPIO Port 4 register base address. More...
#define | P5_BASE (AHBPERIPH_BASE + 0x04140)
| GPIO Port 5 register base address. More...
#define | GPIO_DBNCECON_BASE (AHBPERIPH_BASE + 0x04180)
| GPIO De-bounce register vase. More...
#define | GPIO_PIN_DATA_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO pin data register base address. More...
#define | GPIOBIT0_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO Port 0 bit access register base address. More...
#define | GPIOBIT1_BASE (AHBPERIPH_BASE + 0x04220)
| GPIO Port 1 bit access register base address. More...
#define | GPIOBIT2_BASE (AHBPERIPH_BASE + 0x04240)
| GPIO Port 2 bit access register base address. More...
#define | GPIOBIT3_BASE (AHBPERIPH_BASE + 0x04260)
| GPIO Port 3 bit access register base address. More...
#define | GPIOBIT4_BASE (AHBPERIPH_BASE + 0x04280)
| GPIO Port 4 bit access register base address. More...
#define | GPIOBIT5_BASE (AHBPERIPH_BASE + 0x042A0)
| GPIO Port 5 bit access register base address. More...
#define | FMC_BASE (AHBPERIPH_BASE + 0x0C000)
| FMC register base address. More...
#define | WDT ((WDT_T *) WDT_BASE)
| Pointer to WDT register structure. More...
#define | TIMER0 ((TIMER_T *) TIMER0_BASE)
| Pointer to Timer 0 register structure. More...
#define | TIMER1 ((TIMER_T *) TIMER1_BASE)
| Pointer to Timer 1 register structure. More...
#define | I2C ((I2C_T *) I2C_BASE)
| Pointer to I2C register structure. More...
#define | I2C0 ((I2C_T *) I2C_BASE)
| Pointer to I2C register structure. More...
#define | SPI ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | SPI0 ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | PWM ((PWM_T *) PWM_BASE)
| Pointer to PWM register structure. More...
#define | UART ((UART_T *) UART_BASE)
| Pointer to UART register structure. More...
#define | UART0 ((UART_T *) UART_BASE)
| Pointer to UART register structure. More...
#define | ADC ((ADC_T *) ADC_BASE)
| Pointer to ADC register structure. More...
#define | ACMP ((ACMP_T *) ACMP_BASE)
| Pointer to ACMP register structure. More...
#define | SYS ((GCR_T *) GCR_BASE)
| Pointer to SYS register structure. More...
#define | CLK ((CLK_T *) CLK_BASE)
| Pointer to CLK register structure. More...
#define | INT ((INT_T *) INT_BASE)
| Pointer to INT register structure. More...
#define | P0 ((GPIO_T *) P0_BASE)
| Pointer to GPIO port 0 register structure. More...
#define | P1 ((GPIO_T *) P1_BASE)
| Pointer to GPIO port 1 register structure. More...
#define | P2 ((GPIO_T *) P2_BASE)
| Pointer to GPIO port 2 register structure. More...
#define | P3 ((GPIO_T *) P3_BASE)
| Pointer to GPIO port 3 register structure. More...
#define | P4 ((GPIO_T *) P4_BASE)
| Pointer to GPIO port 4 register structure. More...
#define | P5 ((GPIO_T *) P5_BASE)
| Pointer to GPIO port 5 register structure. More...
#define | GPIO ((GPIO_DBNCECON_T *) GPIO_DBNCECON_BASE)
| Pointer to GPIO de-bounce register structure. More...
#define | FMC ((FMC_T *) FMC_BASE)
| Pointer to FMC register structure. More...
#define | M8(addr) (*((vu8 *) (addr)))
| Get a 8-bit unsigned value from specified address. More...
#define | M16(addr) (*((vu16 *) (addr)))
| Get a 16-bit unsigned value from specified address. More...
#define | M32(addr) (*((vu32 *) (addr)))
| Get a 32-bit unsigned value from specified address. More...
#define | outpw(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inpw(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outps(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inps(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outpb(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inpb(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | outp32(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inp32(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outp16(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inp16(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outp8(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inp8(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | NULL (0)
| NULL pointer. More...
#define | TRUE (1)
| Boolean true, define to use in API parameters or return value. More...
#define | FALSE (0)
| Boolean false, define to use in API parameters or return value. More...
#define | ENABLE (1)
| Enable, define to use in API parameters. More...
#define | DISABLE (0)
| Disable, define to use in API parameters. More...
#define | BIT0 (0x00000001)
| Bit 0 mask of an 32 bit integer. More...
#define | BIT1 (0x00000002)
| Bit 1 mask of an 32 bit integer. More...
#define | BIT2 (0x00000004)
| Bit 2 mask of an 32 bit integer. More...
#define | BIT3 (0x00000008)
| Bit 3 mask of an 32 bit integer. More...
#define | BIT4 (0x00000010)
| Bit 4 mask of an 32 bit integer. More...
#define | BIT5 (0x00000020)
| Bit 5 mask of an 32 bit integer. More...
#define | BIT6 (0x00000040)
| Bit 6 mask of an 32 bit integer. More...
#define | BIT7 (0x00000080)
| Bit 7 mask of an 32 bit integer. More...
#define | BIT8 (0x00000100)
| Bit 8 mask of an 32 bit integer. More...
#define | BIT9 (0x00000200)
| Bit 9 mask of an 32 bit integer. More...
#define | BIT10 (0x00000400)
| Bit 10 mask of an 32 bit integer. More...
#define | BIT11 (0x00000800)
| Bit 11 mask of an 32 bit integer. More...
#define | BIT12 (0x00001000)
| Bit 12 mask of an 32 bit integer. More...
#define | BIT13 (0x00002000)
| Bit 13 mask of an 32 bit integer. More...
#define | BIT14 (0x00004000)
| Bit 14 mask of an 32 bit integer. More...
#define | BIT15 (0x00008000)
| Bit 15 mask of an 32 bit integer. More...
#define | BIT16 (0x00010000)
| Bit 16 mask of an 32 bit integer. More...
#define | BIT17 (0x00020000)
| Bit 17 mask of an 32 bit integer. More...
#define | BIT18 (0x00040000)
| Bit 18 mask of an 32 bit integer. More...
#define | BIT19 (0x00080000)
| Bit 19 mask of an 32 bit integer. More...
#define | BIT20 (0x00100000)
| Bit 20 mask of an 32 bit integer. More...
#define | BIT21 (0x00200000)
| Bit 21 mask of an 32 bit integer. More...
#define | BIT22 (0x00400000)
| Bit 22 mask of an 32 bit integer. More...
#define | BIT23 (0x00800000)
| Bit 23 mask of an 32 bit integer. More...
#define | BIT24 (0x01000000)
| Bit 24 mask of an 32 bit integer. More...
#define | BIT25 (0x02000000)
| Bit 25 mask of an 32 bit integer. More...
#define | BIT26 (0x04000000)
| Bit 26 mask of an 32 bit integer. More...
#define | BIT27 (0x08000000)
| Bit 27 mask of an 32 bit integer. More...
#define | BIT28 (0x10000000)
| Bit 28 mask of an 32 bit integer. More...
#define | BIT29 (0x20000000)
| Bit 29 mask of an 32 bit integer. More...
#define | BIT30 (0x40000000)
| Bit 30 mask of an 32 bit integer. More...
#define | BIT31 (0x80000000)
| Bit 31 mask of an 32 bit integer. More...
#define | BYTE0_Msk (0x000000FF)
| Mask to get bit0~bit7 from a 32 bit integer. More...
#define | BYTE1_Msk (0x0000FF00)
| Mask to get bit8~bit15 from a 32 bit integer. More...
#define | BYTE2_Msk (0x00FF0000)
| Mask to get bit16~bit23 from a 32 bit integer. More...
#define | BYTE3_Msk (0xFF000000)
| Mask to get bit24~bit31 from a 32 bit integer. More...
#define | GET_BYTE0(u32Param) ((u32Param & BYTE0_Msk) )
#define | GET_BYTE1(u32Param) ((u32Param & BYTE1_Msk) >> 8)
#define | GET_BYTE2(u32Param) ((u32Param & BYTE2_Msk) >> 16)
#define | GET_BYTE3(u32Param) ((u32Param & BYTE3_Msk) >> 24)
#define | ACMP_CMPCR_ACMPEN_Pos (0)
#define | ACMP_CMPCR_ACMPEN_Msk (0x1ul << ACMP_CMPCR_ACMPEN_Pos)
#define | ACMP_CMPCR_ACMPIE_Pos (1)
#define | ACMP_CMPCR_ACMPIE_Msk (0x1ul << ACMP_CMPCR_ACMPIE_Pos)
#define | ACMP_CMPCR_HYSEN_Pos (2)
#define | ACMP_CMPCR_HYSEN_Msk (0x1ul << ACMP_CMPCR_HYSEN_Pos)
#define | ACMP_CMPCR_NEGSEL_Pos (4)
#define | ACMP_CMPCR_NEGSEL_Msk (0x1ul << ACMP_CMPCR_NEGSEL_Pos)
#define | ACMP_CMPCR_RISING_Pos (8)
#define | ACMP_CMPCR_RISING_Msk (0x1ul << ACMP_CMPCR_RISING_Pos)
#define | ACMP_CMPCR_FALLING_Pos (9)
#define | ACMP_CMPCR_FALLING_Msk (0x1ul << ACMP_CMPCR_FALLING_Pos)
#define | ACMP_CMPCR_CPPSEL_Pos (29)
#define | ACMP_CMPCR_CPPSEL_Msk (0x3ul << ACMP_CMPCR_CPPSEL_Pos)
#define | ACMP_CMPSR_ACMPF0_Pos (0)
#define | ACMP_CMPSR_ACMPF0_Msk (0x1ul << ACMP_CMPSR_ACMPF0_Pos)
#define | ACMP_CMPSR_ACMPF1_Pos (1)
#define | ACMP_CMPSR_ACMPF1_Msk (0x1ul << ACMP_CMPSR_ACMPF1_Pos)
#define | ACMP_CMPSR_ACMPCO0_Pos (2)
#define | ACMP_CMPSR_ACMPCO0_Msk (0x1ul << ACMP_CMPSR_ACMPCO0_Pos)
#define | ACMP_CMPSR_ACMPCO1_Pos (3)
#define | ACMP_CMPSR_ACMPCO1_Msk (0x1ul << ACMP_CMPSR_ACMPCO1_Pos)
#define | ACMP_CMPRVCR_CRVS_Pos (0)
#define | ACMP_CMPRVCR_CRVS_Msk (0xful << ACMP_CMPRVCR_CRVS_Pos)
#define | ACMP_CMPRVCR_OUT_SEL_Pos (7)
#define | ACMP_CMPRVCR_OUT_SEL_Msk (0x1ul << ACMP_CMPRVCR_OUT_SEL_Pos)
#define | ADC_ADDR_RSLT_Pos (0)
#define | ADC_ADDR_RSLT_Msk (0x3fful << ADC_ADDR_RSLT_Pos)
#define | ADC_ADDR_OVERRUN_Pos (16)
#define | ADC_ADDR_OVERRUN_Msk (0x1ul << ADC_ADDR_OVERRUN_Pos)
#define | ADC_ADDR_VALID_Pos (17)
#define | ADC_ADDR_VALID_Msk (0x1ul << ADC_ADDR_VALID_Pos)
#define | ADC_ADCR_ADEN_Pos (0)
#define | ADC_ADCR_ADEN_Msk (0x1ul << ADC_ADCR_ADEN_Pos)
#define | ADC_ADCR_ADIE_Pos (1)
#define | ADC_ADCR_ADIE_Msk (0x1ul << ADC_ADCR_ADIE_Pos)
#define | ADC_ADCR_TRGS_Pos (4)
#define | ADC_ADCR_TRGS_Msk (0x3ul << ADC_ADCR_TRGS_Pos)
#define | ADC_ADCR_TRGCOND_Pos (6)
#define | ADC_ADCR_TRGCOND_Msk (0x1ul << ADC_ADCR_TRGCOND_Pos)
#define | ADC_ADCR_TRGEN_Pos (8)
#define | ADC_ADCR_TRGEN_Msk (0x1ul << ADC_ADCR_TRGEN_Pos)
#define | ADC_ADCR_ADST_Pos (11)
#define | ADC_ADCR_ADST_Msk (0x1ul << ADC_ADCR_ADST_Pos)
#define | ADC_ADCHER_CHEN_Pos (0)
#define | ADC_ADCHER_CHEN_Msk (0xfful << ADC_ADCHER_CHEN_Pos)
#define | ADC_ADCHER_CHEN0_Pos (0)
#define | ADC_ADCHER_CHEN0_Msk (0x1ul << ADC_ADCHER_CHEN0_Pos)
#define | ADC_ADCHER_CHEN1_Pos (1)
#define | ADC_ADCHER_CHEN1_Msk (0x1ul << ADC_ADCHER_CHEN1_Pos)
#define | ADC_ADCHER_CHEN2_Pos (2)
#define | ADC_ADCHER_CHEN2_Msk (0x1ul << ADC_ADCHER_CHEN2_Pos)
#define | ADC_ADCHER_CHEN3_Pos (3)
#define | ADC_ADCHER_CHEN3_Msk (0x1ul << ADC_ADCHER_CHEN3_Pos)
#define | ADC_ADCHER_CHEN4_Pos (4)
#define | ADC_ADCHER_CHEN4_Msk (0x1ul << ADC_ADCHER_CHEN4_Pos)
#define | ADC_ADCHER_CHEN5_Pos (5)
#define | ADC_ADCHER_CHEN5_Msk (0x1ul << ADC_ADCHER_CHEN5_Pos)
#define | ADC_ADCHER_CHEN6_Pos (6)
#define | ADC_ADCHER_CHEN6_Msk (0x1ul << ADC_ADCHER_CHEN6_Pos)
#define | ADC_ADCHER_CHEN7_Pos (7)
#define | ADC_ADCHER_CHEN7_Msk (0x1ul << ADC_ADCHER_CHEN7_Pos)
#define | ADC_ADCHER_PRESEL_Pos (8)
#define | ADC_ADCHER_PRESEL_Msk (0x1ul << ADC_ADCHER_PRESEL_Pos)
#define | ADC_ADCMPR_CMPEN_Pos (0)
#define | ADC_ADCMPR_CMPEN_Msk (0x1ul << ADC_ADCMPR_CMPEN_Pos)
#define | ADC_ADCMPR_CMPIE_Pos (1)
#define | ADC_ADCMPR_CMPIE_Msk (0x1ul << ADC_ADCMPR_CMPIE_Pos)
#define | ADC_ADCMPR_CMPCOND_Pos (2)
#define | ADC_ADCMPR_CMPCOND_Msk (0x1ul << ADC_ADCMPR_CMPCOND_Pos)
#define | ADC_ADCMPR_CMPCH_Pos (3)
#define | ADC_ADCMPR_CMPCH_Msk (0x7ul << ADC_ADCMPR_CMPCH_Pos)
#define | ADC_ADCMPR_CMPMATCNT_Pos (8)
#define | ADC_ADCMPR_CMPMATCNT_Msk (0xful << ADC_ADCMPR_CMPMATCNT_Pos)
#define | ADC_ADCMPR_CMPD_Pos (16)
#define | ADC_ADCMPR_CMPD_Msk (0x3fful << ADC_ADCMPR_CMPD_Pos)
#define | ADC_ADSR_ADF_Pos (0)
#define | ADC_ADSR_ADF_Msk (0x1ul << ADC_ADSR_ADF_Pos)
#define | ADC_ADSR_CMPF0_Pos (1)
#define | ADC_ADSR_CMPF0_Msk (0x1ul << ADC_ADSR_CMPF0_Pos)
#define | ADC_ADSR_CMPF1_Pos (2)
#define | ADC_ADSR_CMPF1_Msk (0x1ul << ADC_ADSR_CMPF1_Pos)
#define | ADC_ADSR_BUSY_Pos (3)
#define | ADC_ADSR_BUSY_Msk (0x1ul << ADC_ADSR_BUSY_Pos)
#define | ADC_ADSR_CHANNEL_Pos (4)
#define | ADC_ADSR_CHANNEL_Msk (0x7ul << ADC_ADSR_CHANNEL_Pos)
#define | ADC_ADSR_VALID_Pos (8)
#define | ADC_ADSR_VALID_Msk (0x1ul << ADC_ADSR_VALID_Pos)
#define | ADC_ADSR_OVERRUN_Pos (16)
#define | ADC_ADSR_OVERRUN_Msk (0x1ul << ADC_ADSR_OVERRUN_Pos)
#define | ADC_ADTDCR_PTDT_Pos (0)
#define | ADC_ADTDCR_PTDT_Msk (0xfful << ADC_ADTDCR_PTDT_Pos)
#define | ADC_ADSAMP_SAMPCNT_Pos (0)
#define | ADC_ADSAMP_SAMPCNT_Msk (0xful << ADC_ADSAMP_SAMPCNT_Pos)
#define | CLK_PWRCON_XTLCLK_EN_Pos (0)
#define | CLK_PWRCON_XTLCLK_EN_Msk (0x3ul << CLK_PWRCON_XTLCLK_EN_Pos)
#define | CLK_PWRCON_OSC22M_EN_Pos (2)
#define | CLK_PWRCON_OSC22M_EN_Msk (0x1ul << CLK_PWRCON_OSC22M_EN_Pos)
#define | CLK_PWRCON_IRC22M_EN_Pos (2)
#define | CLK_PWRCON_IRC22M_EN_Msk (0x1ul << CLK_PWRCON_IRC22M_EN_Pos)
#define | CLK_PWRCON_HIRC_EN_Pos (2)
#define | CLK_PWRCON_HIRC_EN_Msk (0x1ul << CLK_PWRCON_HIRC_EN_Pos)
#define | CLK_PWRCON_OSC10K_EN_Pos (3)
#define | CLK_PWRCON_OSC10K_EN_Msk (0x1ul << CLK_PWRCON_OSC10K_EN_Pos)
#define | CLK_PWRCON_IRC10K_EN_Pos (3)
#define | CLK_PWRCON_IRC10K_EN_Msk (0x1ul << CLK_PWRCON_IRC10K_EN_Pos)
#define | CLK_PWRCON_LIRC_EN_Pos (3)
#define | CLK_PWRCON_LIRC_EN_Msk (0x1ul << CLK_PWRCON_LIRC_EN_Pos)
#define | CLK_PWRCON_WU_DLY_Pos (4)
#define | CLK_PWRCON_WU_DLY_Msk (0x1ul << CLK_PWRCON_WU_DLY_Pos)
#define | CLK_PWRCON_WINT_EN_Pos (5)
#define | CLK_PWRCON_WINT_EN_Msk (0x1ul << CLK_PWRCON_WINT_EN_Pos)
#define | CLK_PWRCON_PD_WU_STS_Pos (6)
#define | CLK_PWRCON_PD_WU_STS_Msk (0x1ul << CLK_PWRCON_PD_WU_STS_Pos)
#define | CLK_PWRCON_PWR_DOWN_EN_Pos (7)
#define | CLK_PWRCON_PWR_DOWN_EN_Msk (0x1ul << CLK_PWRCON_PWR_DOWN_EN_Pos)
#define | CLK_PWRCON_PD_32K_Pos (9)
#define | CLK_PWRCON_PD_32K_Msk (0x1ul << CLK_PWRCON_PD_32K_Pos)
#define | CLK_AHBCLK_ISP_EN_Pos (2)
#define | CLK_AHBCLK_ISP_EN_Msk (0x1ul << CLK_AHBCLK_ISP_EN_Pos)
#define | CLK_APBCLK_WDT_EN_Pos (0)
#define | CLK_APBCLK_WDT_EN_Msk (0x1ul << CLK_APBCLK_WDT_EN_Pos)
#define | CLK_APBCLK_TMR0_EN_Pos (2)
#define | CLK_APBCLK_TMR0_EN_Msk (0x1ul << CLK_APBCLK_TMR0_EN_Pos)
#define | CLK_APBCLK_TMR1_EN_Pos (3)
#define | CLK_APBCLK_TMR1_EN_Msk (0x1ul << CLK_APBCLK_TMR1_EN_Pos)
#define | CLK_APBCLK_FDIV_EN_Pos (6)
#define | CLK_APBCLK_FDIV_EN_Msk (0x1ul << CLK_APBCLK_FDIV_EN_Pos)
#define | CLK_APBCLK_I2C_EN_Pos (8)
#define | CLK_APBCLK_I2C_EN_Msk (0x1ul << CLK_APBCLK_I2C_EN_Pos)
#define | CLK_APBCLK_SPI_EN_Pos (12)
#define | CLK_APBCLK_SPI_EN_Msk (0x1ul << CLK_APBCLK_SPI_EN_Pos)
#define | CLK_APBCLK_UART_EN_Pos (16)
#define | CLK_APBCLK_UART_EN_Msk (0x1ul << CLK_APBCLK_UART_EN_Pos)
#define | CLK_APBCLK_PWM01_EN_Pos (20)
#define | CLK_APBCLK_PWM01_EN_Msk (0x1ul << CLK_APBCLK_PWM01_EN_Pos)
#define | CLK_APBCLK_PWM23_EN_Pos (21)
#define | CLK_APBCLK_PWM23_EN_Msk (0x1ul << CLK_APBCLK_PWM23_EN_Pos)
#define | CLK_APBCLK_PWM45_EN_Pos (22)
#define | CLK_APBCLK_PWM45_EN_Msk (0x1ul << CLK_APBCLK_PWM45_EN_Pos)
#define | CLK_APBCLK_ADC_EN_Pos (28)
#define | CLK_APBCLK_ADC_EN_Msk (0x1ul << CLK_APBCLK_ADC_EN_Pos)
#define | CLK_APBCLK_CMP_EN_Pos (30)
#define | CLK_APBCLK_CMP_EN_Msk (0x1ul << CLK_APBCLK_CMP_EN_Pos)
#define | CLK_CLKSTATUS_XTL_STB_Pos (0)
#define | CLK_CLKSTATUS_XTL_STB_Msk (0x1ul << CLK_CLKSTATUS_XTL_STB_Pos)
#define | CLK_CLKSTATUS_HXT_STB_Pos (0)
#define | CLK_CLKSTATUS_HXT_STB_Msk (0x1ul << CLK_CLKSTATUS_HXT_STB_Pos)
#define | CLK_CLKSTATUS_LXT_STB_Pos (0)
#define | CLK_CLKSTATUS_LXT_STB_Msk (0x1ul << CLK_CLKSTATUS_LXT_STB_Pos)
#define | CLK_CLKSTATUS_OSC10K_STB_Pos (3)
#define | CLK_CLKSTATUS_OSC10K_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC10K_STB_Pos)
#define | CLK_CLKSTATUS_IRC10K_STB_Pos (3)
#define | CLK_CLKSTATUS_IRC10K_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC10K_STB_Pos)
#define | CLK_CLKSTATUS_LIRC_STB_Pos (3)
#define | CLK_CLKSTATUS_LIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_LIRC_STB_Pos)
#define | CLK_CLKSTATUS_OSC22M_STB_Pos (4)
#define | CLK_CLKSTATUS_OSC22M_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC22M_STB_Pos)
#define | CLK_CLKSTATUS_IRC22M_STB_Pos (4)
#define | CLK_CLKSTATUS_IRC22M_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC22M_STB_Pos)
#define | CLK_CLKSTATUS_HIRC_STB_Pos (4)
#define | CLK_CLKSTATUS_HIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_HIRC_STB_Pos)
#define | CLK_CLKSTATUS_CLK_SW_FAIL_Pos (7)
#define | CLK_CLKSTATUS_CLK_SW_FAIL_Msk (0x1ul << CLK_CLKSTATUS_CLK_SW_FAIL_Pos)
#define | CLK_CLKSEL0_HCLK_S_Pos (0)
#define | CLK_CLKSEL0_HCLK_S_Msk (0x7ul << CLK_CLKSEL0_HCLK_S_Pos)
#define | CLK_CLKSEL0_STCLK_S_Pos (3)
#define | CLK_CLKSEL0_STCLK_S_Msk (0x7ul << CLK_CLKSEL0_STCLK_S_Pos)
#define | CLK_CLKSEL1_WDT_S_Pos (0)
#define | CLK_CLKSEL1_WDT_S_Msk (0x3ul << CLK_CLKSEL1_WDT_S_Pos)
#define | CLK_CLKSEL1_ADC_S_Pos (2)
#define | CLK_CLKSEL1_ADC_S_Msk (0x3ul << CLK_CLKSEL1_ADC_S_Pos)
#define | CLK_CLKSEL1_SPI_S_Pos (4)
#define | CLK_CLKSEL1_SPI_S_Msk (0x1ul << CLK_CLKSEL1_SPI_S_Pos)
#define | CLK_CLKSEL1_TMR0_S_Pos (8)
#define | CLK_CLKSEL1_TMR0_S_Msk (0x7ul << CLK_CLKSEL1_TMR0_S_Pos)
#define | CLK_CLKSEL1_TMR1_S_Pos (12)
#define | CLK_CLKSEL1_TMR1_S_Msk (0x7ul << CLK_CLKSEL1_TMR1_S_Pos)
#define | CLK_CLKSEL1_UART_S_Pos (24)
#define | CLK_CLKSEL1_UART_S_Msk (0x3ul << CLK_CLKSEL1_UART_S_Pos)
#define | CLK_CLKDIV_HCLK_N_Pos (0)
#define | CLK_CLKDIV_HCLK_N_Msk (0xful << CLK_CLKDIV_HCLK_N_Pos)
#define | CLK_CLKDIV_UART_N_Pos (8)
#define | CLK_CLKDIV_UART_N_Msk (0xful << CLK_CLKDIV_UART_N_Pos)
#define | CLK_CLKDIV_ADC_N_Pos (16)
#define | CLK_CLKDIV_ADC_N_Msk (0xfful << CLK_CLKDIV_ADC_N_Pos)
#define | CLK_CLKSEL2_FRQDIV_S_Pos (2)
#define | CLK_CLKSEL2_FRQDIV_S_Msk (0x3ul << CLK_CLKSEL2_FRQDIV_S_Pos)
#define | CLK_FRQDIV_FSEL_Pos (0)
#define | CLK_FRQDIV_FSEL_Msk (0xful << CLK_FRQDIV_FSEL_Pos)
#define | CLK_FRQDIV_DIVIDER_EN_Pos (4)
#define | CLK_FRQDIV_DIVIDER_EN_Msk (0x1ul << CLK_FRQDIV_DIVIDER_EN_Pos)
#define | CLK_FRQDIV_DIVIDER1_Pos (5)
#define | CLK_FRQDIV_DIVIDER1_Msk (0x1ul << CLK_FRQDIV_DIVIDER1_Pos)
#define | FMC_ISPCON_ISPEN_Pos (0)
#define | FMC_ISPCON_ISPEN_Msk (0x1ul << FMC_ISPCON_ISPEN_Pos)
#define | FMC_ISPCON_BS_Pos (1)
#define | FMC_ISPCON_BS_Msk (0x1ul << FMC_ISPCON_BS_Pos)
#define | FMC_ISPCON_APUEN_Pos (3)
#define | FMC_ISPCON_APUEN_Msk (0x1ul << FMC_ISPCON_APUEN_Pos)
#define | FMC_ISPCON_CFGUEN_Pos (4)
#define | FMC_ISPCON_CFGUEN_Msk (0x1ul << FMC_ISPCON_CFGUEN_Pos)
#define | FMC_ISPCON_LDUEN_Pos (5)
#define | FMC_ISPCON_LDUEN_Msk (0x1ul << FMC_ISPCON_LDUEN_Pos)
#define | FMC_ISPCON_ISPFF_Pos (6)
#define | FMC_ISPCON_ISPFF_Msk (0x1ul << FMC_ISPCON_ISPFF_Pos)
#define | FMC_ISPADR_ISPADR_Pos (0)
#define | FMC_ISPADR_ISPADR_Msk (0xfffffffful << FMC_ISPADR_ISPADR_Pos)
#define | FMC_ISPDAT_ISPDAT_Pos (0)
#define | FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)
#define | FMC_ISPCMD_ISPCMD_Pos (0)
#define | FMC_ISPCMD_ISPCMD_Msk (0x3ful << FMC_ISPCMD_ISPCMD_Pos)
#define | FMC_ISPTRG_ISPGO_Pos (0)
#define | FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)
#define | FMC_DFBADR_DFBA_Pos (0)
#define | FMC_DFBADR_DFBA_Msk (0xfffffffful << FMC_DFBA_DFBA_Pos)
#define | FMC_ISPSTA_ISPGO_Pos (0)
#define | FMC_ISPSTA_ISPGO_Msk (0x1ul << FMC_ISPSTA_ISPGO_Pos)
#define | FMC_ISPSTA_CBS_Pos (1)
#define | FMC_ISPSTA_CBS_Msk (0x3ul << FMC_ISPSTA_CBS_Pos)
#define | FMC_ISPSTA_ISPFF_Pos (6)
#define | FMC_ISPSTA_ISPFF_Msk (0x1ul << FMC_ISPSTA_ISPFF_Pos)
#define | FMC_ISPSTA_VECMAP_Pos (9)
#define | FMC_ISPSTA_VECMAP_Msk (0xffful << FMC_ISPSTA_VECMAP_Pos)
#define | SYS_PDID_PDID_Pos (0)
#define | SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)
#define | SYS_RSTSRC_RSTS_POR_Pos (0)
#define | SYS_RSTSRC_RSTS_POR_Msk (0x1ul << SYS_RSTSRC_RSTS_POR_Pos)
#define | SYS_RSTSRC_RSTS_RESET_Pos (1)
#define | SYS_RSTSRC_RSTS_RESET_Msk (0x1ul << SYS_RSTSRC_RSTS_RESET_Pos)
#define | SYS_RSTSRC_RSTS_WDT_Pos (2)
#define | SYS_RSTSRC_RSTS_WDT_Msk (0x1ul << SYS_RSTSRC_RSTS_WDT_Pos)
#define | SYS_RSTSRC_RSTS_BOD_Pos (4)
#define | SYS_RSTSRC_RSTS_BOD_Msk (0x1ul << SYS_RSTSRC_RSTS_BOD_Pos)
#define | SYS_RSTSRC_RSTS_MCU_Pos (5)
#define | SYS_RSTSRC_RSTS_MCU_Msk (0x1ul << SYS_RSTSRC_RSTS_MCU_Pos)
#define | SYS_RSTSRC_RSTS_CPU_Pos (7)
#define | SYS_RSTSRC_RSTS_CPU_Msk (0x1ul << SYS_RSTSRC_RSTS_CPU_Pos)
#define | SYS_IPRSTC1_CHIP_RST_Pos (0)
#define | SYS_IPRSTC1_CHIP_RST_Msk (0x1ul << SYS_IPRSTC1_CHIP_RST_Pos)
#define | SYS_IPRSTC1_CPU_RST_Pos (1)
#define | SYS_IPRSTC1_CPU_RST_Msk (0x1ul << SYS_IPRSTC1_CPU_RST_Pos)
#define | SYS_IPRSTC2_GPIO_RST_Pos (1)
#define | SYS_IPRSTC2_GPIO_RST_Msk (0x1ul << SYS_IPRSTC2_GPIO_RST_Pos)
#define | SYS_IPRSTC2_TMR0_RST_Pos (2)
#define | SYS_IPRSTC2_TMR0_RST_Msk (0x1ul << SYS_IPRSTC2_TMR0_RST_Pos)
#define | SYS_IPRSTC2_TMR1_RST_Pos (3)
#define | SYS_IPRSTC2_TMR1_RST_Msk (0x1ul << SYS_IPRSTC2_TMR1_RST_Pos)
#define | SYS_IPRSTC2_I2C_RST_Pos (8)
#define | SYS_IPRSTC2_I2C_RST_Msk (0x1ul << SYS_IPRSTC2_I2C_RST_Pos)
#define | SYS_IPRSTC2_SPI_RST_Pos (12)
#define | SYS_IPRSTC2_SPI_RST_Msk (0x1ul << SYS_IPRSTC2_SPI_RST_Pos)
#define | SYS_IPRSTC2_UART_RST_Pos (16)
#define | SYS_IPRSTC2_UART_RST_Msk (0x1ul << SYS_IPRSTC2_UART_RST_Pos)
#define | SYS_IPRSTC2_PWM_RST_Pos (20)
#define | SYS_IPRSTC2_PWM_RST_Msk (0x1ul << SYS_IPRSTC2_PWM_RST_Pos)
#define | SYS_IPRSTC2_ACMP_RST_Pos (22)
#define | SYS_IPRSTC2_ACMP_RST_Msk (0x1ul << SYS_IPRSTC2_ACMP_RST_Pos)
#define | SYS_IPRSTC2_ADC_RST_Pos (28)
#define | SYS_IPRSTC2_ADC_RST_Msk (0x1ul << SYS_IPRSTC2_ADC_RST_Pos)
#define | SYS_BODCR_BOD_VL_EXT_Pos (0)
#define | SYS_BODCR_BOD_VL_EXT_Msk (0x1ul << SYS_BODCR_BOD_VL_EXT_Pos)
#define | SYS_BODCR_BOD_VL_Pos (1)
#define | SYS_BODCR_BOD_VL_Msk (0x3ul << SYS_BODCR_BOD_VL_Pos)
#define | SYS_BODCR_BOD_RSTEN_Pos (3)
#define | SYS_BODCR_BOD_RSTEN_Msk (0x1ul << SYS_BODCR_BOD_RSTEN_Pos)
#define | SYS_BODCR_BOD_INTF_Pos (4)
#define | SYS_BODCR_BOD_INTF_Msk (0x1ul << SYS_BODCR_BOD_INTF_Pos)
#define | SYS_BODCR_BOD_LPM_Pos (5)
#define | SYS_BODCR_BOD_LPM_Msk (0x1ul << SYS_BODCR_BOD_LPM_Pos)
#define | SYS_BODCR_BOD_OUT_Pos (6)
#define | SYS_BODCR_BOD_OUT_Msk (0x1ul << SYS_BODCR_BOD_OUT_Pos)
#define | SYS_P0_MFP_P0_MFP_Pos (0)
#define | SYS_P0_MFP_P0_MFP_Msk (0xfful << SYS_P0_MFP_P0_MFP_Pos)
#define | SYS_P0_MFP_P0_ALT_Pos (8)
#define | SYS_P0_MFP_P0_ALT_Msk (0xfful << SYS_P0_MFP_P0_ALT_Pos)
#define | SYS_P0_MFP_P0_ALT0_Pos (8)
#define | SYS_P0_MFP_P0_ALT0_Msk (0x1ul << SYS_P0_MFP_P0_ALT0_Pos)
#define | SYS_P0_MFP_P0_ALT1_Pos (9)
#define | SYS_P0_MFP_P0_ALT1_Msk (0x1ul << SYS_P0_MFP_P0_ALT1_Pos)
#define | SYS_P0_MFP_P0_ALT4_Pos (12)
#define | SYS_P0_MFP_P0_ALT4_Msk (0x1ul << SYS_P0_MFP_P0_ALT4_Pos)
#define | SYS_P0_MFP_P0_ALT5_Pos (13)
#define | SYS_P0_MFP_P0_ALT5_Msk (0x1ul << SYS_P0_MFP_P0_ALT5_Pos)
#define | SYS_P0_MFP_P0_ALT6_Pos (14)
#define | SYS_P0_MFP_P0_ALT6_Msk (0x1ul << SYS_P0_MFP_P0_ALT6_Pos)
#define | SYS_P0_MFP_P0_ALT7_Pos (15)
#define | SYS_P0_MFP_P0_ALT7_Msk (0x1ul << SYS_P0_MFP_P0_ALT7_Pos)
#define | SYS_P0_MFP_P0_TYPE_Pos (16)
#define | SYS_P0_MFP_P0_TYPE_Msk (0xfful << SYS_P0_MFP_P0_TYPE_Pos)
#define | SYS_P1_MFP_P1_MFP_Pos (0)
#define | SYS_P1_MFP_P1_MFP_Msk (0xfful << SYS_P1_MFP_P1_MFP_Pos)
#define | SYS_P1_MFP_P1_ALT_Pos (8)
#define | SYS_P1_MFP_P1_ALT_Msk (0xfful << SYS_P1_MFP_P1_ALT_Pos)
#define | SYS_P1_MFP_P1_ALT0_Pos (8)
#define | SYS_P1_MFP_P1_ALT0_Msk (0x1ul << SYS_P1_MFP_P1_ALT0_Pos)
#define | SYS_P1_MFP_P1_ALT2_Pos (10)
#define | SYS_P1_MFP_P1_ALT2_Msk (0x1ul << SYS_P1_MFP_P1_ALT2_Pos)
#define | SYS_P1_MFP_P1_ALT3_Pos (11)
#define | SYS_P1_MFP_P1_ALT3_Msk (0x1ul << SYS_P1_MFP_P1_ALT3_Pos)
#define | SYS_P1_MFP_P1_ALT4_Pos (12)
#define | SYS_P1_MFP_P1_ALT4_Msk (0x1ul << SYS_P1_MFP_P1_ALT4_Pos)
#define | SYS_P1_MFP_P1_ALT5_Pos (13)
#define | SYS_P1_MFP_P1_ALT5_Msk (0x1ul << SYS_P1_MFP_P1_ALT5_Pos)
#define | SYS_P1_MFP_P1_TYPE_Pos (16)
#define | SYS_P1_MFP_P1_TYPE_Msk (0xfful << SYS_P1_MFP_P1_TYPE_Pos)
#define | SYS_P2_MFP_P2_MFP_Pos (0)
#define | SYS_P2_MFP_P2_MFP_Msk (0xfful << SYS_P2_MFP_P2_MFP_Pos)
#define | SYS_P2_MFP_P2_ALT_Pos (8)
#define | SYS_P2_MFP_P2_ALT_Msk (0xfful << SYS_P2_MFP_P2_ALT_Pos)
#define | SYS_P2_MFP_P2_ALT2_Pos (10)
#define | SYS_P2_MFP_P2_ALT2_Msk (0x1ul << SYS_P2_MFP_P2_ALT2_Pos)
#define | SYS_P2_MFP_P2_ALT3_Pos (11)
#define | SYS_P2_MFP_P2_ALT3_Msk (0x1ul << SYS_P2_MFP_P2_ALT3_Pos)
#define | SYS_P2_MFP_P2_ALT4_Pos (12)
#define | SYS_P2_MFP_P2_ALT4_Msk (0x1ul << SYS_P2_MFP_P2_ALT4_Pos)
#define | SYS_P2_MFP_P2_ALT5_Pos (13)
#define | SYS_P2_MFP_P2_ALT5_Msk (0x1ul << SYS_P2_MFP_P2_ALT5_Pos)
#define | SYS_P2_MFP_P2_ALT6_Pos (14)
#define | SYS_P2_MFP_P2_ALT6_Msk (0x1ul << SYS_P2_MFP_P2_ALT6_Pos)
#define | SYS_P2_MFP_P2_TYPE_Pos (16)
#define | SYS_P2_MFP_P2_TYPE_Msk (0xfful << SYS_P2_MFP_P2_TYPE_Pos)
#define | SYS_P3_MFP_P3_MFP_Pos (0)
#define | SYS_P3_MFP_P3_MFP_Msk (0xfful << SYS_P3_MFP_P3_MFP_Pos)
#define | SYS_P3_MFP_P3_ALT_Pos (8)
#define | SYS_P3_MFP_P3_ALT_Msk (0xfful << SYS_P3_MFP_P3_ALT_Pos)
#define | SYS_P3_MFP_P3_ALT0_Pos (8)
#define | SYS_P3_MFP_P3_ALT0_Msk (0x1ul << SYS_P3_MFP_P3_ALT0_Pos)
#define | SYS_P3_MFP_P3_ALT1_Pos (9)
#define | SYS_P3_MFP_P3_ALT1_Msk (0x1ul << SYS_P3_MFP_P3_ALT1_Pos)
#define | SYS_P3_MFP_P3_ALT2_Pos (10)
#define | SYS_P3_MFP_P3_ALT2_Msk (0x1ul << SYS_P3_MFP_P3_ALT2_Pos)
#define | SYS_P3_MFP_P3_ALT4_Pos (12)
#define | SYS_P3_MFP_P3_ALT4_Msk (0x1ul << SYS_P3_MFP_P3_ALT4_Pos)
#define | SYS_P3_MFP_P3_ALT5_Pos (13)
#define | SYS_P3_MFP_P3_ALT5_Msk (0x1ul << SYS_P3_MFP_P3_ALT5_Pos)
#define | SYS_P3_MFP_P3_ALT6_Pos (14)
#define | SYS_P3_MFP_P3_ALT6_Msk (0x1ul << SYS_P3_MFP_P3_ALT6_Pos)
#define | SYS_P3_MFP_P3_TYPE_Pos (16)
#define | SYS_P3_MFP_P3_TYPE_Msk (0xfful << SYS_P3_MFP_P3_TYPE_Pos)
#define | SYS_P3_MFP_P32CPP1_Pos (24)
#define | SYS_P3_MFP_P32CPP1_Msk (0x1ul << SYS_P3_MFP_P32CPP1_Pos)
#define | SYS_P4_MFP_P4_MFP_Pos (0)
#define | SYS_P4_MFP_P4_MFP_Msk (0xfful << SYS_P4_MFP_P4_MFP_Pos)
#define | SYS_P4_MFP_P4_ALT_Pos (8)
#define | SYS_P4_MFP_P4_ALT_Msk (0xfful << SYS_P4_MFP_P4_ALT_Pos)
#define | SYS_P4_MFP_P4_ALT6_Pos (14)
#define | SYS_P4_MFP_P4_ALT6_Msk (0x1ul << SYS_P4_MFP_P4_ALT6_Pos)
#define | SYS_P4_MFP_P4_ALT7_Pos (15)
#define | SYS_P4_MFP_P4_ALT7_Msk (0x1ul << SYS_P4_MFP_P4_ALT7_Pos)
#define | SYS_P4_MFP_P4_TYPE_Pos (16)
#define | SYS_P4_MFP_P4_TYPE_Msk (0xfful << SYS_P4_MFP_P4_TYPE_Pos)
#define | SYS_P5_MFP_P5_MFP_Pos (0)
#define | SYS_P5_MFP_P5_MFP_Msk (0xfful << SYS_P5_MFP_P5_MFP_Pos)
#define | SYS_P5_MFP_P5_ALT_Pos (8)
#define | SYS_P5_MFP_P5_ALT_Msk (0xFFul << SYS_P5_MFP_P5_ALT_Pos)
#define | SYS_P5_MFP_P5_ALT0_Pos (8)
#define | SYS_P5_MFP_P5_ALT0_Msk (0x1ul << SYS_P5_MFP_P5_ALT0_Pos)
#define | SYS_P5_MFP_P5_ALT1_Pos (9)
#define | SYS_P5_MFP_P5_ALT1_Msk (0x1ul << SYS_P5_MFP_P5_ALT1_Pos)
#define | SYS_P5_MFP_P5_ALT2_Pos (10)
#define | SYS_P5_MFP_P5_ALT2_Msk (0x1ul << SYS_P5_MFP_P5_ALT2_Pos)
#define | SYS_P5_MFP_P5_ALT3_Pos (11)
#define | SYS_P5_MFP_P5_ALT3_Msk (0x1ul << SYS_P5_MFP_P5_ALT3_Pos)
#define | SYS_P5_MFP_P5_ALT4_Pos (12)
#define | SYS_P5_MFP_P5_ALT4_Msk (0x1ul << SYS_P5_MFP_P5_ALT4_Pos)
#define | SYS_P5_MFP_P5_ALT5_Pos (13)
#define | SYS_P5_MFP_P5_ALT5_Msk (0x1ul << SYS_P5_MFP_P5_ALT5_Pos)
#define | SYS_P5_MFP_P5_TYPE_Pos (16)
#define | SYS_P5_MFP_P5_TYPE_Msk (0xfful << SYS_P5_MFP_P5_TYPE_Pos)
#define | SYS_IRCTRIMCTL_TRIM_SEL_Pos (0)
#define | SYS_IRCTRIMCTL_TRIM_SEL_Msk (0x1ul << SYS_IRCTRIMCTL_TRIM_SEL_Pos)
#define | SYS_IRCTRIMCTL_TRIM_LOOP_Pos (4)
#define | SYS_IRCTRIMCTL_TRIM_LOOP_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
#define | SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos (1)
#define | SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos)
#define | SYS_IRCTRIMIEN_32K_ERR_IEN_Pos (2)
#define | SYS_IRCTRIMIEN_32K_ERR_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_32K_ERR_IEN_Pos)
#define | SYS_IRCTRIMINT_FREQ_LOCK_Pos (0)
#define | SYS_IRCTRIMINT_FREQ_LOCK_Msk (0x1ul << SYS_IRCTRIMINT_FREQ_LOCK_Pos)
#define | SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos (1)
#define | SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk (0x1ul << SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos)
#define | SYS_IRCTRIMINT_32K_ERR_INT_Pos (2)
#define | SYS_IRCTRIMINT_32K_ERR_INT_Msk (0x1ul << SYS_IRCTRIMINT_32K_ERR_INT_Pos)
#define | SYS_RegLockAddr_RegUnLock_Pos 0
#define | SYS_RegLockAddr_RegUnLock_Msk (0x1ul << SYS_RegLockAddr_RegUnLock_Pos)
#define | GPIO_PMD_PMD0_Pos (0)
#define | GPIO_PMD_PMD0_Msk (0x3ul << GPIO_PMD_PMD0_Pos)
#define | GPIO_PMD_PMD1_Pos (2)
#define | GPIO_PMD_PMD1_Msk (0x3ul << GPIO_PMD_PMD1_Pos)
#define | GPIO_PMD_PMD2_Pos (4)
#define | GPIO_PMD_PMD2_Msk (0x3ul << GPIO_PMD_PMD2_Pos)
#define | GPIO_PMD_PMD3_Pos (6)
#define | GPIO_PMD_PMD3_Msk (0x3ul << GPIO_PMD_PMD3_Pos)
#define | GPIO_PMD_PMD4_Pos (8)
#define | GPIO_PMD_PMD4_Msk (0x3ul << GPIO_PMD_PMD4_Pos)
#define | GPIO_PMD_PMD5_Pos (10)
#define | GPIO_PMD_PMD5_Msk (0x3ul << GPIO_PMD_PMD5_Pos)
#define | GPIO_PMD_PMD6_Pos (12)
#define | GPIO_PMD_PMD6_Msk (0x3ul << GPIO_PMD_PMD6_Pos)
#define | GPIO_PMD_PMD7_Pos (14)
#define | GPIO_PMD_PMD7_Msk (0x3ul << GPIO_PMD_PMD7_Pos)
#define | GPIO_OFFD_OFFD_Pos (16)
#define | GPIO_OFFD_OFFD_Msk (0xfful << GPIO_OFFD_OFFD_Pos)
#define | GPIO_DOUT_DOUT_Pos (0)
#define | GPIO_DOUT_DOUT_Msk (0xfful << GPIO_DOUT_DOUT_Pos)
#define | GPIO_DMASK_DMASK_Pos (0)
#define | GPIO_DMASK_DMASK_Msk (0xfful << GPIO_DMASK_DMASK_Pos)
#define | GPIO_PIN_PIN_Pos (0)
#define | GPIO_PIN_PIN_Msk (0xfful << GPIO_PIN_PIN_Pos)
#define | GPIO_DBEN_DBEN_Pos (0)
#define | GPIO_DBEN_DBEN_Msk (0xfful << GPIO_DBEN_DBEN_Pos)
#define | GPIO_IMD_IMD_Pos (0)
#define | GPIO_IMD_IMD_Msk (0xfful << GPIO_IMD_IMD_Pos)
#define | GPIO_IEN_IF_EN_Pos (0)
#define | GPIO_IEN_IF_EN_Msk (0x1ul << GPIO_IEN_IF_EN_Pos)
#define | GPIO_IEN_IR_EN_Pos (16)
#define | GPIO_IEN_IR_EN_Msk (0xfful << GPIO_IEN_IR_EN_Pos)
#define | GPIO_ISRC_ISRC_Pos (0)
#define | GPIO_ISRC_ISRC_Msk (0xfful << GPIO_ISRC_ISRC_Pos)
#define | GPIO_DBNCECON_DBCLKSEL_Pos (0)
#define | GPIO_DBNCECON_DBCLKSEL_Msk (0xful << GPIO_DBNCECON_DBCLKSEL_Pos)
#define | GPIO_DBNCECON_DBCLKSRC_Pos (4)
#define | GPIO_DBNCECON_DBCLKSRC_Msk (0x1ul << GPIO_DBNCECON_DBCLKSRC_Pos)
#define | GPIO_DBNCECON_ICLK_ON_Pos (5)
#define | GPIO_DBNCECON_ICLK_ON_Msk (0x1ul << GPIO_DBNCECON_ICLK_ON_Pos)
#define | I2C_I2CON_AA_Pos (2)
#define | I2C_I2CON_AA_Msk (0x1ul << I2C_I2CON_AA_Pos)
#define | I2C_I2CON_SI_Pos (3)
#define | I2C_I2CON_SI_Msk (0x1ul << I2C_I2CON_SI_Pos)
#define | I2C_I2CON_STO_Pos (4)
#define | I2C_I2CON_STO_Msk (0x1ul << I2C_I2CON_STO_Pos)
#define | I2C_I2CON_STA_Pos (5)
#define | I2C_I2CON_STA_Msk (0x1ul << I2C_I2CON_STA_Pos)
#define | I2C_I2CON_ENSI_Pos (6)
#define | I2C_I2CON_ENSI_Msk (0x1ul << I2C_I2CON_ENSI_Pos)
#define | I2C_I2CON_EI_Pos (7)
#define | I2C_I2CON_EI_Msk (0x1ul << I2C_I2CON_EI_Pos)
#define | I2C_I2CADDR_GC_Pos (0)
#define | I2C_I2CADDR_GC_Msk (0x1ul << I2C_I2CADDR_GC_Pos)
#define | I2C_I2CADDR_I2CADDR_Pos (1)
#define | I2C_I2CADDR_I2CADDR_Msk (0x7ful << I2C_I2CADDR_I2CADDR_Pos)
#define | I2C_I2CDAT_I2CDAT_Pos (0)
#define | I2C_I2CDAT_I2CDAT_Msk (0xfful << I2C_I2CDAT_I2CDAT_Pos)
#define | I2C_I2CSTATUS_I2CSTATUS_Pos (0)
#define | I2C_I2CSTATUS_I2CSTATUS_Msk (0xfful << I2C_I2CSTATUS_I2CSTATUS_Pos)
#define | I2C_I2CLK_I2CLK_Pos (0)
#define | I2C_I2CLK_I2CLK_Msk (0xfful << I2C_I2CLK_I2CLK_Pos)
#define | I2C_I2CTOC_TIF_Pos (0)
#define | I2C_I2CTOC_TIF_Msk (0x1ul << I2C_I2CTOC_TIF_Pos)
#define | I2C_I2CTOC_DIV4_Pos (1)
#define | I2C_I2CTOC_DIV4_Msk (0x1ul << I2C_I2CTOC_DIV4_Pos)
#define | I2C_I2CTOC_ENTI_Pos (2)
#define | I2C_I2CTOC_ENTI_Msk (0x1ul << I2C_I2CTOC_ENTI_Pos)
#define | I2C_I2CADM_I2CADM_Pos (1)
#define | I2C_I2CADM_I2CADM_Msk (0x7ful << I2C_I2CADM_I2CADM_Pos)
#define | I2C_I2CON2_WKUPEN_Pos (0)
#define | I2C_I2CON2_WKUPEN_Msk (0x1ul << I2C_I2CON2_WKUPEN_Pos)
#define | I2C_I2CON2_TWOFF_EN_Pos (1)
#define | I2C_I2CON2_TWOFF_EN_Msk (0x1ul << I2C_I2CON2_TWOFF_EN_Pos)
#define | I2C_I2CON2_NOSTRETCH_Pos (2)
#define | I2C_I2CON2_NOSTRETCH_Msk (0x1ul << I2C_I2CON2_NOSTRETCH_Pos)
#define | I2C_I2CON2_OVER_INTEN_Pos (3)
#define | I2C_I2CON2_OVER_INTEN_Msk (0x1ul << I2C_I2CON2_OVER_INTEN_Pos)
#define | I2C_I2CON2_UNDER_INTEN_Pos (4)
#define | I2C_I2CON2_UNDER_INTEN_Msk (0x1ul << I2C_I2CON2_UNDER_INTEN_Pos)
#define | I2C_I2CSTATUS2_WAKEUP_Pos (0)
#define | I2C_I2CSTATUS2_WAKEUP_Msk (0x1ul << I2C_I2CSTATUS2_WAKEUP_Pos)
#define | I2C_I2CSTATUS2_FULL_Pos (1)
#define | I2C_I2CSTATUS2_FULL_Msk (0x1ul << I2C_I2CSTATUS2_FULL_Pos)
#define | I2C_I2CSTATUS2_EMPTY_Pos (2)
#define | I2C_I2CSTATUS2_EMPTY_Msk (0x1ul << I2C_I2CSTATUS2_EMPTY_Pos)
#define | I2C_I2CSTATUS2_OVERUN_Pos (3)
#define | I2C_I2CSTATUS2_OVERUN_Msk (0x1ul << I2C_I2CSTATUS2_OVERUN_Pos)
#define | I2C_I2CSTATUS2_UNDERUN_Pos (4)
#define | I2C_I2CSTATUS2_UNDERUN_Msk (0x1ul << I2C_I2CSTATUS2_UNDERUN_Pos)
#define | INT_SRC_INT_SRC_Pos (0)
#define | INT_SRC_INT_SRC_Msk (0x7ul << INT_SRC_INT_SRC_Pos)
#define | INT_CON_NMI_SEL_Pos (0)
#define | INT_CON_NMI_SEL_Msk (0x1ful << INT_CON_NMI_SEL_Pos)
#define | INT_CON_NMI_SEL_EN_Pos (8)
#define | INT_CON_NMI_SEL_EN_Msk (0x1ul << INT_CON_NMI_SEL_EN_Pos)
#define | INT_IRQ_MCU_IRQ_Pos (0)
#define | INT_IRQ_MCU_IRQ_Msk (0xfffffffful << INT_IRQ_MCU_IRQ_Pos)
#define | PWM_PPR_CP01_Pos (0)
#define | PWM_PPR_CP01_Msk (0xfful << PWM_PPR_CP01_Pos)
#define | PWM_PPR_CP23_Pos (8)
#define | PWM_PPR_CP23_Msk (0xfful << PWM_PPR_CP23_Pos)
#define | PWM_PPR_CP45_Pos (16)
#define | PWM_PPR_CP45_Msk (0xfful << PWM_PPR_CP45_Pos)
#define | PWM_CSR_CSR0_Pos (0)
#define | PWM_CSR_CSR0_Msk (0x7ul << PWM_CSR_CSR0_Pos)
#define | PWM_CSR_CSR1_Pos (4)
#define | PWM_CSR_CSR1_Msk (0x7ul << PWM_CSR_CSR1_Pos)
#define | PWM_CSR_CSR2_Pos (8)
#define | PWM_CSR_CSR2_Msk (0x7ul << PWM_CSR_CSR2_Pos)
#define | PWM_CSR_CSR3_Pos (12)
#define | PWM_CSR_CSR3_Msk (0x7ul << PWM_CSR_CSR3_Pos)
#define | PWM_CSR_CSR4_Pos (16)
#define | PWM_CSR_CSR4_Msk (0x7ul << PWM_CSR_CSR4_Pos)
#define | PWM_CSR_CSR5_Pos (20)
#define | PWM_CSR_CSR5_Msk (0x7ul << PWM_CSR_CSR5_Pos)
#define | PWM_PCR_CH0EN_Pos (0)
#define | PWM_PCR_CH0EN_Msk (0x1ul << PWM_PCR_CH0EN_Pos)
#define | PWM_PCR_DB_MOD_Pos (1)
#define | PWM_PCR_DB_MOD_Msk (0x1ul << PWM_PCR_DB_MOD_Pos)
#define | PWM_PCR_CH0INV_Pos (2)
#define | PWM_PCR_CH0INV_Msk (0x1ul << PWM_PCR_CH0INV_Pos)
#define | PWM_PCR_CH0MOD_Pos (3)
#define | PWM_PCR_CH0MOD_Msk (0x1ul << PWM_PCR_CH0MOD_Pos)
#define | PWM_PCR_CH1EN_Pos (4)
#define | PWM_PCR_CH1EN_Msk (0x1ul << PWM_PCR_CH1EN_Pos)
#define | PWM_PCR_CH1INV_Pos (6)
#define | PWM_PCR_CH1INV_Msk (0x1ul << PWM_PCR_CH1INV_Pos)
#define | PWM_PCR_CH1MOD_Pos (7)
#define | PWM_PCR_CH1MOD_Msk (0x1ul << PWM_PCR_CH1MOD_Pos)
#define | PWM_PCR_CH2EN_Pos (8)
#define | PWM_PCR_CH2EN_Msk (0x1ul << PWM_PCR_CH2EN_Pos)
#define | PWM_PCR_CH2INV_Pos (10)
#define | PWM_PCR_CH2INV_Msk (0x1ul << PWM_PCR_CH2INV_Pos)
#define | PWM_PCR_CH2MOD_Pos (11)
#define | PWM_PCR_CH2MOD_Msk (0x1ul << PWM_PCR_CH2MOD_Pos)
#define | PWM_PCR_CH3EN_Pos (12)
#define | PWM_PCR_CH3EN_Msk (0x1ul << PWM_PCR_CH3EN_Pos)
#define | PWM_PCR_CH3INV_Pos (14)
#define | PWM_PCR_CH3INV_Msk (0x1ul << PWM_PCR_CH3INV_Pos)
#define | PWM_PCR_CH3MOD_Pos (15)
#define | PWM_PCR_CH3MOD_Msk (0x1ul << PWM_PCR_CH3MOD_Pos)
#define | PWM_PCR_CH4EN_Pos (16)
#define | PWM_PCR_CH4EN_Msk (0x1ul << PWM_PCR_CH4EN_Pos)
#define | PWM_PCR_CH4INV_Pos (18)
#define | PWM_PCR_CH4INV_Msk (0x1ul << PWM_PCR_CH4INV_Pos)
#define | PWM_PCR_CH4MOD_Pos (19)
#define | PWM_PCR_CH4MOD_Msk (0x1ul << PWM_PCR_CH4MOD_Pos)
#define | PWM_PCR_CH5EN_Pos (20)
#define | PWM_PCR_CH5EN_Msk (0x1ul << PWM_PCR_CH5EN_Pos)
#define | PWM_PCR_CH5INV_Pos (22)
#define | PWM_PCR_CH5INV_Msk (0x1ul << PWM_PCR_CH5INV_Pos)
#define | PWM_PCR_CH5MOD_Pos (23)
#define | PWM_PCR_CH5MOD_Msk (0x1ul << PWM_PCR_CH5MOD_Pos)
#define | PWM_PCR_DZEN01_Pos (24)
#define | PWM_PCR_DZEN01_Msk (0x1ul << PWM_PCR_DZEN01_Pos)
#define | PWM_PCR_DZEN23_Pos (25)
#define | PWM_PCR_DZEN23_Msk (0x1ul << PWM_PCR_DZEN23_Pos)
#define | PWM_PCR_DZEN45_Pos (26)
#define | PWM_PCR_DZEN45_Msk (0x1ul << PWM_PCR_DZEN45_Pos)
#define | PWM_PCR_CLRPWM_Pos (27)
#define | PWM_PCR_CLRPWM_Msk (0x1ul << PWM_PCR_CLRPWM_Pos)
#define | PWM_PCR_PWMMOD_Pos (28)
#define | PWM_PCR_PWMMOD_Msk (0x3ul << PWM_PCR_PWMMOD_Pos)
#define | PWM_PCR_GRP_Pos (30)
#define | PWM_PCR_GRP_Msk (0x1ul << PWM_PCR_GRP_Pos)
#define | PWM_PCR_PWMTYPE_Pos (31)
#define | PWM_PCR_PWMTYPE_Msk (0x1ul << PWM_PCR_PWMTYPE_Pos)
#define | PWM_CNR_CNR_Pos 0
#define | PWM_CNR_CNR_Msk (0xfffful << PWM_CNR_CNR_Pos)
#define | PWM_CMR_CMR_Pos 0
#define | PWM_CMR_CMR_Msk (0xfffful << PWM_CMR_CMR_Pos)
#define | PWM_PIER_PWMPIE0_Pos (0)
#define | PWM_PIER_PWMPIE0_Msk (0x1ul << PWM_PIER_PWMPIE0_Pos)
#define | PWM_PIER_PWMPIE1_Pos (1)
#define | PWM_PIER_PWMPIE1_Msk (0x1ul << PWM_PIER_PWMPIE1_Pos)
#define | PWM_PIER_PWMPIE2_Pos (2)
#define | PWM_PIER_PWMPIE2_Msk (0x1ul << PWM_PIER_PWMPIE2_Pos)
#define | PWM_PIER_PWMPIE3_Pos (3)
#define | PWM_PIER_PWMPIE3_Msk (0x1ul << PWM_PIER_PWMPIE3_Pos)
#define | PWM_PIER_PWMPIE4_Pos (4)
#define | PWM_PIER_PWMPIE4_Msk (0x1ul << PWM_PIER_PWMPIE4_Pos)
#define | PWM_PIER_PWMPIE5_Pos (5)
#define | PWM_PIER_PWMPIE5_Msk (0x1ul << PWM_PIER_PWMPIE5_Pos)
#define | PWM_PIER_PWMDIE0_Pos (8)
#define | PWM_PIER_PWMDIE0_Msk (0x1ul << PWM_PIER_PWMDIE0_Pos)
#define | PWM_PIER_PWMDIE1_Pos (9)
#define | PWM_PIER_PWMDIE1_Msk (0x1ul << PWM_PIER_PWMDIE1_Pos)
#define | PWM_PIER_PWMDIE2_Pos (10)
#define | PWM_PIER_PWMDIE2_Msk (0x1ul << PWM_PIER_PWMDIE2_Pos)
#define | PWM_PIER_PWMDIE3_Pos (11)
#define | PWM_PIER_PWMDIE3_Msk (0x1ul << PWM_PIER_PWMDIE3_Pos)
#define | PWM_PIER_PWMDIE4_Pos (12)
#define | PWM_PIER_PWMDIE4_Msk (0x1ul << PWM_PIER_PWMDIE4_Pos)
#define | PWM_PIER_PWMDIE5_Pos (13)
#define | PWM_PIER_PWMDIE5_Msk (0x1ul << PWM_PIER_PWMDIE5_Pos)
#define | PWM_PIER_BRKIE_Pos (16)
#define | PWM_PIER_BRKIE_Msk (0x1ul << PWM_PIER_BRKIE_Pos)
#define | PWM_PIER_INT_TYPE_Pos (17)
#define | PWM_PIER_INT_TYPE_Msk (0x1ul << PWM_PIER_INT_TYPE_Pos)
#define | PWM_PIIR_PWMPIF0_Pos (0)
#define | PWM_PIIR_PWMPIF0_Msk (0x1ul << PWM_PIIR_PWMPIF0_Pos)
#define | PWM_PIIR_PWMPIF1_Pos (1)
#define | PWM_PIIR_PWMPIF1_Msk (0x1ul << PWM_PIIR_PWMPIF1_Pos)
#define | PWM_PIIR_PWMPIF2_Pos (2)
#define | PWM_PIIR_PWMPIF2_Msk (0x1ul << PWM_PIIR_PWMPIF2_Pos)
#define | PWM_PIIR_PWMPIF3_Pos (3)
#define | PWM_PIIR_PWMPIF3_Msk (0x1ul << PWM_PIIR_PWMPIF3_Pos)
#define | PWM_PIIR_PWMPIF4_Pos (4)
#define | PWM_PIIR_PWMPIF4_Msk (0x1ul << PWM_PIIR_PWMPIF4_Pos)
#define | PWM_PIIR_PWMPIF5_Pos (5)
#define | PWM_PIIR_PWMPIF5_Msk (0x1ul << PWM_PIIR_PWMPIF5_Pos)
#define | PWM_PIIR_PWMDIF0_Pos (8)
#define | PWM_PIIR_PWMDIF0_Msk (0x1ul << PWM_PIIR_PWMDIF0_Pos)
#define | PWM_PIIR_PWMDIF1_Pos (9)
#define | PWM_PIIR_PWMDIF1_Msk (0x1ul << PWM_PIIR_PWMDIF1_Pos)
#define | PWM_PIIR_PWMDIF2_Pos (10)
#define | PWM_PIIR_PWMDIF2_Msk (0x1ul << PWM_PIIR_PWMDIF2_Pos)
#define | PWM_PIIR_PWMDIF3_Pos (11)
#define | PWM_PIIR_PWMDIF3_Msk (0x1ul << PWM_PIIR_PWMDIF3_Pos)
#define | PWM_PIIR_PWMDIF4_Pos (12)
#define | PWM_PIIR_PWMDIF4_Msk (0x1ul << PWM_PIIR_PWMDIF4_Pos)
#define | PWM_PIIR_PWMDIF5_Pos (13)
#define | PWM_PIIR_PWMDIF5_Msk (0x1ul << PWM_PIIR_PWMDIF5_Pos)
#define | PWM_PIIR_BKF0_Pos (16)
#define | PWM_PIIR_BKF0_Msk (0x1ul << PWM_PIIR_BKF0_Pos)
#define | PWM_PIIR_BKF1_Pos (17)
#define | PWM_PIIR_BKF1_Msk (0x1ul << PWM_PIIR_BKF1_Pos)
#define | PWM_POE_PWM0_Pos (0)
#define | PWM_POE_PWM0_Msk (0x1ul << PWM_POE_PWM0_Pos)
#define | PWM_POE_PWM1_Pos (1)
#define | PWM_POE_PWM1_Msk (0x1ul << PWM_POE_PWM1_Pos)
#define | PWM_POE_PWM2_Pos (2)
#define | PWM_POE_PWM2_Msk (0x1ul << PWM_POE_PWM2_Pos)
#define | PWM_POE_PWM3_Pos (3)
#define | PWM_POE_PWM3_Msk (0x1ul << PWM_POE_PWM3_Pos)
#define | PWM_POE_PWM4_Pos (4)
#define | PWM_POE_PWM4_Msk (0x1ul << PWM_POE_PWM4_Pos)
#define | PWM_POE_PWM5_Pos (5)
#define | PWM_POE_PWM5_Msk (0x1ul << PWM_POE_PWM5_Pos)
#define | PWM_PFBCON_BKEN0_Pos (0)
#define | PWM_PFBCON_BKEN0_Msk (0x1ul << PWM_PFBCON_BKEN0_Pos)
#define | PWM_PFBCON_BKEN1_Pos (1)
#define | PWM_PFBCON_BKEN1_Msk (0x1ul << PWM_PFBCON_BKEN1_Pos)
#define | PWM_PFBCON_CPO0BKEN_Pos (2)
#define | PWM_PFBCON_CPO0BKEN_Msk (0x1ul << PWM_PFBCON_CPO0BKEN_Pos)
#define | PWM_PFBCON_CPO1BKEN_Pos (3)
#define | PWM_PFBCON_CPO1BKEN_Msk (0x1ul << PWM_PFBCON_CPO1BKEN_Pos)
#define | PWM_PFBCON_BKF_Pos (7)
#define | PWM_PFBCON_BKF_Msk (0x1ul << PWM_PFBCON_BKF_Pos)
#define | PWM_PFBCON_PWMBKO0_Pos (24)
#define | PWM_PFBCON_PWMBKO0_Msk (0x1ul << PWM_PFBCON_PWMBKO0_Pos)
#define | PWM_PFBCON_PWMBKO1_Pos (25)
#define | PWM_PFBCON_PWMBKO1_Msk (0x1ul << PWM_PFBCON_PWMBKO1_Pos)
#define | PWM_PFBCON_PWMBKO2_Pos (26)
#define | PWM_PFBCON_PWMBKO2_Msk (0x1ul << PWM_PFBCON_PWMBKO2_Pos)
#define | PWM_PFBCON_PWMBKO3_Pos (27)
#define | PWM_PFBCON_PWMBKO3_Msk (0x1ul << PWM_PFBCON_PWMBKO3_Pos)
#define | PWM_PFBCON_PWMBKO4_Pos (28)
#define | PWM_PFBCON_PWMBKO4_Msk (0x1ul << PWM_PFBCON_PWMBKO4_Pos)
#define | PWM_PFBCON_PWMBKO5_Pos (29)
#define | PWM_PFBCON_PWMBKO5_Msk (0x1ul << PWM_PFBCON_PWMBKO5_Pos)
#define | PWM_PFBCON_D6BKO6_Pos (30)
#define | PWM_PFBCON_D6BKO6_Msk (0x1ul << PWM_PFBCON_D6BKO6_Pos)
#define | PWM_PFBCON_D7BKO7_Pos (31)
#define | PWM_PFBCON_D7BKO7_Msk (0x1ul << PWM_PFBCON_D7BKO7_Pos)
#define | PWM_DZIR_DZI01_Pos (0)
#define | PWM_DZIR_DZI01_Msk (0xfful << PWM_DZIR_DZI01_Pos)
#define | PWM_DZIR_DZI23_Pos (8)
#define | PWM_DZIR_DZI23_Msk (0xfful << PWM_DZIR_DZI23_Pos)
#define | PWM_DZIR_DZI45_Pos (16)
#define | PWM_DZIR_DZI45_Msk (0xfful << PWM_DZIR_DZI45_Pos)
#define | PWM_TRGCON0_CM0TRGREN_Pos (0)
#define | PWM_TRGCON0_CM0TRGREN_Msk (0x1ul << PWM_TRGCON0_CM0TRGREN_Pos)
#define | PWM_TRGCON0_CNT0TRGEN_Pos (1)
#define | PWM_TRGCON0_CNT0TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT0TRGEN_Pos)
#define | PWM_TRGCON0_CM0TRGFEN_Pos (2)
#define | PWM_TRGCON0_CM0TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM0TRGFEN_Pos)
#define | PWM_TRGCON0_P0TRGEN_Pos (3)
#define | PWM_TRGCON0_P0TRGEN_Msk (0x1ul << PWM_TRGCON0_P0TRGEN_Pos)
#define | PWM_TRGCON0_CM1TRGREN_Pos (8)
#define | PWM_TRGCON0_CM1TRGREN_Msk (0x1ul << PWM_TRGCON0_CM1TRGREN_Pos)
#define | PWM_TRGCON0_CNT1TRGEN_Pos (9)
#define | PWM_TRGCON0_CNT1TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT1TRGEN_Pos)
#define | PWM_TRGCON0_CM1TRGFEN_Pos (10)
#define | PWM_TRGCON0_CM1TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM1TRGFEN_Pos)
#define | PWM_TRGCON0_P1TRGEN_Pos (11)
#define | PWM_TRGCON0_P1TRGEN_Msk (0x1ul << PWM_TRGCON0_P1TRGEN_Pos)
#define | PWM_TRGCON0_CM2TRGREN_Pos (16)
#define | PWM_TRGCON0_CM2TRGREN_Msk (0x1ul << PWM_TRGCON0_CM2TRGREN_Pos)
#define | PWM_TRGCON0_CNT2TRGEN_Pos (17)
#define | PWM_TRGCON0_CNT2TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT2TRGEN_Pos)
#define | PWM_TRGCON0_CM2TRGFEN_Pos (18)
#define | PWM_TRGCON0_CM2TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM2TRGFEN_Pos)
#define | PWM_TRGCON0_P2TRGEN_Pos (19)
#define | PWM_TRGCON0_P2TRGEN_Msk (0x1ul << PWM_TRGCON0_P2TRGEN_Pos)
#define | PWM_TRGCON0_CM3TRGREN_Pos (24)
#define | PWM_TRGCON0_CM3TRGREN_Msk (0x1ul << PWM_TRGCON0_CM3TRGREN_Pos)
#define | PWM_TRGCON0_CNT3TRGEN_Pos (25)
#define | PWM_TRGCON0_CNT3TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT3TRGEN_Pos)
#define | PWM_TRGCON0_CM3TRGFEN_Pos (26)
#define | PWM_TRGCON0_CM3TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM3TRGFEN_Pos)
#define | PWM_TRGCON0_P3TRGEN_Pos (27)
#define | PWM_TRGCON0_P3TRGEN_Msk (0x1ul << PWM_TRGCON0_P3TRGEN_Pos)
#define | PWM_TRGCON1_CM4TRGREN_Pos (0)
#define | PWM_TRGCON1_CM4TRGREN_Msk (0x1ul << PWM_TRGCON1_CM4TRGREN_Pos)
#define | PWM_TRGCON1_CNT4TRGEN_Pos (1)
#define | PWM_TRGCON1_CNT4TRGEN_Msk (0x1ul << PWM_TRGCON1_CNT4TRGEN_Pos)
#define | PWM_TRGCON1_CM4TRGFEN_Pos (2)
#define | PWM_TRGCON1_CM4TRGFEN_Msk (0x1ul << PWM_TRGCON1_CM4TRGFEN_Pos)
#define | PWM_TRGCON1_P4TRGEN_Pos (3)
#define | PWM_TRGCON1_P4TRGEN_Msk (0x1ul << PWM_TRGCON1_P4TRGEN_Pos)
#define | PWM_TRGCON1_CM5TRGREN_Pos (8)
#define | PWM_TRGCON1_CM5TRGREN_Msk (0x1ul << PWM_TRGCON1_CM5TRGREN_Pos)
#define | PWM_TRGCON1_CNT5TRGEN_Pos (9)
#define | PWM_TRGCON1_CNT5TRGEN_Msk (0x1ul << PWM_TRGCON1_CNT5TRGEN_Pos)
#define | PWM_TRGCON1_CM5TRGFEN_Pos (10)
#define | PWM_TRGCON1_CM5TRGFEN_Msk (0x1ul << PWM_TRGCON1_CM5TRGFEN_Pos)
#define | PWM_TRGCON1_P5TRGEN_Pos (11)
#define | PWM_TRGCON1_P5TRGEN_Msk (0x1ul << PWM_TRGCON1_P5TRGEN_Pos)
#define | PWM_TRGSTS0_CMR0FLAG_R_Pos (0)
#define | PWM_TRGSTS0_CMR0FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR0FLAG_R_Pos)
#define | PWM_TRGSTS0_CNT0FLAG_Pos (1)
#define | PWM_TRGSTS0_CNT0FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT0FLAG_Pos)
#define | PWM_TRGSTS0_CMR0FLAG_F_Pos (2)
#define | PWM_TRGSTS0_CMR0FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR0FLAG_F_Pos)
#define | PWM_TRGSTS0_PERID0FLAG_Pos (3)
#define | PWM_TRGSTS0_PERID0FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID0FLAG_Pos)
#define | PWM_TRGSTS0_CMR1FLAG_R_Pos (8)
#define | PWM_TRGSTS0_CMR1FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR1FLAG_R_Pos)
#define | PWM_TRGSTS0_CNT1FLAG_Pos (9)
#define | PWM_TRGSTS0_CNT1FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT1FLAG_Pos)
#define | PWM_TRGSTS0_CMR1FLAG_F_Pos (10)
#define | PWM_TRGSTS0_CMR1FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR1FLAG_F_Pos)
#define | PWM_TRGSTS0_PERID1FLAG_Pos (11)
#define | PWM_TRGSTS0_PERID1FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID1FLAG_Pos)
#define | PWM_TRGSTS0_CMR2FLAG_R_Pos (16)
#define | PWM_TRGSTS0_CMR2FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR2FLAG_R_Pos)
#define | PWM_TRGSTS0_CNT2FLAG_Pos (17)
#define | PWM_TRGSTS0_CNT2FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT2FLAG_Pos)
#define | PWM_TRGSTS0_CMR2FLAG_F_Pos (18)
#define | PWM_TRGSTS0_CMR2FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR2FLAG_F_Pos)
#define | PWM_TRGSTS0_PERID2FLAG_Pos (19)
#define | PWM_TRGSTS0_PERID2FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID2FLAG_Pos)
#define | PWM_TRGSTS0_CMR3FLAG_R_Pos (24)
#define | PWM_TRGSTS0_CMR3FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR3FLAG_R_Pos)
#define | PWM_TRGSTS0_CNT3FLAG_Pos (25)
#define | PWM_TRGSTS0_CNT3FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT3FLAG_Pos)
#define | PWM_TRGSTS0_CMR3FLAG_F_Pos (26)
#define | PWM_TRGSTS0_CMR3FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR3FLAG_F_Pos)
#define | PWM_TRGSTS0_PERID3FLAG_Pos (27)
#define | PWM_TRGSTS0_PERID3FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID3FLAG_Pos)
#define | PWM_TRGSTS1_CMR4FLAG_R_Pos (0)
#define | PWM_TRGSTS1_CMR4FLAG_R_Msk (0x1ul << PWM_TRGSTS1_CMR4FLAG_R_Pos)
#define | PWM_TRGSTS1_CNT4FLAG_Pos (1)
#define | PWM_TRGSTS1_CNT4FLAG_Msk (0x1ul << PWM_TRGSTS1_CNT4FLAG_Pos)
#define | PWM_TRGSTS1_CMR4FLAG_F_Pos (2)
#define | PWM_TRGSTS1_CMR4FLAG_F_Msk (0x1ul << PWM_TRGSTS1_CMR4FLAG_F_Pos)
#define | PWM_TRGSTS1_PERID4FLAG_Pos (3)
#define | PWM_TRGSTS1_PERID4FLAG_Msk (0x1ul << PWM_TRGSTS1_PERID4FLAG_Pos)
#define | PWM_TRGSTS1_CMR5FLAG_R_Pos (8)
#define | PWM_TRGSTS1_CMR5FLAG_R_Msk (0x1ul << PWM_TRGSTS1_CMR5FLAG_R_Pos)
#define | PWM_TRGSTS1_CNT5FLAG_Pos (9)
#define | PWM_TRGSTS1_CNT5FLAG_Msk (0x1ul << PWM_TRGSTS1_CNT5FLAG_Pos)
#define | PWM_TRGSTS1_CMR5FLAG_F_Pos (10)
#define | PWM_TRGSTS1_CMR5FLAG_F_Msk (0x1ul << PWM_TRGSTS1_CMR5FLAG_F_Pos)
#define | PWM_TRGSTS1_PERID5FLAG_Pos (11)
#define | PWM_TRGSTS1_PERID5FLAG_Msk (0x1ul << PWM_TRGSTS1_PERID5FLAG_Pos)
#define | PWM_PHCHG_D0_Pos (0)
#define | PWM_PHCHG_D0_Msk (0x1ul << PWM_PHCHG_D0_Pos)
#define | PWM_PHCHG_D1_Pos (1)
#define | PWM_PHCHG_D1_Msk (0x1ul << PWM_PHCHG_D1_Pos)
#define | PWM_PHCHG_D2_Pos (2)
#define | PWM_PHCHG_D2_Msk (0x1ul << PWM_PHCHG_D2_Pos)
#define | PWM_PHCHG_D3_Pos (3)
#define | PWM_PHCHG_D3_Msk (0x1ul << PWM_PHCHG_D3_Pos)
#define | PWM_PHCHG_D4_Pos (4)
#define | PWM_PHCHG_D4_Msk (0x1ul << PWM_PHCHG_D4_Pos)
#define | PWM_PHCHG_D5_Pos (5)
#define | PWM_PHCHG_D5_Msk (0x1ul << PWM_PHCHG_D5_Pos)
#define | PWM_PHCHG_D6_Pos (6)
#define | PWM_PHCHG_D6_Msk (0x1ul << PWM_PHCHG_D6_Pos)
#define | PWM_PHCHG_D7_Pos (7)
#define | PWM_PHCHG_D7_Msk (0x1ul << PWM_PHCHG_D7_Pos)
#define | PWM_PHCHG_PWM0_Pos (8)
#define | PWM_PHCHG_PWM0_Msk (0x1ul << PWM_PHCHG_PWM0_Pos)
#define | PWM_PHCHG_PWM1_Pos (9)
#define | PWM_PHCHG_PWM1_Msk (0x1ul << PWM_PHCHG_PWM1_Pos)
#define | PWM_PHCHG_PWM2_Pos (10)
#define | PWM_PHCHG_PWM2_Msk (0x1ul << PWM_PHCHG_PWM2_Pos)
#define | PWM_PHCHG_PWM3_Pos (11)
#define | PWM_PHCHG_PWM3_Msk (0x1ul << PWM_PHCHG_PWM3_Pos)
#define | PWM_PHCHG_PWM4_Pos (12)
#define | PWM_PHCHG_PWM4_Msk (0x1ul << PWM_PHCHG_PWM4_Pos)
#define | PWM_PHCHG_PWM5_Pos (13)
#define | PWM_PHCHG_PWM5_Msk (0x1ul << PWM_PHCHG_PWM5_Pos)
#define | PWM_PHCHG_ACCNT0_Pos (14)
#define | PWM_PHCHG_ACCNT0_Msk (0x1ul << PWM_PHCHG_ACCNT0_Pos)
#define | PWM_PHCHG_ACCNT1_Pos (15)
#define | PWM_PHCHG_ACCNT1_Msk (0x1ul << PWM_PHCHG_ACCNT1_Pos)
#define | PWM_PHCHG_CH01TOFF1_Pos (16)
#define | PWM_PHCHG_CH01TOFF1_Msk (0x1ul << PWM_PHCHG_CH01TOFF1_Pos)
#define | PWM_PHCHG_CH11TOFF1_Pos (17)
#define | PWM_PHCHG_CH11TOFF1_Msk (0x1ul << PWM_PHCHG_CH11TOFF1_Pos)
#define | PWM_PHCHG_CH21TOFF1_Pos (18)
#define | PWM_PHCHG_CH21TOFF1_Msk (0x1ul << PWM_PHCHG_CH21TOFF1_Pos)
#define | PWM_PHCHG_CH31TOFF1_Pos (19)
#define | PWM_PHCHG_CH31TOFF1_Msk (0x1ul << PWM_PHCHG_CH31TOFF1_Pos)
#define | PWM_PHCHG_CMP1SEL_Pos (20)
#define | PWM_PHCHG_CMP1SEL_Msk (0x3ul << PWM_PHCHG_CMP1SEL_Pos)
#define | PWM_PHCHG_T1_Pos (22)
#define | PWM_PHCHG_T1_Msk (0x1ul << PWM_PHCHG_T1_Pos)
#define | PWM_PHCHG_CE1_Pos (23)
#define | PWM_PHCHG_CE1_Msk (0x1ul << PWM_PHCHG_CE1_Pos)
#define | PWM_PHCHG_CH01TOFF0_Pos (24)
#define | PWM_PHCHG_CH01TOFF0_Msk (0x1ul << PWM_PHCHG_CH01TOFF0_Pos)
#define | PWM_PHCHG_CH11TOFF0_Pos (25)
#define | PWM_PHCHG_CH11TOFF0_Msk (0x1ul << PWM_PHCHG_CH11TOFF0_Pos)
#define | PWM_PHCHG_CH21TOFF0_Pos (26)
#define | PWM_PHCHG_CH21TOFF0_Msk (0x1ul << PWM_PHCHG_CH21TOFF0_Pos)
#define | PWM_PHCHG_CH31TOFF0_Pos (27)
#define | PWM_PHCHG_CH31TOFF0_Msk (0x1ul << PWM_PHCHG_CH31TOFF0_Pos)
#define | PWM_PHCHG_CMP0SEL_Pos (28)
#define | PWM_PHCHG_CMP0SEL_Msk (0x3ul << PWM_PHCHG_CMP0SEL_Pos)
#define | PWM_PHCHG_T0_Pos (30)
#define | PWM_PHCHG_T0_Msk (0x1ul << PWM_PHCHG_T0_Pos)
#define | PWM_PHCHG_CE0_Pos (31)
#define | PWM_PHCHG_CE0_Msk (0x1ul << PWM_PHCHG_CE0_Pos)
#define | PWM_PHCHGNXT_D0_Pos (0)
#define | PWM_PHCHGNXT_D0_Msk (0x1ul << PWM_PHCHGNXT_D0_Pos)
#define | PWM_PHCHGNXT_D1_Pos (1)
#define | PWM_PHCHGNXT_D1_Msk (0x1ul << PWM_PHCHGNXT_D1_Pos)
#define | PWM_PHCHGNXT_D2_Pos (2)
#define | PWM_PHCHGNXT_D2_Msk (0x1ul << PWM_PHCHGNXT_D2_Pos)
#define | PWM_PHCHGNXT_D3_Pos (3)
#define | PWM_PHCHGNXT_D3_Msk (0x1ul << PWM_PHCHGNXT_D3_Pos)
#define | PWM_PHCHGNXT_D4_Pos (4)
#define | PWM_PHCHGNXT_D4_Msk (0x1ul << PWM_PHCHGNXT_D4_Pos)
#define | PWM_PHCHGNXT_D5_Pos (5)
#define | PWM_PHCHGNXT_D5_Msk (0x1ul << PWM_PHCHGNXT_D5_Pos)
#define | PWM_PHCHGNXT_D6_Pos (6)
#define | PWM_PHCHGNXT_D6_Msk (0x1ul << PWM_PHCHGNXT_D6_Pos)
#define | PWM_PHCHGNXT_D7_Pos (7)
#define | PWM_PHCHGNXT_D7_Msk (0x1ul << PWM_PHCHGNXT_D7_Pos)
#define | PWM_PHCHGNXT_PWM0_Pos (8)
#define | PWM_PHCHGNXT_PWM0_Msk (0x1ul << PWM_PHCHGNXT_PWM0_Pos)
#define | PWM_PHCHGNXT_PWM1_Pos (9)
#define | PWM_PHCHGNXT_PWM1_Msk (0x1ul << PWM_PHCHGNXT_PWM1_Pos)
#define | PWM_PHCHGNXT_PWM2_Pos (10)
#define | PWM_PHCHGNXT_PWM2_Msk (0x1ul << PWM_PHCHGNXT_PWM2_Pos)
#define | PWM_PHCHGNXT_PWM3_Pos (11)
#define | PWM_PHCHGNXT_PWM3_Msk (0x1ul << PWM_PHCHGNXT_PWM3_Pos)
#define | PWM_PHCHGNXT_PWM4_Pos (12)
#define | PWM_PHCHGNXT_PWM4_Msk (0x1ul << PWM_PHCHGNXT_PWM4_Pos)
#define | PWM_PHCHGNXT_PWM5_Pos (13)
#define | PWM_PHCHGNXT_PWM5_Msk (0x1ul << PWM_PHCHGNXT_PWM5_Pos)
#define | PWM_PHCHGNXT_ACCNT0_Pos (14)
#define | PWM_PHCHGNXT_ACCNT0_Msk (0x1ul << PWM_PHCHGNXT_ACCNT0_Pos)
#define | PWM_PHCHGNXT_ACCNT1_Pos (15)
#define | PWM_PHCHGNXT_ACCNT1_Msk (0x1ul << PWM_PHCHGNXT_ACCNT1_Pos)
#define | PWM_PHCHGNXT_CH01TOFF1_Pos (16)
#define | PWM_PHCHGNXT_CH01TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH01TOFF1_Pos)
#define | PWM_PHCHGNXT_CH11TOFF1_Pos (17)
#define | PWM_PHCHGNXT_CH11TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH11TOFF1_Pos)
#define | PWM_PHCHGNXT_CH21TOFF1_Pos (18)
#define | PWM_PHCHGNXT_CH21TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH21TOFF1_Pos)
#define | PWM_PHCHGNXT_CH31TOFF1_Pos (19)
#define | PWM_PHCHGNXT_CH31TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH31TOFF1_Pos)
#define | PWM_PHCHGNXT_CMP1SEL_Pos (20)
#define | PWM_PHCHGNXT_CMP1SEL_Msk (0x3ul << PWM_PHCHGNXT_CMP1SEL_Pos)
#define | PWM_PHCHGNXT_T1_Pos (22)
#define | PWM_PHCHGNXT_T1_Msk (0x1ul << PWM_PHCHGNXT_T1_Pos)
#define | PWM_PHCHGNXT_CE1_Pos (23)
#define | PWM_PHCHGNXT_CE1_Msk (0x1ul << PWM_PHCHGNXT_CE1_Pos)
#define | PWM_PHCHGNXT_CH01TOFF0_Pos (24)
#define | PWM_PHCHGNXT_CH01TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH01TOFF0_Pos)
#define | PWM_PHCHGNXT_CH11TOFF0_Pos (25)
#define | PWM_PHCHGNXT_CH11TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH11TOFF0_Pos)
#define | PWM_PHCHGNXT_CH21TOFF0_Pos (26)
#define | PWM_PHCHGNXT_CH21TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH21TOFF0_Pos)
#define | PWM_PHCHGNXT_CH31TOFF0_Pos (27)
#define | PWM_PHCHGNXT_CH31TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH31TOFF0_Pos)
#define | PWM_PHCHGNXT_CMP0SEL_Pos (28)
#define | PWM_PHCHGNXT_CMP0SEL_Msk (0x3ul << PWM_PHCHGNXT_CMP0SEL_Pos)
#define | PWM_PHCHGNXT_T0_Pos (30)
#define | PWM_PHCHGNXT_T0_Msk (0x1ul << PWM_PHCHGNXT_T0_Pos)
#define | PWM_PHCHGNXT_CE0_Pos (31)
#define | PWM_PHCHGNXT_CE0_Msk (0x1ul << PWM_PHCHGNXT_CE0_Pos)
#define | PWM_PHCHGMASK_MASK6_Pos (6)
#define | PWM_PHCHGMASK_MASK6_Msk (0x1ul << PWM_PHCHGMASK_MASK6_Pos)
#define | PWM_PHCHGMASK_MASK7_Pos (7)
#define | PWM_PHCHGMASK_MASK7_Msk (0x1ul << PWM_PHCHGMASK_MASK7_Pos)
#define | PWM_PHCHGMASK_CMPMASK_Pos (8)
#define | PWM_PHCHGMASK_CMPMASK_Msk (0x3ul << PWM_PHCHGMASK_CMPMASK_Pos)
#define | PWM_PHCHGMASK_CMPMASK0_Pos (8)
#define | PWM_PHCHGMASK_CMPMASK0_Msk (0x1ul << PWM_PHCHGMASK_CMPMASK0_Pos)
#define | PWM_PHCHGMASK_CMPMASK1_Pos (9)
#define | PWM_PHCHGMASK_CMPMASK1_Msk (0x1ul << PWM_PHCHGMASK_CMPMASK1_Pos)
#define | PWM_INTACCUCTL_INTACCUEN0_Pos (0)
#define | PWM_INTACCUCTL_INTACCUEN0_Msk (0x1ul << PWM_INTACCUCTL_INTACCUEN0_Pos)
#define | PWM_INTACCUCTL_PERIODCNT_Pos (4)
#define | PWM_INTACCUCTL_PERIODCNT_Msk (0xful << PWM_INTACCUCTL_PERIODCNT_Pos)
#define | SPI_CNTRL_GO_BUSY_Pos (0)
#define | SPI_CNTRL_GO_BUSY_Msk (0x1ul << SPI_CNTRL_GO_BUSY_Pos)
#define | SPI_CNTRL_RX_NEG_Pos (1)
#define | SPI_CNTRL_RX_NEG_Msk (0x1ul << SPI_CNTRL_RX_NEG_Pos)
#define | SPI_CNTRL_TX_NEG_Pos (2)
#define | SPI_CNTRL_TX_NEG_Msk (0x1ul << SPI_CNTRL_TX_NEG_Pos)
#define | SPI_CNTRL_TX_BIT_LEN_Pos (3)
#define | SPI_CNTRL_TX_BIT_LEN_Msk (0x1ful << SPI_CNTRL_TX_BIT_LEN_Pos)
#define | SPI_CNTRL_LSB_Pos (10)
#define | SPI_CNTRL_LSB_Msk (0x1ul << SPI_CNTRL_LSB_Pos)
#define | SPI_CNTRL_CLKP_Pos (11)
#define | SPI_CNTRL_CLKP_Msk (0x1ul << SPI_CNTRL_CLKP_Pos)
#define | SPI_CNTRL_SP_CYCLE_Pos (12)
#define | SPI_CNTRL_SP_CYCLE_Msk (0xful << SPI_CNTRL_SP_CYCLE_Pos)
#define | SPI_CNTRL_IF_Pos (16)
#define | SPI_CNTRL_IF_Msk (0x1ul << SPI_CNTRL_IF_Pos)
#define | SPI_CNTRL_IE_Pos (17)
#define | SPI_CNTRL_IE_Msk (0x1ul << SPI_CNTRL_IE_Pos)
#define | SPI_CNTRL_SLAVE_Pos (18)
#define | SPI_CNTRL_SLAVE_Msk (0x1ul << SPI_CNTRL_SLAVE_Pos)
#define | SPI_CNTRL_REORDER_Pos (19)
#define | SPI_CNTRL_REORDER_Msk (0x1ul << SPI_CNTRL_REORDER_Pos)
#define | SPI_CNTRL_FIFO_Pos (21)
#define | SPI_CNTRL_FIFO_Msk (0x1ul << SPI_CNTRL_FIFO_Pos)
#define | SPI_CNTRL_RX_EMPTY_Pos (24)
#define | SPI_CNTRL_RX_EMPTY_Msk (0x1ul << SPI_CNTRL_RX_EMPTY_Pos)
#define | SPI_CNTRL_RX_FULL_Pos (25)
#define | SPI_CNTRL_RX_FULL_Msk (0x1ul << SPI_CNTRL_RX_FULL_Pos)
#define | SPI_CNTRL_TX_EMPTY_Pos (26)
#define | SPI_CNTRL_TX_EMPTY_Msk (0x1ul << SPI_CNTRL_TX_EMPTY_Pos)
#define | SPI_CNTRL_TX_FULL_Pos (27)
#define | SPI_CNTRL_TX_FULL_Msk (0x1ul << SPI_CNTRL_TX_FULL_Pos)
#define | SPI_DIVIDER_DIVIDER_Pos (0)
#define | SPI_DIVIDER_DIVIDER_Msk (0xfful << SPI_DIVIDER_DIVIDER_Pos)
#define | SPI_SSR_SSR_Pos (0)
#define | SPI_SSR_SSR_Msk (0x1ul << SPI_SSR_SSR_Pos)
#define | SPI_SSR_SS_LVL_Pos (2)
#define | SPI_SSR_SS_LVL_Msk (0x1ul << SPI_SSR_SS_LVL_Pos)
#define | SPI_SSR_AUTOSS_Pos (3)
#define | SPI_SSR_AUTOSS_Msk (0x1ul << SPI_SSR_AUTOSS_Pos)
#define | SPI_SSR_SS_LTRIG_Pos (4)
#define | SPI_SSR_SS_LTRIG_Msk (0x1ul << SPI_SSR_SS_LTRIG_Pos)
#define | SPI_SSR_LTRIG_FLAG_Pos (5)
#define | SPI_SSR_LTRIG_FLAG_Msk (0x1ul << SPI_SSR_LTRIG_FLAG_Pos)
#define | SPI_RX_RX_Pos (0)
#define | SPI_RX_RX_Msk (0xfffffffful << SPI_RX_RX_Pos)
#define | SPI_TX_TX_Pos (0)
#define | SPI_TX_TX_Msk (0xfffffffful << SPI_TX_TX_Pos)
#define | SPI_CNTRL2_NOSLVSEL_Pos (8)
#define | SPI_CNTRL2_NOSLVSEL_Msk (0x1ul << SPI_CNTRL2_NOSLVSEL_Pos)
#define | SPI_CNTRL2_SLV_ABORT_Pos (9)
#define | SPI_CNTRL2_SLV_ABORT_Msk (0x1ul << SPI_CNTRL2_SLV_ABORT_Pos)
#define | SPI_CNTRL2_SSTA_INTEN_Pos (10)
#define | SPI_CNTRL2_SSTA_INTEN_Msk (0x1ul << SPI_CNTRL2_SSTA_INTEN_Pos)
#define | SPI_CNTRL2_SLV_START_INTSTS_Pos (11)
#define | SPI_CNTRL2_SLV_START_INTSTS_Msk (0x1ul << SPI_CNTRL2_SLV_START_INTSTS_Pos)
#define | SPI_CNTRL2_SS_INT_OPT_Pos (16)
#define | SPI_CNTRL2_SS_INT_OPT_Msk (0x1ul << SPI_CNTRL2_SS_INT_OPT_Pos)
#define | SPI_CNTRL2_BCn_Pos (31)
#define | SPI_CNTRL2_BCn_Msk (0x1ul << SPI_CNTRL2_BCn_Pos)
#define | SPI_FIFO_CTL_RX_CLR_Pos (0)
#define | SPI_FIFO_CTL_RX_CLR_Msk (0x1ul << SPI_FIFO_CTL_RX_CLR_Pos)
#define | SPI_FIFO_CTL_TX_CLR_Pos (1)
#define | SPI_FIFO_CTL_TX_CLR_Msk (0x1ul << SPI_FIFO_CTL_TX_CLR_Pos)
#define | SPI_FIFO_CTL_RX_INTEN_Pos (2)
#define | SPI_FIFO_CTL_RX_INTEN_Msk (0x1ul << SPI_FIFO_CTL_RX_INTEN_Pos)
#define | SPI_FIFO_CTL_TX_INTEN_Pos (3)
#define | SPI_FIFO_CTL_TX_INTEN_Msk (0x1ul << SPI_FIFO_CTL_TX_INTEN_Pos)
#define | SPI_FIFO_CTL_RXOV_INTEN_Pos (6)
#define | SPI_FIFO_CTL_RXOV_INTEN_Msk (0x1ul << SPI_FIFO_CTL_RXOV_INTEN_Pos)
#define | SPI_FIFO_CTL_TIMEOUT_INTEN_Pos (21)
#define | SPI_FIFO_CTL_TIMEOUT_INTEN_Msk (0x1ul << SPI_FIFO_CTL_TIMEOUT_INTEN_Pos)
#define | SPI_FIFO_CTL_RX_THRESHOLD_Pos (24)
#define | SPI_FIFO_CTL_RX_THRESHOLD_Msk (0x3ul << SPI_FIFO_CTL_RX_THRESHOLD_Pos)
#define | SPI_FIFO_CTL_TX_THRESHOLD_Pos (28)
#define | SPI_FIFO_CTL_TX_THRESHOLD_Msk (0x3ul << SPI_FIFO_CTL_TX_THRESHOLD_Pos)
#define | SPI_STATUS_RX_INTSTS_Pos (0)
#define | SPI_STATUS_RX_INTSTS_Msk (0x1ul << SPI_STATUS_RX_INTSTS_Pos)
#define | SPI_STATUS_RX_OVERRUN_Pos (2)
#define | SPI_STATUS_RX_OVERRUN_Msk (0x1ul << SPI_STATUS_RX_OVERRUN_Pos)
#define | SPI_STATUS_TX_INTSTS_Pos (4)
#define | SPI_STATUS_TX_INTSTS_Msk (0x1ul << SPI_STATUS_TX_INTSTS_Pos)
#define | SPI_STATUS_SLV_START_INTSTS_Pos (11)
#define | SPI_STATUS_SLV_START_INTSTS_Msk (0x1ul << SPI_STATUS_SLV_START_INTSTS_Pos)
#define | SPI_STATUS_RX_FIFO_COUNT_Pos (12)
#define | SPI_STATUS_RX_FIFO_COUNT_Msk (0xful << SPI_STATUS_RX_FIFO_COUNT_Pos)
#define | SPI_STATUS_IF_Pos (16)
#define | SPI_STATUS_IF_Msk (0x1ul << SPI_STATUS_IF_Pos)
#define | SPI_STATUS_TIMEOUT_Pos (20)
#define | SPI_STATUS_TIMEOUT_Msk (0x1ul << SPI_STATUS_TIMEOUT_Pos)
#define | SPI_STATUS_RX_EMPTY_Pos (24)
#define | SPI_STATUS_RX_EMPTY_Msk (0x1ul << SPI_STATUS_RX_EMPTY_Pos)
#define | SPI_STATUS_RX_FULL_Pos (25)
#define | SPI_STATUS_RX_FULL_Msk (0x1ul << SPI_STATUS_RX_FULL_Pos)
#define | SPI_STATUS_TX_EMPTY_Pos (26)
#define | SPI_STATUS_TX_EMPTY_Msk (0x1ul << SPI_STATUS_TX_EMPTY_Pos)
#define | SPI_STATUS_TX_FULL_Pos (27)
#define | SPI_STATUS_TX_FULL_Msk (0x1ul << SPI_STATUS_TX_FULL_Pos)
#define | SPI_STATUS_TX_FIFO_COUNT_Pos (28)
#define | SPI_STATUS_TX_FIFO_COUNT_Msk (0xful << SPI_STATUS_TX_FIFO_COUNT_Pos)
#define | TIMER_TCSR_PRESCALE_Pos (0)
#define | TIMER_TCSR_PRESCALE_Msk (0xfful << TIMER_TCSR_PRESCALE_Pos)
#define | TIMER_TCSR_TDR_EN_Pos (16)
#define | TIMER_TCSR_TDR_EN_Msk (0x1ul << TIMER_TCSR_TDR_EN_Pos)
#define | TIMER_TCSR_PERIODIC_SEL_Pos (17)
#define | TIMER_TCSR_PERIODIC_SEL_Msk (0x1ul << TIMER_TCSR_PERIODIC_SEL_Pos)
#define | TIMER_TCSR_TOGGLE_PIN_Pos (18)
#define | TIMER_TCSR_TOGGLE_PIN_Msk (0x1ul << TIMER_TCSR_TOGGLE_PIN_Pos)
#define | TIMER_TCSR_TOUT_PIN_Pos (18)
#define | TIMER_TCSR_TOUT_PIN_Msk (0x1ul << TIMER_TCSR_TOUT_PIN_Pos)
#define | TIMER_TCSR_CAP_SRC_Pos (19)
#define | TIMER_TCSR_CAP_SRC_Msk (0x1ul << TIMER_TCSR_CAP_SRC_Pos)
#define | TIMER_TCSR_WAKE_EN_Pos (23)
#define | TIMER_TCSR_WAKE_EN_Msk (0x1ul << TIMER_TCSR_WAKE_EN_Pos)
#define | TIMER_TCSR_CTB_Pos (24)
#define | TIMER_TCSR_CTB_Msk (0x1ul << TIMER_TCSR_CTB_Pos)
#define | TIMER_TCSR_CACT_Pos (25)
#define | TIMER_TCSR_CACT_Msk (0x1ul << TIMER_TCSR_CACT_Pos)
#define | TIMER_TCSR_CRST_Pos (26)
#define | TIMER_TCSR_CRST_Msk (0x1ul << TIMER_TCSR_CRST_Pos)
#define | TIMER_TCSR_MODE_Pos (27)
#define | TIMER_TCSR_MODE_Msk (0x3ul << TIMER_TCSR_MODE_Pos)
#define | TIMER_TCSR_IE_Pos (29)
#define | TIMER_TCSR_IE_Msk (0x1ul << TIMER_TCSR_IE_Pos)
#define | TIMER_TCSR_CEN_Pos (30)
#define | TIMER_TCSR_CEN_Msk (0x1ul << TIMER_TCSR_CEN_Pos)
#define | TIMER_TCSR_DBGACK_TMR_Pos (31)
#define | TIMER_TCSR_DBGACK_TMR_Msk (0x1ul << TIMER_TCSR_DBGACK_TMR_Pos)
#define | TIMER_TCMP_TCMP_Pos (0)
#define | TIMER_TCMP_TCMP_Msk (0xfffffful << TIMER_TCMP_TCMP_Pos)
#define | TIMER_TISR_TIF_Pos (0)
#define | TIMER_TISR_TIF_Msk (0x1ul << TIMER_TISR_TIF_Pos)
#define | TIMER_TISR_TWF_Pos (1)
#define | TIMER_TISR_TWF_Msk (0x1ul << TIMER_TISR_TWF_Pos)
#define | TIMER_TDR_TDR_Pos (0)
#define | TIMER_TDR_TDR_Msk (0xfffffful << TIMER_TDR_TDR_Pos)
#define | TIMER_TCAP_TCAP_Pos (0)
#define | TIMER_TCAP_TCAP_Msk (0xfffffful << TIMER_TCAP_TCAP_Pos)
#define | TIMER_TEXCON_TX_PHASE_Pos (0)
#define | TIMER_TEXCON_TX_PHASE_Msk (0x1ul << TIMER_TEXCON_TX_PHASE_Pos)
#define | TIMER_TEXCON_TEX_EDGE_Pos (1)
#define | TIMER_TEXCON_TEX_EDGE_Msk (0x3ul << TIMER_TEXCON_TEX_EDGE_Pos)
#define | TIMER_TEXCON_TEXEN_Pos (3)
#define | TIMER_TEXCON_TEXEN_Msk (0x1ul << TIMER_TEXCON_TEXEN_Pos)
#define | TIMER_TEXCON_RSTCAPSEL_Pos (4)
#define | TIMER_TEXCON_RSTCAPSEL_Msk (0x1ul << TIMER_TEXCON_RSTCAPSEL_Pos)
#define | TIMER_TEXCON_TEXIEN_Pos (5)
#define | TIMER_TEXCON_TEXIEN_Msk (0x1ul << TIMER_TEXCON_TEXIEN_Pos)
#define | TIMER_TEXCON_TEXDB_Pos (6)
#define | TIMER_TEXCON_TEXDB_Msk (0x1ul << TIMER_TEXCON_TEXDB_Pos)
#define | TIMER_TEXCON_TCDB_Pos (7)
#define | TIMER_TEXCON_TCDB_Msk (0x1ul << TIMER_TEXCON_TCDB_Pos)
#define | TIMER_TEXCON_CAP_MODE_Pos (8)
#define | TIMER_TEXCON_CAP_MODE_Msk (0x1ul << TIMER_TEXCON_CAP_MODE_Pos)
#define | TIMER_TEXISR_TEXIF_Pos (0)
#define | TIMER_TEXISR_TEXIF_Msk (0x1ul << TIMER_TEXISR_TEXIF_Pos)
#define | UART_RBR_RBR_Pos (0)
#define | UART_RBR_RBR_Msk (0xfful << UART_RBR_RBR_Pos)
#define | UART_THR_THR_Pos (0)
#define | UART_THR_THR_Msk (0xfful << UART_THR_THR_Pos)
#define | UART_IER_RDA_IEN_Pos (0)
#define | UART_IER_RDA_IEN_Msk (0x1ul << UART_IER_RDA_IEN_Pos)
#define | UART_IER_THRE_IEN_Pos (1)
#define | UART_IER_THRE_IEN_Msk (0x1ul << UART_IER_THRE_IEN_Pos)
#define | UART_IER_RLS_IEN_Pos (2)
#define | UART_IER_RLS_IEN_Msk (0x1ul << UART_IER_RLS_IEN_Pos)
#define | UART_IER_MODEM_IEN_Pos (3)
#define | UART_IER_MODEM_IEN_Msk (0x1ul << UART_IER_MODEM_IEN_Pos)
#define | UART_IER_RTO_IEN_Pos (4)
#define | UART_IER_RTO_IEN_Msk (0x1ul << UART_IER_RTO_IEN_Pos)
#define | UART_IER_BUF_ERR_IEN_Pos (5)
#define | UART_IER_BUF_ERR_IEN_Msk (0x1ul << UART_IER_BUF_ERR_IEN_Pos)
#define | UART_IER_WAKE_EN_Pos (6)
#define | UART_IER_WAKE_EN_Msk (0x1ul << UART_IER_WAKE_EN_Pos)
#define | UART_IER_TIME_OUT_EN_Pos (11)
#define | UART_IER_TIME_OUT_EN_Msk (0x1ul << UART_IER_TIME_OUT_EN_Pos)
#define | UART_IER_AUTO_RTS_EN_Pos (12)
#define | UART_IER_AUTO_RTS_EN_Msk (0x1ul << UART_IER_AUTO_RTS_EN_Pos)
#define | UART_IER_AUTO_CTS_EN_Pos (13)
#define | UART_IER_AUTO_CTS_EN_Msk (0x1ul << UART_IER_AUTO_CTS_EN_Pos)
#define | UART_FCR_RFR_Pos (1)
#define | UART_FCR_RFR_Msk (0x1ul << UART_FCR_RFR_Pos)
#define | UART_FCR_TFR_Pos (2)
#define | UART_FCR_TFR_Msk (0x1ul << UART_FCR_TFR_Pos)
#define | UART_FCR_RFITL_Pos (4)
#define | UART_FCR_RFITL_Msk (0xful << UART_FCR_RFITL_Pos)
#define | UART_FCR_RX_DIS_Pos (8)
#define | UART_FCR_RX_DIS_Msk (0x1ul << UART_FCR_RX_DIS_Pos)
#define | UART_FCR_RTS_TRI_LEV_Pos (16)
#define | UART_FCR_RTS_TRI_LEV_Msk (0xful << UART_FCR_RTS_TRI_LEV_Pos)
#define | UART_LCR_WLS_Pos (0)
#define | UART_LCR_WLS_Msk (0x3ul << UART_LCR_WLS_Pos)
#define | UART_LCR_NSB_Pos (2)
#define | UART_LCR_NSB_Msk (0x1ul << UART_LCR_NSB_Pos)
#define | UART_LCR_PBE_Pos (3)
#define | UART_LCR_PBE_Msk (0x1ul << UART_LCR_PBE_Pos)
#define | UART_LCR_EPE_Pos (4)
#define | UART_LCR_EPE_Msk (0x1ul << UART_LCR_EPE_Pos)
#define | UART_LCR_SPE_Pos (5)
#define | UART_LCR_SPE_Msk (0x1ul << UART_LCR_SPE_Pos)
#define | UART_LCR_BCB_Pos (6)
#define | UART_LCR_BCB_Msk (0x1ul << UART_LCR_BCB_Pos)
#define | UART_MCR_RTS_Pos (1)
#define | UART_MCR_RTS_Msk (0x1ul << UART_MCR_RTS_Pos)
#define | UART_MCR_LEV_RTS_Pos (9)
#define | UART_MCR_LEV_RTS_Msk (0x1ul << UART_MCR_LEV_RTS_Pos)
#define | UART_MCR_RTS_ST_Pos (13)
#define | UART_MCR_RTS_ST_Msk (0x1ul << UART_MCR_RTS_ST_Pos)
#define | UART_MSR_DCTSF_Pos (0)
#define | UART_MSR_DCTSF_Msk (0x1ul << UART_MSR_DCTSF_Pos)
#define | UART_MSR_CTS_ST_Pos (4)
#define | UART_MSR_CTS_ST_Msk (0x1ul << UART_MSR_CTS_ST_Pos)
#define | UART_MSR_LEV_CTS_Pos (8)
#define | UART_MSR_LEV_CTS_Msk (0x1ul << UART_MSR_LEV_CTS_Pos)
#define | UART_FSR_RX_OVER_IF_Pos (0)
#define | UART_FSR_RX_OVER_IF_Msk (0x1ul << UART_FSR_RX_OVER_IF_Pos)
#define | UART_FSR_RS485_ADD_DETF_Pos (3)
#define | UART_FSR_RS485_ADD_DETF_Msk (0x1ul << UART_FSR_RS485_ADD_DETF_Pos)
#define | UART_FSR_PEF_Pos (4)
#define | UART_FSR_PEF_Msk (0x1ul << UART_FSR_PEF_Pos)
#define | UART_FSR_FEF_Pos (5)
#define | UART_FSR_FEF_Msk (0x1ul << UART_FSR_FEF_Pos)
#define | UART_FSR_BIF_Pos (6)
#define | UART_FSR_BIF_Msk (0x1ul << UART_FSR_BIF_Pos)
#define | UART_FSR_RX_POINTER_Pos (8)
#define | UART_FSR_RX_POINTER_Msk (0x3ful << UART_FSR_RX_POINTER_Pos)
#define | UART_FSR_RX_EMPTY_Pos (14)
#define | UART_FSR_RX_EMPTY_Msk (0x1ul << UART_FSR_RX_EMPTY_Pos)
#define | UART_FSR_RX_FULL_Pos (15)
#define | UART_FSR_RX_FULL_Msk (0x1ul << UART_FSR_RX_FULL_Pos)
#define | UART_FSR_TX_POINTER_Pos (16)
#define | UART_FSR_TX_POINTER_Msk (0x3ful << UART_FSR_TX_POINTER_Pos)
#define | UART_FSR_TX_EMPTY_Pos (22)
#define | UART_FSR_TX_EMPTY_Msk (0x1ul << UART_FSR_TX_EMPTY_Pos)
#define | UART_FSR_TX_FULL_Pos (23)
#define | UART_FSR_TX_FULL_Msk (0x1ul << UART_FSR_TX_FULL_Pos)
#define | UART_FSR_TX_OVER_IF_Pos (24)
#define | UART_FSR_TX_OVER_IF_Msk (0x1ul << UART_FSR_TX_OVER_IF_Pos)
#define | UART_FSR_TE_FLAG_Pos (28)
#define | UART_FSR_TE_FLAG_Msk (0x1ul << UART_FSR_TE_FLAG_Pos)
#define | UART_ISR_RDA_IF_Pos (0)
#define | UART_ISR_RDA_IF_Msk (0x1ul << UART_ISR_RDA_IF_Pos)
#define | UART_ISR_THRE_IF_Pos (1)
#define | UART_ISR_THRE_IF_Msk (0x1ul << UART_ISR_THRE_IF_Pos)
#define | UART_ISR_RLS_IF_Pos (2)
#define | UART_ISR_RLS_IF_Msk (0x1ul << UART_ISR_RLS_IF_Pos)
#define | UART_ISR_MODEM_IF_Pos (3)
#define | UART_ISR_MODEM_IF_Msk (0x1ul << UART_ISR_MODEM_IF_Pos)
#define | UART_ISR_TOUT_IF_Pos (4)
#define | UART_ISR_TOUT_IF_Msk (0x1ul << UART_ISR_TOUT_IF_Pos)
#define | UART_ISR_BUF_ERR_IF_Pos (5)
#define | UART_ISR_BUF_ERR_IF_Msk (0x1ul << UART_ISR_BUF_ERR_IF_Pos)
#define | UART_ISR_RDA_INT_Pos (8)
#define | UART_ISR_RDA_INT_Msk (0x1ul << UART_ISR_RDA_INT_Pos)
#define | UART_ISR_THRE_INT_Pos (9)
#define | UART_ISR_THRE_INT_Msk (0x1ul << UART_ISR_THRE_INT_Pos)
#define | UART_ISR_RLS_INT_Pos (10)
#define | UART_ISR_RLS_INT_Msk (0x1ul << UART_ISR_RLS_INT_Pos)
#define | UART_ISR_MODEM_INT_Pos (11)
#define | UART_ISR_MODEM_INT_Msk (0x1ul << UART_ISR_MODEM_INT_Pos)
#define | UART_ISR_TOUT_INT_Pos (12)
#define | UART_ISR_TOUT_INT_Msk (0x1ul << UART_ISR_TOUT_INT_Pos)
#define | UART_ISR_BUF_ERR_INT_Pos (13)
#define | UART_ISR_BUF_ERR_INT_Msk (0x1ul << UART_ISR_BUF_ERR_INT_Pos)
#define | UART_TOR_TOIC_Pos (0)
#define | UART_TOR_TOIC_Msk (0xfful << UART_TOR_TOIC_Pos)
#define | UART_TOR_DLY_Pos (8)
#define | UART_TOR_DLY_Msk (0xfful << UART_TOR_DLY_Pos)
#define | UART_BAUD_BRD_Pos (0)
#define | UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)
#define | UART_BAUD_DIVIDER_X_Pos (24)
#define | UART_BAUD_DIVIDER_X_Msk (0xful << UART_BAUD_DIVIDER_X_Pos)
#define | UART_BAUD_DIV_X_ONE_Pos (28)
#define | UART_BAUD_DIV_X_ONE_Msk (0x1ul << UART_BAUD_DIV_X_ONE_Pos)
#define | UART_BAUD_DIV_X_EN_Pos (29)
#define | UART_BAUD_DIV_X_EN_Msk (0x1ul << UART_BAUD_DIV_X_EN_Pos)
#define | UART_IRCR_TX_SELECT_Pos (1)
#define | UART_IRCR_TX_SELECT_Msk (0x1ul << UART_IRCR_TX_SELECT_Pos)
#define | UART_IRCR_INV_TX_Pos (5)
#define | UART_IRCR_INV_TX_Msk (0x1ul << UART_IRCR_INV_TX_Pos)
#define | UART_IRCR_INV_RX_Pos (6)
#define | UART_IRCR_INV_RX_Msk (0x1ul << UART_IRCR_INV_RX_Pos)
#define | UART_ALT_CSR_RS485_NMM_Pos (8)
#define | UART_ALT_CSR_RS485_NMM_Msk (0x1ul << UART_ALT_CSR_RS485_NMM_Pos)
#define | UART_ALT_CSR_RS485_AAD_Pos (9)
#define | UART_ALT_CSR_RS485_AAD_Msk (0x1ul << UART_ALT_CSR_RS485_AAD_Pos)
#define | UART_ALT_CSR_RS485_AUD_Pos (10)
#define | UART_ALT_CSR_RS485_AUD_Msk (0x1ul << UART_ALT_CSR_RS485_AUD_Pos)
#define | UART_ALT_CSR_RS485_ADD_EN_Pos (15)
#define | UART_ALT_CSR_RS485_ADD_EN_Msk (0x1ul << UART_ALT_CSR_RS485_ADD_EN_Pos)
#define | UART_ALT_CSR_ADDR_MATCH_Pos (24)
#define | UART_ALT_CSR_ADDR_MATCH_Msk (0xfful << UART_ALT_CSR_ADDR_MATCH_Pos)
#define | UART_FUN_SEL_FUN_SEL_Pos (0)
#define | UART_FUN_SEL_FUN_SEL_Msk (0x3ul << UART_FUN_SEL_FUN_SEL_Pos)
#define | WDT_WTCR_WTR_Pos (0)
#define | WDT_WTCR_WTR_Msk (0x1ul << WDT_WTCR_WTR_Pos)
#define | WDT_WTCR_WTRE_Pos (1)
#define | WDT_WTCR_WTRE_Msk (0x1ul << WDT_WTCR_WTRE_Pos)
#define | WDT_WTCR_WTRF_Pos (2)
#define | WDT_WTCR_WTRF_Msk (0x1ul << WDT_WTCR_WTRF_Pos)
#define | WDT_WTCR_WTIF_Pos (3)
#define | WDT_WTCR_WTIF_Msk (0x1ul << WDT_WTCR_WTIF_Pos)
#define | WDT_WTCR_WTWKE_Pos (4)
#define | WDT_WTCR_WTWKE_Msk (0x1ul << WDT_WTCR_WTWKE_Pos)
#define | WDT_WTCR_WTWKF_Pos (5)
#define | WDT_WTCR_WTWKF_Msk (0x1ul << WDT_WTCR_WTWKF_Pos)
#define | WDT_WTCR_WTIE_Pos (6)
#define | WDT_WTCR_WTIE_Msk (0x1ul << WDT_WTCR_WTIE_Pos)
#define | WDT_WTCR_WTE_Pos (7)
#define | WDT_WTCR_WTE_Msk (0x1ul << WDT_WTCR_WTE_Pos)
#define | WDT_WTCR_WTIS_Pos (8)
#define | WDT_WTCR_WTIS_Msk (0x7ul << WDT_WTCR_WTIS_Pos)
#define | WDT_WTCR_DBGACK_WDT_Pos (31)
#define | WDT_WTCR_DBGACK_WDT_Msk (0x1ul << WDT_WTCR_DBGACK_WDT_Pos)

## Typedefs
typedef enum IRQn | IRQn_Type
typedef volatile unsigned char | vu8
| Define 8-bit unsigned volatile data type. More...
typedef volatile unsigned short | vu16
| Define 16-bit unsigned volatile data type. More...
typedef volatile unsigned long | vu32
| Define 32-bit unsigned volatile data type. More...

## Enumerations
enum | IRQn { NonMaskableInt_IRQn = -14 , HardFault_IRQn = -13 , SVCall_IRQn = -5 , PendSV_IRQn = -2 , SysTick_IRQn = -1 , BOD_IRQn = 0 , WDT_IRQn = 1 , EINT0_IRQn = 2 , EINT1_IRQn = 3 , GPIO01_IRQn = 4 , GPIO234_IRQn = 5 , PWM_IRQn = 6 , FB_IRQn = 7 , TMR0_IRQn = 8 , TMR1_IRQn = 9 , UART_IRQn = 12 , SPI_IRQn = 14 , GPIO5_IRQn = 16 , HIRC_IRQn = 17 , I2C_IRQn = 18 , ACMP_IRQn = 25 , PDWU_IRQn = 28 , ADC_IRQn = 29 }

## Detailed Description

Mini51 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Mini51 series MCU.

Version
  V1.00

Revision
  43

Date
  16/06/08 1:55p

Note
  Copyright (C) 2018 Nuvoton Technology Corp. All rights reserved.

Definition in file Mini51Series.h.

## Macro Definition Documentation

## ◆ FMC_DFBADR_DFBA_Msk

#define FMC_DFBADR_DFBA_Msk (0xfffffffful << FMC_DFBA_DFBA_Pos)

FMC_T::DFBADR: DFBA Mask

Definition at line 1174 of file Mini51Series.h.

## ◆ FMC_DFBADR_DFBA_Pos

#define FMC_DFBADR_DFBA_Pos (0)

FMC_T::DFBADR: DFBA Position

Definition at line 1173 of file Mini51Series.h.

## ◆ FMC_ISPADR_ISPADR_Msk

#define FMC_ISPADR_ISPADR_Msk (0xfffffffful << FMC_ISPADR_ISPADR_Pos)

FMC_T::ISPADR: ISPADR Mask

Definition at line 1162 of file Mini51Series.h.

## ◆ FMC_ISPADR_ISPADR_Pos

#define FMC_ISPADR_ISPADR_Pos (0)

FMC_T::ISPADR: ISPADR Position

Definition at line 1161 of file Mini51Series.h.

## ◆ FMC_ISPCMD_ISPCMD_Msk

#define FMC_ISPCMD_ISPCMD_Msk (0x3ful << FMC_ISPCMD_ISPCMD_Pos)

FMC_T::ISPCMD: ISPCMD Mask

Definition at line 1168 of file Mini51Series.h.

## ◆ FMC_ISPCMD_ISPCMD_Pos

#define FMC_ISPCMD_ISPCMD_Pos (0)

FMC_T::ISPCMD: ISPCMD Position

Definition at line 1167 of file Mini51Series.h.

## ◆ FMC_ISPCON_APUEN_Msk

#define FMC_ISPCON_APUEN_Msk (0x1ul << FMC_ISPCON_APUEN_Pos)

FMC_T::ISPCON: APUEN Mask

Definition at line 1150 of file Mini51Series.h.

## ◆ FMC_ISPCON_APUEN_Pos

#define FMC_ISPCON_APUEN_Pos (3)

FMC_T::ISPCON: APUEN Position

Definition at line 1149 of file Mini51Series.h.

## ◆ FMC_ISPCON_BS_Msk

#define FMC_ISPCON_BS_Msk (0x1ul << FMC_ISPCON_BS_Pos)

FMC_T::ISPCON: BS Mask

Definition at line 1147 of file Mini51Series.h.

## ◆ FMC_ISPCON_BS_Pos

#define FMC_ISPCON_BS_Pos (1)

FMC_T::ISPCON: BS Position

Definition at line 1146 of file Mini51Series.h.

## ◆ FMC_ISPCON_CFGUEN_Msk

#define FMC_ISPCON_CFGUEN_Msk (0x1ul << FMC_ISPCON_CFGUEN_Pos)

FMC_T::ISPCON: CFGUEN Mask

Definition at line 1153 of file Mini51Series.h.

## ◆ FMC_ISPCON_CFGUEN_Pos

#define FMC_ISPCON_CFGUEN_Pos (4)

FMC_T::ISPCON: CFGUEN Position

Definition at line 1152 of file Mini51Series.h.

## ◆ FMC_ISPCON_ISPEN_Msk

#define FMC_ISPCON_ISPEN_Msk (0x1ul << FMC_ISPCON_ISPEN_Pos)

FMC_T::ISPCON: ISPEN Mask

Definition at line 1144 of file Mini51Series.h.

## ◆ FMC_ISPCON_ISPEN_Pos

#define FMC_ISPCON_ISPEN_Pos (0)

    @addtogroup FMC_CONST FMC Bit Field Definition
    Constant Definitions for FMC Controller

FMC_T::ISPCON: ISPEN Position

Definition at line 1143 of file Mini51Series.h.

## ◆ FMC_ISPCON_ISPFF_Msk

#define FMC_ISPCON_ISPFF_Msk (0x1ul << FMC_ISPCON_ISPFF_Pos)

FMC_T::ISPCON: ISPFF Mask

Definition at line 1159 of file Mini51Series.h.

## ◆ FMC_ISPCON_ISPFF_Pos

#define FMC_ISPCON_ISPFF_Pos (6)

FMC_T::ISPCON: ISPFF Position

Definition at line 1158 of file Mini51Series.h.

## ◆ FMC_ISPCON_LDUEN_Msk

#define FMC_ISPCON_LDUEN_Msk (0x1ul << FMC_ISPCON_LDUEN_Pos)

FMC_T::ISPCON: LDUEN Mask

Definition at line 1156 of file Mini51Series.h.

## ◆ FMC_ISPCON_LDUEN_Pos

#define FMC_ISPCON_LDUEN_Pos (5)

FMC_T::ISPCON: LDUEN Position

Definition at line 1155 of file Mini51Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Msk

#define FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)

FMC_T::ISPDAT: ISPDAT Mask

Definition at line 1165 of file Mini51Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Pos

#define FMC_ISPDAT_ISPDAT_Pos (0)

FMC_T::ISPDAT: ISPDAT Position

Definition at line 1164 of file Mini51Series.h.

## ◆ FMC_ISPSTA_CBS_Msk

#define FMC_ISPSTA_CBS_Msk (0x3ul << FMC_ISPSTA_CBS_Pos)

FMC_T::ISPSTA: CBS Mask

Definition at line 1180 of file Mini51Series.h.

## ◆ FMC_ISPSTA_CBS_Pos

#define FMC_ISPSTA_CBS_Pos (1)

FMC_T::ISPSTA: CBS Position

Definition at line 1179 of file Mini51Series.h.

## ◆ FMC_ISPSTA_ISPFF_Msk

#define FMC_ISPSTA_ISPFF_Msk (0x1ul << FMC_ISPSTA_ISPFF_Pos)

FMC_T::ISPSTA: ISPFF Mask

Definition at line 1183 of file Mini51Series.h.

## ◆ FMC_ISPSTA_ISPFF_Pos

#define FMC_ISPSTA_ISPFF_Pos (6)

FMC_T::ISPSTA: ISPFF Position

Definition at line 1182 of file Mini51Series.h.

## ◆ FMC_ISPSTA_ISPGO_Msk

#define FMC_ISPSTA_ISPGO_Msk (0x1ul << FMC_ISPSTA_ISPGO_Pos)

FMC_T::ISPSTA: ISPGO Mask

Definition at line 1177 of file Mini51Series.h.

## ◆ FMC_ISPSTA_ISPGO_Pos

#define FMC_ISPSTA_ISPGO_Pos (0)

FMC_T::ISPSTA: ISPGO Position

Definition at line 1176 of file Mini51Series.h.

## ◆ FMC_ISPSTA_VECMAP_Msk

#define FMC_ISPSTA_VECMAP_Msk (0xffful << FMC_ISPSTA_VECMAP_Pos)

FMC_T::ISPSTA: VECMAP Mask

Definition at line 1186 of file Mini51Series.h.

## ◆ FMC_ISPSTA_VECMAP_Pos

#define FMC_ISPSTA_VECMAP_Pos (9)

FMC_T::ISPSTA: VECMAP Position

Definition at line 1185 of file Mini51Series.h.

## ◆ FMC_ISPTRG_ISPGO_Msk

#define FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)

FMC_T::ISPTRG: ISPGO Mask

Definition at line 1171 of file Mini51Series.h.

## ◆ FMC_ISPTRG_ISPGO_Pos

#define FMC_ISPTRG_ISPGO_Pos (0)

FMC_T::ISPTRG: ISPGO Position

Definition at line 1170 of file Mini51Series.h.

## ◆ GPIO_DBEN_DBEN_Msk

#define GPIO_DBEN_DBEN_Msk (0xfful << GPIO_DBEN_DBEN_Pos)

GPIO_T::DBEN: DBEN Mask

Definition at line 2168 of file Mini51Series.h.

## ◆ GPIO_DBEN_DBEN_Pos

#define GPIO_DBEN_DBEN_Pos (0)

GPIO_T::DBEN: DBEN Position

Definition at line 2167 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_DBCLKSEL_Msk

#define GPIO_DBNCECON_DBCLKSEL_Msk (0xful << GPIO_DBNCECON_DBCLKSEL_Pos)

GPIO_DBNCECON_T::DBNCECON: DBCLKSEL Mask

Definition at line 2183 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_DBCLKSEL_Pos

#define GPIO_DBNCECON_DBCLKSEL_Pos (0)

GPIO_DBNCECON_T::DBNCECON: DBCLKSEL Position

Definition at line 2182 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_DBCLKSRC_Msk

#define GPIO_DBNCECON_DBCLKSRC_Msk (0x1ul << GPIO_DBNCECON_DBCLKSRC_Pos)

GPIO_DBNCECON_T::DBNCECON: DBCLKSRC Mask

Definition at line 2186 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_DBCLKSRC_Pos

#define GPIO_DBNCECON_DBCLKSRC_Pos (4)

GPIO_DBNCECON_T::DBNCECON: DBCLKSRC Position

Definition at line 2185 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_ICLK_ON_Msk

#define GPIO_DBNCECON_ICLK_ON_Msk (0x1ul << GPIO_DBNCECON_ICLK_ON_Pos)

GPIO_DBNCECON_T::DBNCECON: ICLK_ON Mask

Definition at line 2189 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_ICLK_ON_Pos

#define GPIO_DBNCECON_ICLK_ON_Pos (5)

GPIO_DBNCECON_T::DBNCECON: ICLK_ON Position

Definition at line 2188 of file Mini51Series.h.

## ◆ GPIO_DMASK_DMASK_Msk

#define GPIO_DMASK_DMASK_Msk (0xfful << GPIO_DMASK_DMASK_Pos)

GPIO_T::DMASK: DMASK Mask

Definition at line 2162 of file Mini51Series.h.

## ◆ GPIO_DMASK_DMASK_Pos

#define GPIO_DMASK_DMASK_Pos (0)

GPIO_T::DMASK: DMASK Position

Definition at line 2161 of file Mini51Series.h.

## ◆ GPIO_DOUT_DOUT_Msk

#define GPIO_DOUT_DOUT_Msk (0xfful << GPIO_DOUT_DOUT_Pos)

GPIO_T::DOUT: DOUT Mask

Definition at line 2159 of file Mini51Series.h.

## ◆ GPIO_DOUT_DOUT_Pos

#define GPIO_DOUT_DOUT_Pos (0)

GPIO_T::DOUT: DOUT Position

Definition at line 2158 of file Mini51Series.h.

## ◆ GPIO_IEN_IF_EN_Msk

#define GPIO_IEN_IF_EN_Msk (0x1ul << GPIO_IEN_IF_EN_Pos)

GPIO_T::IEN: IF_EN Mask

Definition at line 2174 of file Mini51Series.h.

## ◆ GPIO_IEN_IF_EN_Pos

#define GPIO_IEN_IF_EN_Pos (0)

GPIO_T::IEN: IF_EN Position

Definition at line 2173 of file Mini51Series.h.

## ◆ GPIO_IEN_IR_EN_Msk

#define GPIO_IEN_IR_EN_Msk (0xfful << GPIO_IEN_IR_EN_Pos)

GPIO_T::IEN: IR_EN Mask

Definition at line 2177 of file Mini51Series.h.

## ◆ GPIO_IEN_IR_EN_Pos

#define GPIO_IEN_IR_EN_Pos (16)

GPIO_T::IEN: IR_EN Position

Definition at line 2176 of file Mini51Series.h.

## ◆ GPIO_IMD_IMD_Msk

#define GPIO_IMD_IMD_Msk (0xfful << GPIO_IMD_IMD_Pos)

GPIO_T::IMD: IMD Mask

Definition at line 2171 of file Mini51Series.h.

## ◆ GPIO_IMD_IMD_Pos

#define GPIO_IMD_IMD_Pos (0)

GPIO_T::IMD: IMD Position

Definition at line 2170 of file Mini51Series.h.

## ◆ GPIO_ISRC_ISRC_Msk

#define GPIO_ISRC_ISRC_Msk (0xfful << GPIO_ISRC_ISRC_Pos)

GPIO_T::ISRC: ISRC Mask

Definition at line 2180 of file Mini51Series.h.

## ◆ GPIO_ISRC_ISRC_Pos

#define GPIO_ISRC_ISRC_Pos (0)

GPIO_T::ISRC: ISRC Position

Definition at line 2179 of file Mini51Series.h.

## ◆ GPIO_OFFD_OFFD_Msk

#define GPIO_OFFD_OFFD_Msk (0xfful << GPIO_OFFD_OFFD_Pos)

GPIO_T::OFFD: OFFD Mask

Definition at line 2156 of file Mini51Series.h.

## ◆ GPIO_OFFD_OFFD_Pos

#define GPIO_OFFD_OFFD_Pos (16)

GPIO_T::OFFD: OFFD Position

Definition at line 2155 of file Mini51Series.h.

## ◆ GPIO_PIN_PIN_Msk

#define GPIO_PIN_PIN_Msk (0xfful << GPIO_PIN_PIN_Pos)

GPIO_T::PIN: PIN Mask

Definition at line 2165 of file Mini51Series.h.

## ◆ GPIO_PIN_PIN_Pos

#define GPIO_PIN_PIN_Pos (0)

GPIO_T::PIN: PIN Position

Definition at line 2164 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD0_Msk

#define GPIO_PMD_PMD0_Msk (0x3ul << GPIO_PMD_PMD0_Pos)

GPIO_T::PMD: PMD0 Mask

Definition at line 2132 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD0_Pos

#define GPIO_PMD_PMD0_Pos (0)

    @addtogroup GP_CONST GP Bit Field Definition
    Constant Definitions for GP Controller

GPIO_T::PMD: PMD0 Position

Definition at line 2131 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD1_Msk

#define GPIO_PMD_PMD1_Msk (0x3ul << GPIO_PMD_PMD1_Pos)

GPIO_T::PMD: PMD1 Mask

Definition at line 2135 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD1_Pos

#define GPIO_PMD_PMD1_Pos (2)

GPIO_T::PMD: PMD1 Position

Definition at line 2134 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD2_Msk

#define GPIO_PMD_PMD2_Msk (0x3ul << GPIO_PMD_PMD2_Pos)

GPIO_T::PMD: PMD2 Mask

Definition at line 2138 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD2_Pos

#define GPIO_PMD_PMD2_Pos (4)

GPIO_T::PMD: PMD2 Position

Definition at line 2137 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD3_Msk

#define GPIO_PMD_PMD3_Msk (0x3ul << GPIO_PMD_PMD3_Pos)

GPIO_T::PMD: PMD3 Mask

Definition at line 2141 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD3_Pos

#define GPIO_PMD_PMD3_Pos (6)

GPIO_T::PMD: PMD3 Position

Definition at line 2140 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD4_Msk

#define GPIO_PMD_PMD4_Msk (0x3ul << GPIO_PMD_PMD4_Pos)

GPIO_T::PMD: PMD4 Mask

Definition at line 2144 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD4_Pos

#define GPIO_PMD_PMD4_Pos (8)

GPIO_T::PMD: PMD4 Position

Definition at line 2143 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD5_Msk

#define GPIO_PMD_PMD5_Msk (0x3ul << GPIO_PMD_PMD5_Pos)

GPIO_T::PMD: PMD5 Mask

Definition at line 2147 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD5_Pos

#define GPIO_PMD_PMD5_Pos (10)

GPIO_T::PMD: PMD5 Position

Definition at line 2146 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD6_Msk

#define GPIO_PMD_PMD6_Msk (0x3ul << GPIO_PMD_PMD6_Pos)

GPIO_T::PMD: PMD6 Mask

Definition at line 2150 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD6_Pos

#define GPIO_PMD_PMD6_Pos (12)

GPIO_T::PMD: PMD6 Position

Definition at line 2149 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD7_Msk

#define GPIO_PMD_PMD7_Msk (0x3ul << GPIO_PMD_PMD7_Pos)

GPIO_T::PMD: PMD7 Mask

Definition at line 2153 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD7_Pos

#define GPIO_PMD_PMD7_Pos (14)

GPIO_T::PMD: PMD7 Position

Definition at line 2152 of file Mini51Series.h.

## ◆ I2C_I2CADDR_GC_Msk

#define I2C_I2CADDR_GC_Msk (0x1ul << I2C_I2CADDR_GC_Pos)

I2C_T::I2CADDR0: GC Mask

Definition at line 2456 of file Mini51Series.h.

## ◆ I2C_I2CADDR_GC_Pos

#define I2C_I2CADDR_GC_Pos (0)

I2C_T::I2CADDR0: GC Position

Definition at line 2455 of file Mini51Series.h.

## ◆ I2C_I2CADDR_I2CADDR_Msk

#define I2C_I2CADDR_I2CADDR_Msk (0x7ful << I2C_I2CADDR_I2CADDR_Pos)

I2C_T::I2CADDR0: I2CADDR Mask

Definition at line 2459 of file Mini51Series.h.

## ◆ I2C_I2CADDR_I2CADDR_Pos

#define I2C_I2CADDR_I2CADDR_Pos (1)

I2C_T::I2CADDR0: I2CADDR Position

Definition at line 2458 of file Mini51Series.h.

## ◆ I2C_I2CADM_I2CADM_Msk

#define I2C_I2CADM_I2CADM_Msk (0x7ful << I2C_I2CADM_I2CADM_Pos)

I2C_T::I2CADM0: I2CADM Mask

Definition at line 2480 of file Mini51Series.h.

## ◆ I2C_I2CADM_I2CADM_Pos

#define I2C_I2CADM_I2CADM_Pos (1)

I2C_T::I2CADM0: I2CADM Position

Definition at line 2479 of file Mini51Series.h.

## ◆ I2C_I2CDAT_I2CDAT_Msk

#define I2C_I2CDAT_I2CDAT_Msk (0xfful << I2C_I2CDAT_I2CDAT_Pos)

I2C_T::I2CDAT: I2CDAT Mask

Definition at line 2462 of file Mini51Series.h.

## ◆ I2C_I2CDAT_I2CDAT_Pos

#define I2C_I2CDAT_I2CDAT_Pos (0)

I2C_T::I2CDAT: I2CDAT Position

Definition at line 2461 of file Mini51Series.h.

## ◆ I2C_I2CLK_I2CLK_Msk

#define I2C_I2CLK_I2CLK_Msk (0xfful << I2C_I2CLK_I2CLK_Pos)

I2C_T::I2CLK: I2CLK Mask

Definition at line 2468 of file Mini51Series.h.

## ◆ I2C_I2CLK_I2CLK_Pos

#define I2C_I2CLK_I2CLK_Pos (0)

I2C_T::I2CLK: I2CLK Position

Definition at line 2467 of file Mini51Series.h.

## ◆ I2C_I2CON2_NOSTRETCH_Msk

#define I2C_I2CON2_NOSTRETCH_Msk (0x1ul << I2C_I2CON2_NOSTRETCH_Pos)

I2C_T::I2CON2: NOSTRETCH Mask

Definition at line 2489 of file Mini51Series.h.

## ◆ I2C_I2CON2_NOSTRETCH_Pos

#define I2C_I2CON2_NOSTRETCH_Pos (2)

I2C_T::I2CON2: NOSTRETCH Position

Definition at line 2488 of file Mini51Series.h.

## ◆ I2C_I2CON2_OVER_INTEN_Msk

#define I2C_I2CON2_OVER_INTEN_Msk (0x1ul << I2C_I2CON2_OVER_INTEN_Pos)

I2C_T::I2CON2: OVER_INTEN Mask

Definition at line 2492 of file Mini51Series.h.

## ◆ I2C_I2CON2_OVER_INTEN_Pos

#define I2C_I2CON2_OVER_INTEN_Pos (3)

I2C_T::I2CON2: OVER_INTEN Position

Definition at line 2491 of file Mini51Series.h.

## ◆ I2C_I2CON2_TWOFF_EN_Msk

#define I2C_I2CON2_TWOFF_EN_Msk (0x1ul << I2C_I2CON2_TWOFF_EN_Pos)

I2C_T::I2CON2: TWOFF_EN Mask

Definition at line 2486 of file Mini51Series.h.

## ◆ I2C_I2CON2_TWOFF_EN_Pos

#define I2C_I2CON2_TWOFF_EN_Pos (1)

I2C_T::I2CON2: TWOFF_EN Position

Definition at line 2485 of file Mini51Series.h.

## ◆ I2C_I2CON2_UNDER_INTEN_Msk

#define I2C_I2CON2_UNDER_INTEN_Msk (0x1ul << I2C_I2CON2_UNDER_INTEN_Pos)

I2C_T::I2CON2: UNDER_INTEN Mask

Definition at line 2495 of file Mini51Series.h.

## ◆ I2C_I2CON2_UNDER_INTEN_Pos

#define I2C_I2CON2_UNDER_INTEN_Pos (4)

I2C_T::I2CON2: UNDER_INTEN Position

Definition at line 2494 of file Mini51Series.h.

## ◆ I2C_I2CON2_WKUPEN_Msk

#define I2C_I2CON2_WKUPEN_Msk (0x1ul << I2C_I2CON2_WKUPEN_Pos)

I2C_T::I2CON2: WKUPEN Mask

Definition at line 2483 of file Mini51Series.h.

## ◆ I2C_I2CON2_WKUPEN_Pos

#define I2C_I2CON2_WKUPEN_Pos (0)

I2C_T::I2CON2: WKUPEN Position

Definition at line 2482 of file Mini51Series.h.

## ◆ I2C_I2CON_AA_Msk

#define I2C_I2CON_AA_Msk (0x1ul << I2C_I2CON_AA_Pos)

I2C_T::I2CON: AA Mask

Definition at line 2438 of file Mini51Series.h.

## ◆ I2C_I2CON_AA_Pos

#define I2C_I2CON_AA_Pos (2)

    @addtogroup I2C_CONST I2C Bit Field Definition
    Constant Definitions for I2C Controller

I2C_T::I2CON: AA Position

Definition at line 2437 of file Mini51Series.h.

## ◆ I2C_I2CON_EI_Msk

#define I2C_I2CON_EI_Msk (0x1ul << I2C_I2CON_EI_Pos)

I2C_T::I2CON: EI Mask

Definition at line 2453 of file Mini51Series.h.

## ◆ I2C_I2CON_EI_Pos

#define I2C_I2CON_EI_Pos (7)

I2C_T::I2CON: EI Position

Definition at line 2452 of file Mini51Series.h.

## ◆ I2C_I2CON_ENSI_Msk

#define I2C_I2CON_ENSI_Msk (0x1ul << I2C_I2CON_ENSI_Pos)

I2C_T::I2CON: ENSI Mask

Definition at line 2450 of file Mini51Series.h.

## ◆ I2C_I2CON_ENSI_Pos

#define I2C_I2CON_ENSI_Pos (6)

I2C_T::I2CON: ENSI Position

Definition at line 2449 of file Mini51Series.h.

## ◆ I2C_I2CON_SI_Msk

#define I2C_I2CON_SI_Msk (0x1ul << I2C_I2CON_SI_Pos)

I2C_T::I2CON: SI Mask

Definition at line 2441 of file Mini51Series.h.

## ◆ I2C_I2CON_SI_Pos

#define I2C_I2CON_SI_Pos (3)

I2C_T::I2CON: SI Position

Definition at line 2440 of file Mini51Series.h.

## ◆ I2C_I2CON_STA_Msk

#define I2C_I2CON_STA_Msk (0x1ul << I2C_I2CON_STA_Pos)

I2C_T::I2CON: STA Mask

Definition at line 2447 of file Mini51Series.h.

## ◆ I2C_I2CON_STA_Pos

#define I2C_I2CON_STA_Pos (5)

I2C_T::I2CON: STA Position

Definition at line 2446 of file Mini51Series.h.

## ◆ I2C_I2CON_STO_Msk

#define I2C_I2CON_STO_Msk (0x1ul << I2C_I2CON_STO_Pos)

I2C_T::I2CON: STO Mask

Definition at line 2444 of file Mini51Series.h.

## ◆ I2C_I2CON_STO_Pos

#define I2C_I2CON_STO_Pos (4)

I2C_T::I2CON: STO Position

Definition at line 2443 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_EMPTY_Msk

#define I2C_I2CSTATUS2_EMPTY_Msk (0x1ul << I2C_I2CSTATUS2_EMPTY_Pos)

I2C_T::I2CSTATUS2: EMPTY Mask

Definition at line 2504 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_EMPTY_Pos

#define I2C_I2CSTATUS2_EMPTY_Pos (2)

I2C_T::I2CSTATUS2: EMPTY Position

Definition at line 2503 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_FULL_Msk

#define I2C_I2CSTATUS2_FULL_Msk (0x1ul << I2C_I2CSTATUS2_FULL_Pos)

I2C_T::I2CSTATUS2: FULL Mask

Definition at line 2501 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_FULL_Pos

#define I2C_I2CSTATUS2_FULL_Pos (1)

I2C_T::I2CSTATUS2: FULL Position

Definition at line 2500 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_OVERUN_Msk

#define I2C_I2CSTATUS2_OVERUN_Msk (0x1ul << I2C_I2CSTATUS2_OVERUN_Pos)

I2C_T::I2CSTATUS2: OVERUN Mask

Definition at line 2507 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_OVERUN_Pos

#define I2C_I2CSTATUS2_OVERUN_Pos (3)

I2C_T::I2CSTATUS2: OVERUN Position

Definition at line 2506 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_UNDERUN_Msk

#define I2C_I2CSTATUS2_UNDERUN_Msk (0x1ul << I2C_I2CSTATUS2_UNDERUN_Pos)

I2C_T::I2CSTATUS2: UNDERUN Mask

Definition at line 2510 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_UNDERUN_Pos

#define I2C_I2CSTATUS2_UNDERUN_Pos (4)

I2C_T::I2CSTATUS2: UNDERUN Position

Definition at line 2509 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_WAKEUP_Msk

#define I2C_I2CSTATUS2_WAKEUP_Msk (0x1ul << I2C_I2CSTATUS2_WAKEUP_Pos)

I2C_T::I2CSTATUS2: WAKEUP Mask

Definition at line 2498 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_WAKEUP_Pos

#define I2C_I2CSTATUS2_WAKEUP_Pos (0)

I2C_T::I2CSTATUS2: WAKEUP Position

Definition at line 2497 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS_I2CSTATUS_Msk

#define I2C_I2CSTATUS_I2CSTATUS_Msk (0xfful << I2C_I2CSTATUS_I2CSTATUS_Pos)

I2C_T::I2CSTATUS: I2CSTATUS Mask

Definition at line 2465 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS_I2CSTATUS_Pos

#define I2C_I2CSTATUS_I2CSTATUS_Pos (0)

I2C_T::I2CSTATUS: I2CSTATUS Position

Definition at line 2464 of file Mini51Series.h.

## ◆ I2C_I2CTOC_DIV4_Msk

#define I2C_I2CTOC_DIV4_Msk (0x1ul << I2C_I2CTOC_DIV4_Pos)

I2C_T::I2CTOC: DIV4 Mask

Definition at line 2474 of file Mini51Series.h.

## ◆ I2C_I2CTOC_DIV4_Pos

#define I2C_I2CTOC_DIV4_Pos (1)

I2C_T::I2CTOC: DIV4 Position

Definition at line 2473 of file Mini51Series.h.

## ◆ I2C_I2CTOC_ENTI_Msk

#define I2C_I2CTOC_ENTI_Msk (0x1ul << I2C_I2CTOC_ENTI_Pos)

I2C_T::I2CTOC: ENTI Mask

Definition at line 2477 of file Mini51Series.h.

## ◆ I2C_I2CTOC_ENTI_Pos

#define I2C_I2CTOC_ENTI_Pos (2)

I2C_T::I2CTOC: ENTI Position

Definition at line 2476 of file Mini51Series.h.

## ◆ I2C_I2CTOC_TIF_Msk

#define I2C_I2CTOC_TIF_Msk (0x1ul << I2C_I2CTOC_TIF_Pos)

I2C_T::I2CTOC: TIF Mask

Definition at line 2471 of file Mini51Series.h.

## ◆ I2C_I2CTOC_TIF_Pos

#define I2C_I2CTOC_TIF_Pos (0)

I2C_T::I2CTOC: TIF Position

Definition at line 2470 of file Mini51Series.h.

## ◆ INT_CON_NMI_SEL_EN_Msk

#define INT_CON_NMI_SEL_EN_Msk (0x1ul << INT_CON_NMI_SEL_EN_Pos)

INT_T::NMICON: NMI_SEL_EN Mask

Definition at line 2735 of file Mini51Series.h.

## ◆ INT_CON_NMI_SEL_EN_Pos

#define INT_CON_NMI_SEL_EN_Pos (8)

INT_T::NMICON: NMI_SEL_EN Position

Definition at line 2734 of file Mini51Series.h.

## ◆ INT_CON_NMI_SEL_Msk

#define INT_CON_NMI_SEL_Msk (0x1ful << INT_CON_NMI_SEL_Pos)

INT_T::NMICON: NMI_SEL Mask

Definition at line 2732 of file Mini51Series.h.

## ◆ INT_CON_NMI_SEL_Pos

#define INT_CON_NMI_SEL_Pos (0)

INT_T::NMICON: NMI_SEL Position

Definition at line 2731 of file Mini51Series.h.

## ◆ INT_IRQ_MCU_IRQ_Msk

#define INT_IRQ_MCU_IRQ_Msk (0xfffffffful << INT_IRQ_MCU_IRQ_Pos)

INT_T::MCUIRQ: MCU_IRQ Mask

Definition at line 2738 of file Mini51Series.h.

## ◆ INT_IRQ_MCU_IRQ_Pos

#define INT_IRQ_MCU_IRQ_Pos (0)

INT_T::MCUIRQ: MCU_IRQ Position

Definition at line 2737 of file Mini51Series.h.

## ◆ INT_SRC_INT_SRC_Msk

#define INT_SRC_INT_SRC_Msk (0x7ul << INT_SRC_INT_SRC_Pos)

INT_T::SRC0: INT_SRC Mask

Definition at line 2729 of file Mini51Series.h.

## ◆ INT_SRC_INT_SRC_Pos

#define INT_SRC_INT_SRC_Pos (0)

    @addtogroup INT_CONST INT Bit Field Definition
    Constant Definitions for INT Controller

INT_T::SRC0: INT_SRC Position

Definition at line 2728 of file Mini51Series.h.

## ◆ PWM_CMR_CMR_Msk

#define PWM_CMR_CMR_Msk (0xfffful << PWM_CMR_CMR_Pos)

PWM CMR::CMR Mask

Definition at line 3695 of file Mini51Series.h.

## ◆ PWM_CMR_CMR_Pos

#define PWM_CMR_CMR_Pos 0

PWM CMR::CMR Position

Definition at line 3694 of file Mini51Series.h.

## ◆ PWM_CNR_CNR_Msk

#define PWM_CNR_CNR_Msk (0xfffful << PWM_CNR_CNR_Pos)

PWM CNR::CNR Mask

Definition at line 3692 of file Mini51Series.h.

## ◆ PWM_CNR_CNR_Pos

#define PWM_CNR_CNR_Pos 0

PWM CNR::CNR Position

Definition at line 3691 of file Mini51Series.h.

## ◆ PWM_CSR_CSR0_Msk

#define PWM_CSR_CSR0_Msk (0x7ul << PWM_CSR_CSR0_Pos)

PWM_T::CSR: CSR0 Mask

Definition at line 3596 of file Mini51Series.h.

## ◆ PWM_CSR_CSR0_Pos

#define PWM_CSR_CSR0_Pos (0)

PWM_T::CSR: CSR0 Position

Definition at line 3595 of file Mini51Series.h.

## ◆ PWM_CSR_CSR1_Msk

#define PWM_CSR_CSR1_Msk (0x7ul << PWM_CSR_CSR1_Pos)

PWM_T::CSR: CSR1 Mask

Definition at line 3599 of file Mini51Series.h.

## ◆ PWM_CSR_CSR1_Pos

#define PWM_CSR_CSR1_Pos (4)

PWM_T::CSR: CSR1 Position

Definition at line 3598 of file Mini51Series.h.

## ◆ PWM_CSR_CSR2_Msk

#define PWM_CSR_CSR2_Msk (0x7ul << PWM_CSR_CSR2_Pos)

PWM_T::CSR: CSR2 Mask

Definition at line 3602 of file Mini51Series.h.

## ◆ PWM_CSR_CSR2_Pos

#define PWM_CSR_CSR2_Pos (8)

PWM_T::CSR: CSR2 Position

Definition at line 3601 of file Mini51Series.h.

## ◆ PWM_CSR_CSR3_Msk

#define PWM_CSR_CSR3_Msk (0x7ul << PWM_CSR_CSR3_Pos)

PWM_T::CSR: CSR3 Mask

Definition at line 3605 of file Mini51Series.h.

## ◆ PWM_CSR_CSR3_Pos

#define PWM_CSR_CSR3_Pos (12)

PWM_T::CSR: CSR3 Position

Definition at line 3604 of file Mini51Series.h.

## ◆ PWM_CSR_CSR4_Msk

#define PWM_CSR_CSR4_Msk (0x7ul << PWM_CSR_CSR4_Pos)

PWM_T::CSR: CSR4 Mask

Definition at line 3608 of file Mini51Series.h.

## ◆ PWM_CSR_CSR4_Pos

#define PWM_CSR_CSR4_Pos (16)

PWM_T::CSR: CSR4 Position

Definition at line 3607 of file Mini51Series.h.

## ◆ PWM_CSR_CSR5_Msk

#define PWM_CSR_CSR5_Msk (0x7ul << PWM_CSR_CSR5_Pos)

PWM_T::CSR: CSR5 Mask

Definition at line 3611 of file Mini51Series.h.

## ◆ PWM_CSR_CSR5_Pos

#define PWM_CSR_CSR5_Pos (20)

PWM_T::CSR: CSR5 Position

Definition at line 3610 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI01_Msk

#define PWM_DZIR_DZI01_Msk (0xfful << PWM_DZIR_DZI01_Pos)

PWM_T::PDZIR: DZI01 Mask

Definition at line 3839 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI01_Pos

#define PWM_DZIR_DZI01_Pos (0)

PWM_T::PDZIR: DZI01 Position

Definition at line 3838 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI23_Msk

#define PWM_DZIR_DZI23_Msk (0xfful << PWM_DZIR_DZI23_Pos)

PWM_T::PDZIR: DZI23 Mask

Definition at line 3842 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI23_Pos

#define PWM_DZIR_DZI23_Pos (8)

PWM_T::PDZIR: DZI23 Position

Definition at line 3841 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI45_Msk

#define PWM_DZIR_DZI45_Msk (0xfful << PWM_DZIR_DZI45_Pos)

PWM_T::PDZIR: DZI45 Mask

Definition at line 3845 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI45_Pos

#define PWM_DZIR_DZI45_Pos (16)

PWM_T::PDZIR: DZI45 Position

Definition at line 3844 of file Mini51Series.h.

## ◆ PWM_INTACCUCTL_INTACCUEN0_Msk

#define PWM_INTACCUCTL_INTACCUEN0_Msk (0x1ul << PWM_INTACCUCTL_INTACCUEN0_Pos)

PWM_T::INTACCUCTL: INTACCUEN0 Mask

Definition at line 4187 of file Mini51Series.h.

## ◆ PWM_INTACCUCTL_INTACCUEN0_Pos

#define PWM_INTACCUCTL_INTACCUEN0_Pos (0)

PWM_T::INTACCUCTL: INTACCUEN0 Position

Definition at line 4186 of file Mini51Series.h.

## ◆ PWM_INTACCUCTL_PERIODCNT_Msk

#define PWM_INTACCUCTL_PERIODCNT_Msk (0xful << PWM_INTACCUCTL_PERIODCNT_Pos)

PWM_T::INTACCUCTL: PERIODCNT Mask

Definition at line 4190 of file Mini51Series.h.

## ◆ PWM_INTACCUCTL_PERIODCNT_Pos

#define PWM_INTACCUCTL_PERIODCNT_Pos (4)

PWM_T::INTACCUCTL: PERIODCNT Position

Definition at line 4189 of file Mini51Series.h.

## ◆ PWM_PCR_CH0EN_Msk

#define PWM_PCR_CH0EN_Msk (0x1ul << PWM_PCR_CH0EN_Pos)

PWM_T::PCR: CH0EN Mask

Definition at line 3614 of file Mini51Series.h.

## ◆ PWM_PCR_CH0EN_Pos

#define PWM_PCR_CH0EN_Pos (0)

PWM_T::PCR: CH0EN Position

Definition at line 3613 of file Mini51Series.h.

## ◆ PWM_PCR_CH0INV_Msk

#define PWM_PCR_CH0INV_Msk (0x1ul << PWM_PCR_CH0INV_Pos)

PWM_T::PCR: CH0INV Mask

Definition at line 3620 of file Mini51Series.h.

## ◆ PWM_PCR_CH0INV_Pos

#define PWM_PCR_CH0INV_Pos (2)

PWM_T::PCR: CH0INV Position

Definition at line 3619 of file Mini51Series.h.

## ◆ PWM_PCR_CH0MOD_Msk

#define PWM_PCR_CH0MOD_Msk (0x1ul << PWM_PCR_CH0MOD_Pos)

PWM_T::PCR: CH0MOD Mask

Definition at line 3623 of file Mini51Series.h.

## ◆ PWM_PCR_CH0MOD_Pos

#define PWM_PCR_CH0MOD_Pos (3)

PWM_T::PCR: CH0MOD Position

Definition at line 3622 of file Mini51Series.h.

## ◆ PWM_PCR_CH1EN_Msk

#define PWM_PCR_CH1EN_Msk (0x1ul << PWM_PCR_CH1EN_Pos)

PWM_T::PCR: CH1EN Mask

Definition at line 3626 of file Mini51Series.h.

## ◆ PWM_PCR_CH1EN_Pos

#define PWM_PCR_CH1EN_Pos (4)

PWM_T::PCR: CH1EN Position

Definition at line 3625 of file Mini51Series.h.

## ◆ PWM_PCR_CH1INV_Msk

#define PWM_PCR_CH1INV_Msk (0x1ul << PWM_PCR_CH1INV_Pos)

PWM_T::PCR: CH1INV Mask

Definition at line 3629 of file Mini51Series.h.

## ◆ PWM_PCR_CH1INV_Pos

#define PWM_PCR_CH1INV_Pos (6)

PWM_T::PCR: CH1INV Position

Definition at line 3628 of file Mini51Series.h.

## ◆ PWM_PCR_CH1MOD_Msk

#define PWM_PCR_CH1MOD_Msk (0x1ul << PWM_PCR_CH1MOD_Pos)

PWM_T::PCR: CH1MOD Mask

Definition at line 3632 of file Mini51Series.h.

## ◆ PWM_PCR_CH1MOD_Pos

#define PWM_PCR_CH1MOD_Pos (7)

PWM_T::PCR: CH1MOD Position

Definition at line 3631 of file Mini51Series.h.

## ◆ PWM_PCR_CH2EN_Msk

#define PWM_PCR_CH2EN_Msk (0x1ul << PWM_PCR_CH2EN_Pos)

PWM_T::PCR: CH2EN Mask

Definition at line 3635 of file Mini51Series.h.

## ◆ PWM_PCR_CH2EN_Pos

#define PWM_PCR_CH2EN_Pos (8)

PWM_T::PCR: CH2EN Position

Definition at line 3634 of file Mini51Series.h.

## ◆ PWM_PCR_CH2INV_Msk

#define PWM_PCR_CH2INV_Msk (0x1ul << PWM_PCR_CH2INV_Pos)

PWM_T::PCR: CH2INV Mask

Definition at line 3638 of file Mini51Series.h.

## ◆ PWM_PCR_CH2INV_Pos

#define PWM_PCR_CH2INV_Pos (10)

PWM_T::PCR: CH2INV Position

Definition at line 3637 of file Mini51Series.h.

## ◆ PWM_PCR_CH2MOD_Msk

#define PWM_PCR_CH2MOD_Msk (0x1ul << PWM_PCR_CH2MOD_Pos)

PWM_T::PCR: CH2MOD Mask

Definition at line 3641 of file Mini51Series.h.

## ◆ PWM_PCR_CH2MOD_Pos

#define PWM_PCR_CH2MOD_Pos (11)

PWM_T::PCR: CH2MOD Position

Definition at line 3640 of file Mini51Series.h.

## ◆ PWM_PCR_CH3EN_Msk

#define PWM_PCR_CH3EN_Msk (0x1ul << PWM_PCR_CH3EN_Pos)

PWM_T::PCR: CH3EN Mask

Definition at line 3644 of file Mini51Series.h.

## ◆ PWM_PCR_CH3EN_Pos

#define PWM_PCR_CH3EN_Pos (12)

PWM_T::PCR: CH3EN Position

Definition at line 3643 of file Mini51Series.h.

## ◆ PWM_PCR_CH3INV_Msk

#define PWM_PCR_CH3INV_Msk (0x1ul << PWM_PCR_CH3INV_Pos)

PWM_T::PCR: CH3INV Mask

Definition at line 3647 of file Mini51Series.h.

## ◆ PWM_PCR_CH3INV_Pos

#define PWM_PCR_CH3INV_Pos (14)

PWM_T::PCR: CH3INV Position

Definition at line 3646 of file Mini51Series.h.

## ◆ PWM_PCR_CH3MOD_Msk

#define PWM_PCR_CH3MOD_Msk (0x1ul << PWM_PCR_CH3MOD_Pos)

PWM_T::PCR: CH3MOD Mask

Definition at line 3650 of file Mini51Series.h.

## ◆ PWM_PCR_CH3MOD_Pos

#define PWM_PCR_CH3MOD_Pos (15)

PWM_T::PCR: CH3MOD Position

Definition at line 3649 of file Mini51Series.h.

## ◆ PWM_PCR_CH4EN_Msk

#define PWM_PCR_CH4EN_Msk (0x1ul << PWM_PCR_CH4EN_Pos)

PWM_T::PCR: CH4EN Mask

Definition at line 3653 of file Mini51Series.h.

## ◆ PWM_PCR_CH4EN_Pos

#define PWM_PCR_CH4EN_Pos (16)

PWM_T::PCR: CH4EN Position

Definition at line 3652 of file Mini51Series.h.

## ◆ PWM_PCR_CH4INV_Msk

#define PWM_PCR_CH4INV_Msk (0x1ul << PWM_PCR_CH4INV_Pos)

PWM_T::PCR: CH4INV Mask

Definition at line 3656 of file Mini51Series.h.

## ◆ PWM_PCR_CH4INV_Pos

#define PWM_PCR_CH4INV_Pos (18)

PWM_T::PCR: CH4INV Position

Definition at line 3655 of file Mini51Series.h.

## ◆ PWM_PCR_CH4MOD_Msk

#define PWM_PCR_CH4MOD_Msk (0x1ul << PWM_PCR_CH4MOD_Pos)

PWM_T::PCR: CH4MOD Mask

Definition at line 3659 of file Mini51Series.h.

## ◆ PWM_PCR_CH4MOD_Pos

#define PWM_PCR_CH4MOD_Pos (19)

PWM_T::PCR: CH4MOD Position

Definition at line 3658 of file Mini51Series.h.

## ◆ PWM_PCR_CH5EN_Msk

#define PWM_PCR_CH5EN_Msk (0x1ul << PWM_PCR_CH5EN_Pos)

PWM_T::PCR: CH5EN Mask

Definition at line 3662 of file Mini51Series.h.

## ◆ PWM_PCR_CH5EN_Pos

#define PWM_PCR_CH5EN_Pos (20)

PWM_T::PCR: CH5EN Position

Definition at line 3661 of file Mini51Series.h.

## ◆ PWM_PCR_CH5INV_Msk

#define PWM_PCR_CH5INV_Msk (0x1ul << PWM_PCR_CH5INV_Pos)

PWM_T::PCR: CH5INV Mask

Definition at line 3665 of file Mini51Series.h.

## ◆ PWM_PCR_CH5INV_Pos

#define PWM_PCR_CH5INV_Pos (22)

PWM_T::PCR: CH5INV Position

Definition at line 3664 of file Mini51Series.h.

## ◆ PWM_PCR_CH5MOD_Msk

#define PWM_PCR_CH5MOD_Msk (0x1ul << PWM_PCR_CH5MOD_Pos)

PWM_T::PCR: CH5MOD Mask

Definition at line 3668 of file Mini51Series.h.

## ◆ PWM_PCR_CH5MOD_Pos

#define PWM_PCR_CH5MOD_Pos (23)

PWM_T::PCR: CH5MOD Position

Definition at line 3667 of file Mini51Series.h.

## ◆ PWM_PCR_CLRPWM_Msk

#define PWM_PCR_CLRPWM_Msk (0x1ul << PWM_PCR_CLRPWM_Pos)

PWM_T::PCR: CLRPWM Mask

Definition at line 3680 of file Mini51Series.h.

## ◆ PWM_PCR_CLRPWM_Pos

#define PWM_PCR_CLRPWM_Pos (27)

PWM_T::PCR: CLRPWM Position

Definition at line 3679 of file Mini51Series.h.

## ◆ PWM_PCR_DB_MOD_Msk

#define PWM_PCR_DB_MOD_Msk (0x1ul << PWM_PCR_DB_MOD_Pos)

PWM_T::PCR: DB_MODE Mask

Definition at line 3617 of file Mini51Series.h.

## ◆ PWM_PCR_DB_MOD_Pos

#define PWM_PCR_DB_MOD_Pos (1)

PWM_T::PCR: DB_MODE Position

Definition at line 3616 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN01_Msk

#define PWM_PCR_DZEN01_Msk (0x1ul << PWM_PCR_DZEN01_Pos)

PWM_T::PCR: DZEN01 Mask

Definition at line 3671 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN01_Pos

#define PWM_PCR_DZEN01_Pos (24)

PWM_T::PCR: DZEN01 Position

Definition at line 3670 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN23_Msk

#define PWM_PCR_DZEN23_Msk (0x1ul << PWM_PCR_DZEN23_Pos)

PWM_T::PCR: DZEN23 Mask

Definition at line 3674 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN23_Pos

#define PWM_PCR_DZEN23_Pos (25)

PWM_T::PCR: DZEN23 Position

Definition at line 3673 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN45_Msk

#define PWM_PCR_DZEN45_Msk (0x1ul << PWM_PCR_DZEN45_Pos)

PWM_T::PCR: DZEN45 Mask

Definition at line 3677 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN45_Pos

#define PWM_PCR_DZEN45_Pos (26)

PWM_T::PCR: DZEN45 Position

Definition at line 3676 of file Mini51Series.h.

## ◆ PWM_PCR_GRP_Msk

#define PWM_PCR_GRP_Msk (0x1ul << PWM_PCR_GRP_Pos)

PWM_T::PCR: GRP Mask

Definition at line 3686 of file Mini51Series.h.

## ◆ PWM_PCR_GRP_Pos

#define PWM_PCR_GRP_Pos (30)

PWM_T::PCR: GRP Position

Definition at line 3685 of file Mini51Series.h.

## ◆ PWM_PCR_PWMMOD_Msk

#define PWM_PCR_PWMMOD_Msk (0x3ul << PWM_PCR_PWMMOD_Pos)

PWM_T::PCR: PWMMOD Mask

Definition at line 3683 of file Mini51Series.h.

## ◆ PWM_PCR_PWMMOD_Pos

#define PWM_PCR_PWMMOD_Pos (28)

PWM_T::PCR: PWMMOD Position

Definition at line 3682 of file Mini51Series.h.

## ◆ PWM_PCR_PWMTYPE_Msk

#define PWM_PCR_PWMTYPE_Msk (0x1ul << PWM_PCR_PWMTYPE_Pos)

PWM_T::PCR: PWMTYPE Mask

Definition at line 3689 of file Mini51Series.h.

## ◆ PWM_PCR_PWMTYPE_Pos

#define PWM_PCR_PWMTYPE_Pos (31)

PWM_T::PCR: PWMTYPE Position

Definition at line 3688 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKEN0_Msk

#define PWM_PFBCON_BKEN0_Msk (0x1ul << PWM_PFBCON_BKEN0_Pos)

PWM_T::PFBCON: BKEN0 Mask

Definition at line 3800 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKEN0_Pos

#define PWM_PFBCON_BKEN0_Pos (0)

PWM_T::PFBCON: BKEN0 Position

Definition at line 3799 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKEN1_Msk

#define PWM_PFBCON_BKEN1_Msk (0x1ul << PWM_PFBCON_BKEN1_Pos)

PWM_T::PFBCON: BKEN1 Mask

Definition at line 3803 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKEN1_Pos

#define PWM_PFBCON_BKEN1_Pos (1)

PWM_T::PFBCON: BKEN1 Position

Definition at line 3802 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKF_Msk

#define PWM_PFBCON_BKF_Msk (0x1ul << PWM_PFBCON_BKF_Pos)

PWM_T::PFBCON: BKF Mask

Definition at line 3812 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKF_Pos

#define PWM_PFBCON_BKF_Pos (7)

PWM_T::PFBCON: BKF Position

Definition at line 3811 of file Mini51Series.h.

## ◆ PWM_PFBCON_CPO0BKEN_Msk

#define PWM_PFBCON_CPO0BKEN_Msk (0x1ul << PWM_PFBCON_CPO0BKEN_Pos)

PWM_T::PFBCON: CPO0BKEN Mask

Definition at line 3806 of file Mini51Series.h.

## ◆ PWM_PFBCON_CPO0BKEN_Pos

#define PWM_PFBCON_CPO0BKEN_Pos (2)

PWM_T::PFBCON: CPO0BKEN Position

Definition at line 3805 of file Mini51Series.h.

## ◆ PWM_PFBCON_CPO1BKEN_Msk

#define PWM_PFBCON_CPO1BKEN_Msk (0x1ul << PWM_PFBCON_CPO1BKEN_Pos)

PWM_T::PFBCON: CPO1BKEN Mask

Definition at line 3809 of file Mini51Series.h.

## ◆ PWM_PFBCON_CPO1BKEN_Pos

#define PWM_PFBCON_CPO1BKEN_Pos (3)

PWM_T::PFBCON: CPO1BKEN Position

Definition at line 3808 of file Mini51Series.h.

## ◆ PWM_PFBCON_D6BKO6_Msk

#define PWM_PFBCON_D6BKO6_Msk (0x1ul << PWM_PFBCON_D6BKO6_Pos)

PWM_T::PFBCON: D6BKO6 Mask

Definition at line 3833 of file Mini51Series.h.

## ◆ PWM_PFBCON_D6BKO6_Pos

#define PWM_PFBCON_D6BKO6_Pos (30)

PWM_T::PFBCON: D6BKO6 Position

Definition at line 3832 of file Mini51Series.h.

## ◆ PWM_PFBCON_D7BKO7_Msk

#define PWM_PFBCON_D7BKO7_Msk (0x1ul << PWM_PFBCON_D7BKO7_Pos)

PWM_T::PFBCON: D7BKO7 Mask

Definition at line 3836 of file Mini51Series.h.

## ◆ PWM_PFBCON_D7BKO7_Pos

#define PWM_PFBCON_D7BKO7_Pos (31)

PWM_T::PFBCON: D7BKO7 Position

Definition at line 3835 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO0_Msk

#define PWM_PFBCON_PWMBKO0_Msk (0x1ul << PWM_PFBCON_PWMBKO0_Pos)

PWM_T::PFBCON: PWMBKO0 Mask

Definition at line 3815 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO0_Pos

#define PWM_PFBCON_PWMBKO0_Pos (24)

PWM_T::PFBCON: PWMBKO0 Position

Definition at line 3814 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO1_Msk

#define PWM_PFBCON_PWMBKO1_Msk (0x1ul << PWM_PFBCON_PWMBKO1_Pos)

PWM_T::PFBCON: PWMBKO1 Mask

Definition at line 3818 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO1_Pos

#define PWM_PFBCON_PWMBKO1_Pos (25)

PWM_T::PFBCON: PWMBKO1 Position

Definition at line 3817 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO2_Msk

#define PWM_PFBCON_PWMBKO2_Msk (0x1ul << PWM_PFBCON_PWMBKO2_Pos)

PWM_T::PFBCON: PWMBKO2 Mask

Definition at line 3821 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO2_Pos

#define PWM_PFBCON_PWMBKO2_Pos (26)

PWM_T::PFBCON: PWMBKO2 Position

Definition at line 3820 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO3_Msk

#define PWM_PFBCON_PWMBKO3_Msk (0x1ul << PWM_PFBCON_PWMBKO3_Pos)

PWM_T::PFBCON: PWMBKO3 Mask

Definition at line 3824 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO3_Pos

#define PWM_PFBCON_PWMBKO3_Pos (27)

PWM_T::PFBCON: PWMBKO3 Position

Definition at line 3823 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO4_Msk

#define PWM_PFBCON_PWMBKO4_Msk (0x1ul << PWM_PFBCON_PWMBKO4_Pos)

PWM_T::PFBCON: PWMBKO4 Mask

Definition at line 3827 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO4_Pos

#define PWM_PFBCON_PWMBKO4_Pos (28)

PWM_T::PFBCON: PWMBKO4 Position

Definition at line 3826 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO5_Msk

#define PWM_PFBCON_PWMBKO5_Msk (0x1ul << PWM_PFBCON_PWMBKO5_Pos)

PWM_T::PFBCON: PWMBKO5 Mask

Definition at line 3830 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO5_Pos

#define PWM_PFBCON_PWMBKO5_Pos (29)

PWM_T::PFBCON: PWMBKO5 Position

Definition at line 3829 of file Mini51Series.h.

## ◆ PWM_PHCHG_ACCNT0_Msk

#define PWM_PHCHG_ACCNT0_Msk (0x1ul << PWM_PHCHG_ACCNT0_Pos)

PWM_T::PHCHG: ACCNT0 Mask

Definition at line 4034 of file Mini51Series.h.

## ◆ PWM_PHCHG_ACCNT0_Pos

#define PWM_PHCHG_ACCNT0_Pos (14)

PWM_T::PHCHG: ACCNT0 Position

Definition at line 4033 of file Mini51Series.h.

## ◆ PWM_PHCHG_ACCNT1_Msk

#define PWM_PHCHG_ACCNT1_Msk (0x1ul << PWM_PHCHG_ACCNT1_Pos)

PWM_T::PHCHG: ACCNT1 Mask

Definition at line 4037 of file Mini51Series.h.

## ◆ PWM_PHCHG_ACCNT1_Pos

#define PWM_PHCHG_ACCNT1_Pos (15)

PWM_T::PHCHG: ACCNT1 Position

Definition at line 4036 of file Mini51Series.h.

## ◆ PWM_PHCHG_CE0_Msk

#define PWM_PHCHG_CE0_Msk (0x1ul << PWM_PHCHG_CE0_Pos)

PWM_T::PHCHG: CE0 Mask

Definition at line 4079 of file Mini51Series.h.

## ◆ PWM_PHCHG_CE0_Pos

#define PWM_PHCHG_CE0_Pos (31)

PWM_T::PHCHG: CE0 Position

Definition at line 4078 of file Mini51Series.h.

## ◆ PWM_PHCHG_CE1_Msk

#define PWM_PHCHG_CE1_Msk (0x1ul << PWM_PHCHG_CE1_Pos)

PWM_T::PHCHG: CE1 Mask

Definition at line 4058 of file Mini51Series.h.

## ◆ PWM_PHCHG_CE1_Pos

#define PWM_PHCHG_CE1_Pos (23)

PWM_T::PHCHG: CE1 Position

Definition at line 4057 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH01TOFF0_Msk

#define PWM_PHCHG_CH01TOFF0_Msk (0x1ul << PWM_PHCHG_CH01TOFF0_Pos)

PWM_T::PHCHG: CH01TOFF0 Mask

Definition at line 4061 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH01TOFF0_Pos

#define PWM_PHCHG_CH01TOFF0_Pos (24)

PWM_T::PHCHG: CH01TOFF0 Position

Definition at line 4060 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH01TOFF1_Msk

#define PWM_PHCHG_CH01TOFF1_Msk (0x1ul << PWM_PHCHG_CH01TOFF1_Pos)

PWM_T::PHCHG: CH01TOFF1 Mask

Definition at line 4040 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH01TOFF1_Pos

#define PWM_PHCHG_CH01TOFF1_Pos (16)

PWM_T::PHCHG: CH01TOFF1 Position

Definition at line 4039 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH11TOFF0_Msk

#define PWM_PHCHG_CH11TOFF0_Msk (0x1ul << PWM_PHCHG_CH11TOFF0_Pos)

PWM_T::PHCHG: CH11TOFF0 Mask

Definition at line 4064 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH11TOFF0_Pos

#define PWM_PHCHG_CH11TOFF0_Pos (25)

PWM_T::PHCHG: CH11TOFF0 Position

Definition at line 4063 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH11TOFF1_Msk

#define PWM_PHCHG_CH11TOFF1_Msk (0x1ul << PWM_PHCHG_CH11TOFF1_Pos)

PWM_T::PHCHG: CH11TOFF1 Mask

Definition at line 4043 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH11TOFF1_Pos

#define PWM_PHCHG_CH11TOFF1_Pos (17)

PWM_T::PHCHG: CH11TOFF1 Position

Definition at line 4042 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH21TOFF0_Msk

#define PWM_PHCHG_CH21TOFF0_Msk (0x1ul << PWM_PHCHG_CH21TOFF0_Pos)

PWM_T::PHCHG: CH21TOFF0 Mask

Definition at line 4067 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH21TOFF0_Pos

#define PWM_PHCHG_CH21TOFF0_Pos (26)

PWM_T::PHCHG: CH21TOFF0 Position

Definition at line 4066 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH21TOFF1_Msk

#define PWM_PHCHG_CH21TOFF1_Msk (0x1ul << PWM_PHCHG_CH21TOFF1_Pos)

PWM_T::PHCHG: CH21TOFF1 Mask

Definition at line 4046 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH21TOFF1_Pos

#define PWM_PHCHG_CH21TOFF1_Pos (18)

PWM_T::PHCHG: CH21TOFF1 Position

Definition at line 4045 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH31TOFF0_Msk

#define PWM_PHCHG_CH31TOFF0_Msk (0x1ul << PWM_PHCHG_CH31TOFF0_Pos)

PWM_T::PHCHG: CH31TOFF0 Mask

Definition at line 4070 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH31TOFF0_Pos

#define PWM_PHCHG_CH31TOFF0_Pos (27)

PWM_T::PHCHG: CH31TOFF0 Position

Definition at line 4069 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH31TOFF1_Msk

#define PWM_PHCHG_CH31TOFF1_Msk (0x1ul << PWM_PHCHG_CH31TOFF1_Pos)

PWM_T::PHCHG: CH31TOFF1 Mask

Definition at line 4049 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH31TOFF1_Pos

#define PWM_PHCHG_CH31TOFF1_Pos (19)

PWM_T::PHCHG: CH31TOFF1 Position

Definition at line 4048 of file Mini51Series.h.

## ◆ PWM_PHCHG_CMP0SEL_Msk

#define PWM_PHCHG_CMP0SEL_Msk (0x3ul << PWM_PHCHG_CMP0SEL_Pos)

PWM_T::PHCHG: CMP0SEL Mask

Definition at line 4073 of file Mini51Series.h.

## ◆ PWM_PHCHG_CMP0SEL_Pos

#define PWM_PHCHG_CMP0SEL_Pos (28)

PWM_T::PHCHG: CMP0SEL Position

Definition at line 4072 of file Mini51Series.h.

## ◆ PWM_PHCHG_CMP1SEL_Msk

#define PWM_PHCHG_CMP1SEL_Msk (0x3ul << PWM_PHCHG_CMP1SEL_Pos)

PWM_T::PHCHG: CMP1SEL Mask

Definition at line 4052 of file Mini51Series.h.

## ◆ PWM_PHCHG_CMP1SEL_Pos

#define PWM_PHCHG_CMP1SEL_Pos (20)

PWM_T::PHCHG: CMP1SEL Position

Definition at line 4051 of file Mini51Series.h.

## ◆ PWM_PHCHG_D0_Msk

#define PWM_PHCHG_D0_Msk (0x1ul << PWM_PHCHG_D0_Pos)

PWM_T::PHCHG: D0 Mask

Definition at line 3992 of file Mini51Series.h.

## ◆ PWM_PHCHG_D0_Pos

#define PWM_PHCHG_D0_Pos (0)

PWM_T::PHCHG: D0 Position

Definition at line 3991 of file Mini51Series.h.

## ◆ PWM_PHCHG_D1_Msk

#define PWM_PHCHG_D1_Msk (0x1ul << PWM_PHCHG_D1_Pos)

PWM_T::PHCHG: D1 Mask

Definition at line 3995 of file Mini51Series.h.

## ◆ PWM_PHCHG_D1_Pos

#define PWM_PHCHG_D1_Pos (1)

PWM_T::PHCHG: D1 Position

Definition at line 3994 of file Mini51Series.h.

## ◆ PWM_PHCHG_D2_Msk

#define PWM_PHCHG_D2_Msk (0x1ul << PWM_PHCHG_D2_Pos)

PWM_T::PHCHG: D2 Mask

Definition at line 3998 of file Mini51Series.h.

## ◆ PWM_PHCHG_D2_Pos

#define PWM_PHCHG_D2_Pos (2)

PWM_T::PHCHG: D2 Position

Definition at line 3997 of file Mini51Series.h.

## ◆ PWM_PHCHG_D3_Msk

#define PWM_PHCHG_D3_Msk (0x1ul << PWM_PHCHG_D3_Pos)

PWM_T::PHCHG: D3 Mask

Definition at line 4001 of file Mini51Series.h.

## ◆ PWM_PHCHG_D3_Pos

#define PWM_PHCHG_D3_Pos (3)

PWM_T::PHCHG: D3 Position

Definition at line 4000 of file Mini51Series.h.

## ◆ PWM_PHCHG_D4_Msk

#define PWM_PHCHG_D4_Msk (0x1ul << PWM_PHCHG_D4_Pos)

PWM_T::PHCHG: D4 Mask

Definition at line 4004 of file Mini51Series.h.

## ◆ PWM_PHCHG_D4_Pos

#define PWM_PHCHG_D4_Pos (4)

PWM_T::PHCHG: D4 Position

Definition at line 4003 of file Mini51Series.h.

## ◆ PWM_PHCHG_D5_Msk

#define PWM_PHCHG_D5_Msk (0x1ul << PWM_PHCHG_D5_Pos)

PWM_T::PHCHG: D5 Mask

Definition at line 4007 of file Mini51Series.h.

## ◆ PWM_PHCHG_D5_Pos

#define PWM_PHCHG_D5_Pos (5)

PWM_T::PHCHG: D5 Position

Definition at line 4006 of file Mini51Series.h.

## ◆ PWM_PHCHG_D6_Msk

#define PWM_PHCHG_D6_Msk (0x1ul << PWM_PHCHG_D6_Pos)

PWM_T::PHCHG: D6 Mask

Definition at line 4010 of file Mini51Series.h.

## ◆ PWM_PHCHG_D6_Pos

#define PWM_PHCHG_D6_Pos (6)

PWM_T::PHCHG: D6 Position

Definition at line 4009 of file Mini51Series.h.

## ◆ PWM_PHCHG_D7_Msk

#define PWM_PHCHG_D7_Msk (0x1ul << PWM_PHCHG_D7_Pos)

PWM_T::PHCHG: D7 Mask

Definition at line 4013 of file Mini51Series.h.

## ◆ PWM_PHCHG_D7_Pos

#define PWM_PHCHG_D7_Pos (7)

PWM_T::PHCHG: D7 Position

Definition at line 4012 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM0_Msk

#define PWM_PHCHG_PWM0_Msk (0x1ul << PWM_PHCHG_PWM0_Pos)

PWM_T::PHCHG: PWM0 Mask

Definition at line 4016 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM0_Pos

#define PWM_PHCHG_PWM0_Pos (8)

PWM_T::PHCHG: PWM0 Position

Definition at line 4015 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM1_Msk

#define PWM_PHCHG_PWM1_Msk (0x1ul << PWM_PHCHG_PWM1_Pos)

PWM_T::PHCHG: PWM1 Mask

Definition at line 4019 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM1_Pos

#define PWM_PHCHG_PWM1_Pos (9)

PWM_T::PHCHG: PWM1 Position

Definition at line 4018 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM2_Msk

#define PWM_PHCHG_PWM2_Msk (0x1ul << PWM_PHCHG_PWM2_Pos)

PWM_T::PHCHG: PWM2 Mask

Definition at line 4022 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM2_Pos

#define PWM_PHCHG_PWM2_Pos (10)

PWM_T::PHCHG: PWM2 Position

Definition at line 4021 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM3_Msk

#define PWM_PHCHG_PWM3_Msk (0x1ul << PWM_PHCHG_PWM3_Pos)

PWM_T::PHCHG: PWM3 Mask

Definition at line 4025 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM3_Pos

#define PWM_PHCHG_PWM3_Pos (11)

PWM_T::PHCHG: PWM3 Position

Definition at line 4024 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM4_Msk

#define PWM_PHCHG_PWM4_Msk (0x1ul << PWM_PHCHG_PWM4_Pos)

PWM_T::PHCHG: PWM4 Mask

Definition at line 4028 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM4_Pos

#define PWM_PHCHG_PWM4_Pos (12)

PWM_T::PHCHG: PWM4 Position

Definition at line 4027 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM5_Msk

#define PWM_PHCHG_PWM5_Msk (0x1ul << PWM_PHCHG_PWM5_Pos)

PWM_T::PHCHG: PWM5 Mask

Definition at line 4031 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM5_Pos

#define PWM_PHCHG_PWM5_Pos (13)

PWM_T::PHCHG: PWM5 Position

Definition at line 4030 of file Mini51Series.h.

## ◆ PWM_PHCHG_T0_Msk

#define PWM_PHCHG_T0_Msk (0x1ul << PWM_PHCHG_T0_Pos)

PWM_T::PHCHG: T0 Mask

Definition at line 4076 of file Mini51Series.h.

## ◆ PWM_PHCHG_T0_Pos

#define PWM_PHCHG_T0_Pos (30)

PWM_T::PHCHG: T0 Position

Definition at line 4075 of file Mini51Series.h.

## ◆ PWM_PHCHG_T1_Msk

#define PWM_PHCHG_T1_Msk (0x1ul << PWM_PHCHG_T1_Pos)

PWM_T::PHCHG: T1 Mask

Definition at line 4055 of file Mini51Series.h.

## ◆ PWM_PHCHG_T1_Pos

#define PWM_PHCHG_T1_Pos (22)

PWM_T::PHCHG: T1 Position

Definition at line 4054 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK0_Msk

#define PWM_PHCHGMASK_CMPMASK0_Msk (0x1ul << PWM_PHCHGMASK_CMPMASK0_Pos)

PWM_T::PHCHGMASK: CMPMASK0 Mask

Definition at line 4181 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK0_Pos

#define PWM_PHCHGMASK_CMPMASK0_Pos (8)

PWM_T::PHCHGMASK: CMPMASK0 Position

Definition at line 4180 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK1_Msk

#define PWM_PHCHGMASK_CMPMASK1_Msk (0x1ul << PWM_PHCHGMASK_CMPMASK1_Pos)

PWM_T::PHCHGMASK: CMPMASK1 Mask

Definition at line 4184 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK1_Pos

#define PWM_PHCHGMASK_CMPMASK1_Pos (9)

PWM_T::PHCHGMASK: CMPMASK1 Position

Definition at line 4183 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK_Msk

#define PWM_PHCHGMASK_CMPMASK_Msk (0x3ul << PWM_PHCHGMASK_CMPMASK_Pos)

PWM_T::PHCHGMASK: CMPMASK Mask

Definition at line 4178 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK_Pos

#define PWM_PHCHGMASK_CMPMASK_Pos (8)

PWM_T::PHCHGMASK: CMPMASK Position

Definition at line 4177 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_MASK6_Msk

#define PWM_PHCHGMASK_MASK6_Msk (0x1ul << PWM_PHCHGMASK_MASK6_Pos)

PWM_T::PHCHGMASK: MASK6 Mask

Definition at line 4172 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_MASK6_Pos

#define PWM_PHCHGMASK_MASK6_Pos (6)

PWM_T::PHCHGMASK: MASK6 Position

Definition at line 4171 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_MASK7_Msk

#define PWM_PHCHGMASK_MASK7_Msk (0x1ul << PWM_PHCHGMASK_MASK7_Pos)

PWM_T::PHCHGMASK: MASK7 Mask

Definition at line 4175 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_MASK7_Pos

#define PWM_PHCHGMASK_MASK7_Pos (7)

PWM_T::PHCHGMASK: MASK7 Position

Definition at line 4174 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_ACCNT0_Msk

#define PWM_PHCHGNXT_ACCNT0_Msk (0x1ul << PWM_PHCHGNXT_ACCNT0_Pos)

PWM_T::PHCHGNXT: ACCNT0 Mask

Definition at line 4124 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_ACCNT0_Pos

#define PWM_PHCHGNXT_ACCNT0_Pos (14)

PWM_T::PHCHGNXT: ACCNT0 Position

Definition at line 4123 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_ACCNT1_Msk

#define PWM_PHCHGNXT_ACCNT1_Msk (0x1ul << PWM_PHCHGNXT_ACCNT1_Pos)

PWM_T::PHCHGNXT: ACCNT1 Mask

Definition at line 4127 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_ACCNT1_Pos

#define PWM_PHCHGNXT_ACCNT1_Pos (15)

PWM_T::PHCHGNXT: ACCNT1 Position

Definition at line 4126 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CE0_Msk

#define PWM_PHCHGNXT_CE0_Msk (0x1ul << PWM_PHCHGNXT_CE0_Pos)

PWM_T::PHCHGNXT: CE0 Mask

Definition at line 4169 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CE0_Pos

#define PWM_PHCHGNXT_CE0_Pos (31)

PWM_T::PHCHGNXT: CE0 Position

Definition at line 4168 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CE1_Msk

#define PWM_PHCHGNXT_CE1_Msk (0x1ul << PWM_PHCHGNXT_CE1_Pos)

PWM_T::PHCHGNXT: CE1 Mask

Definition at line 4148 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CE1_Pos

#define PWM_PHCHGNXT_CE1_Pos (23)

PWM_T::PHCHGNXT: CE1 Position

Definition at line 4147 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH01TOFF0_Msk

#define PWM_PHCHGNXT_CH01TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH01TOFF0_Pos)

PWM_T::PHCHGNXT: CH01TOFF0 Mask

Definition at line 4151 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH01TOFF0_Pos

#define PWM_PHCHGNXT_CH01TOFF0_Pos (24)

PWM_T::PHCHGNXT: CH01TOFF0 Position

Definition at line 4150 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH01TOFF1_Msk

#define PWM_PHCHGNXT_CH01TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH01TOFF1_Pos)

PWM_T::PHCHGNXT: CH01TOFF1 Mask

Definition at line 4130 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH01TOFF1_Pos

#define PWM_PHCHGNXT_CH01TOFF1_Pos (16)

PWM_T::PHCHGNXT: CH01TOFF1 Position

Definition at line 4129 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH11TOFF0_Msk

#define PWM_PHCHGNXT_CH11TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH11TOFF0_Pos)

PWM_T::PHCHGNXT: CH11TOFF0 Mask

Definition at line 4154 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH11TOFF0_Pos

#define PWM_PHCHGNXT_CH11TOFF0_Pos (25)

PWM_T::PHCHGNXT: CH11TOFF0 Position

Definition at line 4153 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH11TOFF1_Msk

#define PWM_PHCHGNXT_CH11TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH11TOFF1_Pos)

PWM_T::PHCHGNXT: CH11TOFF1 Mask

Definition at line 4133 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH11TOFF1_Pos

#define PWM_PHCHGNXT_CH11TOFF1_Pos (17)

PWM_T::PHCHGNXT: CH11TOFF1 Position

Definition at line 4132 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH21TOFF0_Msk

#define PWM_PHCHGNXT_CH21TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH21TOFF0_Pos)

PWM_T::PHCHGNXT: CH21TOFF0 Mask

Definition at line 4157 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH21TOFF0_Pos

#define PWM_PHCHGNXT_CH21TOFF0_Pos (26)

PWM_T::PHCHGNXT: CH21TOFF0 Position

Definition at line 4156 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH21TOFF1_Msk

#define PWM_PHCHGNXT_CH21TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH21TOFF1_Pos)

PWM_T::PHCHGNXT: CH21TOFF1 Mask

Definition at line 4136 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH21TOFF1_Pos

#define PWM_PHCHGNXT_CH21TOFF1_Pos (18)

PWM_T::PHCHGNXT: CH21TOFF1 Position

Definition at line 4135 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH31TOFF0_Msk

#define PWM_PHCHGNXT_CH31TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH31TOFF0_Pos)

PWM_T::PHCHGNXT: CH31TOFF0 Mask

Definition at line 4160 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH31TOFF0_Pos

#define PWM_PHCHGNXT_CH31TOFF0_Pos (27)

PWM_T::PHCHGNXT: CH31TOFF0 Position

Definition at line 4159 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH31TOFF1_Msk

#define PWM_PHCHGNXT_CH31TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH31TOFF1_Pos)

PWM_T::PHCHGNXT: CH31TOFF1 Mask

Definition at line 4139 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH31TOFF1_Pos

#define PWM_PHCHGNXT_CH31TOFF1_Pos (19)

PWM_T::PHCHGNXT: CH31TOFF1 Position

Definition at line 4138 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CMP0SEL_Msk

#define PWM_PHCHGNXT_CMP0SEL_Msk (0x3ul << PWM_PHCHGNXT_CMP0SEL_Pos)

PWM_T::PHCHGNXT: CMP0SEL Mask

Definition at line 4163 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CMP0SEL_Pos

#define PWM_PHCHGNXT_CMP0SEL_Pos (28)

PWM_T::PHCHGNXT: CMP0SEL Position

Definition at line 4162 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CMP1SEL_Msk

#define PWM_PHCHGNXT_CMP1SEL_Msk (0x3ul << PWM_PHCHGNXT_CMP1SEL_Pos)

PWM_T::PHCHGNXT: CMP1SEL Mask

Definition at line 4142 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CMP1SEL_Pos

#define PWM_PHCHGNXT_CMP1SEL_Pos (20)

PWM_T::PHCHGNXT: CMP1SEL Position

Definition at line 4141 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D0_Msk

#define PWM_PHCHGNXT_D0_Msk (0x1ul << PWM_PHCHGNXT_D0_Pos)

PWM_T::PHCHGNXT: D0 Mask

Definition at line 4082 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D0_Pos

#define PWM_PHCHGNXT_D0_Pos (0)

PWM_T::PHCHGNXT: D0 Position

Definition at line 4081 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D1_Msk

#define PWM_PHCHGNXT_D1_Msk (0x1ul << PWM_PHCHGNXT_D1_Pos)

PWM_T::PHCHGNXT: D1 Mask

Definition at line 4085 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D1_Pos

#define PWM_PHCHGNXT_D1_Pos (1)

PWM_T::PHCHGNXT: D1 Position

Definition at line 4084 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D2_Msk

#define PWM_PHCHGNXT_D2_Msk (0x1ul << PWM_PHCHGNXT_D2_Pos)

PWM_T::PHCHGNXT: D2 Mask

Definition at line 4088 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D2_Pos

#define PWM_PHCHGNXT_D2_Pos (2)

PWM_T::PHCHGNXT: D2 Position

Definition at line 4087 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D3_Msk

#define PWM_PHCHGNXT_D3_Msk (0x1ul << PWM_PHCHGNXT_D3_Pos)

PWM_T::PHCHGNXT: D3 Mask

Definition at line 4091 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D3_Pos

#define PWM_PHCHGNXT_D3_Pos (3)

PWM_T::PHCHGNXT: D3 Position

Definition at line 4090 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D4_Msk

#define PWM_PHCHGNXT_D4_Msk (0x1ul << PWM_PHCHGNXT_D4_Pos)

PWM_T::PHCHGNXT: D4 Mask

Definition at line 4094 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D4_Pos

#define PWM_PHCHGNXT_D4_Pos (4)

PWM_T::PHCHGNXT: D4 Position

Definition at line 4093 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D5_Msk

#define PWM_PHCHGNXT_D5_Msk (0x1ul << PWM_PHCHGNXT_D5_Pos)

PWM_T::PHCHGNXT: D5 Mask

Definition at line 4097 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D5_Pos

#define PWM_PHCHGNXT_D5_Pos (5)

PWM_T::PHCHGNXT: D5 Position

Definition at line 4096 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D6_Msk

#define PWM_PHCHGNXT_D6_Msk (0x1ul << PWM_PHCHGNXT_D6_Pos)

PWM_T::PHCHGNXT: D6 Mask

Definition at line 4100 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D6_Pos

#define PWM_PHCHGNXT_D6_Pos (6)

PWM_T::PHCHGNXT: D6 Position

Definition at line 4099 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D7_Msk

#define PWM_PHCHGNXT_D7_Msk (0x1ul << PWM_PHCHGNXT_D7_Pos)

PWM_T::PHCHGNXT: D7 Mask

Definition at line 4103 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D7_Pos

#define PWM_PHCHGNXT_D7_Pos (7)

PWM_T::PHCHGNXT: D7 Position

Definition at line 4102 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM0_Msk

#define PWM_PHCHGNXT_PWM0_Msk (0x1ul << PWM_PHCHGNXT_PWM0_Pos)

PWM_T::PHCHGNXT: PWM0 Mask

Definition at line 4106 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM0_Pos

#define PWM_PHCHGNXT_PWM0_Pos (8)

PWM_T::PHCHGNXT: PWM0 Position

Definition at line 4105 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM1_Msk

#define PWM_PHCHGNXT_PWM1_Msk (0x1ul << PWM_PHCHGNXT_PWM1_Pos)

PWM_T::PHCHGNXT: PWM1 Mask

Definition at line 4109 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM1_Pos

#define PWM_PHCHGNXT_PWM1_Pos (9)

PWM_T::PHCHGNXT: PWM1 Position

Definition at line 4108 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM2_Msk

#define PWM_PHCHGNXT_PWM2_Msk (0x1ul << PWM_PHCHGNXT_PWM2_Pos)

PWM_T::PHCHGNXT: PWM2 Mask

Definition at line 4112 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM2_Pos

#define PWM_PHCHGNXT_PWM2_Pos (10)

PWM_T::PHCHGNXT: PWM2 Position

Definition at line 4111 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM3_Msk

#define PWM_PHCHGNXT_PWM3_Msk (0x1ul << PWM_PHCHGNXT_PWM3_Pos)

PWM_T::PHCHGNXT: PWM3 Mask

Definition at line 4115 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM3_Pos

#define PWM_PHCHGNXT_PWM3_Pos (11)

PWM_T::PHCHGNXT: PWM3 Position

Definition at line 4114 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM4_Msk

#define PWM_PHCHGNXT_PWM4_Msk (0x1ul << PWM_PHCHGNXT_PWM4_Pos)

PWM_T::PHCHGNXT: PWM4 Mask

Definition at line 4118 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM4_Pos

#define PWM_PHCHGNXT_PWM4_Pos (12)

PWM_T::PHCHGNXT: PWM4 Position

Definition at line 4117 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM5_Msk

#define PWM_PHCHGNXT_PWM5_Msk (0x1ul << PWM_PHCHGNXT_PWM5_Pos)

PWM_T::PHCHGNXT: PWM5 Mask

Definition at line 4121 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM5_Pos

#define PWM_PHCHGNXT_PWM5_Pos (13)

PWM_T::PHCHGNXT: PWM5 Position

Definition at line 4120 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_T0_Msk

#define PWM_PHCHGNXT_T0_Msk (0x1ul << PWM_PHCHGNXT_T0_Pos)

PWM_T::PHCHGNXT: T0 Mask

Definition at line 4166 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_T0_Pos

#define PWM_PHCHGNXT_T0_Pos (30)

PWM_T::PHCHGNXT: T0 Position

Definition at line 4165 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_T1_Msk

#define PWM_PHCHGNXT_T1_Msk (0x1ul << PWM_PHCHGNXT_T1_Pos)

PWM_T::PHCHGNXT: T1 Mask

Definition at line 4145 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_T1_Pos

#define PWM_PHCHGNXT_T1_Pos (22)

PWM_T::PHCHGNXT: T1 Position

Definition at line 4144 of file Mini51Series.h.

## ◆ PWM_PIER_BRKIE_Msk

#define PWM_PIER_BRKIE_Msk (0x1ul << PWM_PIER_BRKIE_Pos)

PWM_T::PIER: BRKIE Mask

Definition at line 3734 of file Mini51Series.h.

## ◆ PWM_PIER_BRKIE_Pos

#define PWM_PIER_BRKIE_Pos (16)

PWM_T::PIER: BRKIE Position

Definition at line 3733 of file Mini51Series.h.

## ◆ PWM_PIER_INT_TYPE_Msk

#define PWM_PIER_INT_TYPE_Msk (0x1ul << PWM_PIER_INT_TYPE_Pos)

PWM_T::PIER: INT_TYPE Mask

Definition at line 3737 of file Mini51Series.h.

## ◆ PWM_PIER_INT_TYPE_Pos

#define PWM_PIER_INT_TYPE_Pos (17)

PWM_T::PIER: INT_TYPE Position

Definition at line 3736 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE0_Msk

#define PWM_PIER_PWMDIE0_Msk (0x1ul << PWM_PIER_PWMDIE0_Pos)

PWM_T::PIER: PWMDIE0 Mask

Definition at line 3716 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE0_Pos

#define PWM_PIER_PWMDIE0_Pos (8)

PWM_T::PIER: PWMDIE0 Position

Definition at line 3715 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE1_Msk

#define PWM_PIER_PWMDIE1_Msk (0x1ul << PWM_PIER_PWMDIE1_Pos)

PWM_T::PIER: PWMDIE1 Mask

Definition at line 3719 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE1_Pos

#define PWM_PIER_PWMDIE1_Pos (9)

PWM_T::PIER: PWMDIE1 Position

Definition at line 3718 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE2_Msk

#define PWM_PIER_PWMDIE2_Msk (0x1ul << PWM_PIER_PWMDIE2_Pos)

PWM_T::PIER: PWMDIE2 Mask

Definition at line 3722 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE2_Pos

#define PWM_PIER_PWMDIE2_Pos (10)

PWM_T::PIER: PWMDIE2 Position

Definition at line 3721 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE3_Msk

#define PWM_PIER_PWMDIE3_Msk (0x1ul << PWM_PIER_PWMDIE3_Pos)

PWM_T::PIER: PWMDIE3 Mask

Definition at line 3725 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE3_Pos

#define PWM_PIER_PWMDIE3_Pos (11)

PWM_T::PIER: PWMDIE3 Position

Definition at line 3724 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE4_Msk

#define PWM_PIER_PWMDIE4_Msk (0x1ul << PWM_PIER_PWMDIE4_Pos)

PWM_T::PIER: PWMDIE4 Mask

Definition at line 3728 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE4_Pos

#define PWM_PIER_PWMDIE4_Pos (12)

PWM_T::PIER: PWMDIE4 Position

Definition at line 3727 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE5_Msk

#define PWM_PIER_PWMDIE5_Msk (0x1ul << PWM_PIER_PWMDIE5_Pos)

PWM_T::PIER: PWMDIE5 Mask

Definition at line 3731 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE5_Pos

#define PWM_PIER_PWMDIE5_Pos (13)

PWM_T::PIER: PWMDIE5 Position

Definition at line 3730 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE0_Msk

#define PWM_PIER_PWMPIE0_Msk (0x1ul << PWM_PIER_PWMPIE0_Pos)

PWM_T::PIER: PWMPIE0 Mask

Definition at line 3698 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE0_Pos

#define PWM_PIER_PWMPIE0_Pos (0)

PWM_T::PIER: PWMPIE0 Position

Definition at line 3697 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE1_Msk

#define PWM_PIER_PWMPIE1_Msk (0x1ul << PWM_PIER_PWMPIE1_Pos)

PWM_T::PIER: PWMPIE1 Mask

Definition at line 3701 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE1_Pos

#define PWM_PIER_PWMPIE1_Pos (1)

PWM_T::PIER: PWMPIE1 Position

Definition at line 3700 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE2_Msk

#define PWM_PIER_PWMPIE2_Msk (0x1ul << PWM_PIER_PWMPIE2_Pos)

PWM_T::PIER: PWMPIE2 Mask

Definition at line 3704 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE2_Pos

#define PWM_PIER_PWMPIE2_Pos (2)

PWM_T::PIER: PWMPIE2 Position

Definition at line 3703 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE3_Msk

#define PWM_PIER_PWMPIE3_Msk (0x1ul << PWM_PIER_PWMPIE3_Pos)

PWM_T::PIER: PWMPIE3 Mask

Definition at line 3707 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE3_Pos

#define PWM_PIER_PWMPIE3_Pos (3)

PWM_T::PIER: PWMPIE3 Position

Definition at line 3706 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE4_Msk

#define PWM_PIER_PWMPIE4_Msk (0x1ul << PWM_PIER_PWMPIE4_Pos)

PWM_T::PIER: PWMPIE4 Mask

Definition at line 3710 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE4_Pos

#define PWM_PIER_PWMPIE4_Pos (4)

PWM_T::PIER: PWMPIE4 Position

Definition at line 3709 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE5_Msk

#define PWM_PIER_PWMPIE5_Msk (0x1ul << PWM_PIER_PWMPIE5_Pos)

PWM_T::PIER: PWMPIE5 Mask

Definition at line 3713 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE5_Pos

#define PWM_PIER_PWMPIE5_Pos (5)

PWM_T::PIER: PWMPIE5 Position

Definition at line 3712 of file Mini51Series.h.

## ◆ PWM_PIIR_BKF0_Msk

#define PWM_PIIR_BKF0_Msk (0x1ul << PWM_PIIR_BKF0_Pos)

PWM_T::PIIR: BKF0 Mask

Definition at line 3776 of file Mini51Series.h.

## ◆ PWM_PIIR_BKF0_Pos

#define PWM_PIIR_BKF0_Pos (16)

PWM_T::PIIR: BKF0 Position

Definition at line 3775 of file Mini51Series.h.

## ◆ PWM_PIIR_BKF1_Msk

#define PWM_PIIR_BKF1_Msk (0x1ul << PWM_PIIR_BKF1_Pos)

PWM_T::PIIR: BKF1 Mask

Definition at line 3779 of file Mini51Series.h.

## ◆ PWM_PIIR_BKF1_Pos

#define PWM_PIIR_BKF1_Pos (17)

PWM_T::PIIR: BKF1 Position

Definition at line 3778 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF0_Msk

#define PWM_PIIR_PWMDIF0_Msk (0x1ul << PWM_PIIR_PWMDIF0_Pos)

PWM_T::PIIR: PWMDIF0 Mask

Definition at line 3758 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF0_Pos

#define PWM_PIIR_PWMDIF0_Pos (8)

PWM_T::PIIR: PWMDIF0 Position

Definition at line 3757 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF1_Msk

#define PWM_PIIR_PWMDIF1_Msk (0x1ul << PWM_PIIR_PWMDIF1_Pos)

PWM_T::PIIR: PWMDIF1 Mask

Definition at line 3761 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF1_Pos

#define PWM_PIIR_PWMDIF1_Pos (9)

PWM_T::PIIR: PWMDIF1 Position

Definition at line 3760 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF2_Msk

#define PWM_PIIR_PWMDIF2_Msk (0x1ul << PWM_PIIR_PWMDIF2_Pos)

PWM_T::PIIR: PWMDIF2 Mask

Definition at line 3764 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF2_Pos

#define PWM_PIIR_PWMDIF2_Pos (10)

PWM_T::PIIR: PWMDIF2 Position

Definition at line 3763 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF3_Msk

#define PWM_PIIR_PWMDIF3_Msk (0x1ul << PWM_PIIR_PWMDIF3_Pos)

PWM_T::PIIR: PWMDIF3 Mask

Definition at line 3767 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF3_Pos

#define PWM_PIIR_PWMDIF3_Pos (11)

PWM_T::PIIR: PWMDIF3 Position

Definition at line 3766 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF4_Msk

#define PWM_PIIR_PWMDIF4_Msk (0x1ul << PWM_PIIR_PWMDIF4_Pos)

PWM_T::PIIR: PWMDIF4 Mask

Definition at line 3770 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF4_Pos

#define PWM_PIIR_PWMDIF4_Pos (12)

PWM_T::PIIR: PWMDIF4 Position

Definition at line 3769 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF5_Msk

#define PWM_PIIR_PWMDIF5_Msk (0x1ul << PWM_PIIR_PWMDIF5_Pos)

PWM_T::PIIR: PWMDIF5 Mask

Definition at line 3773 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF5_Pos

#define PWM_PIIR_PWMDIF5_Pos (13)

PWM_T::PIIR: PWMDIF5 Position

Definition at line 3772 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF0_Msk

#define PWM_PIIR_PWMPIF0_Msk (0x1ul << PWM_PIIR_PWMPIF0_Pos)

PWM_T::PIIR: PWMPIF0 Mask

Definition at line 3740 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF0_Pos

#define PWM_PIIR_PWMPIF0_Pos (0)

PWM_T::PIIR: PWMPIF0 Position

Definition at line 3739 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF1_Msk

#define PWM_PIIR_PWMPIF1_Msk (0x1ul << PWM_PIIR_PWMPIF1_Pos)

PWM_T::PIIR: PWMPIF1 Mask

Definition at line 3743 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF1_Pos

#define PWM_PIIR_PWMPIF1_Pos (1)

PWM_T::PIIR: PWMPIF1 Position

Definition at line 3742 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF2_Msk

#define PWM_PIIR_PWMPIF2_Msk (0x1ul << PWM_PIIR_PWMPIF2_Pos)

PWM_T::PIIR: PWMPIF2 Mask

Definition at line 3746 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF2_Pos

#define PWM_PIIR_PWMPIF2_Pos (2)

PWM_T::PIIR: PWMPIF2 Position

Definition at line 3745 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF3_Msk

#define PWM_PIIR_PWMPIF3_Msk (0x1ul << PWM_PIIR_PWMPIF3_Pos)

PWM_T::PIIR: PWMPIF3 Mask

Definition at line 3749 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF3_Pos

#define PWM_PIIR_PWMPIF3_Pos (3)

PWM_T::PIIR: PWMPIF3 Position

Definition at line 3748 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF4_Msk

#define PWM_PIIR_PWMPIF4_Msk (0x1ul << PWM_PIIR_PWMPIF4_Pos)

PWM_T::PIIR: PWMPIF4 Mask

Definition at line 3752 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF4_Pos

#define PWM_PIIR_PWMPIF4_Pos (4)

PWM_T::PIIR: PWMPIF4 Position

Definition at line 3751 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF5_Msk

#define PWM_PIIR_PWMPIF5_Msk (0x1ul << PWM_PIIR_PWMPIF5_Pos)

PWM_T::PIIR: PWMPIF5 Mask

Definition at line 3755 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF5_Pos

#define PWM_PIIR_PWMPIF5_Pos (5)

PWM_T::PIIR: PWMPIF5 Position

Definition at line 3754 of file Mini51Series.h.

## ◆ PWM_POE_PWM0_Msk

#define PWM_POE_PWM0_Msk (0x1ul << PWM_POE_PWM0_Pos)

PWM_T::POE: PWM0 Mask

Definition at line 3782 of file Mini51Series.h.

## ◆ PWM_POE_PWM0_Pos

#define PWM_POE_PWM0_Pos (0)

PWM_T::POE: PWM0 Position

Definition at line 3781 of file Mini51Series.h.

## ◆ PWM_POE_PWM1_Msk

#define PWM_POE_PWM1_Msk (0x1ul << PWM_POE_PWM1_Pos)

PWM_T::POE: PWM1 Mask

Definition at line 3785 of file Mini51Series.h.

## ◆ PWM_POE_PWM1_Pos

#define PWM_POE_PWM1_Pos (1)

PWM_T::POE: PWM1 Position

Definition at line 3784 of file Mini51Series.h.

## ◆ PWM_POE_PWM2_Msk

#define PWM_POE_PWM2_Msk (0x1ul << PWM_POE_PWM2_Pos)

PWM_T::POE: PWM2 Mask

Definition at line 3788 of file Mini51Series.h.

## ◆ PWM_POE_PWM2_Pos

#define PWM_POE_PWM2_Pos (2)

PWM_T::POE: PWM2 Position

Definition at line 3787 of file Mini51Series.h.

## ◆ PWM_POE_PWM3_Msk

#define PWM_POE_PWM3_Msk (0x1ul << PWM_POE_PWM3_Pos)

PWM_T::POE: PWM3 Mask

Definition at line 3791 of file Mini51Series.h.

## ◆ PWM_POE_PWM3_Pos

#define PWM_POE_PWM3_Pos (3)

PWM_T::POE: PWM3 Position

Definition at line 3790 of file Mini51Series.h.

## ◆ PWM_POE_PWM4_Msk

#define PWM_POE_PWM4_Msk (0x1ul << PWM_POE_PWM4_Pos)

PWM_T::POE: PWM4 Mask

Definition at line 3794 of file Mini51Series.h.

## ◆ PWM_POE_PWM4_Pos

#define PWM_POE_PWM4_Pos (4)

PWM_T::POE: PWM4 Position

Definition at line 3793 of file Mini51Series.h.

## ◆ PWM_POE_PWM5_Msk

#define PWM_POE_PWM5_Msk (0x1ul << PWM_POE_PWM5_Pos)

PWM_T::POE: PWM5 Mask

Definition at line 3797 of file Mini51Series.h.

## ◆ PWM_POE_PWM5_Pos

#define PWM_POE_PWM5_Pos (5)

PWM_T::POE: PWM5 Position

Definition at line 3796 of file Mini51Series.h.

## ◆ PWM_PPR_CP01_Msk

#define PWM_PPR_CP01_Msk (0xfful << PWM_PPR_CP01_Pos)

PWM_T::PPR: CP01 Mask

Definition at line 3587 of file Mini51Series.h.

## ◆ PWM_PPR_CP01_Pos

#define PWM_PPR_CP01_Pos (0)

    @addtogroup PWM_CONST PWM Bit Field Definition
    Constant Definitions for PWM Controller

PWM_T::PPR: CP01 Position

Definition at line 3586 of file Mini51Series.h.

## ◆ PWM_PPR_CP23_Msk

#define PWM_PPR_CP23_Msk (0xfful << PWM_PPR_CP23_Pos)

PWM_T::PPR: CP23 Mask

Definition at line 3590 of file Mini51Series.h.

## ◆ PWM_PPR_CP23_Pos

#define PWM_PPR_CP23_Pos (8)

PWM_T::PPR: CP23 Position

Definition at line 3589 of file Mini51Series.h.

## ◆ PWM_PPR_CP45_Msk

#define PWM_PPR_CP45_Msk (0xfful << PWM_PPR_CP45_Pos)

PWM_T::PPR: CP45 Mask

Definition at line 3593 of file Mini51Series.h.

## ◆ PWM_PPR_CP45_Pos

#define PWM_PPR_CP45_Pos (16)

PWM_T::PPR: CP45 Position

Definition at line 3592 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM0TRGFEN_Msk

#define PWM_TRGCON0_CM0TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM0TRGFEN_Pos)

PWM_T::TRGCON0: CM0TRGFEN Mask

Definition at line 3854 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM0TRGFEN_Pos

#define PWM_TRGCON0_CM0TRGFEN_Pos (2)

PWM_T::TRGCON0: CM0TRGFEN Position

Definition at line 3853 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM0TRGREN_Msk

#define PWM_TRGCON0_CM0TRGREN_Msk (0x1ul << PWM_TRGCON0_CM0TRGREN_Pos)

PWM_T::TRGCON0: CM0TRGREN Mask

Definition at line 3848 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM0TRGREN_Pos

#define PWM_TRGCON0_CM0TRGREN_Pos (0)

PWM_T::TRGCON0: CM0TRGREN Position

Definition at line 3847 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM1TRGFEN_Msk

#define PWM_TRGCON0_CM1TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM1TRGFEN_Pos)

PWM_T::TRGCON0: CM1TRGFEN Mask

Definition at line 3866 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM1TRGFEN_Pos

#define PWM_TRGCON0_CM1TRGFEN_Pos (10)

PWM_T::TRGCON0: CM1TRGFEN Position

Definition at line 3865 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM1TRGREN_Msk

#define PWM_TRGCON0_CM1TRGREN_Msk (0x1ul << PWM_TRGCON0_CM1TRGREN_Pos)

PWM_T::TRGCON0: CM1TRGREN Mask

Definition at line 3860 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM1TRGREN_Pos

#define PWM_TRGCON0_CM1TRGREN_Pos (8)

PWM_T::TRGCON0: CM1TRGREN Position

Definition at line 3859 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM2TRGFEN_Msk

#define PWM_TRGCON0_CM2TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM2TRGFEN_Pos)

PWM_T::TRGCON0: CM2TRGFEN Mask

Definition at line 3878 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM2TRGFEN_Pos

#define PWM_TRGCON0_CM2TRGFEN_Pos (18)

PWM_T::TRGCON0: CM2TRGFEN Position

Definition at line 3877 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM2TRGREN_Msk

#define PWM_TRGCON0_CM2TRGREN_Msk (0x1ul << PWM_TRGCON0_CM2TRGREN_Pos)

PWM_T::TRGCON0: CM2TRGREN Mask

Definition at line 3872 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM2TRGREN_Pos

#define PWM_TRGCON0_CM2TRGREN_Pos (16)

PWM_T::TRGCON0: CM2TRGREN Position

Definition at line 3871 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM3TRGFEN_Msk

#define PWM_TRGCON0_CM3TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM3TRGFEN_Pos)

PWM_T::TRGCON0: CM3TRGFEN Mask

Definition at line 3890 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM3TRGFEN_Pos

#define PWM_TRGCON0_CM3TRGFEN_Pos (26)

PWM_T::TRGCON0: CM3TRGFEN Position

Definition at line 3889 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM3TRGREN_Msk

#define PWM_TRGCON0_CM3TRGREN_Msk (0x1ul << PWM_TRGCON0_CM3TRGREN_Pos)

PWM_T::TRGCON0: CM3TRGREN Mask

Definition at line 3884 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM3TRGREN_Pos

#define PWM_TRGCON0_CM3TRGREN_Pos (24)

PWM_T::TRGCON0: CM3TRGREN Position

Definition at line 3883 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT0TRGEN_Msk

#define PWM_TRGCON0_CNT0TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT0TRGEN_Pos)

PWM_T::TRGCON0: CNT0TRGEN Mask

Definition at line 3851 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT0TRGEN_Pos

#define PWM_TRGCON0_CNT0TRGEN_Pos (1)

PWM_T::TRGCON0: CNT0TRGEN Position

Definition at line 3850 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT1TRGEN_Msk

#define PWM_TRGCON0_CNT1TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT1TRGEN_Pos)

PWM_T::TRGCON0: CNT1TRGEN Mask

Definition at line 3863 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT1TRGEN_Pos

#define PWM_TRGCON0_CNT1TRGEN_Pos (9)

PWM_T::TRGCON0: CNT1TRGEN Position

Definition at line 3862 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT2TRGEN_Msk

#define PWM_TRGCON0_CNT2TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT2TRGEN_Pos)

PWM_T::TRGCON0: CNT2TRGEN Mask

Definition at line 3875 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT2TRGEN_Pos

#define PWM_TRGCON0_CNT2TRGEN_Pos (17)

PWM_T::TRGCON0: CNT2TRGEN Position

Definition at line 3874 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT3TRGEN_Msk

#define PWM_TRGCON0_CNT3TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT3TRGEN_Pos)

PWM_T::TRGCON0: CNT3TRGEN Mask

Definition at line 3887 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT3TRGEN_Pos

#define PWM_TRGCON0_CNT3TRGEN_Pos (25)

PWM_T::TRGCON0: CNT3TRGEN Position

Definition at line 3886 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P0TRGEN_Msk

#define PWM_TRGCON0_P0TRGEN_Msk (0x1ul << PWM_TRGCON0_P0TRGEN_Pos)

PWM_T::TRGCON0: P0TRGEN Mask

Definition at line 3857 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P0TRGEN_Pos

#define PWM_TRGCON0_P0TRGEN_Pos (3)

PWM_T::TRGCON0: P0TRGEN Position

Definition at line 3856 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P1TRGEN_Msk

#define PWM_TRGCON0_P1TRGEN_Msk (0x1ul << PWM_TRGCON0_P1TRGEN_Pos)

PWM_T::TRGCON0: P1TRGEN Mask

Definition at line 3869 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P1TRGEN_Pos

#define PWM_TRGCON0_P1TRGEN_Pos (11)

PWM_T::TRGCON0: P1TRGEN Position

Definition at line 3868 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P2TRGEN_Msk

#define PWM_TRGCON0_P2TRGEN_Msk (0x1ul << PWM_TRGCON0_P2TRGEN_Pos)

PWM_T::TRGCON0: P2TRGEN Mask

Definition at line 3881 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P2TRGEN_Pos

#define PWM_TRGCON0_P2TRGEN_Pos (19)

PWM_T::TRGCON0: P2TRGEN Position

Definition at line 3880 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P3TRGEN_Msk

#define PWM_TRGCON0_P3TRGEN_Msk (0x1ul << PWM_TRGCON0_P3TRGEN_Pos)

PWM_T::TRGCON0: P3TRGEN Mask

Definition at line 3893 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P3TRGEN_Pos

#define PWM_TRGCON0_P3TRGEN_Pos (27)

PWM_T::TRGCON0: P3TRGEN Position

Definition at line 3892 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM4TRGFEN_Msk

#define PWM_TRGCON1_CM4TRGFEN_Msk (0x1ul << PWM_TRGCON1_CM4TRGFEN_Pos)

PWM_T::TRGCON1: CM4TRGFEN Mask

Definition at line 3902 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM4TRGFEN_Pos

#define PWM_TRGCON1_CM4TRGFEN_Pos (2)

PWM_T::TRGCON1: CM4TRGFEN Position

Definition at line 3901 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM4TRGREN_Msk

#define PWM_TRGCON1_CM4TRGREN_Msk (0x1ul << PWM_TRGCON1_CM4TRGREN_Pos)

PWM_T::TRGCON1: CM4TRGREN Mask

Definition at line 3896 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM4TRGREN_Pos

#define PWM_TRGCON1_CM4TRGREN_Pos (0)

PWM_T::TRGCON1: CM4TRGREN Position

Definition at line 3895 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM5TRGFEN_Msk

#define PWM_TRGCON1_CM5TRGFEN_Msk (0x1ul << PWM_TRGCON1_CM5TRGFEN_Pos)

PWM_T::TRGCON1: CM5TRGFEN Mask

Definition at line 3914 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM5TRGFEN_Pos

#define PWM_TRGCON1_CM5TRGFEN_Pos (10)

PWM_T::TRGCON1: CM5TRGFEN Position

Definition at line 3913 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM5TRGREN_Msk

#define PWM_TRGCON1_CM5TRGREN_Msk (0x1ul << PWM_TRGCON1_CM5TRGREN_Pos)

PWM_T::TRGCON1: CM5TRGREN Mask

Definition at line 3908 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM5TRGREN_Pos

#define PWM_TRGCON1_CM5TRGREN_Pos (8)

PWM_T::TRGCON1: CM5TRGREN Position

Definition at line 3907 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CNT4TRGEN_Msk

#define PWM_TRGCON1_CNT4TRGEN_Msk (0x1ul << PWM_TRGCON1_CNT4TRGEN_Pos)

PWM_T::TRGCON1: CNT4TRGEN Mask

Definition at line 3899 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CNT4TRGEN_Pos

#define PWM_TRGCON1_CNT4TRGEN_Pos (1)

PWM_T::TRGCON1: CNT4TRGEN Position

Definition at line 3898 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CNT5TRGEN_Msk

#define PWM_TRGCON1_CNT5TRGEN_Msk (0x1ul << PWM_TRGCON1_CNT5TRGEN_Pos)

PWM_T::TRGCON1: CNT5TRGEN Mask

Definition at line 3911 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CNT5TRGEN_Pos

#define PWM_TRGCON1_CNT5TRGEN_Pos (9)

PWM_T::TRGCON1: CNT5TRGEN Position

Definition at line 3910 of file Mini51Series.h.

## ◆ PWM_TRGCON1_P4TRGEN_Msk

#define PWM_TRGCON1_P4TRGEN_Msk (0x1ul << PWM_TRGCON1_P4TRGEN_Pos)

PWM_T::TRGCON1: P4TRGEN Mask

Definition at line 3905 of file Mini51Series.h.

## ◆ PWM_TRGCON1_P4TRGEN_Pos

#define PWM_TRGCON1_P4TRGEN_Pos (3)

PWM_T::TRGCON1: P4TRGEN Position

Definition at line 3904 of file Mini51Series.h.

## ◆ PWM_TRGCON1_P5TRGEN_Msk

#define PWM_TRGCON1_P5TRGEN_Msk (0x1ul << PWM_TRGCON1_P5TRGEN_Pos)

PWM_T::TRGCON1: P5TRGEN Mask

Definition at line 3917 of file Mini51Series.h.

## ◆ PWM_TRGCON1_P5TRGEN_Pos

#define PWM_TRGCON1_P5TRGEN_Pos (11)

PWM_T::TRGCON1: P5TRGEN Position

Definition at line 3916 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR0FLAG_F_Msk

#define PWM_TRGSTS0_CMR0FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR0FLAG_F_Pos)

PWM_T::TRGSTS0: CMR0FLAG_F Mask

Definition at line 3926 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR0FLAG_F_Pos

#define PWM_TRGSTS0_CMR0FLAG_F_Pos (2)

PWM_T::TRGSTS0: CMR0FLAG_F Position

Definition at line 3925 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR0FLAG_R_Msk

#define PWM_TRGSTS0_CMR0FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR0FLAG_R_Pos)

PWM_T::TRGSTS0: CMR0FLAG_R Mask

Definition at line 3920 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR0FLAG_R_Pos

#define PWM_TRGSTS0_CMR0FLAG_R_Pos (0)

PWM_T::TRGSTS0: CMR0FLAG_R Position

Definition at line 3919 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR1FLAG_F_Msk

#define PWM_TRGSTS0_CMR1FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR1FLAG_F_Pos)

PWM_T::TRGSTS0: CMR1FLAG_F Mask

Definition at line 3938 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR1FLAG_F_Pos

#define PWM_TRGSTS0_CMR1FLAG_F_Pos (10)

PWM_T::TRGSTS0: CMR1FLAG_F Position

Definition at line 3937 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR1FLAG_R_Msk

#define PWM_TRGSTS0_CMR1FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR1FLAG_R_Pos)

PWM_T::TRGSTS0: CMR1FLAG_R Mask

Definition at line 3932 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR1FLAG_R_Pos

#define PWM_TRGSTS0_CMR1FLAG_R_Pos (8)

PWM_T::TRGSTS0: CMR1FLAG_R Position

Definition at line 3931 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR2FLAG_F_Msk

#define PWM_TRGSTS0_CMR2FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR2FLAG_F_Pos)

PWM_T::TRGSTS0: CMR2FLAG_F Mask

Definition at line 3950 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR2FLAG_F_Pos

#define PWM_TRGSTS0_CMR2FLAG_F_Pos (18)

PWM_T::TRGSTS0: CMR2FLAG_F Position

Definition at line 3949 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR2FLAG_R_Msk

#define PWM_TRGSTS0_CMR2FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR2FLAG_R_Pos)

PWM_T::TRGSTS0: CMR2FLAG_R Mask

Definition at line 3944 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR2FLAG_R_Pos

#define PWM_TRGSTS0_CMR2FLAG_R_Pos (16)

PWM_T::TRGSTS0: CMR2FLAG_R Position

Definition at line 3943 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR3FLAG_F_Msk

#define PWM_TRGSTS0_CMR3FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR3FLAG_F_Pos)

PWM_T::TRGSTS0: CMR3FLAG_F Mask

Definition at line 3962 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR3FLAG_F_Pos

#define PWM_TRGSTS0_CMR3FLAG_F_Pos (26)

PWM_T::TRGSTS0: CMR3FLAG_F Position

Definition at line 3961 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR3FLAG_R_Msk

#define PWM_TRGSTS0_CMR3FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR3FLAG_R_Pos)

PWM_T::TRGSTS0: CMR3FLAG_R Mask

Definition at line 3956 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR3FLAG_R_Pos

#define PWM_TRGSTS0_CMR3FLAG_R_Pos (24)

PWM_T::TRGSTS0: CMR3FLAG_R Position

Definition at line 3955 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT0FLAG_Msk

#define PWM_TRGSTS0_CNT0FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT0FLAG_Pos)

PWM_T::TRGSTS0: CNT0FLAG Mask

Definition at line 3923 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT0FLAG_Pos

#define PWM_TRGSTS0_CNT0FLAG_Pos (1)

PWM_T::TRGSTS0: CNT0FLAG Position

Definition at line 3922 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT1FLAG_Msk

#define PWM_TRGSTS0_CNT1FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT1FLAG_Pos)

PWM_T::TRGSTS0: CNT1FLAG Mask

Definition at line 3935 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT1FLAG_Pos

#define PWM_TRGSTS0_CNT1FLAG_Pos (9)

PWM_T::TRGSTS0: CNT1FLAG Position

Definition at line 3934 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT2FLAG_Msk

#define PWM_TRGSTS0_CNT2FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT2FLAG_Pos)

PWM_T::TRGSTS0: CNT2FLAG Mask

Definition at line 3947 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT2FLAG_Pos

#define PWM_TRGSTS0_CNT2FLAG_Pos (17)

PWM_T::TRGSTS0: CNT2FLAG Position

Definition at line 3946 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT3FLAG_Msk

#define PWM_TRGSTS0_CNT3FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT3FLAG_Pos)

PWM_T::TRGSTS0: CNT3FLAG Mask

Definition at line 3959 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT3FLAG_Pos

#define PWM_TRGSTS0_CNT3FLAG_Pos (25)

PWM_T::TRGSTS0: CNT3FLAG Position

Definition at line 3958 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID0FLAG_Msk

#define PWM_TRGSTS0_PERID0FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID0FLAG_Pos)

PWM_T::TRGSTS0: PERID0FLAG Mask

Definition at line 3929 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID0FLAG_Pos

#define PWM_TRGSTS0_PERID0FLAG_Pos (3)

PWM_T::TRGSTS0: PERID0FLAG Position

Definition at line 3928 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID1FLAG_Msk

#define PWM_TRGSTS0_PERID1FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID1FLAG_Pos)

PWM_T::TRGSTS0: PERID1FLAG Mask

Definition at line 3941 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID1FLAG_Pos

#define PWM_TRGSTS0_PERID1FLAG_Pos (11)

PWM_T::TRGSTS0: PERID1FLAG Position

Definition at line 3940 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID2FLAG_Msk

#define PWM_TRGSTS0_PERID2FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID2FLAG_Pos)

PWM_T::TRGSTS0: PERID2FLAG Mask

Definition at line 3953 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID2FLAG_Pos

#define PWM_TRGSTS0_PERID2FLAG_Pos (19)

PWM_T::TRGSTS0: PERID2FLAG Position

Definition at line 3952 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID3FLAG_Msk

#define PWM_TRGSTS0_PERID3FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID3FLAG_Pos)

PWM_T::TRGSTS0: PERID3FLAG Mask

Definition at line 3965 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID3FLAG_Pos

#define PWM_TRGSTS0_PERID3FLAG_Pos (27)

PWM_T::TRGSTS0: PERID3FLAG Position

Definition at line 3964 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR4FLAG_F_Msk

#define PWM_TRGSTS1_CMR4FLAG_F_Msk (0x1ul << PWM_TRGSTS1_CMR4FLAG_F_Pos)

PWM_T::TRGSTS1: CMR4FLAG_F Mask

Definition at line 3974 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR4FLAG_F_Pos

#define PWM_TRGSTS1_CMR4FLAG_F_Pos (2)

PWM_T::TRGSTS1: CMR4FLAG_F Position

Definition at line 3973 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR4FLAG_R_Msk

#define PWM_TRGSTS1_CMR4FLAG_R_Msk (0x1ul << PWM_TRGSTS1_CMR4FLAG_R_Pos)

PWM_T::TRGSTS1: CMR4FLAG_R Mask

Definition at line 3968 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR4FLAG_R_Pos

#define PWM_TRGSTS1_CMR4FLAG_R_Pos (0)

PWM_T::TRGSTS1: CMR4FLAG_R Position

Definition at line 3967 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR5FLAG_F_Msk

#define PWM_TRGSTS1_CMR5FLAG_F_Msk (0x1ul << PWM_TRGSTS1_CMR5FLAG_F_Pos)

PWM_T::TRGSTS1: CMR5FLAG_F Mask

Definition at line 3986 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR5FLAG_F_Pos

#define PWM_TRGSTS1_CMR5FLAG_F_Pos (10)

PWM_T::TRGSTS1: CMR5FLAG_F Position

Definition at line 3985 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR5FLAG_R_Msk

#define PWM_TRGSTS1_CMR5FLAG_R_Msk (0x1ul << PWM_TRGSTS1_CMR5FLAG_R_Pos)

PWM_T::TRGSTS1: CMR5FLAG_R Mask

Definition at line 3980 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR5FLAG_R_Pos

#define PWM_TRGSTS1_CMR5FLAG_R_Pos (8)

PWM_T::TRGSTS1: CMR5FLAG_R Position

Definition at line 3979 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CNT4FLAG_Msk

#define PWM_TRGSTS1_CNT4FLAG_Msk (0x1ul << PWM_TRGSTS1_CNT4FLAG_Pos)

PWM_T::TRGSTS1: CNT4FLAG Mask

Definition at line 3971 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CNT4FLAG_Pos

#define PWM_TRGSTS1_CNT4FLAG_Pos (1)

PWM_T::TRGSTS1: CNT4FLAG Position

Definition at line 3970 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CNT5FLAG_Msk

#define PWM_TRGSTS1_CNT5FLAG_Msk (0x1ul << PWM_TRGSTS1_CNT5FLAG_Pos)

PWM_T::TRGSTS1: CNT5FLAG Mask

Definition at line 3983 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CNT5FLAG_Pos

#define PWM_TRGSTS1_CNT5FLAG_Pos (9)

PWM_T::TRGSTS1: CNT5FLAG Position

Definition at line 3982 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_PERID4FLAG_Msk

#define PWM_TRGSTS1_PERID4FLAG_Msk (0x1ul << PWM_TRGSTS1_PERID4FLAG_Pos)

PWM_T::TRGSTS1: PERID4FLAG Mask

Definition at line 3977 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_PERID4FLAG_Pos

#define PWM_TRGSTS1_PERID4FLAG_Pos (3)

PWM_T::TRGSTS1: PERID4FLAG Position

Definition at line 3976 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_PERID5FLAG_Msk

#define PWM_TRGSTS1_PERID5FLAG_Msk (0x1ul << PWM_TRGSTS1_PERID5FLAG_Pos)

PWM_T::TRGSTS1: PERID5FLAG Mask

Definition at line 3989 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_PERID5FLAG_Pos

#define PWM_TRGSTS1_PERID5FLAG_Pos (11)

PWM_T::TRGSTS1: PERID5FLAG Position

Definition at line 3988 of file Mini51Series.h.

## ◆ SPI_CNTRL2_BCn_Msk

#define SPI_CNTRL2_BCn_Msk (0x1ul << SPI_CNTRL2_BCn_Pos)

SPI_T::CNTRL2: BCn Mask

Definition at line 4588 of file Mini51Series.h.

## ◆ SPI_CNTRL2_BCn_Pos

#define SPI_CNTRL2_BCn_Pos (31)

SPI_T::CNTRL2: BCn Position

Definition at line 4587 of file Mini51Series.h.

## ◆ SPI_CNTRL2_NOSLVSEL_Msk

#define SPI_CNTRL2_NOSLVSEL_Msk (0x1ul << SPI_CNTRL2_NOSLVSEL_Pos)

SPI_T::CNTRL2: NOSLVSEL Mask

Definition at line 4573 of file Mini51Series.h.

## ◆ SPI_CNTRL2_NOSLVSEL_Pos

#define SPI_CNTRL2_NOSLVSEL_Pos (8)

SPI_T::CNTRL2: NOSLVSEL Position

Definition at line 4572 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SLV_ABORT_Msk

#define SPI_CNTRL2_SLV_ABORT_Msk (0x1ul << SPI_CNTRL2_SLV_ABORT_Pos)

SPI_T::CNTRL2: SLV_ABORT Mask

Definition at line 4576 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SLV_ABORT_Pos

#define SPI_CNTRL2_SLV_ABORT_Pos (9)

SPI_T::CNTRL2: SLV_ABORT Position

Definition at line 4575 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SLV_START_INTSTS_Msk

#define SPI_CNTRL2_SLV_START_INTSTS_Msk (0x1ul << SPI_CNTRL2_SLV_START_INTSTS_Pos)

SPI_T::CNTRL2: SLV_START_INTSTS Mask

Definition at line 4582 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SLV_START_INTSTS_Pos

#define SPI_CNTRL2_SLV_START_INTSTS_Pos (11)

SPI_T::CNTRL2: SLV_START_INTSTS Position

Definition at line 4581 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SS_INT_OPT_Msk

#define SPI_CNTRL2_SS_INT_OPT_Msk (0x1ul << SPI_CNTRL2_SS_INT_OPT_Pos)

SPI_T::CNTRL2: SS_INT_OPT Mask

Definition at line 4585 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SS_INT_OPT_Pos

#define SPI_CNTRL2_SS_INT_OPT_Pos (16)

SPI_T::CNTRL2: SS_INT_OPT Position

Definition at line 4584 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SSTA_INTEN_Msk

#define SPI_CNTRL2_SSTA_INTEN_Msk (0x1ul << SPI_CNTRL2_SSTA_INTEN_Pos)

SPI_T::CNTRL2: SSTA_INTEN Mask

Definition at line 4579 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SSTA_INTEN_Pos

#define SPI_CNTRL2_SSTA_INTEN_Pos (10)

SPI_T::CNTRL2: SSTA_INTEN Position

Definition at line 4578 of file Mini51Series.h.

## ◆ SPI_CNTRL_CLKP_Msk

#define SPI_CNTRL_CLKP_Msk (0x1ul << SPI_CNTRL_CLKP_Pos)

SPI_T::CNTRL: CLKP Mask

Definition at line 4516 of file Mini51Series.h.

## ◆ SPI_CNTRL_CLKP_Pos

#define SPI_CNTRL_CLKP_Pos (11)

SPI_T::CNTRL: CLKP Position

Definition at line 4515 of file Mini51Series.h.

## ◆ SPI_CNTRL_FIFO_Msk

#define SPI_CNTRL_FIFO_Msk (0x1ul << SPI_CNTRL_FIFO_Pos)

SPI_T::CNTRL: FIFO Mask

Definition at line 4534 of file Mini51Series.h.

## ◆ SPI_CNTRL_FIFO_Pos

#define SPI_CNTRL_FIFO_Pos (21)

SPI_T::CNTRL: FIFO Position

Definition at line 4533 of file Mini51Series.h.

## ◆ SPI_CNTRL_GO_BUSY_Msk

#define SPI_CNTRL_GO_BUSY_Msk (0x1ul << SPI_CNTRL_GO_BUSY_Pos)

SPI_T::CNTRL: GO_BUSY Mask

Definition at line 4501 of file Mini51Series.h.

## ◆ SPI_CNTRL_GO_BUSY_Pos

#define SPI_CNTRL_GO_BUSY_Pos (0)

    @addtogroup SPI_CONST SPI Bit Field Definition
    Constant Definitions for SPI Controller

SPI_T::CNTRL: GO_BUSY Position

Definition at line 4500 of file Mini51Series.h.

## ◆ SPI_CNTRL_IE_Msk

#define SPI_CNTRL_IE_Msk (0x1ul << SPI_CNTRL_IE_Pos)

SPI_T::CNTRL: IE Mask

Definition at line 4525 of file Mini51Series.h.

## ◆ SPI_CNTRL_IE_Pos

#define SPI_CNTRL_IE_Pos (17)

SPI_T::CNTRL: IE Position

Definition at line 4524 of file Mini51Series.h.

## ◆ SPI_CNTRL_IF_Msk

#define SPI_CNTRL_IF_Msk (0x1ul << SPI_CNTRL_IF_Pos)

SPI_T::CNTRL: IF Mask

Definition at line 4522 of file Mini51Series.h.

## ◆ SPI_CNTRL_IF_Pos

#define SPI_CNTRL_IF_Pos (16)

SPI_T::CNTRL: IF Position

Definition at line 4521 of file Mini51Series.h.

## ◆ SPI_CNTRL_LSB_Msk

#define SPI_CNTRL_LSB_Msk (0x1ul << SPI_CNTRL_LSB_Pos)

SPI_T::CNTRL: LSB Mask

Definition at line 4513 of file Mini51Series.h.

## ◆ SPI_CNTRL_LSB_Pos

#define SPI_CNTRL_LSB_Pos (10)

SPI_T::CNTRL: LSB Position

Definition at line 4512 of file Mini51Series.h.

## ◆ SPI_CNTRL_REORDER_Msk

#define SPI_CNTRL_REORDER_Msk (0x1ul << SPI_CNTRL_REORDER_Pos)

SPI_T::CNTRL: REORDER Mask

Definition at line 4531 of file Mini51Series.h.

## ◆ SPI_CNTRL_REORDER_Pos

#define SPI_CNTRL_REORDER_Pos (19)

SPI_T::CNTRL: REORDER Position

Definition at line 4530 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_EMPTY_Msk

#define SPI_CNTRL_RX_EMPTY_Msk (0x1ul << SPI_CNTRL_RX_EMPTY_Pos)

SPI_T::CNTRL: RX_EMPTY Mask

Definition at line 4537 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_EMPTY_Pos

#define SPI_CNTRL_RX_EMPTY_Pos (24)

SPI_T::CNTRL: RX_EMPTY Position

Definition at line 4536 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_FULL_Msk

#define SPI_CNTRL_RX_FULL_Msk (0x1ul << SPI_CNTRL_RX_FULL_Pos)

SPI_T::CNTRL: RX_FULL Mask

Definition at line 4540 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_FULL_Pos

#define SPI_CNTRL_RX_FULL_Pos (25)

SPI_T::CNTRL: RX_FULL Position

Definition at line 4539 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_NEG_Msk

#define SPI_CNTRL_RX_NEG_Msk (0x1ul << SPI_CNTRL_RX_NEG_Pos)

SPI_T::CNTRL: RX_NEG Mask

Definition at line 4504 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_NEG_Pos

#define SPI_CNTRL_RX_NEG_Pos (1)

SPI_T::CNTRL: RX_NEG Position

Definition at line 4503 of file Mini51Series.h.

## ◆ SPI_CNTRL_SLAVE_Msk

#define SPI_CNTRL_SLAVE_Msk (0x1ul << SPI_CNTRL_SLAVE_Pos)

SPI_T::CNTRL: SLAVE Mask

Definition at line 4528 of file Mini51Series.h.

## ◆ SPI_CNTRL_SLAVE_Pos

#define SPI_CNTRL_SLAVE_Pos (18)

SPI_T::CNTRL: SLAVE Position

Definition at line 4527 of file Mini51Series.h.

## ◆ SPI_CNTRL_SP_CYCLE_Msk

#define SPI_CNTRL_SP_CYCLE_Msk (0xful << SPI_CNTRL_SP_CYCLE_Pos)

SPI_T::CNTRL: SP_CYCLE Mask

Definition at line 4519 of file Mini51Series.h.

## ◆ SPI_CNTRL_SP_CYCLE_Pos

#define SPI_CNTRL_SP_CYCLE_Pos (12)

SPI_T::CNTRL: SP_CYCLE Position

Definition at line 4518 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_BIT_LEN_Msk

#define SPI_CNTRL_TX_BIT_LEN_Msk (0x1ful << SPI_CNTRL_TX_BIT_LEN_Pos)

SPI_T::CNTRL: TX_BIT_LEN Mask

Definition at line 4510 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_BIT_LEN_Pos

#define SPI_CNTRL_TX_BIT_LEN_Pos (3)

SPI_T::CNTRL: TX_BIT_LEN Position

Definition at line 4509 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_EMPTY_Msk

#define SPI_CNTRL_TX_EMPTY_Msk (0x1ul << SPI_CNTRL_TX_EMPTY_Pos)

SPI_T::CNTRL: TX_EMPTY Mask

Definition at line 4543 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_EMPTY_Pos

#define SPI_CNTRL_TX_EMPTY_Pos (26)

SPI_T::CNTRL: TX_EMPTY Position

Definition at line 4542 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_FULL_Msk

#define SPI_CNTRL_TX_FULL_Msk (0x1ul << SPI_CNTRL_TX_FULL_Pos)

SPI_T::CNTRL: TX_FULL Mask

Definition at line 4546 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_FULL_Pos

#define SPI_CNTRL_TX_FULL_Pos (27)

SPI_T::CNTRL: TX_FULL Position

Definition at line 4545 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_NEG_Msk

#define SPI_CNTRL_TX_NEG_Msk (0x1ul << SPI_CNTRL_TX_NEG_Pos)

SPI_T::CNTRL: TX_NEG Mask

Definition at line 4507 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_NEG_Pos

#define SPI_CNTRL_TX_NEG_Pos (2)

SPI_T::CNTRL: TX_NEG Position

Definition at line 4506 of file Mini51Series.h.

## ◆ SPI_DIVIDER_DIVIDER_Msk

#define SPI_DIVIDER_DIVIDER_Msk (0xfful << SPI_DIVIDER_DIVIDER_Pos)

SPI_T::DIVIDER: DIVIDER Mask

Definition at line 4549 of file Mini51Series.h.

## ◆ SPI_DIVIDER_DIVIDER_Pos

#define SPI_DIVIDER_DIVIDER_Pos (0)

SPI_T::DIVIDER: DIVIDER Position

Definition at line 4548 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_CLR_Msk

#define SPI_FIFO_CTL_RX_CLR_Msk (0x1ul << SPI_FIFO_CTL_RX_CLR_Pos)

SPI_T::FIFO_CTL: RX_CLR Mask

Definition at line 4591 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_CLR_Pos

#define SPI_FIFO_CTL_RX_CLR_Pos (0)

SPI_T::FIFO_CTL: RX_CLR Position

Definition at line 4590 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_INTEN_Msk

#define SPI_FIFO_CTL_RX_INTEN_Msk (0x1ul << SPI_FIFO_CTL_RX_INTEN_Pos)

SPI_T::FIFO_CTL: RX_INTEN Mask

Definition at line 4597 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_INTEN_Pos

#define SPI_FIFO_CTL_RX_INTEN_Pos (2)

SPI_T::FIFO_CTL: RX_INTEN Position

Definition at line 4596 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_THRESHOLD_Msk

#define SPI_FIFO_CTL_RX_THRESHOLD_Msk (0x3ul << SPI_FIFO_CTL_RX_THRESHOLD_Pos)

SPI_T::FIFO_CTL: RX_THRESHOLD Mask

Definition at line 4609 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_THRESHOLD_Pos

#define SPI_FIFO_CTL_RX_THRESHOLD_Pos (24)

SPI_T::FIFO_CTL: RX_THRESHOLD Position

Definition at line 4608 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RXOV_INTEN_Msk

#define SPI_FIFO_CTL_RXOV_INTEN_Msk (0x1ul << SPI_FIFO_CTL_RXOV_INTEN_Pos)

SPI_T::FIFO_CTL: RXOV_INTEN Mask

Definition at line 4603 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RXOV_INTEN_Pos

#define SPI_FIFO_CTL_RXOV_INTEN_Pos (6)

SPI_T::FIFO_CTL: RXOV_INTEN Position

Definition at line 4602 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TIMEOUT_INTEN_Msk

#define SPI_FIFO_CTL_TIMEOUT_INTEN_Msk (0x1ul << SPI_FIFO_CTL_TIMEOUT_INTEN_Pos)

SPI_T::FIFO_CTL: TIMEOUT_INTEN Mask

Definition at line 4606 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TIMEOUT_INTEN_Pos

#define SPI_FIFO_CTL_TIMEOUT_INTEN_Pos (21)

SPI_T::FIFO_CTL: TIMEOUT_INTEN Position

Definition at line 4605 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_CLR_Msk

#define SPI_FIFO_CTL_TX_CLR_Msk (0x1ul << SPI_FIFO_CTL_TX_CLR_Pos)

SPI_T::FIFO_CTL: TX_CLR Mask

Definition at line 4594 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_CLR_Pos

#define SPI_FIFO_CTL_TX_CLR_Pos (1)

SPI_T::FIFO_CTL: TX_CLR Position

Definition at line 4593 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_INTEN_Msk

#define SPI_FIFO_CTL_TX_INTEN_Msk (0x1ul << SPI_FIFO_CTL_TX_INTEN_Pos)

SPI_T::FIFO_CTL: TX_INTEN Mask

Definition at line 4600 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_INTEN_Pos

#define SPI_FIFO_CTL_TX_INTEN_Pos (3)

SPI_T::FIFO_CTL: TX_INTEN Position

Definition at line 4599 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_THRESHOLD_Msk

#define SPI_FIFO_CTL_TX_THRESHOLD_Msk (0x3ul << SPI_FIFO_CTL_TX_THRESHOLD_Pos)

SPI_T::FIFO_CTL: TX_THRESHOLD Mask

Definition at line 4612 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_THRESHOLD_Pos

#define SPI_FIFO_CTL_TX_THRESHOLD_Pos (28)

SPI_T::FIFO_CTL: TX_THRESHOLD Position

Definition at line 4611 of file Mini51Series.h.

## ◆ SPI_RX_RX_Msk

#define SPI_RX_RX_Msk (0xfffffffful << SPI_RX_RX_Pos)

SPI_T::RX: RX Mask

Definition at line 4567 of file Mini51Series.h.

## ◆ SPI_RX_RX_Pos

#define SPI_RX_RX_Pos (0)

SPI_T::RX: RX Position

Definition at line 4566 of file Mini51Series.h.

## ◆ SPI_SSR_AUTOSS_Msk

#define SPI_SSR_AUTOSS_Msk (0x1ul << SPI_SSR_AUTOSS_Pos)

SPI_T::SSR: AUTOSS Mask

Definition at line 4558 of file Mini51Series.h.

## ◆ SPI_SSR_AUTOSS_Pos

#define SPI_SSR_AUTOSS_Pos (3)

SPI_T::SSR: AUTOSS Position

Definition at line 4557 of file Mini51Series.h.

## ◆ SPI_SSR_LTRIG_FLAG_Msk

#define SPI_SSR_LTRIG_FLAG_Msk (0x1ul << SPI_SSR_LTRIG_FLAG_Pos)

SPI_T::SSR: LTRIG_FLAG Mask

Definition at line 4564 of file Mini51Series.h.

## ◆ SPI_SSR_LTRIG_FLAG_Pos

#define SPI_SSR_LTRIG_FLAG_Pos (5)

SPI_T::SSR: LTRIG_FLAG Position

Definition at line 4563 of file Mini51Series.h.

## ◆ SPI_SSR_SS_LTRIG_Msk

#define SPI_SSR_SS_LTRIG_Msk (0x1ul << SPI_SSR_SS_LTRIG_Pos)

SPI_T::SSR: SS_LTRIG Mask

Definition at line 4561 of file Mini51Series.h.

## ◆ SPI_SSR_SS_LTRIG_Pos

#define SPI_SSR_SS_LTRIG_Pos (4)

SPI_T::SSR: SS_LTRIG Position

Definition at line 4560 of file Mini51Series.h.

## ◆ SPI_SSR_SS_LVL_Msk

#define SPI_SSR_SS_LVL_Msk (0x1ul << SPI_SSR_SS_LVL_Pos)

SPI_T::SSR: SS_LVL Mask

Definition at line 4555 of file Mini51Series.h.

## ◆ SPI_SSR_SS_LVL_Pos

#define SPI_SSR_SS_LVL_Pos (2)

SPI_T::SSR: SS_LVL Position

Definition at line 4554 of file Mini51Series.h.

## ◆ SPI_SSR_SSR_Msk

#define SPI_SSR_SSR_Msk (0x1ul << SPI_SSR_SSR_Pos)

SPI_T::SSR: SSR Mask

Definition at line 4552 of file Mini51Series.h.

## ◆ SPI_SSR_SSR_Pos

#define SPI_SSR_SSR_Pos (0)

SPI_T::SSR: SSR Position

Definition at line 4551 of file Mini51Series.h.

## ◆ SPI_STATUS_IF_Msk

#define SPI_STATUS_IF_Msk (0x1ul << SPI_STATUS_IF_Pos)

SPI_T::STATUS: IF Mask

Definition at line 4630 of file Mini51Series.h.

## ◆ SPI_STATUS_IF_Pos

#define SPI_STATUS_IF_Pos (16)

SPI_T::STATUS: IF Position

Definition at line 4629 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_EMPTY_Msk

#define SPI_STATUS_RX_EMPTY_Msk (0x1ul << SPI_STATUS_RX_EMPTY_Pos)

SPI_T::STATUS: RX_EMPTY Mask

Definition at line 4636 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_EMPTY_Pos

#define SPI_STATUS_RX_EMPTY_Pos (24)

SPI_T::STATUS: RX_EMPTY Position

Definition at line 4635 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_FIFO_COUNT_Msk

#define SPI_STATUS_RX_FIFO_COUNT_Msk (0xful << SPI_STATUS_RX_FIFO_COUNT_Pos)

SPI_T::STATUS: RX_FIFO_COUNT Mask

Definition at line 4627 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_FIFO_COUNT_Pos

#define SPI_STATUS_RX_FIFO_COUNT_Pos (12)

SPI_T::STATUS: RX_FIFO_COUNT Position

Definition at line 4626 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_FULL_Msk

#define SPI_STATUS_RX_FULL_Msk (0x1ul << SPI_STATUS_RX_FULL_Pos)

SPI_T::STATUS: RX_FULL Mask

Definition at line 4639 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_FULL_Pos

#define SPI_STATUS_RX_FULL_Pos (25)

SPI_T::STATUS: RX_FULL Position

Definition at line 4638 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_INTSTS_Msk

#define SPI_STATUS_RX_INTSTS_Msk (0x1ul << SPI_STATUS_RX_INTSTS_Pos)

SPI_T::STATUS: RX_INTSTS Mask

Definition at line 4615 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_INTSTS_Pos

#define SPI_STATUS_RX_INTSTS_Pos (0)

SPI_T::STATUS: RX_INTSTS Position

Definition at line 4614 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_OVERRUN_Msk

#define SPI_STATUS_RX_OVERRUN_Msk (0x1ul << SPI_STATUS_RX_OVERRUN_Pos)

SPI_T::STATUS: RX_OVERRUN Mask

Definition at line 4618 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_OVERRUN_Pos

#define SPI_STATUS_RX_OVERRUN_Pos (2)

SPI_T::STATUS: RX_OVERRUN Position

Definition at line 4617 of file Mini51Series.h.

## ◆ SPI_STATUS_SLV_START_INTSTS_Msk

#define SPI_STATUS_SLV_START_INTSTS_Msk (0x1ul << SPI_STATUS_SLV_START_INTSTS_Pos)

SPI_T::STATUS: SLV_START_INTSTS Mask

Definition at line 4624 of file Mini51Series.h.

## ◆ SPI_STATUS_SLV_START_INTSTS_Pos

#define SPI_STATUS_SLV_START_INTSTS_Pos (11)

SPI_T::STATUS: SLV_START_INTSTS Position

Definition at line 4623 of file Mini51Series.h.

## ◆ SPI_STATUS_TIMEOUT_Msk

#define SPI_STATUS_TIMEOUT_Msk (0x1ul << SPI_STATUS_TIMEOUT_Pos)

SPI_T::STATUS: TIMEOUT Mask

Definition at line 4633 of file Mini51Series.h.

## ◆ SPI_STATUS_TIMEOUT_Pos

#define SPI_STATUS_TIMEOUT_Pos (20)

SPI_T::STATUS: TIMEOUT Position

Definition at line 4632 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_EMPTY_Msk

#define SPI_STATUS_TX_EMPTY_Msk (0x1ul << SPI_STATUS_TX_EMPTY_Pos)

SPI_T::STATUS: TX_EMPTY Mask

Definition at line 4642 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_EMPTY_Pos

#define SPI_STATUS_TX_EMPTY_Pos (26)

SPI_T::STATUS: TX_EMPTY Position

Definition at line 4641 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_FIFO_COUNT_Msk

#define SPI_STATUS_TX_FIFO_COUNT_Msk (0xful << SPI_STATUS_TX_FIFO_COUNT_Pos)

SPI_T::STATUS: TX_FIFO_COUNT Mask

Definition at line 4648 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_FIFO_COUNT_Pos

#define SPI_STATUS_TX_FIFO_COUNT_Pos (28)

SPI_T::STATUS: TX_FIFO_COUNT Position

Definition at line 4647 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_FULL_Msk

#define SPI_STATUS_TX_FULL_Msk (0x1ul << SPI_STATUS_TX_FULL_Pos)

SPI_T::STATUS: TX_FULL Mask

Definition at line 4645 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_FULL_Pos

#define SPI_STATUS_TX_FULL_Pos (27)

SPI_T::STATUS: TX_FULL Position

Definition at line 4644 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_INTSTS_Msk

#define SPI_STATUS_TX_INTSTS_Msk (0x1ul << SPI_STATUS_TX_INTSTS_Pos)

SPI_T::STATUS: TX_INTSTS Mask

Definition at line 4621 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_INTSTS_Pos

#define SPI_STATUS_TX_INTSTS_Pos (4)

SPI_T::STATUS: TX_INTSTS Position

Definition at line 4620 of file Mini51Series.h.

## ◆ SPI_TX_TX_Msk

#define SPI_TX_TX_Msk (0xfffffffful << SPI_TX_TX_Pos)

SPI_T::TX: TX Mask

Definition at line 4570 of file Mini51Series.h.

## ◆ SPI_TX_TX_Pos

#define SPI_TX_TX_Pos (0)

SPI_T::TX: TX Position

Definition at line 4569 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_INTF_Msk

#define SYS_BODCR_BOD_INTF_Msk (0x1ul << SYS_BODCR_BOD_INTF_Pos)

GCR_T::BODCTL: BOD_INTF Mask

Definition at line 1605 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_INTF_Pos

#define SYS_BODCR_BOD_INTF_Pos (4)

GCR_T::BODCTL: BOD_INTF Position

Definition at line 1604 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_LPM_Msk

#define SYS_BODCR_BOD_LPM_Msk (0x1ul << SYS_BODCR_BOD_LPM_Pos)

GCR_T::BODCTL: BOD_LPM Mask

Definition at line 1608 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_LPM_Pos

#define SYS_BODCR_BOD_LPM_Pos (5)

GCR_T::BODCTL: BOD_LPM Position

Definition at line 1607 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_OUT_Msk

#define SYS_BODCR_BOD_OUT_Msk (0x1ul << SYS_BODCR_BOD_OUT_Pos)

GCR_T::BODCTL: BOD_OUT Mask

Definition at line 1611 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_OUT_Pos

#define SYS_BODCR_BOD_OUT_Pos (6)

GCR_T::BODCTL: BOD_OUT Position

Definition at line 1610 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_RSTEN_Msk

#define SYS_BODCR_BOD_RSTEN_Msk (0x1ul << SYS_BODCR_BOD_RSTEN_Pos)

GCR_T::BODCTL: BOD_RSTEN Mask

Definition at line 1602 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_RSTEN_Pos

#define SYS_BODCR_BOD_RSTEN_Pos (3)

GCR_T::BODCTL: BOD_RSTEN Position

Definition at line 1601 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_VL_EXT_Msk

#define SYS_BODCR_BOD_VL_EXT_Msk (0x1ul << SYS_BODCR_BOD_VL_EXT_Pos)

GCR_T::BODCTL: BOD_VL_EXT Mask

Definition at line 1596 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_VL_EXT_Pos

#define SYS_BODCR_BOD_VL_EXT_Pos (0)

GCR_T::BODCTL: BOD_VL_EXT Position

Definition at line 1595 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_VL_Msk

#define SYS_BODCR_BOD_VL_Msk (0x3ul << SYS_BODCR_BOD_VL_Pos)

GCR_T::BODCTL: BOD_VL Mask

Definition at line 1599 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_VL_Pos

#define SYS_BODCR_BOD_VL_Pos (1)

GCR_T::BODCTL: BOD_VL Position

Definition at line 1598 of file Mini51Series.h.

## ◆ SYS_IPRSTC1_CHIP_RST_Msk

#define SYS_IPRSTC1_CHIP_RST_Msk (0x1ul << SYS_IPRSTC1_CHIP_RST_Pos)

GCR_T::IPRSTC1: CHIP_RST Mask

Definition at line 1563 of file Mini51Series.h.

## ◆ SYS_IPRSTC1_CHIP_RST_Pos

#define SYS_IPRSTC1_CHIP_RST_Pos (0)

GCR_T::IPRSTC1: CHIP_RST Position

Definition at line 1562 of file Mini51Series.h.

## ◆ SYS_IPRSTC1_CPU_RST_Msk

#define SYS_IPRSTC1_CPU_RST_Msk (0x1ul << SYS_IPRSTC1_CPU_RST_Pos)

GCR_T::IPRSTC1: CPU_RST Mask

Definition at line 1566 of file Mini51Series.h.

## ◆ SYS_IPRSTC1_CPU_RST_Pos

#define SYS_IPRSTC1_CPU_RST_Pos (1)

GCR_T::IPRSTC1: CPU_RST Position

Definition at line 1565 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_ACMP_RST_Msk

#define SYS_IPRSTC2_ACMP_RST_Msk (0x1ul << SYS_IPRSTC2_ACMP_RST_Pos)

GCR_T::IPRSTC2: ACMP_RST Mask

Definition at line 1590 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_ACMP_RST_Pos

#define SYS_IPRSTC2_ACMP_RST_Pos (22)

GCR_T::IPRSTC2: ACMP_RST Position

Definition at line 1589 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_ADC_RST_Msk

#define SYS_IPRSTC2_ADC_RST_Msk (0x1ul << SYS_IPRSTC2_ADC_RST_Pos)

GCR_T::IPRSTC2: ADC_RST Mask

Definition at line 1593 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_ADC_RST_Pos

#define SYS_IPRSTC2_ADC_RST_Pos (28)

GCR_T::IPRSTC2: ADC_RST Position

Definition at line 1592 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_GPIO_RST_Msk

#define SYS_IPRSTC2_GPIO_RST_Msk (0x1ul << SYS_IPRSTC2_GPIO_RST_Pos)

GCR_T::IPRSTC2: GPIO_RST Mask

Definition at line 1569 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_GPIO_RST_Pos

#define SYS_IPRSTC2_GPIO_RST_Pos (1)

GCR_T::IPRSTC2: GPIO_RST Position

Definition at line 1568 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_I2C_RST_Msk

#define SYS_IPRSTC2_I2C_RST_Msk (0x1ul << SYS_IPRSTC2_I2C_RST_Pos)

GCR_T::IPRSTC2: I2C_RST Mask

Definition at line 1578 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_I2C_RST_Pos

#define SYS_IPRSTC2_I2C_RST_Pos (8)

GCR_T::IPRSTC2: I2C_RST Position

Definition at line 1577 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_PWM_RST_Msk

#define SYS_IPRSTC2_PWM_RST_Msk (0x1ul << SYS_IPRSTC2_PWM_RST_Pos)

GCR_T::IPRSTC2: PWM_RST Mask

Definition at line 1587 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_PWM_RST_Pos

#define SYS_IPRSTC2_PWM_RST_Pos (20)

GCR_T::IPRSTC2: PWM_RST Position

Definition at line 1586 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_SPI_RST_Msk

#define SYS_IPRSTC2_SPI_RST_Msk (0x1ul << SYS_IPRSTC2_SPI_RST_Pos)

GCR_T::IPRSTC2: SPI_RST Mask

Definition at line 1581 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_SPI_RST_Pos

#define SYS_IPRSTC2_SPI_RST_Pos (12)

GCR_T::IPRSTC2: SPI_RST Position

Definition at line 1580 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_TMR0_RST_Msk

#define SYS_IPRSTC2_TMR0_RST_Msk (0x1ul << SYS_IPRSTC2_TMR0_RST_Pos)

GCR_T::IPRSTC2: TMR0_RST Mask

Definition at line 1572 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_TMR0_RST_Pos

#define SYS_IPRSTC2_TMR0_RST_Pos (2)

GCR_T::IPRSTC2: TMR0_RST Position

Definition at line 1571 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_TMR1_RST_Msk

#define SYS_IPRSTC2_TMR1_RST_Msk (0x1ul << SYS_IPRSTC2_TMR1_RST_Pos)

GCR_T::IPRSTC2: TMR1_RST Mask

Definition at line 1575 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_TMR1_RST_Pos

#define SYS_IPRSTC2_TMR1_RST_Pos (3)

GCR_T::IPRSTC2: TMR1_RST Position

Definition at line 1574 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_UART_RST_Msk

#define SYS_IPRSTC2_UART_RST_Msk (0x1ul << SYS_IPRSTC2_UART_RST_Pos)

GCR_T::IPRSTC2: UART_RST Mask

Definition at line 1584 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_UART_RST_Pos

#define SYS_IPRSTC2_UART_RST_Pos (16)

GCR_T::IPRSTC2: UART_RST Position

Definition at line 1583 of file Mini51Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_LOOP_Msk

#define SYS_IRCTRIMCTL_TRIM_LOOP_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_LOOP_Pos)

GCR_T::IRCTRIMCTL: TRIM_LOOP Mask

Definition at line 1764 of file Mini51Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_LOOP_Pos

#define SYS_IRCTRIMCTL_TRIM_LOOP_Pos (4)

GCR_T::IRCTRIMCTL: TRIM_LOOP Position

Definition at line 1763 of file Mini51Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_SEL_Msk

#define SYS_IRCTRIMCTL_TRIM_SEL_Msk (0x1ul << SYS_IRCTRIMCTL_TRIM_SEL_Pos)

GCR_T::IRCTRIMCTL: TRIM_SEL Mask

Definition at line 1761 of file Mini51Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_SEL_Pos

#define SYS_IRCTRIMCTL_TRIM_SEL_Pos (0)

GCR_T::IRCTRIMCTL: TRIM_SEL Position

Definition at line 1760 of file Mini51Series.h.

## ◆ SYS_IRCTRIMIEN_32K_ERR_IEN_Msk

#define SYS_IRCTRIMIEN_32K_ERR_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_32K_ERR_IEN_Pos)

GCR_T::IRCTRIMIER: 32K_ERR_IEN Mask

Definition at line 1770 of file Mini51Series.h.

## ◆ SYS_IRCTRIMIEN_32K_ERR_IEN_Pos

#define SYS_IRCTRIMIEN_32K_ERR_IEN_Pos (2)

GCR_T::IRCTRIMIER: 32K_ERR_IEN Position

Definition at line 1769 of file Mini51Series.h.

## ◆ SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk

#define SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos)

GCR_T::IRCTRIMIER: TRIM_FAIL_IEN Mask

Definition at line 1767 of file Mini51Series.h.

## ◆ SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos

#define SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos (1)

GCR_T::IRCTRIMIER: TRIM_FAIL_IEN Position

Definition at line 1766 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_32K_ERR_INT_Msk

#define SYS_IRCTRIMINT_32K_ERR_INT_Msk (0x1ul << SYS_IRCTRIMINT_32K_ERR_INT_Pos)

GCR_T::IRCTRIMISR: 32K_ERR_INT Mask

Definition at line 1779 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_32K_ERR_INT_Pos

#define SYS_IRCTRIMINT_32K_ERR_INT_Pos (2)

GCR_T::IRCTRIMISR: 32K_ERR_INT Position

Definition at line 1778 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_FREQ_LOCK_Msk

#define SYS_IRCTRIMINT_FREQ_LOCK_Msk (0x1ul << SYS_IRCTRIMINT_FREQ_LOCK_Pos)

GCR_T::IRCTRIMISR: FREQ_LOCK Mask

Definition at line 1773 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_FREQ_LOCK_Pos

#define SYS_IRCTRIMINT_FREQ_LOCK_Pos (0)

GCR_T::IRCTRIMISR: FREQ_LOCK Position

Definition at line 1772 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk

#define SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk (0x1ul << SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos)

GCR_T::IRCTRIMISR: TRIM_FAIL_INT Mask

Definition at line 1776 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos

#define SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos (1)

GCR_T::IRCTRIMISR: TRIM_FAIL_INT Position

Definition at line 1775 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT0_Msk

#define SYS_P0_MFP_P0_ALT0_Msk (0x1ul << SYS_P0_MFP_P0_ALT0_Pos)

GCR_T::P0_MFP: P0_ALT0 Mask

Definition at line 1620 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT0_Pos

#define SYS_P0_MFP_P0_ALT0_Pos (8)

GCR_T::P0_MFP: P0_ALT0 Position

Definition at line 1619 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT1_Msk

#define SYS_P0_MFP_P0_ALT1_Msk (0x1ul << SYS_P0_MFP_P0_ALT1_Pos)

GCR_T::P0_MFP: P0_ALT1 Mask

Definition at line 1623 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT1_Pos

#define SYS_P0_MFP_P0_ALT1_Pos (9)

GCR_T::P0_MFP: P0_ALT1 Position

Definition at line 1622 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT4_Msk

#define SYS_P0_MFP_P0_ALT4_Msk (0x1ul << SYS_P0_MFP_P0_ALT4_Pos)

GCR_T::P0_MFP: P0_ALT4 Mask

Definition at line 1626 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT4_Pos

#define SYS_P0_MFP_P0_ALT4_Pos (12)

GCR_T::P0_MFP: P0_ALT4 Position

Definition at line 1625 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT5_Msk

#define SYS_P0_MFP_P0_ALT5_Msk (0x1ul << SYS_P0_MFP_P0_ALT5_Pos)

GCR_T::P0_MFP: P0_ALT5 Mask

Definition at line 1629 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT5_Pos

#define SYS_P0_MFP_P0_ALT5_Pos (13)

GCR_T::P0_MFP: P0_ALT5 Position

Definition at line 1628 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT6_Msk

#define SYS_P0_MFP_P0_ALT6_Msk (0x1ul << SYS_P0_MFP_P0_ALT6_Pos)

GCR_T::P0_MFP: P0_ALT6 Mask

Definition at line 1632 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT6_Pos

#define SYS_P0_MFP_P0_ALT6_Pos (14)

GCR_T::P0_MFP: P0_ALT6 Position

Definition at line 1631 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT7_Msk

#define SYS_P0_MFP_P0_ALT7_Msk (0x1ul << SYS_P0_MFP_P0_ALT7_Pos)

GCR_T::P0_MFP: P0_ALT7 Mask

Definition at line 1635 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT7_Pos

#define SYS_P0_MFP_P0_ALT7_Pos (15)

GCR_T::P0_MFP: P0_ALT7 Position

Definition at line 1634 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT_Msk

#define SYS_P0_MFP_P0_ALT_Msk (0xfful << SYS_P0_MFP_P0_ALT_Pos)

GCR_T::P0_MFP: P0_ALT Mask

Definition at line 1617 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT_Pos

#define SYS_P0_MFP_P0_ALT_Pos (8)

GCR_T::P0_MFP: P0_ALT Position

Definition at line 1616 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_MFP_Msk

#define SYS_P0_MFP_P0_MFP_Msk (0xfful << SYS_P0_MFP_P0_MFP_Pos)

GCR_T::P0_MFP: P0_MFP Mask

Definition at line 1614 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_MFP_Pos

#define SYS_P0_MFP_P0_MFP_Pos (0)

GCR_T::P0_MFP: P0_MFP Position

Definition at line 1613 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_TYPE_Msk

#define SYS_P0_MFP_P0_TYPE_Msk (0xfful << SYS_P0_MFP_P0_TYPE_Pos)

GCR_T::P0_MFP: P0_TYPE Mask

Definition at line 1638 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_TYPE_Pos

#define SYS_P0_MFP_P0_TYPE_Pos (16)

GCR_T::P0_MFP: P0_TYPE Position

Definition at line 1637 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT0_Msk

#define SYS_P1_MFP_P1_ALT0_Msk (0x1ul << SYS_P1_MFP_P1_ALT0_Pos)

GCR_T::P1_MFP: P1_ALT0 Mask

Definition at line 1647 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT0_Pos

#define SYS_P1_MFP_P1_ALT0_Pos (8)

GCR_T::P1_MFP: P1_ALT0 Position

Definition at line 1646 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT2_Msk

#define SYS_P1_MFP_P1_ALT2_Msk (0x1ul << SYS_P1_MFP_P1_ALT2_Pos)

GCR_T::P1_MFP: P1_ALT2 Mask

Definition at line 1650 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT2_Pos

#define SYS_P1_MFP_P1_ALT2_Pos (10)

GCR_T::P1_MFP: P1_ALT2 Position

Definition at line 1649 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT3_Msk

#define SYS_P1_MFP_P1_ALT3_Msk (0x1ul << SYS_P1_MFP_P1_ALT3_Pos)

GCR_T::P1_MFP: P1_ALT3 Mask

Definition at line 1653 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT3_Pos

#define SYS_P1_MFP_P1_ALT3_Pos (11)

GCR_T::P1_MFP: P1_ALT3 Position

Definition at line 1652 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT4_Msk

#define SYS_P1_MFP_P1_ALT4_Msk (0x1ul << SYS_P1_MFP_P1_ALT4_Pos)

GCR_T::P1_MFP: P1_ALT4 Mask

Definition at line 1656 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT4_Pos

#define SYS_P1_MFP_P1_ALT4_Pos (12)

GCR_T::P1_MFP: P1_ALT4 Position

Definition at line 1655 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT5_Msk

#define SYS_P1_MFP_P1_ALT5_Msk (0x1ul << SYS_P1_MFP_P1_ALT5_Pos)

GCR_T::P1_MFP: P1_ALT5 Mask

Definition at line 1659 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT5_Pos

#define SYS_P1_MFP_P1_ALT5_Pos (13)

GCR_T::P1_MFP: P1_ALT5 Position

Definition at line 1658 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT_Msk

#define SYS_P1_MFP_P1_ALT_Msk (0xfful << SYS_P1_MFP_P1_ALT_Pos)

GCR_T::P1_MFP: P1_ALT Mask

Definition at line 1644 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT_Pos

#define SYS_P1_MFP_P1_ALT_Pos (8)

GCR_T::P1_MFP: P1_ALT Position

Definition at line 1643 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_MFP_Msk

#define SYS_P1_MFP_P1_MFP_Msk (0xfful << SYS_P1_MFP_P1_MFP_Pos)

GCR_T::P1_MFP: P1_MFP Mask

Definition at line 1641 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_MFP_Pos

#define SYS_P1_MFP_P1_MFP_Pos (0)

GCR_T::P1_MFP: P1_MFP Position

Definition at line 1640 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_TYPE_Msk

#define SYS_P1_MFP_P1_TYPE_Msk (0xfful << SYS_P1_MFP_P1_TYPE_Pos)

GCR_T::P1_MFP: P1_TYPE Mask

Definition at line 1662 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_TYPE_Pos

#define SYS_P1_MFP_P1_TYPE_Pos (16)

GCR_T::P1_MFP: P1_TYPE Position

Definition at line 1661 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT2_Msk

#define SYS_P2_MFP_P2_ALT2_Msk (0x1ul << SYS_P2_MFP_P2_ALT2_Pos)

GCR_T::P2_MFP: P2_ALT2 Mask

Definition at line 1671 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT2_Pos

#define SYS_P2_MFP_P2_ALT2_Pos (10)

GCR_T::P2_MFP: P2_ALT2 Position

Definition at line 1670 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT3_Msk

#define SYS_P2_MFP_P2_ALT3_Msk (0x1ul << SYS_P2_MFP_P2_ALT3_Pos)

GCR_T::P2_MFP: P2_ALT3 Mask

Definition at line 1674 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT3_Pos

#define SYS_P2_MFP_P2_ALT3_Pos (11)

GCR_T::P2_MFP: P2_ALT3 Position

Definition at line 1673 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT4_Msk

#define SYS_P2_MFP_P2_ALT4_Msk (0x1ul << SYS_P2_MFP_P2_ALT4_Pos)

GCR_T::P2_MFP: P2_ALT4 Mask

Definition at line 1677 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT4_Pos

#define SYS_P2_MFP_P2_ALT4_Pos (12)

GCR_T::P2_MFP: P2_ALT4 Position

Definition at line 1676 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT5_Msk

#define SYS_P2_MFP_P2_ALT5_Msk (0x1ul << SYS_P2_MFP_P2_ALT5_Pos)

GCR_T::P2_MFP: P2_ALT5 Mask

Definition at line 1680 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT5_Pos

#define SYS_P2_MFP_P2_ALT5_Pos (13)

GCR_T::P2_MFP: P2_ALT5 Position

Definition at line 1679 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT6_Msk

#define SYS_P2_MFP_P2_ALT6_Msk (0x1ul << SYS_P2_MFP_P2_ALT6_Pos)

GCR_T::P2_MFP: P2_ALT6 Mask

Definition at line 1683 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT6_Pos

#define SYS_P2_MFP_P2_ALT6_Pos (14)

GCR_T::P2_MFP: P2_ALT6 Position

Definition at line 1682 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT_Msk

#define SYS_P2_MFP_P2_ALT_Msk (0xfful << SYS_P2_MFP_P2_ALT_Pos)

GCR_T::P2_MFP: P2_ALT Mask

Definition at line 1668 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT_Pos

#define SYS_P2_MFP_P2_ALT_Pos (8)

GCR_T::P2_MFP: P2_ALT Position

Definition at line 1667 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_MFP_Msk

#define SYS_P2_MFP_P2_MFP_Msk (0xfful << SYS_P2_MFP_P2_MFP_Pos)

GCR_T::P2_MFP: P2_MFP Mask

Definition at line 1665 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_MFP_Pos

#define SYS_P2_MFP_P2_MFP_Pos (0)

GCR_T::P2_MFP: P2_MFP Position

Definition at line 1664 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_TYPE_Msk

#define SYS_P2_MFP_P2_TYPE_Msk (0xfful << SYS_P2_MFP_P2_TYPE_Pos)

GCR_T::P2_MFP: P2_TYPE Mask

Definition at line 1686 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_TYPE_Pos

#define SYS_P2_MFP_P2_TYPE_Pos (16)

GCR_T::P2_MFP: P2_TYPE Position

Definition at line 1685 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P32CPP1_Msk

#define SYS_P3_MFP_P32CPP1_Msk (0x1ul << SYS_P3_MFP_P32CPP1_Pos)

GCR_T::P3_MFP: P32CPP1 Mask

Definition at line 1716 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P32CPP1_Pos

#define SYS_P3_MFP_P32CPP1_Pos (24)

GCR_T::P3_MFP: P32CPP1 Position

Definition at line 1715 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT0_Msk

#define SYS_P3_MFP_P3_ALT0_Msk (0x1ul << SYS_P3_MFP_P3_ALT0_Pos)

GCR_T::P3_MFP: P3_ALT0 Mask

Definition at line 1695 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT0_Pos

#define SYS_P3_MFP_P3_ALT0_Pos (8)

GCR_T::P3_MFP: P3_ALT0 Position

Definition at line 1694 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT1_Msk

#define SYS_P3_MFP_P3_ALT1_Msk (0x1ul << SYS_P3_MFP_P3_ALT1_Pos)

GCR_T::P3_MFP: P3_ALT1 Mask

Definition at line 1698 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT1_Pos

#define SYS_P3_MFP_P3_ALT1_Pos (9)

GCR_T::P3_MFP: P3_ALT1 Position

Definition at line 1697 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT2_Msk

#define SYS_P3_MFP_P3_ALT2_Msk (0x1ul << SYS_P3_MFP_P3_ALT2_Pos)

GCR_T::P3_MFP: P3_ALT2 Mask

Definition at line 1701 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT2_Pos

#define SYS_P3_MFP_P3_ALT2_Pos (10)

GCR_T::P3_MFP: P3_ALT2 Position

Definition at line 1700 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT4_Msk

#define SYS_P3_MFP_P3_ALT4_Msk (0x1ul << SYS_P3_MFP_P3_ALT4_Pos)

GCR_T::P3_MFP: P3_ALT4 Mask

Definition at line 1704 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT4_Pos

#define SYS_P3_MFP_P3_ALT4_Pos (12)

GCR_T::P3_MFP: P3_ALT4 Position

Definition at line 1703 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT5_Msk

#define SYS_P3_MFP_P3_ALT5_Msk (0x1ul << SYS_P3_MFP_P3_ALT5_Pos)

GCR_T::P3_MFP: P3_ALT5 Mask

Definition at line 1707 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT5_Pos

#define SYS_P3_MFP_P3_ALT5_Pos (13)

GCR_T::P3_MFP: P3_ALT5 Position

Definition at line 1706 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT6_Msk

#define SYS_P3_MFP_P3_ALT6_Msk (0x1ul << SYS_P3_MFP_P3_ALT6_Pos)

GCR_T::P3_MFP: P3_ALT6 Mask

Definition at line 1710 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT6_Pos

#define SYS_P3_MFP_P3_ALT6_Pos (14)

GCR_T::P3_MFP: P3_ALT6 Position

Definition at line 1709 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT_Msk

#define SYS_P3_MFP_P3_ALT_Msk (0xfful << SYS_P3_MFP_P3_ALT_Pos)

GCR_T::P3_MFP: P3_ALT Mask

Definition at line 1692 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT_Pos

#define SYS_P3_MFP_P3_ALT_Pos (8)

GCR_T::P3_MFP: P3_ALT Position

Definition at line 1691 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_MFP_Msk

#define SYS_P3_MFP_P3_MFP_Msk (0xfful << SYS_P3_MFP_P3_MFP_Pos)

GCR_T::P3_MFP: P3_MFP Mask

Definition at line 1689 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_MFP_Pos

#define SYS_P3_MFP_P3_MFP_Pos (0)

GCR_T::P3_MFP: P3_MFP Position

Definition at line 1688 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_TYPE_Msk

#define SYS_P3_MFP_P3_TYPE_Msk (0xfful << SYS_P3_MFP_P3_TYPE_Pos)

GCR_T::P3_MFP: P3_TYPE Mask

Definition at line 1713 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_TYPE_Pos

#define SYS_P3_MFP_P3_TYPE_Pos (16)

GCR_T::P3_MFP: P3_TYPE Position

Definition at line 1712 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT6_Msk

#define SYS_P4_MFP_P4_ALT6_Msk (0x1ul << SYS_P4_MFP_P4_ALT6_Pos)

GCR_T::P4_MFP: P4_ALT6 Mask

Definition at line 1725 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT6_Pos

#define SYS_P4_MFP_P4_ALT6_Pos (14)

GCR_T::P4_MFP: P4_ALT6 Position

Definition at line 1724 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT7_Msk

#define SYS_P4_MFP_P4_ALT7_Msk (0x1ul << SYS_P4_MFP_P4_ALT7_Pos)

GCR_T::P4_MFP: P4_ALT7 Mask

Definition at line 1728 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT7_Pos

#define SYS_P4_MFP_P4_ALT7_Pos (15)

GCR_T::P4_MFP: P4_ALT7 Position

Definition at line 1727 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT_Msk

#define SYS_P4_MFP_P4_ALT_Msk (0xfful << SYS_P4_MFP_P4_ALT_Pos)

GCR_T::P4_MFP: P4_ALT Mask

Definition at line 1722 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT_Pos

#define SYS_P4_MFP_P4_ALT_Pos (8)

GCR_T::P4_MFP: P4_ALT Position

Definition at line 1721 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_MFP_Msk

#define SYS_P4_MFP_P4_MFP_Msk (0xfful << SYS_P4_MFP_P4_MFP_Pos)

GCR_T::P4_MFP: P4_MFP Mask

Definition at line 1719 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_MFP_Pos

#define SYS_P4_MFP_P4_MFP_Pos (0)

GCR_T::P4_MFP: P4_MFP Position

Definition at line 1718 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_TYPE_Msk

#define SYS_P4_MFP_P4_TYPE_Msk (0xfful << SYS_P4_MFP_P4_TYPE_Pos)

GCR_T::P4_MFP: P4_TYPE Mask

Definition at line 1731 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_TYPE_Pos

#define SYS_P4_MFP_P4_TYPE_Pos (16)

GCR_T::P4_MFP: P4_TYPE Position

Definition at line 1730 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT0_Msk

#define SYS_P5_MFP_P5_ALT0_Msk (0x1ul << SYS_P5_MFP_P5_ALT0_Pos)

GCR_T::P5_MFP: P5_ALT0 Mask

Definition at line 1740 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT0_Pos

#define SYS_P5_MFP_P5_ALT0_Pos (8)

GCR_T::P5_MFP: P5_ALT0 Position

Definition at line 1739 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT1_Msk

#define SYS_P5_MFP_P5_ALT1_Msk (0x1ul << SYS_P5_MFP_P5_ALT1_Pos)

GCR_T::P5_MFP: P5_ALT1 Mask

Definition at line 1743 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT1_Pos

#define SYS_P5_MFP_P5_ALT1_Pos (9)

GCR_T::P5_MFP: P5_ALT1 Position

Definition at line 1742 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT2_Msk

#define SYS_P5_MFP_P5_ALT2_Msk (0x1ul << SYS_P5_MFP_P5_ALT2_Pos)

GCR_T::P5_MFP: P5_ALT2 Mask

Definition at line 1746 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT2_Pos

#define SYS_P5_MFP_P5_ALT2_Pos (10)

GCR_T::P5_MFP: P5_ALT2 Position

Definition at line 1745 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT3_Msk

#define SYS_P5_MFP_P5_ALT3_Msk (0x1ul << SYS_P5_MFP_P5_ALT3_Pos)

GCR_T::P5_MFP: P5_ALT3 Mask

Definition at line 1749 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT3_Pos

#define SYS_P5_MFP_P5_ALT3_Pos (11)

GCR_T::P5_MFP: P5_ALT3 Position

Definition at line 1748 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT4_Msk

#define SYS_P5_MFP_P5_ALT4_Msk (0x1ul << SYS_P5_MFP_P5_ALT4_Pos)

GCR_T::P5_MFP: P5_ALT4 Mask

Definition at line 1752 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT4_Pos

#define SYS_P5_MFP_P5_ALT4_Pos (12)

GCR_T::P5_MFP: P5_ALT4 Position

Definition at line 1751 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT5_Msk

#define SYS_P5_MFP_P5_ALT5_Msk (0x1ul << SYS_P5_MFP_P5_ALT5_Pos)

GCR_T::P5_MFP: P5_ALT5 Mask

Definition at line 1755 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT5_Pos

#define SYS_P5_MFP_P5_ALT5_Pos (13)

GCR_T::P5_MFP: P5_ALT5 Position

Definition at line 1754 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT_Msk

#define SYS_P5_MFP_P5_ALT_Msk (0xFFul << SYS_P5_MFP_P5_ALT_Pos)

GCR_T::P5_MFP: P5_ALT Mask

Definition at line 1737 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT_Pos

#define SYS_P5_MFP_P5_ALT_Pos (8)

GCR_T::P5_MFP: P5_ALT Position

Definition at line 1736 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_MFP_Msk

#define SYS_P5_MFP_P5_MFP_Msk (0xfful << SYS_P5_MFP_P5_MFP_Pos)

GCR_T::P5_MFP: P5_MFP Mask

Definition at line 1734 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_MFP_Pos

#define SYS_P5_MFP_P5_MFP_Pos (0)

GCR_T::P5_MFP: P5_MFP Position

Definition at line 1733 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_TYPE_Msk

#define SYS_P5_MFP_P5_TYPE_Msk (0xfful << SYS_P5_MFP_P5_TYPE_Pos)

GCR_T::P5_MFP: P5_TYPE Mask

Definition at line 1758 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_TYPE_Pos

#define SYS_P5_MFP_P5_TYPE_Pos (16)

GCR_T::P5_MFP: P5_TYPE Position

Definition at line 1757 of file Mini51Series.h.

## ◆ SYS_PDID_PDID_Msk

#define SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)

GCR_T::PDID: PDID Mask

Definition at line 1542 of file Mini51Series.h.

## ◆ SYS_PDID_PDID_Pos

#define SYS_PDID_PDID_Pos (0)

    @addtogroup GCR_CONST GCR Bit Field Definition
    Constant Definitions for GCR Controller

GCR_T::PDID: PDID Position

Definition at line 1541 of file Mini51Series.h.

## ◆ SYS_RegLockAddr_RegUnLock_Msk

#define SYS_RegLockAddr_RegUnLock_Msk (0x1ul << SYS_RegLockAddr_RegUnLock_Pos)

GCR_T::RegLockAddr: RegUnLock Mask

Definition at line 1782 of file Mini51Series.h.

## ◆ SYS_RegLockAddr_RegUnLock_Pos

#define SYS_RegLockAddr_RegUnLock_Pos 0

GCR_T::RegLockAddr: RegUnLock Position

Definition at line 1781 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_BOD_Msk

#define SYS_RSTSRC_RSTS_BOD_Msk (0x1ul << SYS_RSTSRC_RSTS_BOD_Pos)

GCR_T::RSTSRC: RSTS_BOD Mask

Definition at line 1554 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_BOD_Pos

#define SYS_RSTSRC_RSTS_BOD_Pos (4)

GCR_T::RSTSRC: RSTS_BOD Position

Definition at line 1553 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_CPU_Msk

#define SYS_RSTSRC_RSTS_CPU_Msk (0x1ul << SYS_RSTSRC_RSTS_CPU_Pos)

GCR_T::RSTSRC: RSTS_CPU Mask

Definition at line 1560 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_CPU_Pos

#define SYS_RSTSRC_RSTS_CPU_Pos (7)

GCR_T::RSTSRC: RSTS_CPU Position

Definition at line 1559 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_MCU_Msk

#define SYS_RSTSRC_RSTS_MCU_Msk (0x1ul << SYS_RSTSRC_RSTS_MCU_Pos)

GCR_T::RSTSRC: RSTS_MCU Mask

Definition at line 1557 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_MCU_Pos

#define SYS_RSTSRC_RSTS_MCU_Pos (5)

GCR_T::RSTSRC: RSTS_MCU Position

Definition at line 1556 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_POR_Msk

#define SYS_RSTSRC_RSTS_POR_Msk (0x1ul << SYS_RSTSRC_RSTS_POR_Pos)

GCR_T::RSTSRC: RSTS_POR Mask

Definition at line 1545 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_POR_Pos

#define SYS_RSTSRC_RSTS_POR_Pos (0)

GCR_T::RSTSRC: RSTS_POR Position

Definition at line 1544 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_RESET_Msk

#define SYS_RSTSRC_RSTS_RESET_Msk (0x1ul << SYS_RSTSRC_RSTS_RESET_Pos)

GCR_T::RSTSRC: RSTS_RESET Mask

Definition at line 1548 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_RESET_Pos

#define SYS_RSTSRC_RSTS_RESET_Pos (1)

GCR_T::RSTSRC: RSTS_RESET Position

Definition at line 1547 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_WDT_Msk

#define SYS_RSTSRC_RSTS_WDT_Msk (0x1ul << SYS_RSTSRC_RSTS_WDT_Pos)

GCR_T::RSTSRC: RSTS_WDT Mask

Definition at line 1551 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_WDT_Pos

#define SYS_RSTSRC_RSTS_WDT_Pos (2)

GCR_T::RSTSRC: RSTS_WDT Position

Definition at line 1550 of file Mini51Series.h.

## ◆ TIMER_TCAP_TCAP_Msk

#define TIMER_TCAP_TCAP_Msk (0xfffffful << TIMER_TCAP_TCAP_Pos)

TIMER_T::TCAP: TCAP Mask

Definition at line 4890 of file Mini51Series.h.

## ◆ TIMER_TCAP_TCAP_Pos

#define TIMER_TCAP_TCAP_Pos (0)

TIMER_T::TCAP: TCAP Position

Definition at line 4889 of file Mini51Series.h.

## ◆ TIMER_TCMP_TCMP_Msk

#define TIMER_TCMP_TCMP_Msk (0xfffffful << TIMER_TCMP_TCMP_Pos)

TIMER_T::TCMPR: TCMP Mask

Definition at line 4878 of file Mini51Series.h.

## ◆ TIMER_TCMP_TCMP_Pos

#define TIMER_TCMP_TCMP_Pos (0)

TIMER_T::TCMPR: TCMP Position

Definition at line 4877 of file Mini51Series.h.

## ◆ TIMER_TCSR_CACT_Msk

#define TIMER_TCSR_CACT_Msk (0x1ul << TIMER_TCSR_CACT_Pos)

TIMER_T::TCSR: CACT Mask

Definition at line 4860 of file Mini51Series.h.

## ◆ TIMER_TCSR_CACT_Pos

#define TIMER_TCSR_CACT_Pos (25)

TIMER_T::TCSR: CACT Position

Definition at line 4859 of file Mini51Series.h.

## ◆ TIMER_TCSR_CAP_SRC_Msk

#define TIMER_TCSR_CAP_SRC_Msk (0x1ul << TIMER_TCSR_CAP_SRC_Pos)

TIMER_T::TCSR: CAP_SRC Mask

Definition at line 4851 of file Mini51Series.h.

## ◆ TIMER_TCSR_CAP_SRC_Pos

#define TIMER_TCSR_CAP_SRC_Pos (19)

TIMER_T::TCSR: CAP_SRC Position

Definition at line 4850 of file Mini51Series.h.

## ◆ TIMER_TCSR_CEN_Msk

#define TIMER_TCSR_CEN_Msk (0x1ul << TIMER_TCSR_CEN_Pos)

TIMER_T::TCSR: CEN Mask

Definition at line 4872 of file Mini51Series.h.

## ◆ TIMER_TCSR_CEN_Pos

#define TIMER_TCSR_CEN_Pos (30)

TIMER_T::TCSR: CEN Position

Definition at line 4871 of file Mini51Series.h.

## ◆ TIMER_TCSR_CRST_Msk

#define TIMER_TCSR_CRST_Msk (0x1ul << TIMER_TCSR_CRST_Pos)

TIMER_T::TCSR: CRST Mask

Definition at line 4863 of file Mini51Series.h.

## ◆ TIMER_TCSR_CRST_Pos

#define TIMER_TCSR_CRST_Pos (26)

TIMER_T::TCSR: CRST Position

Definition at line 4862 of file Mini51Series.h.

## ◆ TIMER_TCSR_CTB_Msk

#define TIMER_TCSR_CTB_Msk (0x1ul << TIMER_TCSR_CTB_Pos)

TIMER_T::TCSR: CTB Mask

Definition at line 4857 of file Mini51Series.h.

## ◆ TIMER_TCSR_CTB_Pos

#define TIMER_TCSR_CTB_Pos (24)

TIMER_T::TCSR: CTB Position

Definition at line 4856 of file Mini51Series.h.

## ◆ TIMER_TCSR_DBGACK_TMR_Msk

#define TIMER_TCSR_DBGACK_TMR_Msk (0x1ul << TIMER_TCSR_DBGACK_TMR_Pos)

TIMER_T::TCSR: DBGACK_TMR Mask

Definition at line 4875 of file Mini51Series.h.

## ◆ TIMER_TCSR_DBGACK_TMR_Pos

#define TIMER_TCSR_DBGACK_TMR_Pos (31)

TIMER_T::TCSR: DBGACK_TMR Position

Definition at line 4874 of file Mini51Series.h.

## ◆ TIMER_TCSR_IE_Msk

#define TIMER_TCSR_IE_Msk (0x1ul << TIMER_TCSR_IE_Pos)

TIMER_T::TCSR: IE Mask

Definition at line 4869 of file Mini51Series.h.

## ◆ TIMER_TCSR_IE_Pos

#define TIMER_TCSR_IE_Pos (29)

TIMER_T::TCSR: IE Position

Definition at line 4868 of file Mini51Series.h.

## ◆ TIMER_TCSR_MODE_Msk

#define TIMER_TCSR_MODE_Msk (0x3ul << TIMER_TCSR_MODE_Pos)

TIMER_T::TCSR: MODE Mask

Definition at line 4866 of file Mini51Series.h.

## ◆ TIMER_TCSR_MODE_Pos

#define TIMER_TCSR_MODE_Pos (27)

TIMER_T::TCSR: MODE Position

Definition at line 4865 of file Mini51Series.h.

## ◆ TIMER_TCSR_PERIODIC_SEL_Msk

#define TIMER_TCSR_PERIODIC_SEL_Msk (0x1ul << TIMER_TCSR_PERIODIC_SEL_Pos)

TIMER_T::TCSR: PERIODIC_SEL Mask

Definition at line 4842 of file Mini51Series.h.

## ◆ TIMER_TCSR_PERIODIC_SEL_Pos

#define TIMER_TCSR_PERIODIC_SEL_Pos (17)

TIMER_T::TCSR: PERIODIC_SEL Position

Definition at line 4841 of file Mini51Series.h.

## ◆ TIMER_TCSR_PRESCALE_Msk

#define TIMER_TCSR_PRESCALE_Msk (0xfful << TIMER_TCSR_PRESCALE_Pos)

TIMER_T::TCSR: PRESCALE Mask

Definition at line 4836 of file Mini51Series.h.

## ◆ TIMER_TCSR_PRESCALE_Pos

#define TIMER_TCSR_PRESCALE_Pos (0)

    @addtogroup TMR_CONST TMR Bit Field Definition
    Constant Definitions for TMR Controller

TIMER_T::TCSR: PRESCALE Position

Definition at line 4835 of file Mini51Series.h.

## ◆ TIMER_TCSR_TDR_EN_Msk

#define TIMER_TCSR_TDR_EN_Msk (0x1ul << TIMER_TCSR_TDR_EN_Pos)

TIMER_T::TCSR: TDR_EN Mask

Definition at line 4839 of file Mini51Series.h.

## ◆ TIMER_TCSR_TDR_EN_Pos

#define TIMER_TCSR_TDR_EN_Pos (16)

TIMER_T::TCSR: TDR_EN Position

Definition at line 4838 of file Mini51Series.h.

## ◆ TIMER_TCSR_TOGGLE_PIN_Msk

#define TIMER_TCSR_TOGGLE_PIN_Msk (0x1ul << TIMER_TCSR_TOGGLE_PIN_Pos)

TIMER TCSR: TOGGLE_PIN Mask

Definition at line 4845 of file Mini51Series.h.

## ◆ TIMER_TCSR_TOGGLE_PIN_Pos

#define TIMER_TCSR_TOGGLE_PIN_Pos (18)

TIMER TCSR: TOGGLE_PIN Position

Definition at line 4844 of file Mini51Series.h.

## ◆ TIMER_TCSR_TOUT_PIN_Msk

#define TIMER_TCSR_TOUT_PIN_Msk (0x1ul << TIMER_TCSR_TOUT_PIN_Pos)

TIMER_T::TCSR: TOUT_PIN Mask

Definition at line 4848 of file Mini51Series.h.

## ◆ TIMER_TCSR_TOUT_PIN_Pos

#define TIMER_TCSR_TOUT_PIN_Pos (18)

TIMER_T::TCSR: TOUT_PIN Position

Definition at line 4847 of file Mini51Series.h.

## ◆ TIMER_TCSR_WAKE_EN_Msk

#define TIMER_TCSR_WAKE_EN_Msk (0x1ul << TIMER_TCSR_WAKE_EN_Pos)

TIMER_T::TCSR: WAKE_EN Mask

Definition at line 4854 of file Mini51Series.h.

## ◆ TIMER_TCSR_WAKE_EN_Pos

#define TIMER_TCSR_WAKE_EN_Pos (23)

TIMER_T::TCSR: WAKE_EN Position

Definition at line 4853 of file Mini51Series.h.

## ◆ TIMER_TDR_TDR_Msk

#define TIMER_TDR_TDR_Msk (0xfffffful << TIMER_TDR_TDR_Pos)

TIMER_T::TDR: TDR Mask

Definition at line 4887 of file Mini51Series.h.

## ◆ TIMER_TDR_TDR_Pos

#define TIMER_TDR_TDR_Pos (0)

TIMER_T::TDR: TDR Position

Definition at line 4886 of file Mini51Series.h.

## ◆ TIMER_TEXCON_CAP_MODE_Msk

#define TIMER_TEXCON_CAP_MODE_Msk (0x1ul << TIMER_TEXCON_CAP_MODE_Pos)

TIMER_T::TEXCON: CAP_MODE Mask

Definition at line 4914 of file Mini51Series.h.

## ◆ TIMER_TEXCON_CAP_MODE_Pos

#define TIMER_TEXCON_CAP_MODE_Pos (8)

TIMER_T::TEXCON: CAP_MODE Position

Definition at line 4913 of file Mini51Series.h.

## ◆ TIMER_TEXCON_RSTCAPSEL_Msk

#define TIMER_TEXCON_RSTCAPSEL_Msk (0x1ul << TIMER_TEXCON_RSTCAPSEL_Pos)

TIMER_T::TEXCON: RSTCAPSEL Mask

Definition at line 4902 of file Mini51Series.h.

## ◆ TIMER_TEXCON_RSTCAPSEL_Pos

#define TIMER_TEXCON_RSTCAPSEL_Pos (4)

TIMER_T::TEXCON: RSTCAPSEL Position

Definition at line 4901 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TCDB_Msk

#define TIMER_TEXCON_TCDB_Msk (0x1ul << TIMER_TEXCON_TCDB_Pos)

TIMER_T::TEXCON: TCDB Mask

Definition at line 4911 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TCDB_Pos

#define TIMER_TEXCON_TCDB_Pos (7)

TIMER_T::TEXCON: TCDB Position

Definition at line 4910 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEX_EDGE_Msk

#define TIMER_TEXCON_TEX_EDGE_Msk (0x3ul << TIMER_TEXCON_TEX_EDGE_Pos)

TIMER_T::TEXCON: TEX_EDGE Mask

Definition at line 4896 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEX_EDGE_Pos

#define TIMER_TEXCON_TEX_EDGE_Pos (1)

TIMER_T::TEXCON: TEX_EDGE Position

Definition at line 4895 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXDB_Msk

#define TIMER_TEXCON_TEXDB_Msk (0x1ul << TIMER_TEXCON_TEXDB_Pos)

TIMER_T::TEXCON: TEXDB Mask

Definition at line 4908 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXDB_Pos

#define TIMER_TEXCON_TEXDB_Pos (6)

TIMER_T::TEXCON: TEXDB Position

Definition at line 4907 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXEN_Msk

#define TIMER_TEXCON_TEXEN_Msk (0x1ul << TIMER_TEXCON_TEXEN_Pos)

TIMER_T::TEXCON: TEXEN Mask

Definition at line 4899 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXEN_Pos

#define TIMER_TEXCON_TEXEN_Pos (3)

TIMER_T::TEXCON: TEXEN Position

Definition at line 4898 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXIEN_Msk

#define TIMER_TEXCON_TEXIEN_Msk (0x1ul << TIMER_TEXCON_TEXIEN_Pos)

TIMER_T::TEXCON: TEXIEN Mask

Definition at line 4905 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXIEN_Pos

#define TIMER_TEXCON_TEXIEN_Pos (5)

TIMER_T::TEXCON: TEXIEN Position

Definition at line 4904 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TX_PHASE_Msk

#define TIMER_TEXCON_TX_PHASE_Msk (0x1ul << TIMER_TEXCON_TX_PHASE_Pos)

TIMER_T::TEXCON: TX_PHASE Mask

Definition at line 4893 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TX_PHASE_Pos

#define TIMER_TEXCON_TX_PHASE_Pos (0)

TIMER_T::TEXCON: TX_PHASE Position

Definition at line 4892 of file Mini51Series.h.

## ◆ TIMER_TEXISR_TEXIF_Msk

#define TIMER_TEXISR_TEXIF_Msk (0x1ul << TIMER_TEXISR_TEXIF_Pos)

TIMER_T::TEXISR: TEXIF Mask

Definition at line 4917 of file Mini51Series.h.

## ◆ TIMER_TEXISR_TEXIF_Pos

#define TIMER_TEXISR_TEXIF_Pos (0)

TIMER_T::TEXISR: TEXIF Position

Definition at line 4916 of file Mini51Series.h.

## ◆ TIMER_TISR_TIF_Msk

#define TIMER_TISR_TIF_Msk (0x1ul << TIMER_TISR_TIF_Pos)

TIMER_T::TISR: TIF Mask

Definition at line 4881 of file Mini51Series.h.

## ◆ TIMER_TISR_TIF_Pos

#define TIMER_TISR_TIF_Pos (0)

TIMER_T::TISR: TIF Position

Definition at line 4880 of file Mini51Series.h.

## ◆ TIMER_TISR_TWF_Msk

#define TIMER_TISR_TWF_Msk (0x1ul << TIMER_TISR_TWF_Pos)

TIMER_T::TISR: TWF Mask

Definition at line 4884 of file Mini51Series.h.

## ◆ TIMER_TISR_TWF_Pos

#define TIMER_TISR_TWF_Pos (1)

TIMER_T::TISR: TWF Position

Definition at line 4883 of file Mini51Series.h.

## ◆ UART_ALT_CSR_ADDR_MATCH_Msk

#define UART_ALT_CSR_ADDR_MATCH_Msk (0xfful << UART_ALT_CSR_ADDR_MATCH_Pos)

UART_T::ALT_CSR: ADDR_MATCH Mask

Definition at line 5548 of file Mini51Series.h.

## ◆ UART_ALT_CSR_ADDR_MATCH_Pos

#define UART_ALT_CSR_ADDR_MATCH_Pos (24)

UART_T::ALT_CSR: ADDR_MATCH Position

Definition at line 5547 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_AAD_Msk

#define UART_ALT_CSR_RS485_AAD_Msk (0x1ul << UART_ALT_CSR_RS485_AAD_Pos)

UART_T::ALT_CSR: RS485_AAD Mask

Definition at line 5539 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_AAD_Pos

#define UART_ALT_CSR_RS485_AAD_Pos (9)

UART_T::ALT_CSR: RS485_AAD Position

Definition at line 5538 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_ADD_EN_Msk

#define UART_ALT_CSR_RS485_ADD_EN_Msk (0x1ul << UART_ALT_CSR_RS485_ADD_EN_Pos)

UART_T::ALT_CSR: RS485_ADD_EN Mask

Definition at line 5545 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_ADD_EN_Pos

#define UART_ALT_CSR_RS485_ADD_EN_Pos (15)

UART_T::ALT_CSR: RS485_ADD_EN Position

Definition at line 5544 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_AUD_Msk

#define UART_ALT_CSR_RS485_AUD_Msk (0x1ul << UART_ALT_CSR_RS485_AUD_Pos)

UART_T::ALT_CSR: RS485_AUD Mask

Definition at line 5542 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_AUD_Pos

#define UART_ALT_CSR_RS485_AUD_Pos (10)

UART_T::ALT_CSR: RS485_AUD Position

Definition at line 5541 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_NMM_Msk

#define UART_ALT_CSR_RS485_NMM_Msk (0x1ul << UART_ALT_CSR_RS485_NMM_Pos)

UART_T::ALT_CSR: RS485_NMM Mask

Definition at line 5536 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_NMM_Pos

#define UART_ALT_CSR_RS485_NMM_Pos (8)

UART_T::ALT_CSR: RS485_NMM Position

Definition at line 5535 of file Mini51Series.h.

## ◆ UART_BAUD_BRD_Msk

#define UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)

UART_T::BAUD: BRD Mask

Definition at line 5515 of file Mini51Series.h.

## ◆ UART_BAUD_BRD_Pos

#define UART_BAUD_BRD_Pos (0)

UART_T::BAUD: BRD Position

Definition at line 5514 of file Mini51Series.h.

## ◆ UART_BAUD_DIV_X_EN_Msk

#define UART_BAUD_DIV_X_EN_Msk (0x1ul << UART_BAUD_DIV_X_EN_Pos)

UART_T::BAUD: DIV_X_EN Mask

Definition at line 5524 of file Mini51Series.h.

## ◆ UART_BAUD_DIV_X_EN_Pos

#define UART_BAUD_DIV_X_EN_Pos (29)

UART_T::BAUD: DIV_X_EN Position

Definition at line 5523 of file Mini51Series.h.

## ◆ UART_BAUD_DIV_X_ONE_Msk

#define UART_BAUD_DIV_X_ONE_Msk (0x1ul << UART_BAUD_DIV_X_ONE_Pos)

UART_T::BAUD: DIV_X_ONE Mask

Definition at line 5521 of file Mini51Series.h.

## ◆ UART_BAUD_DIV_X_ONE_Pos

#define UART_BAUD_DIV_X_ONE_Pos (28)

UART_T::BAUD: DIV_X_ONE Position

Definition at line 5520 of file Mini51Series.h.

## ◆ UART_BAUD_DIVIDER_X_Msk

#define UART_BAUD_DIVIDER_X_Msk (0xful << UART_BAUD_DIVIDER_X_Pos)

UART_T::BAUD: DIVIDER_X Mask

Definition at line 5518 of file Mini51Series.h.

## ◆ UART_BAUD_DIVIDER_X_Pos

#define UART_BAUD_DIVIDER_X_Pos (24)

UART_T::BAUD: DIVIDER_X Position

Definition at line 5517 of file Mini51Series.h.

## ◆ UART_FCR_RFITL_Msk

#define UART_FCR_RFITL_Msk (0xful << UART_FCR_RFITL_Pos)

UART_T::FCR: RFITL Mask

Definition at line 5389 of file Mini51Series.h.

## ◆ UART_FCR_RFITL_Pos

#define UART_FCR_RFITL_Pos (4)

UART_T::FCR: RFITL Position

Definition at line 5388 of file Mini51Series.h.

## ◆ UART_FCR_RFR_Msk

#define UART_FCR_RFR_Msk (0x1ul << UART_FCR_RFR_Pos)

UART_T::FCR: RFR Mask

Definition at line 5383 of file Mini51Series.h.

## ◆ UART_FCR_RFR_Pos

#define UART_FCR_RFR_Pos (1)

UART_T::FCR: RFR Position

Definition at line 5382 of file Mini51Series.h.

## ◆ UART_FCR_RTS_TRI_LEV_Msk

#define UART_FCR_RTS_TRI_LEV_Msk (0xful << UART_FCR_RTS_TRI_LEV_Pos)

UART_T::FCR: RTS_TRI_LEV Mask

Definition at line 5395 of file Mini51Series.h.

## ◆ UART_FCR_RTS_TRI_LEV_Pos

#define UART_FCR_RTS_TRI_LEV_Pos (16)

UART_T::FCR: RTS_TRI_LEV Position

Definition at line 5394 of file Mini51Series.h.

## ◆ UART_FCR_RX_DIS_Msk

#define UART_FCR_RX_DIS_Msk (0x1ul << UART_FCR_RX_DIS_Pos)

UART_T::FCR: RX_DIS Mask

Definition at line 5392 of file Mini51Series.h.

## ◆ UART_FCR_RX_DIS_Pos

#define UART_FCR_RX_DIS_Pos (8)

UART_T::FCR: RX_DIS Position

Definition at line 5391 of file Mini51Series.h.

## ◆ UART_FCR_TFR_Msk

#define UART_FCR_TFR_Msk (0x1ul << UART_FCR_TFR_Pos)

UART_T::FCR: TFR Mask

Definition at line 5386 of file Mini51Series.h.

## ◆ UART_FCR_TFR_Pos

#define UART_FCR_TFR_Pos (2)

UART_T::FCR: TFR Position

Definition at line 5385 of file Mini51Series.h.

## ◆ UART_FSR_BIF_Msk

#define UART_FSR_BIF_Msk (0x1ul << UART_FSR_BIF_Pos)

UART_T::FSR: BIF Mask

Definition at line 5446 of file Mini51Series.h.

## ◆ UART_FSR_BIF_Pos

#define UART_FSR_BIF_Pos (6)

UART_T::FSR: BIF Position

Definition at line 5445 of file Mini51Series.h.

## ◆ UART_FSR_FEF_Msk

#define UART_FSR_FEF_Msk (0x1ul << UART_FSR_FEF_Pos)

UART_T::FSR: FEF Mask

Definition at line 5443 of file Mini51Series.h.

## ◆ UART_FSR_FEF_Pos

#define UART_FSR_FEF_Pos (5)

UART_T::FSR: FEF Position

Definition at line 5442 of file Mini51Series.h.

## ◆ UART_FSR_PEF_Msk

#define UART_FSR_PEF_Msk (0x1ul << UART_FSR_PEF_Pos)

UART_T::FSR: PEF Mask

Definition at line 5440 of file Mini51Series.h.

## ◆ UART_FSR_PEF_Pos

#define UART_FSR_PEF_Pos (4)

UART_T::FSR: PEF Position

Definition at line 5439 of file Mini51Series.h.

## ◆ UART_FSR_RS485_ADD_DETF_Msk

#define UART_FSR_RS485_ADD_DETF_Msk (0x1ul << UART_FSR_RS485_ADD_DETF_Pos)

UART_T::FSR: RS485_ADD_DETF Mask

Definition at line 5437 of file Mini51Series.h.

## ◆ UART_FSR_RS485_ADD_DETF_Pos

#define UART_FSR_RS485_ADD_DETF_Pos (3)

UART_T::FSR: RS485_ADD_DETF Position

Definition at line 5436 of file Mini51Series.h.

## ◆ UART_FSR_RX_EMPTY_Msk

#define UART_FSR_RX_EMPTY_Msk (0x1ul << UART_FSR_RX_EMPTY_Pos)

UART_T::FSR: RX_EMPTY Mask

Definition at line 5452 of file Mini51Series.h.

## ◆ UART_FSR_RX_EMPTY_Pos

#define UART_FSR_RX_EMPTY_Pos (14)

UART_T::FSR: RX_EMPTY Position

Definition at line 5451 of file Mini51Series.h.

## ◆ UART_FSR_RX_FULL_Msk

#define UART_FSR_RX_FULL_Msk (0x1ul << UART_FSR_RX_FULL_Pos)

UART_T::FSR: RX_FULL Mask

Definition at line 5455 of file Mini51Series.h.

## ◆ UART_FSR_RX_FULL_Pos

#define UART_FSR_RX_FULL_Pos (15)

UART_T::FSR: RX_FULL Position

Definition at line 5454 of file Mini51Series.h.

## ◆ UART_FSR_RX_OVER_IF_Msk

#define UART_FSR_RX_OVER_IF_Msk (0x1ul << UART_FSR_RX_OVER_IF_Pos)

UART_T::FSR: RX_OVER_IF Mask

Definition at line 5434 of file Mini51Series.h.

## ◆ UART_FSR_RX_OVER_IF_Pos

#define UART_FSR_RX_OVER_IF_Pos (0)

UART_T::FSR: RX_OVER_IF Position

Definition at line 5433 of file Mini51Series.h.

## ◆ UART_FSR_RX_POINTER_Msk

#define UART_FSR_RX_POINTER_Msk (0x3ful << UART_FSR_RX_POINTER_Pos)

UART_T::FSR: RX_POINTER Mask

Definition at line 5449 of file Mini51Series.h.

## ◆ UART_FSR_RX_POINTER_Pos

#define UART_FSR_RX_POINTER_Pos (8)

UART_T::FSR: RX_POINTER Position

Definition at line 5448 of file Mini51Series.h.

## ◆ UART_FSR_TE_FLAG_Msk

#define UART_FSR_TE_FLAG_Msk (0x1ul << UART_FSR_TE_FLAG_Pos)

UART_T::FSR: TE_FLAG Mask

Definition at line 5470 of file Mini51Series.h.

## ◆ UART_FSR_TE_FLAG_Pos

#define UART_FSR_TE_FLAG_Pos (28)

UART_T::FSR: TE_FLAG Position

Definition at line 5469 of file Mini51Series.h.

## ◆ UART_FSR_TX_EMPTY_Msk

#define UART_FSR_TX_EMPTY_Msk (0x1ul << UART_FSR_TX_EMPTY_Pos)

UART_T::FSR: TX_EMPTY Mask

Definition at line 5461 of file Mini51Series.h.

## ◆ UART_FSR_TX_EMPTY_Pos

#define UART_FSR_TX_EMPTY_Pos (22)

UART_T::FSR: TX_EMPTY Position

Definition at line 5460 of file Mini51Series.h.

## ◆ UART_FSR_TX_FULL_Msk

#define UART_FSR_TX_FULL_Msk (0x1ul << UART_FSR_TX_FULL_Pos)

UART_T::FSR: TX_FULL Mask

Definition at line 5464 of file Mini51Series.h.

## ◆ UART_FSR_TX_FULL_Pos

#define UART_FSR_TX_FULL_Pos (23)

UART_T::FSR: TX_FULL Position

Definition at line 5463 of file Mini51Series.h.

## ◆ UART_FSR_TX_OVER_IF_Msk

#define UART_FSR_TX_OVER_IF_Msk (0x1ul << UART_FSR_TX_OVER_IF_Pos)

UART_T::FSR: TX_OVER_IF Mask

Definition at line 5467 of file Mini51Series.h.

## ◆ UART_FSR_TX_OVER_IF_Pos

#define UART_FSR_TX_OVER_IF_Pos (24)

UART_T::FSR: TX_OVER_IF Position

Definition at line 5466 of file Mini51Series.h.

## ◆ UART_FSR_TX_POINTER_Msk

#define UART_FSR_TX_POINTER_Msk (0x3ful << UART_FSR_TX_POINTER_Pos)

UART_T::FSR: TX_POINTER Mask

Definition at line 5458 of file Mini51Series.h.

## ◆ UART_FSR_TX_POINTER_Pos

#define UART_FSR_TX_POINTER_Pos (16)

UART_T::FSR: TX_POINTER Position

Definition at line 5457 of file Mini51Series.h.

## ◆ UART_FUN_SEL_FUN_SEL_Msk

#define UART_FUN_SEL_FUN_SEL_Msk (0x3ul << UART_FUN_SEL_FUN_SEL_Pos)

UART_T::FUN_SEL: FUN_SEL Mask

Definition at line 5551 of file Mini51Series.h.

## ◆ UART_FUN_SEL_FUN_SEL_Pos

#define UART_FUN_SEL_FUN_SEL_Pos (0)

UART_T::FUN_SEL: FUN_SEL Position

Definition at line 5550 of file Mini51Series.h.

## ◆ UART_IER_AUTO_CTS_EN_Msk

#define UART_IER_AUTO_CTS_EN_Msk (0x1ul << UART_IER_AUTO_CTS_EN_Pos)

UART_T::IER: AUTO_CTS_EN Mask

Definition at line 5380 of file Mini51Series.h.

## ◆ UART_IER_AUTO_CTS_EN_Pos

#define UART_IER_AUTO_CTS_EN_Pos (13)

UART_T::IER: AUTO_CTS_EN Position

Definition at line 5379 of file Mini51Series.h.

## ◆ UART_IER_AUTO_RTS_EN_Msk

#define UART_IER_AUTO_RTS_EN_Msk (0x1ul << UART_IER_AUTO_RTS_EN_Pos)

UART_T::IER: AUTO_RTS_EN Mask

Definition at line 5377 of file Mini51Series.h.

## ◆ UART_IER_AUTO_RTS_EN_Pos

#define UART_IER_AUTO_RTS_EN_Pos (12)

UART_T::IER: AUTO_RTS_EN Position

Definition at line 5376 of file Mini51Series.h.

## ◆ UART_IER_BUF_ERR_IEN_Msk

#define UART_IER_BUF_ERR_IEN_Msk (0x1ul << UART_IER_BUF_ERR_IEN_Pos)

UART_T::IER: BUF_ERR_IEN Mask

Definition at line 5368 of file Mini51Series.h.

## ◆ UART_IER_BUF_ERR_IEN_Pos

#define UART_IER_BUF_ERR_IEN_Pos (5)

UART_T::IER: BUF_ERR_IEN Position

Definition at line 5367 of file Mini51Series.h.

## ◆ UART_IER_MODEM_IEN_Msk

#define UART_IER_MODEM_IEN_Msk (0x1ul << UART_IER_MODEM_IEN_Pos)

UART_T::IER: MODEM_IEN Mask

Definition at line 5362 of file Mini51Series.h.

## ◆ UART_IER_MODEM_IEN_Pos

#define UART_IER_MODEM_IEN_Pos (3)

UART_T::IER: MODEM_IEN Position

Definition at line 5361 of file Mini51Series.h.

## ◆ UART_IER_RDA_IEN_Msk

#define UART_IER_RDA_IEN_Msk (0x1ul << UART_IER_RDA_IEN_Pos)

UART_T::IER: RDA_IEN Mask

Definition at line 5353 of file Mini51Series.h.

## ◆ UART_IER_RDA_IEN_Pos

#define UART_IER_RDA_IEN_Pos (0)

UART_T::IER: RDA_IEN Position

Definition at line 5352 of file Mini51Series.h.

## ◆ UART_IER_RLS_IEN_Msk

#define UART_IER_RLS_IEN_Msk (0x1ul << UART_IER_RLS_IEN_Pos)

UART_T::IER: RLS_IEN Mask

Definition at line 5359 of file Mini51Series.h.

## ◆ UART_IER_RLS_IEN_Pos

#define UART_IER_RLS_IEN_Pos (2)

UART_T::IER: RLS_IEN Position

Definition at line 5358 of file Mini51Series.h.

## ◆ UART_IER_RTO_IEN_Msk

#define UART_IER_RTO_IEN_Msk (0x1ul << UART_IER_RTO_IEN_Pos)

UART_T::IER: RTO_IEN Mask

Definition at line 5365 of file Mini51Series.h.

## ◆ UART_IER_RTO_IEN_Pos

#define UART_IER_RTO_IEN_Pos (4)

UART_T::IER: RTO_IEN Position

Definition at line 5364 of file Mini51Series.h.

## ◆ UART_IER_THRE_IEN_Msk

#define UART_IER_THRE_IEN_Msk (0x1ul << UART_IER_THRE_IEN_Pos)

UART_T::IER: THRE_IEN Mask

Definition at line 5356 of file Mini51Series.h.

## ◆ UART_IER_THRE_IEN_Pos

#define UART_IER_THRE_IEN_Pos (1)

UART_T::IER: THRE_IEN Position

Definition at line 5355 of file Mini51Series.h.

## ◆ UART_IER_TIME_OUT_EN_Msk

#define UART_IER_TIME_OUT_EN_Msk (0x1ul << UART_IER_TIME_OUT_EN_Pos)

UART_T::IER: TIME_OUT_EN Mask

Definition at line 5374 of file Mini51Series.h.

## ◆ UART_IER_TIME_OUT_EN_Pos

#define UART_IER_TIME_OUT_EN_Pos (11)

UART_T::IER: TIME_OUT_EN Position

Definition at line 5373 of file Mini51Series.h.

## ◆ UART_IER_WAKE_EN_Msk

#define UART_IER_WAKE_EN_Msk (0x1ul << UART_IER_WAKE_EN_Pos)

UART_T::IER: WAKE_EN Mask

Definition at line 5371 of file Mini51Series.h.

## ◆ UART_IER_WAKE_EN_Pos

#define UART_IER_WAKE_EN_Pos (6)

UART_T::IER: WAKE_EN Position

Definition at line 5370 of file Mini51Series.h.

## ◆ UART_IRCR_INV_RX_Msk

#define UART_IRCR_INV_RX_Msk (0x1ul << UART_IRCR_INV_RX_Pos)

UART_T::IRCR: INV_RX Mask

Definition at line 5533 of file Mini51Series.h.

## ◆ UART_IRCR_INV_RX_Pos

#define UART_IRCR_INV_RX_Pos (6)

UART_T::IRCR: INV_RX Position

Definition at line 5532 of file Mini51Series.h.

## ◆ UART_IRCR_INV_TX_Msk

#define UART_IRCR_INV_TX_Msk (0x1ul << UART_IRCR_INV_TX_Pos)

UART_T::IRCR: INV_TX Mask

Definition at line 5530 of file Mini51Series.h.

## ◆ UART_IRCR_INV_TX_Pos

#define UART_IRCR_INV_TX_Pos (5)

UART_T::IRCR: INV_TX Position

Definition at line 5529 of file Mini51Series.h.

## ◆ UART_IRCR_TX_SELECT_Msk

#define UART_IRCR_TX_SELECT_Msk (0x1ul << UART_IRCR_TX_SELECT_Pos)

UART_T::IRCR: TX_SELECT Mask

Definition at line 5527 of file Mini51Series.h.

## ◆ UART_IRCR_TX_SELECT_Pos

#define UART_IRCR_TX_SELECT_Pos (1)

UART_T::IRCR: TX_SELECT Position

Definition at line 5526 of file Mini51Series.h.

## ◆ UART_ISR_BUF_ERR_IF_Msk

#define UART_ISR_BUF_ERR_IF_Msk (0x1ul << UART_ISR_BUF_ERR_IF_Pos)

UART_T::ISR: BUF_ERR_IF Mask

Definition at line 5488 of file Mini51Series.h.

## ◆ UART_ISR_BUF_ERR_IF_Pos

#define UART_ISR_BUF_ERR_IF_Pos (5)

UART_T::ISR: BUF_ERR_IF Position

Definition at line 5487 of file Mini51Series.h.

## ◆ UART_ISR_BUF_ERR_INT_Msk

#define UART_ISR_BUF_ERR_INT_Msk (0x1ul << UART_ISR_BUF_ERR_INT_Pos)

UART_T::ISR: BUF_ERR_INT Mask

Definition at line 5506 of file Mini51Series.h.

## ◆ UART_ISR_BUF_ERR_INT_Pos

#define UART_ISR_BUF_ERR_INT_Pos (13)

UART_T::ISR: BUF_ERR_INT Position

Definition at line 5505 of file Mini51Series.h.

## ◆ UART_ISR_MODEM_IF_Msk

#define UART_ISR_MODEM_IF_Msk (0x1ul << UART_ISR_MODEM_IF_Pos)

UART_T::ISR: MODEM_IF Mask

Definition at line 5482 of file Mini51Series.h.

## ◆ UART_ISR_MODEM_IF_Pos

#define UART_ISR_MODEM_IF_Pos (3)

UART_T::ISR: MODEM_IF Position

Definition at line 5481 of file Mini51Series.h.

## ◆ UART_ISR_MODEM_INT_Msk

#define UART_ISR_MODEM_INT_Msk (0x1ul << UART_ISR_MODEM_INT_Pos)

UART_T::ISR: MODEM_INT Mask

Definition at line 5500 of file Mini51Series.h.

## ◆ UART_ISR_MODEM_INT_Pos

#define UART_ISR_MODEM_INT_Pos (11)

UART_T::ISR: MODEM_INT Position

Definition at line 5499 of file Mini51Series.h.

## ◆ UART_ISR_RDA_IF_Msk

#define UART_ISR_RDA_IF_Msk (0x1ul << UART_ISR_RDA_IF_Pos)

UART_T::ISR: RDA_IF Mask

Definition at line 5473 of file Mini51Series.h.

## ◆ UART_ISR_RDA_IF_Pos

#define UART_ISR_RDA_IF_Pos (0)

UART_T::ISR: RDA_IF Position

Definition at line 5472 of file Mini51Series.h.

## ◆ UART_ISR_RDA_INT_Msk

#define UART_ISR_RDA_INT_Msk (0x1ul << UART_ISR_RDA_INT_Pos)

UART_T::ISR: RDA_INT Mask

Definition at line 5491 of file Mini51Series.h.

## ◆ UART_ISR_RDA_INT_Pos

#define UART_ISR_RDA_INT_Pos (8)

UART_T::ISR: RDA_INT Position

Definition at line 5490 of file Mini51Series.h.

## ◆ UART_ISR_RLS_IF_Msk

#define UART_ISR_RLS_IF_Msk (0x1ul << UART_ISR_RLS_IF_Pos)

UART_T::ISR: RLS_IF Mask

Definition at line 5479 of file Mini51Series.h.

## ◆ UART_ISR_RLS_IF_Pos

#define UART_ISR_RLS_IF_Pos (2)

UART_T::ISR: RLS_IF Position

Definition at line 5478 of file Mini51Series.h.

## ◆ UART_ISR_RLS_INT_Msk

#define UART_ISR_RLS_INT_Msk (0x1ul << UART_ISR_RLS_INT_Pos)

UART_T::ISR: RLS_INT Mask

Definition at line 5497 of file Mini51Series.h.

## ◆ UART_ISR_RLS_INT_Pos

#define UART_ISR_RLS_INT_Pos (10)

UART_T::ISR: RLS_INT Position

Definition at line 5496 of file Mini51Series.h.

## ◆ UART_ISR_THRE_IF_Msk

#define UART_ISR_THRE_IF_Msk (0x1ul << UART_ISR_THRE_IF_Pos)

UART_T::ISR: THRE_IF Mask

Definition at line 5476 of file Mini51Series.h.

## ◆ UART_ISR_THRE_IF_Pos

#define UART_ISR_THRE_IF_Pos (1)

UART_T::ISR: THRE_IF Position

Definition at line 5475 of file Mini51Series.h.

## ◆ UART_ISR_THRE_INT_Msk

#define UART_ISR_THRE_INT_Msk (0x1ul << UART_ISR_THRE_INT_Pos)

UART_T::ISR: THRE_INT Mask

Definition at line 5494 of file Mini51Series.h.

## ◆ UART_ISR_THRE_INT_Pos

#define UART_ISR_THRE_INT_Pos (9)

UART_T::ISR: THRE_INT Position

Definition at line 5493 of file Mini51Series.h.

## ◆ UART_ISR_TOUT_IF_Msk

#define UART_ISR_TOUT_IF_Msk (0x1ul << UART_ISR_TOUT_IF_Pos)

UART_T::ISR: TOUT_IF Mask

Definition at line 5485 of file Mini51Series.h.

## ◆ UART_ISR_TOUT_IF_Pos

#define UART_ISR_TOUT_IF_Pos (4)

UART_T::ISR: TOUT_IF Position

Definition at line 5484 of file Mini51Series.h.

## ◆ UART_ISR_TOUT_INT_Msk

#define UART_ISR_TOUT_INT_Msk (0x1ul << UART_ISR_TOUT_INT_Pos)

UART_T::ISR: TOUT_INT Mask

Definition at line 5503 of file Mini51Series.h.

## ◆ UART_ISR_TOUT_INT_Pos

#define UART_ISR_TOUT_INT_Pos (12)

UART_T::ISR: TOUT_INT Position

Definition at line 5502 of file Mini51Series.h.

## ◆ UART_LCR_BCB_Msk

#define UART_LCR_BCB_Msk (0x1ul << UART_LCR_BCB_Pos)

UART_T::LCR: BCB Mask

Definition at line 5413 of file Mini51Series.h.

## ◆ UART_LCR_BCB_Pos

#define UART_LCR_BCB_Pos (6)

UART_T::LCR: BCB Position

Definition at line 5412 of file Mini51Series.h.

## ◆ UART_LCR_EPE_Msk

#define UART_LCR_EPE_Msk (0x1ul << UART_LCR_EPE_Pos)

UART_T::LCR: EPE Mask

Definition at line 5407 of file Mini51Series.h.

## ◆ UART_LCR_EPE_Pos

#define UART_LCR_EPE_Pos (4)

UART_T::LCR: EPE Position

Definition at line 5406 of file Mini51Series.h.

## ◆ UART_LCR_NSB_Msk

#define UART_LCR_NSB_Msk (0x1ul << UART_LCR_NSB_Pos)

UART_T::LCR: NSB Mask

Definition at line 5401 of file Mini51Series.h.

## ◆ UART_LCR_NSB_Pos

#define UART_LCR_NSB_Pos (2)

UART_T::LCR: NSB Position

Definition at line 5400 of file Mini51Series.h.

## ◆ UART_LCR_PBE_Msk

#define UART_LCR_PBE_Msk (0x1ul << UART_LCR_PBE_Pos)

UART_T::LCR: PBE Mask

Definition at line 5404 of file Mini51Series.h.

## ◆ UART_LCR_PBE_Pos

#define UART_LCR_PBE_Pos (3)

UART_T::LCR: PBE Position

Definition at line 5403 of file Mini51Series.h.

## ◆ UART_LCR_SPE_Msk

#define UART_LCR_SPE_Msk (0x1ul << UART_LCR_SPE_Pos)

UART_T::LCR: SPE Mask

Definition at line 5410 of file Mini51Series.h.

## ◆ UART_LCR_SPE_Pos

#define UART_LCR_SPE_Pos (5)

UART_T::LCR: SPE Position

Definition at line 5409 of file Mini51Series.h.

## ◆ UART_LCR_WLS_Msk

#define UART_LCR_WLS_Msk (0x3ul << UART_LCR_WLS_Pos)

UART_T::LCR: WLS Mask

Definition at line 5398 of file Mini51Series.h.

## ◆ UART_LCR_WLS_Pos

#define UART_LCR_WLS_Pos (0)

UART_T::LCR: WLS Position

Definition at line 5397 of file Mini51Series.h.

## ◆ UART_MCR_LEV_RTS_Msk

#define UART_MCR_LEV_RTS_Msk (0x1ul << UART_MCR_LEV_RTS_Pos)

UART_T::MCR: LEV_RTS Mask

Definition at line 5419 of file Mini51Series.h.

## ◆ UART_MCR_LEV_RTS_Pos

#define UART_MCR_LEV_RTS_Pos (9)

UART_T::MCR: LEV_RTS Position

Definition at line 5418 of file Mini51Series.h.

## ◆ UART_MCR_RTS_Msk

#define UART_MCR_RTS_Msk (0x1ul << UART_MCR_RTS_Pos)

UART_T::MCR: RTS Mask

Definition at line 5416 of file Mini51Series.h.

## ◆ UART_MCR_RTS_Pos

#define UART_MCR_RTS_Pos (1)

UART_T::MCR: RTS Position

Definition at line 5415 of file Mini51Series.h.

## ◆ UART_MCR_RTS_ST_Msk

#define UART_MCR_RTS_ST_Msk (0x1ul << UART_MCR_RTS_ST_Pos)

UART_T::MCR: RTS_ST Mask

Definition at line 5422 of file Mini51Series.h.

## ◆ UART_MCR_RTS_ST_Pos

#define UART_MCR_RTS_ST_Pos (13)

UART_T::MCR: RTS_ST Position

Definition at line 5421 of file Mini51Series.h.

## ◆ UART_MSR_CTS_ST_Msk

#define UART_MSR_CTS_ST_Msk (0x1ul << UART_MSR_CTS_ST_Pos)

UART_T::MSR: CTS_ST Mask

Definition at line 5428 of file Mini51Series.h.

## ◆ UART_MSR_CTS_ST_Pos

#define UART_MSR_CTS_ST_Pos (4)

UART_T::MSR: CTS_ST Position

Definition at line 5427 of file Mini51Series.h.

## ◆ UART_MSR_DCTSF_Msk

#define UART_MSR_DCTSF_Msk (0x1ul << UART_MSR_DCTSF_Pos)

UART_T::MSR: DCTSF Mask

Definition at line 5425 of file Mini51Series.h.

## ◆ UART_MSR_DCTSF_Pos

#define UART_MSR_DCTSF_Pos (0)

UART_T::MSR: DCTSF Position

Definition at line 5424 of file Mini51Series.h.

## ◆ UART_MSR_LEV_CTS_Msk

#define UART_MSR_LEV_CTS_Msk (0x1ul << UART_MSR_LEV_CTS_Pos)

UART_T::MSR: LEV_CTS Mask

Definition at line 5431 of file Mini51Series.h.

## ◆ UART_MSR_LEV_CTS_Pos

#define UART_MSR_LEV_CTS_Pos (8)

UART_T::MSR: LEV_CTS Position

Definition at line 5430 of file Mini51Series.h.

## ◆ UART_RBR_RBR_Msk

#define UART_RBR_RBR_Msk (0xfful << UART_RBR_RBR_Pos)

UART_T::RBR: RBR Mask

Definition at line 5347 of file Mini51Series.h.

## ◆ UART_RBR_RBR_Pos

#define UART_RBR_RBR_Pos (0)

    @addtogroup UART_CONST UART Bit Field Definition
    Constant Definitions for UART Controller

UART_T::RBR: RBR Position

Definition at line 5346 of file Mini51Series.h.

## ◆ UART_THR_THR_Msk

#define UART_THR_THR_Msk (0xfful << UART_THR_THR_Pos)

UART_T::THR: THR Mask

Definition at line 5350 of file Mini51Series.h.

## ◆ UART_THR_THR_Pos

#define UART_THR_THR_Pos (0)

UART_T::THR: THR Position

Definition at line 5349 of file Mini51Series.h.

## ◆ UART_TOR_DLY_Msk

#define UART_TOR_DLY_Msk (0xfful << UART_TOR_DLY_Pos)

UART_T::TOR: DLY Mask

Definition at line 5512 of file Mini51Series.h.

## ◆ UART_TOR_DLY_Pos

#define UART_TOR_DLY_Pos (8)

UART_T::TOR: DLY Position

Definition at line 5511 of file Mini51Series.h.

## ◆ UART_TOR_TOIC_Msk

#define UART_TOR_TOIC_Msk (0xfful << UART_TOR_TOIC_Pos)

UART_T::TOR: TOIC Mask

Definition at line 5509 of file Mini51Series.h.

## ◆ UART_TOR_TOIC_Pos

#define UART_TOR_TOIC_Pos (0)

UART_T::TOR: TOIC Position

Definition at line 5508 of file Mini51Series.h.

## ◆ WDT_WTCR_DBGACK_WDT_Msk

#define WDT_WTCR_DBGACK_WDT_Msk (0x1ul << WDT_WTCR_DBGACK_WDT_Pos)

WDT_T::WTCR: DBGACK_WDT Mask

Definition at line 5664 of file Mini51Series.h.

## ◆ WDT_WTCR_DBGACK_WDT_Pos

#define WDT_WTCR_DBGACK_WDT_Pos (31)

WDT_T::WTCR: DBGACK_WDT Position

Definition at line 5663 of file Mini51Series.h.

## ◆ WDT_WTCR_WTE_Msk

#define WDT_WTCR_WTE_Msk (0x1ul << WDT_WTCR_WTE_Pos)

WDT_T::WTCR: WTE Mask

Definition at line 5658 of file Mini51Series.h.

## ◆ WDT_WTCR_WTE_Pos

#define WDT_WTCR_WTE_Pos (7)

WDT_T::WTCR: WTE Position

Definition at line 5657 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIE_Msk

#define WDT_WTCR_WTIE_Msk (0x1ul << WDT_WTCR_WTIE_Pos)

WDT_T::WTCR: WTIE Mask

Definition at line 5655 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIE_Pos

#define WDT_WTCR_WTIE_Pos (6)

WDT_T::WTCR: WTIE Position

Definition at line 5654 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIF_Msk

#define WDT_WTCR_WTIF_Msk (0x1ul << WDT_WTCR_WTIF_Pos)

WDT_T::WTCR: WTIF Mask

Definition at line 5646 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIF_Pos

#define WDT_WTCR_WTIF_Pos (3)

WDT_T::WTCR: WTIF Position

Definition at line 5645 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIS_Msk

#define WDT_WTCR_WTIS_Msk (0x7ul << WDT_WTCR_WTIS_Pos)

WDT_T::WTCR: WTIS Mask

Definition at line 5661 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIS_Pos

#define WDT_WTCR_WTIS_Pos (8)

WDT_T::WTCR: WTIS Position

Definition at line 5660 of file Mini51Series.h.

## ◆ WDT_WTCR_WTR_Msk

#define WDT_WTCR_WTR_Msk (0x1ul << WDT_WTCR_WTR_Pos)

WDT_T::WTCR: WTR Mask

Definition at line 5637 of file Mini51Series.h.

## ◆ WDT_WTCR_WTR_Pos

#define WDT_WTCR_WTR_Pos (0)

    @addtogroup WDT_CONST WDT Bit Field Definition
    Constant Definitions for WDT Controller

WDT_T::WTCR: WTR Position

Definition at line 5636 of file Mini51Series.h.

## ◆ WDT_WTCR_WTRE_Msk

#define WDT_WTCR_WTRE_Msk (0x1ul << WDT_WTCR_WTRE_Pos)

WDT_T::WTCR: WTRE Mask

Definition at line 5640 of file Mini51Series.h.

## ◆ WDT_WTCR_WTRE_Pos

#define WDT_WTCR_WTRE_Pos (1)

WDT_T::WTCR: WTRE Position

Definition at line 5639 of file Mini51Series.h.

## ◆ WDT_WTCR_WTRF_Msk

#define WDT_WTCR_WTRF_Msk (0x1ul << WDT_WTCR_WTRF_Pos)

WDT_T::WTCR: WTRF Mask

Definition at line 5643 of file Mini51Series.h.

## ◆ WDT_WTCR_WTRF_Pos

#define WDT_WTCR_WTRF_Pos (2)

WDT_T::WTCR: WTRF Position

Definition at line 5642 of file Mini51Series.h.

## ◆ WDT_WTCR_WTWKE_Msk

#define WDT_WTCR_WTWKE_Msk (0x1ul << WDT_WTCR_WTWKE_Pos)

WDT_T::WTCR: WTWKE Mask

Definition at line 5649 of file Mini51Series.h.

## ◆ WDT_WTCR_WTWKE_Pos

#define WDT_WTCR_WTWKE_Pos (4)

WDT_T::WTCR: WTWKE Position

Definition at line 5648 of file Mini51Series.h.

## ◆ WDT_WTCR_WTWKF_Msk

#define WDT_WTCR_WTWKF_Msk (0x1ul << WDT_WTCR_WTWKF_Pos)

WDT_T::WTCR: WTWKF Mask

Definition at line 5652 of file Mini51Series.h.

## ◆ WDT_WTCR_WTWKF_Pos

#define WDT_WTCR_WTWKF_Pos (5)

WDT_T::WTCR: WTWKF Position

Definition at line 5651 of file Mini51Series.h.