| MINI51DE_BSP V3.02.004 The Board Support Package for Mini51DE Series MCU

Macros | Enumerator | Variables
MINI51 Legacy Constants
MINI51 Peripheral Memory Map » MINI51 Peripheral Declaration » MINI51 I/O routines
Collaboration diagram for MINI51 Legacy Constants:

## Macros
#define | NULL (0)
| NULL pointer. More...
#define | TRUE (1)
| Boolean true, define to use in API parameters or return value. More...
#define | FALSE (0)
| Boolean false, define to use in API parameters or return value. More...
#define | ENABLE (1)
| Enable, define to use in API parameters. More...
#define | DISABLE (0)
| Disable, define to use in API parameters. More...
#define | BIT0 (0x00000001)
| Bit 0 mask of an 32 bit integer. More...
#define | BIT1 (0x00000002)
| Bit 1 mask of an 32 bit integer. More...
#define | BIT2 (0x00000004)
| Bit 2 mask of an 32 bit integer. More...
#define | BIT3 (0x00000008)
| Bit 3 mask of an 32 bit integer. More...
#define | BIT4 (0x00000010)
| Bit 4 mask of an 32 bit integer. More...
#define | BIT5 (0x00000020)
| Bit 5 mask of an 32 bit integer. More...
#define | BIT6 (0x00000040)
| Bit 6 mask of an 32 bit integer. More...
#define | BIT7 (0x00000080)
| Bit 7 mask of an 32 bit integer. More...
#define | BIT8 (0x00000100)
| Bit 8 mask of an 32 bit integer. More...
#define | BIT9 (0x00000200)
| Bit 9 mask of an 32 bit integer. More...
#define | BIT10 (0x00000400)
| Bit 10 mask of an 32 bit integer. More...
#define | BIT11 (0x00000800)
| Bit 11 mask of an 32 bit integer. More...
#define | BIT12 (0x00001000)
| Bit 12 mask of an 32 bit integer. More...
#define | BIT13 (0x00002000)
| Bit 13 mask of an 32 bit integer. More...
#define | BIT14 (0x00004000)
| Bit 14 mask of an 32 bit integer. More...
#define | BIT15 (0x00008000)
| Bit 15 mask of an 32 bit integer. More...
#define | BIT16 (0x00010000)
| Bit 16 mask of an 32 bit integer. More...
#define | BIT17 (0x00020000)
| Bit 17 mask of an 32 bit integer. More...
#define | BIT18 (0x00040000)
| Bit 18 mask of an 32 bit integer. More...
#define | BIT19 (0x00080000)
| Bit 19 mask of an 32 bit integer. More...
#define | BIT20 (0x00100000)
| Bit 20 mask of an 32 bit integer. More...
#define | BIT21 (0x00200000)
| Bit 21 mask of an 32 bit integer. More...
#define | BIT22 (0x00400000)
| Bit 22 mask of an 32 bit integer. More...
#define | BIT23 (0x00800000)
| Bit 23 mask of an 32 bit integer. More...
#define | BIT24 (0x01000000)
| Bit 24 mask of an 32 bit integer. More...
#define | BIT25 (0x02000000)
| Bit 25 mask of an 32 bit integer. More...
#define | BIT26 (0x04000000)
| Bit 26 mask of an 32 bit integer. More...
#define | BIT27 (0x08000000)
| Bit 27 mask of an 32 bit integer. More...
#define | BIT28 (0x10000000)
| Bit 28 mask of an 32 bit integer. More...
#define | BIT29 (0x20000000)
| Bit 29 mask of an 32 bit integer. More...
#define | BIT30 (0x40000000)
| Bit 30 mask of an 32 bit integer. More...
#define | BIT31 (0x80000000)
| Bit 31 mask of an 32 bit integer. More...
#define | BYTE0_Msk (0x000000FF)
| Mask to get bit0~bit7 from a 32 bit integer. More...
#define | BYTE1_Msk (0x0000FF00)
| Mask to get bit8~bit15 from a 32 bit integer. More...
#define | BYTE2_Msk (0x00FF0000)
| Mask to get bit16~bit23 from a 32 bit integer. More...
#define | BYTE3_Msk (0xFF000000)
| Mask to get bit24~bit31 from a 32 bit integer. More...
#define | GET_BYTE0(u32Param) ((u32Param & BYTE0_Msk) )
#define | GET_BYTE1(u32Param) ((u32Param & BYTE1_Msk) >> 8)
#define | GET_BYTE2(u32Param) ((u32Param & BYTE2_Msk) >> 16)
#define | GET_BYTE3(u32Param) ((u32Param & BYTE3_Msk) >> 24)

## Variables
__IO uint32_t | ACMP_T::CMPCR [2]
__IO uint32_t | ACMP_T::CMPSR
__IO uint32_t | ACMP_T::CMPRVCR
__I uint32_t | ADC_T::ADDR
__IO uint32_t | ADC_T::ADCR
__IO uint32_t | ADC_T::ADCHER
__IO uint32_t | ADC_T::ADCMPR [2]
__IO uint32_t | ADC_T::ADSR
__IO uint32_t | ADC_T::ADTDCR
__IO uint32_t | ADC_T::ADSAMP
__IO uint32_t | CLK_T::PWRCON
__IO uint32_t | CLK_T::AHBCLK
__IO uint32_t | CLK_T::APBCLK
__IO uint32_t | CLK_T::CLKSTATUS
__IO uint32_t | CLK_T::CLKSEL0
__IO uint32_t | CLK_T::CLKSEL1
__IO uint32_t | CLK_T::CLKDIV
__IO uint32_t | CLK_T::CLKSEL2
__IO uint32_t | CLK_T::FRQDIV
__IO uint32_t | FMC_T::ISPCON
__IO uint32_t | FMC_T::ISPADR
__IO uint32_t | FMC_T::ISPDAT
__IO uint32_t | FMC_T::ISPCMD
__IO uint32_t | FMC_T::ISPTRG
__I uint32_t | FMC_T::DFBADR
__I uint32_t | FMC_T::ISPSTA
__I uint32_t | GCR_T::PDID
__IO uint32_t | GCR_T::RSTSRC
__IO uint32_t | GCR_T::IPRSTC1
__IO uint32_t | GCR_T::IPRSTC2
__IO uint32_t | GCR_T::BODCTL
__IO uint32_t | GCR_T::P0_MFP
__IO uint32_t | GCR_T::P1_MFP
__IO uint32_t | GCR_T::P2_MFP
__IO uint32_t | GCR_T::P3_MFP
__IO uint32_t | GCR_T::P4_MFP
__IO uint32_t | GCR_T::P5_MFP
__IO uint32_t | GCR_T::IRCTRIMCTL
__IO uint32_t | GCR_T::IRCTRIMIER
__IO uint32_t | GCR_T::IRCTRIMISR
__IO uint32_t | GCR_T::RegLockAddr
__IO uint32_t | GPIO_T::PMD
__IO uint32_t | GPIO_T::OFFD
__IO uint32_t | GPIO_T::DOUT
__IO uint32_t | GPIO_T::DMASK
__I uint32_t | GPIO_T::PIN
__IO uint32_t | GPIO_T::DBEN
__IO uint32_t | GPIO_T::IMD
__IO uint32_t | GPIO_T::IEN
__IO uint32_t | GPIO_T::ISRC
__IO uint32_t | GPIO_DBNCECON_T::DBNCECON
__IO uint32_t | I2C_T::I2CON
__IO uint32_t | I2C_T::I2CADDR0
__IO uint32_t | I2C_T::I2CDAT
__I uint32_t | I2C_T::I2CSTATUS
__IO uint32_t | I2C_T::I2CLK
__IO uint32_t | I2C_T::I2CTOC
__IO uint32_t | I2C_T::I2CADDR1
__IO uint32_t | I2C_T::I2CADDR2
__IO uint32_t | I2C_T::I2CADDR3
__IO uint32_t | I2C_T::I2CADM0
__IO uint32_t | I2C_T::I2CADM1
__IO uint32_t | I2C_T::I2CADM2
__IO uint32_t | I2C_T::I2CADM3
__IO uint32_t | I2C_T::I2CON2
__IO uint32_t | I2C_T::I2CSTATUS2
__I uint32_t | INT_T::SRC0
__I uint32_t | INT_T::SRC1
__I uint32_t | INT_T::SRC2
__I uint32_t | INT_T::SRC3
__I uint32_t | INT_T::SRC4
__I uint32_t | INT_T::SRC5
__I uint32_t | INT_T::SRC6
__I uint32_t | INT_T::SRC7
__I uint32_t | INT_T::SRC8
__I uint32_t | INT_T::SRC9
__I uint32_t | INT_T::SRC12
__I uint32_t | INT_T::SRC14
__I uint32_t | INT_T::SRC16
__I uint32_t | INT_T::SRC17
__I uint32_t | INT_T::SRC18
__I uint32_t | INT_T::SRC25
__I uint32_t | INT_T::SRC28
__I uint32_t | INT_T::SRC29
__IO uint32_t | INT_T::NMICON
__IO uint32_t | INT_T::MCUIRQ
__IO uint32_t | PWM_T::PPR
__IO uint32_t | PWM_T::CSR
__IO uint32_t | PWM_T::PCR
__IO uint32_t | PWM_T::CNR [6]
__IO uint32_t | PWM_T::CMR [6]
__IO uint32_t | PWM_T::PIER
__IO uint32_t | PWM_T::PIIR
__IO uint32_t | PWM_T::POE
__IO uint32_t | PWM_T::PFBCON
__IO uint32_t | PWM_T::PDZIR
__IO uint32_t | PWM_T::TRGCON0
__IO uint32_t | PWM_T::TRGCON1
__IO uint32_t | PWM_T::TRGSTS0
__IO uint32_t | PWM_T::TRGSTS1
__IO uint32_t | PWM_T::PHCHG
__IO uint32_t | PWM_T::PHCHGNXT
__IO uint32_t | PWM_T::PHCHGMASK
__IO uint32_t | PWM_T::INTACCUCTL
__IO uint32_t | SPI_T::CNTRL
__IO uint32_t | SPI_T::DIVIDER
__IO uint32_t | SPI_T::SSR
__I uint32_t | SPI_T::RX
__O uint32_t | SPI_T::TX
__IO uint32_t | SPI_T::CNTRL2
__IO uint32_t | SPI_T::FIFO_CTL
__IO uint32_t | SPI_T::STATUS
__IO uint32_t | TIMER_T::TCSR
__IO uint32_t | TIMER_T::TCMPR
__IO uint32_t | TIMER_T::TISR
__I uint32_t | TIMER_T::TDR
__I uint32_t | TIMER_T::TCAP
__IO uint32_t | TIMER_T::TEXCON
__IO uint32_t | TIMER_T::TEXISR
__I uint32_t UART_T::RBR
__O uint32_t UART_T::THR
union {
__I uint32_t UART_T::RBR
__O uint32_t UART_T::THR
}; |
__IO uint32_t | UART_T::IER
__IO uint32_t | UART_T::FCR
__IO uint32_t | UART_T::LCR
__IO uint32_t | UART_T::MCR
__IO uint32_t | UART_T::MSR
__IO uint32_t | UART_T::FSR
__IO uint32_t | UART_T::ISR
__IO uint32_t | UART_T::TOR
__IO uint32_t | UART_T::BAUD
__IO uint32_t | UART_T::IRCR
__IO uint32_t | UART_T::ALT_CSR
__IO uint32_t | UART_T::FUN_SEL
__IO uint32_t | WDT_T::WTCR

## Detailed Description

MINI51 Legacy Constants

## Macro Definition Documentation

## ◆ BIT0

#define BIT0 (0x00000001)

Bit 0 mask of an 32 bit integer.

Definition at line 5902 of file Mini51Series.h.

## ◆ BIT1

#define BIT1 (0x00000002)

Bit 1 mask of an 32 bit integer.

Definition at line 5903 of file Mini51Series.h.

## ◆ BIT10

#define BIT10 (0x00000400)

Bit 10 mask of an 32 bit integer.

Definition at line 5912 of file Mini51Series.h.

## ◆ BIT11

#define BIT11 (0x00000800)

Bit 11 mask of an 32 bit integer.

Definition at line 5913 of file Mini51Series.h.

## ◆ BIT12

#define BIT12 (0x00001000)

Bit 12 mask of an 32 bit integer.

Definition at line 5914 of file Mini51Series.h.

## ◆ BIT13

#define BIT13 (0x00002000)

Bit 13 mask of an 32 bit integer.

Definition at line 5915 of file Mini51Series.h.

## ◆ BIT14

#define BIT14 (0x00004000)

Bit 14 mask of an 32 bit integer.

Definition at line 5916 of file Mini51Series.h.

## ◆ BIT15

#define BIT15 (0x00008000)

Bit 15 mask of an 32 bit integer.

Definition at line 5917 of file Mini51Series.h.

## ◆ BIT16

#define BIT16 (0x00010000)

Bit 16 mask of an 32 bit integer.

Definition at line 5918 of file Mini51Series.h.

## ◆ BIT17

#define BIT17 (0x00020000)

Bit 17 mask of an 32 bit integer.

Definition at line 5919 of file Mini51Series.h.

## ◆ BIT18

#define BIT18 (0x00040000)

Bit 18 mask of an 32 bit integer.

Definition at line 5920 of file Mini51Series.h.

## ◆ BIT19

#define BIT19 (0x00080000)

Bit 19 mask of an 32 bit integer.

Definition at line 5921 of file Mini51Series.h.

## ◆ BIT2

#define BIT2 (0x00000004)

Bit 2 mask of an 32 bit integer.

Definition at line 5904 of file Mini51Series.h.

## ◆ BIT20

#define BIT20 (0x00100000)

Bit 20 mask of an 32 bit integer.

Definition at line 5922 of file Mini51Series.h.

## ◆ BIT21

#define BIT21 (0x00200000)

Bit 21 mask of an 32 bit integer.

Definition at line 5923 of file Mini51Series.h.

## ◆ BIT22

#define BIT22 (0x00400000)

Bit 22 mask of an 32 bit integer.

Definition at line 5924 of file Mini51Series.h.

## ◆ BIT23

#define BIT23 (0x00800000)

Bit 23 mask of an 32 bit integer.

Definition at line 5925 of file Mini51Series.h.

## ◆ BIT24

#define BIT24 (0x01000000)

Bit 24 mask of an 32 bit integer.

Definition at line 5926 of file Mini51Series.h.

## ◆ BIT25

#define BIT25 (0x02000000)

Bit 25 mask of an 32 bit integer.

Definition at line 5927 of file Mini51Series.h.

## ◆ BIT26

#define BIT26 (0x04000000)

Bit 26 mask of an 32 bit integer.

Definition at line 5928 of file Mini51Series.h.

## ◆ BIT27

#define BIT27 (0x08000000)

Bit 27 mask of an 32 bit integer.

Definition at line 5929 of file Mini51Series.h.

## ◆ BIT28

#define BIT28 (0x10000000)

Bit 28 mask of an 32 bit integer.

Definition at line 5930 of file Mini51Series.h.

## ◆ BIT29

#define BIT29 (0x20000000)

Bit 29 mask of an 32 bit integer.

Definition at line 5931 of file Mini51Series.h.

## ◆ BIT3

#define BIT3 (0x00000008)

Bit 3 mask of an 32 bit integer.

Definition at line 5905 of file Mini51Series.h.

## ◆ BIT30

#define BIT30 (0x40000000)

Bit 30 mask of an 32 bit integer.

Definition at line 5932 of file Mini51Series.h.

## ◆ BIT31

#define BIT31 (0x80000000)

Bit 31 mask of an 32 bit integer.

Definition at line 5933 of file Mini51Series.h.

## ◆ BIT4

#define BIT4 (0x00000010)

Bit 4 mask of an 32 bit integer.

Definition at line 5906 of file Mini51Series.h.

## ◆ BIT5

#define BIT5 (0x00000020)

Bit 5 mask of an 32 bit integer.

Definition at line 5907 of file Mini51Series.h.

## ◆ BIT6

#define BIT6 (0x00000040)

Bit 6 mask of an 32 bit integer.

Definition at line 5908 of file Mini51Series.h.

## ◆ BIT7

#define BIT7 (0x00000080)

Bit 7 mask of an 32 bit integer.

Definition at line 5909 of file Mini51Series.h.

## ◆ BIT8

#define BIT8 (0x00000100)

Bit 8 mask of an 32 bit integer.

Definition at line 5910 of file Mini51Series.h.

## ◆ BIT9

#define BIT9 (0x00000200)

Bit 9 mask of an 32 bit integer.

Definition at line 5911 of file Mini51Series.h.

## ◆ BYTE0_Msk

#define BYTE0_Msk (0x000000FF)

Mask to get bit0~bit7 from a 32 bit integer.

Definition at line 5936 of file Mini51Series.h.

## ◆ BYTE1_Msk

#define BYTE1_Msk (0x0000FF00)

Mask to get bit8~bit15 from a 32 bit integer.

Definition at line 5937 of file Mini51Series.h.

## ◆ BYTE2_Msk

#define BYTE2_Msk (0x00FF0000)

Mask to get bit16~bit23 from a 32 bit integer.

Definition at line 5938 of file Mini51Series.h.

## ◆ BYTE3_Msk

#define BYTE3_Msk (0xFF000000)

Mask to get bit24~bit31 from a 32 bit integer.

Definition at line 5939 of file Mini51Series.h.

## ◆ DISABLE

#define DISABLE (0)

Disable, define to use in API parameters.

Definition at line 5899 of file Mini51Series.h.

## ◆ ENABLE

#define ENABLE (1)

Enable, define to use in API parameters.

Definition at line 5898 of file Mini51Series.h.

## ◆ FALSE

#define FALSE (0)

Boolean false, define to use in API parameters or return value.

Definition at line 5896 of file Mini51Series.h.

## ◆ GET_BYTE0

#define GET_BYTE0 | ( |  | u32Param | ) | ((u32Param & BYTE0_Msk) )

Extract Byte 0 (Bit 0~ 7) from parameter u32Param

Definition at line 5941 of file Mini51Series.h.

## ◆ GET_BYTE1

#define GET_BYTE1 | ( |  | u32Param | ) | ((u32Param & BYTE1_Msk) >> 8)

Extract Byte 1 (Bit 8~15) from parameter u32Param

Definition at line 5942 of file Mini51Series.h.

## ◆ GET_BYTE2

#define GET_BYTE2 | ( |  | u32Param | ) | ((u32Param & BYTE2_Msk) >> 16)

Extract Byte 2 (Bit 16~23) from parameter u32Param

Definition at line 5943 of file Mini51Series.h.

## ◆ GET_BYTE3

#define GET_BYTE3 | ( |  | u32Param | ) | ((u32Param & BYTE3_Msk) >> 24)

Extract Byte 3 (Bit 24~31) from parameter u32Param

Definition at line 5944 of file Mini51Series.h.

## ◆ NULL

#define NULL (0)

NULL pointer.

Definition at line 5892 of file Mini51Series.h.

## ◆ TRUE

#define TRUE (1)

Boolean true, define to use in API parameters or return value.

Definition at line 5895 of file Mini51Series.h.

## Variable Documentation

## ◆

union { ... } UART_T::@1

## ◆ ADCHER

ADC_T::ADCHER

## Offset: 0x24 ADC Channel Enable Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | CHEN0 | Analog Input Channel 0 Enable Control
|  | 0 = Channel 0 Disabled.
|  | 1 = Channel 0 Enabled.
|  | Note: If software enables more than one channel, the channel with the smallest number will be selected and the other enabled channels will be ignored.
[1] | CHEN1 | Analog Input Channel 1 Enable Control
|  | 0 = Channel 1 Disabled.
|  | 1 = Channel 1 Enabled.
[2] | CHEN2 | Analog Input Channel 2 Enable Control
|  | 0 = Channel 2 Disabled.
|  | 1 = Channel 2 Enabled.
[3] | CHEN3 | Analog Input Channel 3 Enable Control
|  | 0 = Channel 3 Disabled.
|  | 1 = Channel 3 Enabled.
[4] | CHEN4 | Analog Input Channel 4 Enable Control
|  | 0 = Channel 4 Disabled.
|  | 1 = Channel 4 Enabled.
[5] | CHEN5 | Analog Input Channel 5 Enable Control
|  | 0 = Channel 5 Disabled.
|  | 1 = Channel 5 Enabled.
[6] | CHEN6 | Analog Input Channel 6 Enable Control
|  | 0 = Channel 6 Disabled.
|  | 1 = Channel 6 Enabled.
[7] | CHEN7 | Analog Input Channel 7 Enable Control
|  | 0 = Channel 7 Disabled.
|  | 1 = Channel 7 Enabled.
[8] | PRESEL | Analog Input Channel 7 Selection
|  | 0 = External analog input.
|  | 1 = Internal band-gap voltage (VBG).
|  | Note: When software selects the band-gap voltage as the analog input source of ADC channel 7, the ADC clock rate needs to be limited to lower than 300 kHz.

Definition at line 476 of file Mini51Series.h.

## ◆ ADCMPR

ADC_T::ADCMPR

## Offset: 0x28 ~ 0x2C ADC Compare Register

Bits | Field | Descriptions
--- | --- | ---
[0] | CMPEN | Compare Enable Control
|  | Set 1 to this bit to enable comparing CMPD[9:0] with specified channel conversion results when converted data is loaded into the ADDR register.
|  | 0 = Compare function Disabled.
|  | 1 = Compare function Enabled.
[1] | CMPIE | Compare Interrupt Enable Control
|  | If the compare function is enabled and the compare condition matches the setting of CMPCOND and CMPMATCNT, CMPFx bit will be asserted, in the meanwhile, if CMPIE is set to 1, a compare interrupt request is generated.
|  | 0 = Compare function interrupt Disabled.
|  | 1 = Compare function interrupt Enabled.
[2] | CMPCOND | Compare Condition
|  | 0 = Set the compare condition as that when a 10-bit A/D conversion result is less than the 10-bit CMPD (ADCMPRx[25:16]), the internal match counter will increase one.
|  | 1 = Set the compare condition as that when a 10-bit A/D conversion result is greater or equal to the 10-bit CMPD (ADCMPRx[25:16]), the internal match counter will increase one.
|  | Note: When the internal counter reaches the value to (CMPMATCNT +1), the CMPFx bit will be set.
[5:3] | CMPCH | Compare Channel Selection
|  | 000 = Channel 0 conversion result is selected to be compared.
|  | 001 = Channel 1 conversion result is selected to be compared.
|  | 010 = Channel 2 conversion result is selected to be compared.
|  | 011 = Channel 3 conversion result is selected to be compared.
|  | 100 = Channel 4 conversion result is selected to be compared.
|  | 101 = Channel 5 conversion result is selected to be compared.
|  | 110 = Channel 6 conversion result is selected to be compared.
|  | 111 = Channel 7 conversion result is selected to be compared.
[11:8] | CMPMATCNT | Compare Match Count
|  | When the specified A/D channel analog conversion result matches the compare condition defined by CMPCOND, the internal match counter will increase 1.
|  | When the internal counter reaches the value to (CMPMATCNT +1), the CMPFx bit will be set.
[25:16] | CMPD | Comparison Data
|  | The 10-bit data is used to compare with conversion result of specified channel.

Definition at line 477 of file Mini51Series.h.

## ◆ ADCR

ADC_T::ADCR

## Offset: 0x20 ADC Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | ADEN | A/D Converter Enable Control
|  | 0 = A/D Converter Disabled.
|  | 1 = A/D Converter Enabled.
|  | Note: Before starting A/D conversion function, this bit should be set to 1.
|  | Clear it to 0 to disable A/D converter analog circuit to save power consumption.
[1] | ADIE | A/D Interrupt Enable Control
|  | A/D conversion end interrupt request is generated if ADIE bit is set to 1.
|  | 0 = A/D interrupt function Disabled.
|  | 1 = A/D interrupt function Enabled.
[5:4] | TRGS | Hardware Trigger Source
|  | 00 = A/D conversion is started by external STADC pin.
|  | 11 = A/D conversion is started by PWM trigger.
|  | Others = Reserved.
|  | Note: Software should disable TRGEN and ADST before change TRGS.
[6] | TRGCOND | External Trigger Condition
|  | This bit decides whether the external pin STADC trigger event is falling or raising edge.
|  | The signal must be kept at stable state at least 4 PCLKs at high and low state for edge trigger.
|  | 0 = Falling edge.
|  | 1 = Raising edge.
[8] | TRGEN | External Trigger Enable Control
|  | Enable or disable triggering of A/D conversion by external STADC pin.
|  | If external trigger is enabled, the ADST bit can be set to 1 by the selected hardware trigger source.
|  | 0= External trigger Disabled.
|  | 1= External trigger Enabled.
[11] | ADST | A/D Conversion Start
|  | ADST bit can be set to 1 from three sources: software or PWM trigger and external pin STADC.
|  | ADST will be cleared to 0 by hardware automatically after conversion complete.
|  | 0 = Conversion stopped and A/D converter entered idle state.
|  | 1 = Conversion start.

Definition at line 475 of file Mini51Series.h.

## ◆ ADDR

ADC_T::ADDR

## Offset: 0x00 ADC Data Register

Bits | Field | Descriptions
--- | --- | ---
[9:0] | RSLT | A/D Conversion Result
|  | This field contains conversion result of ADC.
[16] | OVERRUN | Over Run Flag
|  | 0 = Data in RSLT (ADDR[9:0])is recent conversion result.
|  | 1 = Data in RSLT (ADDR[9:0])overwrote.
|  | If converted data in RSLT[9:0] has not been read before the new conversion result is loaded to this register, OVERRUN is set to 1.
|  | It is cleared by hardware after the ADDR register is read.
[17] | VALID | Valid Flag
|  | 0 = Data in RSLT (ADDR[9:0]) bits not valid.
|  | 1 = Data in RSLT (ADDR[9:0]) bits valid.
|  | This bit is set to 1 when ADC conversion is completed and cleared by hardware after the ADDR register is read.

Definition at line 471 of file Mini51Series.h.

## ◆ ADSAMP

ADC_T::ADSAMP

## Offset: 0x48 ADC Sampling Time Counter Register

Bits | Field | Descriptions
--- | --- | ---
[3:0] | ADSAMPCNT | ADC Sampling Counter
|  | If the ADC input is unstable, user can set this register to increase the sampling time to get a stable ADC input signal.
|  | The default sampling time is 1 ADC clock.
|  | The additional clock number will be inserted to lengthen the sampling clock.
|  | 0000 = 0 additional ADC sample clock.
|  | 0001 = 1 additional ADC sample clock.
|  | 0010 = 2 additional ADC sample clock.
|  | 0011 = 4 additional ADC sample clock.
|  | 0100 = 8 additional ADC sample clock.
|  | 0101 = 16 additional ADC sample clock.
|  | 0110 = 32 additional ADC sample clock.
|  | 0111 = 64 additional ADC sample clock.
|  | 1000 = 128 additional ADC sample clock.
|  | 1001 = 256 additional ADC sample clock.
|  | 1010 = 512 additional ADC sample clock.
|  | 1011 = 1024 additional ADC sample clock.
|  | 1100 = 1024 additional ADC sample clock.
|  | 1101 = 1024 additional ADC sample clock.
|  | 1110 = 1024 additional ADC sample clock.
|  | 1111 = 1024 additional ADC sample clock.

Definition at line 483 of file Mini51Series.h.

## ◆ ADSR

ADC_T::ADSR

## Offset: 0x30 ADC Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | ADF | A/D Conversion End Flag
|  | A status flag that indicates the end of A/D conversion. ADF is set to 1 When A/D conversion ends.
|  | Software can write 1 to clear this bit to 0.
[1] | CMPF0 | Compare Flag 0
|  | When the selected channel A/D conversion result meets the setting condition in ADCMPR0, this bit is set to 1.
|  | Software can write 1 to clear this bit to 0.
|  | 0 = Conversion result in ADDR does not meet the ADCMPR0 setting.
|  | 1 = Conversion result in ADDR meets the ADCMPR0 setting.
[2] | CMPF1 | Compare Flag 1
|  | When the selected channel A/D conversion result meets the setting condition in ADCMPR1, this bit is set to 1.
|  | Software can write 1 to clear this bit to 0.
|  | 0 = Conversion result in ADDR does not meet the ADCMPR1 setting.
|  | 1 = Conversion result in ADDR meets the ADCMPR1 setting.
[3] | BUSY | BUSY/IDLE (Read Only)
|  | This bit is mirror of as ADST bit in ADCR
|  | 0 = A/D converter is in idle state.
|  | 1 = A/D converter is busy at conversion.
[6:4] | CHANNEL | Current Conversion Channel (Read Only)
|  | This filed reflects the current conversion channel when BUSY=1.
|  | When BUSY=0, it shows the number of the next converted channel.
[8] | VALID | Data Valid Flag (Read Only)
|  | It is a mirror of VALID (ADDR[17]) bit in ADDR register.
[16] | OVERRUN | Overrun Flag (Read Only)
|  | It is a mirror to OVERRUN (ADSR[16]) bit in ADDR register.

Definition at line 478 of file Mini51Series.h.

## ◆ ADTDCR

ADC_T::ADTDCR

## Offset: 0x44 ADC Trigger Delay Control Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | PTDT | PWM Trigger Delay Timer
|  | Set this field will delay ADC start conversion time after PWM trigger.
|  | PWM trigger delay time is (4 * PTDT) * system clock.

Definition at line 482 of file Mini51Series.h.

## ◆ AHBCLK

CLK_T::AHBCLK

## Offset: 0x04 AHB Devices Clock Enable Control Register

Bits | Field | Descriptions
--- | --- | ---
[2] | ISP_EN | Flash ISP Controller Clock Enable Control
|  | 0 = Flash ISP peripheral clock Disabled.
|  | 1 = Flash ISP peripheral clock Enabled.

Definition at line 845 of file Mini51Series.h.

## ◆ ALT_CSR

UART_T::ALT_CSR

## Offset: 0x2C UART Alternate Control/Status Register

Bits | Field | Descriptions
--- | --- | ---
[8] | RS485_NMM | RS-485 Normal Multi-drop Operation Mode (NMM) Control
|  | 0 = RS-485 Normal Multi-drop Operation Mode (NMM) Disabled.
|  | 1 = RS-485 Normal Multi-drop Operation Mode (NMM) Enabled.
|  | Note: This bit cannot be active with RS485_AAD operation mode.
[9] | RS485_AAD | RS-485 Auto Address Detection Operation Mode (AAD)
|  | 0 = RS-485 Auto Address Detection Operation Mode (AAD) Disabled.
|  | 1 = RS-485 Auto Address Detection Operation Mode (AAD) Enabled.
|  | Note: This bit cannot be active with RS485_NMM operation mode.
[10] | RS485_AUD | RS-485 Auto Direction Mode (AUD) Control
|  | 0 = RS-485 Auto Address Detection Operation Mode (AAD) Disabled.
|  | 1 = RS-485 Auto Address Detection Operation Mode (AAD) Enabled.
|  | Note: This bit cannot be active with RS485_NMM operation mode.
[15] | RS485_ADD_EN | RS-485 Address Detection Enable Control
|  | This bit is used to enable RS-485 Address Detection mode.
|  | 0 = RS-485 address detection mode Disabled.
|  | 1 = RS-485 address detection mode Enabled.
|  | Note: This field is used for RS-485 any operation mode.
[31:24] | ADDR_MATCH | Address Match Value
|  | This field contains the RS-485 address match values.
|  | Note: This field is used for RS-485 auto address detection mode.

Definition at line 5334 of file Mini51Series.h.

## ◆ APBCLK

CLK_T::APBCLK

## Offset: 0x08 APB Devices Clock Enable Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | WDT_EN | Watchdog Timer Clock Enable Control (Write Protect)
|  | 0 = Watchdog Timer clock Disabled.
|  | 1 = Watchdog Timer clock Enabled.
|  | Note: This bit is the protected bit, and programming it needs to write 0x59, 0x16, and 0x88 to address 0x5000_0100 to disable register protection.
|  | Refer to the register REGWRPROT at address GCR_BA + 0x100.
[2] | TMR0_EN | Timer0 Clock Enable Control
|  | 0 = Timer0 clock Disabled.
|  | 1 = Timer0 clock Enabled.
[3] | TMR1_EN | Timer1 Clock Enable Control
|  | 0 = Timer1 clock Disabled.
|  | 1 = Timer1 clock Enabled.
[6] | FDIV_EN | Frequency Divider Output Clock Enable Control
|  | 0 = FDIV clock Disabled.
|  | 1 = FDIV clock Enabled.
[8] | I2C_EN | I2C Clock Enable Control
|  | 0 = I2C clock Disabled.
|  | 1 = I2C clock Enabled.
[12] | SPI_EN | SPI Peripheral Clock Enable Control
|  | 0 = SPI peripheral clock Disabled.
|  | 1 = SPI peripheral clock Enabled.
[16] | UART_EN | UART Clock Enable Control
|  | 0 = UART clock Disabled.
|  | 1 = UART clock Enabled.
[20] | PWM01_EN | PWM_01 Clock Enable Control
|  | 0 = PWM01 clock Disabled.
|  | 1 = PWM01 clock Enabled.
[21] | PWM23_EN | PWM_23 Clock Enable Control
|  | 0 = PWM23 clock Disabled.
|  | 1 = PWM23 clock Enabled.
[22] | PWM45_EN | PWM_45 Clock Enable Control
|  | 0 = PWM45 clock Disabled.
|  | 1 = PWM45 clock Enabled.
[28] | ADC_EN | Analog-digital-converter (ADC) Clock Enable Control
|  | 0 = ADC peripheral clock Disabled.
|  | 1 = ADC peripheral clock Enabled.
[30] | ACMP_EN | Analog Comparator Clock Enable Control
|  | 0 = Analog Comparator clock Disabled.
|  | 1 = Analog Comparator clock Enabled.

Definition at line 846 of file Mini51Series.h.

## ◆ BAUD

UART_T::BAUD

## Offset: 0x24 UART Baud Rate Divisor Register

Bits | Field | Descriptions
--- | --- | ---
[15:0] | BRD | Baud Rate Divider
|  | The field indicates the baud rate divider.
[27:24] | DIVIDER_X | Divider X
|  | The baud rate divider M = X+1.
[28] | DIV_X_ONE | Divider X Equal 1
|  | 0 = Divider M = X (the equation of M = X+1, but DIVIDER_X[27:24] must >= 8).
|  | 1 = Divider M = 1 (the equation of M = 1, but BRD [15:0] must >= 8).
|  | Refer to section "UART Controller Baud Rate Generator" for more information.
[29] | DIV_X_EN | Divider X Enable Control
|  | The BRD = Baud Rate Divider, and the baud rate equation is: Baud Rate = Clock / [M * (BRD + 2)], The default value of M is 16.
|  | 0 = Divider X Disabled (the equation of M = 16).
|  | 1 = Divider X Enabled (the equation of M = X+1, but DIVIDER_X [27:24] must >= 8).
|  | Note: When in IrDA mode, this bit must be disabled.

Definition at line 5332 of file Mini51Series.h.

## ◆ BODCTL

GCR_T::BODCTL

## Offset: 0x18 Brown-out Detector Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | BOD_VL_EXT | Brown-out Detector Selection Extension (Initiated & Write-protected Bit)
|  | The default value is set by flash controller user configuration CBOVEXT bit (config0 [23]).
|  | If config0 bit[23] is set to 1, default value of BOD_VL_EXT is 0.
|  | If config0 bit[23] is set to 0, default value of BOD_VL_EXT is 1.
|  | 0 = Brown-out detector threshold voltage is selected by the table defined in BOD_VL.
|  | 1 = Brown-out detector threshold voltage is selected by the table defined below.
|  | 11 = 4.4V
|  | 10 = 3.7V
|  | 01 = 2.7V
|  | 00 = 2.2V
[2:1] | BOD_VL | Brown-out Detector Threshold Voltage Selection (Initiated & Write-protected Bit)
|  | The default value is set by flash controller user configuration CBOV bit (config0 [22:21]).
|  | BOD_VL[1]
|  | BOD_VL[0]
|  | Brown-out voltage
|  | 11 = Disable
|  | 10 = 3.7V
|  | 01 = 2.7V
|  | 00 = Reserved
[3] | BOD_RSTEN | Brown-out Reset Enable Control (Initiated And Write-protected Bit)
|  | 0 = Brown-out "INTERRUPT" function Enabled; when the Brown-out Detector function is enable and the detected voltage is lower than the threshold, then assert a signal to interrupt the Cortex-M0 CPU.
|  | 1 = Brown-out "RESET" function Enabled; when the Brown-out Detector function is enable and the detected voltage is lower than the threshold then assert a signal to reset the chip.
|  | The default value is set by flash controller user configuration register config0 bit[20].
|  | When the BOD_EN is enabled and the interrupt is asserted, the interrupt will be kept till the BOD_EN is set to 0.
|  | The interrupt for CPU can be blocked by disabling the NVIC in CPU for BOD interrupt or disable the interrupt source by disabling the BOD_EN and then re-enabling the BOD_EN function if the BOD function is required.
[4] | BOD_INTF | Brown-out Detector Interrupt Flag
|  | 0 = Brown-out Detector does not detect any voltage dropped at AVDD down through or up through the voltage of BOD_VL setting.
|  | 1 = When Brown-out Detector detects the AVDD is dropped through the voltage of BOD_VL setting or the AVDD is raised up through the voltage of BOD_VL setting, this bit is set to 1 and the Brown-out interrupt is requested if Brown-out interrupt is enabled.
[5] | BOD_LPM | Brown-out Detector Low Power Mode (Write Protect)
|  | 0 = BOD operate in normal mode (default).
|  | 1 = Enable the BOD low power mode.
|  | The BOD consumes about 100uA in normal mode, the low power mode can reduce the current to about 1uA but slow the BOD response.
[6] | BOD_OUT | Brown-out Detector Output State
|  | 0 = Brown-out Detector status output is 0, the detected voltage is higher than BOD_VL setting.
|  | 1 = Brown-out Detector status output is 1, the detected voltage is lower than BOD_VL setting.

Definition at line 1511 of file Mini51Series.h.

## ◆ CLKDIV

CLK_T::CLKDIV

## Offset: 0x18 Clock Divider Number Register

Bits | Field | Descriptions
--- | --- | ---
[3:0] | HCLK_N | HCLK Clock Divide Number From HCLK Clock Source
|  | HCLK clock frequency = (HCLK clock source frequency) / (HCLK_N + 1).
[11:8] | UART_N | UART Clock Divide Number From UART Clock Source
|  | UART clock frequency = (UART clock source frequency) / (UART_N + 1).
[23:16] | ADC_N | ADC Peripheral Clock Divide Number From ADC Peripheral Clock Source
|  | ADC peripheral clock frequency = (ADC peripheral clock source frequency) / (ADC_N + 1).

Definition at line 850 of file Mini51Series.h.

## ◆ CLKSEL0

CLK_T::CLKSEL0

## Offset: 0x10 Clock Source Select Control Register 0

Bits | Field | Descriptions
--- | --- | ---
[2:0] | HCLK_S | HCLK Clock Source Selection (Write Protect)
|  | 000 = Clock source is from HXT or LXT.
|  | 001 = Reserved.
|  | 010 = Reserved.
|  | 011 = Clock source is from LIRC.
|  | 111 = Clock source is from HIRC.
|  | Others = Reserved.
|  | Note1: Before clock switching, the related clock sources (both pre-select and new-select) must be turn-on and stable.
|  | Note2: These bits are protected bit, and programming them needs to write 0x59, 0x16, and 0x88 to address 0x5000_0100 to disable register protection.
|  | Refer to the register REGWRPROT at address GCR_BA + 0x100.
|  | Note3: To set PWRCON[1:0], select HXT or LXT crystal clock.
[5:3] | STCLK_S | Cortex-M0 SysTick Clock Source Selection From Reference Clock (Write Protect)
|  | If SYST_CSR[2] = 1, SysTick clock source is from HCLK.
|  | If SYST_CSR[2] = 0, SysTick clock source is defined by below settings.
|  | 000 = Clock source is from HXT or LXT.
|  | 001 = Reserved.
|  | 010 = Clock source is from HXT/2 or LXT/2.
|  | 011 = Clock source is from HCLK/2.
|  | 111 = Clock source is from HIRC /2.
|  | Others = Reserved.
|  | Note1: These bits are protected bit, and programming them needs to write 0x59, 0x16, and 0x88 to address 0x5000_0100 to disable register protection.
|  | Refer to the register REGWRPROT at address GCR_BA + 0x100.
|  | Note2: If the SysTick clock source is not from HCLK (i.e. SYST_CSR[2] = 0), SysTick clock source must less than or equal to HCLK/2.
|  | Note3: To set PWRCON[1:0], select HXT or LXT crystal clock.

Definition at line 848 of file Mini51Series.h.

## ◆ CLKSEL1

CLK_T::CLKSEL1

## Offset: 0x14 Clock Source Select Control Register 1

Bits | Field | Descriptions
--- | --- | ---
[1:0] | WDT_S | WDT CLK Clock Source Selection (Write Protect)
|  | 00 = Clock source is from HXT or LXT.
|  | 01 = Reserved.
|  | 10 = Clock source is from HCLK/2048 clock.
|  | 11 = Clock source is from LIRC.
|  | Note1: These bits are the protected bit, and programming them needs to write 0x59, 0x16, and 0x88 to address 0x5000_0100 to disable register protection.
|  | Refer to the register REGWRPROT at address GCR_BA + 0x100.
|  | Note2: To set PWRCON[1:0], select HXT or LXT crystal clock.
[3:2] | ADC_S | ADC Peripheral Clock Source Selection
|  | 00 = Clock source is from HXT or LXT.
|  | 01 = Reserved.
|  | 10 = Clock source is from HCLK.
|  | 11 = Clock source is from HIRC.
|  | Note: To set PWRCON[1:0], select HXT or LXT crystal clock.
[4] | SPI_S | SPI Clock Source Selection
|  | 0 = Clock source is from HXT or LXT.
|  | 1 = Clock source is from HCLK.
|  | Note: To set PWRCON[1:0], select HXT or LXT crystal clock.
[10:8] | TMR0_S | TIMER0 Clock Source Selection
|  | 000 = Clock source is from HXT or LXT.
|  | 001 = Clock source is from LIRC.
|  | 010 = Clock source is from HCLK.
|  | 011 = Clock source is from external trigger.
|  | 111 = Clock source is from HIRC.
|  | Others = Reserved.
|  | Note: To set PWRCON[1:0], select HXT or LXT crystal clock.
[14:12] | TMR1_S | TIMER1 Clock Source Selection
|  | 000 = Clock source is from HXT or LXT.
|  | 001 = Clock source is from LIRC.
|  | 010 = Clock source is from HCLK.
|  | 011 = Clock source is from external trigger.
|  | 111 = Clock source is from HIRC.
|  | Others = Reserved.
|  | Note: To set PWRCON[1:0], select HXT or LXT crystal clock.
[25:24] | UART_S | UART Clock Source Selection
|  | 00 = Clock source is from HXT or LXT.
|  | 01 = Reserved.
|  | 10 = Clock source is from HIRC.
|  | 11 = Clock source is from HIRC .
|  | Note: To set PWRCON[1:0], select HXT or LXT crystal clock.

Definition at line 849 of file Mini51Series.h.

## ◆ CLKSEL2

CLK_T::CLKSEL2

## Offset: 0x1C Clock Source Select Control Register 2

Bits | Field | Descriptions
--- | --- | ---
[3:2] | FRQDIV_S | Clock Divider Clock Source Selection
|  | 00 = Clock source is from HXT or LXT.
|  | 01 = Reserved.
|  | 10 = Clock source is from HCLK.
|  | 11 = Clock source is from HIRC.
|  | Note: To set PWRCON[1:0], select HXT or LXT crystal clock.

Definition at line 851 of file Mini51Series.h.

## ◆ CLKSTATUS

CLK_T::CLKSTATUS

## Offset: 0x0C Clock Status Monitor Register

Bits | Field | Descriptions
--- | --- | ---
[0] | XTL_STB | HXT Or LXT Clock Source Stable Flag
|  | 0 = HXT or LXT clock is not stable or disabled.
|  | 1 = HXT or LXT clock is stable.
[3] | OSC10K_STB | LIRC Clock Source Stable Flag (Read Only)
|  | 0 = LIRC clock is not stable or disabled.
|  | 1 = LIRC clock is stable.
[4] | OSC22M_STB | HIRC Clock Source Stable Flag (Read Only)
|  | 0 = HIRC clock is not stable or disabled.
|  | 1 = HIRC clock is stable.
[7] | CLK_SW_FAIL | Clock Switch Fail Flag
|  | 0 = Clock switching success.
|  | 1 = Clock switching failed.
|  | Note1: This bit is updated when software switches system clock source.
|  | If switch target clock is stable, this bit will be set to 0.
|  | If switch target clock is not stable, this bit will be set to 1.
|  | Note2: This bit is read only.
|  | After selected clock source is stable, hardware will switch system clock to selected clock automatically, and CLK_SE_FAIL will be cleared automatically by hardware.

Definition at line 847 of file Mini51Series.h.

## ◆ CMPCR

ACMP_T::CMPCR

## Offset: 0x00 Analog Comparator 0 Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | ACMPEN | Analog Comparator Enable Control
|  | 0 = Analog Comparator Disabled.
|  | 1 = Analog Comparator Enabled.
|  | Note: Analog comparator output needs to wait 2 us stable time after this bit is set.
[1] | ACMPIE | Analog Comparator 0 Interrupt Enable Control
|  | 0 = Interrupt function Disabled.
|  | 1 = Interrupt function Enabled.
[2] | HYSEN | Analog Comparator Hysteresis Enable Control
|  | 0 = Hysteresis function Disabled.
|  | 1 = Hysteresis function Enabled.
[4] | NEGSEL | Analog Comparator Negative Input Selection
|  | 0 = The source of the negative comparator input is from CPN pin.
|  | 1 = The source of the negative comparator input is from internal band-gap voltage or comparator reference voltage.
[8] | RISING | Analog Comparator Rising Edge Trigger Enable Control
|  | 0 = Analog comparator rising edge trigger Disabled.
|  | 1 = Analog comparator rising edge trigger PWM or Timer Enabled.
|  | Note: The bit is only effective while analog comparator triggers PWM or Timer.
[9] | FALLING | Analog Comparator Falling Edge Trigger Enable Control
|  | 0 = Analog comparator falling edge trigger Disabled.
|  | 1 = Analog comparator falling edge trigger PWM or Timer Enabled.
|  | Note: The bit is only effective while analog comparator triggers PWM or Timer.
[30:29] | CPPSEL | Analog Comparator Positive Input Selection

Definition at line 226 of file Mini51Series.h.

## ◆ CMPRVCR

ACMP_T::CMPRVCR

## Offset: 0x0C Analog Comparator Reference Voltage Control Register

Bits | Field | Descriptions
--- | --- | ---
[3:0] | CRVS | Comparator Reference Voltage Setting
|  | Comparator reference voltage = AVDD * (1 / 6 + CRVS[3:0] / 24).
[7] | OUT_SEL | CRV Module Output Selection
|  | 0 = Band-gap voltage.
|  | 1 = Internal comparator reference voltage.

Definition at line 228 of file Mini51Series.h.

## ◆ CMPSR

ACMP_T::CMPSR

## Offset: 0x08 Analog Comparator 0/1 Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | ACMPF0 | Analog Comparator 0 Flag
|  | This bit is set by hardware whenever the comparator 0 output changes state.
|  | This will generate an interrupt if ACMPIE(ACMP_CR0[1]) = 1.
|  | 0 = Analog comparator 0 output does not change.
|  | 1 = Analog comparator 0 output changed.
|  | Note: Software can write 1 to clear this bit to 0.
[1] | ACMPF1 | Analog Comparator 1 Flag
|  | This bit is set by hardware whenever the comparator 1 output changes state.
|  | This will generate an interrupt if ACMPIE(ACMP_CR1[1]) = 1.
|  | 0 = Analog comparator 1 output does not change.
|  | 1 = Analog comparator 1 output changed.
|  | Note: Software can write 1 to clear this bit to 0.
[2] | ACMPO0 | Analog Comparator 0 Output
|  | Synchronized to the APB clock to allow reading by software.
|  | Cleared when the comparator 0 is disabled ACMPEN(ACMP_CR0[0]) = 0.
|  | 0 = Analog comparator 0 outputs 0.
|  | 1 = Analog comparator 0 outputs 1.
[3] | ACMPO1 | Analog Comparator 1 Output
|  | Synchronized to the APB clock to allow reading by software.
|  | Cleared when the comparator 1 is disabled ACMPEN(ACMP_CR1[0]) = 0.
|  | 0 = Analog comparator 1 outputs 0.
|  | 1 = Analog comparator 1 outputs 1.

Definition at line 227 of file Mini51Series.h.

## ◆ CMR

PWM_T::CMR

## Offset: 0x24 ~ 0x38 PWM Comparator Register

Bits | Field | Descriptions
--- | --- | ---
[15:0] | CMRn | PWM Comparator Bits
|  | CMR determines the PWM duty. n = 0, 1..5.
|  | Edge-aligned mode:
|  | PWM frequency = HCLK/((prescale+1)*(clock divider))/(CNRn+1); where xy, could be 01, 23, 45 depending on the selected PWM channel.
|  | Duty ratio = (CMRn+1)/(CNRn+1).
|  | CMRn >= CNRn: PWM output is always high.
|  | CMRn < CNRn: PWM low width = (CNRn-CMRn) unit; PWM high width = (CMR+1) unit.
|  | CMRn = 0: PWM low width = (CNRn) unit; PWM high width = 1 unit.
|  | Center-aligned mode:
|  | PWM frequency = HCLK/((prescale+1)*(clock divider)) /(2*CNRn+1); where xy, could be 01, 23, 45 depending on the selected PWM channel.
|  | Duty ratio = (CNRn - CMRn)/(CNRn+1).
|  | CMRn >= CNRn: PWM output is always low.
|  | CMRn < CNRn: PWM low width = (CMRn + 1) * 2 unit; PWM high width = (CNRn - CMRn) * 2 unit.
|  | CMRn = 0: PWM low width = 2 unit; PWM high width = (CNRn) * 2 unit.
|  | (Unit = One PWM clock cycle).
|  | Note: Any write to CMRn will take effect in next PWM cycle.

Definition at line 3559 of file Mini51Series.h.

## ◆ CNR

PWM_T::CNR

## Offset: 0x0C ~ 0x20 PWM Counter Register

Bits | Field | Descriptions
--- | --- | ---
[15:0] | CNRn | PWM Counter/Timer Loaded Value
|  | CNRn determines the PWM period. n = 0, 1..5.
|  | Edge-aligned mode:
|  | PWM frequency = HCLK/((prescale+1)*(clock divider))/(CNRn+1); where xy, could be 01, 23, 45 depending on the selected PWM channel.
|  | Duty ratio = (CMRn+1)/(CNRn+1).
|  | CMRn >= CNRn: PWM output is always high.
|  | CMRn < CNRn: PWM low width = (CNRn-CMRn) unit; PWM high width = (CMR+1) unit.
|  | CMRn = 0: PWM low width = (CNRn) unit; PWM high width = 1 unit.
|  | Center-aligned mode:
|  | PWM frequency = HCLK/((prescale+1)*(clock divider))/ (2*CNRn+1); where xy, could be 01, 23, 45 depending on the selected PWM channel.
|  | Duty ratio = (CNRn - CMRn)/(CNRn+1).
|  | CMRn >= CNRn: PWM output is always low.
|  | CMRn < CNRn: PWM low width = (CMRn + 1) * 2 unit; PWM high width = (CNRn - CMRn) * 2 unit.
|  | CMRn = 0: PWM low width = 2 unit; PWM high width = (CNRn) * 2 unit.
|  | (Unit = One PWM clock cycle).
|  | Note: Any write to CNRn will take effect in next PWM cycle.

Definition at line 3558 of file Mini51Series.h.

## ◆ CNTRL

SPI_T::CNTRL

## Offset: 0x00 SPI Control and Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | GO_BUSY | SPI Transfer Control Bit And Busy Status
|  | If FIFO mode is enabled, this bit will be controlled by hardware and is Read only.
|  | If FIFO mode is disabled, during the data transfer, this bit keeps the value of 1.
|  | As the transfer is finished, this bit will be cleared automatically.
|  | 0 = Writing 0 to this bit to stop data transfer if SPI is transferring.
|  | 1 = In Master mode, writing 1 to this bit to start the SPI data transfer; in Slave mode, writing 1 to this bit indicates that the slave is ready to communicate with a master.
|  | Note 1: When FIFO mode is disabled, all configurations should be ready before writing 1 to the GO_BUSY bit.
|  | Note 2: In SPI Slave mode, if FIFO mode is disabled and the SPI bus clock is kept at idle state during a data transfer, the GO_BUSY bit will not be cleared to 0 when slave select signal goes to inactive state.
[1] | RX_NEG | Receive On Negative Edge
|  | 0 = The received data input signal latched on the Rising edge of SPICLK.
|  | 1 = The received data input signal latched on the Falling edge of SPICLK.
[2] | TX_NEG | Transmit On Negative Edge
|  | 0 = The transmitted data output signal is driven on the Rising edge of SPICLK.
|  | 1 = The transmitted data output signal is driven on the Falling edge of SPICLK.
[7:3] | TX_BIT_LEN | Transmit Bit Length
|  | This field specifies how many bits are transmitted in one transmit/receive.
|  | The minimum bit length is 8 bits and can up to 32 bits.
|  | TX_BIT_LEN = 0x08 ... 8 bits.
|  | TX_BIT_LEN = 0x09 ... 9 bits.
|  | .....
|  | TX_BIT_LEN = 0x1F ... 31 bits.
|  | TX_BIT_LEN = 0x00 ... 32 bits.
[10] | LSB | LSB First
|  | 0 = The MSB is transmitted/received first.
|  | 1 = The LSB is transmitted/received first.
[11] | CLKP | Clock Polarity
|  | 0 = SPICLK idle low.
|  | 1 = SPICLK idle high.
[15:12] | SP_CYCLE | Suspend Interval (Master Only)
|  | The four bits provide configurable suspend interval between two successive transactions in a transfer.
|  | The definition of the suspend interval is the interval between the last clock edge of the preceding transaction word and the first clock edge of the following transaction word.
|  | The default value is 0x3.
|  | The period of the suspend interval is obtained according to the following equation:
|  | (SP_CYCLE[3:0] + 0.5) * period of SPICLK clock cycle
|  | Example:
|  | SP_CYCLE = 0x0 ... 0.5 SPICLK clock cycle.
|  | SP_CYCLE = 0x1 ... 1.5 SPICLK clock cycle.
|  | .....
|  | SP_CYCLE = 0xE ... 14.5 SPICLK clock cycle.
|  | SP_CYCLE = 0xF ... 15.5 SPICLK clock cycle.
[16] | IF | Unit-transfer Interrupt Flag
|  | 0 = The transfer does not finish yet.
|  | 1 = The SPI controller has finished one unit transfer.
|  | Note 1: This bit will be cleared by writing 1 to itself.
|  | Note 2: It's a mutual mirror bit of SPI_STATUS[16].
[17] | IE | Unit-transfer Interrupt Enable Control
|  | 0 = SPI unit-transfer interrupt Disabled.
|  | 1 = SPI unit-transfer interrupt Enabled.
[18] | SLAVE | Slave Mode Control
|  | 0 = Master mode.
|  | 1 = Slave mode.
[19] | REORDER | Byte Reorder Function
|  | 0 = Byte reorder function Disabled.
|  | 1 = Byte reorder function Enabled.
|  | Note: This setting is only available if TX_BIT_LEN is defined as 16, 24, and 32 bits.
[21] | FIFO | FIFO Mode Enable Control
|  | 0 = FIFO Mode Disabled.
|  | 1 = FIFO Mode Enabled.
|  | Note 1: Before enabling FIFO mode, the other related settings should be set in advance.
|  | Note 2: In Master mode, if the FIFO mode is enabled, the GO_BUSY bit will be set to 1 automatically after writing data into the 4-depth transmit FIFO.
|  | When all data stored at transmit FIFO buffer are transferred, the GO_BUSY bit will back to 0.
[24] | RX_EMPTY | Receive FIFO Buffer Empty Indicator (Read Only)
|  | 0 = The receive FIFO buffer is not empty.
|  | 1 = The receive FIFO buffer is empty.
|  | Note: It's a mutual mirror bit of SPI_CNTRL[24].
[25] | RX_FULL | Receive FIFO Buffer Full Indicator (Read Only)
|  | 0 = The receive FIFO buffer is not full.
|  | 1 = The receive FIFO buffer is full.
|  | Note: It's a mutual mirror bit of SPI_STATUS[25]
[26] | TX_EMPTY | Transmit FIFO Buffer Empty Indicator (Read Only)
|  | 0 = The transmit FIFO buffer is not empty.
|  | 1 = The transmit FIFO buffer is empty.
|  | Note: It's a mutual mirror bit of SPI_STAUTS[26].
[27] | TX_FULL | Transmit FIFO Buffer Full Indicator (Read Only)
|  | 0 =The transmit FIFO buffer is not full.
|  | 1 =The transmit FIFO buffer is full.
|  | Note: It's a mutual mirror bit of SPI_STATUS[27].

Definition at line 4473 of file Mini51Series.h.

## ◆ CNTRL2

SPI_T::CNTRL2

## Offset: 0x3C SPI Control and Status Register 2

Bits | Field | Descriptions
--- | --- | ---
[8] | NOSLVSEL | Slave 3-wire Mode Enable Control (Slave Only)
|  | The SPI controller work with 3-wire interface including SPICLK, SPI_MISO, and SPI_MOSI
|  | 0 = The controller is 4-wire bi-direction interface.
|  | 1 = The controller is 3-wire bi-direction interface in Slave mode.
|  | The controller will be ready to transmit/receive data after the GO_BUSY bit is set to 1.
|  | Note: In Slave 3-wire mode, the SS_LTRIG bit (SPI_SSR[4]) shall be set as 1.
[9] | SLV_ABORT | Slave 3-wire Mode Abort Control Bit (Slave Only)
|  | In normal operation, there is an interrupt event when the number of received bits meets the requirement which defined in TX_BIT_LEN.
|  | If the number of received bits is less than the requirement and there is no more bus clock input over one transfer time in Slave 3-wire mode, user can set this bit to force the current transfer done and then user can get a unit transfer interrupt event.
|  | 0 = No force the transfer done when the NOSLVSEL bit is set to 1.
|  | 1 = Force the transfer done when the NOSLVSEL bit is set to 1.
|  | Note: This bit will be cleared to 0 automatically by hardware after it is set to 1 by software.
[10] | SSTA_INTEN | Slave 3-wire Mode Start Interrupt Enable Control (Slave Only)
|  | It is used to enable interrupt when the transfer has started in slave 3-wire mode.
|  | If there is no transfer done interrupt over the time period which is defined by user after the transfer start, user can set the SLV_ABORT bit to force the transfer done.
|  | 0 = Transaction start interrupt Disabled.
|  | 1 = Transaction start interrupt Enabled.
|  | Note: It will be cleared to 0 as the current transfer is done or the SLV_START_INTSTS bit is cleared to 0.
[11] | SLV_START_INTSTS | Slave 3-wire Mode Start Interrupt Status (Slave Only)
|  | This bit dedicates if a transaction has started in slave 3-wire mode.
|  | 0 = Slave does not detect any SPI bus clock transfer since the SSTA_INTEN bit was set to 1.
|  | 1 = The transfer has started in slave 3-wire mode.
|  | Note 1: It will be cleared automatically when a transaction is done or by writing 1 to this bit.
|  | Note 2: It is a mutual mirror bit of SPI_STATUS[11].
[16] | SS_INT_OPT | Slave Select Inactive Interrupt Option (Slave Only)
|  | 0 = As the slave select signal goes to inactive level, the IF bit will NOT be set to 1.
|  | 1 = As the slave select signal goes to inactive level, the IF bit will be set to 1.
|  | Note: This setting is only available if the SPI controller is configured as level trigger in slave device.
[31] | BCn | Clock Configuration Backward Compatible Option
|  | 0 = The clock configuration is backward compatible.
|  | 1 = The clock configuration is not backward compatible.
|  | Note: Refer to the description of SPI_DIVIDER register for details.

Definition at line 4487 of file Mini51Series.h.

## ◆ CSR

PWM_T::CSR

## Offset: 0x04 PWM Clock Select Register

Bits | Field | Descriptions
--- | --- | ---
[2:0] | CSR0 | Timer 0 Clock Source Selection
|  | Select clock input for PWM timer.
|  | (Table is the same as CSR5.)
[6:4] | CSR1 | Timer 1 Clock Source Selection
|  | Select clock input for PWM timer.
|  | (Table is the same as CSR5.)
[10:8] | CSR2 | Timer 2 Clock Source Selection
|  | Select clock input for PWM timer.
|  | (Table is the same as CSR5.)
[14:12] | CSR3 | Timer 3 Clock Source Selection
|  | Select clock input for PWM timer.
|  | (Table is the same as CSR5.)
[18:16] | CSR4 | Timer 4 Clock Source Selection
|  | Select clock input for PWM timer.
|  | (Table is the same as CSR5.)
[22:20] | CSR5 | Timer 5 Clock Source Selection
|  | Select clock input for PWM timer.
|  | 000 = Input Clock Divided by 2.
|  | 001 = Input Clock Divided by 4.
|  | 010 = Input Clock Divided by 8.
|  | 011 = Input Clock Divided by 16.
|  | 100 = Input Clock Divided by 1.

Definition at line 3556 of file Mini51Series.h.

## ◆ DBEN

GPIO_T::DBEN

## Offset: 0x14 Px De-bounce Enable Control

Bits | Field | Descriptions
--- | --- | ---
[7:0] | DBEN | Port 0-5 Pin [N] Input Signal De-bounce Enable Control
|  | DBEN[n] bit is used to enable the de-bounce function for each corresponding bit.
|  | If the input signal pulse width cannot be sampled by continuous two de-bounce sample cycle, the input signal transition is seen as the signal bounce and will not trigger the interrupt.
|  | The de-bounce clock source is controlled by DBNCECON[4], one de-bounce sample cycle period is controlled by DBNCECON[3:0].
|  | 0 = Px.n de-bounce function Disabled.
|  | 1 = Px.n de-bounce function Enabled.
|  | The de-bounce function is valid only for edge triggered interrupt.
|  | If the interrupt mode is level triggered, the de-bounce enable bit is ignored.
|  | Note1: x = 0~5, n = 0~7.
|  | Note2: If Px.n pin is chosen as Power-down wake-up source, user should be disable the de-bounce function before entering Power-down mode to avoid the second interrupt event occurred after system woken up caused by the Px.n de-bounce function.
|  | Note3:
|  | P0_DBEN[3:2] are reserved.
|  | P1_DBEN[7:6], [1] are reserved.
|  | P2_DBEN[7], [1:0] are reserved.
|  | P3_DBEN[7], [3] are reserved.
|  | P4_DBEN[5:0] are reserved.
|  | P5_DBEN[7:6] are reserved.

Definition at line 2079 of file Mini51Series.h.

## ◆ DBNCECON

GPIO_DBNCECON_T::DBNCECON

## Offset: 0x180 Interrupt De-bounce Control

Bits | Field | Descriptions
--- | --- | ---
[3:0] | DBCLKSEL | De-bounce Sampling Cycle Selection
|  | 0000 = Sample interrupt input once per 1 clock.
|  | 0001 = Sample interrupt input once per 2 clocks.
|  | 0010 = Sample interrupt input once per 4 clocks.
|  | 0011 = Sample interrupt input once per 8 clocks.
|  | 0100 = Sample interrupt input once per 16 clocks.
|  | 0101 = Sample interrupt input once per 32 clocks.
|  | 0110 = Sample interrupt input once per 64 clocks.
|  | 0111 = Sample interrupt input once per 128 clocks.
|  | 1000 = Sample interrupt input once per 256 clocks.
|  | 1001 = Sample interrupt input once per 2*256 clocks.
|  | 1010 = Sample interrupt input once per 4*256 clocks.
|  | 1011 = Sample interrupt input once per 8*256 clocks.
|  | 1100 = Sample interrupt input once per 16*256 clocks.
|  | 1101 = Sample interrupt input once per 32*256 clocks.
|  | 1110 = Sample interrupt input once per 64*256 clocks.
|  | 1111 = Sample interrupt input once per 128*256 clocks.
[4] | DBCLKSRC | De-bounce Counter Clock Source Selection
|  | 0 = De-bounce counter clock source is the HCLK.
|  | 1 = De-bounce counter clock source is the 10 kHz internal low speed oscillator.
[5] | ICLK_ON | Interrupt Clock On Mode
|  | 0 = Edge detection circuit is active only if I/O pin corresponding Px_IEN bit is set to 1.
|  | 1 = All I/O pins edge detection circuit is always active after reset.
|  | Note: It is recommended to turn off this bit to save system power if no special application concern.

Definition at line 2121 of file Mini51Series.h.

## ◆ DFBADR

FMC_T::DFBADR

## Offset: 0x14 Data Flash Start Address

Bits | Field | Descriptions
--- | --- | ---
[31:0] | DFBA | Data Flash Base Address
|  | This register indicates Data Flash start address. It is a read only register.
|  | The Data Flash start address is defined by user.
|  | Since on chip flash erase unit is 512 bytes, it is mandatory to keep bit 8-0 as 0.

Definition at line 1128 of file Mini51Series.h.

## ◆ DIVIDER

SPI_T::DIVIDER

## Offset: 0x04 SPI Clock Divider Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | DIVIDER | Clock Divider Bits (Master Only)
|  | The value in this field is the frequency divider to determine the SPI peripheral clock frequency fspi, and the SPI master's bus clock frequency on the SPICLK output pin.
|  | The frequency is obtained according to the following equation:
|  | If the bit of BCn, SPI_CNTRL2[31], is set to 0.
|  | else if BCn is set to 1,
|  | where
|  | is the SPI peripheral clock source which is defined in the CLKSEL1 register.

Definition at line 4474 of file Mini51Series.h.

## ◆ DMASK

GPIO_T::DMASK

## Offset: 0x0C Px Data Output Write Mask

Bits | Field | Descriptions
--- | --- | ---
[7:0] | DMASK | Port 0-5 Pin [N] Data Output Write Mask
|  | These bits are used to protect the corresponding Px_DOUT[n] bit.
|  | When the DMASK[n] bit is set to 1, the corresponding Px_DOUT[n] bit is protected.
|  | If the write signal is masked, writing data to the protect bit is ignored.
|  | 0 = Corresponding Px_DOUT[n] bit can be updated.
|  | 1 = Corresponding Px_DOUT[n] bit is protected.
|  | Note1: x = 0~5, n = 0~7.
|  | Note2: This function only protects the corresponding Px_DOUT[n] bit, and will not protect the corresponding Pxn_PDIO bit.
|  | Note3:
|  | P0_DMASK[3:2] are reserved.
|  | P1_DMASK[7:6], [1] are reserved.
|  | P2_DMASK[7], [1:0] are reserved.
|  | P3_DMASK[7], [3] are reserved.
|  | P4_DMASK[5:0] are reserved.
|  | P5_DMASK[7:6] are reserved.

Definition at line 2077 of file Mini51Series.h.

## ◆ DOUT

GPIO_T::DOUT

## Offset: 0x08 Px Data Output Value

Bits | Field | Descriptions
--- | --- | ---
[7:0] | DOUT | Port 0-5 Pin [N] Output Value
|  | Each of these bits controls the status of a Px.n pin when the Px.n is configured as Push-pull output, Open-drain output and Quasi-bidirectional mode.
|  | 0 = Px.n will drive Low if the Px.n pin is configured as Push-pull output, Open-drain output or Quasi-bidirectional mode.
|  | 1 = Px.n will drive High if the Px.n pin is configured as Push-pull output or Quasi-bidirectional mode.
|  | Note1: x = 0~5, n = 0~7.
|  | Note2:
|  | P0_DOUT[3:2] are reserved.
|  | P1_DOUT[7:6], [1] are reserved.
|  | P2_DOUT[7], [1:0] are reserved.
|  | P3_DOUT[7], [3] are reserved.
|  | P4_DOUT[5:0] are reserved.
|  | P5_DOUT[7:6] are reserved.

Definition at line 2076 of file Mini51Series.h.

## ◆ FCR

UART_T::FCR

## Offset: 0x08 UART FIFO Control Register

Bits | Field | Descriptions
--- | --- | ---
[1] | RFR | RX Field Software Reset
|  | When RX_RST is set, all the byte in the receiver FIFO and RX internal state machine are cleared.
|  | 0 = No effect.
|  | 1 = The RX internal state machine and pointers reset.
|  | Note: This bit will auto clear needs at least 3 UART Controller peripheral clock cycles.
[2] | TFR | TX Field Software Reset
|  | When TX_RST is set, all the byte in the transmit FIFO and TX internal state machine are cleared.
|  | 0 = No effect.
|  | 1 = The TX internal state machine and pointers reset.
|  | Note: This bit will auto clear needs at least 3 UART Controller peripheral clock cycles.
[7:4] | RFITL | RX FIFO Interrupt (RDA_INT) Trigger Level
|  | When the number of bytes in the receive FIFO equals the RFITL then the RDA_IF will be set (if RDA_IEN in UA_IER register is enable, an interrupt will generated).
|  | 0000 = RX FIFO Interrupt Trigger Level is 1 byte.
|  | 0001 = RX FIFO Interrupt Trigger Level is 4 bytes.
|  | 0010 = RX FIFO Interrupt Trigger Level is 8 bytes.
|  | 0011 = RX FIFO Interrupt Trigger Level is 14 bytes.
|  | Other = Reserved.
[8] | RX_DIS | Receiver Disable Control
|  | The receiver is disabled or not (setting 1 to disable the receiver).
|  | 0 = Receiver Enabled.
|  | 1 = Receiver Disabled.
|  | Note1: This field is only used for RS-485 Normal Multi-drop mode.
|  | It should be programmed firstly to avoid receiving unknown data before RS-485_NMM (UA_ALT_CSR [8]) is programmed.
|  | Note2: After RS-485 receives an address byte in RS-485 Normal Multi-drop mode, this bit (RX_DIS) will be cleared to "0" by hardware.
[19:16] | RTS_TRI_LEV | RTS Trigger Level (For Auto-flow Control Use)
|  | 0000 = RTS Trigger Level is 1 byte.
|  | 0001 = RTS Trigger Level is 4 bytes.
|  | 0010 = RTS Trigger Level is 8 bytes.
|  | 0011 = RTS Trigger Level is 14 bytes.
|  | Other = Reserved.
|  | Note: This field is used for RTS auto-flow control.

Definition at line 5325 of file Mini51Series.h.

## ◆ FIFO_CTL

SPI_T::FIFO_CTL

## Offset: 0x40 SPI FIFO Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | RX_CLR | Clear Receive FIFO Buffer
|  | 0 = No effect.
|  | 1 = Clear receive FIFO buffer.
|  | Note: This bit will be cleared to 0 by hardware after software sets it to 1 and the receive FIFO is cleared.
[1] | TX_CLR | Clear Transmit FIFO Buffer
|  | 0 = No effect.
|  | 1 = Clear transmit FIFO buffer.
|  | Note: This bit will be cleared to 0 by hardware after software sets it to 1 and the transmit FIFO is cleared.
[2] | RX_INTEN | Receive Threshold Interrupt Enable Control
|  | 0 = Receive threshold interrupt Disabled.
|  | 1 = Receive threshold interrupt Enabled.
[3] | TX_INTEN | Transmit Threshold Interrupt Enable Control
|  | 0 = Transmit threshold interrupt Disabled.
|  | 1 = Transmit threshold interrupt Enabled.
[6] | RXOV_INTEN | Receive FIFO Overrun Interrupt Enable Control
|  | 0 = Receive FIFO overrun interrupt Disabled.
|  | 1 = Receive FIFO overrun interrupt Enabled.
[21] | TIMEOUT_INTEN | Receive FIFO Time-out Interrupt Enable Control
|  | 0 = Time-out interrupt Disabled.
|  | 1 = Time-out interrupt Enabled.
[25:24] | RX_THRESHOLD | Received FIFO Threshold
|  | If the valid data count of the receive FIFO buffer is larger than the RX_THRESHOLD setting, the RX_INTSTS bit will be set to 1, else the RX_INTSTS bit will be cleared to 0.
[29:28] | TX_THRESHOLD | Transmit FIFO Threshold
|  | If the valid data count of the transmit FIFO buffer is less than or equal to the TX_THRESHOLD setting, the TX_INTSTS bit will be set to 1, else the TX_INTSTS bit will be cleared to 0.

Definition at line 4488 of file Mini51Series.h.

## ◆ FRQDIV

CLK_T::FRQDIV

## Offset: 0x24 Frequency Divider Control Register

Bits | Field | Descriptions
--- | --- | ---
[3:0] | FSEL | Divider Output Frequency Selection
|  | The formula of output frequency is
|  | Fout = Fin/2(N+1),.
|  | Fin is the input clock frequency.
|  | Fout is the frequency of divider output clock.
|  | N is the 4-bit value of FSEL[3:0].
[4] | DIVIDER_EN | Frequency Divider Enable Control
|  | 0 = Frequency Divider Disabled.
|  | 1 = Frequency Divider Enabled.
[5] | DIVIDER1 | Frequency Divider 1 Enable Control
|  | 0 = Divider output frequency is depended on FSEL value.
|  | 1 = Divider output frequency is the same as input clock frequency.

Definition at line 855 of file Mini51Series.h.

## ◆ FSR

UART_T::FSR

## Offset: 0x18 UART FIFO Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | RX_OVER_IF | RX Overflow Error Interrupt Flag
|  | This bit is set when RX FIFO overflow.
|  | If the number of bytes of received data is greater than RX_FIFO (UA_RBR) size 16 bytes, this bit will be set.
|  | 0 = RX FIFO is not overflow.
|  | 1 = RX FIFO is overflow.
|  | Note: This bit is cleared by writing 1 to it.
[3] | RS485_ADD_DETF | RS-485 Address Byte Detection Flag
|  | This bit is set to 1 while RS485_ADD_EN (UA_ALT_CSR[15]) is set to 1 to enable Address detection mode and receive detect a data with an address bit (bit 9 = 1).
|  | Note1: This field is used for RS-485 function mode.
|  | Note2: This bit is cleared by writing 1 to it.
[4] | PEF | Parity Error Flag (Read Only)
|  | This bit is set to logic 1 whenever the received character does not have a valid "parity bit".
|  | 0 = No parity error is generated.
|  | 1 = Parity error is generated.Note: This bit is read only, but can be cleared by writing '1' to it .
[5] | FEF | Framing Error Flag (Read Only)
|  | This bit is set to logic 1 whenever the received character does not have a valid "stop bit" (that is, the stop bit follows the last data bit or parity bit is detected as as logic 0).
|  | 0 = No framing error is generated.
|  | 1 = Framing error is generated.
|  | Note: This bit is read only, but can be cleared by writing '1' to it .
[6] | BIF | Break Interrupt Flag (Read Only)
|  | This bit is set to logic 1 whenever the received data input (RX) is held in the "spacing state" (logic 0) for longer than a full word transmission time (that is, the total time of "start bit" + data bits + parity + stop bits).
|  | 0 = No Break interrupt is generated.
|  | 1 = Break interrupt is generated.
|  | Note: This bit is read only, but software can write 1 to clear it.
[13:8] | RX_POINTER | RX FIFO Pointer (Read Only)
|  | This field indicates the RX FIFO Buffer Pointer.
|  | When UART receives one byte from external device, RX_POINTER increases one.
|  | When one byte of RX FIFO is read by CPU, RX_POINTER decreases one.
|  | The Maximum value shown in RX_POINTER is 15.
|  | When the using level of RX FIFO Buffer equal to 16, the RX_FULL bit is set to 1 and RX_POINTER will show 0.
|  | As one byte of RX FIFO is read by CPU, the RX_FULL bit is cleared to 0 and RX_POINTER will show 15.
[14] | RX_EMPTY | Receiver FIFO Empty (Read Only)
|  | This bit initiate RX FIFO empty or not.
|  | 0 = RX FIFO is not empty.
|  | 1 = RX FIFO is empty.
|  | Note: When the last byte of RX FIFO has been read by CPU, hardware sets this bit high.
|  | It will be cleared when UART receives any new data.
[15] | RX_FULL | Receiver FIFO Full (Read Only)
|  | This bit initiates RX FIFO full or not.
|  | 0 = RX FIFO is not full.
|  | 1 = RX FIFO is full.
|  | Note: This bit is set when the number of usage in RX FIFO Buffer is equal to 16, otherwise is cleared by hardware.
[21:16] | TX_POINTER | TX FIFO Pointer (Read Only)
|  | This field indicates the TX FIFO Buffer Pointer.
|  | When CPU writes one byte into UA_THR, TX_POINTER increases one.
|  | When one byte of TX FIFO is transferred to Transmitter Shift Register, TX_POINTER decreases one.
|  | The Maximum value shown in TX_POINTER is 15.
|  | When the using level of TX FIFO Buffer equal to 16, the TX_FULL bit is set to 1 and TX_POINTER will show 0.
|  | As one byte of TX FIFO is transferred to Transmitter Shift Register, the TX_FULL bit is cleared to 0 and TX_POINTER will show 15.
[22] | TX_EMPTY | Transmitter FIFO Empty (Read Only)
|  | This bit indicates TX FIFO is empty or not.
|  | 0 = TX FIFO is not empty.
|  | 1 = TX FIFO is empty.
|  | Note: When the last byte of TX FIFO has been transferred to Transmitter Shift Register, hardware sets this bit high.
|  | It will be cleared when writing data into THR (TX FIFO not empty).
[23] | TX_FULL | Transmitter FIFO Full (Read Only)
|  | This bit indicates TX FIFO full or not.
|  | 0 = TX FIFO is not full.
|  | 1 = TX FIFO is full.
|  | Note: This bit is set when the number of usage in TX FIFO Buffer is equal to 16, otherwise is cleared by hardware.
[24] | TX_OVER_IF | TX Overflow Error Interrupt Flag
|  | If TX FIFO (UA_THR) is full, an additional write to UA_THR will cause this bit to logic 1.
|  | 0 = TX FIFO is not overflow.
|  | 1 = TX FIFO is overflow.
|  | Note: This bit is cleared by writing 1 to it.
[28] | TE_FLAG | Transmitter Empty Flag (Read Only)
|  | This bit is set by hardware when TX FIFO (UA_THR) is empty and the STOP bit of the last byte has been transmitted.
|  | 0 = TX FIFO is not empty.
|  | 1 = TX FIFO is empty and the STOP bit of the last byte has been transmitted.
|  | Note: This bit is cleared automatically when TX FIFO is not empty or the last byte transmission has not completed.

Definition at line 5329 of file Mini51Series.h.

## ◆ FUN_SEL

UART_T::FUN_SEL

## Offset: 0x30 UART Function Select Register

Bits | Field | Descriptions
--- | --- | ---
[1:0] | FUN_SEL | Function Selection
|  | 00 = UART function mode.
|  | 01 = Reserved.
|  | 10 = IrDA function mode.
|  | 11 = RS-485 function mode.

Definition at line 5335 of file Mini51Series.h.

## ◆ I2CADDR0

I2C_T::I2CADDR0

## Offset: 0x04 I2C Slave Address Register 0

Bits | Field | Descriptions
--- | --- | ---
[0] | GC | General Call Function
|  | 0 = General Call Function Disabled.
|  | 1 = General Call Function Enabled.
[7:1] | I2CADDR | I2C Address Bits
|  | The content of this register is irrelevant when I2C is in Master mode.
|  | In Slave mode, the seven most significant bits must be loaded with the MCU's own address.
|  | The I2C hardware will react if either of the address is matched.

Definition at line 2410 of file Mini51Series.h.

## ◆ I2CADDR1

I2C_T::I2CADDR1

## Offset: 0x18 I2C Slave Address Register 1

Bits | Field | Descriptions
--- | --- | ---
[0] | GC | General Call Function
|  | 0 = General Call Function Disabled.
|  | 1 = General Call Function Enabled.
[7:1] | I2CADDR | I2C Address Bits
|  | The content of this register is irrelevant when I2C is in Master mode.
|  | In Slave mode, the seven most significant bits must be loaded with the MCU's own address.
|  | The I2C hardware will react if either of the address is matched.

Definition at line 2415 of file Mini51Series.h.

## ◆ I2CADDR2

I2C_T::I2CADDR2

## Offset: 0x1C I2C Slave Address Register 2

Bits | Field | Descriptions
--- | --- | ---
[0] | GC | General Call Function
|  | 0 = General Call Function Disabled.
|  | 1 = General Call Function Enabled.
[7:1] | I2CADDR | I2C Address Bits
|  | The content of this register is irrelevant when I2C is in Master mode.
|  | In Slave mode, the seven most significant bits must be loaded with the MCU's own address.
|  | The I2C hardware will react if either of the address is matched.

Definition at line 2416 of file Mini51Series.h.

## ◆ I2CADDR3

I2C_T::I2CADDR3

## Offset: 0x20 I2C Slave Address Register 3

Bits | Field | Descriptions
--- | --- | ---
[0] | GC | General Call Function
|  | 0 = General Call Function Disabled.
|  | 1 = General Call Function Enabled.
[7:1] | I2CADDR | I2C Address Bits
|  | The content of this register is irrelevant when I2C is in Master mode.
|  | In Slave mode, the seven most significant bits must be loaded with the MCU's own address.
|  | The I2C hardware will react if either of the address is matched.

Definition at line 2417 of file Mini51Series.h.

## ◆ I2CADM0

I2C_T::I2CADM0

## Offset: 0x24 I2C Slave Address Mask Register 0

Bits | Field | Descriptions
--- | --- | ---
[7:1] | I2CADM | I2C Address Mask Bits
|  | 0 = I2C address mask Disabled (the received corresponding register bit should be exactly the same as address register).
|  | 1 = I2C address mask Enabled (the received corresponding address bit is "Don't care").

Definition at line 2418 of file Mini51Series.h.

## ◆ I2CADM1

I2C_T::I2CADM1

## Offset: 0x28 I2C Slave Address Mask Register 1

Bits | Field | Descriptions
--- | --- | ---
[7:1] | I2CADM | I2C Address Mask Bits
|  | 0 = I2C address mask Disabled (the received corresponding register bit should be exactly the same as address register).
|  | 1 = I2C address mask Enabled (the received corresponding address bit is "Don't care").

Definition at line 2419 of file Mini51Series.h.

## ◆ I2CADM2

I2C_T::I2CADM2

## Offset: 0x2C I2C Slave Address Mask Register 2

Bits | Field | Descriptions
--- | --- | ---
[7:1] | I2CADM | I2C Address Mask Bits
|  | 0 = I2C address mask Disabled (the received corresponding register bit should be exactly the same as address register).
|  | 1 = I2C address mask Enabled (the received corresponding address bit is "Don't care").

Definition at line 2420 of file Mini51Series.h.

## ◆ I2CADM3

I2C_T::I2CADM3

## Offset: 0x30 I2C Slave Address Mask Register 3

Bits | Field | Descriptions
--- | --- | ---
[7:1] | I2CADM | I2C Address Mask Bits
|  | 0 = I2C address mask Disabled (the received corresponding register bit should be exactly the same as address register).
|  | 1 = I2C address mask Enabled (the received corresponding address bit is "Don't care").

Definition at line 2421 of file Mini51Series.h.

## ◆ I2CDAT

I2C_T::I2CDAT

## Offset: 0x08 I2C DATA Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | I2CDAT | I2C Data Bits
|  | Bit [7:0] is located with the 8-bit transferred data of the I2C serial port.

Definition at line 2411 of file Mini51Series.h.

## ◆ I2CLK

I2C_T::I2CLK

## Offset: 0x10 I2C Clock Divided Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | I2CLK | I2C Clock Divided Bits
|  | The I2C clock rate bits: Data Baud Rate of I2C = (system clock) / (4x (I2CLK+1)).
|  | Note: The minimum value of I2CLK is 4.

Definition at line 2413 of file Mini51Series.h.

## ◆ I2CON

I2C_T::I2CON

## Offset: 0x00 I2C Control Register

Bits | Field | Descriptions
--- | --- | ---
[2] | AA | Assert Acknowledge Control Bit
|  | When AA=1 is prior to address or data received, an acknowledged (low level to SDA) will be returned during the acknowledge clock pulse on the SCL line when 1.) A slave is acknowledging the address sent from master, 2.) The receiver devices are acknowledging the data sent by transmitter.
|  | When AA=0 prior to address or data received, a Not acknowledged (high level to SDA) will be returned during the acknowledge clock pulse on the SCL line.
[3] | SI | I2C Interrupt Flag
|  | When a new I2C state is present in the I2CSTATUS register, the SI flag is set by hardware, and if bit EI (I2CON[7]) is set, the I2C interrupt is requested.
|  | SI must be cleared by software.
|  | Software can write 1 to clear this bit.
[4] | STO | I2C STOP Control Bit
|  | In Master mode, setting STO to transmit a STOP condition to bus then I2C hardware will check the bus condition if a STOP condition is detected this bit will be cleared by hardware automatically.
|  | In Slave mode, setting STO resets I2C hardware to the defined "not addressed" Slave mode.
|  | This means it is NO LONGER in the Slave receiver mode to receive data from the master transmit device.
[5] | STA | I2C START Control Bit
|  | Setting STA to logic 1 to enter Master mode.
|  | I2C hardware sends a START or repeats the START condition to bus when the bus is free.
[6] | ENS1 | I2C Controller Enable Control
|  | 0 = I2C Controller Disabled.
|  | 1 = I2C Controller Enabled.
|  | Set to enable I2C serial function controller.
|  | When ENS1=1 the I2C serial function enables.
|  | The function of multi-function pin must be set to I2C first.
[7] | EI | Interrupt Enable Control
|  | 0 = I2C interrupt Disabled.
|  | 1 = I2C interrupt Enabled.

Definition at line 2409 of file Mini51Series.h.

## ◆ I2CON2

I2C_T::I2CON2

## Offset: 0x3C I2C Control Register 2

Bits | Field | Descriptions
--- | --- | ---
[0] | WAKEUPEN | Wake-up Enable Control
|  | 0 = I2C wake-up function Disabled.
|  | 1 = I2C wake-up function Enabled.
|  | The system can be wake-up by I2C bus when the system is set into power mode and the received data matched one of the addresses in Address Register.
[1] | TWOFF_EN | TWO LEVEL FIFO Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Set to enable the two-level FIFO for I2C transmitted or received buffer.
|  | It is used to improve the performance of the I2C bus.
|  | If this bit is set = 1, the control bit of STA for repeat start or STO bit should be set after the current SI is clear.
|  | For example: if there are 4 data shall be transmitted and then stop it.
|  | The STO bit shall be set after the 3rd data's SI event being clear.
|  | In this time, the 4th data can be transmitted and the I2C stop after the 4th data transmission done.
[2] | NOSTRETCH | NO STRETCH The I2C BUS
|  | 0 = The I2C SCL bus is stretched by hardware if the SI is not cleared in master mode.
|  | 1 = The I2C SCL bus is not stretched by hardware if the SI is not cleared in master mode.
[3] | OVER_INTEN | I2C OVER RUN Interrupt Control Bit
|  | Setting OVER_INTEN to enable will send a interrupt to system when the TWOFF bit is enabled and there is over run event in received FIFO.
|  | 0 = Disabled.
|  | 1 = Enabled.
[4] | UNDER_INTEN | I2C UNDER RUN Interrupt Control Bit
|  | Setting UNDER_INTEN to enable will send a interrupt to system when the TWOFF bit is enabled and there is under run event happened in transmitted FIFO.
|  | 0 = Disabled.
|  | 1 = Enabled.

Definition at line 2425 of file Mini51Series.h.

## ◆ I2CSTATUS

I2C_T::I2CSTATUS

## Offset: 0x0C I2C Status Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | I2CSTATUS | I2C Status Bits
|  | The three least significant bits are always 0.
|  | The five most significant bits contain the status code.
|  | There are 26 possible status codes.
|  | When I2CSTATUS contains F8H, no serial interrupt is requested.
|  | All the other I2CSTATUS values correspond to defined I2C states.
|  | When each of these states is entered, a status interrupt is requested (SI = 1).
|  | A valid status code is present in I2CSTATUS one cycle after SI is set by hardware and is still present one cycle after SI has been reset by software.
|  | In addition, the states 00H stands for a Bus Error.
|  | A Bus Error occurs when a START or STOP condition is present at an illegal position in the formation frame.
|  | Examples of illegal position are during the serial transfer of an address byte, a data byte or an acknowledge bit.

Definition at line 2412 of file Mini51Series.h.

## ◆ I2CSTATUS2

I2C_T::I2CSTATUS2

## Offset: 0x40 I2C Status Register 2

Bits | Field | Descriptions
--- | --- | ---
[0] | WAKEUP | I2C Wake-up Interrupt Flag
|  | When chip is woken up from Power-Down mode by I2C, this bit is set to 1.
|  | Software can write 1 to clear this bit.
[1] | FULL | I2C TWO LEVEL FIFO FULL
|  | This bit indicates TX FIFO full or not when the TWOFF_EN = 1.
[2] | EMPTY | I2C TWO LEVEL FIFO EMPTY
|  | This bit indicates RX FIFO empty or not when the TWOFF_EN = 1.
[3] | OVERUN | I2C OVER RUN Status Bit
|  | This bit indicates the received FIFO is over run when the TWOFF_EN = 1.
[4] | UNDERUN | I2C UNDER RUN Status Bit
|  | This bit indicates the transmitted FIFO is under run when the TWOFF_EN = 1.

Definition at line 2426 of file Mini51Series.h.

## ◆ I2CTOC

I2C_T::I2CTOC

## Offset: 0x14 I2C Time-Out Counter Register

Bits | Field | Descriptions
--- | --- | ---
[0] | TIF | Time-out Flag
|  | This bit is set by hardware when I2C time-out happened and it can interrupt CPU if I2C interrupt enable bit (EI) is set to 1.
|  | Note: Software can write 1 to clear this bit.
[1] | DIV4 | Time-out Counter Input Clock Divided By 4
|  | 0 = Time-out counter input clock divided by 4 Disabled.
|  | 1 = Time-out counter input clock divided by 4 Enabled.
|  | Note: When enabled, the time-out period is extended 4 times.
[2] | ENTI | Time-out Counter Enable Control
|  | 0 = Time-out counter Disabled.
|  | 1 = Time-out counter Enabled.
|  | Note: When the 14-bit time-out counter is enabled, it will start counting when SI is clear.
|  | Setting 1to the SI flag will reset counter and re-start up counting after SI is cleared.

Definition at line 2414 of file Mini51Series.h.

## ◆ IEN

GPIO_T::IEN

## Offset: 0x1C Px Interrupt Enable Control

Bits | Field | Descriptions
--- | --- | ---
[0] | IF_EN | Port 0-5 Pin [N] Interrupt Enabled By Input Falling Edge Or Input Level Low
|  | IF_EN[n] is used to enable the interrupt for each of the corresponding input Px.n pin.
|  | Set bit to 1 also enable the pin wake-up function.
|  | When setting the IF_EB[n] bit to 1:
|  | If the interrupt is level trigger (IMD[n] is 1), the input Px.n pin will generate the interrupt while this pin state is at low level.
|  | If the interrupt is edge mode trigger (IMD[n] is 0), the input Px.n pin will generate the interrupt while this pin state changed from high to low.
|  | 0 = Px.n low level or high to low interrupt Disabled.
|  | 1 = Px.n low level or high to low interrupt Enabled.
|  | Note1: x = 0~5, n = 0~7.
|  | Note2:
|  | P0_IEN[19:18], [3:2] are reserved.
|  | P1_IEN[23:22], [17], [7:6], [1] are reserved.
|  | P2_IEN[23], [17:16], [7], [1:0] are reserved.
|  | P3_IEN[23], [19], [7], [3] are reserved.
|  | P4_IEN[21:16], [5:0] are reserved.
|  | P5_IEN[23:22], [7:6] are reserved.
[23:16] | IR_EN | Port 0-5 Pin [N] Interrupt Enabled By Input Rising Edge Or Input Level High
|  | IR_EN[n] bit is used to enable the interrupt for each of the corresponding input Px.n pin.
|  | Set bit to 1 also enable the pin wake-up function.
|  | When setting the IR_EN[n] bit to 1:
|  | If the interrupt is level trigger (IMD[n] is 1), the input Px.n pin will generate the interrupt while this pin state is at high level.
|  | If the interrupt is edge trigger (IMD[n] is 0), the input Px.n pin will generate the interrupt while this pin state changed from low to high.
|  | 0 = Px.n level high or low to high interrupt Disabled.
|  | 1 = Px.n level high or low to high interrupt Enabled.
|  | Note: x = 0~5, n = 0~7.

Definition at line 2081 of file Mini51Series.h.

## ◆ IER

UART_T::IER

## Offset: 0x04 UART Interrupt Enable Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | RDA_IEN | Receive Data Available Interrupt Enable Control
|  | 0 = RDA_INT Masked off.
|  | 1 = RDA_INT Enabled.
[1] | THRE_IEN | Transmit Holding Register Empty Interrupt Enable Control
|  | 0 = THRE_INT Masked off.
|  | 1 = THRE_INT Enabled.
[2] | RLS_IEN | Receive Line Status Interrupt Enable Control
|  | 0 = RLS_INT Masked off.
|  | 1 = RLS_INT Enabled.
[3] | MODEM_IEN | Modem Status Interrupt Enable Control
|  | 0 = MODEM_INT Masked off.
|  | 1 = MODEM_INT Enabled.
[4] | RTO_IEN | RX Time-out Interrupt Enable Control
|  | 0 = TOUT_INT Masked off.
|  | 1 = TOUT_INT Enabled.
[5] | BUF_ERR_IEN | Buffer Error Interrupt Enable Control
|  | 0 = INT_BUF_ERR Masked Disabled.
|  | 1 = INT_BUF_ERR Enabled.
[6] | WAKE_EN | Wake-up CPU Function Enable Control
|  | 0 = UART wake-up function Disabled.
|  | 1 = UART Wake-up function Enabled.
|  | Note: when the chip is in Power-down mode, an external CTS change will wake-up chip from Power-down mode.
[11] | TIME_OUT_EN | Time-out Counter Enable Control
|  | 0 = Time-out counter Disabled.
|  | 1 = Time-out counter Enabled.
[12] | AUTO_RTS_EN | RTS Auto Flow Control Enable Control
|  | 0 = RTS auto flow control Disabled.
|  | 1 = RTS auto flow control Enabled.
|  | Note: When RTS auto-flow is enabled, if the number of bytes in the RX FIFO equals the RTS_TRI_LEV (UA_FCR [19:16]), the UART will de-assert RTS signal.
[13] | AUTO_CTS_EN | CTS Auto Flow Control Enable Control
|  | 0 = CTS auto flow control Disabled.
|  | 1 = CTS auto flow control Enabled.
|  | Note: When CTS auto-flow is enabled, the UART will send data to external device when CTS input assert (UART will not send data to device until CTS is asserted).

Definition at line 5324 of file Mini51Series.h.

## ◆ IMD

GPIO_T::IMD

## Offset: 0x18 Px Interrupt Mode Control

Bits | Field | Descriptions
--- | --- | ---
[7:0] | IMD | Port 0-5 Pin [N] Edge Or Level Detection Interrupt Mode Control
|  | IMD[n] bit is used to control the triggered interrupt is by level trigger or by edge trigger.
|  | If the interrupt is by edge trigger, the trigger source can be controlled by de-bounce.
|  | If the interrupt is by level trigger, the input source is sampled by one HCLK clock and generates the interrupt.
|  | 0 = Edge trigger interrupt.
|  | 1 = Level trigger interrupt.
|  | If pin is set as the level trigger interrupt, only one level can be set on the registers Px_IEN.
|  | If both levels to trigger interrupt are set, the setting is ignored and no interrupt will occur.
|  | The de-bounce function is valid only for edge triggered interrupt.
|  | If the interrupt mode is level triggered, the de-bounce enable bit is ignored.
|  | Note1: x = 0~5, n = 0~7.
|  | Note2:
|  | P0_IMD[3:2] are reserved.
|  | P1_IMD[7:6], [1] are reserved.
|  | P2_IMD[7], [1:0] are reserved.
|  | P3_IMD[7], [3] are reserved.
|  | P4_IMD[5:0] are reserved.
|  | P5_IMD[7:6] are reserved.

Definition at line 2080 of file Mini51Series.h.

## ◆ INTACCUCTL

PWM_T::INTACCUCTL

## Offset: 0x84 Period Interrupt Accumulation Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | INTACCUEN0 | Interrupt Accumulation Function Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[7:4] | PERIODCNT | Interrupt Accumulation Bits
|  | When INTACCUEN0 is set, PERIODCNT will decrease when every PWMPIF0 flag is set and when PERIODCNT reach to zero, the PWM0 interrupt will occurred and PERIODCNT will reload itself.

Definition at line 3575 of file Mini51Series.h.

## ◆ IPRSTC1

GCR_T::IPRSTC1

## Offset: 0x08 Peripheral Reset Control Resister 1

Bits | Field | Descriptions
--- | --- | ---
[0] | CHIP_RST | CHIP One-shot Reset (Write Protect)
|  | Setting this bit will reset the CHIP, including CPU kernel and all peripherals, and this bit will automatically return to 0 after the 2 clock cycles.
|  | The CHIP_RST is the same as the POR reset, and all the chip module is reset and the chip settings from flash are also reloaded.
|  | 0 = Chip normal operation.
|  | 1 = CHIP one-shot reset.
|  | Note: This bit is the protected bit, and programming it needs to write 0x59, 0x16, and 0x88 to address 0x5000_0100 to disable register protection.
|  | Refer to the register REGWRPROT at address GCR_BA + 0x100.
[1] | CPU_RST | CPU Kernel Reset
|  | Setting this bit will reset the CPU kernel, and this bit will automatically return to 0 after the 2 clock cycles.
|  | 0 = CPU normal operation.
|  | 1 = Reset CPU Kernel.
|  | Note: This bit is the protected bit, and programming it needs to write 0x59, 0x16, and 0x88 to address 0x5000_0100 to disable register protection.
|  | Refer to the register REGWRPROT at address GCR_BA + 0x100.

Definition at line 1506 of file Mini51Series.h.

## ◆ IPRSTC2

GCR_T::IPRSTC2

## Offset: 0x0C Peripheral Reset Control Resister 2

Bits | Field | Descriptions
--- | --- | ---
[1] | GPIO_RST | GPIO (P0~P5) Controller Reset
|  | 0 = GPIO module normal operation.
|  | 1 = GPIO module reset.
[2] | TMR0_RST | Timer0 Controller Reset
|  | 0 = Timer0 module normal operation.
|  | 1 = Timer0 module reset.
[3] | TMR1_RST | Timer1 Controller Reset
|  | 0 = Timer1 module normal operation.
|  | 1 = Timer1 module reset.
[8] | I2C_RST | I2C Controller Reset
|  | 0 = I2C module normal operation.
|  | 1 = I2C module reset.
[12] | SPI_RST | SPI Controller Reset
|  | 0 = SPI module normal operation.
|  | 1 = SPI module reset.
[16] | UART_RST | UART Controller Reset
|  | 0 = UART module normal operation.
|  | 1 = UART module reset.
[20] | PWM_RST | PWM Controller Reset
|  | 0 = PWM module normal operation.
|  | 1 = PWM module reset.
[22] | ACMP_RST | ACMP Controller Reset
|  | 0 = ACMP module normal operation.
|  | 1 = ACMP module reset.
[28] | ADC_RST | ADC Controller Reset
|  | 0 = ADC module normal operation.
|  | 1 = ADC module reset.

Definition at line 1507 of file Mini51Series.h.

## ◆ IRCR

UART_T::IRCR

## Offset: 0x28 UART IrDA Control Register

Bits | Field | Descriptions
--- | --- | ---
[1] | TX_SELECT | TX_SELECT
|  | 0 = IrDA receiver Enabled.
|  | 1 = IrDA transmitter Enabled.
[5] | INV_TX | INV_TX
|  | 0 = No inversion.
|  | 1 = Inverse TX output signal.
[6] | INV_RX | INV_RX
|  | 0 = No inversion.
|  | 1 = Inverse RX input signal.

Definition at line 5333 of file Mini51Series.h.

## ◆ IRCTRIMCTL

GCR_T::IRCTRIMCTL

## Offset: 0x80 HIRC Trim Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | TRIM_SEL | Trim Frequency Selection
|  | This bit is to enable the HIRC auto trim.
|  | When setting this bit to 1, the HIRC auto trim function will trim HIRC to 22.1184 MHz automatically based on the LXT reference clock.
|  | During auto trim operation, if LXT clock error is detected or trim retry limitation count reached, this field will be cleared to 0 automatically.
|  | 0 = HIRC auto trim function Disabled.
|  | 1 = HIRC auto trim function Enabled and HIRC trimmed to 22.1184 MHz.
[5:4] | TRIM_LOOP | Trim Calculation Loop
|  | This field defines that trim value calculation is based on how many LXT clocks in.
|  | For example, if TRIM_LOOP is set as 00, auto trim circuit will calculate trim value based on the average frequency difference in 4 LXT clock.
|  | 00 = Trim value calculation is based on average difference in 4 LXT clocks.
|  | 01 = Trim value calculation is based on average difference in 8 LXT clocks.
|  | 10 = Trim value calculation is based on average difference in 16 LXT clocks.
|  | 11 = Trim value calculation is based on average difference in 32 LXT clocks.

Definition at line 1524 of file Mini51Series.h.

## ◆ IRCTRIMIER

GCR_T::IRCTRIMIER

## Offset: 0x84 HIRC Trim Interrupt Enable Control Register

Bits | Field | Descriptions
--- | --- | ---
[1] | TRIM_FAIL_IEN | Trim Failure Interrupt Enable Control
|  | This bit controls if an interrupt will be triggered while HIRC trim value update limitation count is reached and HIRC frequency is still not locked on target frequency set by TRIM_SEL.
|  | If this bit is high and TRIM_FAIL_INT is set during auto trim operation, an interrupt will be triggered to notify that HIRC trim value update limitation count is reached.
|  | 0 = TRIM_FAIL_INT status Disabled to trigger an interrupt to CPU.
|  | 1 = TRIM_FAIL_INT status Enabled to trigger an interrupt to CPU.
[2] | 32K_ERR_IEN | LXT Clock Error Interrupt Enable Control
|  | This bit controls if CPU could get an interrupt while LXT clock is inaccurate during auto trim operation.
|  | If this bit is high, and 32K_ERR_INT is set during auto trim operation, an interrupt will be triggered to notify the LXT clock frequency is inaccurate.
|  | 0 = 32K_ERR_INT status Disabled to trigger an interrupt to CPU.
|  | 1 = 32K_ERR_INT status Enabled to trigger an interrupt to CPU.

Definition at line 1525 of file Mini51Series.h.

## ◆ IRCTRIMISR

GCR_T::IRCTRIMISR

## Offset: 0x88 HIRC Trim Interrupt Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | FREQ_LOCK | HIRC Frequency Lock Status
|  | This bit indicates the HIRC frequency locked in 22.1184 MHz.
|  | This is a read only status bit and doesn't trigger any interrupt.
[1] | TRIM_FAIL_INT | Trim Failure Interrupt Status
|  | This bit indicates that HIRC trim value update limitation count reached and HIRC clock frequency still doesn't lock.
|  | Once this bit is set, the auto trim operation stopped and TRIM_SEL will be cleared to 0 by hardware automatically.
|  | If this bit is set and TRIM_FAIL_IEN is high, an interrupt will be triggered to notify that HIRC trim value update limitation count was reached.
|  | Software can write 1 to clear this bit to 0.
|  | 0 = Trim value update limitation count is not reached.
|  | 1 = Trim value update limitation count is reached and HIRC frequency is still not locked.
[2] | 32K_ERR_INT | LXT Clock Error Interrupt Status
|  | This bit indicates that LXT clock frequency is inaccuracy.
|  | Once this bit is set, the auto trim operation stopped and TRIM_SEL will be cleared to 0 by hardware automatically.
|  | If this bit is set and 32K_ERR_IEN is high, an interrupt will be triggered to notify the LXT clock frequency is inaccuracy.
|  | Software can write 1 to clear this bit to 0.
|  | 0 = LXT clock frequency is accuracy.
|  | 1 = LXT clock frequency is inaccuracy.

Definition at line 1526 of file Mini51Series.h.

## ◆ ISPADR

FMC_T::ISPADR

## Offset: 0x04 ISP Address Register

Bits | Field | Descriptions
--- | --- | ---
[31:0] | ISPADR | ISP Address
|  | The NuMicro Mini51TM series supports word program only. ISPADR[1:0] must be kept 00 for ISP operation.

Definition at line 1124 of file Mini51Series.h.

## ◆ ISPCMD

FMC_T::ISPCMD

## Offset: 0x0C ISP Command Register

Bits | Field | Descriptions
--- | --- | ---
[5:0] | ISPCMD | ISP Command
|  | ISP commands are shown below:
|  | 0x00 = Read.
|  | 0x04 = Read Unique ID.
|  | 0x0B = Read Company ID (0xDA).
|  | 0x21 = Program.
|  | 0x22 = Page Erase.
|  | 0x2E = Set Vector Page Re-Map.

Definition at line 1126 of file Mini51Series.h.

## ◆ ISPCON

FMC_T::ISPCON

## Offset: 0x00 ISP Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | ISPEN | ISP Enable Control (Write Protect)
|  | Set this bit to enable ISP function.
|  | 0 = ISP function Disabled.
|  | 1 = ISP function Enabled.
[1] | BS | Boot Select (Write Protect)
|  | Set/clear this bit to select next booting from LDROM/APROM, respectively.
|  | This bit also functions as chip booting status flag, which can be used to check where chip booted from.
|  | This bit is initiated with the inversed value of CBS in CONFIG0 after any reset is happened except CPU reset (RSTS_CPU is 1) or system reset (RSTS_SYS) is happened.
|  | 0 = Boot from APROM.
|  | 1 = Boot from LDROM.
[3] | APUEN | APROM Update Enable Control (Write Protect)
|  | 0 = APROM cannot be updated when chip runs in APROM.
|  | 1 = APROM can be updated when chip runs in APROM.
[4] | CFGUEN | CONFIG Update Enable Control (Write Protect)
|  | Writing this bit to 1 enables software to update CONFIG value by ISP register control procedure regardless of program code is running in APROM or LDROM.
|  | 0 = ISP update User Configuration Disabled.
|  | 1 = ISP update User Configuration Enabled.
[5] | LDUEN | LDROM Update Enable Control (Write Protect)
|  | 0 = LDROM cannot be updated.
|  | 1 = LDROM can be updated when the MCU runs in APROM.
[6] | ISPFF | ISP Fail Flag (Write Protect)
|  | This bit is set by hardware when a triggered ISP meets any of the following conditions:
|  | (1) APROM writes to itself if APUEN is set to 0 or CBS[0]=1.
|  | (2) LDROM writes to itself if LDUEN is set to 0 or CBS[0]=1.
|  | (3) User Configuration is erased/programmed when CFGUEN is 0.
|  | (4) Destination address is illegal, such as over an available range.
|  | Note: Write 1 to clear this bit to 0.

Definition at line 1123 of file Mini51Series.h.

## ◆ ISPDAT

FMC_T::ISPDAT

## Offset: 0x08 ISP Data Register

Bits | Field | Descriptions
--- | --- | ---
[31:0] | ISPDAT | ISP Data
|  | Write data to this register before ISP program operation.
|  | Read data from this register after ISP read operation.

Definition at line 1125 of file Mini51Series.h.

## ◆ ISPSTA

FMC_T::ISPSTA

## Offset: 0x40 ISP Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | ISPGO | ISP Start Trigger (Read Only)
|  | Write 1 to start ISP operation and this bit will be cleared to 0 by hardware automatically when ISP operation is finished.
|  | 0 = ISP operation is finished.
|  | 1 = ISP operation is progressed.
|  | Note: This bit is the same with ISPTRG bit 0.
[2:1] | CBS | Config Boot Selection (Read Only)
|  | This is a mirror of CBS in CONFIG0.
[6] | ISPFF | ISP Fail Flag (Write Protect)
|  | This bit is set by hardware when a triggered ISP meets any of the following conditions:
|  | (1) APROM writes to itself if APUEN is set to 0 or CBS[0]=1.
|  | (2) LDROM writes to itself if LDUEN is set to 0 or CBS[0]=1.
|  | (3) User Configuration is erased/programmed when CFGUEN is 0.
|  | (4) Destination address is illegal, such as over an available range.
|  | Write 1 to clear.
|  | Note: This bit functions the same as ISPCON bit 6.
[20:9] | VECMAP | Vector Page Mapping Address (Read Only)
|  | The current flash address space 0x0000_0000~0x0000_01FF is mapping to address {VECMAP[11:0], 9'h000} ~ {VECMAP[11:0], 9'h1FF}.

Definition at line 1132 of file Mini51Series.h.

## ◆ ISPTRG

FMC_T::ISPTRG

## Offset: 0x10 ISP Trigger Register

Bits | Field | Descriptions
--- | --- | ---
[0] | ISPGO | ISP Start Trigger (Write Protect)
|  | Write 1 to start ISP operation and this bit will be cleared to 0 by hardware automatically when ISP operation is finished.
|  | 0 = ISP operation is finished.
|  | 1 = ISP operation is progressed.

Definition at line 1127 of file Mini51Series.h.

## ◆ ISR

UART_T::ISR

## Offset: 0x1C UART Interrupt Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | RDA_IF | Receive Data Available Interrupt Flag (Read Only)
|  | When the number of bytes in the RX FIFO equals the RFITL then the RDA_IF will be set.
|  | If RDA_IEN (UA_IER [0]) is enabled, the RDA interrupt will be generated.
|  | 0 = No RDA interrupt flag is generated.
|  | 1 = RDA interrupt flag is generated.
|  | Note: This bit is read only and it will be cleared when the number of unread bytes of RX FIFO drops below the threshold level (RFITL).
[1] | THRE_IF | Transmit Holding Register Empty Interrupt Flag (Read Only)
|  | This bit is set when the last data of TX FIFO is transferred to Transmitter Shift Register.
|  | If THRE_IEN (UA_IER [1]) is enabled, the THRE interrupt will be generated.
|  | 0 = No THRE interrupt flag is generated.
|  | 1 = THRE interrupt flag is generated.
|  | Note: This bit is read only and it will be cleared when writing data into THR (TX FIFO not empty).
[2] | RLS_IF | Receive Line Interrupt Flag (Read Only)
|  | This bit is set when the RX receive data have parity error, framing error or break error (at least one of 3 bits, BIF, FEF and PEF, is set).
|  | If RLS_IEN (UA_IER [2]) is enabled, the RLS interrupt will be generated.
|  | 0 = No RLS interrupt flag is generated.
|  | 1 = RLS interrupt flag is generated.
|  | Note1: In RS-485 function mode, this field is set including "receiver detect and received address byte character (bit 9 = 1) bit".
|  | At the same time, the bit of RS485_ADD_DETF (UA_FSR[3]) is also set.
|  | Note2: This bit is read only and reset to 0 when all bits of BIF, FEF, PEF and RS485_ADD_DETF are cleared.
[3] | MODEM_IF | MODEM Interrupt Flag (Read Only)
|  | This bit is set when the CTS pin has state change (DCTSF = 1).
|  | If UA_IER [MODEM_IEN] is enabled, the Modem interrupt will be generated.
|  | 0 = No Modem interrupt flag is generated.
|  | 1 = Modem interrupt flag is generated.
|  | Note: This bit is read only and reset to 0 when bit DCTSF is cleared by a write 1 on DCTSF.
[4] | TOUT_IF | Time-out Interrupt Flag (Read Only)
|  | This bit is set when the RX FIFO is not empty and no activities occurred in the RX FIFO and the time-out counter equal to TOIC.
|  | If RTO_IEN (UA_IER [4]) is enabled, the Tout interrupt will be generated.
|  | 0 = No Time-out interrupt flag is generated.
|  | 1 = Time-out interrupt flag is generated.
|  | Note: This bit is read only and user can read UA_RBR (RX is in active) to clear it.
[5] | BUF_ERR_IF | Buffer Error Interrupt Flag (Read Only)
|  | This bit is set when the TX/RX FIFO overflow flag (TX_OVER_IF or RX_OVER_IF) is set.
|  | When BUF_ERR_IF is set, the transfer is not correct.
|  | If BUF_ERR_IEN (UA_IER [5]) is enabled, the buffer error interrupt will be generated.
|  | 0 = No buffer error interrupt flag is generated.
|  | 1 = Buffer error interrupt flag is generated.
|  | Note: This bit is read only and reset to 0 when all bits of TX_OVER_IF and RX_OVER_IF are cleared.
[8] | RDA_INT | Receive Data Available Interrupt Indicator (Read Only)
|  | This bit is set if RDA_IEN and RDA_IF are both set to 1.
|  | This bit is set if RDA_IEN and RDA_IF are both set to 1.
|  | 0 = No RDA interrupt is generated.
|  | 1 = RDA interrupt is generated.
[9] | THRE_INT | Transmit Holding Register Empty Interrupt Indicator (Read Only)
|  | This bit is set if THRE_IEN and THRE_IF are both set to 1.
|  | 0 = No THRE interrupt is generated.
|  | 1 = THRE interrupt is generated.
[10] | RLS_INT | Receive Line Status Interrupt (Read Only)
|  | This bit is set if RLS_IEN and RLS_IF are both set to 1.
|  | 0 = No RLS interrupt is generated.
|  | 1 = RLS interrupt is generated.
[11] | MODEM_INT | MODEM Status Interrupt Indicator (Read Only)
|  | This bit is set if MODEM_IEN and MODEM_IF are both set to 1.
|  | 0 = No Modem interrupt is generated.
|  | 1 = Modem interrupt is generated.
[12] | TOUT_INT | Time-out Interrupt Indicator (Read Only)
|  | This bit is set if RTO_IEN and TOUT_IF are both set to 1.
|  | 0 = No Time-out interrupt is generated.
|  | 1 = Time-out interrupt is generated.
[13] | BUF_ERR_INT | Buffer Error Interrupt Indicator (Read Only)
|  | This bit is set if BUF_ERR_IEN and BUF_ERR_IF are both set to 1.
|  | 0 = No buffer error interrupt is generated.
|  | 1 = buffer error interrupt is generated.

Definition at line 5330 of file Mini51Series.h.

## ◆ ISRC

GPIO_T::ISRC

## Offset: 0x20 Px Interrupt Source Flag

Bits | Field | Descriptions
--- | --- | ---
[7:0] | ISRC | Port 0-5 Pin [N] Interrupt Source Flag
|  | Write :
|  | 0 = No action.
|  | 1 = Clear the corresponding pending interrupt.
|  | Read :
|  | 0 = No interrupt at Px.n.
|  | 1 = Px.n generates an interrupt.
|  | Note1: x = 0~5, n = 0~7.
|  | Note2:
|  | P0_ISRC[3:2] are reserved.
|  | P1_ISRC[7:6], [1] are reserved.
|  | P2_ISRC[7], [1:0] are reserved.
|  | P3_ISRC[7], [3] are reserved.
|  | P4_ISRC[5:0] are reserved.
|  | P5_ISRC[7:6] are reserved.

Definition at line 2082 of file Mini51Series.h.

## ◆ LCR

UART_T::LCR

## Offset: 0x0C UART Line Control Register

Bits | Field | Descriptions
--- | --- | ---
[1:0] | WLS | Word Length Selection
|  | 00 = Word length is 5-bit.
|  | 01 = Word length is 6-bit.
|  | 10 = Word length is 7-bit.
|  | 11 = Word length is 8-bit.
[2] | NSB | Number Of "STOP Bit"
|  | 0 = One "STOP bit" is generated in the transmitted data.
|  | 1 = When select 5-bit word length, 1.5 "STOP bit" is generated in the transmitted data.
|  | When select 6-, 7- and 8-bit word length, 2 "STOP bit" is generated in the transmitted data.
[3] | PBE | Parity Bit Enable Control
|  | 0 = No parity bit.
|  | 1 = Parity bit is generated on each outgoing character and is checked on each incoming data.
[4] | EPE | Even Parity Enable Control
|  | 0 = Odd number of logic 1's is transmitted and checked in each word.
|  | 1 = Even number of logic 1's is transmitted and checked in each word.
|  | This bit has effect only when PBE (UA_LCR[3]) is set.
[5] | SPE | Stick Parity Enable Control
|  | 0 = Stick parity Disabled.
|  | 1 = If PBE (UA_LCR[3]) and EBE (UA_LCR[4]) are logic 1, the parity bit is transmitted and checked as logic 0.
|  | If PBE (UA_LCR[3]) is 1 and EBE (UA_LCR[4]) is 0 then the parity bit is transmitted and checked as 1.
[6] | BCB | Break Control Bit
|  | When this bit is set to logic 1, the serial data output (TX) is forced to the Spacing State (logic 0).
|  | This bit acts only on TX and has no effect on the transmitter logic.
|  | 0 = Break control Disabled.
|  | 1 = Break control Enabled.

Definition at line 5326 of file Mini51Series.h.

## ◆ MCR

UART_T::MCR

## Offset: 0x10 UART Modem Control Register

Bits | Field | Descriptions
--- | --- | ---
[1] | RTS | RTS (Request-to-send) Signal Control
|  | This bit is direct control internal RTS signal active or not, and then drive the RTS pin output with LEV_RTS bit configuration.
|  | 0 = RTS signal is active.
|  | 1 = RTS signal is inactive.
|  | Note1: This RTS signal control bit is not effective when RTS auto-flow control (AUTO_RTS_EN) is enabled in UART function mode.
|  | Note2: This RTS signal control bit is not effective when RS-485 auto direction mode (RS485_AUD) is enabled in RS-485 function mode.
[9] | LEV_RTS | RTS Pin Active Level
|  | This bit defines the active level state of RTS pin output.
|  | 0 = RTS pin output is high level active.
|  | 1 = RTS pin output is low level active.
|  | Note1: Refer to and UART function mode.
|  | Note2: Refer to and for RS-485 function mode.
[13] | RTS_ST | RTS Pin State (Read Only)
|  | This bit mirror from RTS pin output of voltage logic status.
|  | 0 = RTS pin output is low level voltage logic state.
|  | 1 = RTS pin output is high level voltage logic state.

Definition at line 5327 of file Mini51Series.h.

## ◆ MCUIRQ

INT_T::MCUIRQ

## Offset: 0x84 MCU IRQ Number Identity Register

Bits | Field | Descriptions
--- | --- | ---
[31:0] | MCU_IRQ | MCU IRQ Source
|  | The MCU_IRQ collects all the interrupts from the peripherals and generates the synchronous interrupt to Cortex-M0 core.
|  | This modes to generate interrupt to Cortex-M0 - the normal mode.
|  | The MCU_IRQ collects all interrupts from each peripheral and synchronizes them then interrupts the Cortex-M0.
|  | When the MCU_IRQ[n] is 0, setting MCU_IRQ[n] to 1 will generate an interrupt to Cortex-M0 NVIC[n].
|  | When the MCU_IRQ[n] is 1 (mean an interrupt is assert), setting 1 to the MCU_bit[n] will clear the interrupt and setting MCU_IRQ[n] 0 has no effect.

Definition at line 2717 of file Mini51Series.h.

## ◆ MSR

UART_T::MSR

## Offset: 0x14 UART Modem Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | DCTSF | Detect CTS State Change Flag
|  | This bit is set whenever CTS input has change state, and it will generate Modem interrupt to CPU when MODEM_IEN (UA_IER [3]) is set to 1.
|  | 0 = CTS input has not change state.
|  | 1 = CTS input has change state.
|  | Note: This bit is cleared by writing 1 to it.
[4] | CTS_ST | CTS Pin Status (Read Only)
|  | This bit mirror from CTS pin input of voltage logic status.
|  | 0 = CTS pin input is low level voltage logic state.
|  | 1 = CTS pin input is high level voltage logic state.
|  | Note: This bit echoes when UART Controller peripheral clock is enabled, and CTS multi-function port is selected.
[8] | LEV_CTS | CTS Pin Active Level
|  | This bit defines the active level state of CTS pin input.
|  | 0 = CTS pin input is high level active.
|  | 1 = CTS pin input is low level active.
|  | Note: Refer to

Definition at line 5328 of file Mini51Series.h.

## ◆ NMICON

INT_T::NMICON

## Offset: 0x80 NMI Source Interrupt Select Control Register

Bits | Field | Descriptions
--- | --- | ---
[4:0] | NMI_SEL | NMI Interrupt Source Selection
|  | The NMI interrupt to Cortex-M0 can be selected from one of the peripheral interrupt by setting NMI_SEL.
[8] | NMI_SEL_EN | NMI Interrupt Enable Control (Write Protect)
|  | 0 = NMI interrupt Disabled.
|  | 1 = NMI interrupt Enabled.
|  | Note: This bit is the protected bit, and programming it needs to write 0x59, 0x16, and 0x88 to address 0x5000_0100 to disable register protection.
|  | Refer to the register REGWRPROT at address GCR_BA+0x100.

Definition at line 2716 of file Mini51Series.h.

## ◆ OFFD

GPIO_T::OFFD

## Offset: 0x04 Px Digital Input Path Disable Control

Bits | Field | Descriptions
--- | --- | ---
[23:16] | OFFD | Port 0-5 Pin [N] Digital Input Path Disable Control
|  | 0 = Px.n digital input path Enabled.
|  | 1 = Px.n digital input path Disabled (digital input tied to low).
|  | Note: x = 0~5, n = 0~7.

Definition at line 2075 of file Mini51Series.h.

## ◆ P0_MFP

GCR_T::P0_MFP

## Offset: 0x30 P0 Multiple Function and Input Type Control Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | P0_MFP | P0 Multiple Function Selection
[8] | P0_ALT0 | P0.0 Alternate Function Selection
[9] | P0_ALT1 | P0.1 Alternate Function Selection
[12] | P0_ALT4 | P0.4 Alternate Function Selection
[13] | P0_ALT5 | P0.5 Alternate Function Selection
[14] | P0_ALT6 | P0.6 Alternate Function Selection
[15] | P0_ALT7 | P0.7 Alternate Function Selection
[23:16] | P0_TYPE | P0[7:0] TTL Or Schmitt Trigger Function Enable Control
|  | 0 = P0[7:0]Select I/O input as TTL function.
|  | 1 = P0[7:0] Select I/O input as Schmitt Trigger function .

Definition at line 1515 of file Mini51Series.h.

## ◆ P1_MFP

GCR_T::P1_MFP

## Offset: 0x34 P1 Multiple Function and Input Type Control Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | P1_MFP | P1 Multiple Function Selection
[8] | P1_ALT0 | P1.0 Alternate Function Selection
[10] | P1_ALT2 | P1.2 Alternate Function Selection
[11] | P1_ALT3 | P1.3 Alternate Function Selection
[12] | P1_ALT4 | P1.4 Alternate Function Selection
[13] | P1_ALT5 | P1.5 Alternate Function Selection
[23:16] | P1_TYPE | P1[7:0] TTL Or Schmitt Trigger Function Enable Control
|  | 0 = P1[7:0]Select I/O input as TTL function.
|  | 1 = P1[7:0] Select I/O input as Schmitt Trigger function .

Definition at line 1516 of file Mini51Series.h.

## ◆ P2_MFP

GCR_T::P2_MFP

## Offset: 0x38 P2 Multiple Function and Input Type Control Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | P2_MFP | P2 Multiple Function Selection
[10] | P2_ALT2 | P2.2 Alternate Function Selection
[11] | P2_ALT3 | P2.3 Alternate Function Selection
[12] | P2_ALT4 | P2.4 Alternate Function Selection
[13] | P2_ALT5 | P2.5 Alternate Function Selection
[14] | P2_ALT6 | P2.6 Alternate Function Selection
[23:16] | P2_TYPE | P2[7:0] TTL Or Schmitt Trigger Function Enable Control
|  | 0 = P2[7:0]Select I/O input as TTL function.
|  | 1 = P2[7:0] Select I/O input as Schmitt Trigger function .

Definition at line 1517 of file Mini51Series.h.

## ◆ P3_MFP

GCR_T::P3_MFP

## Offset: 0x3C P3 Multiple Function and Input Type Control Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | P3_MFP | P3 Multiple Function Selection
[8] | P3_ALT0 | P3.0 Alternate Function Selection
[9] | P3_ALT1 | P3.1 Alternate Function Selection
[10] | P3_ALT2 | P3.2 Alternate Function Selection
[12] | P3_ALT4 | P3.4 Alternate Function Selection
[13] | P3_ALT5 | P3.5 Alternate Function Selection
[14] | P3_ALT6 | P3.6 Alternate Function Selection
[23:16] | P3_TYPE | P3[7:0] TTL Or Schmitt Trigger Function Enable Control
|  | 0 = P3[7:0]Select I/O input as TTL function.
|  | 1 = P3[7:0] Select I/O input as Schmitt Trigger function .
[24] | P32CPP1 | P3.2 Alternate Function Selection Extension

Definition at line 1518 of file Mini51Series.h.

## ◆ P4_MFP

GCR_T::P4_MFP

## Offset: 0x40 P4 Multiple Function and Input Type Control Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | P4_MFP | P4 Multiple Function Selection
[14] | P4_ALT6 | P4.6 Alternate Function Selection
[15] | P4_ALT7 | P4.7 Alternate Function Selection
[23:16] | P4_TYPE | P4[7:0] TTL Or Schmitt Trigger Function Enable Control
|  | 0 = P4[7:0]Select I/O input as TTL function.
|  | 1 = P4[7:0] Select I/O input as Schmitt Trigger function .

Definition at line 1519 of file Mini51Series.h.

## ◆ P5_MFP

GCR_T::P5_MFP

## Offset: 0x44 P5 Multiple Function and Input Type Control Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | P5_MFP | P5 Multiple Function Selection
[8] | P5_ALT0 | P5.0 Alternate Function Selection
[9] | P5_ALT1 | P5.1 Alternate Function Selection
[10] | P5_ALT2 | P5.2 Alternate Function Selection
[11] | P5_ALT3 | P5.3 Alternate Function Selection
[12] | P5_ALT4 | P5.4 Alternate Function Selection
[13] | P5_ALT5 | P5.5 Alternate Function Selection
[23:16] | P5_TYPE | P5[7:0] TTL Or Schmitt Trigger Function Enable Control
|  | 0 = P5[7:0]Select I/O input as TTL function.
|  | 1 = P5[7:0] Select I/O input as Schmitt Trigger function .

Definition at line 1520 of file Mini51Series.h.

## ◆ PCR

PWM_T::PCR

## Offset: 0x08 PWM Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | CH0EN | PWM-timer 0 Enable/Disable Start Run
|  | 0 = Corresponding PWM-timer running Stopped.
|  | 1 = Corresponding PWM-timer start run Enabled.
[1] | DB_MODE | PWM Debug Mode Configuration Bit (Available In DEBUG Mode Only)
|  | 0 = Safe mode: The timer is frozen and PWM outputs are shut down Safe state for the inverter.
|  | The timer can still be re-started from where it stops.
|  | 1 = Normal mode: The timer continues to operate normally May be dangerous in some cases since a constant duty cycle is applied to the inverter (no more interrupts serviced).
[2] | CH0INV | PWM-timer 0 Output Inverter Enable Control
|  | 0 = Inverter Disabled.
|  | 1 = Inverter Enabled.
[3] | CH0MOD | PWM-timer 0 Auto-reload/One-shot Mode
|  | 0 = One-shot mode.
|  | 1 = Auto-reload mode.
|  | Note: If there is a rising transition at this bit, it will cause CNR0 and CMR0 cleared.
[4] | CH1EN | PWM-timer 1 Enable/Disable Start Run
|  | 0 = Corresponding PWM-timer running Stopped.
|  | 1 = Corresponding PWM-timer start run Enabled.
[6] | CH1INV | PWM-timer 1 Output Inverter ON/OFF
|  | 0 = Inverter OFF.
|  | 1 = Inverter ON.
[7] | CH1MOD | PWM-timer 1 Auto-reload/One-shot Mode
|  | 0 = One-shot mode.
|  | 1 = Auto-reload mode.
|  | Note: If there is a rising transition at this bit, it will cause CNR1 and CMR1 cleared.
[8] | CH2EN | PWM-timer 2 Enable/Disable Start Run
|  | 0 = Corresponding PWM-timer running Stopped.
|  | 1 = Corresponding PWM-timer start run Enabled.
[10] | CH2INV | PWM-timer 2 Output Inverter Enable Control
|  | 0 = Inverter Disabled.
|  | 1 = Inverter Enabled.
[11] | CH2MOD | PWM-timer 2 Auto-reload/One-shot Mode
|  | 0 = One-shot mode.
|  | 1 = Auto-reload mode.
|  | Note: If there is a rising transition at this bit, it will cause CNR2 and CMR2 cleared.
[12] | CH3EN | PWM-timer 3 Enable/Disable Start Run
|  | 0 = Corresponding PWM-timer running Stopped.
|  | 1 = Corresponding PWM-timer start run Enabled.
[14] | CH3INV | PWM-timer 3 Output Inverter Enable Control
|  | 0 = Inverter Disabled.
|  | 1 = Inverter Enabled.
[15] | CH3MOD | PWM-timer 3 Auto-reload/One-shot Mode
|  | 0 = One-shot mode.
|  | 1 = Auto-reload mode.
|  | Note: If there is a rising transition at this bit, it will cause CNR3 and CMR3 cleared.
[16] | CH4EN | PWM-timer 4 Enable/Disable Start Run
|  | 0 = Corresponding PWM-timer running Stopped.
|  | 1 = Corresponding PWM-timer start run Enabled.
[18] | CH4INV | PWM-timer 4 Output Inverter Enable Control
|  | 0 = Inverter Disabled.
|  | 1 = Inverter Enabled.
[19] | CH4MOD | PWM-timer 4 Auto-reload/One-shot Mode
|  | 0 = One-shot mode.
|  | 1 = Auto-reload mode.
|  | Note: If there is a rising transition at this bit, it will cause CNR4 and CMR4 cleared.
[20] | CH5EN | PWM-timer 5 Enable/Disable Start Run
|  | 0 = Corresponding PWM-timer running Stopped.
|  | 1 = Corresponding PWM-timer start run Enabled.
[22] | CH5INV | PWM-timer 5 Output Inverter Enable Control
|  | 0 = Inverter Disabled.
|  | 1 = Inverter Enabled.
[23] | CH5MOD | PWM-timer 5 Auto-reload/One-shot Mode
|  | 0 = One-shot mode.
|  | 1 = Auto-reload mode.
|  | Note: If there is a rising transition at this bit, it will cause CNR5 and CMR5 cleared.
[24] | DZEN01 | Dead-zone 0 Generator Enable Control (PWM0 And PWM1 Pair For PWM Group)
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: When the dead-zone generator is enabled, the pair of PWM0 and PWM1 becomes a complementary pair for PWM group.
[25] | DZEN23 | Dead-zone 2 Generator Enable Control (PWM2 And PWM3 Pair For PWM Group)
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: When the dead-zone generator is enabled, the pair of PWM2 and PWM3 becomes a complementary pair for PWM group.
[26] | DZEN45 | Dead-zone 4 Generator Enable Control (PWM4 And PWM5 Pair For PWM Group)
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: When the dead-zone generator is enabled, the pair of PWM4 and PWM5 becomes a complementary pair for PWM group.
[27] | CLRPWM | Clear PWM Counter Control Bit
|  | 0 = Do not clear PWM counter.
|  | 1 = All 16-bit PWM counters cleared to 0x0000.
|  | Note: It is automatically cleared by hardware.
[29:28] | PWMMOD | PWM Operating Mode Selection
|  | 00 = Independent mode.
|  | 01 = Complementary mode.
|  | 10 = Synchronized mode.
|  | 11 = Reserved.
[30] | GRP | Group Bit
|  | 0 = The signals timing of all PWM channels are independent.
|  | 1 = Unify the signals timing of PWM0, PWM2 and PWM4 in the same phase which is controlled by PWM0 and also unify the signals timing of PWM1, PWM3 and PWM5 in the same phase which is controlled by PWM1.
[31] | PWMTYPE | PWM Aligned Type Selection Bit
|  | 0 = Edge-aligned type.
|  | 1 = Center-aligned type.

Definition at line 3557 of file Mini51Series.h.

## ◆ PDID

GCR_T::PDID

## Offset: 0x00 Part Device Identification Number Register

Bits | Field | Descriptions
--- | --- | ---
[31:0] | PDID | Product Device Identification Number
|  | This register reflects the device part number code.
|  | Software can read this register to identify which device is used.
|  | For example, the MINI51LDE PDID code is "0x20205100".

Definition at line 1504 of file Mini51Series.h.

## ◆ PDZIR

PWM_T::PDZIR

## Offset: 0x64 PWM Dead-zone Interval Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | DZI01 | Dead-zone Interval Register For Pair Of Channel0 And Channel1 (PWM0 And PWM1 Pair)
|  | These 8 bits determine dead-zone length.
|  | The unit time of dead-zone length is received from corresponding CSR bits.
[15:8] | DZI23 | Dead-zone Interval Register For Pair Of Channel2 And Channel3 (PWM2 And PWM3 Pair)
|  | These 8 bits determine dead-zone length.
|  | The unit time of dead-zone length is received from corresponding CSR bits.
[23:16] | DZI45 | Dead-zone Interval Register For Pair Of Channel4 And Channel5 (PWM4 And PWM5 Pair)
|  | These 8 bits determine dead-zone length.
|  | The unit time of dead-zone length is received from corresponding CSR bits.

Definition at line 3567 of file Mini51Series.h.

## ◆ PFBCON

PWM_T::PFBCON

## Offset: 0x60 PWM Fault Brake Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | BKEN0 | Enable BKP0 Pin Trigger Fault Brake Function 0
|  | 0 = Disabling BKP0 pin can trigger brake function 0 (EINT0 or CPO1).
|  | 1 = Enabling a falling at BKP0 pin can trigger brake function 0.
[1] | BKEN1 | Enable BKP1 Pin Trigger Fault Brake Function 1
|  | 0 = Disabling BKP1 pin can trigger brake function 1 (EINT1 or CPO0).
|  | 1 = Enabling a falling at BKP1 pin can trigger brake function 1.
[2] | CPO0BKEN | BKP1 Fault Brake Function Source Selection
|  | 0 = EINT1 as one brake source in BKP1.
|  | 1 = CPO0 as one brake source in BKP1.
[3] | CPO1BKEN | BKP0 Fault Brake Function Source Selection
|  | 0 = EINT0 as one brake source in BKP0.
|  | 1 = CPO1 as one brake source in BKP0.
[7] | BKF | PWM Fault Brake Event Flag (Write 1 Clear)
|  | 0 = PWM output initial state when fault brake conditions asserted.
|  | 1 = PWM output fault brake state when fault brake conditions asserted.
|  | Software can write 1 to clear this bit and must clear this bit before restart PWM counter.
[24] | PWMBKO0 | PWM Channel 0 Brake Output Select Bit
|  | 0 = PWM output low when fault brake conditions asserted.
|  | 1 = PWM output high when fault brake conditions asserted.
[25] | PWMBKO1 | PWM Channel 1 Brake Output Select Bit
|  | 0 = PWM output low when fault brake conditions asserted.
|  | 1 = PWM output high when fault brake conditions asserted.
[26] | PWMBKO2 | PWM Channel 2 Brake Output Select Bit
|  | 0 = PWM output low when fault brake conditions asserted.
|  | 1 = PWM output high when fault brake conditions asserted.
[27] | PWMBKO3 | PWM Channel 3 Brake Output Select Bit
|  | 0 = PWM output low when fault brake conditions asserted.
|  | 1 = PWM output high when fault brake conditions asserted.
[28] | PWMBKO4 | PWM Channel 4 Brake Output Select Bit
|  | 0 = PWM output low when fault brake conditions asserted.
|  | 1 = PWM output high when fault brake conditions asserted.
[29] | PWMBKO5 | PWM Channel 5 Brake Output Select Bit
|  | 0 = PWM output low when fault brake conditions asserted.
|  | 1 = PWM output high when fault brake conditions asserted.
[30] | D6BKO6 | D6 Brake Output Select Bit
|  | 0 = D6 output low when fault brake conditions asserted.
|  | 1 = D6 output high when fault brake conditions asserted.
[31] | D7BKO7 | D7 Brake Output Select Bit
|  | 0 = D7 output low when fault brake conditions asserted.
|  | 1 = D7 output high when fault brake conditions asserted.

Definition at line 3566 of file Mini51Series.h.

## ◆ PHCHG

PWM_T::PHCHG

## Offset: 0x78 Phase Change Register

Bits | Field | Descriptions
--- | --- | ---
[0] | D0 | D0: When PWM0 Is Zero, Channel 0's Output Waveform Is D0
|  | 0 = Output low.
|  | 1 = Output high.
[1] | D1 | D1: When PWM1 Is Zero, Channel 1's Output Waveform Is D1
|  | 0 = Output low.
|  | 1 = Output high.
[2] | D2 | D2: When PWM2 Is Zero, Channel 2's Output Waveform Is D2
|  | 0 = Output low.
|  | 1 = Output high.
[3] | D3 | D3: When PWM3 Is Zero, Channel 3's Output Waveform Is D3
|  | 0 = Output low.
|  | 1 = Output high.
[4] | D4 | D4: When PWM4 Is Zero, Channel 4's Output Waveform Is D4
|  | 0 = Output low.
|  | 1 = Output high.
[5] | D5 | D5: When PWM5 Is Zero, Channel 5's Output Waveform Is D5
|  | 0 = Output low.
|  | 1 = Output high.
[6] | D6 | D6: When MASK6 Is 1, Channel 6's Output Waveform Is D6
|  | 0 = Output low.
|  | 1 = Output high.
[7] | D7 | D7: When MASK7 Is 1, Channel 7's Output Waveform Is D7
|  | 0 = Output low.
|  | 1 = Output high.
[8] | PWM0 | PWM Channel 0 Output Enable Control
|  | 0 = Output D0 specified in bit 0 of PHCHG register.
|  | 1 = Output the original channel 0 waveform.
[9] | PWM1 | PWM Channel 1 Output Enable Control
|  | 0 = Output D1 specified in bit 1 of PHCHG register.
|  | 1 = Output the original channel 1 waveform.
[10] | PWM2 | PWM Channel 2 Output Enable Control
|  | 0 = Output D2 specified in bit 2 of PHCHG register.
|  | 1 = Output the original channel 2 waveform.
[11] | PWM3 | PWM Channel 3 Output Enable Control
|  | 0 = Output D3 specified in bit 3 of PHCHG register.
|  | 1 = Output the original channel 3 waveform.
[12] | PWM4 | PWM Channel 4 Output Enable Control
|  | 0 = Output D4 specified in bit 4 of PHCHG register.
|  | 1 = Output the original channel 4 waveform.
[13] | PWM5 | PWM Channel 5 Output Enable Control
|  | 0 = Output D5 specified in bit 5 of PHCHG register.
|  | 1 = Output the original channel 5 waveform.
[14] | ACCNT0 | Hardware Auto Clear CE0 When ACMP0 Trigger It
|  | 0 = Enabled.
|  | 1 = Disabled.
[15] | ACCNT1 | Hardware Auto Clear CE1 When ACMP1 Trigger It
|  | 0 = Enabled.
|  | 1 = Disabled.
[16] | CH01TOFF1 | Setting This Bit Will Force PWM0 To Output Low Lasting For At Most One Period Cycle As Long As ACMP1 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: only for PWM0,PWM1,PWM2,PWM3.
[17] | CH11TOFF1 | Setting This Bit Will Force PWM1 To Output Low Lasting For At Most One Period Cycle As Long As ACMP1 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[18] | CH21TOFF1 | Setting This Bit Will Force PWM2 To Output Low Lasting For At Most One Period Cycle As Long As ACMP1 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[19] | CH31TOFF1 | Setting This Bit Will Force PWM3 To Output Low Lasting For At Most One Period Cycle As Long As ACMP1 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[21:20] | CMP1SEL | CMP1SEL
|  | Select the positive input source of ACMP1.
|  | 00 = Select P3.1 as the input of ACMP1.
|  | 01 = Select P3.2 as the input of ACMP1.
|  | 10 = Select P3.3 as the input of ACMP1.
|  | 11 = Select P3.4 as the input of ACMP1.
[22] | T1 | Timer1 Trigger PWM Function Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | When this bit is set, timer1 time-out event will update PHCHG with PHCHG_NXT register.
[23] | CE1 | ACMP1 Trigger Function Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit will be auto cleared when ACMP1 trigger PWM if ACCNT1 is set.
[24] | CH01TOFF0 | Setting This Bit Will Force PWM0 To Output Low Lasting For At Most One Period Cycle As Long As ACMP0 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[25] | CH11TOFF0 | Setting This Bit Will Force PWM1 To Output Low Lasting For At Most One Period Cycle As Long As ACMP0 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[26] | CH21TOFF0 | Setting This Bit Will Force PWM2 To Output Low Lasting For At Most One Period Cycle As Long As ACMP0 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[27] | CH31TOFF0 | Setting This Bit Will Force PWM3 To Output Low Lasting For At Most One Period Cycle As Long As ACMP0 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[29:28] | CMP0SEL | CMP0SEL
|  | Select the positive input source of ACMP0.
|  | 00 = Select P1.5 as the input of ACMP0.
|  | 01 = Select P1.0 as the input of ACMP0.
|  | 10 = Select P1.2 as the input of ACMP0.
|  | 11 = Select P1.3 as the input of ACMP0.
[30] | T0 | Timer0 Trigger PWM Function Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | When this bit is set, timer0 time-out event will update PHCHG with PHCHG_NXT register.
[31] | CE0 | ACMP0 Trigger Function Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit will be auto cleared when ACMP0 trigger PWM if ACCNT0 is set.

Definition at line 3572 of file Mini51Series.h.

## ◆ PHCHGMASK

PWM_T::PHCHGMASK

## Offset: 0x80 Phase Change MASK Register

Bits | Field | Descriptions
--- | --- | ---
[6] | MASK6 | MASK For D6
|  | 0 = Original GPIO P0.1.
|  | 1 = D6.
[7] | MASK7 | MASK For D7
|  | 0 = Original GPIO P0.0.
|  | 1 = D7.
[8] | CMPMASK0 | MASK For ACMP0
|  | 0 = The input of ACMP is controlled by CMP0CR.
|  | 1 = The input of ACMP is controlled by CMP0SEL of PHCHG register.
|  | Note: Register CMP0CR is describe in Comparator Controller chapter
[9] | CMPMASK1 | MASK For ACMP1
|  | 0 = The input of ACMP is controlled by CMP1CR.
|  | 1 = The input of ACMP is controlled by CMP1SEL of PHCHG register.
|  | Note: Register CMP1CR is describe in Comparator Controller chapter

Definition at line 3574 of file Mini51Series.h.

## ◆ PHCHGNXT

PWM_T::PHCHGNXT

## Offset: 0x7C Next Phase Change Register

Bits | Field | Descriptions
--- | --- | ---
[0] | D0 | D0: When PWM0 Is Zero, Channel 0's Output Waveform Is D0
|  | 0 = Output low.
|  | 1 = Output high.
[1] | D1 | D1: When PWM1 Is Zero, Channel 1's Output Waveform Is D1
|  | 0 = Output low.
|  | 1 = Output high.
[2] | D2 | D2: When PWM2 Is Zero, Channel 2's Output Waveform Is D2
|  | 0 = Output low.
|  | 1 = Output high.
[3] | D3 | D3: When PWM3 Is Zero, Channel 3's Output Waveform Is D3
|  | 0 = Output low.
|  | 1 = Output high.
[4] | D4 | D4: When PWM4 Is Zero, Channel 4's Output Waveform Is D4
|  | 0 = Output low.
|  | 1 = Output high.
[5] | D5 | D5: When PWM5 Is Zero, Channel 5's Output Waveform Is D5
|  | 0 = Output low.
|  | 1 = Output high.
[6] | D6 | D6: When MASK6 Is 1, Channel 6's Output Waveform Is D6
|  | 0 = Output low.
|  | 1 = Output high.
[7] | D7 | D7: When MASK7 Is 1, Channel 7's Output Waveform Is D7
|  | 0 = Output low.
|  | 1 = Output high.
[8] | PWM0 | PWM Channel 0 Output Enable Control
|  | 0 = Output D0 specified in bit 0 of PHCHG register.
|  | 1 = Output the original channel 0 waveform.
[9] | PWM1 | PWM Channel 1 Output Enable Control
|  | 0 = Output D1 specified in bit 1 of PHCHG register.
|  | 1 = Output the original channel 1 waveform.
[10] | PWM2 | PWM Channel 2 Output Enable Control
|  | 0 = Output D2 specified in bit 2 of PHCHG register.
|  | 1 = Output the original channel 2 waveform.
[11] | PWM3 | PWM Channel 3 Output Enable Control
|  | 0 = Output D3 specified in bit 3 of PHCHG register.
|  | 1 = Output the original channel 3 waveform.
[12] | PWM4 | PWM Channel 4 Output Enable Control
|  | 0 = Output D4 specified in bit 4 of PHCHG register.
|  | 1 = Output the original channel 4 waveform.
[13] | PWM5 | PWM Channel 5 Output Enable Control
|  | 0 = Output D5 specified in bit 5 of PHCHG register.
|  | 1 = Output the original channel 5 waveform.
[14] | ACCNT0 | Hardware Auto Clear CE0 When ACMP0 Trigger It
|  | 0 = Enabled.
|  | 1 = Disabled.
[15] | ACCNT1 | Hardware Auto Clear CE1 When ACMP1 Trigger It
|  | 0 = Enabled.
|  | 1 = Disabled.
[16] | CH01TOFF1 | Setting This Bit Will Force PWM0 To Output Low Lasting For At Most One Period Cycle As Long As ACMP1 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: only for PWM0,PWM1,PWM2,PWM3.
[17] | CH11TOFF1 | Setting This Bit Will Force PWM1 To Output Low Lasting For At Most One Period Cycle As Long As ACMP1 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[18] | CH21TOFF1 | Setting This Bit Will Force PWM2 To Output Low Lasting For At Most One Period Cycle As Long As ACMP1 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[19] | CH31TOFF1 | Setting This Bit Will Force PWM3 To Output Low Lasting For At Most One Period Cycle As Long As ACMP1 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[21:20] | CMP1SEL | CMP1SEL
|  | Select the positive input source of ACMP1.
|  | 00 = Select P3.1 as the input of ACMP1.
|  | 01 = Select P3.2 as the input of ACMP1.
|  | 10 = Select P3.3 as the input of ACMP1.
|  | 11 = Select P3.4 as the input of ACMP1.
[22] | T1 | Timer1 Trigger PWM Function Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | When this bit is set, timer1 time-out event will update PHCHG with PHCHG_NXT register.
[23] | CE1 | ACMP1 Trigger Function Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit will be auto cleared when ACMP1 trigger PWM if ACCNT1 is set.
[24] | CH01TOFF0 | Setting This Bit Will Force PWM0 To Output Low Lasting For At Most One Period Cycle As Long As ACMP0 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[25] | CH11TOFF0 | Setting This Bit Will Force PWM1 To Output Low Lasting For At Most One Period Cycle As Long As ACMP0 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[26] | CH21TOFF0 | Setting This Bit Will Force PWM2 To Output Low Lasting For At Most One Period Cycle As Long As ACMP0 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[27] | CH31TOFF0 | Setting This Bit Will Force PWM3 To Output Low Lasting For At Most One Period Cycle As Long As ACMP0 Trigger It; This Feature Is Usually In Step Motor Application
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: Only for PWM0, PWM1, PWM2, PWM3.
[29:28] | CMP0SEL | CMP0SEL
|  | Select the positive input source of ACMP0.
|  | 00 = Select P1.5 as the input of ACMP0.
|  | 01 = Select P1.0 as the input of ACMP0.
|  | 10 = Select P1.2 as the input of ACMP0.
|  | 11 = Select P1.3 as the input of ACMP0.
[30] | T0 | Timer0 Trigger PWM Function Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | When this bit is set, timer0 time-out event will update PHCHG with PHCHG_NXT register.
[31] | CE0 | ACMP0 Trigger Function Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit will be auto cleared when ACMP0 trigger PWM if ACCNT0 is set.

Definition at line 3573 of file Mini51Series.h.

## ◆ PIER

PWM_T::PIER

## Offset: 0x54 PWM Interrupt Enable Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | PWMPIE0 | PWM Channel 0 Period Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[1] | PWMPIE1 | PWM Channel 1 Period Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[2] | PWMPIE2 | PWM Channel 2 Period Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[3] | PWMPIE3 | PWM Channel 3 Period Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[4] | PWMPIE4 | PWM Channel 4 Period Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[5] | PWMPIE5 | PWM Channel 5 Period Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[8] | PWMDIE0 | PWM Channel 0 Duty Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[9] | PWMDIE1 | PWM Channel 1 Duty Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[10] | PWMDIE2 | PWM Channel 2 Duty Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[11] | PWMDIE3 | PWM Channel 3 Duty Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[12] | PWMDIE4 | PWM Channel 4 Duty Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[13] | PWMDIE5 | PWM Channel 5 Duty Interrupt Enable Control
|  | 0 = Disabled.
|  | 1 = Enabled.
[16] | BRKIE | Fault Brake0 And 1 Interrupt Enable Control
|  | 0 = Disabling flags BKF0 and BKF1 to trigger PWM interrupt.
|  | 1 = Enabling flags BKF0 and BKF1 can trigger PWM interrupt.
[17] | INT_TYPE | PWM Interrupt Type Selection Bit
|  | 0 = PWMPIFn will be set if PWM counter underflows.
|  | 1 = PWMPIFn will be set if PWM counter matches CNRn register.
|  | Note: This bit is effective when PWM in central align mode only.

Definition at line 3563 of file Mini51Series.h.

## ◆ PIIR

PWM_T::PIIR

## Offset: 0x58 PWM Interrupt Indication Register

Bits | Field | Descriptions
--- | --- | ---
[0] | PWMPIF0 | PWM Channel 0 Period Interrupt Flag
|  | Flag is set by hardware when PWM0 down counter reaches zero.
|  | Note: Software can write 1 to clear this bit.
[1] | PWMPIF1 | PWM Channel 1 Period Interrupt Flag
|  | Flag is set by hardware when PWM1 down counter reaches zero.
|  | Note: Software can write 1 to clear this bit.
[2] | PWMPIF2 | PWM Channel 2 Period Interrupt Flag
|  | Flag is set by hardware when PWM2 down counter reaches zero.
|  | Note: Software can write 1 to clear this bit.
[3] | PWMPIF3 | PWM Channel 3 Period Interrupt Flag
|  | Flag is set by hardware when PWM3 down counter reaches zero.
|  | Note: Software can write 1 to clear this bit.
[4] | PWMPIF4 | PWM Channel 4 Period Interrupt Flag
|  | Flag is set by hardware when PWM4 down counter reaches zero.
|  | Note: Software can write 1 to clear this bit.
[5] | PWMPIF5 | PWM Channel 5 Period Interrupt Flag
|  | Flag is set by hardware when PWM5 down counter reaches zero.
|  | Note: Software can write 1 to clear this bit.
[8] | PWMDIF0 | PWM Channel 0 Duty Interrupt Flag
|  | Flag is set by hardware when a channel 0 PWM counter reaches CMR0 in down-count direction.
|  | Note: Software can write 1 to clear this bit.
[9] | PWMDIF1 | PWM Channel 1 Duty Interrupt Flag
|  | Flag is set by hardware when a channel 1 PWM counter reaches CMR1 in down-count direction.
|  | Note: Software can write 1 to clear this bit.
[10] | PWMDIF2 | PWM Channel 2 Duty Interrupt Flag
|  | Flag is set by hardware when a channel 2 PWM counter reaches CMR2 in down-count direction.
|  | Note: Software can write 1 to clear this bit.
[11] | PWMDIF3 | PWM Channel 3 Duty Interrupt Flag
|  | Flag is set by hardware when a channel 3 PWM counter reaches CMR3 in down-count direction.
|  | Note: Software can write 1 to clear this bit.
[12] | PWMDIF4 | PWM Channel 4 Duty Interrupt Flag
|  | Flag is set by hardware when a channel 4 PWM counter reaches CMR4 in down-count direction.
|  | Note: Software can write 1 to clear this bit.
[13] | PWMDIF5 | PWM Channel 5 Duty Interrupt Flag
|  | Flag is set by hardware when a channel 5 PWM counter reaches CMR5 in down-count direction.
|  | Note: Software can write 1 to clear this bit.
[16] | BKF0 | PWM Brake0 Flag
|  | 0 = PWM Brake does not recognize a falling signal at BKP0.
|  | 1 = When PWM Brake detects a falling signal at pin BKP0, this flag will be set to high.
|  | Note: Software can write 1 to clear this bit.
[17] | BKF1 | PWM Brake1 Flag
|  | 0 = PWM Brake does not recognize a falling signal at BKP1.
|  | 1 = When PWM Brake detects a falling signal at pin BKP1, this flag will be set to high.
|  | Note: Software can write 1 to clear this bit.

Definition at line 3564 of file Mini51Series.h.

## ◆ PIN

GPIO_T::PIN

## Offset: 0x10 Px Pin Value

Bits | Field | Descriptions
--- | --- | ---
[7:0] | PIN | Port 0-5 Pin [N] Pin Value
|  | Each bit of the register reflects the actual status of the respective Px.n pin.
|  | If the bit is 1, it indicates the corresponding pin status is high; else the pin status is low.
|  | Note1: x = 0~5, n = 0~7.
|  | Note2:
|  | P0_PIN[3:2] are reserved.
|  | P1_PIN[7:6], [1] are reserved.
|  | P2_PIN[7], [1:0] are reserved.
|  | P3_PIN[7], [3] are reserved.
|  | P4_PIN[5:0] are reserved.
|  | P5_PIN[7:6] are reserved.

Definition at line 2078 of file Mini51Series.h.

## ◆ PMD

GPIO_T::PMD

## Offset: 0x00 Px I/O Mode Control

Bits | Field | Descriptions
--- | --- | ---
[1:0] | PMD0 | Port 0-5 I/O Pin [N] Mode Control
|  | Determine each I/O mode of Px.n pin. Default mode is controlled by CIOINI (CONFIG0[10]).
|  | 00 = Px.n is in Input mode.
|  | 01 = Px.n is in Push-pull Output mode.
|  | 10 = Px.n is in Open-drain Output mode.
|  | 11 = Px.n is in Quasi-bidirectional mode.
|  | Note1: x = 0~4, n = 0~7.
|  | Note2:
|  | P0_PMD[7:4] are reserved.
|  | P1_PMD[15:12], [3:2] are reserved.
|  | P2_PMD[15:14], [3:0] are reserved.
|  | P3_PMD[15:14], [7:6] are reserved.
|  | P4_PMD[11:0] are reserved.
|  | P5_PMD[15:12] are reserved.
[3:2] | PMD1 | Port 0-5 I/O Pin [N] Mode Control
|  | Determine each I/O mode of Px.n pin. Default mode is controlled by CIOINI (CONFIG0[10]).
|  | 00 = Px.n is in Input mode.
|  | 01 = Px.n is in Push-pull Output mode.
|  | 10 = Px.n is in Open-drain Output mode.
|  | 11 = Px.n is in Quasi-bidirectional mode.
|  | Note1: x = 0~4, n = 0~7.
|  | Note2:
|  | P0_PMD[7:4] are reserved.
|  | P1_PMD[15:12], [3:2] are reserved.
|  | P2_PMD[15:14], [3:0] are reserved.
|  | P3_PMD[15:14], [7:6] are reserved.
|  | P4_PMD[11:0] are reserved.
|  | P5_PMD[15:12] are reserved.
[5:4] | PMD2 | Port 0-5 I/O Pin [N] Mode Control
|  | Determine each I/O mode of Px.n pin. Default mode is controlled by CIOINI (CONFIG0[10]).
|  | 00 = Px.n is in Input mode.
|  | 01 = Px.n is in Push-pull Output mode.
|  | 10 = Px.n is in Open-drain Output mode.
|  | 11 = Px.n is in Quasi-bidirectional mode.
|  | Note1: x = 0~4, n = 0~7.
|  | Note2:
|  | P0_PMD[7:4] are reserved.
|  | P1_PMD[15:12], [3:2] are reserved.
|  | P2_PMD[15:14], [3:0] are reserved.
|  | P3_PMD[15:14], [7:6] are reserved.
|  | P4_PMD[11:0] are reserved.
|  | P5_PMD[15:12] are reserved.
[7:6] | PMD3 | Port 0-5 I/O Pin [N] Mode Control
|  | Determine each I/O mode of Px.n pin. Default mode is controlled by CIOINI (CONFIG0[10]).
|  | 00 = Px.n is in Input mode.
|  | 01 = Px.n is in Push-pull Output mode.
|  | 10 = Px.n is in Open-drain Output mode.
|  | 11 = Px.n is in Quasi-bidirectional mode.
|  | Note1: x = 0~4, n = 0~7.
|  | Note2:
|  | P0_PMD[7:4] are reserved.
|  | P1_PMD[15:12], [3:2] are reserved.
|  | P2_PMD[15:14], [3:0] are reserved.
|  | P3_PMD[15:14], [7:6] are reserved.
|  | P4_PMD[11:0] are reserved.
|  | P5_PMD[15:12] are reserved.
[9:8] | PMD4 | Port 0-5 I/O Pin [N] Mode Control
|  | Determine each I/O mode of Px.n pin. Default mode is controlled by CIOINI (CONFIG0[10]).
|  | 00 = Px.n is in Input mode.
|  | 01 = Px.n is in Push-pull Output mode.
|  | 10 = Px.n is in Open-drain Output mode.
|  | 11 = Px.n is in Quasi-bidirectional mode.
|  | Note1: x = 0~4, n = 0~7.
|  | Note2:
|  | P0_PMD[7:4] are reserved.
|  | P1_PMD[15:12], [3:2] are reserved.
|  | P2_PMD[15:14], [3:0] are reserved.
|  | P3_PMD[15:14], [7:6] are reserved.
|  | P4_PMD[11:0] are reserved.
|  | P5_PMD[15:12] are reserved.
[11:10] | PMD5 | Port 0-5 I/O Pin [N] Mode Control
|  | Determine each I/O mode of Px.n pin. Default mode is controlled by CIOINI (CONFIG0[10]).
|  | 00 = Px.n is in Input mode.
|  | 01 = Px.n is in Push-pull Output mode.
|  | 10 = Px.n is in Open-drain Output mode.
|  | 11 = Px.n is in Quasi-bidirectional mode.
|  | Note1: x = 0~4, n = 0~7.
|  | Note2:
|  | P0_PMD[7:4] are reserved.
|  | P1_PMD[15:12], [3:2] are reserved.
|  | P2_PMD[15:14], [3:0] are reserved.
|  | P3_PMD[15:14], [7:6] are reserved.
|  | P4_PMD[11:0] are reserved.
|  | P5_PMD[15:12] are reserved.
[13:12] | PMD6 | Port 0-5 I/O Pin [N] Mode Control
|  | Determine each I/O mode of Px.n pin. Default mode is controlled by CIOINI (CONFIG0[10]).
|  | 00 = Px.n is in Input mode.
|  | 01 = Px.n is in Push-pull Output mode.
|  | 10 = Px.n is in Open-drain Output mode.
|  | 11 = Px.n is in Quasi-bidirectional mode.
|  | Note1: x = 0~4, n = 0~7.
|  | Note2:
|  | P0_PMD[7:4] are reserved.
|  | P1_PMD[15:12], [3:2] are reserved.
|  | P2_PMD[15:14], [3:0] are reserved.
|  | P3_PMD[15:14], [7:6] are reserved.
|  | P4_PMD[11:0] are reserved.
|  | P5_PMD[15:12] are reserved.
[15:14] | PMD7 | Port 0-5 I/O Pin [N] Mode Control
|  | Determine each I/O mode of Px.n pin. Default mode is controlled by CIOINI (CONFIG0[10]).
|  | 00 = Px.n is in Input mode.
|  | 01 = Px.n is in Push-pull Output mode.
|  | 10 = Px.n is in Open-drain Output mode.
|  | 11 = Px.n is in Quasi-bidirectional mode.
|  | Note1: x = 0~4, n = 0~7.
|  | Note2:
|  | P0_PMD[7:4] are reserved.
|  | P1_PMD[15:12], [3:2] are reserved.
|  | P2_PMD[15:14], [3:0] are reserved.
|  | P3_PMD[15:14], [7:6] are reserved.
|  | P4_PMD[11:0] are reserved.
|  | P5_PMD[15:12] are reserved.

Definition at line 2074 of file Mini51Series.h.

## ◆ POE

PWM_T::POE

## Offset: 0x5C PWM Output Enable for Channel 0~5

Bits | Field | Descriptions
--- | --- | ---
[0] | PWM0 | PWM Channel 0 Output Enable Control
|  | 0 = PWM channel 0 output to pin Disabled.
|  | 1 = PWM channel 0 output to pin Enabled.
|  | Note: The corresponding GPIO pin must be switched to PWM function.
[1] | PWM1 | PWM Channel 1 Output Enable Control
|  | 0 = PWM channel 1 output to pin Disabled.
|  | 1 = PWM channel 1 output to pin Enabled.
|  | Note: The corresponding GPIO pin must be switched to PWM function.
[2] | PWM2 | PWM Channel 2 Output Enable Control
|  | 0 = PWM channel 2 output to pin Disabled.
|  | 1 = PWM channel 2 output to pin Enabled.
|  | Note: The corresponding GPIO pin must be switched to PWM function.
[3] | PWM3 | PWM Channel 3 Output Enable Control
|  | 0 = PWM channel 3 output to pin Disabled.
|  | 1 = PWM channel 3 output to pin Enabled.
|  | Note: The corresponding GPIO pin must be switched to PWM function.
[4] | PWM4 | PWM Channel 4 Output Enable Control
|  | 0 = PWM channel 4 output to pin Disabled.
|  | 1 = PWM channel 4 output to pin Enabled.
|  | Note: The corresponding GPIO pin must be switched to PWM function.
[5] | PWM5 | PWM Channel 5 Output Enable Control
|  | 0 = PWM channel 5 output to pin Disabled.
|  | 1 = PWM channel 5 output to pin Enabled.
|  | Note: The corresponding GPIO pin must be switched to PWM function.

Definition at line 3565 of file Mini51Series.h.

## ◆ PPR

PWM_T::PPR

## Offset: 0x00 PWM Pre-scale Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | CP01 | Clock Prescaler 0 For PWM Counter 0 And 1
|  | Clock input is divided by (CP01 + 1) before it is fed to the corresponding PWM counter.
|  | If CP01 = 0, the clock prescaler 0 output clock will be stopped.
|  | So the corresponding PWM counter will also be stopped.
[15:8] | CP23 | Clock Prescaler 2 For PWM Counter 2 And 3
|  | Clock input is divided by (CP23 + 1) before it is fed to the corresponding PWM counter.
|  | If CP23 = 0, the clock prescaler 2 output clock will be stopped.
|  | So the corresponding PWM counter will also be stopped.
[23:16] | CP45 | Clock Prescaler 4 For PWM Counter 4 And 5
|  | Clock input is divided by (CP45 + 1) before it is fed to the corresponding PWM counter.
|  | If CP45 = 0, the clock prescaler 4 output clock will be stopped.
|  | So the corresponding PWM counter will also be stopped.

Definition at line 3555 of file Mini51Series.h.

## ◆ PWRCON

CLK_T::PWRCON

## Offset: 0x00 System Power-down Control Register

Bits | Field | Descriptions
--- | --- | ---
[1:0] | XTLCLK_EN | External Crystal HXT Or LXT Enable Control (Write Protect)
|  | The default clock source is from HIRC.
|  | These two bits are default set to "00" and the XTAL1 and XTAL2 pins are GPIO.
|  | 00 = XTAL1 and XTAL2 are GPIO, disable both LXT & HXT (default).
|  | 01 = HXT Enabled.
|  | 10 = LXT Enabled.
|  | 11 = XTAL1 is external clock input pin, XTAL2 is GPIO.
|  | Note: To enable the external XTAL function, the P5_ALT[1:0] and P5_MFP[1:0] bits must also be set in P5_MFP.
[2] | OSC22M_EN | 22.1184 MHz Internal High Speed RC Oscillator (HIRC) Enable Control (Write Protect)
|  | 0 = 22.1184 MHz internal high speed RC oscillator (HIRC) Disabled.
|  | 1 = 22.1184 MHz internal high speed RC oscillator (HIRC) Enabled.
|  | Note: The default of OSC22M_EN bit is 1.
[3] | OSC10K_EN | 10 KHz Internal Low Speed RC Oscillator (LIRC) Enable Control (Write Protect)
|  | 0 = 10 kHz internal low speed RC oscillator (LIRC) Disabled.
|  | 1 = 10 kHz internal low speed RC oscillator (LIRC) Enabled.
[4] | PD_WU_DLY | Wake-up Delay Counter Enable Control (Write Protect)
|  | When the chip wakes up from Power-down mode, the clock control will delay certain clock cycles to wait system clock stable.
|  | The delayed clock cycle is 4096 clock cycles when chip work at 4~24 MHz external high speed crystal (HXT), 4096 clock cycles for 32.768 kHz external low speed crystal (LXT), and 16 clock cycles when chip works at 22.1184 MHz internal high speed RC oscillator (HIRC).
|  | 0 = Clock cycles delay Disabled.
|  | 1 = Clock cycles delay Enabled.
[5] | PD_WU_INT_EN | Power-down Mode Wake-up Interrupt Enable Control (Write Protect)
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: The interrupt will occur when both PD_WU_STS and PD_WU_INT_EN are high.
[6] | PD_WU_STS | Power-down Mode Wake-up Interrupt Status
|  | Set by "Power-down wake-up event", which indicates that resume from Power-down mode.
|  | The flag is set if the GPIO, UART, WDT, I2C, ACMP, Timer or BOD wake-up occurred.
|  | Note: This bit works only if PD_WU_INT_EN (PWRCON[5]) set to 1. Write 1 to clear the bit to 0.
[7] | PWR_DOWN_EN | System Power-down Enable Bit (Write Protect)
|  | When chip wakes up from Power-down mode, this bit is cleared by hardware.
|  | User needs to set this bit again for next Power-down.
|  | In Power-down mode, 4~24 MHz external high speed crystal oscillator (HXT), 32.768 kHz external low speed crystal oscillator (LXT), and the 22.1184 MHz internal high speed oscillator (HIRC) will be disabled in this mode, and 10 kHz internal low speed RC oscillator (LIRC) are not controlled by Power-down mode.
|  | In Power-down mode, the system clock is disabled, and ignored the clock source selection.
|  | The clocks of peripheral are not controlled by Power-down mode, if the peripheral clock source is from 10 kHz internal low speed oscillator.
|  | 0 = Chip operating normally or chip in Idle mode because of WFI command.
|  | 1 = Chip enters Power-down mode instantly or waits CPU sleep command WFI.
[9] | PD_32K | Enable LXT In Power-down Mode
|  | This bit controls the crystal oscillator active or not in Power-down mode.
|  | 0 = No effect to Power-down mode.
|  | 1 = If XTLCLK_EN[1:0] = 10, LXT is still active in Power-down mode.

Definition at line 844 of file Mini51Series.h.

## ◆ RBR [1/2]

UART_T::RBR

## Offset: 0x00 UART Receive Buffer Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | RBR | Receive Buffer Bits (Read Only)
|  | By reading this register, the UART Controller will return an 8-bit data received from RX pin (LSB first).

Definition at line 5321 of file Mini51Series.h.

## ◆ [2/2]

__I uint32_t { ... } ::RBR

Definition at line 5321 of file Mini51Series.h.

## ◆ RegLockAddr

GCR_T::RegLockAddr

## Offset: 0x100 Register Write-Protection Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | RegUnLock | Register Write-protection Disable Index (Read Only)
|  | 0 = Write-protection Enabled for writing protected registers.
|  | Any write to the protected register is ignored.
|  | 1 = Write-protection Disabled for writing protected registers.
|  | The Protected registers are:
|  | IPRSTC1 (0x5000_0008)
|  | BODCTL (0x5000_0018)
|  | PWRCON (0x5000_0200), bit[6] is not protected for power wake-up interrupt clear
|  | APBCLK (0x5000_0208), bit[0] watchdog clock enable only
|  | CLKSEL0 (0x5000_0210)
|  | CLKSEL1 (0x5000_0214), bit[1:0] Watchdog clock source select only
|  | NMI_SEL (0x5000_0380), bit[8] NMI interrupt enable only
|  | ISPCON (0x5000_C000)
|  | ISPTRG (0x5000_C010)
|  | WTCR (0x4000_4000)
|  | Note: The bits which are write-protected will be noted as" (Write Protect)" beside the description.
[7:0] | REGWRPROT | Register Write-protection Code (Write Only)
|  | Some registers have write-protection function.
|  | Writing these registers have to disable the protected function by writing the sequence value 0x59, 0x16, 0x88 to this field.
|  | After this sequence is completed, the REGPROTDIS bit will be set to 1 and write-protection registers can be normal write.

Definition at line 1530 of file Mini51Series.h.

## ◆ RSTSRC

GCR_T::RSTSRC

## Offset: 0x04 System Reset Source Register

Bits | Field | Descriptions
--- | --- | ---
[0] | RSTS_POR | Power-on Reset Flag
|  | The RSTS_POR flag is set by the "reset signal", which is from the Power-On Reset (POR) controller or bit CHIP_RST (IPRSTC1[0]), to indicate the previous reset source.
|  | 0 = No reset from POR or CHIP_RST.
|  | 1 = Power-on-Reset (POR) or CHIP_RST had issued the reset signal to reset the system.
|  | Note: Software can write 1 to clear this bit to 0.
[1] | RSTS_RESET | Reset Pin Reset Flag
|  | The RSTS_RESET flag is set by the "reset signal" from the /RESET pin to indicate the previous reset source.
|  | 0 = No reset from pin /RESET pin.
|  | 1 = The /RESET pin had issued the reset signal to reset the system.
|  | Note: Software can write 1 to clear this bit to 0.
[2] | RSTS_WDT | Watchdog Reset Flag
|  | The RSTS_WDT flag is set by the "reset signal" from the Watchdog timer to indicate the previous reset source.
|  | 0 = No reset from Watchdog timer.
|  | 1 = The Watchdog timer had issued the reset signal to reset the system.
|  | Note: Software can write 1 to clear this bit to 0.
[4] | RSTS_BOD | Brown-out Detector Reset Flag
|  | The RSTS_BOD flag is set by the "reset signal" from the Brown-out Detector to indicate the previous reset source.
|  | 0 = No reset from BOD.
|  | 1 = The BOD had issued the reset signal to reset the system.
|  | Note: Software can write 1 to clear this bit to 0.
[5] | RSTS_MCU | MCU Reset Flag
|  | The RSTS_MCU flag is set by the "reset signal" from the Cortex-M0 core to indicate the previous reset source.
|  | 0 = No reset from Cortex-M0.
|  | 1 = The Cortex-M0 had issued the reset signal to reset the system by writing 1 to bit SYSRESETREQ (AIRCR[2]), Application Interrupt and Reset Control Register, address = 0xE000ED0C in system control registers of Cortex-M0 core.
|  | Note: Software can write 1 to clear this bit to 0.
[7] | RSTS_CPU | CPU Reset Flag
|  | The RSTS_CPU flag is set by hardware if software writes CPU_RST (IPRSTC1[1]) 1 to reset Cortex-M0 core and Flash memory controller (FMC).
|  | 0 = No reset from CPU.
|  | 1 = Cortex-M0 core and FMC are reset by software setting CPU_RST to 1.
|  | Note: Software can write 1 to clear this bit to 0.

Definition at line 1505 of file Mini51Series.h.

## ◆ RX

SPI_T::RX

## Offset: 0x10 SPI Data Receive Register

Bits | Field | Descriptions
--- | --- | ---
[31:0] | RX | Data Receive Bits (Read Only)
|  | The Data Receive Registers hold the value of received data of the last executed transfer.
|  | Valid bits depend on the transmit bit length field in the SPI_CNTRL register.
|  | For example, if TX_BIT_LEN is set to 0x08, bit RX [7:0] holds the received data.
|  | The values of the other bits are unknown.

Definition at line 4479 of file Mini51Series.h.

## ◆ SRC0

INT_T::SRC0

## Offset: 0x00 IRQ0 (BOD) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2680 of file Mini51Series.h.

## ◆ SRC1

INT_T::SRC1

## Offset: 0x04 IRQ1 (WDT) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2681 of file Mini51Series.h.

## ◆ SRC12

INT_T::SRC12

## Offset: 0x30 IRQ12 (UART) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2693 of file Mini51Series.h.

## ◆ SRC14

INT_T::SRC14

## Offset: 0x38 IRQ14 (SPI) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2697 of file Mini51Series.h.

## ◆ SRC16

INT_T::SRC16

## Offset: 0x40 IRQ16 (GP5) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2701 of file Mini51Series.h.

## ◆ SRC17

INT_T::SRC17

## Offset: 0x44 IRQ17 (HIRC trim) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2702 of file Mini51Series.h.

## ◆ SRC18

INT_T::SRC18

## Offset: 0x48 IRQ18 (I2C) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2703 of file Mini51Series.h.

## ◆ SRC2

INT_T::SRC2

## Offset: 0x08 IRQ2 (EINT0) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2682 of file Mini51Series.h.

## ◆ SRC25

INT_T::SRC25

## Offset: 0x64 IRQ25 (ACMP) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2707 of file Mini51Series.h.

## ◆ SRC28

INT_T::SRC28

## Offset: 0x70 IRQ28 (PWRWU) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2711 of file Mini51Series.h.

## ◆ SRC29

INT_T::SRC29

## Offset: 0x74 IRQ29 (ADC) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2712 of file Mini51Series.h.

## ◆ SRC3

INT_T::SRC3

## Offset: 0x0C IRQ3 (EINT1) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2683 of file Mini51Series.h.

## ◆ SRC4

INT_T::SRC4

## Offset: 0x10 IRQ4 (GP0/1) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2684 of file Mini51Series.h.

## ◆ SRC5

INT_T::SRC5

## Offset: 0x14 IRQ5 (GP2/3/4) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2685 of file Mini51Series.h.

## ◆ SRC6

INT_T::SRC6

## Offset: 0x18 IRQ6 (PWM) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2686 of file Mini51Series.h.

## ◆ SRC7

INT_T::SRC7

## Offset: 0x1C IRQ7 (BRAKE) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2687 of file Mini51Series.h.

## ◆ SRC8

INT_T::SRC8

## Offset: 0x20 IRQ8 (TMR0) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2688 of file Mini51Series.h.

## ◆ SRC9

INT_T::SRC9

## Offset: 0x24 IRQ9 (TMR1) Interrupt Source Identity

Bits | Field | Descriptions
--- | --- | ---
[2:0] | INT_SRC | Interrupt Source
|  | Define the interrupt sources for interrupt event.

Definition at line 2689 of file Mini51Series.h.

## ◆ SSR

SPI_T::SSR

## Offset: 0x08 SPI Slave Select Register

Bits | Field | Descriptions
--- | --- | ---
[0] | SSR | Slave Select Control Bit (Master Only)
|  | If AUTOSS bit is 0,
|  | 0 = Set the SPISS line to inactive state.
|  | 1 = Set the proper SPISS line to active state.
|  | If AUTOSS bit is 1,
|  | 0 = Keep the SPISS line at inactive state.
|  | 1 = Select the SPISS line to be automatically driven to active state for the duration of transmission/reception, and will be driven to inactive state for the rest of the time.
|  | The active state of SPISS is specified in SS_LVL bit.
[2] | SS_LVL | Slave Select Active Level (Slave Only)
|  | It defines the active status of slave select signal (SPISS).
|  | If SS_LTRIG bit is 1:
|  | 0 = The slave select signal SPISS is active at Low-level.
|  | 1 = The slave select signal SPISS is active at High-level.
|  | If SS_LTRIG bit is 0:
|  | 0 = The slave select signal SPISS is active at Falling-edge.
|  | 1 = The slave select signal SPISS is active at Rising-edge.
[3] | AUTOSS | Automatic Slave Selection Function Enable Bit (Master Only)
|  | 0 = SPISS pin signal will be asserted/de-asserted by setting /clearing SSR bit.
|  | 1 = SPISS pin signal will be generated automatically, which means that slave select signal will be asserted by the SPI controller when transmit/receive is started by setting GO_BUSY, and will be de-asserted after each transmit/receive is finished.
[4] | SS_LTRIG | Slave Select Level Trigger Enable Bit (Slave Only)
|  | 0 = The input slave select signal is edge-trigger.
|  | 1 = The input slave select signal is level-trigger.
[5] | LTRIG_FLAG | Level Trigger Flag (Read Only, Slave Only)
|  | When the SS_LTRIG bit is set in Slave mode, this bit can be read to indicate the received bit number is met the requirement or not.
|  | 0 = The transaction number or the transferred bit length of one transaction does not meet the specified requirements.
|  | 1 = The transaction number and the transferred bit length met the specified requirements which defined in TX_BIT_LEN.

Definition at line 4475 of file Mini51Series.h.

## ◆ STATUS

SPI_T::STATUS

## Offset: 0x44 SPI Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | RX_INTSTS | Receive FIFO Threshold Interrupt Status (Read Only)
|  | 0 = The valid data count within the Rx FIFO buffer is smaller than or equal to the setting value of RX_THRESHOLD.
|  | 1 = The valid data count within the receive FIFO buffer is larger than the setting value of RX_THRESHOLD.
|  | Note: If RX_INTEN = 1 and RX_INTSTS = 1, the SPI controller will generate a SPI interrupt request.
[2] | RX_OVERRUN | Receive FIFO Overrun Status
|  | When the receive FIFO buffer is full, the follow-up data will be dropped and this bit will be set to 1.
|  | 0 = No overrun in receive FIFO.
|  | 1 = Overrun in receive FIFO.
|  | Note: This bit will be cleared by writing 1 to itself.
[4] | TX_INTSTS | Transmit FIFO Threshold Interrupt Status (Read Only)
|  | 0 = The valid data count within the transmit FIFO buffer is larger than the setting value of TX_THRESHOLD.
|  | 1 = The valid data count within the transmit FIFO buffer is less than or equal to the setting value of TX_THRESHOLD.
|  | Note: If TX_INTEN = 1 and TX_INTSTS = 1, the SPI controller will generate a SPI interrupt request.
[11] | SLV_START_INTSTS | Slave Start Interrupt Status (Slave Only)
|  | It is used to dedicate that the transfer has started in slave 3-wire mode.
|  | 0 = Slave does not detect any SPI bus clock transfer since the SSTA_INTEN bit was set to 1.
|  | 1 = The transfer has started in slave 3-wire mode.
|  | Note 1: It will be cleared as transfer done or by writing one to this bit.
|  | Note 2: It's a mutual mirror bit of SPI_CNTRL2[11].
[15:12] | RX_FIFO_COUNT | Receive FIFO Data Count (Read Only)
|  | Indicates the valid data count of receive FIFO buffer.
[16] | IF | SPI Unit-transfer Interrupt Flag
|  | 0 = The transfer does not finish yet.
|  | 1 = The SPI controller has finished one unit transfer.
|  | Note 1: This bit will be cleared by writing 1 to itself.
|  | Note 2: It's a mutual mirror bit of SPI_CNTRL[16].
[20] | TIMEOUT | Time-out Interrupt Flag
|  | 0 = No receive FIFO time-out event.
|  | 1 = The receive FIFO buffer is not empty and it does not be read over 64 SPI clock periods in Master mode or over 576 SPI peripheral clock periods in Slave mode.
|  | When the received FIFO buffer is read by software, the time-out status will be cleared automatically.
|  | Note: This bit will be cleared by writing 1 to itself.
[24] | RX_EMPTY | Receive FIFO Buffer Empty Indicator (Read Only)
|  | 0 = The receive FIFO buffer is not empty.
|  | 1 = The receive FIFO buffer is empty.
|  | Note: It's a mutual mirror bit of SPI_CNTRL[24].
[25] | RX_FULL | Receive FIFO Buffer Full Indicator (Read Only)
|  | 0 = The receive FIFO buffer is not full.
|  | 1 = The receive FIFO buffer is full.
|  | Note: It's a mutual mirror bit of SPI_CNTRL[25].
[26] | TX_EMPTY | Transmit FIFO Buffer Empty Indicator (Read Only)
|  | 0 = The transmit FIFO buffer is not empty.
|  | 1 = The transmit FIFO buffer is empty.
|  | Note: It's a mutual mirror bit of SPI_CNTRL[26].
[27] | TX_FULL | Transmit FIFO Buffer Full Indicator (Read Only)
|  | 0 = The transmit FIFO buffer is not full.
|  | 1 = The transmit FIFO buffer is full.
|  | Note: It's a mutual mirror bit of SPI_CNTRL[27].
[31:28] | TX_FIFO_COUNT | Transmit FIFO Data Count (Read Only)
|  | Indicates the valid data count of transmit FIFO buffer.

Definition at line 4489 of file Mini51Series.h.

## ◆ TCAP

TIMER_T::TCAP

## Offset: 0x10 Timer Capture Data Register

Bits | Field | Descriptions
--- | --- | ---
[23:0] | TCAP | Timer Capture Data Register
|  | When TEXIF flag is set to 1, the current TDR value will be auto-loaded into this TCAP filed immediately.

Definition at line 4823 of file Mini51Series.h.

## ◆ TCMPR

TIMER_T::TCMPR

## Offset: 0x04 Timer Compare Register

Bits | Field | Descriptions
--- | --- | ---
[23:0] | TCMP | Timer Compared Value
|  | TCMP is a 24-bit compared value register.
|  | When the internal 24-bit up counter value is equal to TCMP value, the TIF flag will set to 1.
|  | Time-out period = (Period of Timer clock source) * (8-bit PRESCALE + 1) * (24-bit TCMP).
|  | Note1: Never write 0x0 or 0x1 in TCMP field, or the core will run into unknown state.

Definition at line 4820 of file Mini51Series.h.

## ◆ TCSR

TIMER_T::TCSR

## Offset: 0x00 Timer Control and Status Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | PRESCALE | Prescale Counter
|  | Timer input clock source is divided by (PRESCALE+1) before it is fed to the Timer up counter.
|  | If this field is 0 (PRESCALE = 0), then there is no scaling.
[16] | TDR_EN | Data Load Enable Control
|  | When TDR_EN is set, TDR (Timer Data Register) will be updated continuously with the 24-bit up-timer value as the timer is counting.
|  | 0 = Timer Data Register update Disabled.
|  | 1 = Timer Data Register update Enabled while Timer counter is active.
[17] | PERIODIC_SEL | Periodic Mode Behavior Selection
|  | 0 = In One-shot or Periodic mode, when write new TCMP, timer counter will reset.
|  | 1 = In One-shot or Periodic mode, when write new TCMP if new TCMP > TDR(current counter) , timer counter keep counting and will not reset.
|  | If new TCMP <= TDR(current counter) , timer counter will reset.
[18] | TOUT_PIN | Toggle Out Pin Selection
|  | When Timer is set to toggle mode,
|  | 0 = Time0/1 toggle output pin is T0/T1 pin.
|  | 1 = Time0/1 toggle output pin is T0EX/T1EX pin.
[19] | CAP_SRC | Capture Pin Source Selection
|  | 0 = Capture Function source is from TxEX pin.
|  | 1 = Capture Function source is from ACMPx output signal.
[23] | WAKE_EN | Wake-up Enable Control
|  | When WAKE_EN (UA_IER[6]) is set and the TIF or TEXIF (TEXISR[0]) is set, the timer controller will generator a wake-up trigger event to CPU.
|  | 0 = Wake-up trigger event Disabled.
|  | 1 = Wake-up trigger event Enabled.
[24] | CTB | Counter Mode Enable Control
|  | This bit is for external counting pin function enabled.
|  | When timer is used as an event counter, this bit should be set to 1 and select HCLK as timer clock source.
|  | Please refer to section 6.12.5.3 for detail description.
|  | 0 = External event counter mode Disabled.
|  | 1 = External event counter mode Enabled.
[25] | CACT | Timer Active Status (Read Only)
|  | This bit indicates the 24-bit up counter status.
|  | 0 = 24-bit up counter is not active.
|  | 1 = 24-bit up counter is active.
[26] | CRST | Timer Reset
|  | 0 = No effect.
|  | 1 = Reset 8-bit prescale counter, 24-bit up counter value and CEN bit if CACT is 1.
[28:27] | MODE | Timer Operating Mode
|  | 00 = The timer is operating in the One-shot mode.
|  | The associated interrupt signal is generated once (if IE is enabled) and CEN is automatically cleared by hardware.
|  | 01 = The timer is operating in Periodic mode.
|  | The associated interrupt signal is generated periodically (if IE is enabled).
|  | 10 = The timer is operating in Toggle mode.
|  | The interrupt signal is generated periodically (if IE is enabled).
|  | The associated signal (tout) is changing back and forth with 50% duty cycle.
|  | 11 = The timer is operating in Continuous Counting mode.
|  | The associated interrupt signal is generated when TDR = TCMPR (if IE is enabled).
|  | However, the 24-bit up-timer counts continuously.
|  | Please refer to 6.12.5.2 for detailed description about Continuous Counting mode operation.
[29] | IE | Interrupt Enable Control
|  | 0 = Timer Interrupt function Disabled.
|  | 1 = Timer Interrupt function Enabled.
|  | If this bit is enabled, when the timer interrupt flag (TIF) is set to 1, the timer interrupt signal is generated and inform to CPU.
[30] | CEN | Timer Enable Control
|  | 0 = Stops/Suspends counting.
|  | 1 = Starts counting.
|  | Note1: In stop status, and then set CEN to 1 will enable the 24-bit up counter to keep counting from the last stop counting value.
|  | Note2: This bit is auto-cleared by hardware in one-shot mode (MODE (TCSRx[28:27]) = 00) when the timer interrupt flag (TIF) is generated.
[31] | DBGACK_TMR | ICE Debug Mode Acknowledge Disable Control (Write Protect)
|  | 0 = ICE debug mode acknowledgement effects TIMER counting.
|  | Timer counter will be held while CPU is held by ICE.
|  | 1 = ICE debug mode acknowledgement Disabled.
|  | Timer counter will keep going no matter CPU is held by ICE or not.

Definition at line 4819 of file Mini51Series.h.

## ◆ TDR

TIMER_T::TDR

## Offset: 0x0C Timer Data Register

Bits | Field | Descriptions
--- | --- | ---
[23:0] | TDR | Timer Data Register
|  | If TDR_EN (TCSRx[16]) is set to 1, TDR register value will be updated continuously to monitor 24-bit up counter value.

Definition at line 4822 of file Mini51Series.h.

## ◆ TEXCON

TIMER_T::TEXCON

## Offset: 0x14 Timer External Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | TX_PHASE | Timer External Count Pin Phase Detect Selection
|  | This bit indicates the detection phase of Tx (x = 0~1) pin.
|  | 0 = A falling edge of Tx (x = 0~1) pin will be counted.
|  | 1 = A rising edge of Tx (x = 0~1) pin will be counted.
[2:1] | TEX_EDGE | Timer External Pin Edge Detection
|  | 00 = A 1 to 0 transition on TxEX (x = 0~1) will be detected.
|  | 01 = A 0 to 1 transition on TxEX (x = 0~1) will be detected.
|  | 10 = Either 1 to 0 or 0 to 1 transition on TxEX (x = 0~1) will be detected.
|  | 11 = Reserved.
[3] | TEXEN | Timer External Pin Function Enable Control
|  | This bit enables the RSTCAPSEL function on the TxEX (x = 0~1) pin.
|  | 0 = RSTCAPSEL function of TxEX (x = 0~1) pin will be ignored.
|  | 1 = RSTCAPSEL function of TxEX (x = 0~1) pin is active.
[4] | RSTCAPSEL | Timer External Reset Counter / Timer External Capture Mode Selection
|  | 0 = Transition on TxEX (x = 0~1) pin is using to save the TDR value into TCAP value if TEXIF flag is set to 1.
|  | 1 = Transition on TxEX (x = 0~1) pin is using to reset the 24-bit up counter.
[5] | TEXIEN | Timer External Capture Interrupt Enable Control
|  | 0 = TxEX (x = 0~1) pin detection Interrupt Disabled.
|  | 1 = TxEX (x = 0~1) pin detection Interrupt Enabled.
|  | If TEXIEN enabled, Timer will raise an external capture interrupt signal and inform to CPU while TEXIF flag is set to 1.
[6] | TEXDB | Timer External Capture Input Pin De-bounce Enable Control
|  | 0 = TxEX (x = 0~1) pin de-bounce Disabled.
|  | 1 = TxEX (x = 0~1) pin de-bounce Enabled.
|  | If this bit is enabled, the edge detection of TxEX (x = 0~1) pin is detected with de-bounce circuit.
[7] | TCDB | Timer External Counter Input Pin De-bounce Enable Control
|  | 0 = Tx (x = 0~1) pin de-bounce Disabled.
|  | 1 = Tx (x = 0~1) pin de-bounce Enabled.
|  | If this bit is enabled, the edge detection of Tx (x = 0~1) pin is detected with de-bounce circuit.
[8] | CAP_MODE | Capture Mode Selection
|  | 0 = Timer counter reset function or free-counting mode of timer capture function.
|  | 1 = Trigger-counting mode of timer capture function.

Definition at line 4824 of file Mini51Series.h.

## ◆ TEXISR

TIMER_T::TEXISR

## Offset: 0x18 Timer External Interrupt Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | TEXIF | Timer External Interrupt Flag
|  | This bit indicates the external capture interrupt flag status
|  | When TEXEN enabled, TxEX (x = 0, 1) pin selected as external capture function, and a transition on TxEX (x = 0, 1) pin matched the TEX_EDGE setting, this flag will set to 1 by hardware.
|  | 0 = TxEX (x = 0, 1) pin interrupt did not occur.
|  | 1 = TxEX (x = 0, 1) pin interrupt occurred.
|  | Note: This bit is cleared by writing 1 to it

Definition at line 4825 of file Mini51Series.h.

## ◆ THR [1/2]

UART_T::THR

## Offset: 0x00 UART Transmit Holding Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | THR | Transmit Holding Bits
|  | By writing to this register, the UART sends out an 8-bit data through the TX pin (LSB first).

Definition at line 5322 of file Mini51Series.h.

## ◆ [2/2]

__O uint32_t { ... } ::THR

Definition at line 5322 of file Mini51Series.h.

## ◆ TISR

TIMER_T::TISR

## Offset: 0x08 Timer Interrupt Status Register

Bits | Field | Descriptions
--- | --- | ---
[0] | TIF | Timer Interrupt Flag
|  | This bit indicates the interrupt flag status of Timer while TDR value reaches to TCMP value.
|  | 0 = No effect.
|  | 1 = TDR value matches the TCMP value.
|  | Note: This bit is cleared by writing 1 to it.
[1] | TWF | Timer Wake-up Flag
|  | This bit indicates the interrupt wake-up flag status of Time.
|  | 0 = Timer does not cause chip wake-up.
|  | 1 = Chip wake-up from Idle or Power-down mode if Timer time-out interrupt signal generated.
|  | Note: This bit is cleared by writing 1 to it.

Definition at line 4821 of file Mini51Series.h.

## ◆ TOR

UART_T::TOR

## Offset: 0x20 UART Time-out Register

Bits | Field | Descriptions
--- | --- | ---
[7:0] | TOIC | Time-out Interrupt Comparator
|  | The time-out counter resets and starts counting (the counting clock = baud rate) whenever the RX FIFO receives a new data word.
|  | Once the content of time-out counter (TOUT_CNT) is equal to that of time-out interrupt comparator (TOIC), a receiver time-out interrupt (TOUT_INT) is generated if RTO_IEN (UA_IER [4]).
|  | A new incoming data word or RX FIFO empty clears TOUT_INT.
|  | In order to avoid receiver time-out interrupt generation immediately during one character is being received, TOIC value should be set between 40 and 255.
|  | So, for example, if TOIC is set with 40, the time-out interrupt is generated after four characters are not received when 1 stop bit and no parity check is set for UART transfer.
[15:8] | DLY | TX Delay Time Value
|  | This field is used to program the transfer delay time between the last stop bit and next start bit.

Definition at line 5331 of file Mini51Series.h.

## ◆ TRGCON0

PWM_T::TRGCON0

## Offset: 0x68 PWM Trigger Control Register 0

Bits | Field | Descriptions
--- | --- | ---
[0] | CM0TRGREN | Enable PWM Trigger ADC Function While Channel0's Counter Matching CMR0 In Up-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[1] | CNT0TRGEN | Enable PWM Trigger ADC Function While Channel0's Counter Matching CNR0
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[2] | CM0TRGFEN | Enable PWM Trigger ADC Function While Channel0's Counter Matching CMR0 In Down-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[3] | P0TRGEN | Enable PWM Trigger ADC Function While Channel0's Counter Matching 0
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[8] | CM1TRGREN | Enable PWM Trigger ADC Function While Channel1's Counter Matching CMR1 In Up-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[9] | CNT1TRGEN | Enable PWM Trigger ADC Function While Channel1's Counter Matching CNR1
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[10] | CM1TRGFEN | Enable PWM Trigger ADC Function While Channel1's Counter Matching CMR1 In Down-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[11] | P1TRGEN | Enable PWM Trigger ADC Function While Channel1's Counter Matching 0
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[16] | CM2TRGREN | Enable PWM Trigger ADC Function While Channel2's Counter Matching CMR2 In Up-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[17] | CNT2TRGEN | Enable PWM Trigger ADC Function While Channel2's Counter Matching CNR2
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[18] | CM2TRGFEN | Enable PWM Trigger ADC Function While Channel2's Counter Matching CMR2 In Down-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[19] | P2TRGEN | Enable PWM Trigger ADC Function While Channel2's Counter Matching 0
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[24] | CM3TRGREN | Enable PWM Trigger ADC Function While Channel3's Counter Matching CMR3 In Up-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[25] | CNT3TRGEN | Enable PWM Trigger ADC Function While Channel3's Counter Matching CNR3
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[26] | CM3TRGFEN | Enable PWM Trigger ADC Function While Channel3's Counter Matching CMR3 In Down-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[27] | P3TRGEN | Enable PWM Trigger ADC Function While Channel3's Counter Matching 0
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.

Definition at line 3568 of file Mini51Series.h.

## ◆ TRGCON1

PWM_T::TRGCON1

## Offset: 0x6C PWM Trigger Control Register 1

Bits | Field | Descriptions
--- | --- | ---
[0] | CM4TRGREN | Enable PWM Trigger ADC Function While Channel4's Counter Matching CMR4 In Up-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[1] | CNT4TRGEN | Enable PWM Trigger ADC Function While Channel4's Counter Matching CNR4
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[2] | CM4TRGFEN | Enable PWM Trigger ADC Function While Channel4's Counter Matching CMR4 In Down-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[3] | P4TRGEN | Enable PWM Trigger ADC Function While Channel4's Counter Matching 0
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[8] | CM5TRGREN | Enable PWM Trigger ADC Function While Channel5's Counter Matching CMR5 In Up-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[9] | CNT5TRGEN | Enable PWM Trigger ADC Function While Channel5's Counter Matching CNR5
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is only valid for PWM in center aligned mode.
|  | When PWM is in edged aligned mode, setting this bit is meaningless and will not take any effect.
[10] | CM5TRGFEN | Enable PWM Trigger ADC Function While Channel5's Counter Matching CMR5 In Down-count Direction
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.
[11] | P5TRGEN | Enable PWM Trigger ADC Function While Channel5's Counter Matching 0
|  | 0 = Disabled.
|  | 1 = Enabled.
|  | Note: This bit is valid for both center aligned mode and edged aligned mode.

Definition at line 3569 of file Mini51Series.h.

## ◆ TRGSTS0

PWM_T::TRGSTS0

## Offset: 0x70 PWM Trigger Status Register 0

Bits | Field | Descriptions
--- | --- | ---
[0] | CMR0FLAG_R | ADC Trigger Flag By Counting Up To CMR
|  | Note: Software can write 1 to clear this bit.
[1] | CNT0FLAG | ADC Trigger Flag By Counting To CNR
|  | Note: Software can write 1 to clear this bit.
[2] | CMR0FLAG_F | ADC Trigger Flag By Counting Down To CMR
|  | Note: Software can write 1 to clear this bit.
[3] | PERID0FLAG | ADC Trigger Flag By Period
|  | Note: Software can write 1 to clear this bit.
[8] | CMR1FLAG_R | ADC Trigger Flag By Counting Up To CMR
|  | Note: Software can write 1 to clear this bit.
[9] | CNT1FLAG | ADC Trigger Flag By Counting To CNR
|  | Note: Software can write 1 to clear this bit.
[10] | CMR1FLAG_F | ADC Trigger Flag By Counting Down To CMR
|  | Note: Software can write 1 to clear this bit.
[11] | PERID1FLAG | ADC Trigger Flag By Period
|  | Note: Software can write 1 to clear this bit.
[16] | CMR2FLAG_R | ADC Trigger Flag By Counting Up To CMR
|  | Note: Software can write 1 to clear this bit.
[17] | CNT2FLAG | ADC Trigger Flag By Counting To CNR
|  | Note: Software can write 1 to clear this bit.
[18] | CMR2FLAG_F | ADC Trigger Flag By Counting Down To CMR
|  | Note: Software can write 1 to clear this bit.
[19] | PERID2FLAG | ADC Trigger Flag By Period
|  | Note: Software can write 1 to clear this bit.
[24] | CMR3FLAG_R | When Counter Counting Up To CMR, This Bit Will Be Set For Trigger ADC
|  | Note: Software can write 1 to clear this bit.
[25] | CNT3FLAG | When Counter Counting To CNR, This Bit Will Be Set For Trigger ADC
|  | Note: Software can write 1 to clear this bit.
[26] | CMR3FLAG_F | When Counter Counting Down To CMR, This Bit Will Be Set For Trigger ADC
|  | Note: Software can write 1 to clear this bit.
[27] | PERID3FLAG | When Counter Counting To Period, This Bit Will Be Set For Trigger ADC
|  | Note: Software can write 1 to clear this bit.

Definition at line 3570 of file Mini51Series.h.

## ◆ TRGSTS1

PWM_T::TRGSTS1

## Offset: 0x74 PWM Trigger Status Register 1

Bits | Field | Descriptions
--- | --- | ---
[0] | CMR4FLAG_R | ADC Trigger Flag By Counting Up To CMR
|  | Note: Software can write 1 to clear this bit.
[1] | CNT4FLAG | ADC Trigger Flag By Counting To CNR
|  | Note: Software can write 1 to clear this bit.
[2] | CMR4FLAG_F | ADC Trigger Flag By Counting Down To CMR
|  | Note: Software can write 1 to clear this bit.
[3] | PERID4FLAG | ADC Trigger Flag By Period
|  | Note: Software can write 1 to clear this bit.
[8] | CMR5FLAG_R | ADC Trigger Flag By Counting Up To CMR
|  | Note: Software can write 1 to clear this bit.
[9] | CNT5FLAG | ADC Trigger Flag By Counting To CNR
|  | Note: Software can write 1 to clear this bit.
[10] | CMR5FLAG_F | ADC Trigger Flag By Counting Down To CMR
|  | Note: Software can write 1 to clear this bit.
[11] | PERID5FLAG | ADC Trigger Flag By Period
|  | Note: Software can write 1 to clear this bit.

Definition at line 3571 of file Mini51Series.h.

## ◆ TX

SPI_T::TX

## Offset: 0x20 SPI Data Transmit Register

Bits | Field | Descriptions
--- | --- | ---
[31:0] | TX | Data Transmit Bits (Write Only)
|  | The Data Transmit Registers hold the data to be transmitted in the next transfer.
|  | Valid bits depend on the transmit bit length field in the CNTRL register.
|  | For example, if TX_BIT_LEN is set to 0x08, the bit TX [7:0] will be transmitted in next transfer.

Definition at line 4483 of file Mini51Series.h.

## ◆ WTCR

WDT_T::WTCR

## Offset: 0x00 Watchdog Timer Control Register

Bits | Field | Descriptions
--- | --- | ---
[0] | WTR | Reset Watchdog Timer Up Counter (Write Protect)
|  | 0 = No effect.
|  | 1 = Reset the internal 18-bit WDT up counter value.
|  | Note: This bit will be automatically cleared by hardware.
[1] | WTRE | Watchdog Timer Time-out Reset Enable Control (Write Protect)
|  | Setting this bit will enable the WDT time-out reset function if the WDT up counter value has not been cleared after the specific WDT reset delay period (1024 * TWDT) expires.
|  | 0 = WDT time-out reset function Disabled.
|  | 1 = WDT time-out reset function Enabled.
[2] | WTRF | Watchdog Timer Time-out Reset Flag
|  | This bit indicates the system has been reset by WDT time-out reset or not.
|  | 0 = WDT time-out reset did not occur.
|  | 1 = WDT time-out reset occurred.
|  | Note: This bit is cleared by writing 1 to it.
[3] | WTIF | Watchdog Timer Time-out Interrupt Flag
|  | This bit will be set to 1 while WDT up counter value reaches the selected WDT time-out interval.
|  | 0 = WDT time-out interrupt did not occur.
|  | 1 = WDT time-out interrupt occurred.
|  | Note: This bit is cleared by writing 1 to it.
[4] | WTWKE | Watchdog Timer Time-out Wake-up Function Control (Write Protect)
|  | If this bit is set to 1, while WTIF is generated to 1 and WTIE enabled, the WDT time-out interrupt signal will generate a wake-up trigger event to chip.
|  | 0 = Wake-up trigger event Disabled if WDT time-out interrupt signal generated.
|  | 1 = Wake-up trigger event Enabled if WDT time-out interrupt signal generated.
|  | Note: Chip can be woken-up by WDT time-out interrupt signal generated only if WDT clock source is selected to 10 kHz oscillator.
[5] | WTWKF | Watchdog Timer Time-out Wake-up Flag
|  | This bit indicates the interrupt wake-up flag status of WDT.
|  | 0 = WDT does not cause chip wake-up.
|  | 1 = Chip wake-up from Idle or Power-down mode if WDT time-out interrupt signal generated.
|  | Note: This bit is cleared by writing 1 to it.
[6] | WTIE | Watchdog Timer Time-out Interrupt Enable Control (Write Protect)
|  | If this bit is enabled, the WDT time-out interrupt signal is generated and inform to CPU.
|  | 0 = WDT time-out interrupt Disabled.
|  | 1 = WDT time-out interrupt Enabled.
[7] | WTE | Watchdog Timer Enable Control (Write Protect)
|  | 0 = WDT Disabled. (This action will reset the internal up counter value.)
|  | 1 = WDT Enabled.
[10:8] | WTIS | Watchdog Timer Interval Selection
|  | These three bits select the time-out interval for the Watchdog Timer.
|  | 000 = 24 * TWDT.
|  | 001 = 26 * TWDT.
|  | 010 = 28 * TWDT.
|  | 011 = 210 * TWDT.
|  | 100 = 212 * TWDT.
|  | 101 = 214 * TWDT.
|  | 110 = 216 * TWDT.
|  | 111 = 218 * TWDT.
[31] | DBGACK_WDT | ICE Debug Mode Acknowledge Disable Control (Write Protect)
|  | 0 = ICE debug mode acknowledgement effects WDT counting.
|  | WDT up counter will be kept while CPU is hanging by ICE.
|  | 1 = ICE debug mode acknowledgement Disabled.
|  | WDT up counter will keep going no matter CPU is hanging by ICE or not.

Definition at line 5625 of file Mini51Series.h.