| MINI51DE_BSP V3.02.004 The Board Support Package for Mini51DE Series MCU

Macros | Functions
fmc.h File Reference

MINI51 series FMC driver header file. More...

This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Macros
#define | FMC_APROM_BASE 0x00000000UL
#define | FMC_LDROM_BASE 0x00100000UL
#define | FMC_LDROM_END 0x00100800UL
#define | FMC_CONFIG_BASE 0x00300000UL
#define | FMC_FLASH_PAGE_SIZE 0x200
#define | FMC_LDROM_SIZE 0x800
#define | FMC_TIMEOUT_READ
#define | FMC_TIMEOUT_WRITE
#define | FMC_TIMEOUT_ERASE
#define | FMC_TIMEOUT_CHKSUM
#define | FMC_ISPCMD_READ 0x00
#define | FMC_ISPCMD_PROGRAM 0x21
#define | FMC_ISPCMD_PAGE_ERASE 0x22
#define | FMC_ISPCMD_READ_CID 0x0B
#define | FMC_ISPCMD_READ_PID 0x0C
#define | FMC_ISPCMD_READ_UID 0x04
#define | FMC_ISPCMD_VECMAP 0x2E
#define | FMC_SET_APROM_BOOT() (FMC->ISPCON &= ~FMC_ISPCON_BS_Msk)
#define | FMC_SET_LDROM_BOOT() (FMC->ISPCON |= FMC_ISPCON_BS_Msk)
#define | FMC_DISABLE_AP_UPDATE() (FMC->ISPCON &= ~FMC_ISPCON_APUEN_Msk)
#define | FMC_DISABLE_CFG_UPDATE() (FMC->ISPCON &= ~FMC_ISPCON_CFGUEN_Msk)
#define | FMC_DISABLE_LD_UPDATE() (FMC->ISPCON &= ~FMC_ISPCON_LDUEN_Msk)
#define | FMC_DISABLE_ISP() (FMC->ISPCON &= ~FMC_ISPCON_ISPEN_Msk)
#define | FMC_ENABLE_AP_UPDATE() (FMC->ISPCON |= FMC_ISPCON_APUEN_Msk)
#define | FMC_ENABLE_LD_UPDATE() (FMC->ISPCON |= FMC_ISPCON_LDUEN_Msk)
#define | FMC_ENABLE_CFG_UPDATE() (FMC->ISPCON |= FMC_ISPCON_CFGUEN_Msk)
#define | FMC_ENABLE_ISP() (FMC->ISPCON |= FMC_ISPCON_ISPEN_Msk)
#define | FMC_GET_FAIL_FLAG() ((FMC->ISPCON & FMC_ISPCON_ISPFF_Msk) ? 1 : 0)
#define | FMC_CLR_FAIL_FLAG() (FMC->ISPCON |= FMC_ISPCON_ISPFF_Msk)

## Functions
void | FMC_Close (void)
| Disable all FMC functions. More...
int32_t | FMC_Erase (uint32_t u32PageAddr)
| Erase a page. The page size is 512 bytes. More...
int32_t | FMC_GetBootSource (void)
| get the current boot source More...
void | FMC_Open (void)
| Enable FMC ISP function. More...
uint32_t | FMC_Read (uint32_t u32Addr)
| Read a word from specified flash address. More...
uint32_t | FMC_ReadCID (void)
| Read company ID. More...
uint32_t | FMC_ReadPID (void)
| Read product ID. More...
uint32_t | FMC_ReadUCID (uint32_t u32Index)
| This function reads one of the four UCID. More...
uint32_t | FMC_ReadUID (uint32_t u32Index)
| This function reads one of the three UID. More...
uint32_t | FMC_ReadDataFlashBaseAddr (void)
| Get the base address of Data Flash if enabled. More...
uint32_t | FMC_SetVectorPageAddr (uint32_t u32PageAddr)
| This function will force re-map assigned flash page to CPU address 0x0. More...
uint32_t | FMC_GetVectorPageAddr (void)
| Obtain the current vector page address setting. More...
uint32_t | FMC_Write (uint32_t u32Addr, uint32_t u32Data)
| Writes a word data to specified flash address. More...
int32_t | FMC_ReadConfig (uint32_t *u32Config, uint32_t u32Count)
| Read the User Configuration words. More...
int32_t | FMC_WriteConfig (uint32_t *u32Config, uint32_t u32Count)
| Write User Configuration. More...

## Detailed Description

MINI51 series FMC driver header file.

Version
  V1.00

Revision
  11

Date
  15/09/16 11:12a

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file fmc.h.