| Mini51 BSP V3.02.002 The Board Support Package for Mini51 Series

Macros | Functions
adc.h File Reference

Mini51 series ADC driver header file. More...

Go to the source code of this file.

## Macros
#define | ADC_CH7_EXT (0UL)
#define | ADC_CH7_BGP (ADC_ADCHER_PRESEL_Msk)
#define | ADC_CMP_LESS_THAN (0UL)
#define | ADC_CMP_GREATER_OR_EQUAL_TO (ADC_ADCMPR_CMPCOND_Msk)
#define | ADC_TRIGGER_BY_EXT_PIN (0UL)
#define | ADC_TRIGGER_BY_PWM (ADC_ADCR_TRGS_Msk)
#define | ADC_FALLING_EDGE_TRIGGER (0UL)
#define | ADC_RISING_EDGE_TRIGGER (ADC_ADCR_TRGCOND_Msk)
#define | ADC_ADF_INT (ADC_ADSR_ADF_Msk)
#define | ADC_CMP0_INT (ADC_ADSR_CMPF0_Msk)
#define | ADC_CMP1_INT (ADC_ADSR_CMPF1_Msk)
#define | ADC_SAMPLE_CLOCK_0 (0UL)
#define | ADC_SAMPLE_CLOCK_1 (1UL)
#define | ADC_SAMPLE_CLOCK_2 (2UL)
#define | ADC_SAMPLE_CLOCK_4 (3UL)
#define | ADC_SAMPLE_CLOCK_8 (4UL)
#define | ADC_SAMPLE_CLOCK_16 (5UL)
#define | ADC_SAMPLE_CLOCK_32 (6UL)
#define | ADC_SAMPLE_CLOCK_64 (7UL)
#define | ADC_SAMPLE_CLOCK_128 (8UL)
#define | ADC_SAMPLE_CLOCK_256 (9UL)
#define | ADC_SAMPLE_CLOCK_512 (10UL)
#define | ADC_SAMPLE_CLOCK_1024 (11UL)
#define | ADC_CONFIG_CH7(adc, u32Source)
| Configure the analog input source of channel 7. More...
#define | ADC_GET_CONVERSION_DATA(adc, u32ChNum)
| Get the latest ADC conversion data. More...
#define | ADC_GET_INT_FLAG(adc, u32Mask)
| Return the user-specified interrupt flags. More...
#define | ADC_CLR_INT_FLAG(adc, u32Mask)
| This macro clear the selected interrupt status bits. More...
#define | ADC_IS_BUSY(adc)
| Get the busy state of ADC. More...
#define | ADC_IS_DATA_OVERRUN(adc, u32ChNum)
| Check if the ADC conversion data is over written or not. More...
#define | ADC_IS_DATA_VALID(adc, u32ChNum)
| Check if the ADC conversion data is valid or not. More...
#define | ADC_POWER_DOWN(adc)
| Power down ADC module. More...
#define | ADC_POWER_ON(adc)
| Power on ADC module. More...
#define | ADC_ENABLE_CMP0(adc, u32ChNum, u32Condition, u32Data, u32MatchCount)
| Configure the comparator 0 and enable it. More...
#define | ADC_DISABLE_CMP0(adc)
| Disable comparator 0. More...
#define | ADC_ENABLE_CMP1(adc, u32ChNum, u32Condition, u32Data, u32MatchCount)
| Configure the comparator 1 and enable it. More...
#define | ADC_DISABLE_CMP1(adc)
| Disable comparator 1. More...
#define | ADC_SET_INPUT_CHANNEL(adc, u32Mask)
| Set ADC input channel. Enabled channel will be converted while ADC starts. More...
#define | ADC_START_CONV(adc)
| Start the A/D conversion. More...
#define | ADC_STOP_CONV(adc)
| Stop the A/D conversion. More...

## Functions
void | ADC_Open (ADC_T *adc, uint32_t u32InputMode, uint32_t u32OpMode, uint32_t u32ChMask)
| This API configures ADC module to be ready for convert the input from selected channel. More...
void | ADC_Close (ADC_T *adc)
| Disable ADC module. More...
void | ADC_EnableHWTrigger (ADC_T *adc, uint32_t u32Source, uint32_t u32Param)
| Configure the hardware trigger condition and enable hardware trigger. More...
void | ADC_DisableHWTrigger (ADC_T *adc)
| Disable hardware trigger ADC function. More...
void | ADC_SetExtraSampleTime (ADC_T *adc, uint32_t u32ChNum, uint32_t u32SampleTime)
| Set ADC sample time for designated channel. More...
void | ADC_EnableInt (ADC_T *adc, uint32_t u32Mask)
| Enable the interrupt(s) selected by u32Mask parameter. More...
void | ADC_DisableInt (ADC_T *adc, uint32_t u32Mask)
| Disable the interrupt(s) selected by u32Mask parameter. More...

## Detailed Description

Mini51 series ADC driver header file.

Version
  V1.00

Revision
  9

Date
  14/01/14 5:29p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2013 Nuvoton Technology Corp. All rights reserved.

Definition in file adc.h.