| MINI51DE_BSP V3.02.004 The Board Support Package for Mini51DE Series MCU

Here is a list of all functions, variables, defines, enums, and typedefs with links to the files they belong to:

### - i -

- I2C : Mini51Series.h
- I2C0 : Mini51Series.h
- I2C_AA : i2c.h
- I2C_BASE : Mini51Series.h
- I2C_CLEAR_WAKEUP_FLAG : i2c.h
- I2C_ClearTimeoutFlag() : i2c.h
- I2C_Close() : i2c.h
- I2C_DISABLE_CLOCK_STRETCH : i2c.h
- I2C_DISABLE_FIFO : i2c.h
- I2C_DISABLE_OVERRUN_INT : i2c.h
- I2C_DISABLE_UNDERRUN_INT : i2c.h
- I2C_DisableInt() : i2c.h
- I2C_DisableTimeout() : i2c.h
- I2C_DisableWakeup() : i2c.h
- I2C_ENABLE_CLOCK_STRETCH : i2c.h
- I2C_ENABLE_FIFO : i2c.h
- I2C_ENABLE_OVERRUN_INT : i2c.h
- I2C_ENABLE_UNDERRUN_INT : i2c.h
- I2C_EnableInt() : i2c.h
- I2C_EnableTimeout() : i2c.h
- I2C_EnableWakeup() : i2c.h
- I2C_GET_DATA : i2c.h
- I2C_GET_STATUS : i2c.h
- I2C_GET_TIMEOUT_FLAG : i2c.h
- I2C_GET_WAKEUP_FLAG : i2c.h
- I2C_GetBusClockFreq() : i2c.h
- I2C_GetData() : i2c.h
- I2C_GetIntFlag() : i2c.h
- I2C_GetStatus() : i2c.h
- I2C_I2CADDR_GC_Msk : Mini51Series.h
- I2C_I2CADDR_GC_Pos : Mini51Series.h
- I2C_I2CADDR_I2CADDR_Msk : Mini51Series.h
- I2C_I2CADDR_I2CADDR_Pos : Mini51Series.h
- I2C_I2CADM_I2CADM_Msk : Mini51Series.h
- I2C_I2CADM_I2CADM_Pos : Mini51Series.h
- I2C_I2CDAT_I2CDAT_Msk : Mini51Series.h
- I2C_I2CDAT_I2CDAT_Pos : Mini51Series.h
- I2C_I2CLK_I2CLK_Msk : Mini51Series.h
- I2C_I2CLK_I2CLK_Pos : Mini51Series.h
- I2C_I2CON2_NOSTRETCH_Msk : Mini51Series.h
- I2C_I2CON2_NOSTRETCH_Pos : Mini51Series.h
- I2C_I2CON2_OVER_INTEN_Msk : Mini51Series.h
- I2C_I2CON2_OVER_INTEN_Pos : Mini51Series.h
- I2C_I2CON2_TWOFF_EN_Msk : Mini51Series.h
- I2C_I2CON2_TWOFF_EN_Pos : Mini51Series.h
- I2C_I2CON2_UNDER_INTEN_Msk : Mini51Series.h
- I2C_I2CON2_UNDER_INTEN_Pos : Mini51Series.h
- I2C_I2CON2_WKUPEN_Msk : Mini51Series.h
- I2C_I2CON2_WKUPEN_Pos : Mini51Series.h
- I2C_I2CON_AA_Msk : Mini51Series.h
- I2C_I2CON_AA_Pos : Mini51Series.h
- I2C_I2CON_EI_Msk : Mini51Series.h
- I2C_I2CON_EI_Pos : Mini51Series.h
- I2C_I2CON_ENSI_Msk : Mini51Series.h
- I2C_I2CON_ENSI_Pos : Mini51Series.h
- I2C_I2CON_SI_Msk : Mini51Series.h
- I2C_I2CON_SI_Pos : Mini51Series.h
- I2C_I2CON_STA_Msk : Mini51Series.h
- I2C_I2CON_STA_Pos : Mini51Series.h
- I2C_I2CON_STO_Msk : Mini51Series.h
- I2C_I2CON_STO_Pos : Mini51Series.h
- I2C_I2CSTATUS2_EMPTY_Msk : Mini51Series.h
- I2C_I2CSTATUS2_EMPTY_Pos : Mini51Series.h
- I2C_I2CSTATUS2_FULL_Msk : Mini51Series.h
- I2C_I2CSTATUS2_FULL_Pos : Mini51Series.h
- I2C_I2CSTATUS2_OVERUN_Msk : Mini51Series.h
- I2C_I2CSTATUS2_OVERUN_Pos : Mini51Series.h
- I2C_I2CSTATUS2_UNDERUN_Msk : Mini51Series.h
- I2C_I2CSTATUS2_UNDERUN_Pos : Mini51Series.h
- I2C_I2CSTATUS2_WAKEUP_Msk : Mini51Series.h
- I2C_I2CSTATUS2_WAKEUP_Pos : Mini51Series.h
- I2C_I2CSTATUS_I2CSTATUS_Msk : Mini51Series.h
- I2C_I2CSTATUS_I2CSTATUS_Pos : Mini51Series.h
- I2C_I2CTOC_DIV4_Msk : Mini51Series.h
- I2C_I2CTOC_DIV4_Pos : Mini51Series.h
- I2C_I2CTOC_ENTI_Msk : Mini51Series.h
- I2C_I2CTOC_ENTI_Pos : Mini51Series.h
- I2C_I2CTOC_TIF_Msk : Mini51Series.h
- I2C_I2CTOC_TIF_Pos : Mini51Series.h
- I2C_IRQn : Mini51Series.h
- I2C_MODULE : clk.h
- I2C_Open() : i2c.h
- I2C_RST : sys.h
- I2C_SET_CONTROL_REG : i2c.h
- I2C_SET_DATA : i2c.h
- I2C_SetBusClockFreq() : i2c.h
- I2C_SetData() : i2c.h
- I2C_SetSlaveAddr() : i2c.h
- I2C_SetSlaveAddrMask() : i2c.h
- I2C_SI : i2c.h
- I2C_STA : i2c.h
- I2C_START : i2c.h
- I2C_STO : i2c.h
- I2C_STOP() : i2c.h
- I2C_SW_CLK : i2c_software_gpio.c, i2c_software_gpio_with_timer.c
- I2C_SW_Get() : i2c_software_gpio.h, i2c_software_gpio.c
- I2C_SW_Get_byte() : i2c_software_gpio.c
- I2C_SW_I_Count() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Get() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Get_Byte() : i2c_software_gpio_with_timer.c
- I2C_SW_I_IsBZ() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Open() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Send() : i2c_software_gpio_with_timer.h, i2c_software_gpio_with_timer.c
- I2C_SW_I_Send_Byte() : i2c_software_gpio_with_timer.c
- I2C_SW_I_Send_Start() : i2c_software_gpio_with_timer.c
- I2C_SW_I_Send_Stop() : i2c_software_gpio_with_timer.c
- I2C_SW_Open() : i2c_software_gpio.h, i2c_software_gpio.c
- I2C_SW_SDA : i2c_software_gpio.c, i2c_software_gpio_with_timer.c
- I2C_SW_Send() : i2c_software_gpio.h, i2c_software_gpio.c
- I2C_SW_Send_byte() : i2c_software_gpio.c
- I2C_SW_STATUS : i2c_software_gpio_with_timer.c
- I2C_Trigger() : i2c.h
- I2C_WAIT_READY() : i2c.h
- inp16 : Mini51Series.h
- inp32 : Mini51Series.h
- inp8 : Mini51Series.h
- inpb : Mini51Series.h
- inps : Mini51Series.h
- inpw : Mini51Series.h
- INT : Mini51Series.h
- INT_BASE : Mini51Series.h
- INT_CON_NMI_SEL_EN_Msk : Mini51Series.h
- INT_CON_NMI_SEL_EN_Pos : Mini51Series.h
- INT_CON_NMI_SEL_Msk : Mini51Series.h
- INT_CON_NMI_SEL_Pos : Mini51Series.h
- INT_IRQ_MCU_IRQ_Msk : Mini51Series.h
- INT_IRQ_MCU_IRQ_Pos : Mini51Series.h
- INT_SRC_INT_SRC_Msk : Mini51Series.h
- INT_SRC_INT_SRC_Pos : Mini51Series.h
- IRQn : Mini51Series.h
- IRQn_Type : Mini51Series.h
- IsDebugFifoEmpty() : retarget.c