| MINI51DE_BSP V3.02.004 The Board Support Package for Mini51DE Series MCU

- __stdin : retarget.c
- __stdout : retarget.c
- arg : semihosting.h
- Ascii : ascii_table.c, lcd_driver.c
- CyclesPerUs : system_Mini51Series.h, system_Mini51Series.c
- errno : _syscalls.c
- funPtr : i2c_software_gpio_with_timer.c
- I2C_SW_STATUS : i2c_software_gpio_with_timer.c
- p8I2C_Data : i2c_software_gpio_with_timer.c
- SystemCoreClock : system_Mini51Series.h, system_Mini51Series.c
- u32_I2C_SW_Delay : i2c_software_gpio.c
- u32I2C_ByteSize : i2c_software_gpio_with_timer.c
- u32I2C_ByteSizeCount : i2c_software_gpio_with_timer.c
- u8I2C_Buffer : i2c_software_gpio_with_timer.c
- value : semihosting.h