| Mini51 BSP V3.02.002 The Board Support Package for Mini51 Series

Data Fields
I2C_SW_FLAG_T Struct Reference

`#include <i2c_software_gpio_with_timer.h>`

## Data Fields
uint32_t | COUNT:4
uint32_t | NACK:1
uint32_t | START:1
uint32_t | STOP:1
uint32_t | RW:1
uint32_t | BUSY:1
uint32_t | RESERVE:23

## Detailed Description

Definition at line 17 of file i2c_software_gpio_with_timer.h.

## Field Documentation

## ◆ BUSY

uint32_t I2C_SW_FLAG_T::BUSY

I2C Busy flag

Definition at line 24 of file i2c_software_gpio_with_timer.h.

## ◆ COUNT

uint32_t I2C_SW_FLAG_T::COUNT

Data Bit Count

Definition at line 19 of file i2c_software_gpio_with_timer.h.

## ◆ NACK

uint32_t I2C_SW_FLAG_T::NACK

I2C NACK

Definition at line 20 of file i2c_software_gpio_with_timer.h.

## ◆ RESERVE

uint32_t I2C_SW_FLAG_T::RESERVE

Reserve

Definition at line 25 of file i2c_software_gpio_with_timer.h.

## ◆ RW

uint32_t I2C_SW_FLAG_T::RW

I2C Read/Write Bit

Definition at line 23 of file i2c_software_gpio_with_timer.h.

## ◆ START

uint32_t I2C_SW_FLAG_T::START

I2C START

Definition at line 21 of file i2c_software_gpio_with_timer.h.

## ◆ STOP

uint32_t I2C_SW_FLAG_T::STOP

I2C STOP

Definition at line 22 of file i2c_software_gpio_with_timer.h.

The documentation for this struct was generated from the following file:

- Nu-LB-Mini51/inc/i2c_software_gpio_with_timer.h