| MINI51DE_BSP V3.02.004 The Board Support Package for Mini51DE Series MCU

Data Fields
UART_T Struct Reference

`#include <Mini51Series.h>`

## Data Fields
union {
__I uint32_t UART_T::RBR
__O uint32_t UART_T::THR
}; |
__IO uint32_t | IER
__IO uint32_t | FCR
__IO uint32_t | LCR
__IO uint32_t | MCR
__IO uint32_t | MSR
__IO uint32_t | FSR
__IO uint32_t | ISR
__IO uint32_t | TOR
__IO uint32_t | BAUD
__IO uint32_t | IRCR
__IO uint32_t | ALT_CSR
__IO uint32_t | FUN_SEL

## Detailed Description

    @addtogroup UART Universal Asynchronous Receiver/Transmitter Controller(UART)
    Memory Mapped Structure for UART Controller

Definition at line 4930 of file Mini51Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Mini51Series/Include/Mini51Series.h