| Mini51 BSP V3.02.002 The Board Support Package for Mini51 Series

Data Structures | Macros | Typedefs | Enumerations
Mini51Series.h File Reference

Mini51 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Mini51 series MCU. More...

`#include "core_cm0.h"`
`#include "system_Mini51Series.h"`
`#include <stdint.h>`
`#include "sys.h"`
`#include "clk.h"`
`#include "acmp.h"`
`#include "adc.h"`
`#include "fmc.h"`
`#include "gpio.h"`
`#include "i2c.h"`
`#include "pwm.h"`
`#include "spi.h"`
`#include "timer.h"`
`#include "uart.h"`
`#include "wdt.h"`

Go to the source code of this file.

## Data Structures
struct | ACMP_T
struct | ADC_T
struct | CLK_T
struct | FMC_T
struct | GCR_T
struct | GPIO_T
struct | GPIO_DBNCECON_T
| GPIO debounce register map. More...
struct | I2C_T
struct | INT_T
struct | PWM_T
struct | SPI_T
struct | TIMER_T
struct | UART_T
struct | WDT_T

## Macros
#define | __CM0_REV 0x0201
#define | __NVIC_PRIO_BITS 2
#define | __Vendor_SysTickConfig 0
#define | __MPU_PRESENT 0
#define | __FPU_PRESENT 0
#define | FLASH_BASE ((uint32_t)0x00000000)
| Flash base address. More...
#define | SRAM_BASE ((uint32_t)0x20000000)
| SRAM base address. More...
#define | APB1PERIPH_BASE ((uint32_t)0x40000000)
| APB1 base address. More...
#define | APB2PERIPH_BASE ((uint32_t)0x40100000)
| APB2 base address. More...
#define | AHBPERIPH_BASE ((uint32_t)0x50000000)
| AHB base address. More...
#define | WDT_BASE (APB1PERIPH_BASE + 0x04000)
| WDT register base address. More...
#define | TIMER0_BASE (APB1PERIPH_BASE + 0x10000)
| TIMER0 register base address. More...
#define | TIMER1_BASE (APB1PERIPH_BASE + 0x10020)
| TIMER1 register base address. More...
#define | I2C_BASE (APB1PERIPH_BASE + 0x20000)
| I2C register base address. More...
#define | SPI_BASE (APB1PERIPH_BASE + 0x30000)
| SPI register base address. More...
#define | PWM_BASE (APB1PERIPH_BASE + 0x40000)
| PWM register base address. More...
#define | UART_BASE (APB1PERIPH_BASE + 0x50000)
| UART register base address. More...
#define | ACMP_BASE (APB1PERIPH_BASE + 0xD0000)
| ACMP register base address. More...
#define | ADC_BASE (APB1PERIPH_BASE + 0xE0000)
| ADC register base address. More...
#define | GCR_BASE (AHBPERIPH_BASE + 0x00000)
| GCR register base address. More...
#define | CLK_BASE (AHBPERIPH_BASE + 0x00200)
| CLK register base address. More...
#define | INT_BASE (AHBPERIPH_BASE + 0x00300)
| INT register base address. More...
#define | P0_BASE (AHBPERIPH_BASE + 0x04000)
| GPIO Port 0 register base address. More...
#define | P1_BASE (AHBPERIPH_BASE + 0x04040)
| GPIO Port 1 register base address. More...
#define | P2_BASE (AHBPERIPH_BASE + 0x04080)
| GPIO Port 2 register base address. More...
#define | P3_BASE (AHBPERIPH_BASE + 0x040C0)
| GPIO Port 3 register base address. More...
#define | P4_BASE (AHBPERIPH_BASE + 0x04100)
| GPIO Port 4 register base address. More...
#define | P5_BASE (AHBPERIPH_BASE + 0x04140)
| GPIO Port 5 register base address. More...
#define | GPIO_DBNCECON_BASE (AHBPERIPH_BASE + 0x04180)
| GPIO De-bounce register vase. More...
#define | GPIO_PIN_DATA_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO pin data register base address. More...
#define | GPIOBIT0_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO Port 0 bit access register base address. More...
#define | GPIOBIT1_BASE (AHBPERIPH_BASE + 0x04220)
| GPIO Port 1 bit access register base address. More...
#define | GPIOBIT2_BASE (AHBPERIPH_BASE + 0x04240)
| GPIO Port 2 bit access register base address. More...
#define | GPIOBIT3_BASE (AHBPERIPH_BASE + 0x04260)
| GPIO Port 3 bit access register base address. More...
#define | GPIOBIT4_BASE (AHBPERIPH_BASE + 0x04280)
| GPIO Port 4 bit access register base address. More...
#define | GPIOBIT5_BASE (AHBPERIPH_BASE + 0x042A0)
| GPIO Port 5 bit access register base address. More...
#define | FMC_BASE (AHBPERIPH_BASE + 0x0C000)
| FMC register base address. More...
#define | WDT ((WDT_T *) WDT_BASE)
| Pointer to WDT register structure. More...
#define | TIMER0 ((TIMER_T *) TIMER0_BASE)
| Pointer to Timer 0 register structure. More...
#define | TIMER1 ((TIMER_T *) TIMER1_BASE)
| Pointer to Timer 1 register structure. More...
#define | I2C ((I2C_T *) I2C_BASE)
| Pointer to I2C register structure. More...
#define | I2C0 ((I2C_T *) I2C_BASE)
| Pointer to I2C register structure. More...
#define | SPI ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | SPI0 ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | PWM ((PWM_T *) PWM_BASE)
| Pointer to PWM register structure. More...
#define | UART ((UART_T *) UART_BASE)
| Pointer to UART register structure. More...
#define | UART0 ((UART_T *) UART_BASE)
| Pointer to UART register structure. More...
#define | ADC ((ADC_T *) ADC_BASE)
| Pointer to ADC register structure. More...
#define | ACMP ((ACMP_T *) ACMP_BASE)
| Pointer to ACMP register structure. More...
#define | SYS ((GCR_T *) GCR_BASE)
| Pointer to SYS register structure. More...
#define | CLK ((CLK_T *) CLK_BASE)
| Pointer to CLK register structure. More...
#define | INT ((INT_T *) INT_BASE)
| Pointer to INT register structure. More...
#define | P0 ((GPIO_T *) P0_BASE)
| Pointer to GPIO port 0 register structure. More...
#define | P1 ((GPIO_T *) P1_BASE)
| Pointer to GPIO port 1 register structure. More...
#define | P2 ((GPIO_T *) P2_BASE)
| Pointer to GPIO port 2 register structure. More...
#define | P3 ((GPIO_T *) P3_BASE)
| Pointer to GPIO port 3 register structure. More...
#define | P4 ((GPIO_T *) P4_BASE)
| Pointer to GPIO port 4 register structure. More...
#define | P5 ((GPIO_T *) P5_BASE)
| Pointer to GPIO port 5 register structure. More...
#define | GPIO ((GPIO_DBNCECON_T *) GPIO_DBNCECON_BASE)
| Pointer to GPIO de-bounce register structure. More...
#define | FMC ((FMC_T *) FMC_BASE)
| Pointer to FMC register structure. More...
#define | M8(addr) (*((vu8 *) (addr)))
| Get a 8-bit unsigned value from specified address. More...
#define | M16(addr) (*((vu16 *) (addr)))
| Get a 16-bit unsigned value from specified address. More...
#define | M32(addr) (*((vu32 *) (addr)))
| Get a 32-bit unsigned value from specified address. More...
#define | outpw(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inpw(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outps(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inps(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outpb(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inpb(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | outp32(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inp32(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outp16(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inp16(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outp8(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inp8(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | NULL (0)
| NULL pointer. More...
#define | TRUE (1)
| Boolean true, define to use in API parameters or return value. More...
#define | FALSE (0)
| Boolean false, define to use in API parameters or return value. More...
#define | ENABLE (1)
| Enable, define to use in API parameters. More...
#define | DISABLE (0)
| Disable, define to use in API parameters. More...
#define | BIT0 (0x00000001)
| Bit 0 mask of an 32 bit integer. More...
#define | BIT1 (0x00000002)
| Bit 1 mask of an 32 bit integer. More...
#define | BIT2 (0x00000004)
| Bit 2 mask of an 32 bit integer. More...
#define | BIT3 (0x00000008)
| Bit 3 mask of an 32 bit integer. More...
#define | BIT4 (0x00000010)
| Bit 4 mask of an 32 bit integer. More...
#define | BIT5 (0x00000020)
| Bit 5 mask of an 32 bit integer. More...
#define | BIT6 (0x00000040)
| Bit 6 mask of an 32 bit integer. More...
#define | BIT7 (0x00000080)
| Bit 7 mask of an 32 bit integer. More...
#define | BIT8 (0x00000100)
| Bit 8 mask of an 32 bit integer. More...
#define | BIT9 (0x00000200)
| Bit 9 mask of an 32 bit integer. More...
#define | BIT10 (0x00000400)
| Bit 10 mask of an 32 bit integer. More...
#define | BIT11 (0x00000800)
| Bit 11 mask of an 32 bit integer. More...
#define | BIT12 (0x00001000)
| Bit 12 mask of an 32 bit integer. More...
#define | BIT13 (0x00002000)
| Bit 13 mask of an 32 bit integer. More...
#define | BIT14 (0x00004000)
| Bit 14 mask of an 32 bit integer. More...
#define | BIT15 (0x00008000)
| Bit 15 mask of an 32 bit integer. More...
#define | BIT16 (0x00010000)
| Bit 16 mask of an 32 bit integer. More...
#define | BIT17 (0x00020000)
| Bit 17 mask of an 32 bit integer. More...
#define | BIT18 (0x00040000)
| Bit 18 mask of an 32 bit integer. More...
#define | BIT19 (0x00080000)
| Bit 19 mask of an 32 bit integer. More...
#define | BIT20 (0x00100000)
| Bit 20 mask of an 32 bit integer. More...
#define | BIT21 (0x00200000)
| Bit 21 mask of an 32 bit integer. More...
#define | BIT22 (0x00400000)
| Bit 22 mask of an 32 bit integer. More...
#define | BIT23 (0x00800000)
| Bit 23 mask of an 32 bit integer. More...
#define | BIT24 (0x01000000)
| Bit 24 mask of an 32 bit integer. More...
#define | BIT25 (0x02000000)
| Bit 25 mask of an 32 bit integer. More...
#define | BIT26 (0x04000000)
| Bit 26 mask of an 32 bit integer. More...
#define | BIT27 (0x08000000)
| Bit 27 mask of an 32 bit integer. More...
#define | BIT28 (0x10000000)
| Bit 28 mask of an 32 bit integer. More...
#define | BIT29 (0x20000000)
| Bit 29 mask of an 32 bit integer. More...
#define | BIT30 (0x40000000)
| Bit 30 mask of an 32 bit integer. More...
#define | BIT31 (0x80000000)
| Bit 31 mask of an 32 bit integer. More...
#define | BYTE0_Msk (0x000000FF)
| Mask to get bit0~bit7 from a 32 bit integer. More...
#define | BYTE1_Msk (0x0000FF00)
| Mask to get bit8~bit15 from a 32 bit integer. More...
#define | BYTE2_Msk (0x00FF0000)
| Mask to get bit16~bit23 from a 32 bit integer. More...
#define | BYTE3_Msk (0xFF000000)
| Mask to get bit24~bit31 from a 32 bit integer. More...
#define | GET_BYTE0(u32Param) ((u32Param & BYTE0_Msk) )
#define | GET_BYTE1(u32Param) ((u32Param & BYTE1_Msk) >> 8)
#define | GET_BYTE2(u32Param) ((u32Param & BYTE2_Msk) >> 16)
#define | GET_BYTE3(u32Param) ((u32Param & BYTE3_Msk) >> 24)
#define | ACMP_CMPCR_ACMPEN_Pos (0)
#define | ACMP_CMPCR_ACMPEN_Msk (0x1ul << ACMP_CMPCR_ACMPEN_Pos)
#define | ACMP_CMPCR_ACMPIE_Pos (1)
#define | ACMP_CMPCR_ACMPIE_Msk (0x1ul << ACMP_CMPCR_ACMPIE_Pos)
#define | ACMP_CMPCR_HYSEN_Pos (2)
#define | ACMP_CMPCR_HYSEN_Msk (0x1ul << ACMP_CMPCR_HYSEN_Pos)
#define | ACMP_CMPCR_NEGSEL_Pos (4)
#define | ACMP_CMPCR_NEGSEL_Msk (0x1ul << ACMP_CMPCR_NEGSEL_Pos)
#define | ACMP_CMPCR_RISING_Pos (8)
#define | ACMP_CMPCR_RISING_Msk (0x1ul << ACMP_CMPCR_RISING_Pos)
#define | ACMP_CMPCR_FALLING_Pos (9)
#define | ACMP_CMPCR_FALLING_Msk (0x1ul << ACMP_CMPCR_FALLING_Pos)
#define | ACMP_CMPCR_CPPSEL_Pos (29)
#define | ACMP_CMPCR_CPPSEL_Msk (0x3ul << ACMP_CMPCR_CPPSEL_Pos)
#define | ACMP_CMPSR_ACMPF0_Pos (0)
#define | ACMP_CMPSR_ACMPF0_Msk (0x1ul << ACMP_CMPSR_ACMPF0_Pos)
#define | ACMP_CMPSR_ACMPF1_Pos (1)
#define | ACMP_CMPSR_ACMPF1_Msk (0x1ul << ACMP_CMPSR_ACMPF1_Pos)
#define | ACMP_CMPSR_ACMPCO0_Pos (2)
#define | ACMP_CMPSR_ACMPCO0_Msk (0x1ul << ACMP_CMPSR_ACMPCO0_Pos)
#define | ACMP_CMPSR_ACMPCO1_Pos (3)
#define | ACMP_CMPSR_ACMPCO1_Msk (0x1ul << ACMP_CMPSR_ACMPCO1_Pos)
#define | ACMP_CMPRVCR_CRVS_Pos (0)
#define | ACMP_CMPRVCR_CRVS_Msk (0xful << ACMP_CMPRVCR_CRVS_Pos)
#define | ACMP_CMPRVCR_OUT_SEL_Pos (7)
#define | ACMP_CMPRVCR_OUT_SEL_Msk (0x1ul << ACMP_CMPRVCR_OUT_SEL_Pos)
#define | ADC_ADDR_RSLT_Pos (0)
#define | ADC_ADDR_RSLT_Msk (0x3fful << ADC_ADDR_RSLT_Pos)
#define | ADC_ADDR_OVERRUN_Pos (16)
#define | ADC_ADDR_OVERRUN_Msk (0x1ul << ADC_ADDR_OVERRUN_Pos)
#define | ADC_ADDR_VALID_Pos (17)
#define | ADC_ADDR_VALID_Msk (0x1ul << ADC_ADDR_VALID_Pos)
#define | ADC_ADCR_ADEN_Pos (0)
#define | ADC_ADCR_ADEN_Msk (0x1ul << ADC_ADCR_ADEN_Pos)
#define | ADC_ADCR_ADIE_Pos (1)
#define | ADC_ADCR_ADIE_Msk (0x1ul << ADC_ADCR_ADIE_Pos)
#define | ADC_ADCR_TRGS_Pos (4)
#define | ADC_ADCR_TRGS_Msk (0x3ul << ADC_ADCR_TRGS_Pos)
#define | ADC_ADCR_TRGCOND_Pos (6)
#define | ADC_ADCR_TRGCOND_Msk (0x1ul << ADC_ADCR_TRGCOND_Pos)
#define | ADC_ADCR_TRGEN_Pos (8)
#define | ADC_ADCR_TRGEN_Msk (0x1ul << ADC_ADCR_TRGEN_Pos)
#define | ADC_ADCR_ADST_Pos (11)
#define | ADC_ADCR_ADST_Msk (0x1ul << ADC_ADCR_ADST_Pos)
#define | ADC_ADCHER_CHEN_Pos (0)
#define | ADC_ADCHER_CHEN_Msk (0xfful << ADC_ADCHER_CHEN_Pos)
#define | ADC_ADCHER_CHEN0_Pos (0)
#define | ADC_ADCHER_CHEN0_Msk (0x1ul << ADC_ADCHER_CHEN0_Pos)
#define | ADC_ADCHER_CHEN1_Pos (1)
#define | ADC_ADCHER_CHEN1_Msk (0x1ul << ADC_ADCHER_CHEN1_Pos)
#define | ADC_ADCHER_CHEN2_Pos (2)
#define | ADC_ADCHER_CHEN2_Msk (0x1ul << ADC_ADCHER_CHEN2_Pos)
#define | ADC_ADCHER_CHEN3_Pos (3)
#define | ADC_ADCHER_CHEN3_Msk (0x1ul << ADC_ADCHER_CHEN3_Pos)
#define | ADC_ADCHER_CHEN4_Pos (4)
#define | ADC_ADCHER_CHEN4_Msk (0x1ul << ADC_ADCHER_CHEN4_Pos)
#define | ADC_ADCHER_CHEN5_Pos (5)
#define | ADC_ADCHER_CHEN5_Msk (0x1ul << ADC_ADCHER_CHEN5_Pos)
#define | ADC_ADCHER_CHEN6_Pos (6)
#define | ADC_ADCHER_CHEN6_Msk (0x1ul << ADC_ADCHER_CHEN6_Pos)
#define | ADC_ADCHER_CHEN7_Pos (7)
#define | ADC_ADCHER_CHEN7_Msk (0x1ul << ADC_ADCHER_CHEN7_Pos)
#define | ADC_ADCHER_PRESEL_Pos (8)
#define | ADC_ADCHER_PRESEL_Msk (0x1ul << ADC_ADCHER_PRESEL_Pos)
#define | ADC_ADCMPR_CMPEN_Pos (0)
#define | ADC_ADCMPR_CMPEN_Msk (0x1ul << ADC_ADCMPR_CMPEN_Pos)
#define | ADC_ADCMPR_CMPIE_Pos (1)
#define | ADC_ADCMPR_CMPIE_Msk (0x1ul << ADC_ADCMPR_CMPIE_Pos)
#define | ADC_ADCMPR_CMPCOND_Pos (2)
#define | ADC_ADCMPR_CMPCOND_Msk (0x1ul << ADC_ADCMPR_CMPCOND_Pos)
#define | ADC_ADCMPR_CMPCH_Pos (3)
#define | ADC_ADCMPR_CMPCH_Msk (0x7ul << ADC_ADCMPR_CMPCH_Pos)
#define | ADC_ADCMPR_CMPMATCNT_Pos (8)
#define | ADC_ADCMPR_CMPMATCNT_Msk (0xful << ADC_ADCMPR_CMPMATCNT_Pos)
#define | ADC_ADCMPR_CMPD_Pos (16)
#define | ADC_ADCMPR_CMPD_Msk (0x3fful << ADC_ADCMPR_CMPD_Pos)
#define | ADC_ADSR_ADF_Pos (0)
#define | ADC_ADSR_ADF_Msk (0x1ul << ADC_ADSR_ADF_Pos)
#define | ADC_ADSR_CMPF0_Pos (1)
#define | ADC_ADSR_CMPF0_Msk (0x1ul << ADC_ADSR_CMPF0_Pos)
#define | ADC_ADSR_CMPF1_Pos (2)
#define | ADC_ADSR_CMPF1_Msk (0x1ul << ADC_ADSR_CMPF1_Pos)
#define | ADC_ADSR_BUSY_Pos (3)
#define | ADC_ADSR_BUSY_Msk (0x1ul << ADC_ADSR_BUSY_Pos)
#define | ADC_ADSR_CHANNEL_Pos (4)
#define | ADC_ADSR_CHANNEL_Msk (0x7ul << ADC_ADSR_CHANNEL_Pos)
#define | ADC_ADSR_VALID_Pos (8)
#define | ADC_ADSR_VALID_Msk (0x1ul << ADC_ADSR_VALID_Pos)
#define | ADC_ADSR_OVERRUN_Pos (16)
#define | ADC_ADSR_OVERRUN_Msk (0x1ul << ADC_ADSR_OVERRUN_Pos)
#define | ADC_ADTDCR_PTDT_Pos (0)
#define | ADC_ADTDCR_PTDT_Msk (0xfful << ADC_ADTDCR_PTDT_Pos)
#define | ADC_ADSAMP_SAMPCNT_Pos (0)
#define | ADC_ADSAMP_SAMPCNT_Msk (0xful << ADC_ADSAMP_SAMPCNT_Pos)
#define | CLK_PWRCON_XTLCLK_EN_Pos (0)
#define | CLK_PWRCON_XTLCLK_EN_Msk (0x3ul << CLK_PWRCON_XTLCLK_EN_Pos)
#define | CLK_PWRCON_OSC22M_EN_Pos (2)
#define | CLK_PWRCON_OSC22M_EN_Msk (0x1ul << CLK_PWRCON_OSC22M_EN_Pos)
#define | CLK_PWRCON_IRC22M_EN_Pos (2)
#define | CLK_PWRCON_IRC22M_EN_Msk (0x1ul << CLK_PWRCON_IRC22M_EN_Pos)
#define | CLK_PWRCON_HIRC_EN_Pos (2)
#define | CLK_PWRCON_HIRC_EN_Msk (0x1ul << CLK_PWRCON_HIRC_EN_Pos)
#define | CLK_PWRCON_OSC10K_EN_Pos (3)
#define | CLK_PWRCON_OSC10K_EN_Msk (0x1ul << CLK_PWRCON_OSC10K_EN_Pos)
#define | CLK_PWRCON_IRC10K_EN_Pos (3)
#define | CLK_PWRCON_IRC10K_EN_Msk (0x1ul << CLK_PWRCON_IRC10K_EN_Pos)
#define | CLK_PWRCON_LIRC_EN_Pos (3)
#define | CLK_PWRCON_LIRC_EN_Msk (0x1ul << CLK_PWRCON_LIRC_EN_Pos)
#define | CLK_PWRCON_WU_DLY_Pos (4)
#define | CLK_PWRCON_WU_DLY_Msk (0x1ul << CLK_PWRCON_WU_DLY_Pos)
#define | CLK_PWRCON_WINT_EN_Pos (5)
#define | CLK_PWRCON_WINT_EN_Msk (0x1ul << CLK_PWRCON_WINT_EN_Pos)
#define | CLK_PWRCON_PD_WU_STS_Pos (6)
#define | CLK_PWRCON_PD_WU_STS_Msk (0x1ul << CLK_PWRCON_PD_WU_STS_Pos)
#define | CLK_PWRCON_PWR_DOWN_EN_Pos (7)
#define | CLK_PWRCON_PWR_DOWN_EN_Msk (0x1ul << CLK_PWRCON_PWR_DOWN_EN_Pos)
#define | CLK_PWRCON_PD_32K_Pos (9)
#define | CLK_PWRCON_PD_32K_Msk (0x1ul << CLK_PWRCON_PD_32K_Pos)
#define | CLK_AHBCLK_ISP_EN_Pos (2)
#define | CLK_AHBCLK_ISP_EN_Msk (0x1ul << CLK_AHBCLK_ISP_EN_Pos)
#define | CLK_APBCLK_WDT_EN_Pos (0)
#define | CLK_APBCLK_WDT_EN_Msk (0x1ul << CLK_APBCLK_WDT_EN_Pos)
#define | CLK_APBCLK_TMR0_EN_Pos (2)
#define | CLK_APBCLK_TMR0_EN_Msk (0x1ul << CLK_APBCLK_TMR0_EN_Pos)
#define | CLK_APBCLK_TMR1_EN_Pos (3)
#define | CLK_APBCLK_TMR1_EN_Msk (0x1ul << CLK_APBCLK_TMR1_EN_Pos)
#define | CLK_APBCLK_FDIV_EN_Pos (6)
#define | CLK_APBCLK_FDIV_EN_Msk (0x1ul << CLK_APBCLK_FDIV_EN_Pos)
#define | CLK_APBCLK_I2C_EN_Pos (8)
#define | CLK_APBCLK_I2C_EN_Msk (0x1ul << CLK_APBCLK_I2C_EN_Pos)
#define | CLK_APBCLK_SPI_EN_Pos (12)
#define | CLK_APBCLK_SPI_EN_Msk (0x1ul << CLK_APBCLK_SPI_EN_Pos)
#define | CLK_APBCLK_UART_EN_Pos (16)
#define | CLK_APBCLK_UART_EN_Msk (0x1ul << CLK_APBCLK_UART_EN_Pos)
#define | CLK_APBCLK_PWM01_EN_Pos (20)
#define | CLK_APBCLK_PWM01_EN_Msk (0x1ul << CLK_APBCLK_PWM01_EN_Pos)
#define | CLK_APBCLK_PWM23_EN_Pos (21)
#define | CLK_APBCLK_PWM23_EN_Msk (0x1ul << CLK_APBCLK_PWM23_EN_Pos)
#define | CLK_APBCLK_PWM45_EN_Pos (22)
#define | CLK_APBCLK_PWM45_EN_Msk (0x1ul << CLK_APBCLK_PWM45_EN_Pos)
#define | CLK_APBCLK_ADC_EN_Pos (28)
#define | CLK_APBCLK_ADC_EN_Msk (0x1ul << CLK_APBCLK_ADC_EN_Pos)
#define | CLK_APBCLK_CMP_EN_Pos (30)
#define | CLK_APBCLK_CMP_EN_Msk (0x1ul << CLK_APBCLK_CMP_EN_Pos)
#define | CLK_CLKSTATUS_XTL_STB_Pos (0)
#define | CLK_CLKSTATUS_XTL_STB_Msk (0x1ul << CLK_CLKSTATUS_XTL_STB_Pos)
#define | CLK_CLKSTATUS_HXT_STB_Pos (0)
#define | CLK_CLKSTATUS_HXT_STB_Msk (0x1ul << CLK_CLKSTATUS_HXT_STB_Pos)
#define | CLK_CLKSTATUS_LXT_STB_Pos (0)
#define | CLK_CLKSTATUS_LXT_STB_Msk (0x1ul << CLK_CLKSTATUS_LXT_STB_Pos)
#define | CLK_CLKSTATUS_OSC10K_STB_Pos (3)
#define | CLK_CLKSTATUS_OSC10K_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC10K_STB_Pos)
#define | CLK_CLKSTATUS_IRC10K_STB_Pos (3)
#define | CLK_CLKSTATUS_IRC10K_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC10K_STB_Pos)
#define | CLK_CLKSTATUS_LIRC_STB_Pos (3)
#define | CLK_CLKSTATUS_LIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_LIRC_STB_Pos)
#define | CLK_CLKSTATUS_OSC22M_STB_Pos (4)
#define | CLK_CLKSTATUS_OSC22M_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC22M_STB_Pos)
#define | CLK_CLKSTATUS_IRC22M_STB_Pos (4)
#define | CLK_CLKSTATUS_IRC22M_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC22M_STB_Pos)
#define | CLK_CLKSTATUS_HIRC_STB_Pos (4)
#define | CLK_CLKSTATUS_HIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_HIRC_STB_Pos)
#define | CLK_CLKSTATUS_CLK_SW_FAIL_Pos (7)
#define | CLK_CLKSTATUS_CLK_SW_FAIL_Msk (0x1ul << CLK_CLKSTATUS_CLK_SW_FAIL_Pos)
#define | CLK_CLKSEL0_HCLK_S_Pos (0)
#define | CLK_CLKSEL0_HCLK_S_Msk (0x7ul << CLK_CLKSEL0_HCLK_S_Pos)
#define | CLK_CLKSEL0_STCLK_S_Pos (3)
#define | CLK_CLKSEL0_STCLK_S_Msk (0x7ul << CLK_CLKSEL0_STCLK_S_Pos)
#define | CLK_CLKSEL1_WDT_S_Pos (0)
#define | CLK_CLKSEL1_WDT_S_Msk (0x3ul << CLK_CLKSEL1_WDT_S_Pos)
#define | CLK_CLKSEL1_ADC_S_Pos (2)
#define | CLK_CLKSEL1_ADC_S_Msk (0x3ul << CLK_CLKSEL1_ADC_S_Pos)
#define | CLK_CLKSEL1_SPI_S_Pos (4)
#define | CLK_CLKSEL1_SPI_S_Msk (0x1ul << CLK_CLKSEL1_SPI_S_Pos)
#define | CLK_CLKSEL1_TMR0_S_Pos (8)
#define | CLK_CLKSEL1_TMR0_S_Msk (0x7ul << CLK_CLKSEL1_TMR0_S_Pos)
#define | CLK_CLKSEL1_TMR1_S_Pos (12)
#define | CLK_CLKSEL1_TMR1_S_Msk (0x7ul << CLK_CLKSEL1_TMR1_S_Pos)
#define | CLK_CLKSEL1_UART_S_Pos (24)
#define | CLK_CLKSEL1_UART_S_Msk (0x3ul << CLK_CLKSEL1_UART_S_Pos)
#define | CLK_CLKDIV_HCLK_N_Pos (0)
#define | CLK_CLKDIV_HCLK_N_Msk (0xful << CLK_CLKDIV_HCLK_N_Pos)
#define | CLK_CLKDIV_UART_N_Pos (8)
#define | CLK_CLKDIV_UART_N_Msk (0xful << CLK_CLKDIV_UART_N_Pos)
#define | CLK_CLKDIV_ADC_N_Pos (16)
#define | CLK_CLKDIV_ADC_N_Msk (0xfful << CLK_CLKDIV_ADC_N_Pos)
#define | CLK_CLKSEL2_FRQDIV_S_Pos (2)
#define | CLK_CLKSEL2_FRQDIV_S_Msk (0x3ul << CLK_CLKSEL2_FRQDIV_S_Pos)
#define | CLK_FRQDIV_FSEL_Pos (0)
#define | CLK_FRQDIV_FSEL_Msk (0xful << CLK_FRQDIV_FSEL_Pos)
#define | CLK_FRQDIV_DIVIDER_EN_Pos (4)
#define | CLK_FRQDIV_DIVIDER_EN_Msk (0x1ul << CLK_FRQDIV_DIVIDER_EN_Pos)
#define | CLK_FRQDIV_DIVIDER1_Pos (5)
#define | CLK_FRQDIV_DIVIDER1_Msk (0x1ul << CLK_FRQDIV_DIVIDER1_Pos)
#define | FMC_ISPCON_ISPEN_Pos (0)
#define | FMC_ISPCON_ISPEN_Msk (0x1ul << FMC_ISPCON_ISPEN_Pos)
#define | FMC_ISPCON_BS_Pos (1)
#define | FMC_ISPCON_BS_Msk (0x1ul << FMC_ISPCON_BS_Pos)
#define | FMC_ISPCON_APUEN_Pos (3)
#define | FMC_ISPCON_APUEN_Msk (0x1ul << FMC_ISPCON_APUEN_Pos)
#define | FMC_ISPCON_CFGUEN_Pos (4)
#define | FMC_ISPCON_CFGUEN_Msk (0x1ul << FMC_ISPCON_CFGUEN_Pos)
#define | FMC_ISPCON_LDUEN_Pos (5)
#define | FMC_ISPCON_LDUEN_Msk (0x1ul << FMC_ISPCON_LDUEN_Pos)
#define | FMC_ISPCON_ISPFF_Pos (6)
#define | FMC_ISPCON_ISPFF_Msk (0x1ul << FMC_ISPCON_ISPFF_Pos)
#define | FMC_ISPADR_ISPADR_Pos (0)
#define | FMC_ISPADR_ISPADR_Msk (0xfffffffful << FMC_ISPADR_ISPADR_Pos)
#define | FMC_ISPDAT_ISPDAT_Pos (0)
#define | FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)
#define | FMC_ISPCMD_ISPCMD_Pos (0)
#define | FMC_ISPCMD_ISPCMD_Msk (0x3ful << FMC_ISPCMD_ISPCMD_Pos)
#define | FMC_ISPTRG_ISPGO_Pos (0)
#define | FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)
#define | FMC_DFBADR_DFBA_Pos (0)
#define | FMC_DFBADR_DFBA_Msk (0xfffffffful << FMC_DFBA_DFBA_Pos)
#define | FMC_ISPSTA_ISPGO_Pos (0)
#define | FMC_ISPSTA_ISPGO_Msk (0x1ul << FMC_ISPSTA_ISPGO_Pos)
#define | FMC_ISPSTA_CBS_Pos (1)
#define | FMC_ISPSTA_CBS_Msk (0x3ul << FMC_ISPSTA_CBS_Pos)
#define | FMC_ISPSTA_ISPFF_Pos (6)
#define | FMC_ISPSTA_ISPFF_Msk (0x1ul << FMC_ISPSTA_ISPFF_Pos)
#define | FMC_ISPSTA_VECMAP_Pos (9)
#define | FMC_ISPSTA_VECMAP_Msk (0xffful << FMC_ISPSTA_VECMAP_Pos)
#define | SYS_PDID_PDID_Pos (0)
#define | SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)
#define | SYS_RSTSRC_RSTS_POR_Pos (0)
#define | SYS_RSTSRC_RSTS_POR_Msk (0x1ul << SYS_RSTSRC_RSTS_POR_Pos)
#define | SYS_RSTSRC_RSTS_RESET_Pos (1)
#define | SYS_RSTSRC_RSTS_RESET_Msk (0x1ul << SYS_RSTSRC_RSTS_RESET_Pos)
#define | SYS_RSTSRC_RSTS_WDT_Pos (2)
#define | SYS_RSTSRC_RSTS_WDT_Msk (0x1ul << SYS_RSTSRC_RSTS_WDT_Pos)
#define | SYS_RSTSRC_RSTS_BOD_Pos (4)
#define | SYS_RSTSRC_RSTS_BOD_Msk (0x1ul << SYS_RSTSRC_RSTS_BOD_Pos)
#define | SYS_RSTSRC_RSTS_MCU_Pos (5)
#define | SYS_RSTSRC_RSTS_MCU_Msk (0x1ul << SYS_RSTSRC_RSTS_MCU_Pos)
#define | SYS_RSTSRC_RSTS_CPU_Pos (7)
#define | SYS_RSTSRC_RSTS_CPU_Msk (0x1ul << SYS_RSTSRC_RSTS_CPU_Pos)
#define | SYS_IPRSTC1_CHIP_RST_Pos (0)
#define | SYS_IPRSTC1_CHIP_RST_Msk (0x1ul << SYS_IPRSTC1_CHIP_RST_Pos)
#define | SYS_IPRSTC1_CPU_RST_Pos (1)
#define | SYS_IPRSTC1_CPU_RST_Msk (0x1ul << SYS_IPRSTC1_CPU_RST_Pos)
#define | SYS_IPRSTC2_GPIO_RST_Pos (1)
#define | SYS_IPRSTC2_GPIO_RST_Msk (0x1ul << SYS_IPRSTC2_GPIO_RST_Pos)
#define | SYS_IPRSTC2_TMR0_RST_Pos (2)
#define | SYS_IPRSTC2_TMR0_RST_Msk (0x1ul << SYS_IPRSTC2_TMR0_RST_Pos)
#define | SYS_IPRSTC2_TMR1_RST_Pos (3)
#define | SYS_IPRSTC2_TMR1_RST_Msk (0x1ul << SYS_IPRSTC2_TMR1_RST_Pos)
#define | SYS_IPRSTC2_I2C_RST_Pos (8)
#define | SYS_IPRSTC2_I2C_RST_Msk (0x1ul << SYS_IPRSTC2_I2C_RST_Pos)
#define | SYS_IPRSTC2_SPI_RST_Pos (12)
#define | SYS_IPRSTC2_SPI_RST_Msk (0x1ul << SYS_IPRSTC2_SPI_RST_Pos)
#define | SYS_IPRSTC2_UART_RST_Pos (16)
#define | SYS_IPRSTC2_UART_RST_Msk (0x1ul << SYS_IPRSTC2_UART_RST_Pos)
#define | SYS_IPRSTC2_PWM_RST_Pos (20)
#define | SYS_IPRSTC2_PWM_RST_Msk (0x1ul << SYS_IPRSTC2_PWM_RST_Pos)
#define | SYS_IPRSTC2_ACMP_RST_Pos (22)
#define | SYS_IPRSTC2_ACMP_RST_Msk (0x1ul << SYS_IPRSTC2_ACMP_RST_Pos)
#define | SYS_IPRSTC2_ADC_RST_Pos (28)
#define | SYS_IPRSTC2_ADC_RST_Msk (0x1ul << SYS_IPRSTC2_ADC_RST_Pos)
#define | SYS_BODCR_BOD_VL_EXT_Pos (0)
#define | SYS_BODCR_BOD_VL_EXT_Msk (0x1ul << SYS_BODCR_BOD_VL_EXT_Pos)
#define | SYS_BODCR_BOD_VL_Pos (1)
#define | SYS_BODCR_BOD_VL_Msk (0x3ul << SYS_BODCR_BOD_VL_Pos)
#define | SYS_BODCR_BOD_RSTEN_Pos (3)
#define | SYS_BODCR_BOD_RSTEN_Msk (0x1ul << SYS_BODCR_BOD_RSTEN_Pos)
#define | SYS_BODCR_BOD_INTF_Pos (4)
#define | SYS_BODCR_BOD_INTF_Msk (0x1ul << SYS_BODCR_BOD_INTF_Pos)
#define | SYS_BODCR_BOD_LPM_Pos (5)
#define | SYS_BODCR_BOD_LPM_Msk (0x1ul << SYS_BODCR_BOD_LPM_Pos)
#define | SYS_BODCR_BOD_OUT_Pos (6)
#define | SYS_BODCR_BOD_OUT_Msk (0x1ul << SYS_BODCR_BOD_OUT_Pos)
#define | SYS_P0_MFP_P0_MFP_Pos (0)
#define | SYS_P0_MFP_P0_MFP_Msk (0xfful << SYS_P0_MFP_P0_MFP_Pos)
#define | SYS_P0_MFP_P0_ALT_Pos (8)
#define | SYS_P0_MFP_P0_ALT_Msk (0xfful << SYS_P0_MFP_P0_ALT_Pos)
#define | SYS_P0_MFP_P0_ALT0_Pos (8)
#define | SYS_P0_MFP_P0_ALT0_Msk (0x1ul << SYS_P0_MFP_P0_ALT0_Pos)
#define | SYS_P0_MFP_P0_ALT1_Pos (9)
#define | SYS_P0_MFP_P0_ALT1_Msk (0x1ul << SYS_P0_MFP_P0_ALT1_Pos)
#define | SYS_P0_MFP_P0_ALT4_Pos (12)
#define | SYS_P0_MFP_P0_ALT4_Msk (0x1ul << SYS_P0_MFP_P0_ALT4_Pos)
#define | SYS_P0_MFP_P0_ALT5_Pos (13)
#define | SYS_P0_MFP_P0_ALT5_Msk (0x1ul << SYS_P0_MFP_P0_ALT5_Pos)
#define | SYS_P0_MFP_P0_ALT6_Pos (14)
#define | SYS_P0_MFP_P0_ALT6_Msk (0x1ul << SYS_P0_MFP_P0_ALT6_Pos)
#define | SYS_P0_MFP_P0_ALT7_Pos (15)
#define | SYS_P0_MFP_P0_ALT7_Msk (0x1ul << SYS_P0_MFP_P0_ALT7_Pos)
#define | SYS_P0_MFP_P0_TYPE_Pos (16)
#define | SYS_P0_MFP_P0_TYPE_Msk (0xfful << SYS_P0_MFP_P0_TYPE_Pos)
#define | SYS_P1_MFP_P1_MFP_Pos (0)
#define | SYS_P1_MFP_P1_MFP_Msk (0xfful << SYS_P1_MFP_P1_MFP_Pos)
#define | SYS_P1_MFP_P1_ALT_Pos (8)
#define | SYS_P1_MFP_P1_ALT_Msk (0xfful << SYS_P1_MFP_P1_ALT_Pos)
#define | SYS_P1_MFP_P1_ALT0_Pos (8)
#define | SYS_P1_MFP_P1_ALT0_Msk (0x1ul << SYS_P1_MFP_P1_ALT0_Pos)
#define | SYS_P1_MFP_P1_ALT2_Pos (10)
#define | SYS_P1_MFP_P1_ALT2_Msk (0x1ul << SYS_P1_MFP_P1_ALT2_Pos)
#define | SYS_P1_MFP_P1_ALT3_Pos (11)
#define | SYS_P1_MFP_P1_ALT3_Msk (0x1ul << SYS_P1_MFP_P1_ALT3_Pos)
#define | SYS_P1_MFP_P1_ALT4_Pos (12)
#define | SYS_P1_MFP_P1_ALT4_Msk (0x1ul << SYS_P1_MFP_P1_ALT4_Pos)
#define | SYS_P1_MFP_P1_ALT5_Pos (13)
#define | SYS_P1_MFP_P1_ALT5_Msk (0x1ul << SYS_P1_MFP_P1_ALT5_Pos)
#define | SYS_P1_MFP_P1_TYPE_Pos (16)
#define | SYS_P1_MFP_P1_TYPE_Msk (0xfful << SYS_P1_MFP_P1_TYPE_Pos)
#define | SYS_P2_MFP_P2_MFP_Pos (0)
#define | SYS_P2_MFP_P2_MFP_Msk (0xfful << SYS_P2_MFP_P2_MFP_Pos)
#define | SYS_P2_MFP_P2_ALT_Pos (8)
#define | SYS_P2_MFP_P2_ALT_Msk (0xfful << SYS_P2_MFP_P2_ALT_Pos)
#define | SYS_P2_MFP_P2_ALT2_Pos (10)
#define | SYS_P2_MFP_P2_ALT2_Msk (0x1ul << SYS_P2_MFP_P2_ALT2_Pos)
#define | SYS_P2_MFP_P2_ALT3_Pos (11)
#define | SYS_P2_MFP_P2_ALT3_Msk (0x1ul << SYS_P2_MFP_P2_ALT3_Pos)
#define | SYS_P2_MFP_P2_ALT4_Pos (12)
#define | SYS_P2_MFP_P2_ALT4_Msk (0x1ul << SYS_P2_MFP_P2_ALT4_Pos)
#define | SYS_P2_MFP_P2_ALT5_Pos (13)
#define | SYS_P2_MFP_P2_ALT5_Msk (0x1ul << SYS_P2_MFP_P2_ALT5_Pos)
#define | SYS_P2_MFP_P2_ALT6_Pos (14)
#define | SYS_P2_MFP_P2_ALT6_Msk (0x1ul << SYS_P2_MFP_P2_ALT6_Pos)
#define | SYS_P2_MFP_P2_TYPE_Pos (16)
#define | SYS_P2_MFP_P2_TYPE_Msk (0xfful << SYS_P2_MFP_P2_TYPE_Pos)
#define | SYS_P3_MFP_P3_MFP_Pos (0)
#define | SYS_P3_MFP_P3_MFP_Msk (0xfful << SYS_P3_MFP_P3_MFP_Pos)
#define | SYS_P3_MFP_P3_ALT_Pos (8)
#define | SYS_P3_MFP_P3_ALT_Msk (0xfful << SYS_P3_MFP_P3_ALT_Pos)
#define | SYS_P3_MFP_P3_ALT0_Pos (8)
#define | SYS_P3_MFP_P3_ALT0_Msk (0x1ul << SYS_P3_MFP_P3_ALT0_Pos)
#define | SYS_P3_MFP_P3_ALT1_Pos (9)
#define | SYS_P3_MFP_P3_ALT1_Msk (0x1ul << SYS_P3_MFP_P3_ALT1_Pos)
#define | SYS_P3_MFP_P3_ALT2_Pos (10)
#define | SYS_P3_MFP_P3_ALT2_Msk (0x1ul << SYS_P3_MFP_P3_ALT2_Pos)
#define | SYS_P3_MFP_P3_ALT4_Pos (12)
#define | SYS_P3_MFP_P3_ALT4_Msk (0x1ul << SYS_P3_MFP_P3_ALT4_Pos)
#define | SYS_P3_MFP_P3_ALT5_Pos (13)
#define | SYS_P3_MFP_P3_ALT5_Msk (0x1ul << SYS_P3_MFP_P3_ALT5_Pos)
#define | SYS_P3_MFP_P3_ALT6_Pos (14)
#define | SYS_P3_MFP_P3_ALT6_Msk (0x1ul << SYS_P3_MFP_P3_ALT6_Pos)
#define | SYS_P3_MFP_P3_TYPE_Pos (16)
#define | SYS_P3_MFP_P3_TYPE_Msk (0xfful << SYS_P3_MFP_P3_TYPE_Pos)
#define | SYS_P3_MFP_P32CPP1_Pos (24)
#define | SYS_P3_MFP_P32CPP1_Msk (0x1ul << SYS_P3_MFP_P32CPP1_Pos)
#define | SYS_P4_MFP_P4_MFP_Pos (0)
#define | SYS_P4_MFP_P4_MFP_Msk (0xfful << SYS_P4_MFP_P4_MFP_Pos)
#define | SYS_P4_MFP_P4_ALT_Pos (8)
#define | SYS_P4_MFP_P4_ALT_Msk (0xfful << SYS_P4_MFP_P4_ALT_Pos)
#define | SYS_P4_MFP_P4_ALT6_Pos (14)
#define | SYS_P4_MFP_P4_ALT6_Msk (0x1ul << SYS_P4_MFP_P4_ALT6_Pos)
#define | SYS_P4_MFP_P4_ALT7_Pos (15)
#define | SYS_P4_MFP_P4_ALT7_Msk (0x1ul << SYS_P4_MFP_P4_ALT7_Pos)
#define | SYS_P4_MFP_P4_TYPE_Pos (16)
#define | SYS_P4_MFP_P4_TYPE_Msk (0xfful << SYS_P4_MFP_P4_TYPE_Pos)
#define | SYS_P5_MFP_P5_MFP_Pos (0)
#define | SYS_P5_MFP_P5_MFP_Msk (0xfful << SYS_P5_MFP_P5_MFP_Pos)
#define | SYS_P5_MFP_P5_ALT_Pos (8)
#define | SYS_P5_MFP_P5_ALT_Msk (0xFFul << SYS_P5_MFP_P5_ALT_Pos)
#define | SYS_P5_MFP_P5_ALT0_Pos (8)
#define | SYS_P5_MFP_P5_ALT0_Msk (0x1ul << SYS_P5_MFP_P5_ALT0_Pos)
#define | SYS_P5_MFP_P5_ALT1_Pos (9)
#define | SYS_P5_MFP_P5_ALT1_Msk (0x1ul << SYS_P5_MFP_P5_ALT1_Pos)
#define | SYS_P5_MFP_P5_ALT2_Pos (10)
#define | SYS_P5_MFP_P5_ALT2_Msk (0x1ul << SYS_P5_MFP_P5_ALT2_Pos)
#define | SYS_P5_MFP_P5_ALT3_Pos (11)
#define | SYS_P5_MFP_P5_ALT3_Msk (0x1ul << SYS_P5_MFP_P5_ALT3_Pos)
#define | SYS_P5_MFP_P5_ALT4_Pos (12)
#define | SYS_P5_MFP_P5_ALT4_Msk (0x1ul << SYS_P5_MFP_P5_ALT4_Pos)
#define | SYS_P5_MFP_P5_ALT5_Pos (13)
#define | SYS_P5_MFP_P5_ALT5_Msk (0x1ul << SYS_P5_MFP_P5_ALT5_Pos)
#define | SYS_P5_MFP_P5_TYPE_Pos (16)
#define | SYS_P5_MFP_P5_TYPE_Msk (0xfful << SYS_P5_MFP_P5_TYPE_Pos)
#define | SYS_IRCTRIMCTL_TRIM_SEL_Pos (0)
#define | SYS_IRCTRIMCTL_TRIM_SEL_Msk (0x1ul << SYS_IRCTRIMCTL_TRIM_SEL_Pos)
#define | SYS_IRCTRIMCTL_TRIM_LOOP_Pos (4)
#define | SYS_IRCTRIMCTL_TRIM_LOOP_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_LOOP_Pos)
#define | SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos (1)
#define | SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos)
#define | SYS_IRCTRIMIEN_32K_ERR_IEN_Pos (2)
#define | SYS_IRCTRIMIEN_32K_ERR_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_32K_ERR_IEN_Pos)
#define | SYS_IRCTRIMINT_FREQ_LOCK_Pos (0)
#define | SYS_IRCTRIMINT_FREQ_LOCK_Msk (0x1ul << SYS_IRCTRIMINT_FREQ_LOCK_Pos)
#define | SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos (1)
#define | SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk (0x1ul << SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos)
#define | SYS_IRCTRIMINT_32K_ERR_INT_Pos (2)
#define | SYS_IRCTRIMINT_32K_ERR_INT_Msk (0x1ul << SYS_IRCTRIMINT_32K_ERR_INT_Pos)
#define | SYS_RegLockAddr_RegUnLock_Pos 0
#define | SYS_RegLockAddr_RegUnLock_Msk (0x1ul << SYS_RegLockAddr_RegUnLock_Pos)
#define | GPIO_PMD_PMD0_Pos (0)
#define | GPIO_PMD_PMD0_Msk (0x3ul << GPIO_PMD_PMD0_Pos)
#define | GPIO_PMD_PMD1_Pos (2)
#define | GPIO_PMD_PMD1_Msk (0x3ul << GPIO_PMD_PMD1_Pos)
#define | GPIO_PMD_PMD2_Pos (4)
#define | GPIO_PMD_PMD2_Msk (0x3ul << GPIO_PMD_PMD2_Pos)
#define | GPIO_PMD_PMD3_Pos (6)
#define | GPIO_PMD_PMD3_Msk (0x3ul << GPIO_PMD_PMD3_Pos)
#define | GPIO_PMD_PMD4_Pos (8)
#define | GPIO_PMD_PMD4_Msk (0x3ul << GPIO_PMD_PMD4_Pos)
#define | GPIO_PMD_PMD5_Pos (10)
#define | GPIO_PMD_PMD5_Msk (0x3ul << GPIO_PMD_PMD5_Pos)
#define | GPIO_PMD_PMD6_Pos (12)
#define | GPIO_PMD_PMD6_Msk (0x3ul << GPIO_PMD_PMD6_Pos)
#define | GPIO_PMD_PMD7_Pos (14)
#define | GPIO_PMD_PMD7_Msk (0x3ul << GPIO_PMD_PMD7_Pos)
#define | GPIO_OFFD_OFFD_Pos (16)
#define | GPIO_OFFD_OFFD_Msk (0xfful << GPIO_OFFD_OFFD_Pos)
#define | GPIO_DOUT_DOUT_Pos (0)
#define | GPIO_DOUT_DOUT_Msk (0xfful << GPIO_DOUT_DOUT_Pos)
#define | GPIO_DMASK_DMASK_Pos (0)
#define | GPIO_DMASK_DMASK_Msk (0xfful << GPIO_DMASK_DMASK_Pos)
#define | GPIO_PIN_PIN_Pos (0)
#define | GPIO_PIN_PIN_Msk (0xfful << GPIO_PIN_PIN_Pos)
#define | GPIO_DBEN_DBEN_Pos (0)
#define | GPIO_DBEN_DBEN_Msk (0xfful << GPIO_DBEN_DBEN_Pos)
#define | GPIO_IMD_IMD_Pos (0)
#define | GPIO_IMD_IMD_Msk (0xfful << GPIO_IMD_IMD_Pos)
#define | GPIO_IEN_IF_EN_Pos (0)
#define | GPIO_IEN_IF_EN_Msk (0x1ul << GPIO_IEN_IF_EN_Pos)
#define | GPIO_IEN_IR_EN_Pos (16)
#define | GPIO_IEN_IR_EN_Msk (0xfful << GPIO_IEN_IR_EN_Pos)
#define | GPIO_ISRC_ISRC_Pos (0)
#define | GPIO_ISRC_ISRC_Msk (0xfful << GPIO_ISRC_ISRC_Pos)
#define | GPIO_DBNCECON_DBCLKSEL_Pos (0)
#define | GPIO_DBNCECON_DBCLKSEL_Msk (0xful << GPIO_DBNCECON_DBCLKSEL_Pos)
#define | GPIO_DBNCECON_DBCLKSRC_Pos (4)
#define | GPIO_DBNCECON_DBCLKSRC_Msk (0x1ul << GPIO_DBNCECON_DBCLKSRC_Pos)
#define | GPIO_DBNCECON_ICLK_ON_Pos (5)
#define | GPIO_DBNCECON_ICLK_ON_Msk (0x1ul << GPIO_DBNCECON_ICLK_ON_Pos)
#define | I2C_I2CON_AA_Pos (2)
#define | I2C_I2CON_AA_Msk (0x1ul << I2C_I2CON_AA_Pos)
#define | I2C_I2CON_SI_Pos (3)
#define | I2C_I2CON_SI_Msk (0x1ul << I2C_I2CON_SI_Pos)
#define | I2C_I2CON_STO_Pos (4)
#define | I2C_I2CON_STO_Msk (0x1ul << I2C_I2CON_STO_Pos)
#define | I2C_I2CON_STA_Pos (5)
#define | I2C_I2CON_STA_Msk (0x1ul << I2C_I2CON_STA_Pos)
#define | I2C_I2CON_ENSI_Pos (6)
#define | I2C_I2CON_ENSI_Msk (0x1ul << I2C_I2CON_ENSI_Pos)
#define | I2C_I2CON_EI_Pos (7)
#define | I2C_I2CON_EI_Msk (0x1ul << I2C_I2CON_EI_Pos)
#define | I2C_I2CADDR_GC_Pos (0)
#define | I2C_I2CADDR_GC_Msk (0x1ul << I2C_I2CADDR_GC_Pos)
#define | I2C_I2CADDR_I2CADDR_Pos (1)
#define | I2C_I2CADDR_I2CADDR_Msk (0x7ful << I2C_I2CADDR_I2CADDR_Pos)
#define | I2C_I2CDAT_I2CDAT_Pos (0)
#define | I2C_I2CDAT_I2CDAT_Msk (0xfful << I2C_I2CDAT_I2CDAT_Pos)
#define | I2C_I2CSTATUS_I2CSTATUS_Pos (0)
#define | I2C_I2CSTATUS_I2CSTATUS_Msk (0xfful << I2C_I2CSTATUS_I2CSTATUS_Pos)
#define | I2C_I2CLK_I2CLK_Pos (0)
#define | I2C_I2CLK_I2CLK_Msk (0xfful << I2C_I2CLK_I2CLK_Pos)
#define | I2C_I2CTOC_TIF_Pos (0)
#define | I2C_I2CTOC_TIF_Msk (0x1ul << I2C_I2CTOC_TIF_Pos)
#define | I2C_I2CTOC_DIV4_Pos (1)
#define | I2C_I2CTOC_DIV4_Msk (0x1ul << I2C_I2CTOC_DIV4_Pos)
#define | I2C_I2CTOC_ENTI_Pos (2)
#define | I2C_I2CTOC_ENTI_Msk (0x1ul << I2C_I2CTOC_ENTI_Pos)
#define | I2C_I2CADM_I2CADM_Pos (1)
#define | I2C_I2CADM_I2CADM_Msk (0x7ful << I2C_I2CADM_I2CADM_Pos)
#define | I2C_I2CON2_WKUPEN_Pos (0)
#define | I2C_I2CON2_WKUPEN_Msk (0x1ul << I2C_I2CON2_WKUPEN_Pos)
#define | I2C_I2CON2_TWOFF_EN_Pos (1)
#define | I2C_I2CON2_TWOFF_EN_Msk (0x1ul << I2C_I2CON2_TWOFF_EN_Pos)
#define | I2C_I2CON2_NOSTRETCH_Pos (2)
#define | I2C_I2CON2_NOSTRETCH_Msk (0x1ul << I2C_I2CON2_NOSTRETCH_Pos)
#define | I2C_I2CON2_OVER_INTEN_Pos (3)
#define | I2C_I2CON2_OVER_INTEN_Msk (0x1ul << I2C_I2CON2_OVER_INTEN_Pos)
#define | I2C_I2CON2_UNDER_INTEN_Pos (4)
#define | I2C_I2CON2_UNDER_INTEN_Msk (0x1ul << I2C_I2CON2_UNDER_INTEN_Pos)
#define | I2C_I2CSTATUS2_WAKEUP_Pos (0)
#define | I2C_I2CSTATUS2_WAKEUP_Msk (0x1ul << I2C_I2CSTATUS2_WAKEUP_Pos)
#define | I2C_I2CSTATUS2_FULL_Pos (1)
#define | I2C_I2CSTATUS2_FULL_Msk (0x1ul << I2C_I2CSTATUS2_FULL_Pos)
#define | I2C_I2CSTATUS2_EMPTY_Pos (2)
#define | I2C_I2CSTATUS2_EMPTY_Msk (0x1ul << I2C_I2CSTATUS2_EMPTY_Pos)
#define | I2C_I2CSTATUS2_OVERUN_Pos (3)
#define | I2C_I2CSTATUS2_OVERUN_Msk (0x1ul << I2C_I2CSTATUS2_OVERUN_Pos)
#define | I2C_I2CSTATUS2_UNDERUN_Pos (4)
#define | I2C_I2CSTATUS2_UNDERUN_Msk (0x1ul << I2C_I2CSTATUS2_UNDERUN_Pos)
#define | INT_SRC_INT_SRC_Pos (0)
#define | INT_SRC_INT_SRC_Msk (0x7ul << INT_SRC_INT_SRC_Pos)
#define | INT_CON_NMI_SEL_Pos (0)
#define | INT_CON_NMI_SEL_Msk (0x1ful << INT_CON_NMI_SEL_Pos)
#define | INT_CON_NMI_SEL_EN_Pos (8)
#define | INT_CON_NMI_SEL_EN_Msk (0x1ul << INT_CON_NMI_SEL_EN_Pos)
#define | INT_IRQ_MCU_IRQ_Pos (0)
#define | INT_IRQ_MCU_IRQ_Msk (0xfffffffful << INT_IRQ_MCU_IRQ_Pos)
#define | PWM_PPR_CP01_Pos (0)
#define | PWM_PPR_CP01_Msk (0xfful << PWM_PPR_CP01_Pos)
#define | PWM_PPR_CP23_Pos (8)
#define | PWM_PPR_CP23_Msk (0xfful << PWM_PPR_CP23_Pos)
#define | PWM_PPR_CP45_Pos (16)
#define | PWM_PPR_CP45_Msk (0xfful << PWM_PPR_CP45_Pos)
#define | PWM_CSR_CSR0_Pos (0)
#define | PWM_CSR_CSR0_Msk (0x7ul << PWM_CSR_CSR0_Pos)
#define | PWM_CSR_CSR1_Pos (4)
#define | PWM_CSR_CSR1_Msk (0x7ul << PWM_CSR_CSR1_Pos)
#define | PWM_CSR_CSR2_Pos (8)
#define | PWM_CSR_CSR2_Msk (0x7ul << PWM_CSR_CSR2_Pos)
#define | PWM_CSR_CSR3_Pos (12)
#define | PWM_CSR_CSR3_Msk (0x7ul << PWM_CSR_CSR3_Pos)
#define | PWM_CSR_CSR4_Pos (16)
#define | PWM_CSR_CSR4_Msk (0x7ul << PWM_CSR_CSR4_Pos)
#define | PWM_CSR_CSR5_Pos (20)
#define | PWM_CSR_CSR5_Msk (0x7ul << PWM_CSR_CSR5_Pos)
#define | PWM_PCR_CH0EN_Pos (0)
#define | PWM_PCR_CH0EN_Msk (0x1ul << PWM_PCR_CH0EN_Pos)
#define | PWM_PCR_DB_MOD_Pos (1)
#define | PWM_PCR_DB_MOD_Msk (0x1ul << PWM_PCR_DB_MOD_Pos)
#define | PWM_PCR_CH0INV_Pos (2)
#define | PWM_PCR_CH0INV_Msk (0x1ul << PWM_PCR_CH0INV_Pos)
#define | PWM_PCR_CH0MOD_Pos (3)
#define | PWM_PCR_CH0MOD_Msk (0x1ul << PWM_PCR_CH0MOD_Pos)
#define | PWM_PCR_CH1EN_Pos (4)
#define | PWM_PCR_CH1EN_Msk (0x1ul << PWM_PCR_CH1EN_Pos)
#define | PWM_PCR_CH1INV_Pos (6)
#define | PWM_PCR_CH1INV_Msk (0x1ul << PWM_PCR_CH1INV_Pos)
#define | PWM_PCR_CH1MOD_Pos (7)
#define | PWM_PCR_CH1MOD_Msk (0x1ul << PWM_PCR_CH1MOD_Pos)
#define | PWM_PCR_CH2EN_Pos (8)
#define | PWM_PCR_CH2EN_Msk (0x1ul << PWM_PCR_CH2EN_Pos)
#define | PWM_PCR_CH2INV_Pos (10)
#define | PWM_PCR_CH2INV_Msk (0x1ul << PWM_PCR_CH2INV_Pos)
#define | PWM_PCR_CH2MOD_Pos (11)
#define | PWM_PCR_CH2MOD_Msk (0x1ul << PWM_PCR_CH2MOD_Pos)
#define | PWM_PCR_CH3EN_Pos (12)
#define | PWM_PCR_CH3EN_Msk (0x1ul << PWM_PCR_CH3EN_Pos)
#define | PWM_PCR_CH3INV_Pos (14)
#define | PWM_PCR_CH3INV_Msk (0x1ul << PWM_PCR_CH3INV_Pos)
#define | PWM_PCR_CH3MOD_Pos (15)
#define | PWM_PCR_CH3MOD_Msk (0x1ul << PWM_PCR_CH3MOD_Pos)
#define | PWM_PCR_CH4EN_Pos (16)
#define | PWM_PCR_CH4EN_Msk (0x1ul << PWM_PCR_CH4EN_Pos)
#define | PWM_PCR_CH4INV_Pos (18)
#define | PWM_PCR_CH4INV_Msk (0x1ul << PWM_PCR_CH4INV_Pos)
#define | PWM_PCR_CH4MOD_Pos (19)
#define | PWM_PCR_CH4MOD_Msk (0x1ul << PWM_PCR_CH4MOD_Pos)
#define | PWM_PCR_CH5EN_Pos (20)
#define | PWM_PCR_CH5EN_Msk (0x1ul << PWM_PCR_CH5EN_Pos)
#define | PWM_PCR_CH5INV_Pos (22)
#define | PWM_PCR_CH5INV_Msk (0x1ul << PWM_PCR_CH5INV_Pos)
#define | PWM_PCR_CH5MOD_Pos (23)
#define | PWM_PCR_CH5MOD_Msk (0x1ul << PWM_PCR_CH5MOD_Pos)
#define | PWM_PCR_DZEN01_Pos (24)
#define | PWM_PCR_DZEN01_Msk (0x1ul << PWM_PCR_DZEN01_Pos)
#define | PWM_PCR_DZEN23_Pos (25)
#define | PWM_PCR_DZEN23_Msk (0x1ul << PWM_PCR_DZEN23_Pos)
#define | PWM_PCR_DZEN45_Pos (26)
#define | PWM_PCR_DZEN45_Msk (0x1ul << PWM_PCR_DZEN45_Pos)
#define | PWM_PCR_CLRPWM_Pos (27)
#define | PWM_PCR_CLRPWM_Msk (0x1ul << PWM_PCR_CLRPWM_Pos)
#define | PWM_PCR_PWMMOD_Pos (28)
#define | PWM_PCR_PWMMOD_Msk (0x3ul << PWM_PCR_PWMMOD_Pos)
#define | PWM_PCR_GRP_Pos (30)
#define | PWM_PCR_GRP_Msk (0x1ul << PWM_PCR_GRP_Pos)
#define | PWM_PCR_PWMTYPE_Pos (31)
#define | PWM_PCR_PWMTYPE_Msk (0x1ul << PWM_PCR_PWMTYPE_Pos)
#define | PWM_CNR_CNR_Pos 0
#define | PWM_CNR_CNR_Msk (0xfffful << PWM_CNR_CNR_Pos)
#define | PWM_CMR_CMR_Pos 0
#define | PWM_CMR_CMR_Msk (0xfffful << PWM_CMR_CMR_Pos)
#define | PWM_PIER_PWMPIE0_Pos (0)
#define | PWM_PIER_PWMPIE0_Msk (0x1ul << PWM_PIER_PWMPIE0_Pos)
#define | PWM_PIER_PWMPIE1_Pos (1)
#define | PWM_PIER_PWMPIE1_Msk (0x1ul << PWM_PIER_PWMPIE1_Pos)
#define | PWM_PIER_PWMPIE2_Pos (2)
#define | PWM_PIER_PWMPIE2_Msk (0x1ul << PWM_PIER_PWMPIE2_Pos)
#define | PWM_PIER_PWMPIE3_Pos (3)
#define | PWM_PIER_PWMPIE3_Msk (0x1ul << PWM_PIER_PWMPIE3_Pos)
#define | PWM_PIER_PWMPIE4_Pos (4)
#define | PWM_PIER_PWMPIE4_Msk (0x1ul << PWM_PIER_PWMPIE4_Pos)
#define | PWM_PIER_PWMPIE5_Pos (5)
#define | PWM_PIER_PWMPIE5_Msk (0x1ul << PWM_PIER_PWMPIE5_Pos)
#define | PWM_PIER_PWMDIE0_Pos (8)
#define | PWM_PIER_PWMDIE0_Msk (0x1ul << PWM_PIER_PWMDIE0_Pos)
#define | PWM_PIER_PWMDIE1_Pos (9)
#define | PWM_PIER_PWMDIE1_Msk (0x1ul << PWM_PIER_PWMDIE1_Pos)
#define | PWM_PIER_PWMDIE2_Pos (10)
#define | PWM_PIER_PWMDIE2_Msk (0x1ul << PWM_PIER_PWMDIE2_Pos)
#define | PWM_PIER_PWMDIE3_Pos (11)
#define | PWM_PIER_PWMDIE3_Msk (0x1ul << PWM_PIER_PWMDIE3_Pos)
#define | PWM_PIER_PWMDIE4_Pos (12)
#define | PWM_PIER_PWMDIE4_Msk (0x1ul << PWM_PIER_PWMDIE4_Pos)
#define | PWM_PIER_PWMDIE5_Pos (13)
#define | PWM_PIER_PWMDIE5_Msk (0x1ul << PWM_PIER_PWMDIE5_Pos)
#define | PWM_PIER_BRKIE_Pos (16)
#define | PWM_PIER_BRKIE_Msk (0x1ul << PWM_PIER_BRKIE_Pos)
#define | PWM_PIER_INT_TYPE_Pos (17)
#define | PWM_PIER_INT_TYPE_Msk (0x1ul << PWM_PIER_INT_TYPE_Pos)
#define | PWM_PIIR_PWMPIF0_Pos (0)
#define | PWM_PIIR_PWMPIF0_Msk (0x1ul << PWM_PIIR_PWMPIF0_Pos)
#define | PWM_PIIR_PWMPIF1_Pos (1)
#define | PWM_PIIR_PWMPIF1_Msk (0x1ul << PWM_PIIR_PWMPIF1_Pos)
#define | PWM_PIIR_PWMPIF2_Pos (2)
#define | PWM_PIIR_PWMPIF2_Msk (0x1ul << PWM_PIIR_PWMPIF2_Pos)
#define | PWM_PIIR_PWMPIF3_Pos (3)
#define | PWM_PIIR_PWMPIF3_Msk (0x1ul << PWM_PIIR_PWMPIF3_Pos)
#define | PWM_PIIR_PWMPIF4_Pos (4)
#define | PWM_PIIR_PWMPIF4_Msk (0x1ul << PWM_PIIR_PWMPIF4_Pos)
#define | PWM_PIIR_PWMPIF5_Pos (5)
#define | PWM_PIIR_PWMPIF5_Msk (0x1ul << PWM_PIIR_PWMPIF5_Pos)
#define | PWM_PIIR_PWMDIF0_Pos (8)
#define | PWM_PIIR_PWMDIF0_Msk (0x1ul << PWM_PIIR_PWMDIF0_Pos)
#define | PWM_PIIR_PWMDIF1_Pos (9)
#define | PWM_PIIR_PWMDIF1_Msk (0x1ul << PWM_PIIR_PWMDIF1_Pos)
#define | PWM_PIIR_PWMDIF2_Pos (10)
#define | PWM_PIIR_PWMDIF2_Msk (0x1ul << PWM_PIIR_PWMDIF2_Pos)
#define | PWM_PIIR_PWMDIF3_Pos (11)
#define | PWM_PIIR_PWMDIF3_Msk (0x1ul << PWM_PIIR_PWMDIF3_Pos)
#define | PWM_PIIR_PWMDIF4_Pos (12)
#define | PWM_PIIR_PWMDIF4_Msk (0x1ul << PWM_PIIR_PWMDIF4_Pos)
#define | PWM_PIIR_PWMDIF5_Pos (13)
#define | PWM_PIIR_PWMDIF5_Msk (0x1ul << PWM_PIIR_PWMDIF5_Pos)
#define | PWM_PIIR_BKF0_Pos (16)
#define | PWM_PIIR_BKF0_Msk (0x1ul << PWM_PIIR_BKF0_Pos)
#define | PWM_PIIR_BKF1_Pos (17)
#define | PWM_PIIR_BKF1_Msk (0x1ul << PWM_PIIR_BKF1_Pos)
#define | PWM_POE_PWM0_Pos (0)
#define | PWM_POE_PWM0_Msk (0x1ul << PWM_POE_PWM0_Pos)
#define | PWM_POE_PWM1_Pos (1)
#define | PWM_POE_PWM1_Msk (0x1ul << PWM_POE_PWM1_Pos)
#define | PWM_POE_PWM2_Pos (2)
#define | PWM_POE_PWM2_Msk (0x1ul << PWM_POE_PWM2_Pos)
#define | PWM_POE_PWM3_Pos (3)
#define | PWM_POE_PWM3_Msk (0x1ul << PWM_POE_PWM3_Pos)
#define | PWM_POE_PWM4_Pos (4)
#define | PWM_POE_PWM4_Msk (0x1ul << PWM_POE_PWM4_Pos)
#define | PWM_POE_PWM5_Pos (5)
#define | PWM_POE_PWM5_Msk (0x1ul << PWM_POE_PWM5_Pos)
#define | PWM_PFBCON_BKEN0_Pos (0)
#define | PWM_PFBCON_BKEN0_Msk (0x1ul << PWM_PFBCON_BKEN0_Pos)
#define | PWM_PFBCON_BKEN1_Pos (1)
#define | PWM_PFBCON_BKEN1_Msk (0x1ul << PWM_PFBCON_BKEN1_Pos)
#define | PWM_PFBCON_CPO0BKEN_Pos (2)
#define | PWM_PFBCON_CPO0BKEN_Msk (0x1ul << PWM_PFBCON_CPO0BKEN_Pos)
#define | PWM_PFBCON_CPO1BKEN_Pos (3)
#define | PWM_PFBCON_CPO1BKEN_Msk (0x1ul << PWM_PFBCON_CPO1BKEN_Pos)
#define | PWM_PFBCON_BKF_Pos (7)
#define | PWM_PFBCON_BKF_Msk (0x1ul << PWM_PFBCON_BKF_Pos)
#define | PWM_PFBCON_PWMBKO0_Pos (24)
#define | PWM_PFBCON_PWMBKO0_Msk (0x1ul << PWM_PFBCON_PWMBKO0_Pos)
#define | PWM_PFBCON_PWMBKO1_Pos (25)
#define | PWM_PFBCON_PWMBKO1_Msk (0x1ul << PWM_PFBCON_PWMBKO1_Pos)
#define | PWM_PFBCON_PWMBKO2_Pos (26)
#define | PWM_PFBCON_PWMBKO2_Msk (0x1ul << PWM_PFBCON_PWMBKO2_Pos)
#define | PWM_PFBCON_PWMBKO3_Pos (27)
#define | PWM_PFBCON_PWMBKO3_Msk (0x1ul << PWM_PFBCON_PWMBKO3_Pos)
#define | PWM_PFBCON_PWMBKO4_Pos (28)
#define | PWM_PFBCON_PWMBKO4_Msk (0x1ul << PWM_PFBCON_PWMBKO4_Pos)
#define | PWM_PFBCON_PWMBKO5_Pos (29)
#define | PWM_PFBCON_PWMBKO5_Msk (0x1ul << PWM_PFBCON_PWMBKO5_Pos)
#define | PWM_PFBCON_D6BKO6_Pos (30)
#define | PWM_PFBCON_D6BKO6_Msk (0x1ul << PWM_PFBCON_D6BKO6_Pos)
#define | PWM_PFBCON_D7BKO7_Pos (31)
#define | PWM_PFBCON_D7BKO7_Msk (0x1ul << PWM_PFBCON_D7BKO7_Pos)
#define | PWM_DZIR_DZI01_Pos (0)
#define | PWM_DZIR_DZI01_Msk (0xfful << PWM_DZIR_DZI01_Pos)
#define | PWM_DZIR_DZI23_Pos (8)
#define | PWM_DZIR_DZI23_Msk (0xfful << PWM_DZIR_DZI23_Pos)
#define | PWM_DZIR_DZI45_Pos (16)
#define | PWM_DZIR_DZI45_Msk (0xfful << PWM_DZIR_DZI45_Pos)
#define | PWM_TRGCON0_CM0TRGREN_Pos (0)
#define | PWM_TRGCON0_CM0TRGREN_Msk (0x1ul << PWM_TRGCON0_CM0TRGREN_Pos)
#define | PWM_TRGCON0_CNT0TRGEN_Pos (1)
#define | PWM_TRGCON0_CNT0TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT0TRGEN_Pos)
#define | PWM_TRGCON0_CM0TRGFEN_Pos (2)
#define | PWM_TRGCON0_CM0TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM0TRGFEN_Pos)
#define | PWM_TRGCON0_P0TRGEN_Pos (3)
#define | PWM_TRGCON0_P0TRGEN_Msk (0x1ul << PWM_TRGCON0_P0TRGEN_Pos)
#define | PWM_TRGCON0_CM1TRGREN_Pos (8)
#define | PWM_TRGCON0_CM1TRGREN_Msk (0x1ul << PWM_TRGCON0_CM1TRGREN_Pos)
#define | PWM_TRGCON0_CNT1TRGEN_Pos (9)
#define | PWM_TRGCON0_CNT1TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT1TRGEN_Pos)
#define | PWM_TRGCON0_CM1TRGFEN_Pos (10)
#define | PWM_TRGCON0_CM1TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM1TRGFEN_Pos)
#define | PWM_TRGCON0_P1TRGEN_Pos (11)
#define | PWM_TRGCON0_P1TRGEN_Msk (0x1ul << PWM_TRGCON0_P1TRGEN_Pos)
#define | PWM_TRGCON0_CM2TRGREN_Pos (16)
#define | PWM_TRGCON0_CM2TRGREN_Msk (0x1ul << PWM_TRGCON0_CM2TRGREN_Pos)
#define | PWM_TRGCON0_CNT2TRGEN_Pos (17)
#define | PWM_TRGCON0_CNT2TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT2TRGEN_Pos)
#define | PWM_TRGCON0_CM2TRGFEN_Pos (18)
#define | PWM_TRGCON0_CM2TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM2TRGFEN_Pos)
#define | PWM_TRGCON0_P2TRGEN_Pos (19)
#define | PWM_TRGCON0_P2TRGEN_Msk (0x1ul << PWM_TRGCON0_P2TRGEN_Pos)
#define | PWM_TRGCON0_CM3TRGREN_Pos (24)
#define | PWM_TRGCON0_CM3TRGREN_Msk (0x1ul << PWM_TRGCON0_CM3TRGREN_Pos)
#define | PWM_TRGCON0_CNT3TRGEN_Pos (25)
#define | PWM_TRGCON0_CNT3TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT3TRGEN_Pos)
#define | PWM_TRGCON0_CM3TRGFEN_Pos (26)
#define | PWM_TRGCON0_CM3TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM3TRGFEN_Pos)
#define | PWM_TRGCON0_P3TRGEN_Pos (27)
#define | PWM_TRGCON0_P3TRGEN_Msk (0x1ul << PWM_TRGCON0_P3TRGEN_Pos)
#define | PWM_TRGCON1_CM4TRGREN_Pos (0)
#define | PWM_TRGCON1_CM4TRGREN_Msk (0x1ul << PWM_TRGCON1_CM4TRGREN_Pos)
#define | PWM_TRGCON1_CNT4TRGEN_Pos (1)
#define | PWM_TRGCON1_CNT4TRGEN_Msk (0x1ul << PWM_TRGCON1_CNT4TRGEN_Pos)
#define | PWM_TRGCON1_CM4TRGFEN_Pos (2)
#define | PWM_TRGCON1_CM4TRGFEN_Msk (0x1ul << PWM_TRGCON1_CM4TRGFEN_Pos)
#define | PWM_TRGCON1_P4TRGEN_Pos (3)
#define | PWM_TRGCON1_P4TRGEN_Msk (0x1ul << PWM_TRGCON1_P4TRGEN_Pos)
#define | PWM_TRGCON1_CM5TRGREN_Pos (8)
#define | PWM_TRGCON1_CM5TRGREN_Msk (0x1ul << PWM_TRGCON1_CM5TRGREN_Pos)
#define | PWM_TRGCON1_CNT5TRGEN_Pos (9)
#define | PWM_TRGCON1_CNT5TRGEN_Msk (0x1ul << PWM_TRGCON1_CNT5TRGEN_Pos)
#define | PWM_TRGCON1_CM5TRGFEN_Pos (10)
#define | PWM_TRGCON1_CM5TRGFEN_Msk (0x1ul << PWM_TRGCON1_CM5TRGFEN_Pos)
#define | PWM_TRGCON1_P5TRGEN_Pos (11)
#define | PWM_TRGCON1_P5TRGEN_Msk (0x1ul << PWM_TRGCON1_P5TRGEN_Pos)
#define | PWM_TRGSTS0_CMR0FLAG_R_Pos (0)
#define | PWM_TRGSTS0_CMR0FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR0FLAG_R_Pos)
#define | PWM_TRGSTS0_CNT0FLAG_Pos (1)
#define | PWM_TRGSTS0_CNT0FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT0FLAG_Pos)
#define | PWM_TRGSTS0_CMR0FLAG_F_Pos (2)
#define | PWM_TRGSTS0_CMR0FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR0FLAG_F_Pos)
#define | PWM_TRGSTS0_PERID0FLAG_Pos (3)
#define | PWM_TRGSTS0_PERID0FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID0FLAG_Pos)
#define | PWM_TRGSTS0_CMR1FLAG_R_Pos (8)
#define | PWM_TRGSTS0_CMR1FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR1FLAG_R_Pos)
#define | PWM_TRGSTS0_CNT1FLAG_Pos (9)
#define | PWM_TRGSTS0_CNT1FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT1FLAG_Pos)
#define | PWM_TRGSTS0_CMR1FLAG_F_Pos (10)
#define | PWM_TRGSTS0_CMR1FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR1FLAG_F_Pos)
#define | PWM_TRGSTS0_PERID1FLAG_Pos (11)
#define | PWM_TRGSTS0_PERID1FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID1FLAG_Pos)
#define | PWM_TRGSTS0_CMR2FLAG_R_Pos (16)
#define | PWM_TRGSTS0_CMR2FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR2FLAG_R_Pos)
#define | PWM_TRGSTS0_CNT2FLAG_Pos (17)
#define | PWM_TRGSTS0_CNT2FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT2FLAG_Pos)
#define | PWM_TRGSTS0_CMR2FLAG_F_Pos (18)
#define | PWM_TRGSTS0_CMR2FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR2FLAG_F_Pos)
#define | PWM_TRGSTS0_PERID2FLAG_Pos (19)
#define | PWM_TRGSTS0_PERID2FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID2FLAG_Pos)
#define | PWM_TRGSTS0_CMR3FLAG_R_Pos (24)
#define | PWM_TRGSTS0_CMR3FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR3FLAG_R_Pos)
#define | PWM_TRGSTS0_CNT3FLAG_Pos (25)
#define | PWM_TRGSTS0_CNT3FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT3FLAG_Pos)
#define | PWM_TRGSTS0_CMR3FLAG_F_Pos (26)
#define | PWM_TRGSTS0_CMR3FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR3FLAG_F_Pos)
#define | PWM_TRGSTS0_PERID3FLAG_Pos (27)
#define | PWM_TRGSTS0_PERID3FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID3FLAG_Pos)
#define | PWM_TRGSTS1_CMR4FLAG_R_Pos (0)
#define | PWM_TRGSTS1_CMR4FLAG_R_Msk (0x1ul << PWM_TRGSTS1_CMR4FLAG_R_Pos)
#define | PWM_TRGSTS1_CNT4FLAG_Pos (1)
#define | PWM_TRGSTS1_CNT4FLAG_Msk (0x1ul << PWM_TRGSTS1_CNT4FLAG_Pos)
#define | PWM_TRGSTS1_CMR4FLAG_F_Pos (2)
#define | PWM_TRGSTS1_CMR4FLAG_F_Msk (0x1ul << PWM_TRGSTS1_CMR4FLAG_F_Pos)
#define | PWM_TRGSTS1_PERID4FLAG_Pos (3)
#define | PWM_TRGSTS1_PERID4FLAG_Msk (0x1ul << PWM_TRGSTS1_PERID4FLAG_Pos)
#define | PWM_TRGSTS1_CMR5FLAG_R_Pos (8)
#define | PWM_TRGSTS1_CMR5FLAG_R_Msk (0x1ul << PWM_TRGSTS1_CMR5FLAG_R_Pos)
#define | PWM_TRGSTS1_CNT5FLAG_Pos (9)
#define | PWM_TRGSTS1_CNT5FLAG_Msk (0x1ul << PWM_TRGSTS1_CNT5FLAG_Pos)
#define | PWM_TRGSTS1_CMR5FLAG_F_Pos (10)
#define | PWM_TRGSTS1_CMR5FLAG_F_Msk (0x1ul << PWM_TRGSTS1_CMR5FLAG_F_Pos)
#define | PWM_TRGSTS1_PERID5FLAG_Pos (11)
#define | PWM_TRGSTS1_PERID5FLAG_Msk (0x1ul << PWM_TRGSTS1_PERID5FLAG_Pos)
#define | PWM_PHCHG_D0_Pos (0)
#define | PWM_PHCHG_D0_Msk (0x1ul << PWM_PHCHG_D0_Pos)
#define | PWM_PHCHG_D1_Pos (1)
#define | PWM_PHCHG_D1_Msk (0x1ul << PWM_PHCHG_D1_Pos)
#define | PWM_PHCHG_D2_Pos (2)
#define | PWM_PHCHG_D2_Msk (0x1ul << PWM_PHCHG_D2_Pos)
#define | PWM_PHCHG_D3_Pos (3)
#define | PWM_PHCHG_D3_Msk (0x1ul << PWM_PHCHG_D3_Pos)
#define | PWM_PHCHG_D4_Pos (4)
#define | PWM_PHCHG_D4_Msk (0x1ul << PWM_PHCHG_D4_Pos)
#define | PWM_PHCHG_D5_Pos (5)
#define | PWM_PHCHG_D5_Msk (0x1ul << PWM_PHCHG_D5_Pos)
#define | PWM_PHCHG_D6_Pos (6)
#define | PWM_PHCHG_D6_Msk (0x1ul << PWM_PHCHG_D6_Pos)
#define | PWM_PHCHG_D7_Pos (7)
#define | PWM_PHCHG_D7_Msk (0x1ul << PWM_PHCHG_D7_Pos)
#define | PWM_PHCHG_PWM0_Pos (8)
#define | PWM_PHCHG_PWM0_Msk (0x1ul << PWM_PHCHG_PWM0_Pos)
#define | PWM_PHCHG_PWM1_Pos (9)
#define | PWM_PHCHG_PWM1_Msk (0x1ul << PWM_PHCHG_PWM1_Pos)
#define | PWM_PHCHG_PWM2_Pos (10)
#define | PWM_PHCHG_PWM2_Msk (0x1ul << PWM_PHCHG_PWM2_Pos)
#define | PWM_PHCHG_PWM3_Pos (11)
#define | PWM_PHCHG_PWM3_Msk (0x1ul << PWM_PHCHG_PWM3_Pos)
#define | PWM_PHCHG_PWM4_Pos (12)
#define | PWM_PHCHG_PWM4_Msk (0x1ul << PWM_PHCHG_PWM4_Pos)
#define | PWM_PHCHG_PWM5_Pos (13)
#define | PWM_PHCHG_PWM5_Msk (0x1ul << PWM_PHCHG_PWM5_Pos)
#define | PWM_PHCHG_ACCNT0_Pos (14)
#define | PWM_PHCHG_ACCNT0_Msk (0x1ul << PWM_PHCHG_ACCNT0_Pos)
#define | PWM_PHCHG_ACCNT1_Pos (15)
#define | PWM_PHCHG_ACCNT1_Msk (0x1ul << PWM_PHCHG_ACCNT1_Pos)
#define | PWM_PHCHG_CH01TOFF1_Pos (16)
#define | PWM_PHCHG_CH01TOFF1_Msk (0x1ul << PWM_PHCHG_CH01TOFF1_Pos)
#define | PWM_PHCHG_CH11TOFF1_Pos (17)
#define | PWM_PHCHG_CH11TOFF1_Msk (0x1ul << PWM_PHCHG_CH11TOFF1_Pos)
#define | PWM_PHCHG_CH21TOFF1_Pos (18)
#define | PWM_PHCHG_CH21TOFF1_Msk (0x1ul << PWM_PHCHG_CH21TOFF1_Pos)
#define | PWM_PHCHG_CH31TOFF1_Pos (19)
#define | PWM_PHCHG_CH31TOFF1_Msk (0x1ul << PWM_PHCHG_CH31TOFF1_Pos)
#define | PWM_PHCHG_CMP1SEL_Pos (20)
#define | PWM_PHCHG_CMP1SEL_Msk (0x3ul << PWM_PHCHG_CMP1SEL_Pos)
#define | PWM_PHCHG_T1_Pos (22)
#define | PWM_PHCHG_T1_Msk (0x1ul << PWM_PHCHG_T1_Pos)
#define | PWM_PHCHG_CE1_Pos (23)
#define | PWM_PHCHG_CE1_Msk (0x1ul << PWM_PHCHG_CE1_Pos)
#define | PWM_PHCHG_CH01TOFF0_Pos (24)
#define | PWM_PHCHG_CH01TOFF0_Msk (0x1ul << PWM_PHCHG_CH01TOFF0_Pos)
#define | PWM_PHCHG_CH11TOFF0_Pos (25)
#define | PWM_PHCHG_CH11TOFF0_Msk (0x1ul << PWM_PHCHG_CH11TOFF0_Pos)
#define | PWM_PHCHG_CH21TOFF0_Pos (26)
#define | PWM_PHCHG_CH21TOFF0_Msk (0x1ul << PWM_PHCHG_CH21TOFF0_Pos)
#define | PWM_PHCHG_CH31TOFF0_Pos (27)
#define | PWM_PHCHG_CH31TOFF0_Msk (0x1ul << PWM_PHCHG_CH31TOFF0_Pos)
#define | PWM_PHCHG_CMP0SEL_Pos (28)
#define | PWM_PHCHG_CMP0SEL_Msk (0x3ul << PWM_PHCHG_CMP0SEL_Pos)
#define | PWM_PHCHG_T0_Pos (30)
#define | PWM_PHCHG_T0_Msk (0x1ul << PWM_PHCHG_T0_Pos)
#define | PWM_PHCHG_CE0_Pos (31)
#define | PWM_PHCHG_CE0_Msk (0x1ul << PWM_PHCHG_CE0_Pos)
#define | PWM_PHCHGNXT_D0_Pos (0)
#define | PWM_PHCHGNXT_D0_Msk (0x1ul << PWM_PHCHGNXT_D0_Pos)
#define | PWM_PHCHGNXT_D1_Pos (1)
#define | PWM_PHCHGNXT_D1_Msk (0x1ul << PWM_PHCHGNXT_D1_Pos)
#define | PWM_PHCHGNXT_D2_Pos (2)
#define | PWM_PHCHGNXT_D2_Msk (0x1ul << PWM_PHCHGNXT_D2_Pos)
#define | PWM_PHCHGNXT_D3_Pos (3)
#define | PWM_PHCHGNXT_D3_Msk (0x1ul << PWM_PHCHGNXT_D3_Pos)
#define | PWM_PHCHGNXT_D4_Pos (4)
#define | PWM_PHCHGNXT_D4_Msk (0x1ul << PWM_PHCHGNXT_D4_Pos)
#define | PWM_PHCHGNXT_D5_Pos (5)
#define | PWM_PHCHGNXT_D5_Msk (0x1ul << PWM_PHCHGNXT_D5_Pos)
#define | PWM_PHCHGNXT_D6_Pos (6)
#define | PWM_PHCHGNXT_D6_Msk (0x1ul << PWM_PHCHGNXT_D6_Pos)
#define | PWM_PHCHGNXT_D7_Pos (7)
#define | PWM_PHCHGNXT_D7_Msk (0x1ul << PWM_PHCHGNXT_D7_Pos)
#define | PWM_PHCHGNXT_PWM0_Pos (8)
#define | PWM_PHCHGNXT_PWM0_Msk (0x1ul << PWM_PHCHGNXT_PWM0_Pos)
#define | PWM_PHCHGNXT_PWM1_Pos (9)
#define | PWM_PHCHGNXT_PWM1_Msk (0x1ul << PWM_PHCHGNXT_PWM1_Pos)
#define | PWM_PHCHGNXT_PWM2_Pos (10)
#define | PWM_PHCHGNXT_PWM2_Msk (0x1ul << PWM_PHCHGNXT_PWM2_Pos)
#define | PWM_PHCHGNXT_PWM3_Pos (11)
#define | PWM_PHCHGNXT_PWM3_Msk (0x1ul << PWM_PHCHGNXT_PWM3_Pos)
#define | PWM_PHCHGNXT_PWM4_Pos (12)
#define | PWM_PHCHGNXT_PWM4_Msk (0x1ul << PWM_PHCHGNXT_PWM4_Pos)
#define | PWM_PHCHGNXT_PWM5_Pos (13)
#define | PWM_PHCHGNXT_PWM5_Msk (0x1ul << PWM_PHCHGNXT_PWM5_Pos)
#define | PWM_PHCHGNXT_ACCNT0_Pos (14)
#define | PWM_PHCHGNXT_ACCNT0_Msk (0x1ul << PWM_PHCHGNXT_ACCNT0_Pos)
#define | PWM_PHCHGNXT_ACCNT1_Pos (15)
#define | PWM_PHCHGNXT_ACCNT1_Msk (0x1ul << PWM_PHCHGNXT_ACCNT1_Pos)
#define | PWM_PHCHGNXT_CH01TOFF1_Pos (16)
#define | PWM_PHCHGNXT_CH01TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH01TOFF1_Pos)
#define | PWM_PHCHGNXT_CH11TOFF1_Pos (17)
#define | PWM_PHCHGNXT_CH11TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH11TOFF1_Pos)
#define | PWM_PHCHGNXT_CH21TOFF1_Pos (18)
#define | PWM_PHCHGNXT_CH21TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH21TOFF1_Pos)
#define | PWM_PHCHGNXT_CH31TOFF1_Pos (19)
#define | PWM_PHCHGNXT_CH31TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH31TOFF1_Pos)
#define | PWM_PHCHGNXT_CMP1SEL_Pos (20)
#define | PWM_PHCHGNXT_CMP1SEL_Msk (0x3ul << PWM_PHCHGNXT_CMP1SEL_Pos)
#define | PWM_PHCHGNXT_T1_Pos (22)
#define | PWM_PHCHGNXT_T1_Msk (0x1ul << PWM_PHCHGNXT_T1_Pos)
#define | PWM_PHCHGNXT_CE1_Pos (23)
#define | PWM_PHCHGNXT_CE1_Msk (0x1ul << PWM_PHCHGNXT_CE1_Pos)
#define | PWM_PHCHGNXT_CH01TOFF0_Pos (24)
#define | PWM_PHCHGNXT_CH01TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH01TOFF0_Pos)
#define | PWM_PHCHGNXT_CH11TOFF0_Pos (25)
#define | PWM_PHCHGNXT_CH11TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH11TOFF0_Pos)
#define | PWM_PHCHGNXT_CH21TOFF0_Pos (26)
#define | PWM_PHCHGNXT_CH21TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH21TOFF0_Pos)
#define | PWM_PHCHGNXT_CH31TOFF0_Pos (27)
#define | PWM_PHCHGNXT_CH31TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH31TOFF0_Pos)
#define | PWM_PHCHGNXT_CMP0SEL_Pos (28)
#define | PWM_PHCHGNXT_CMP0SEL_Msk (0x3ul << PWM_PHCHGNXT_CMP0SEL_Pos)
#define | PWM_PHCHGNXT_T0_Pos (30)
#define | PWM_PHCHGNXT_T0_Msk (0x1ul << PWM_PHCHGNXT_T0_Pos)
#define | PWM_PHCHGNXT_CE0_Pos (31)
#define | PWM_PHCHGNXT_CE0_Msk (0x1ul << PWM_PHCHGNXT_CE0_Pos)
#define | PWM_PHCHGMASK_MASK6_Pos (6)
#define | PWM_PHCHGMASK_MASK6_Msk (0x1ul << PWM_PHCHGMASK_MASK6_Pos)
#define | PWM_PHCHGMASK_MASK7_Pos (7)
#define | PWM_PHCHGMASK_MASK7_Msk (0x1ul << PWM_PHCHGMASK_MASK7_Pos)
#define | PWM_PHCHGMASK_CMPMASK_Pos (8)
#define | PWM_PHCHGMASK_CMPMASK_Msk (0x3ul << PWM_PHCHGMASK_CMPMASK_Pos)
#define | PWM_PHCHGMASK_CMPMASK0_Pos (8)
#define | PWM_PHCHGMASK_CMPMASK0_Msk (0x1ul << PWM_PHCHGMASK_CMPMASK0_Pos)
#define | PWM_PHCHGMASK_CMPMASK1_Pos (9)
#define | PWM_PHCHGMASK_CMPMASK1_Msk (0x1ul << PWM_PHCHGMASK_CMPMASK1_Pos)
#define | PWM_INTACCUCTL_INTACCUEN0_Pos (0)
#define | PWM_INTACCUCTL_INTACCUEN0_Msk (0x1ul << PWM_INTACCUCTL_INTACCUEN0_Pos)
#define | PWM_INTACCUCTL_PERIODCNT_Pos (4)
#define | PWM_INTACCUCTL_PERIODCNT_Msk (0xful << PWM_INTACCUCTL_PERIODCNT_Pos)
#define | SPI_CNTRL_GO_BUSY_Pos (0)
#define | SPI_CNTRL_GO_BUSY_Msk (0x1ul << SPI_CNTRL_GO_BUSY_Pos)
#define | SPI_CNTRL_RX_NEG_Pos (1)
#define | SPI_CNTRL_RX_NEG_Msk (0x1ul << SPI_CNTRL_RX_NEG_Pos)
#define | SPI_CNTRL_TX_NEG_Pos (2)
#define | SPI_CNTRL_TX_NEG_Msk (0x1ul << SPI_CNTRL_TX_NEG_Pos)
#define | SPI_CNTRL_TX_BIT_LEN_Pos (3)
#define | SPI_CNTRL_TX_BIT_LEN_Msk (0x1ful << SPI_CNTRL_TX_BIT_LEN_Pos)
#define | SPI_CNTRL_LSB_Pos (10)
#define | SPI_CNTRL_LSB_Msk (0x1ul << SPI_CNTRL_LSB_Pos)
#define | SPI_CNTRL_CLKP_Pos (11)
#define | SPI_CNTRL_CLKP_Msk (0x1ul << SPI_CNTRL_CLKP_Pos)
#define | SPI_CNTRL_SP_CYCLE_Pos (12)
#define | SPI_CNTRL_SP_CYCLE_Msk (0xful << SPI_CNTRL_SP_CYCLE_Pos)
#define | SPI_CNTRL_IF_Pos (16)
#define | SPI_CNTRL_IF_Msk (0x1ul << SPI_CNTRL_IF_Pos)
#define | SPI_CNTRL_IE_Pos (17)
#define | SPI_CNTRL_IE_Msk (0x1ul << SPI_CNTRL_IE_Pos)
#define | SPI_CNTRL_SLAVE_Pos (18)
#define | SPI_CNTRL_SLAVE_Msk (0x1ul << SPI_CNTRL_SLAVE_Pos)
#define | SPI_CNTRL_REORDER_Pos (19)
#define | SPI_CNTRL_REORDER_Msk (0x1ul << SPI_CNTRL_REORDER_Pos)
#define | SPI_CNTRL_FIFO_Pos (21)
#define | SPI_CNTRL_FIFO_Msk (0x1ul << SPI_CNTRL_FIFO_Pos)
#define | SPI_CNTRL_RX_EMPTY_Pos (24)
#define | SPI_CNTRL_RX_EMPTY_Msk (0x1ul << SPI_CNTRL_RX_EMPTY_Pos)
#define | SPI_CNTRL_RX_FULL_Pos (25)
#define | SPI_CNTRL_RX_FULL_Msk (0x1ul << SPI_CNTRL_RX_FULL_Pos)
#define | SPI_CNTRL_TX_EMPTY_Pos (26)
#define | SPI_CNTRL_TX_EMPTY_Msk (0x1ul << SPI_CNTRL_TX_EMPTY_Pos)
#define | SPI_CNTRL_TX_FULL_Pos (27)
#define | SPI_CNTRL_TX_FULL_Msk (0x1ul << SPI_CNTRL_TX_FULL_Pos)
#define | SPI_DIVIDER_DIVIDER_Pos (0)
#define | SPI_DIVIDER_DIVIDER_Msk (0xfful << SPI_DIVIDER_DIVIDER_Pos)
#define | SPI_SSR_SSR_Pos (0)
#define | SPI_SSR_SSR_Msk (0x1ul << SPI_SSR_SSR_Pos)
#define | SPI_SSR_SS_LVL_Pos (2)
#define | SPI_SSR_SS_LVL_Msk (0x1ul << SPI_SSR_SS_LVL_Pos)
#define | SPI_SSR_AUTOSS_Pos (3)
#define | SPI_SSR_AUTOSS_Msk (0x1ul << SPI_SSR_AUTOSS_Pos)
#define | SPI_SSR_SS_LTRIG_Pos (4)
#define | SPI_SSR_SS_LTRIG_Msk (0x1ul << SPI_SSR_SS_LTRIG_Pos)
#define | SPI_SSR_LTRIG_FLAG_Pos (5)
#define | SPI_SSR_LTRIG_FLAG_Msk (0x1ul << SPI_SSR_LTRIG_FLAG_Pos)
#define | SPI_RX_RX_Pos (0)
#define | SPI_RX_RX_Msk (0xfffffffful << SPI_RX_RX_Pos)
#define | SPI_TX_TX_Pos (0)
#define | SPI_TX_TX_Msk (0xfffffffful << SPI_TX_TX_Pos)
#define | SPI_CNTRL2_NOSLVSEL_Pos (8)
#define | SPI_CNTRL2_NOSLVSEL_Msk (0x1ul << SPI_CNTRL2_NOSLVSEL_Pos)
#define | SPI_CNTRL2_SLV_ABORT_Pos (9)
#define | SPI_CNTRL2_SLV_ABORT_Msk (0x1ul << SPI_CNTRL2_SLV_ABORT_Pos)
#define | SPI_CNTRL2_SSTA_INTEN_Pos (10)
#define | SPI_CNTRL2_SSTA_INTEN_Msk (0x1ul << SPI_CNTRL2_SSTA_INTEN_Pos)
#define | SPI_CNTRL2_SLV_START_INTSTS_Pos (11)
#define | SPI_CNTRL2_SLV_START_INTSTS_Msk (0x1ul << SPI_CNTRL2_SLV_START_INTSTS_Pos)
#define | SPI_CNTRL2_SS_INT_OPT_Pos (16)
#define | SPI_CNTRL2_SS_INT_OPT_Msk (0x1ul << SPI_CNTRL2_SS_INT_OPT_Pos)
#define | SPI_CNTRL2_BCn_Pos (31)
#define | SPI_CNTRL2_BCn_Msk (0x1ul << SPI_CNTRL2_BCn_Pos)
#define | SPI_FIFO_CTL_RX_CLR_Pos (0)
#define | SPI_FIFO_CTL_RX_CLR_Msk (0x1ul << SPI_FIFO_CTL_RX_CLR_Pos)
#define | SPI_FIFO_CTL_TX_CLR_Pos (1)
#define | SPI_FIFO_CTL_TX_CLR_Msk (0x1ul << SPI_FIFO_CTL_TX_CLR_Pos)
#define | SPI_FIFO_CTL_RX_INTEN_Pos (2)
#define | SPI_FIFO_CTL_RX_INTEN_Msk (0x1ul << SPI_FIFO_CTL_RX_INTEN_Pos)
#define | SPI_FIFO_CTL_TX_INTEN_Pos (3)
#define | SPI_FIFO_CTL_TX_INTEN_Msk (0x1ul << SPI_FIFO_CTL_TX_INTEN_Pos)
#define | SPI_FIFO_CTL_RXOV_INTEN_Pos (6)
#define | SPI_FIFO_CTL_RXOV_INTEN_Msk (0x1ul << SPI_FIFO_CTL_RXOV_INTEN_Pos)
#define | SPI_FIFO_CTL_TIMEOUT_INTEN_Pos (21)
#define | SPI_FIFO_CTL_TIMEOUT_INTEN_Msk (0x1ul << SPI_FIFO_CTL_TIMEOUT_INTEN_Pos)
#define | SPI_FIFO_CTL_RX_THRESHOLD_Pos (24)
#define | SPI_FIFO_CTL_RX_THRESHOLD_Msk (0x3ul << SPI_FIFO_CTL_RX_THRESHOLD_Pos)
#define | SPI_FIFO_CTL_TX_THRESHOLD_Pos (28)
#define | SPI_FIFO_CTL_TX_THRESHOLD_Msk (0x3ul << SPI_FIFO_CTL_TX_THRESHOLD_Pos)
#define | SPI_STATUS_RX_INTSTS_Pos (0)
#define | SPI_STATUS_RX_INTSTS_Msk (0x1ul << SPI_STATUS_RX_INTSTS_Pos)
#define | SPI_STATUS_RX_OVERRUN_Pos (2)
#define | SPI_STATUS_RX_OVERRUN_Msk (0x1ul << SPI_STATUS_RX_OVERRUN_Pos)
#define | SPI_STATUS_TX_INTSTS_Pos (4)
#define | SPI_STATUS_TX_INTSTS_Msk (0x1ul << SPI_STATUS_TX_INTSTS_Pos)
#define | SPI_STATUS_SLV_START_INTSTS_Pos (11)
#define | SPI_STATUS_SLV_START_INTSTS_Msk (0x1ul << SPI_STATUS_SLV_START_INTSTS_Pos)
#define | SPI_STATUS_RX_FIFO_COUNT_Pos (12)
#define | SPI_STATUS_RX_FIFO_COUNT_Msk (0xful << SPI_STATUS_RX_FIFO_COUNT_Pos)
#define | SPI_STATUS_IF_Pos (16)
#define | SPI_STATUS_IF_Msk (0x1ul << SPI_STATUS_IF_Pos)
#define | SPI_STATUS_TIMEOUT_Pos (20)
#define | SPI_STATUS_TIMEOUT_Msk (0x1ul << SPI_STATUS_TIMEOUT_Pos)
#define | SPI_STATUS_RX_EMPTY_Pos (24)
#define | SPI_STATUS_RX_EMPTY_Msk (0x1ul << SPI_STATUS_RX_EMPTY_Pos)
#define | SPI_STATUS_RX_FULL_Pos (25)
#define | SPI_STATUS_RX_FULL_Msk (0x1ul << SPI_STATUS_RX_FULL_Pos)
#define | SPI_STATUS_TX_EMPTY_Pos (26)
#define | SPI_STATUS_TX_EMPTY_Msk (0x1ul << SPI_STATUS_TX_EMPTY_Pos)
#define | SPI_STATUS_TX_FULL_Pos (27)
#define | SPI_STATUS_TX_FULL_Msk (0x1ul << SPI_STATUS_TX_FULL_Pos)
#define | SPI_STATUS_TX_FIFO_COUNT_Pos (28)
#define | SPI_STATUS_TX_FIFO_COUNT_Msk (0xful << SPI_STATUS_TX_FIFO_COUNT_Pos)
#define | TIMER_TCSR_PRESCALE_Pos (0)
#define | TIMER_TCSR_PRESCALE_Msk (0xfful << TIMER_TCSR_PRESCALE_Pos)
#define | TIMER_TCSR_TDR_EN_Pos (16)
#define | TIMER_TCSR_TDR_EN_Msk (0x1ul << TIMER_TCSR_TDR_EN_Pos)
#define | TIMER_TCSR_PERIODIC_SEL_Pos (17)
#define | TIMER_TCSR_PERIODIC_SEL_Msk (0x1ul << TIMER_TCSR_PERIODIC_SEL_Pos)
#define | TIMER_TCSR_TOGGLE_PIN_Pos (18)
#define | TIMER_TCSR_TOGGLE_PIN_Msk (0x1ul << TIMER_TCSR_TOGGLE_PIN_Pos)
#define | TIMER_TCSR_TOUT_PIN_Pos (18)
#define | TIMER_TCSR_TOUT_PIN_Msk (0x1ul << TIMER_TCSR_TOUT_PIN_Pos)
#define | TIMER_TCSR_CAP_SRC_Pos (19)
#define | TIMER_TCSR_CAP_SRC_Msk (0x1ul << TIMER_TCSR_CAP_SRC_Pos)
#define | TIMER_TCSR_WAKE_EN_Pos (23)
#define | TIMER_TCSR_WAKE_EN_Msk (0x1ul << TIMER_TCSR_WAKE_EN_Pos)
#define | TIMER_TCSR_CTB_Pos (24)
#define | TIMER_TCSR_CTB_Msk (0x1ul << TIMER_TCSR_CTB_Pos)
#define | TIMER_TCSR_CACT_Pos (25)
#define | TIMER_TCSR_CACT_Msk (0x1ul << TIMER_TCSR_CACT_Pos)
#define | TIMER_TCSR_CRST_Pos (26)
#define | TIMER_TCSR_CRST_Msk (0x1ul << TIMER_TCSR_CRST_Pos)
#define | TIMER_TCSR_MODE_Pos (27)
#define | TIMER_TCSR_MODE_Msk (0x3ul << TIMER_TCSR_MODE_Pos)
#define | TIMER_TCSR_IE_Pos (29)
#define | TIMER_TCSR_IE_Msk (0x1ul << TIMER_TCSR_IE_Pos)
#define | TIMER_TCSR_CEN_Pos (30)
#define | TIMER_TCSR_CEN_Msk (0x1ul << TIMER_TCSR_CEN_Pos)
#define | TIMER_TCSR_DBGACK_TMR_Pos (31)
#define | TIMER_TCSR_DBGACK_TMR_Msk (0x1ul << TIMER_TCSR_DBGACK_TMR_Pos)
#define | TIMER_TCMP_TCMP_Pos (0)
#define | TIMER_TCMP_TCMP_Msk (0xfffffful << TIMER_TCMP_TCMP_Pos)
#define | TIMER_TISR_TIF_Pos (0)
#define | TIMER_TISR_TIF_Msk (0x1ul << TIMER_TISR_TIF_Pos)
#define | TIMER_TISR_TWF_Pos (1)
#define | TIMER_TISR_TWF_Msk (0x1ul << TIMER_TISR_TWF_Pos)
#define | TIMER_TDR_TDR_Pos (0)
#define | TIMER_TDR_TDR_Msk (0xfffffful << TIMER_TDR_TDR_Pos)
#define | TIMER_TCAP_TCAP_Pos (0)
#define | TIMER_TCAP_TCAP_Msk (0xfffffful << TIMER_TCAP_TCAP_Pos)
#define | TIMER_TEXCON_TX_PHASE_Pos (0)
#define | TIMER_TEXCON_TX_PHASE_Msk (0x1ul << TIMER_TEXCON_TX_PHASE_Pos)
#define | TIMER_TEXCON_TEX_EDGE_Pos (1)
#define | TIMER_TEXCON_TEX_EDGE_Msk (0x3ul << TIMER_TEXCON_TEX_EDGE_Pos)
#define | TIMER_TEXCON_TEXEN_Pos (3)
#define | TIMER_TEXCON_TEXEN_Msk (0x1ul << TIMER_TEXCON_TEXEN_Pos)
#define | TIMER_TEXCON_RSTCAPSEL_Pos (4)
#define | TIMER_TEXCON_RSTCAPSEL_Msk (0x1ul << TIMER_TEXCON_RSTCAPSEL_Pos)
#define | TIMER_TEXCON_TEXIEN_Pos (5)
#define | TIMER_TEXCON_TEXIEN_Msk (0x1ul << TIMER_TEXCON_TEXIEN_Pos)
#define | TIMER_TEXCON_TEXDB_Pos (6)
#define | TIMER_TEXCON_TEXDB_Msk (0x1ul << TIMER_TEXCON_TEXDB_Pos)
#define | TIMER_TEXCON_TCDB_Pos (7)
#define | TIMER_TEXCON_TCDB_Msk (0x1ul << TIMER_TEXCON_TCDB_Pos)
#define | TIMER_TEXCON_CAP_MODE_Pos (8)
#define | TIMER_TEXCON_CAP_MODE_Msk (0x1ul << TIMER_TEXCON_CAP_MODE_Pos)
#define | TIMER_TEXISR_TEXIF_Pos (0)
#define | TIMER_TEXISR_TEXIF_Msk (0x1ul << TIMER_TEXISR_TEXIF_Pos)
#define | UART_RBR_RBR_Pos (0)
#define | UART_RBR_RBR_Msk (0xfful << UART_RBR_RBR_Pos)
#define | UART_THR_THR_Pos (0)
#define | UART_THR_THR_Msk (0xfful << UART_THR_THR_Pos)
#define | UART_IER_RDA_IEN_Pos (0)
#define | UART_IER_RDA_IEN_Msk (0x1ul << UART_IER_RDA_IEN_Pos)
#define | UART_IER_THRE_IEN_Pos (1)
#define | UART_IER_THRE_IEN_Msk (0x1ul << UART_IER_THRE_IEN_Pos)
#define | UART_IER_RLS_IEN_Pos (2)
#define | UART_IER_RLS_IEN_Msk (0x1ul << UART_IER_RLS_IEN_Pos)
#define | UART_IER_MODEM_IEN_Pos (3)
#define | UART_IER_MODEM_IEN_Msk (0x1ul << UART_IER_MODEM_IEN_Pos)
#define | UART_IER_RTO_IEN_Pos (4)
#define | UART_IER_RTO_IEN_Msk (0x1ul << UART_IER_RTO_IEN_Pos)
#define | UART_IER_BUF_ERR_IEN_Pos (5)
#define | UART_IER_BUF_ERR_IEN_Msk (0x1ul << UART_IER_BUF_ERR_IEN_Pos)
#define | UART_IER_WAKE_EN_Pos (6)
#define | UART_IER_WAKE_EN_Msk (0x1ul << UART_IER_WAKE_EN_Pos)
#define | UART_IER_TIME_OUT_EN_Pos (11)
#define | UART_IER_TIME_OUT_EN_Msk (0x1ul << UART_IER_TIME_OUT_EN_Pos)
#define | UART_IER_AUTO_RTS_EN_Pos (12)
#define | UART_IER_AUTO_RTS_EN_Msk (0x1ul << UART_IER_AUTO_RTS_EN_Pos)
#define | UART_IER_AUTO_CTS_EN_Pos (13)
#define | UART_IER_AUTO_CTS_EN_Msk (0x1ul << UART_IER_AUTO_CTS_EN_Pos)
#define | UART_FCR_RFR_Pos (1)
#define | UART_FCR_RFR_Msk (0x1ul << UART_FCR_RFR_Pos)
#define | UART_FCR_TFR_Pos (2)
#define | UART_FCR_TFR_Msk (0x1ul << UART_FCR_TFR_Pos)
#define | UART_FCR_RFITL_Pos (4)
#define | UART_FCR_RFITL_Msk (0xful << UART_FCR_RFITL_Pos)
#define | UART_FCR_RX_DIS_Pos (8)
#define | UART_FCR_RX_DIS_Msk (0x1ul << UART_FCR_RX_DIS_Pos)
#define | UART_FCR_RTS_TRI_LEV_Pos (16)
#define | UART_FCR_RTS_TRI_LEV_Msk (0xful << UART_FCR_RTS_TRI_LEV_Pos)
#define | UART_LCR_WLS_Pos (0)
#define | UART_LCR_WLS_Msk (0x3ul << UART_LCR_WLS_Pos)
#define | UART_LCR_NSB_Pos (2)
#define | UART_LCR_NSB_Msk (0x1ul << UART_LCR_NSB_Pos)
#define | UART_LCR_PBE_Pos (3)
#define | UART_LCR_PBE_Msk (0x1ul << UART_LCR_PBE_Pos)
#define | UART_LCR_EPE_Pos (4)
#define | UART_LCR_EPE_Msk (0x1ul << UART_LCR_EPE_Pos)
#define | UART_LCR_SPE_Pos (5)
#define | UART_LCR_SPE_Msk (0x1ul << UART_LCR_SPE_Pos)
#define | UART_LCR_BCB_Pos (6)
#define | UART_LCR_BCB_Msk (0x1ul << UART_LCR_BCB_Pos)
#define | UART_MCR_RTS_Pos (1)
#define | UART_MCR_RTS_Msk (0x1ul << UART_MCR_RTS_Pos)
#define | UART_MCR_LEV_RTS_Pos (9)
#define | UART_MCR_LEV_RTS_Msk (0x1ul << UART_MCR_LEV_RTS_Pos)
#define | UART_MCR_RTS_ST_Pos (13)
#define | UART_MCR_RTS_ST_Msk (0x1ul << UART_MCR_RTS_ST_Pos)
#define | UART_MSR_DCTSF_Pos (0)
#define | UART_MSR_DCTSF_Msk (0x1ul << UART_MSR_DCTSF_Pos)
#define | UART_MSR_CTS_ST_Pos (4)
#define | UART_MSR_CTS_ST_Msk (0x1ul << UART_MSR_CTS_ST_Pos)
#define | UART_MSR_LEV_CTS_Pos (8)
#define | UART_MSR_LEV_CTS_Msk (0x1ul << UART_MSR_LEV_CTS_Pos)
#define | UART_FSR_RX_OVER_IF_Pos (0)
#define | UART_FSR_RX_OVER_IF_Msk (0x1ul << UART_FSR_RX_OVER_IF_Pos)
#define | UART_FSR_RS485_ADD_DETF_Pos (3)
#define | UART_FSR_RS485_ADD_DETF_Msk (0x1ul << UART_FSR_RS485_ADD_DETF_Pos)
#define | UART_FSR_PEF_Pos (4)
#define | UART_FSR_PEF_Msk (0x1ul << UART_FSR_PEF_Pos)
#define | UART_FSR_FEF_Pos (5)
#define | UART_FSR_FEF_Msk (0x1ul << UART_FSR_FEF_Pos)
#define | UART_FSR_BIF_Pos (6)
#define | UART_FSR_BIF_Msk (0x1ul << UART_FSR_BIF_Pos)
#define | UART_FSR_RX_POINTER_Pos (8)
#define | UART_FSR_RX_POINTER_Msk (0x3ful << UART_FSR_RX_POINTER_Pos)
#define | UART_FSR_RX_EMPTY_Pos (14)
#define | UART_FSR_RX_EMPTY_Msk (0x1ul << UART_FSR_RX_EMPTY_Pos)
#define | UART_FSR_RX_FULL_Pos (15)
#define | UART_FSR_RX_FULL_Msk (0x1ul << UART_FSR_RX_FULL_Pos)
#define | UART_FSR_TX_POINTER_Pos (16)
#define | UART_FSR_TX_POINTER_Msk (0x3ful << UART_FSR_TX_POINTER_Pos)
#define | UART_FSR_TX_EMPTY_Pos (22)
#define | UART_FSR_TX_EMPTY_Msk (0x1ul << UART_FSR_TX_EMPTY_Pos)
#define | UART_FSR_TX_FULL_Pos (23)
#define | UART_FSR_TX_FULL_Msk (0x1ul << UART_FSR_TX_FULL_Pos)
#define | UART_FSR_TX_OVER_IF_Pos (24)
#define | UART_FSR_TX_OVER_IF_Msk (0x1ul << UART_FSR_TX_OVER_IF_Pos)
#define | UART_FSR_TE_FLAG_Pos (28)
#define | UART_FSR_TE_FLAG_Msk (0x1ul << UART_FSR_TE_FLAG_Pos)
#define | UART_ISR_RDA_IF_Pos (0)
#define | UART_ISR_RDA_IF_Msk (0x1ul << UART_ISR_RDA_IF_Pos)
#define | UART_ISR_THRE_IF_Pos (1)
#define | UART_ISR_THRE_IF_Msk (0x1ul << UART_ISR_THRE_IF_Pos)
#define | UART_ISR_RLS_IF_Pos (2)
#define | UART_ISR_RLS_IF_Msk (0x1ul << UART_ISR_RLS_IF_Pos)
#define | UART_ISR_MODEM_IF_Pos (3)
#define | UART_ISR_MODEM_IF_Msk (0x1ul << UART_ISR_MODEM_IF_Pos)
#define | UART_ISR_TOUT_IF_Pos (4)
#define | UART_ISR_TOUT_IF_Msk (0x1ul << UART_ISR_TOUT_IF_Pos)
#define | UART_ISR_BUF_ERR_IF_Pos (5)
#define | UART_ISR_BUF_ERR_IF_Msk (0x1ul << UART_ISR_BUF_ERR_IF_Pos)
#define | UART_ISR_RDA_INT_Pos (8)
#define | UART_ISR_RDA_INT_Msk (0x1ul << UART_ISR_RDA_INT_Pos)
#define | UART_ISR_THRE_INT_Pos (9)
#define | UART_ISR_THRE_INT_Msk (0x1ul << UART_ISR_THRE_INT_Pos)
#define | UART_ISR_RLS_INT_Pos (10)
#define | UART_ISR_RLS_INT_Msk (0x1ul << UART_ISR_RLS_INT_Pos)
#define | UART_ISR_MODEM_INT_Pos (11)
#define | UART_ISR_MODEM_INT_Msk (0x1ul << UART_ISR_MODEM_INT_Pos)
#define | UART_ISR_TOUT_INT_Pos (12)
#define | UART_ISR_TOUT_INT_Msk (0x1ul << UART_ISR_TOUT_INT_Pos)
#define | UART_ISR_BUF_ERR_INT_Pos (13)
#define | UART_ISR_BUF_ERR_INT_Msk (0x1ul << UART_ISR_BUF_ERR_INT_Pos)
#define | UART_TOR_TOIC_Pos (0)
#define | UART_TOR_TOIC_Msk (0xfful << UART_TOR_TOIC_Pos)
#define | UART_TOR_DLY_Pos (8)
#define | UART_TOR_DLY_Msk (0xfful << UART_TOR_DLY_Pos)
#define | UART_BAUD_BRD_Pos (0)
#define | UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)
#define | UART_BAUD_DIVIDER_X_Pos (24)
#define | UART_BAUD_DIVIDER_X_Msk (0xful << UART_BAUD_DIVIDER_X_Pos)
#define | UART_BAUD_DIV_X_ONE_Pos (28)
#define | UART_BAUD_DIV_X_ONE_Msk (0x1ul << UART_BAUD_DIV_X_ONE_Pos)
#define | UART_BAUD_DIV_X_EN_Pos (29)
#define | UART_BAUD_DIV_X_EN_Msk (0x1ul << UART_BAUD_DIV_X_EN_Pos)
#define | UART_IRCR_TX_SELECT_Pos (1)
#define | UART_IRCR_TX_SELECT_Msk (0x1ul << UART_IRCR_TX_SELECT_Pos)
#define | UART_IRCR_INV_TX_Pos (5)
#define | UART_IRCR_INV_TX_Msk (0x1ul << UART_IRCR_INV_TX_Pos)
#define | UART_IRCR_INV_RX_Pos (6)
#define | UART_IRCR_INV_RX_Msk (0x1ul << UART_IRCR_INV_RX_Pos)
#define | UART_ALT_CSR_RS485_NMM_Pos (8)
#define | UART_ALT_CSR_RS485_NMM_Msk (0x1ul << UART_ALT_CSR_RS485_NMM_Pos)
#define | UART_ALT_CSR_RS485_AAD_Pos (9)
#define | UART_ALT_CSR_RS485_AAD_Msk (0x1ul << UART_ALT_CSR_RS485_AAD_Pos)
#define | UART_ALT_CSR_RS485_AUD_Pos (10)
#define | UART_ALT_CSR_RS485_AUD_Msk (0x1ul << UART_ALT_CSR_RS485_AUD_Pos)
#define | UART_ALT_CSR_RS485_ADD_EN_Pos (15)
#define | UART_ALT_CSR_RS485_ADD_EN_Msk (0x1ul << UART_ALT_CSR_RS485_ADD_EN_Pos)
#define | UART_ALT_CSR_ADDR_MATCH_Pos (24)
#define | UART_ALT_CSR_ADDR_MATCH_Msk (0xfful << UART_ALT_CSR_ADDR_MATCH_Pos)
#define | UART_FUN_SEL_FUN_SEL_Pos (0)
#define | UART_FUN_SEL_FUN_SEL_Msk (0x3ul << UART_FUN_SEL_FUN_SEL_Pos)
#define | WDT_WTCR_WTR_Pos (0)
#define | WDT_WTCR_WTR_Msk (0x1ul << WDT_WTCR_WTR_Pos)
#define | WDT_WTCR_WTRE_Pos (1)
#define | WDT_WTCR_WTRE_Msk (0x1ul << WDT_WTCR_WTRE_Pos)
#define | WDT_WTCR_WTRF_Pos (2)
#define | WDT_WTCR_WTRF_Msk (0x1ul << WDT_WTCR_WTRF_Pos)
#define | WDT_WTCR_WTIF_Pos (3)
#define | WDT_WTCR_WTIF_Msk (0x1ul << WDT_WTCR_WTIF_Pos)
#define | WDT_WTCR_WTWKE_Pos (4)
#define | WDT_WTCR_WTWKE_Msk (0x1ul << WDT_WTCR_WTWKE_Pos)
#define | WDT_WTCR_WTWKF_Pos (5)
#define | WDT_WTCR_WTWKF_Msk (0x1ul << WDT_WTCR_WTWKF_Pos)
#define | WDT_WTCR_WTIE_Pos (6)
#define | WDT_WTCR_WTIE_Msk (0x1ul << WDT_WTCR_WTIE_Pos)
#define | WDT_WTCR_WTE_Pos (7)
#define | WDT_WTCR_WTE_Msk (0x1ul << WDT_WTCR_WTE_Pos)
#define | WDT_WTCR_WTIS_Pos (8)
#define | WDT_WTCR_WTIS_Msk (0x7ul << WDT_WTCR_WTIS_Pos)
#define | WDT_WTCR_DBGACK_WDT_Pos (31)
#define | WDT_WTCR_DBGACK_WDT_Msk (0x1ul << WDT_WTCR_DBGACK_WDT_Pos)

## Typedefs
typedef enum IRQn | IRQn_Type
typedef volatile unsigned char | vu8
| Define 8-bit unsigned volatile data type. More...
typedef volatile unsigned short | vu16
| Define 16-bit unsigned volatile data type. More...
typedef volatile unsigned long | vu32
| Define 32-bit unsigned volatile data type. More...

## Enumerations
enum | IRQn { NonMaskableInt_IRQn = -14, HardFault_IRQn = -13, SVCall_IRQn = -5, PendSV_IRQn = -2, SysTick_IRQn = -1, BOD_IRQn = 0, WDT_IRQn = 1, EINT0_IRQn = 2, EINT1_IRQn = 3, GPIO01_IRQn = 4, GPIO234_IRQn = 5, PWM_IRQn = 6, FB_IRQn = 7, TMR0_IRQn = 8, TMR1_IRQn = 9, UART_IRQn = 12, SPI_IRQn = 14, GPIO5_IRQn = 16, HIRC_IRQn = 17, I2C_IRQn = 18, ACMP_IRQn = 25, PDWU_IRQn = 28, ADC_IRQn = 29 }

## Detailed Description

Mini51 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Mini51 series MCU.

Version
  V1.00

Revision
  43

Date
  16/06/08 1:55p

Note
  Copyright (C) 2018 Nuvoton Technology Corp. All rights reserved.

Definition in file Mini51Series.h.

## Macro Definition Documentation

## ◆ CLK_AHBCLK_ISP_EN_Msk

#define CLK_AHBCLK_ISP_EN_Msk (0x1ul << CLK_AHBCLK_ISP_EN_Pos)

CLK_T::AHBCLK: ISP_EN Mask

Definition at line 1517 of file Mini51Series.h.

## ◆ CLK_AHBCLK_ISP_EN_Pos

#define CLK_AHBCLK_ISP_EN_Pos (2)

CLK_T::AHBCLK: ISP_EN Position

Definition at line 1516 of file Mini51Series.h.

## ◆ CLK_APBCLK_ADC_EN_Msk

#define CLK_APBCLK_ADC_EN_Msk (0x1ul << CLK_APBCLK_ADC_EN_Pos)

CLK_T::APBCLK: ADC_EN Mask

Definition at line 1550 of file Mini51Series.h.

## ◆ CLK_APBCLK_ADC_EN_Pos

#define CLK_APBCLK_ADC_EN_Pos (28)

CLK_T::APBCLK: ADC_EN Position

Definition at line 1549 of file Mini51Series.h.

## ◆ CLK_APBCLK_CMP_EN_Msk

#define CLK_APBCLK_CMP_EN_Msk (0x1ul << CLK_APBCLK_CMP_EN_Pos)

CLK_T::APBCLK: ACMP_EN Mask

Definition at line 1553 of file Mini51Series.h.

## ◆ CLK_APBCLK_CMP_EN_Pos

#define CLK_APBCLK_CMP_EN_Pos (30)

CLK_T::APBCLK: ACMP_EN Position

Definition at line 1552 of file Mini51Series.h.

## ◆ CLK_APBCLK_FDIV_EN_Msk

#define CLK_APBCLK_FDIV_EN_Msk (0x1ul << CLK_APBCLK_FDIV_EN_Pos)

CLK_T::APBCLK: FDIV_EN Mask

Definition at line 1529 of file Mini51Series.h.

## ◆ CLK_APBCLK_FDIV_EN_Pos

#define CLK_APBCLK_FDIV_EN_Pos (6)

CLK_T::APBCLK: FDIV_EN Position

Definition at line 1528 of file Mini51Series.h.

## ◆ CLK_APBCLK_I2C_EN_Msk

#define CLK_APBCLK_I2C_EN_Msk (0x1ul << CLK_APBCLK_I2C_EN_Pos)

CLK_T::APBCLK: I2C_EN Mask

Definition at line 1532 of file Mini51Series.h.

## ◆ CLK_APBCLK_I2C_EN_Pos

#define CLK_APBCLK_I2C_EN_Pos (8)

CLK_T::APBCLK: I2C_EN Position

Definition at line 1531 of file Mini51Series.h.

## ◆ CLK_APBCLK_PWM01_EN_Msk

#define CLK_APBCLK_PWM01_EN_Msk (0x1ul << CLK_APBCLK_PWM01_EN_Pos)

CLK_T::APBCLK: PWM01_EN Mask

Definition at line 1541 of file Mini51Series.h.

## ◆ CLK_APBCLK_PWM01_EN_Pos

#define CLK_APBCLK_PWM01_EN_Pos (20)

CLK_T::APBCLK: PWM01_EN Position

Definition at line 1540 of file Mini51Series.h.

## ◆ CLK_APBCLK_PWM23_EN_Msk

#define CLK_APBCLK_PWM23_EN_Msk (0x1ul << CLK_APBCLK_PWM23_EN_Pos)

CLK_T::APBCLK: PWM23_EN Mask

Definition at line 1544 of file Mini51Series.h.

## ◆ CLK_APBCLK_PWM23_EN_Pos

#define CLK_APBCLK_PWM23_EN_Pos (21)

CLK_T::APBCLK: PWM23_EN Position

Definition at line 1543 of file Mini51Series.h.

## ◆ CLK_APBCLK_PWM45_EN_Msk

#define CLK_APBCLK_PWM45_EN_Msk (0x1ul << CLK_APBCLK_PWM45_EN_Pos)

CLK_T::APBCLK: PWM45_EN Mask

Definition at line 1547 of file Mini51Series.h.

## ◆ CLK_APBCLK_PWM45_EN_Pos

#define CLK_APBCLK_PWM45_EN_Pos (22)

CLK_T::APBCLK: PWM45_EN Position

Definition at line 1546 of file Mini51Series.h.

## ◆ CLK_APBCLK_SPI_EN_Msk

#define CLK_APBCLK_SPI_EN_Msk (0x1ul << CLK_APBCLK_SPI_EN_Pos)

CLK_T::APBCLK: SPI_EN Mask

Definition at line 1535 of file Mini51Series.h.

## ◆ CLK_APBCLK_SPI_EN_Pos

#define CLK_APBCLK_SPI_EN_Pos (12)

CLK_T::APBCLK: SPI_EN Position

Definition at line 1534 of file Mini51Series.h.

## ◆ CLK_APBCLK_TMR0_EN_Msk

#define CLK_APBCLK_TMR0_EN_Msk (0x1ul << CLK_APBCLK_TMR0_EN_Pos)

CLK_T::APBCLK: TMR0_EN Mask

Definition at line 1523 of file Mini51Series.h.

## ◆ CLK_APBCLK_TMR0_EN_Pos

#define CLK_APBCLK_TMR0_EN_Pos (2)

CLK_T::APBCLK: TMR0_EN Position

Definition at line 1522 of file Mini51Series.h.

## ◆ CLK_APBCLK_TMR1_EN_Msk

#define CLK_APBCLK_TMR1_EN_Msk (0x1ul << CLK_APBCLK_TMR1_EN_Pos)

CLK_T::APBCLK: TMR1_EN Mask

Definition at line 1526 of file Mini51Series.h.

## ◆ CLK_APBCLK_TMR1_EN_Pos

#define CLK_APBCLK_TMR1_EN_Pos (3)

CLK_T::APBCLK: TMR1_EN Position

Definition at line 1525 of file Mini51Series.h.

## ◆ CLK_APBCLK_UART_EN_Msk

#define CLK_APBCLK_UART_EN_Msk (0x1ul << CLK_APBCLK_UART_EN_Pos)

CLK_T::APBCLK: UART_EN Mask

Definition at line 1538 of file Mini51Series.h.

## ◆ CLK_APBCLK_UART_EN_Pos

#define CLK_APBCLK_UART_EN_Pos (16)

CLK_T::APBCLK: UART_EN Position

Definition at line 1537 of file Mini51Series.h.

## ◆ CLK_APBCLK_WDT_EN_Msk

#define CLK_APBCLK_WDT_EN_Msk (0x1ul << CLK_APBCLK_WDT_EN_Pos)

CLK_T::APBCLK: WDT_EN Mask

Definition at line 1520 of file Mini51Series.h.

## ◆ CLK_APBCLK_WDT_EN_Pos

#define CLK_APBCLK_WDT_EN_Pos (0)

CLK_T::APBCLK: WDT_EN Position

Definition at line 1519 of file Mini51Series.h.

## ◆ CLK_CLKDIV_ADC_N_Msk

#define CLK_CLKDIV_ADC_N_Msk (0xfful << CLK_CLKDIV_ADC_N_Pos)

CLK_T::CLKDIV: ADC_N Mask

Definition at line 1610 of file Mini51Series.h.

## ◆ CLK_CLKDIV_ADC_N_Pos

#define CLK_CLKDIV_ADC_N_Pos (16)

CLK_T::CLKDIV: ADC_N Position

Definition at line 1609 of file Mini51Series.h.

## ◆ CLK_CLKDIV_HCLK_N_Msk

#define CLK_CLKDIV_HCLK_N_Msk (0xful << CLK_CLKDIV_HCLK_N_Pos)

CLK_T::CLKDIV: HCLK_N Mask

Definition at line 1604 of file Mini51Series.h.

## ◆ CLK_CLKDIV_HCLK_N_Pos

#define CLK_CLKDIV_HCLK_N_Pos (0)

CLK_T::CLKDIV: HCLK_N Position

Definition at line 1603 of file Mini51Series.h.

## ◆ CLK_CLKDIV_UART_N_Msk

#define CLK_CLKDIV_UART_N_Msk (0xful << CLK_CLKDIV_UART_N_Pos)

CLK_T::CLKDIV: UART_N Mask

Definition at line 1607 of file Mini51Series.h.

## ◆ CLK_CLKDIV_UART_N_Pos

#define CLK_CLKDIV_UART_N_Pos (8)

CLK_T::CLKDIV: UART_N Position

Definition at line 1606 of file Mini51Series.h.

## ◆ CLK_CLKSEL0_HCLK_S_Msk

#define CLK_CLKSEL0_HCLK_S_Msk (0x7ul << CLK_CLKSEL0_HCLK_S_Pos)

CLK_T::CLKSEL0: HCLK_S Mask

Definition at line 1580 of file Mini51Series.h.

## ◆ CLK_CLKSEL0_HCLK_S_Pos

#define CLK_CLKSEL0_HCLK_S_Pos (0)

CLK_T::CLKSEL0: HCLK_S Position

Definition at line 1579 of file Mini51Series.h.

## ◆ CLK_CLKSEL0_STCLK_S_Msk

#define CLK_CLKSEL0_STCLK_S_Msk (0x7ul << CLK_CLKSEL0_STCLK_S_Pos)

CLK_T::CLKSEL0: STCLK_S Mask

Definition at line 1583 of file Mini51Series.h.

## ◆ CLK_CLKSEL0_STCLK_S_Pos

#define CLK_CLKSEL0_STCLK_S_Pos (3)

CLK_T::CLKSEL0: STCLK_S Position

Definition at line 1582 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_ADC_S_Msk

#define CLK_CLKSEL1_ADC_S_Msk (0x3ul << CLK_CLKSEL1_ADC_S_Pos)

CLK_T::CLKSEL1: ADC_S Mask

Definition at line 1589 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_ADC_S_Pos

#define CLK_CLKSEL1_ADC_S_Pos (2)

CLK_T::CLKSEL1: ADC_S Position

Definition at line 1588 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_SPI_S_Msk

#define CLK_CLKSEL1_SPI_S_Msk (0x1ul << CLK_CLKSEL1_SPI_S_Pos)

CLK_T::CLKSEL1: SPI_S Mask

Definition at line 1592 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_SPI_S_Pos

#define CLK_CLKSEL1_SPI_S_Pos (4)

CLK_T::CLKSEL1: SPI_S Position

Definition at line 1591 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_TMR0_S_Msk

#define CLK_CLKSEL1_TMR0_S_Msk (0x7ul << CLK_CLKSEL1_TMR0_S_Pos)

CLK_T::CLKSEL1: TMR0_S Mask

Definition at line 1595 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_TMR0_S_Pos

#define CLK_CLKSEL1_TMR0_S_Pos (8)

CLK_T::CLKSEL1: TMR0_S Position

Definition at line 1594 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_TMR1_S_Msk

#define CLK_CLKSEL1_TMR1_S_Msk (0x7ul << CLK_CLKSEL1_TMR1_S_Pos)

CLK_T::CLKSEL1: TMR1_S Mask

Definition at line 1598 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_TMR1_S_Pos

#define CLK_CLKSEL1_TMR1_S_Pos (12)

CLK_T::CLKSEL1: TMR1_S Position

Definition at line 1597 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_UART_S_Msk

#define CLK_CLKSEL1_UART_S_Msk (0x3ul << CLK_CLKSEL1_UART_S_Pos)

CLK_T::CLKSEL1: UART_S Mask

Definition at line 1601 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_UART_S_Pos

#define CLK_CLKSEL1_UART_S_Pos (24)

CLK_T::CLKSEL1: UART_S Position

Definition at line 1600 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_WDT_S_Msk

#define CLK_CLKSEL1_WDT_S_Msk (0x3ul << CLK_CLKSEL1_WDT_S_Pos)

CLK_T::CLKSEL1: WDT_S Mask

Definition at line 1586 of file Mini51Series.h.

## ◆ CLK_CLKSEL1_WDT_S_Pos

#define CLK_CLKSEL1_WDT_S_Pos (0)

CLK_T::CLKSEL1: WDT_S Position

Definition at line 1585 of file Mini51Series.h.

## ◆ CLK_CLKSEL2_FRQDIV_S_Msk

#define CLK_CLKSEL2_FRQDIV_S_Msk (0x3ul << CLK_CLKSEL2_FRQDIV_S_Pos)

CLK_T::CLKSEL2: FRQDIV_S Mask

Definition at line 1613 of file Mini51Series.h.

## ◆ CLK_CLKSEL2_FRQDIV_S_Pos

#define CLK_CLKSEL2_FRQDIV_S_Pos (2)

CLK_T::CLKSEL2: FRQDIV_S Position

Definition at line 1612 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_CLK_SW_FAIL_Msk

#define CLK_CLKSTATUS_CLK_SW_FAIL_Msk (0x1ul << CLK_CLKSTATUS_CLK_SW_FAIL_Pos)

CLK_T::CLKSTATUS: CLK_SW_FAIL Mask

Definition at line 1577 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_CLK_SW_FAIL_Pos

#define CLK_CLKSTATUS_CLK_SW_FAIL_Pos (7)

CLK_T::CLKSTATUS: CLK_SW_FAIL Position

Definition at line 1576 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_HIRC_STB_Msk

#define CLK_CLKSTATUS_HIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_HIRC_STB_Pos)

CLK_T::CLKSTATUS: OSC22M_STB Mask

Definition at line 1574 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_HIRC_STB_Pos

#define CLK_CLKSTATUS_HIRC_STB_Pos (4)

CLK_T::CLKSTATUS: OSC22M_STB Position

Definition at line 1573 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_HXT_STB_Msk

#define CLK_CLKSTATUS_HXT_STB_Msk (0x1ul << CLK_CLKSTATUS_HXT_STB_Pos)

CLK_T::CLKSTATUS: XTL_STB Mask

Definition at line 1558 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_HXT_STB_Pos

#define CLK_CLKSTATUS_HXT_STB_Pos (0)

CLK_T::CLKSTATUS: XTL_STB Position

Definition at line 1557 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_IRC10K_STB_Msk

#define CLK_CLKSTATUS_IRC10K_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC10K_STB_Pos)

CLK_T::CLKSTATUS: OSC10K_STB Mask

Definition at line 1565 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_IRC10K_STB_Pos

#define CLK_CLKSTATUS_IRC10K_STB_Pos (3)

CLK_T::CLKSTATUS: OSC10K_STB Position

Definition at line 1564 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_IRC22M_STB_Msk

#define CLK_CLKSTATUS_IRC22M_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC22M_STB_Pos)

CLK_T::CLKSTATUS: OSC22M_STB Mask

Definition at line 1572 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_IRC22M_STB_Pos

#define CLK_CLKSTATUS_IRC22M_STB_Pos (4)

CLK_T::CLKSTATUS: OSC22M_STB Position

Definition at line 1571 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_LIRC_STB_Msk

#define CLK_CLKSTATUS_LIRC_STB_Msk (0x1ul << CLK_CLKSTATUS_LIRC_STB_Pos)

CLK_T::CLKSTATUS: OSC10K_STB Mask

Definition at line 1567 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_LIRC_STB_Pos

#define CLK_CLKSTATUS_LIRC_STB_Pos (3)

CLK_T::CLKSTATUS: OSC10K_STB Position

Definition at line 1566 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_LXT_STB_Msk

#define CLK_CLKSTATUS_LXT_STB_Msk (0x1ul << CLK_CLKSTATUS_LXT_STB_Pos)

CLK_T::CLKSTATUS: XTL_STB Mask

Definition at line 1560 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_LXT_STB_Pos

#define CLK_CLKSTATUS_LXT_STB_Pos (0)

CLK_T::CLKSTATUS: XTL_STB Position

Definition at line 1559 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_OSC10K_STB_Msk

#define CLK_CLKSTATUS_OSC10K_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC10K_STB_Pos)

CLK_T::CLKSTATUS: OSC10K_STB Mask

Definition at line 1563 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_OSC10K_STB_Pos

#define CLK_CLKSTATUS_OSC10K_STB_Pos (3)

CLK_T::CLKSTATUS: OSC10K_STB Position

Definition at line 1562 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_OSC22M_STB_Msk

#define CLK_CLKSTATUS_OSC22M_STB_Msk (0x1ul << CLK_CLKSTATUS_OSC22M_STB_Pos)

CLK_T::CLKSTATUS: OSC22M_STB Mask

Definition at line 1570 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_OSC22M_STB_Pos

#define CLK_CLKSTATUS_OSC22M_STB_Pos (4)

CLK_T::CLKSTATUS: OSC22M_STB Position

Definition at line 1569 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_XTL_STB_Msk

#define CLK_CLKSTATUS_XTL_STB_Msk (0x1ul << CLK_CLKSTATUS_XTL_STB_Pos)

CLK_T::CLKSTATUS: XTL_STB Mask

Definition at line 1556 of file Mini51Series.h.

## ◆ CLK_CLKSTATUS_XTL_STB_Pos

#define CLK_CLKSTATUS_XTL_STB_Pos (0)

CLK_T::CLKSTATUS: XTL_STB Position

Definition at line 1555 of file Mini51Series.h.

## ◆ CLK_FRQDIV_DIVIDER1_Msk

#define CLK_FRQDIV_DIVIDER1_Msk (0x1ul << CLK_FRQDIV_DIVIDER1_Pos)

CLK_T::FRQDIV: DIVIDER1 Mask

Definition at line 1622 of file Mini51Series.h.

## ◆ CLK_FRQDIV_DIVIDER1_Pos

#define CLK_FRQDIV_DIVIDER1_Pos (5)

CLK_T::FRQDIV: DIVIDER1 Position

Definition at line 1621 of file Mini51Series.h.

## ◆ CLK_FRQDIV_DIVIDER_EN_Msk

#define CLK_FRQDIV_DIVIDER_EN_Msk (0x1ul << CLK_FRQDIV_DIVIDER_EN_Pos)

CLK_T::FRQDIV: DIVIDER_EN Mask

Definition at line 1619 of file Mini51Series.h.

## ◆ CLK_FRQDIV_DIVIDER_EN_Pos

#define CLK_FRQDIV_DIVIDER_EN_Pos (4)

CLK_T::FRQDIV: DIVIDER_EN Position

Definition at line 1618 of file Mini51Series.h.

## ◆ CLK_FRQDIV_FSEL_Msk

#define CLK_FRQDIV_FSEL_Msk (0xful << CLK_FRQDIV_FSEL_Pos)

CLK_T::FRQDIV: FSEL Mask

Definition at line 1616 of file Mini51Series.h.

## ◆ CLK_FRQDIV_FSEL_Pos

#define CLK_FRQDIV_FSEL_Pos (0)

CLK_T::FRQDIV: FSEL Position

Definition at line 1615 of file Mini51Series.h.

## ◆ CLK_PWRCON_HIRC_EN_Msk

#define CLK_PWRCON_HIRC_EN_Msk (0x1ul << CLK_PWRCON_HIRC_EN_Pos)

CLK_T::PWRCON: OSC22M_EN Mask

Definition at line 1492 of file Mini51Series.h.

## ◆ CLK_PWRCON_HIRC_EN_Pos

#define CLK_PWRCON_HIRC_EN_Pos (2)

CLK_T::PWRCON: OSC22M_EN Position

Definition at line 1491 of file Mini51Series.h.

## ◆ CLK_PWRCON_IRC10K_EN_Msk

#define CLK_PWRCON_IRC10K_EN_Msk (0x1ul << CLK_PWRCON_IRC10K_EN_Pos)

CLK_T::PWRCON: OSC10K_EN Mask

Definition at line 1497 of file Mini51Series.h.

## ◆ CLK_PWRCON_IRC10K_EN_Pos

#define CLK_PWRCON_IRC10K_EN_Pos (3)

CLK_T::PWRCON: OSC10K_EN Position

Definition at line 1496 of file Mini51Series.h.

## ◆ CLK_PWRCON_IRC22M_EN_Msk

#define CLK_PWRCON_IRC22M_EN_Msk (0x1ul << CLK_PWRCON_IRC22M_EN_Pos)

CLK_T::PWRCON: OSC22M_EN Mask

Definition at line 1490 of file Mini51Series.h.

## ◆ CLK_PWRCON_IRC22M_EN_Pos

#define CLK_PWRCON_IRC22M_EN_Pos (2)

CLK_T::PWRCON: OSC22M_EN Position

Definition at line 1489 of file Mini51Series.h.

## ◆ CLK_PWRCON_LIRC_EN_Msk

#define CLK_PWRCON_LIRC_EN_Msk (0x1ul << CLK_PWRCON_LIRC_EN_Pos)

CLK_T::PWRCON: OSC10K_EN Mask

Definition at line 1499 of file Mini51Series.h.

## ◆ CLK_PWRCON_LIRC_EN_Pos

#define CLK_PWRCON_LIRC_EN_Pos (3)

CLK_T::PWRCON: OSC10K_EN Position

Definition at line 1498 of file Mini51Series.h.

## ◆ CLK_PWRCON_OSC10K_EN_Msk

#define CLK_PWRCON_OSC10K_EN_Msk (0x1ul << CLK_PWRCON_OSC10K_EN_Pos)

CLK_T::PWRCON: OSC10K_EN Mask

Definition at line 1495 of file Mini51Series.h.

## ◆ CLK_PWRCON_OSC10K_EN_Pos

#define CLK_PWRCON_OSC10K_EN_Pos (3)

CLK_T::PWRCON: OSC10K_EN Position

Definition at line 1494 of file Mini51Series.h.

## ◆ CLK_PWRCON_OSC22M_EN_Msk

#define CLK_PWRCON_OSC22M_EN_Msk (0x1ul << CLK_PWRCON_OSC22M_EN_Pos)

CLK_T::PWRCON: OSC22M_EN Mask

Definition at line 1488 of file Mini51Series.h.

## ◆ CLK_PWRCON_OSC22M_EN_Pos

#define CLK_PWRCON_OSC22M_EN_Pos (2)

CLK_T::PWRCON: OSC22M_EN Position

Definition at line 1487 of file Mini51Series.h.

## ◆ CLK_PWRCON_PD_32K_Msk

#define CLK_PWRCON_PD_32K_Msk (0x1ul << CLK_PWRCON_PD_32K_Pos)

CLK_T::PWRCON: PD_32K Mask

Definition at line 1514 of file Mini51Series.h.

## ◆ CLK_PWRCON_PD_32K_Pos

#define CLK_PWRCON_PD_32K_Pos (9)

CLK_T::PWRCON: PD_32K Position

Definition at line 1513 of file Mini51Series.h.

## ◆ CLK_PWRCON_PD_WU_STS_Msk

#define CLK_PWRCON_PD_WU_STS_Msk (0x1ul << CLK_PWRCON_PD_WU_STS_Pos)

CLK_T::PWRCON: PD_WU_STS Mask

Definition at line 1508 of file Mini51Series.h.

## ◆ CLK_PWRCON_PD_WU_STS_Pos

#define CLK_PWRCON_PD_WU_STS_Pos (6)

CLK_T::PWRCON: PD_WU_STS Position

Definition at line 1507 of file Mini51Series.h.

## ◆ CLK_PWRCON_PWR_DOWN_EN_Msk

#define CLK_PWRCON_PWR_DOWN_EN_Msk (0x1ul << CLK_PWRCON_PWR_DOWN_EN_Pos)

CLK_T::PWRCON: PWR_DOWN_EN Mask

Definition at line 1511 of file Mini51Series.h.

## ◆ CLK_PWRCON_PWR_DOWN_EN_Pos

#define CLK_PWRCON_PWR_DOWN_EN_Pos (7)

CLK_T::PWRCON: PWR_DOWN_EN Position

Definition at line 1510 of file Mini51Series.h.

## ◆ CLK_PWRCON_WINT_EN_Msk

#define CLK_PWRCON_WINT_EN_Msk (0x1ul << CLK_PWRCON_WINT_EN_Pos)

CLK_T::PWRCON: PD_WU_INT_EN Mask

Definition at line 1505 of file Mini51Series.h.

## ◆ CLK_PWRCON_WINT_EN_Pos

#define CLK_PWRCON_WINT_EN_Pos (5)

CLK_T::PWRCON: PD_WU_INT_EN Position

Definition at line 1504 of file Mini51Series.h.

## ◆ CLK_PWRCON_WU_DLY_Msk

#define CLK_PWRCON_WU_DLY_Msk (0x1ul << CLK_PWRCON_WU_DLY_Pos)

CLK_T::PWRCON: PD_WU_DLY Mask

Definition at line 1502 of file Mini51Series.h.

## ◆ CLK_PWRCON_WU_DLY_Pos

#define CLK_PWRCON_WU_DLY_Pos (4)

CLK_T::PWRCON: PD_WU_DLY Position

Definition at line 1501 of file Mini51Series.h.

## ◆ CLK_PWRCON_XTLCLK_EN_Msk

#define CLK_PWRCON_XTLCLK_EN_Msk (0x3ul << CLK_PWRCON_XTLCLK_EN_Pos)

CLK_T::PWRCON: XTLCLK_EN Mask

Definition at line 1485 of file Mini51Series.h.

## ◆ CLK_PWRCON_XTLCLK_EN_Pos

#define CLK_PWRCON_XTLCLK_EN_Pos (0)

    @addtogroup CLK_CONST CLK Bit Field Definition
    Constant Definitions for CLK Controller

CLK_T::PWRCON: XTLCLK_EN Position

Definition at line 1484 of file Mini51Series.h.

## ◆ FMC_DFBADR_DFBA_Msk

#define FMC_DFBADR_DFBA_Msk (0xfffffffful << FMC_DFBA_DFBA_Pos)

FMC_T::DFBADR: DFBA Mask

Definition at line 1929 of file Mini51Series.h.

## ◆ FMC_DFBADR_DFBA_Pos

#define FMC_DFBADR_DFBA_Pos (0)

FMC_T::DFBADR: DFBA Position

Definition at line 1928 of file Mini51Series.h.

## ◆ FMC_ISPADR_ISPADR_Msk

#define FMC_ISPADR_ISPADR_Msk (0xfffffffful << FMC_ISPADR_ISPADR_Pos)

FMC_T::ISPADR: ISPADR Mask

Definition at line 1917 of file Mini51Series.h.

## ◆ FMC_ISPADR_ISPADR_Pos

#define FMC_ISPADR_ISPADR_Pos (0)

FMC_T::ISPADR: ISPADR Position

Definition at line 1916 of file Mini51Series.h.

## ◆ FMC_ISPCMD_ISPCMD_Msk

#define FMC_ISPCMD_ISPCMD_Msk (0x3ful << FMC_ISPCMD_ISPCMD_Pos)

FMC_T::ISPCMD: ISPCMD Mask

Definition at line 1923 of file Mini51Series.h.

## ◆ FMC_ISPCMD_ISPCMD_Pos

#define FMC_ISPCMD_ISPCMD_Pos (0)

FMC_T::ISPCMD: ISPCMD Position

Definition at line 1922 of file Mini51Series.h.

## ◆ FMC_ISPCON_APUEN_Msk

#define FMC_ISPCON_APUEN_Msk (0x1ul << FMC_ISPCON_APUEN_Pos)

FMC_T::ISPCON: APUEN Mask

Definition at line 1905 of file Mini51Series.h.

## ◆ FMC_ISPCON_APUEN_Pos

#define FMC_ISPCON_APUEN_Pos (3)

FMC_T::ISPCON: APUEN Position

Definition at line 1904 of file Mini51Series.h.

## ◆ FMC_ISPCON_BS_Msk

#define FMC_ISPCON_BS_Msk (0x1ul << FMC_ISPCON_BS_Pos)

FMC_T::ISPCON: BS Mask

Definition at line 1902 of file Mini51Series.h.

## ◆ FMC_ISPCON_BS_Pos

#define FMC_ISPCON_BS_Pos (1)

FMC_T::ISPCON: BS Position

Definition at line 1901 of file Mini51Series.h.

## ◆ FMC_ISPCON_CFGUEN_Msk

#define FMC_ISPCON_CFGUEN_Msk (0x1ul << FMC_ISPCON_CFGUEN_Pos)

FMC_T::ISPCON: CFGUEN Mask

Definition at line 1908 of file Mini51Series.h.

## ◆ FMC_ISPCON_CFGUEN_Pos

#define FMC_ISPCON_CFGUEN_Pos (4)

FMC_T::ISPCON: CFGUEN Position

Definition at line 1907 of file Mini51Series.h.

## ◆ FMC_ISPCON_ISPEN_Msk

#define FMC_ISPCON_ISPEN_Msk (0x1ul << FMC_ISPCON_ISPEN_Pos)

FMC_T::ISPCON: ISPEN Mask

Definition at line 1899 of file Mini51Series.h.

## ◆ FMC_ISPCON_ISPEN_Pos

#define FMC_ISPCON_ISPEN_Pos (0)

    @addtogroup FMC_CONST FMC Bit Field Definition
    Constant Definitions for FMC Controller

FMC_T::ISPCON: ISPEN Position

Definition at line 1898 of file Mini51Series.h.

## ◆ FMC_ISPCON_ISPFF_Msk

#define FMC_ISPCON_ISPFF_Msk (0x1ul << FMC_ISPCON_ISPFF_Pos)

FMC_T::ISPCON: ISPFF Mask

Definition at line 1914 of file Mini51Series.h.

## ◆ FMC_ISPCON_ISPFF_Pos

#define FMC_ISPCON_ISPFF_Pos (6)

FMC_T::ISPCON: ISPFF Position

Definition at line 1913 of file Mini51Series.h.

## ◆ FMC_ISPCON_LDUEN_Msk

#define FMC_ISPCON_LDUEN_Msk (0x1ul << FMC_ISPCON_LDUEN_Pos)

FMC_T::ISPCON: LDUEN Mask

Definition at line 1911 of file Mini51Series.h.

## ◆ FMC_ISPCON_LDUEN_Pos

#define FMC_ISPCON_LDUEN_Pos (5)

FMC_T::ISPCON: LDUEN Position

Definition at line 1910 of file Mini51Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Msk

#define FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)

FMC_T::ISPDAT: ISPDAT Mask

Definition at line 1920 of file Mini51Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Pos

#define FMC_ISPDAT_ISPDAT_Pos (0)

FMC_T::ISPDAT: ISPDAT Position

Definition at line 1919 of file Mini51Series.h.

## ◆ FMC_ISPSTA_CBS_Msk

#define FMC_ISPSTA_CBS_Msk (0x3ul << FMC_ISPSTA_CBS_Pos)

FMC_T::ISPSTA: CBS Mask

Definition at line 1935 of file Mini51Series.h.

## ◆ FMC_ISPSTA_CBS_Pos

#define FMC_ISPSTA_CBS_Pos (1)

FMC_T::ISPSTA: CBS Position

Definition at line 1934 of file Mini51Series.h.

## ◆ FMC_ISPSTA_ISPFF_Msk

#define FMC_ISPSTA_ISPFF_Msk (0x1ul << FMC_ISPSTA_ISPFF_Pos)

FMC_T::ISPSTA: ISPFF Mask

Definition at line 1938 of file Mini51Series.h.

## ◆ FMC_ISPSTA_ISPFF_Pos

#define FMC_ISPSTA_ISPFF_Pos (6)

FMC_T::ISPSTA: ISPFF Position

Definition at line 1937 of file Mini51Series.h.

## ◆ FMC_ISPSTA_ISPGO_Msk

#define FMC_ISPSTA_ISPGO_Msk (0x1ul << FMC_ISPSTA_ISPGO_Pos)

FMC_T::ISPSTA: ISPGO Mask

Definition at line 1932 of file Mini51Series.h.

## ◆ FMC_ISPSTA_ISPGO_Pos

#define FMC_ISPSTA_ISPGO_Pos (0)

FMC_T::ISPSTA: ISPGO Position

Definition at line 1931 of file Mini51Series.h.

## ◆ FMC_ISPSTA_VECMAP_Msk

#define FMC_ISPSTA_VECMAP_Msk (0xffful << FMC_ISPSTA_VECMAP_Pos)

FMC_T::ISPSTA: VECMAP Mask

Definition at line 1941 of file Mini51Series.h.

## ◆ FMC_ISPSTA_VECMAP_Pos

#define FMC_ISPSTA_VECMAP_Pos (9)

FMC_T::ISPSTA: VECMAP Position

Definition at line 1940 of file Mini51Series.h.

## ◆ FMC_ISPTRG_ISPGO_Msk

#define FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)

FMC_T::ISPTRG: ISPGO Mask

Definition at line 1926 of file Mini51Series.h.

## ◆ FMC_ISPTRG_ISPGO_Pos

#define FMC_ISPTRG_ISPGO_Pos (0)

FMC_T::ISPTRG: ISPGO Position

Definition at line 1925 of file Mini51Series.h.

## ◆ GPIO_DBEN_DBEN_Msk

#define GPIO_DBEN_DBEN_Msk (0xfful << GPIO_DBEN_DBEN_Pos)

GPIO_T::DBEN: DBEN Mask

Definition at line 3699 of file Mini51Series.h.

## ◆ GPIO_DBEN_DBEN_Pos

#define GPIO_DBEN_DBEN_Pos (0)

GPIO_T::DBEN: DBEN Position

Definition at line 3698 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_DBCLKSEL_Msk

#define GPIO_DBNCECON_DBCLKSEL_Msk (0xful << GPIO_DBNCECON_DBCLKSEL_Pos)

GPIO_DBNCECON_T::DBNCECON: DBCLKSEL Mask

Definition at line 3714 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_DBCLKSEL_Pos

#define GPIO_DBNCECON_DBCLKSEL_Pos (0)

GPIO_DBNCECON_T::DBNCECON: DBCLKSEL Position

Definition at line 3713 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_DBCLKSRC_Msk

#define GPIO_DBNCECON_DBCLKSRC_Msk (0x1ul << GPIO_DBNCECON_DBCLKSRC_Pos)

GPIO_DBNCECON_T::DBNCECON: DBCLKSRC Mask

Definition at line 3717 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_DBCLKSRC_Pos

#define GPIO_DBNCECON_DBCLKSRC_Pos (4)

GPIO_DBNCECON_T::DBNCECON: DBCLKSRC Position

Definition at line 3716 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_ICLK_ON_Msk

#define GPIO_DBNCECON_ICLK_ON_Msk (0x1ul << GPIO_DBNCECON_ICLK_ON_Pos)

GPIO_DBNCECON_T::DBNCECON: ICLK_ON Mask

Definition at line 3720 of file Mini51Series.h.

## ◆ GPIO_DBNCECON_ICLK_ON_Pos

#define GPIO_DBNCECON_ICLK_ON_Pos (5)

GPIO_DBNCECON_T::DBNCECON: ICLK_ON Position

Definition at line 3719 of file Mini51Series.h.

## ◆ GPIO_DMASK_DMASK_Msk

#define GPIO_DMASK_DMASK_Msk (0xfful << GPIO_DMASK_DMASK_Pos)

GPIO_T::DMASK: DMASK Mask

Definition at line 3693 of file Mini51Series.h.

## ◆ GPIO_DMASK_DMASK_Pos

#define GPIO_DMASK_DMASK_Pos (0)

GPIO_T::DMASK: DMASK Position

Definition at line 3692 of file Mini51Series.h.

## ◆ GPIO_DOUT_DOUT_Msk

#define GPIO_DOUT_DOUT_Msk (0xfful << GPIO_DOUT_DOUT_Pos)

GPIO_T::DOUT: DOUT Mask

Definition at line 3690 of file Mini51Series.h.

## ◆ GPIO_DOUT_DOUT_Pos

#define GPIO_DOUT_DOUT_Pos (0)

GPIO_T::DOUT: DOUT Position

Definition at line 3689 of file Mini51Series.h.

## ◆ GPIO_IEN_IF_EN_Msk

#define GPIO_IEN_IF_EN_Msk (0x1ul << GPIO_IEN_IF_EN_Pos)

GPIO_T::IEN: IF_EN Mask

Definition at line 3705 of file Mini51Series.h.

## ◆ GPIO_IEN_IF_EN_Pos

#define GPIO_IEN_IF_EN_Pos (0)

GPIO_T::IEN: IF_EN Position

Definition at line 3704 of file Mini51Series.h.

## ◆ GPIO_IEN_IR_EN_Msk

#define GPIO_IEN_IR_EN_Msk (0xfful << GPIO_IEN_IR_EN_Pos)

GPIO_T::IEN: IR_EN Mask

Definition at line 3708 of file Mini51Series.h.

## ◆ GPIO_IEN_IR_EN_Pos

#define GPIO_IEN_IR_EN_Pos (16)

GPIO_T::IEN: IR_EN Position

Definition at line 3707 of file Mini51Series.h.

## ◆ GPIO_IMD_IMD_Msk

#define GPIO_IMD_IMD_Msk (0xfful << GPIO_IMD_IMD_Pos)

GPIO_T::IMD: IMD Mask

Definition at line 3702 of file Mini51Series.h.

## ◆ GPIO_IMD_IMD_Pos

#define GPIO_IMD_IMD_Pos (0)

GPIO_T::IMD: IMD Position

Definition at line 3701 of file Mini51Series.h.

## ◆ GPIO_ISRC_ISRC_Msk

#define GPIO_ISRC_ISRC_Msk (0xfful << GPIO_ISRC_ISRC_Pos)

GPIO_T::ISRC: ISRC Mask

Definition at line 3711 of file Mini51Series.h.

## ◆ GPIO_ISRC_ISRC_Pos

#define GPIO_ISRC_ISRC_Pos (0)

GPIO_T::ISRC: ISRC Position

Definition at line 3710 of file Mini51Series.h.

## ◆ GPIO_OFFD_OFFD_Msk

#define GPIO_OFFD_OFFD_Msk (0xfful << GPIO_OFFD_OFFD_Pos)

GPIO_T::OFFD: OFFD Mask

Definition at line 3687 of file Mini51Series.h.

## ◆ GPIO_OFFD_OFFD_Pos

#define GPIO_OFFD_OFFD_Pos (16)

GPIO_T::OFFD: OFFD Position

Definition at line 3686 of file Mini51Series.h.

## ◆ GPIO_PIN_PIN_Msk

#define GPIO_PIN_PIN_Msk (0xfful << GPIO_PIN_PIN_Pos)

GPIO_T::PIN: PIN Mask

Definition at line 3696 of file Mini51Series.h.

## ◆ GPIO_PIN_PIN_Pos

#define GPIO_PIN_PIN_Pos (0)

GPIO_T::PIN: PIN Position

Definition at line 3695 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD0_Msk

#define GPIO_PMD_PMD0_Msk (0x3ul << GPIO_PMD_PMD0_Pos)

GPIO_T::PMD: PMD0 Mask

Definition at line 3663 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD0_Pos

#define GPIO_PMD_PMD0_Pos (0)

    @addtogroup GP_CONST GP Bit Field Definition
    Constant Definitions for GP Controller

GPIO_T::PMD: PMD0 Position

Definition at line 3662 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD1_Msk

#define GPIO_PMD_PMD1_Msk (0x3ul << GPIO_PMD_PMD1_Pos)

GPIO_T::PMD: PMD1 Mask

Definition at line 3666 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD1_Pos

#define GPIO_PMD_PMD1_Pos (2)

GPIO_T::PMD: PMD1 Position

Definition at line 3665 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD2_Msk

#define GPIO_PMD_PMD2_Msk (0x3ul << GPIO_PMD_PMD2_Pos)

GPIO_T::PMD: PMD2 Mask

Definition at line 3669 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD2_Pos

#define GPIO_PMD_PMD2_Pos (4)

GPIO_T::PMD: PMD2 Position

Definition at line 3668 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD3_Msk

#define GPIO_PMD_PMD3_Msk (0x3ul << GPIO_PMD_PMD3_Pos)

GPIO_T::PMD: PMD3 Mask

Definition at line 3672 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD3_Pos

#define GPIO_PMD_PMD3_Pos (6)

GPIO_T::PMD: PMD3 Position

Definition at line 3671 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD4_Msk

#define GPIO_PMD_PMD4_Msk (0x3ul << GPIO_PMD_PMD4_Pos)

GPIO_T::PMD: PMD4 Mask

Definition at line 3675 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD4_Pos

#define GPIO_PMD_PMD4_Pos (8)

GPIO_T::PMD: PMD4 Position

Definition at line 3674 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD5_Msk

#define GPIO_PMD_PMD5_Msk (0x3ul << GPIO_PMD_PMD5_Pos)

GPIO_T::PMD: PMD5 Mask

Definition at line 3678 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD5_Pos

#define GPIO_PMD_PMD5_Pos (10)

GPIO_T::PMD: PMD5 Position

Definition at line 3677 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD6_Msk

#define GPIO_PMD_PMD6_Msk (0x3ul << GPIO_PMD_PMD6_Pos)

GPIO_T::PMD: PMD6 Mask

Definition at line 3681 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD6_Pos

#define GPIO_PMD_PMD6_Pos (12)

GPIO_T::PMD: PMD6 Position

Definition at line 3680 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD7_Msk

#define GPIO_PMD_PMD7_Msk (0x3ul << GPIO_PMD_PMD7_Pos)

GPIO_T::PMD: PMD7 Mask

Definition at line 3684 of file Mini51Series.h.

## ◆ GPIO_PMD_PMD7_Pos

#define GPIO_PMD_PMD7_Pos (14)

GPIO_T::PMD: PMD7 Position

Definition at line 3683 of file Mini51Series.h.

## ◆ I2C_I2CADDR_GC_Msk

#define I2C_I2CADDR_GC_Msk (0x1ul << I2C_I2CADDR_GC_Pos)

I2C_T::I2CADDR0: GC Mask

Definition at line 4268 of file Mini51Series.h.

## ◆ I2C_I2CADDR_GC_Pos

#define I2C_I2CADDR_GC_Pos (0)

I2C_T::I2CADDR0: GC Position

Definition at line 4267 of file Mini51Series.h.

## ◆ I2C_I2CADDR_I2CADDR_Msk

#define I2C_I2CADDR_I2CADDR_Msk (0x7ful << I2C_I2CADDR_I2CADDR_Pos)

I2C_T::I2CADDR0: I2CADDR Mask

Definition at line 4271 of file Mini51Series.h.

## ◆ I2C_I2CADDR_I2CADDR_Pos

#define I2C_I2CADDR_I2CADDR_Pos (1)

I2C_T::I2CADDR0: I2CADDR Position

Definition at line 4270 of file Mini51Series.h.

## ◆ I2C_I2CADM_I2CADM_Msk

#define I2C_I2CADM_I2CADM_Msk (0x7ful << I2C_I2CADM_I2CADM_Pos)

I2C_T::I2CADM0: I2CADM Mask

Definition at line 4292 of file Mini51Series.h.

## ◆ I2C_I2CADM_I2CADM_Pos

#define I2C_I2CADM_I2CADM_Pos (1)

I2C_T::I2CADM0: I2CADM Position

Definition at line 4291 of file Mini51Series.h.

## ◆ I2C_I2CDAT_I2CDAT_Msk

#define I2C_I2CDAT_I2CDAT_Msk (0xfful << I2C_I2CDAT_I2CDAT_Pos)

I2C_T::I2CDAT: I2CDAT Mask

Definition at line 4274 of file Mini51Series.h.

## ◆ I2C_I2CDAT_I2CDAT_Pos

#define I2C_I2CDAT_I2CDAT_Pos (0)

I2C_T::I2CDAT: I2CDAT Position

Definition at line 4273 of file Mini51Series.h.

## ◆ I2C_I2CLK_I2CLK_Msk

#define I2C_I2CLK_I2CLK_Msk (0xfful << I2C_I2CLK_I2CLK_Pos)

I2C_T::I2CLK: I2CLK Mask

Definition at line 4280 of file Mini51Series.h.

## ◆ I2C_I2CLK_I2CLK_Pos

#define I2C_I2CLK_I2CLK_Pos (0)

I2C_T::I2CLK: I2CLK Position

Definition at line 4279 of file Mini51Series.h.

## ◆ I2C_I2CON2_NOSTRETCH_Msk

#define I2C_I2CON2_NOSTRETCH_Msk (0x1ul << I2C_I2CON2_NOSTRETCH_Pos)

I2C_T::I2CON2: NOSTRETCH Mask

Definition at line 4301 of file Mini51Series.h.

## ◆ I2C_I2CON2_NOSTRETCH_Pos

#define I2C_I2CON2_NOSTRETCH_Pos (2)

I2C_T::I2CON2: NOSTRETCH Position

Definition at line 4300 of file Mini51Series.h.

## ◆ I2C_I2CON2_OVER_INTEN_Msk

#define I2C_I2CON2_OVER_INTEN_Msk (0x1ul << I2C_I2CON2_OVER_INTEN_Pos)

I2C_T::I2CON2: OVER_INTEN Mask

Definition at line 4304 of file Mini51Series.h.

## ◆ I2C_I2CON2_OVER_INTEN_Pos

#define I2C_I2CON2_OVER_INTEN_Pos (3)

I2C_T::I2CON2: OVER_INTEN Position

Definition at line 4303 of file Mini51Series.h.

## ◆ I2C_I2CON2_TWOFF_EN_Msk

#define I2C_I2CON2_TWOFF_EN_Msk (0x1ul << I2C_I2CON2_TWOFF_EN_Pos)

I2C_T::I2CON2: TWOFF_EN Mask

Definition at line 4298 of file Mini51Series.h.

## ◆ I2C_I2CON2_TWOFF_EN_Pos

#define I2C_I2CON2_TWOFF_EN_Pos (1)

I2C_T::I2CON2: TWOFF_EN Position

Definition at line 4297 of file Mini51Series.h.

## ◆ I2C_I2CON2_UNDER_INTEN_Msk

#define I2C_I2CON2_UNDER_INTEN_Msk (0x1ul << I2C_I2CON2_UNDER_INTEN_Pos)

I2C_T::I2CON2: UNDER_INTEN Mask

Definition at line 4307 of file Mini51Series.h.

## ◆ I2C_I2CON2_UNDER_INTEN_Pos

#define I2C_I2CON2_UNDER_INTEN_Pos (4)

I2C_T::I2CON2: UNDER_INTEN Position

Definition at line 4306 of file Mini51Series.h.

## ◆ I2C_I2CON2_WKUPEN_Msk

#define I2C_I2CON2_WKUPEN_Msk (0x1ul << I2C_I2CON2_WKUPEN_Pos)

I2C_T::I2CON2: WKUPEN Mask

Definition at line 4295 of file Mini51Series.h.

## ◆ I2C_I2CON2_WKUPEN_Pos

#define I2C_I2CON2_WKUPEN_Pos (0)

I2C_T::I2CON2: WKUPEN Position

Definition at line 4294 of file Mini51Series.h.

## ◆ I2C_I2CON_AA_Msk

#define I2C_I2CON_AA_Msk (0x1ul << I2C_I2CON_AA_Pos)

I2C_T::I2CON: AA Mask

Definition at line 4250 of file Mini51Series.h.

## ◆ I2C_I2CON_AA_Pos

#define I2C_I2CON_AA_Pos (2)

    @addtogroup I2C_CONST I2C Bit Field Definition
    Constant Definitions for I2C Controller

I2C_T::I2CON: AA Position

Definition at line 4249 of file Mini51Series.h.

## ◆ I2C_I2CON_EI_Msk

#define I2C_I2CON_EI_Msk (0x1ul << I2C_I2CON_EI_Pos)

I2C_T::I2CON: EI Mask

Definition at line 4265 of file Mini51Series.h.

## ◆ I2C_I2CON_EI_Pos

#define I2C_I2CON_EI_Pos (7)

I2C_T::I2CON: EI Position

Definition at line 4264 of file Mini51Series.h.

## ◆ I2C_I2CON_ENSI_Msk

#define I2C_I2CON_ENSI_Msk (0x1ul << I2C_I2CON_ENSI_Pos)

I2C_T::I2CON: ENSI Mask

Definition at line 4262 of file Mini51Series.h.

## ◆ I2C_I2CON_ENSI_Pos

#define I2C_I2CON_ENSI_Pos (6)

I2C_T::I2CON: ENSI Position

Definition at line 4261 of file Mini51Series.h.

## ◆ I2C_I2CON_SI_Msk

#define I2C_I2CON_SI_Msk (0x1ul << I2C_I2CON_SI_Pos)

I2C_T::I2CON: SI Mask

Definition at line 4253 of file Mini51Series.h.

## ◆ I2C_I2CON_SI_Pos

#define I2C_I2CON_SI_Pos (3)

I2C_T::I2CON: SI Position

Definition at line 4252 of file Mini51Series.h.

## ◆ I2C_I2CON_STA_Msk

#define I2C_I2CON_STA_Msk (0x1ul << I2C_I2CON_STA_Pos)

I2C_T::I2CON: STA Mask

Definition at line 4259 of file Mini51Series.h.

## ◆ I2C_I2CON_STA_Pos

#define I2C_I2CON_STA_Pos (5)

I2C_T::I2CON: STA Position

Definition at line 4258 of file Mini51Series.h.

## ◆ I2C_I2CON_STO_Msk

#define I2C_I2CON_STO_Msk (0x1ul << I2C_I2CON_STO_Pos)

I2C_T::I2CON: STO Mask

Definition at line 4256 of file Mini51Series.h.

## ◆ I2C_I2CON_STO_Pos

#define I2C_I2CON_STO_Pos (4)

I2C_T::I2CON: STO Position

Definition at line 4255 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_EMPTY_Msk

#define I2C_I2CSTATUS2_EMPTY_Msk (0x1ul << I2C_I2CSTATUS2_EMPTY_Pos)

I2C_T::I2CSTATUS2: EMPTY Mask

Definition at line 4316 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_EMPTY_Pos

#define I2C_I2CSTATUS2_EMPTY_Pos (2)

I2C_T::I2CSTATUS2: EMPTY Position

Definition at line 4315 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_FULL_Msk

#define I2C_I2CSTATUS2_FULL_Msk (0x1ul << I2C_I2CSTATUS2_FULL_Pos)

I2C_T::I2CSTATUS2: FULL Mask

Definition at line 4313 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_FULL_Pos

#define I2C_I2CSTATUS2_FULL_Pos (1)

I2C_T::I2CSTATUS2: FULL Position

Definition at line 4312 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_OVERUN_Msk

#define I2C_I2CSTATUS2_OVERUN_Msk (0x1ul << I2C_I2CSTATUS2_OVERUN_Pos)

I2C_T::I2CSTATUS2: OVERUN Mask

Definition at line 4319 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_OVERUN_Pos

#define I2C_I2CSTATUS2_OVERUN_Pos (3)

I2C_T::I2CSTATUS2: OVERUN Position

Definition at line 4318 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_UNDERUN_Msk

#define I2C_I2CSTATUS2_UNDERUN_Msk (0x1ul << I2C_I2CSTATUS2_UNDERUN_Pos)

I2C_T::I2CSTATUS2: UNDERUN Mask

Definition at line 4322 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_UNDERUN_Pos

#define I2C_I2CSTATUS2_UNDERUN_Pos (4)

I2C_T::I2CSTATUS2: UNDERUN Position

Definition at line 4321 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_WAKEUP_Msk

#define I2C_I2CSTATUS2_WAKEUP_Msk (0x1ul << I2C_I2CSTATUS2_WAKEUP_Pos)

I2C_T::I2CSTATUS2: WAKEUP Mask

Definition at line 4310 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS2_WAKEUP_Pos

#define I2C_I2CSTATUS2_WAKEUP_Pos (0)

I2C_T::I2CSTATUS2: WAKEUP Position

Definition at line 4309 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS_I2CSTATUS_Msk

#define I2C_I2CSTATUS_I2CSTATUS_Msk (0xfful << I2C_I2CSTATUS_I2CSTATUS_Pos)

I2C_T::I2CSTATUS: I2CSTATUS Mask

Definition at line 4277 of file Mini51Series.h.

## ◆ I2C_I2CSTATUS_I2CSTATUS_Pos

#define I2C_I2CSTATUS_I2CSTATUS_Pos (0)

I2C_T::I2CSTATUS: I2CSTATUS Position

Definition at line 4276 of file Mini51Series.h.

## ◆ I2C_I2CTOC_DIV4_Msk

#define I2C_I2CTOC_DIV4_Msk (0x1ul << I2C_I2CTOC_DIV4_Pos)

I2C_T::I2CTOC: DIV4 Mask

Definition at line 4286 of file Mini51Series.h.

## ◆ I2C_I2CTOC_DIV4_Pos

#define I2C_I2CTOC_DIV4_Pos (1)

I2C_T::I2CTOC: DIV4 Position

Definition at line 4285 of file Mini51Series.h.

## ◆ I2C_I2CTOC_ENTI_Msk

#define I2C_I2CTOC_ENTI_Msk (0x1ul << I2C_I2CTOC_ENTI_Pos)

I2C_T::I2CTOC: ENTI Mask

Definition at line 4289 of file Mini51Series.h.

## ◆ I2C_I2CTOC_ENTI_Pos

#define I2C_I2CTOC_ENTI_Pos (2)

I2C_T::I2CTOC: ENTI Position

Definition at line 4288 of file Mini51Series.h.

## ◆ I2C_I2CTOC_TIF_Msk

#define I2C_I2CTOC_TIF_Msk (0x1ul << I2C_I2CTOC_TIF_Pos)

I2C_T::I2CTOC: TIF Mask

Definition at line 4283 of file Mini51Series.h.

## ◆ I2C_I2CTOC_TIF_Pos

#define I2C_I2CTOC_TIF_Pos (0)

I2C_T::I2CTOC: TIF Position

Definition at line 4282 of file Mini51Series.h.

## ◆ INT_CON_NMI_SEL_EN_Msk

#define INT_CON_NMI_SEL_EN_Msk (0x1ul << INT_CON_NMI_SEL_EN_Pos)

INT_T::NMICON: NMI_SEL_EN Mask

Definition at line 4778 of file Mini51Series.h.

## ◆ INT_CON_NMI_SEL_EN_Pos

#define INT_CON_NMI_SEL_EN_Pos (8)

INT_T::NMICON: NMI_SEL_EN Position

Definition at line 4777 of file Mini51Series.h.

## ◆ INT_CON_NMI_SEL_Msk

#define INT_CON_NMI_SEL_Msk (0x1ful << INT_CON_NMI_SEL_Pos)

INT_T::NMICON: NMI_SEL Mask

Definition at line 4775 of file Mini51Series.h.

## ◆ INT_CON_NMI_SEL_Pos

#define INT_CON_NMI_SEL_Pos (0)

INT_T::NMICON: NMI_SEL Position

Definition at line 4774 of file Mini51Series.h.

## ◆ INT_IRQ_MCU_IRQ_Msk

#define INT_IRQ_MCU_IRQ_Msk (0xfffffffful << INT_IRQ_MCU_IRQ_Pos)

INT_T::MCUIRQ: MCU_IRQ Mask

Definition at line 4781 of file Mini51Series.h.

## ◆ INT_IRQ_MCU_IRQ_Pos

#define INT_IRQ_MCU_IRQ_Pos (0)

INT_T::MCUIRQ: MCU_IRQ Position

Definition at line 4780 of file Mini51Series.h.

## ◆ INT_SRC_INT_SRC_Msk

#define INT_SRC_INT_SRC_Msk (0x7ul << INT_SRC_INT_SRC_Pos)

INT_T::SRC0: INT_SRC Mask

Definition at line 4772 of file Mini51Series.h.

## ◆ INT_SRC_INT_SRC_Pos

#define INT_SRC_INT_SRC_Pos (0)

    @addtogroup INT_CONST INT Bit Field Definition
    Constant Definitions for INT Controller

INT_T::SRC0: INT_SRC Position

Definition at line 4771 of file Mini51Series.h.

## ◆ PWM_CMR_CMR_Msk

#define PWM_CMR_CMR_Msk (0xfffful << PWM_CMR_CMR_Pos)

PWM CMR::CMR Mask

Definition at line 6792 of file Mini51Series.h.

## ◆ PWM_CMR_CMR_Pos

#define PWM_CMR_CMR_Pos 0

PWM CMR::CMR Position

Definition at line 6791 of file Mini51Series.h.

## ◆ PWM_CNR_CNR_Msk

#define PWM_CNR_CNR_Msk (0xfffful << PWM_CNR_CNR_Pos)

PWM CNR::CNR Mask

Definition at line 6789 of file Mini51Series.h.

## ◆ PWM_CNR_CNR_Pos

#define PWM_CNR_CNR_Pos 0

PWM CNR::CNR Position

Definition at line 6788 of file Mini51Series.h.

## ◆ PWM_CSR_CSR0_Msk

#define PWM_CSR_CSR0_Msk (0x7ul << PWM_CSR_CSR0_Pos)

PWM_T::CSR: CSR0 Mask

Definition at line 6693 of file Mini51Series.h.

## ◆ PWM_CSR_CSR0_Pos

#define PWM_CSR_CSR0_Pos (0)

PWM_T::CSR: CSR0 Position

Definition at line 6692 of file Mini51Series.h.

## ◆ PWM_CSR_CSR1_Msk

#define PWM_CSR_CSR1_Msk (0x7ul << PWM_CSR_CSR1_Pos)

PWM_T::CSR: CSR1 Mask

Definition at line 6696 of file Mini51Series.h.

## ◆ PWM_CSR_CSR1_Pos

#define PWM_CSR_CSR1_Pos (4)

PWM_T::CSR: CSR1 Position

Definition at line 6695 of file Mini51Series.h.

## ◆ PWM_CSR_CSR2_Msk

#define PWM_CSR_CSR2_Msk (0x7ul << PWM_CSR_CSR2_Pos)

PWM_T::CSR: CSR2 Mask

Definition at line 6699 of file Mini51Series.h.

## ◆ PWM_CSR_CSR2_Pos

#define PWM_CSR_CSR2_Pos (8)

PWM_T::CSR: CSR2 Position

Definition at line 6698 of file Mini51Series.h.

## ◆ PWM_CSR_CSR3_Msk

#define PWM_CSR_CSR3_Msk (0x7ul << PWM_CSR_CSR3_Pos)

PWM_T::CSR: CSR3 Mask

Definition at line 6702 of file Mini51Series.h.

## ◆ PWM_CSR_CSR3_Pos

#define PWM_CSR_CSR3_Pos (12)

PWM_T::CSR: CSR3 Position

Definition at line 6701 of file Mini51Series.h.

## ◆ PWM_CSR_CSR4_Msk

#define PWM_CSR_CSR4_Msk (0x7ul << PWM_CSR_CSR4_Pos)

PWM_T::CSR: CSR4 Mask

Definition at line 6705 of file Mini51Series.h.

## ◆ PWM_CSR_CSR4_Pos

#define PWM_CSR_CSR4_Pos (16)

PWM_T::CSR: CSR4 Position

Definition at line 6704 of file Mini51Series.h.

## ◆ PWM_CSR_CSR5_Msk

#define PWM_CSR_CSR5_Msk (0x7ul << PWM_CSR_CSR5_Pos)

PWM_T::CSR: CSR5 Mask

Definition at line 6708 of file Mini51Series.h.

## ◆ PWM_CSR_CSR5_Pos

#define PWM_CSR_CSR5_Pos (20)

PWM_T::CSR: CSR5 Position

Definition at line 6707 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI01_Msk

#define PWM_DZIR_DZI01_Msk (0xfful << PWM_DZIR_DZI01_Pos)

PWM_T::PDZIR: DZI01 Mask

Definition at line 6936 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI01_Pos

#define PWM_DZIR_DZI01_Pos (0)

PWM_T::PDZIR: DZI01 Position

Definition at line 6935 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI23_Msk

#define PWM_DZIR_DZI23_Msk (0xfful << PWM_DZIR_DZI23_Pos)

PWM_T::PDZIR: DZI23 Mask

Definition at line 6939 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI23_Pos

#define PWM_DZIR_DZI23_Pos (8)

PWM_T::PDZIR: DZI23 Position

Definition at line 6938 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI45_Msk

#define PWM_DZIR_DZI45_Msk (0xfful << PWM_DZIR_DZI45_Pos)

PWM_T::PDZIR: DZI45 Mask

Definition at line 6942 of file Mini51Series.h.

## ◆ PWM_DZIR_DZI45_Pos

#define PWM_DZIR_DZI45_Pos (16)

PWM_T::PDZIR: DZI45 Position

Definition at line 6941 of file Mini51Series.h.

## ◆ PWM_INTACCUCTL_INTACCUEN0_Msk

#define PWM_INTACCUCTL_INTACCUEN0_Msk (0x1ul << PWM_INTACCUCTL_INTACCUEN0_Pos)

PWM_T::INTACCUCTL: INTACCUEN0 Mask

Definition at line 7284 of file Mini51Series.h.

## ◆ PWM_INTACCUCTL_INTACCUEN0_Pos

#define PWM_INTACCUCTL_INTACCUEN0_Pos (0)

PWM_T::INTACCUCTL: INTACCUEN0 Position

Definition at line 7283 of file Mini51Series.h.

## ◆ PWM_INTACCUCTL_PERIODCNT_Msk

#define PWM_INTACCUCTL_PERIODCNT_Msk (0xful << PWM_INTACCUCTL_PERIODCNT_Pos)

PWM_T::INTACCUCTL: PERIODCNT Mask

Definition at line 7287 of file Mini51Series.h.

## ◆ PWM_INTACCUCTL_PERIODCNT_Pos

#define PWM_INTACCUCTL_PERIODCNT_Pos (4)

PWM_T::INTACCUCTL: PERIODCNT Position

Definition at line 7286 of file Mini51Series.h.

## ◆ PWM_PCR_CH0EN_Msk

#define PWM_PCR_CH0EN_Msk (0x1ul << PWM_PCR_CH0EN_Pos)

PWM_T::PCR: CH0EN Mask

Definition at line 6711 of file Mini51Series.h.

## ◆ PWM_PCR_CH0EN_Pos

#define PWM_PCR_CH0EN_Pos (0)

PWM_T::PCR: CH0EN Position

Definition at line 6710 of file Mini51Series.h.

## ◆ PWM_PCR_CH0INV_Msk

#define PWM_PCR_CH0INV_Msk (0x1ul << PWM_PCR_CH0INV_Pos)

PWM_T::PCR: CH0INV Mask

Definition at line 6717 of file Mini51Series.h.

## ◆ PWM_PCR_CH0INV_Pos

#define PWM_PCR_CH0INV_Pos (2)

PWM_T::PCR: CH0INV Position

Definition at line 6716 of file Mini51Series.h.

## ◆ PWM_PCR_CH0MOD_Msk

#define PWM_PCR_CH0MOD_Msk (0x1ul << PWM_PCR_CH0MOD_Pos)

PWM_T::PCR: CH0MOD Mask

Definition at line 6720 of file Mini51Series.h.

## ◆ PWM_PCR_CH0MOD_Pos

#define PWM_PCR_CH0MOD_Pos (3)

PWM_T::PCR: CH0MOD Position

Definition at line 6719 of file Mini51Series.h.

## ◆ PWM_PCR_CH1EN_Msk

#define PWM_PCR_CH1EN_Msk (0x1ul << PWM_PCR_CH1EN_Pos)

PWM_T::PCR: CH1EN Mask

Definition at line 6723 of file Mini51Series.h.

## ◆ PWM_PCR_CH1EN_Pos

#define PWM_PCR_CH1EN_Pos (4)

PWM_T::PCR: CH1EN Position

Definition at line 6722 of file Mini51Series.h.

## ◆ PWM_PCR_CH1INV_Msk

#define PWM_PCR_CH1INV_Msk (0x1ul << PWM_PCR_CH1INV_Pos)

PWM_T::PCR: CH1INV Mask

Definition at line 6726 of file Mini51Series.h.

## ◆ PWM_PCR_CH1INV_Pos

#define PWM_PCR_CH1INV_Pos (6)

PWM_T::PCR: CH1INV Position

Definition at line 6725 of file Mini51Series.h.

## ◆ PWM_PCR_CH1MOD_Msk

#define PWM_PCR_CH1MOD_Msk (0x1ul << PWM_PCR_CH1MOD_Pos)

PWM_T::PCR: CH1MOD Mask

Definition at line 6729 of file Mini51Series.h.

## ◆ PWM_PCR_CH1MOD_Pos

#define PWM_PCR_CH1MOD_Pos (7)

PWM_T::PCR: CH1MOD Position

Definition at line 6728 of file Mini51Series.h.

## ◆ PWM_PCR_CH2EN_Msk

#define PWM_PCR_CH2EN_Msk (0x1ul << PWM_PCR_CH2EN_Pos)

PWM_T::PCR: CH2EN Mask

Definition at line 6732 of file Mini51Series.h.

## ◆ PWM_PCR_CH2EN_Pos

#define PWM_PCR_CH2EN_Pos (8)

PWM_T::PCR: CH2EN Position

Definition at line 6731 of file Mini51Series.h.

## ◆ PWM_PCR_CH2INV_Msk

#define PWM_PCR_CH2INV_Msk (0x1ul << PWM_PCR_CH2INV_Pos)

PWM_T::PCR: CH2INV Mask

Definition at line 6735 of file Mini51Series.h.

## ◆ PWM_PCR_CH2INV_Pos

#define PWM_PCR_CH2INV_Pos (10)

PWM_T::PCR: CH2INV Position

Definition at line 6734 of file Mini51Series.h.

## ◆ PWM_PCR_CH2MOD_Msk

#define PWM_PCR_CH2MOD_Msk (0x1ul << PWM_PCR_CH2MOD_Pos)

PWM_T::PCR: CH2MOD Mask

Definition at line 6738 of file Mini51Series.h.

## ◆ PWM_PCR_CH2MOD_Pos

#define PWM_PCR_CH2MOD_Pos (11)

PWM_T::PCR: CH2MOD Position

Definition at line 6737 of file Mini51Series.h.

## ◆ PWM_PCR_CH3EN_Msk

#define PWM_PCR_CH3EN_Msk (0x1ul << PWM_PCR_CH3EN_Pos)

PWM_T::PCR: CH3EN Mask

Definition at line 6741 of file Mini51Series.h.

## ◆ PWM_PCR_CH3EN_Pos

#define PWM_PCR_CH3EN_Pos (12)

PWM_T::PCR: CH3EN Position

Definition at line 6740 of file Mini51Series.h.

## ◆ PWM_PCR_CH3INV_Msk

#define PWM_PCR_CH3INV_Msk (0x1ul << PWM_PCR_CH3INV_Pos)

PWM_T::PCR: CH3INV Mask

Definition at line 6744 of file Mini51Series.h.

## ◆ PWM_PCR_CH3INV_Pos

#define PWM_PCR_CH3INV_Pos (14)

PWM_T::PCR: CH3INV Position

Definition at line 6743 of file Mini51Series.h.

## ◆ PWM_PCR_CH3MOD_Msk

#define PWM_PCR_CH3MOD_Msk (0x1ul << PWM_PCR_CH3MOD_Pos)

PWM_T::PCR: CH3MOD Mask

Definition at line 6747 of file Mini51Series.h.

## ◆ PWM_PCR_CH3MOD_Pos

#define PWM_PCR_CH3MOD_Pos (15)

PWM_T::PCR: CH3MOD Position

Definition at line 6746 of file Mini51Series.h.

## ◆ PWM_PCR_CH4EN_Msk

#define PWM_PCR_CH4EN_Msk (0x1ul << PWM_PCR_CH4EN_Pos)

PWM_T::PCR: CH4EN Mask

Definition at line 6750 of file Mini51Series.h.

## ◆ PWM_PCR_CH4EN_Pos

#define PWM_PCR_CH4EN_Pos (16)

PWM_T::PCR: CH4EN Position

Definition at line 6749 of file Mini51Series.h.

## ◆ PWM_PCR_CH4INV_Msk

#define PWM_PCR_CH4INV_Msk (0x1ul << PWM_PCR_CH4INV_Pos)

PWM_T::PCR: CH4INV Mask

Definition at line 6753 of file Mini51Series.h.

## ◆ PWM_PCR_CH4INV_Pos

#define PWM_PCR_CH4INV_Pos (18)

PWM_T::PCR: CH4INV Position

Definition at line 6752 of file Mini51Series.h.

## ◆ PWM_PCR_CH4MOD_Msk

#define PWM_PCR_CH4MOD_Msk (0x1ul << PWM_PCR_CH4MOD_Pos)

PWM_T::PCR: CH4MOD Mask

Definition at line 6756 of file Mini51Series.h.

## ◆ PWM_PCR_CH4MOD_Pos

#define PWM_PCR_CH4MOD_Pos (19)

PWM_T::PCR: CH4MOD Position

Definition at line 6755 of file Mini51Series.h.

## ◆ PWM_PCR_CH5EN_Msk

#define PWM_PCR_CH5EN_Msk (0x1ul << PWM_PCR_CH5EN_Pos)

PWM_T::PCR: CH5EN Mask

Definition at line 6759 of file Mini51Series.h.

## ◆ PWM_PCR_CH5EN_Pos

#define PWM_PCR_CH5EN_Pos (20)

PWM_T::PCR: CH5EN Position

Definition at line 6758 of file Mini51Series.h.

## ◆ PWM_PCR_CH5INV_Msk

#define PWM_PCR_CH5INV_Msk (0x1ul << PWM_PCR_CH5INV_Pos)

PWM_T::PCR: CH5INV Mask

Definition at line 6762 of file Mini51Series.h.

## ◆ PWM_PCR_CH5INV_Pos

#define PWM_PCR_CH5INV_Pos (22)

PWM_T::PCR: CH5INV Position

Definition at line 6761 of file Mini51Series.h.

## ◆ PWM_PCR_CH5MOD_Msk

#define PWM_PCR_CH5MOD_Msk (0x1ul << PWM_PCR_CH5MOD_Pos)

PWM_T::PCR: CH5MOD Mask

Definition at line 6765 of file Mini51Series.h.

## ◆ PWM_PCR_CH5MOD_Pos

#define PWM_PCR_CH5MOD_Pos (23)

PWM_T::PCR: CH5MOD Position

Definition at line 6764 of file Mini51Series.h.

## ◆ PWM_PCR_CLRPWM_Msk

#define PWM_PCR_CLRPWM_Msk (0x1ul << PWM_PCR_CLRPWM_Pos)

PWM_T::PCR: CLRPWM Mask

Definition at line 6777 of file Mini51Series.h.

## ◆ PWM_PCR_CLRPWM_Pos

#define PWM_PCR_CLRPWM_Pos (27)

PWM_T::PCR: CLRPWM Position

Definition at line 6776 of file Mini51Series.h.

## ◆ PWM_PCR_DB_MOD_Msk

#define PWM_PCR_DB_MOD_Msk (0x1ul << PWM_PCR_DB_MOD_Pos)

PWM_T::PCR: DB_MODE Mask

Definition at line 6714 of file Mini51Series.h.

## ◆ PWM_PCR_DB_MOD_Pos

#define PWM_PCR_DB_MOD_Pos (1)

PWM_T::PCR: DB_MODE Position

Definition at line 6713 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN01_Msk

#define PWM_PCR_DZEN01_Msk (0x1ul << PWM_PCR_DZEN01_Pos)

PWM_T::PCR: DZEN01 Mask

Definition at line 6768 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN01_Pos

#define PWM_PCR_DZEN01_Pos (24)

PWM_T::PCR: DZEN01 Position

Definition at line 6767 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN23_Msk

#define PWM_PCR_DZEN23_Msk (0x1ul << PWM_PCR_DZEN23_Pos)

PWM_T::PCR: DZEN23 Mask

Definition at line 6771 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN23_Pos

#define PWM_PCR_DZEN23_Pos (25)

PWM_T::PCR: DZEN23 Position

Definition at line 6770 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN45_Msk

#define PWM_PCR_DZEN45_Msk (0x1ul << PWM_PCR_DZEN45_Pos)

PWM_T::PCR: DZEN45 Mask

Definition at line 6774 of file Mini51Series.h.

## ◆ PWM_PCR_DZEN45_Pos

#define PWM_PCR_DZEN45_Pos (26)

PWM_T::PCR: DZEN45 Position

Definition at line 6773 of file Mini51Series.h.

## ◆ PWM_PCR_GRP_Msk

#define PWM_PCR_GRP_Msk (0x1ul << PWM_PCR_GRP_Pos)

PWM_T::PCR: GRP Mask

Definition at line 6783 of file Mini51Series.h.

## ◆ PWM_PCR_GRP_Pos

#define PWM_PCR_GRP_Pos (30)

PWM_T::PCR: GRP Position

Definition at line 6782 of file Mini51Series.h.

## ◆ PWM_PCR_PWMMOD_Msk

#define PWM_PCR_PWMMOD_Msk (0x3ul << PWM_PCR_PWMMOD_Pos)

PWM_T::PCR: PWMMOD Mask

Definition at line 6780 of file Mini51Series.h.

## ◆ PWM_PCR_PWMMOD_Pos

#define PWM_PCR_PWMMOD_Pos (28)

PWM_T::PCR: PWMMOD Position

Definition at line 6779 of file Mini51Series.h.

## ◆ PWM_PCR_PWMTYPE_Msk

#define PWM_PCR_PWMTYPE_Msk (0x1ul << PWM_PCR_PWMTYPE_Pos)

PWM_T::PCR: PWMTYPE Mask

Definition at line 6786 of file Mini51Series.h.

## ◆ PWM_PCR_PWMTYPE_Pos

#define PWM_PCR_PWMTYPE_Pos (31)

PWM_T::PCR: PWMTYPE Position

Definition at line 6785 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKEN0_Msk

#define PWM_PFBCON_BKEN0_Msk (0x1ul << PWM_PFBCON_BKEN0_Pos)

PWM_T::PFBCON: BKEN0 Mask

Definition at line 6897 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKEN0_Pos

#define PWM_PFBCON_BKEN0_Pos (0)

PWM_T::PFBCON: BKEN0 Position

Definition at line 6896 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKEN1_Msk

#define PWM_PFBCON_BKEN1_Msk (0x1ul << PWM_PFBCON_BKEN1_Pos)

PWM_T::PFBCON: BKEN1 Mask

Definition at line 6900 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKEN1_Pos

#define PWM_PFBCON_BKEN1_Pos (1)

PWM_T::PFBCON: BKEN1 Position

Definition at line 6899 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKF_Msk

#define PWM_PFBCON_BKF_Msk (0x1ul << PWM_PFBCON_BKF_Pos)

PWM_T::PFBCON: BKF Mask

Definition at line 6909 of file Mini51Series.h.

## ◆ PWM_PFBCON_BKF_Pos

#define PWM_PFBCON_BKF_Pos (7)

PWM_T::PFBCON: BKF Position

Definition at line 6908 of file Mini51Series.h.

## ◆ PWM_PFBCON_CPO0BKEN_Msk

#define PWM_PFBCON_CPO0BKEN_Msk (0x1ul << PWM_PFBCON_CPO0BKEN_Pos)

PWM_T::PFBCON: CPO0BKEN Mask

Definition at line 6903 of file Mini51Series.h.

## ◆ PWM_PFBCON_CPO0BKEN_Pos

#define PWM_PFBCON_CPO0BKEN_Pos (2)

PWM_T::PFBCON: CPO0BKEN Position

Definition at line 6902 of file Mini51Series.h.

## ◆ PWM_PFBCON_CPO1BKEN_Msk

#define PWM_PFBCON_CPO1BKEN_Msk (0x1ul << PWM_PFBCON_CPO1BKEN_Pos)

PWM_T::PFBCON: CPO1BKEN Mask

Definition at line 6906 of file Mini51Series.h.

## ◆ PWM_PFBCON_CPO1BKEN_Pos

#define PWM_PFBCON_CPO1BKEN_Pos (3)

PWM_T::PFBCON: CPO1BKEN Position

Definition at line 6905 of file Mini51Series.h.

## ◆ PWM_PFBCON_D6BKO6_Msk

#define PWM_PFBCON_D6BKO6_Msk (0x1ul << PWM_PFBCON_D6BKO6_Pos)

PWM_T::PFBCON: D6BKO6 Mask

Definition at line 6930 of file Mini51Series.h.

## ◆ PWM_PFBCON_D6BKO6_Pos

#define PWM_PFBCON_D6BKO6_Pos (30)

PWM_T::PFBCON: D6BKO6 Position

Definition at line 6929 of file Mini51Series.h.

## ◆ PWM_PFBCON_D7BKO7_Msk

#define PWM_PFBCON_D7BKO7_Msk (0x1ul << PWM_PFBCON_D7BKO7_Pos)

PWM_T::PFBCON: D7BKO7 Mask

Definition at line 6933 of file Mini51Series.h.

## ◆ PWM_PFBCON_D7BKO7_Pos

#define PWM_PFBCON_D7BKO7_Pos (31)

PWM_T::PFBCON: D7BKO7 Position

Definition at line 6932 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO0_Msk

#define PWM_PFBCON_PWMBKO0_Msk (0x1ul << PWM_PFBCON_PWMBKO0_Pos)

PWM_T::PFBCON: PWMBKO0 Mask

Definition at line 6912 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO0_Pos

#define PWM_PFBCON_PWMBKO0_Pos (24)

PWM_T::PFBCON: PWMBKO0 Position

Definition at line 6911 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO1_Msk

#define PWM_PFBCON_PWMBKO1_Msk (0x1ul << PWM_PFBCON_PWMBKO1_Pos)

PWM_T::PFBCON: PWMBKO1 Mask

Definition at line 6915 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO1_Pos

#define PWM_PFBCON_PWMBKO1_Pos (25)

PWM_T::PFBCON: PWMBKO1 Position

Definition at line 6914 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO2_Msk

#define PWM_PFBCON_PWMBKO2_Msk (0x1ul << PWM_PFBCON_PWMBKO2_Pos)

PWM_T::PFBCON: PWMBKO2 Mask

Definition at line 6918 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO2_Pos

#define PWM_PFBCON_PWMBKO2_Pos (26)

PWM_T::PFBCON: PWMBKO2 Position

Definition at line 6917 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO3_Msk

#define PWM_PFBCON_PWMBKO3_Msk (0x1ul << PWM_PFBCON_PWMBKO3_Pos)

PWM_T::PFBCON: PWMBKO3 Mask

Definition at line 6921 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO3_Pos

#define PWM_PFBCON_PWMBKO3_Pos (27)

PWM_T::PFBCON: PWMBKO3 Position

Definition at line 6920 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO4_Msk

#define PWM_PFBCON_PWMBKO4_Msk (0x1ul << PWM_PFBCON_PWMBKO4_Pos)

PWM_T::PFBCON: PWMBKO4 Mask

Definition at line 6924 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO4_Pos

#define PWM_PFBCON_PWMBKO4_Pos (28)

PWM_T::PFBCON: PWMBKO4 Position

Definition at line 6923 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO5_Msk

#define PWM_PFBCON_PWMBKO5_Msk (0x1ul << PWM_PFBCON_PWMBKO5_Pos)

PWM_T::PFBCON: PWMBKO5 Mask

Definition at line 6927 of file Mini51Series.h.

## ◆ PWM_PFBCON_PWMBKO5_Pos

#define PWM_PFBCON_PWMBKO5_Pos (29)

PWM_T::PFBCON: PWMBKO5 Position

Definition at line 6926 of file Mini51Series.h.

## ◆ PWM_PHCHG_ACCNT0_Msk

#define PWM_PHCHG_ACCNT0_Msk (0x1ul << PWM_PHCHG_ACCNT0_Pos)

PWM_T::PHCHG: ACCNT0 Mask

Definition at line 7131 of file Mini51Series.h.

## ◆ PWM_PHCHG_ACCNT0_Pos

#define PWM_PHCHG_ACCNT0_Pos (14)

PWM_T::PHCHG: ACCNT0 Position

Definition at line 7130 of file Mini51Series.h.

## ◆ PWM_PHCHG_ACCNT1_Msk

#define PWM_PHCHG_ACCNT1_Msk (0x1ul << PWM_PHCHG_ACCNT1_Pos)

PWM_T::PHCHG: ACCNT1 Mask

Definition at line 7134 of file Mini51Series.h.

## ◆ PWM_PHCHG_ACCNT1_Pos

#define PWM_PHCHG_ACCNT1_Pos (15)

PWM_T::PHCHG: ACCNT1 Position

Definition at line 7133 of file Mini51Series.h.

## ◆ PWM_PHCHG_CE0_Msk

#define PWM_PHCHG_CE0_Msk (0x1ul << PWM_PHCHG_CE0_Pos)

PWM_T::PHCHG: CE0 Mask

Definition at line 7176 of file Mini51Series.h.

## ◆ PWM_PHCHG_CE0_Pos

#define PWM_PHCHG_CE0_Pos (31)

PWM_T::PHCHG: CE0 Position

Definition at line 7175 of file Mini51Series.h.

## ◆ PWM_PHCHG_CE1_Msk

#define PWM_PHCHG_CE1_Msk (0x1ul << PWM_PHCHG_CE1_Pos)

PWM_T::PHCHG: CE1 Mask

Definition at line 7155 of file Mini51Series.h.

## ◆ PWM_PHCHG_CE1_Pos

#define PWM_PHCHG_CE1_Pos (23)

PWM_T::PHCHG: CE1 Position

Definition at line 7154 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH01TOFF0_Msk

#define PWM_PHCHG_CH01TOFF0_Msk (0x1ul << PWM_PHCHG_CH01TOFF0_Pos)

PWM_T::PHCHG: CH01TOFF0 Mask

Definition at line 7158 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH01TOFF0_Pos

#define PWM_PHCHG_CH01TOFF0_Pos (24)

PWM_T::PHCHG: CH01TOFF0 Position

Definition at line 7157 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH01TOFF1_Msk

#define PWM_PHCHG_CH01TOFF1_Msk (0x1ul << PWM_PHCHG_CH01TOFF1_Pos)

PWM_T::PHCHG: CH01TOFF1 Mask

Definition at line 7137 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH01TOFF1_Pos

#define PWM_PHCHG_CH01TOFF1_Pos (16)

PWM_T::PHCHG: CH01TOFF1 Position

Definition at line 7136 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH11TOFF0_Msk

#define PWM_PHCHG_CH11TOFF0_Msk (0x1ul << PWM_PHCHG_CH11TOFF0_Pos)

PWM_T::PHCHG: CH11TOFF0 Mask

Definition at line 7161 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH11TOFF0_Pos

#define PWM_PHCHG_CH11TOFF0_Pos (25)

PWM_T::PHCHG: CH11TOFF0 Position

Definition at line 7160 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH11TOFF1_Msk

#define PWM_PHCHG_CH11TOFF1_Msk (0x1ul << PWM_PHCHG_CH11TOFF1_Pos)

PWM_T::PHCHG: CH11TOFF1 Mask

Definition at line 7140 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH11TOFF1_Pos

#define PWM_PHCHG_CH11TOFF1_Pos (17)

PWM_T::PHCHG: CH11TOFF1 Position

Definition at line 7139 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH21TOFF0_Msk

#define PWM_PHCHG_CH21TOFF0_Msk (0x1ul << PWM_PHCHG_CH21TOFF0_Pos)

PWM_T::PHCHG: CH21TOFF0 Mask

Definition at line 7164 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH21TOFF0_Pos

#define PWM_PHCHG_CH21TOFF0_Pos (26)

PWM_T::PHCHG: CH21TOFF0 Position

Definition at line 7163 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH21TOFF1_Msk

#define PWM_PHCHG_CH21TOFF1_Msk (0x1ul << PWM_PHCHG_CH21TOFF1_Pos)

PWM_T::PHCHG: CH21TOFF1 Mask

Definition at line 7143 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH21TOFF1_Pos

#define PWM_PHCHG_CH21TOFF1_Pos (18)

PWM_T::PHCHG: CH21TOFF1 Position

Definition at line 7142 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH31TOFF0_Msk

#define PWM_PHCHG_CH31TOFF0_Msk (0x1ul << PWM_PHCHG_CH31TOFF0_Pos)

PWM_T::PHCHG: CH31TOFF0 Mask

Definition at line 7167 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH31TOFF0_Pos

#define PWM_PHCHG_CH31TOFF0_Pos (27)

PWM_T::PHCHG: CH31TOFF0 Position

Definition at line 7166 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH31TOFF1_Msk

#define PWM_PHCHG_CH31TOFF1_Msk (0x1ul << PWM_PHCHG_CH31TOFF1_Pos)

PWM_T::PHCHG: CH31TOFF1 Mask

Definition at line 7146 of file Mini51Series.h.

## ◆ PWM_PHCHG_CH31TOFF1_Pos

#define PWM_PHCHG_CH31TOFF1_Pos (19)

PWM_T::PHCHG: CH31TOFF1 Position

Definition at line 7145 of file Mini51Series.h.

## ◆ PWM_PHCHG_CMP0SEL_Msk

#define PWM_PHCHG_CMP0SEL_Msk (0x3ul << PWM_PHCHG_CMP0SEL_Pos)

PWM_T::PHCHG: CMP0SEL Mask

Definition at line 7170 of file Mini51Series.h.

## ◆ PWM_PHCHG_CMP0SEL_Pos

#define PWM_PHCHG_CMP0SEL_Pos (28)

PWM_T::PHCHG: CMP0SEL Position

Definition at line 7169 of file Mini51Series.h.

## ◆ PWM_PHCHG_CMP1SEL_Msk

#define PWM_PHCHG_CMP1SEL_Msk (0x3ul << PWM_PHCHG_CMP1SEL_Pos)

PWM_T::PHCHG: CMP1SEL Mask

Definition at line 7149 of file Mini51Series.h.

## ◆ PWM_PHCHG_CMP1SEL_Pos

#define PWM_PHCHG_CMP1SEL_Pos (20)

PWM_T::PHCHG: CMP1SEL Position

Definition at line 7148 of file Mini51Series.h.

## ◆ PWM_PHCHG_D0_Msk

#define PWM_PHCHG_D0_Msk (0x1ul << PWM_PHCHG_D0_Pos)

PWM_T::PHCHG: D0 Mask

Definition at line 7089 of file Mini51Series.h.

## ◆ PWM_PHCHG_D0_Pos

#define PWM_PHCHG_D0_Pos (0)

PWM_T::PHCHG: D0 Position

Definition at line 7088 of file Mini51Series.h.

## ◆ PWM_PHCHG_D1_Msk

#define PWM_PHCHG_D1_Msk (0x1ul << PWM_PHCHG_D1_Pos)

PWM_T::PHCHG: D1 Mask

Definition at line 7092 of file Mini51Series.h.

## ◆ PWM_PHCHG_D1_Pos

#define PWM_PHCHG_D1_Pos (1)

PWM_T::PHCHG: D1 Position

Definition at line 7091 of file Mini51Series.h.

## ◆ PWM_PHCHG_D2_Msk

#define PWM_PHCHG_D2_Msk (0x1ul << PWM_PHCHG_D2_Pos)

PWM_T::PHCHG: D2 Mask

Definition at line 7095 of file Mini51Series.h.

## ◆ PWM_PHCHG_D2_Pos

#define PWM_PHCHG_D2_Pos (2)

PWM_T::PHCHG: D2 Position

Definition at line 7094 of file Mini51Series.h.

## ◆ PWM_PHCHG_D3_Msk

#define PWM_PHCHG_D3_Msk (0x1ul << PWM_PHCHG_D3_Pos)

PWM_T::PHCHG: D3 Mask

Definition at line 7098 of file Mini51Series.h.

## ◆ PWM_PHCHG_D3_Pos

#define PWM_PHCHG_D3_Pos (3)

PWM_T::PHCHG: D3 Position

Definition at line 7097 of file Mini51Series.h.

## ◆ PWM_PHCHG_D4_Msk

#define PWM_PHCHG_D4_Msk (0x1ul << PWM_PHCHG_D4_Pos)

PWM_T::PHCHG: D4 Mask

Definition at line 7101 of file Mini51Series.h.

## ◆ PWM_PHCHG_D4_Pos

#define PWM_PHCHG_D4_Pos (4)

PWM_T::PHCHG: D4 Position

Definition at line 7100 of file Mini51Series.h.

## ◆ PWM_PHCHG_D5_Msk

#define PWM_PHCHG_D5_Msk (0x1ul << PWM_PHCHG_D5_Pos)

PWM_T::PHCHG: D5 Mask

Definition at line 7104 of file Mini51Series.h.

## ◆ PWM_PHCHG_D5_Pos

#define PWM_PHCHG_D5_Pos (5)

PWM_T::PHCHG: D5 Position

Definition at line 7103 of file Mini51Series.h.

## ◆ PWM_PHCHG_D6_Msk

#define PWM_PHCHG_D6_Msk (0x1ul << PWM_PHCHG_D6_Pos)

PWM_T::PHCHG: D6 Mask

Definition at line 7107 of file Mini51Series.h.

## ◆ PWM_PHCHG_D6_Pos

#define PWM_PHCHG_D6_Pos (6)

PWM_T::PHCHG: D6 Position

Definition at line 7106 of file Mini51Series.h.

## ◆ PWM_PHCHG_D7_Msk

#define PWM_PHCHG_D7_Msk (0x1ul << PWM_PHCHG_D7_Pos)

PWM_T::PHCHG: D7 Mask

Definition at line 7110 of file Mini51Series.h.

## ◆ PWM_PHCHG_D7_Pos

#define PWM_PHCHG_D7_Pos (7)

PWM_T::PHCHG: D7 Position

Definition at line 7109 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM0_Msk

#define PWM_PHCHG_PWM0_Msk (0x1ul << PWM_PHCHG_PWM0_Pos)

PWM_T::PHCHG: PWM0 Mask

Definition at line 7113 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM0_Pos

#define PWM_PHCHG_PWM0_Pos (8)

PWM_T::PHCHG: PWM0 Position

Definition at line 7112 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM1_Msk

#define PWM_PHCHG_PWM1_Msk (0x1ul << PWM_PHCHG_PWM1_Pos)

PWM_T::PHCHG: PWM1 Mask

Definition at line 7116 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM1_Pos

#define PWM_PHCHG_PWM1_Pos (9)

PWM_T::PHCHG: PWM1 Position

Definition at line 7115 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM2_Msk

#define PWM_PHCHG_PWM2_Msk (0x1ul << PWM_PHCHG_PWM2_Pos)

PWM_T::PHCHG: PWM2 Mask

Definition at line 7119 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM2_Pos

#define PWM_PHCHG_PWM2_Pos (10)

PWM_T::PHCHG: PWM2 Position

Definition at line 7118 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM3_Msk

#define PWM_PHCHG_PWM3_Msk (0x1ul << PWM_PHCHG_PWM3_Pos)

PWM_T::PHCHG: PWM3 Mask

Definition at line 7122 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM3_Pos

#define PWM_PHCHG_PWM3_Pos (11)

PWM_T::PHCHG: PWM3 Position

Definition at line 7121 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM4_Msk

#define PWM_PHCHG_PWM4_Msk (0x1ul << PWM_PHCHG_PWM4_Pos)

PWM_T::PHCHG: PWM4 Mask

Definition at line 7125 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM4_Pos

#define PWM_PHCHG_PWM4_Pos (12)

PWM_T::PHCHG: PWM4 Position

Definition at line 7124 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM5_Msk

#define PWM_PHCHG_PWM5_Msk (0x1ul << PWM_PHCHG_PWM5_Pos)

PWM_T::PHCHG: PWM5 Mask

Definition at line 7128 of file Mini51Series.h.

## ◆ PWM_PHCHG_PWM5_Pos

#define PWM_PHCHG_PWM5_Pos (13)

PWM_T::PHCHG: PWM5 Position

Definition at line 7127 of file Mini51Series.h.

## ◆ PWM_PHCHG_T0_Msk

#define PWM_PHCHG_T0_Msk (0x1ul << PWM_PHCHG_T0_Pos)

PWM_T::PHCHG: T0 Mask

Definition at line 7173 of file Mini51Series.h.

## ◆ PWM_PHCHG_T0_Pos

#define PWM_PHCHG_T0_Pos (30)

PWM_T::PHCHG: T0 Position

Definition at line 7172 of file Mini51Series.h.

## ◆ PWM_PHCHG_T1_Msk

#define PWM_PHCHG_T1_Msk (0x1ul << PWM_PHCHG_T1_Pos)

PWM_T::PHCHG: T1 Mask

Definition at line 7152 of file Mini51Series.h.

## ◆ PWM_PHCHG_T1_Pos

#define PWM_PHCHG_T1_Pos (22)

PWM_T::PHCHG: T1 Position

Definition at line 7151 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK0_Msk

#define PWM_PHCHGMASK_CMPMASK0_Msk (0x1ul << PWM_PHCHGMASK_CMPMASK0_Pos)

PWM_T::PHCHGMASK: CMPMASK0 Mask

Definition at line 7278 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK0_Pos

#define PWM_PHCHGMASK_CMPMASK0_Pos (8)

PWM_T::PHCHGMASK: CMPMASK0 Position

Definition at line 7277 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK1_Msk

#define PWM_PHCHGMASK_CMPMASK1_Msk (0x1ul << PWM_PHCHGMASK_CMPMASK1_Pos)

PWM_T::PHCHGMASK: CMPMASK1 Mask

Definition at line 7281 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK1_Pos

#define PWM_PHCHGMASK_CMPMASK1_Pos (9)

PWM_T::PHCHGMASK: CMPMASK1 Position

Definition at line 7280 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK_Msk

#define PWM_PHCHGMASK_CMPMASK_Msk (0x3ul << PWM_PHCHGMASK_CMPMASK_Pos)

PWM_T::PHCHGMASK: CMPMASK Mask

Definition at line 7275 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_CMPMASK_Pos

#define PWM_PHCHGMASK_CMPMASK_Pos (8)

PWM_T::PHCHGMASK: CMPMASK Position

Definition at line 7274 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_MASK6_Msk

#define PWM_PHCHGMASK_MASK6_Msk (0x1ul << PWM_PHCHGMASK_MASK6_Pos)

PWM_T::PHCHGMASK: MASK6 Mask

Definition at line 7269 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_MASK6_Pos

#define PWM_PHCHGMASK_MASK6_Pos (6)

PWM_T::PHCHGMASK: MASK6 Position

Definition at line 7268 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_MASK7_Msk

#define PWM_PHCHGMASK_MASK7_Msk (0x1ul << PWM_PHCHGMASK_MASK7_Pos)

PWM_T::PHCHGMASK: MASK7 Mask

Definition at line 7272 of file Mini51Series.h.

## ◆ PWM_PHCHGMASK_MASK7_Pos

#define PWM_PHCHGMASK_MASK7_Pos (7)

PWM_T::PHCHGMASK: MASK7 Position

Definition at line 7271 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_ACCNT0_Msk

#define PWM_PHCHGNXT_ACCNT0_Msk (0x1ul << PWM_PHCHGNXT_ACCNT0_Pos)

PWM_T::PHCHGNXT: ACCNT0 Mask

Definition at line 7221 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_ACCNT0_Pos

#define PWM_PHCHGNXT_ACCNT0_Pos (14)

PWM_T::PHCHGNXT: ACCNT0 Position

Definition at line 7220 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_ACCNT1_Msk

#define PWM_PHCHGNXT_ACCNT1_Msk (0x1ul << PWM_PHCHGNXT_ACCNT1_Pos)

PWM_T::PHCHGNXT: ACCNT1 Mask

Definition at line 7224 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_ACCNT1_Pos

#define PWM_PHCHGNXT_ACCNT1_Pos (15)

PWM_T::PHCHGNXT: ACCNT1 Position

Definition at line 7223 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CE0_Msk

#define PWM_PHCHGNXT_CE0_Msk (0x1ul << PWM_PHCHGNXT_CE0_Pos)

PWM_T::PHCHGNXT: CE0 Mask

Definition at line 7266 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CE0_Pos

#define PWM_PHCHGNXT_CE0_Pos (31)

PWM_T::PHCHGNXT: CE0 Position

Definition at line 7265 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CE1_Msk

#define PWM_PHCHGNXT_CE1_Msk (0x1ul << PWM_PHCHGNXT_CE1_Pos)

PWM_T::PHCHGNXT: CE1 Mask

Definition at line 7245 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CE1_Pos

#define PWM_PHCHGNXT_CE1_Pos (23)

PWM_T::PHCHGNXT: CE1 Position

Definition at line 7244 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH01TOFF0_Msk

#define PWM_PHCHGNXT_CH01TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH01TOFF0_Pos)

PWM_T::PHCHGNXT: CH01TOFF0 Mask

Definition at line 7248 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH01TOFF0_Pos

#define PWM_PHCHGNXT_CH01TOFF0_Pos (24)

PWM_T::PHCHGNXT: CH01TOFF0 Position

Definition at line 7247 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH01TOFF1_Msk

#define PWM_PHCHGNXT_CH01TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH01TOFF1_Pos)

PWM_T::PHCHGNXT: CH01TOFF1 Mask

Definition at line 7227 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH01TOFF1_Pos

#define PWM_PHCHGNXT_CH01TOFF1_Pos (16)

PWM_T::PHCHGNXT: CH01TOFF1 Position

Definition at line 7226 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH11TOFF0_Msk

#define PWM_PHCHGNXT_CH11TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH11TOFF0_Pos)

PWM_T::PHCHGNXT: CH11TOFF0 Mask

Definition at line 7251 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH11TOFF0_Pos

#define PWM_PHCHGNXT_CH11TOFF0_Pos (25)

PWM_T::PHCHGNXT: CH11TOFF0 Position

Definition at line 7250 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH11TOFF1_Msk

#define PWM_PHCHGNXT_CH11TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH11TOFF1_Pos)

PWM_T::PHCHGNXT: CH11TOFF1 Mask

Definition at line 7230 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH11TOFF1_Pos

#define PWM_PHCHGNXT_CH11TOFF1_Pos (17)

PWM_T::PHCHGNXT: CH11TOFF1 Position

Definition at line 7229 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH21TOFF0_Msk

#define PWM_PHCHGNXT_CH21TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH21TOFF0_Pos)

PWM_T::PHCHGNXT: CH21TOFF0 Mask

Definition at line 7254 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH21TOFF0_Pos

#define PWM_PHCHGNXT_CH21TOFF0_Pos (26)

PWM_T::PHCHGNXT: CH21TOFF0 Position

Definition at line 7253 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH21TOFF1_Msk

#define PWM_PHCHGNXT_CH21TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH21TOFF1_Pos)

PWM_T::PHCHGNXT: CH21TOFF1 Mask

Definition at line 7233 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH21TOFF1_Pos

#define PWM_PHCHGNXT_CH21TOFF1_Pos (18)

PWM_T::PHCHGNXT: CH21TOFF1 Position

Definition at line 7232 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH31TOFF0_Msk

#define PWM_PHCHGNXT_CH31TOFF0_Msk (0x1ul << PWM_PHCHGNXT_CH31TOFF0_Pos)

PWM_T::PHCHGNXT: CH31TOFF0 Mask

Definition at line 7257 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH31TOFF0_Pos

#define PWM_PHCHGNXT_CH31TOFF0_Pos (27)

PWM_T::PHCHGNXT: CH31TOFF0 Position

Definition at line 7256 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH31TOFF1_Msk

#define PWM_PHCHGNXT_CH31TOFF1_Msk (0x1ul << PWM_PHCHGNXT_CH31TOFF1_Pos)

PWM_T::PHCHGNXT: CH31TOFF1 Mask

Definition at line 7236 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CH31TOFF1_Pos

#define PWM_PHCHGNXT_CH31TOFF1_Pos (19)

PWM_T::PHCHGNXT: CH31TOFF1 Position

Definition at line 7235 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CMP0SEL_Msk

#define PWM_PHCHGNXT_CMP0SEL_Msk (0x3ul << PWM_PHCHGNXT_CMP0SEL_Pos)

PWM_T::PHCHGNXT: CMP0SEL Mask

Definition at line 7260 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CMP0SEL_Pos

#define PWM_PHCHGNXT_CMP0SEL_Pos (28)

PWM_T::PHCHGNXT: CMP0SEL Position

Definition at line 7259 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CMP1SEL_Msk

#define PWM_PHCHGNXT_CMP1SEL_Msk (0x3ul << PWM_PHCHGNXT_CMP1SEL_Pos)

PWM_T::PHCHGNXT: CMP1SEL Mask

Definition at line 7239 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_CMP1SEL_Pos

#define PWM_PHCHGNXT_CMP1SEL_Pos (20)

PWM_T::PHCHGNXT: CMP1SEL Position

Definition at line 7238 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D0_Msk

#define PWM_PHCHGNXT_D0_Msk (0x1ul << PWM_PHCHGNXT_D0_Pos)

PWM_T::PHCHGNXT: D0 Mask

Definition at line 7179 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D0_Pos

#define PWM_PHCHGNXT_D0_Pos (0)

PWM_T::PHCHGNXT: D0 Position

Definition at line 7178 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D1_Msk

#define PWM_PHCHGNXT_D1_Msk (0x1ul << PWM_PHCHGNXT_D1_Pos)

PWM_T::PHCHGNXT: D1 Mask

Definition at line 7182 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D1_Pos

#define PWM_PHCHGNXT_D1_Pos (1)

PWM_T::PHCHGNXT: D1 Position

Definition at line 7181 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D2_Msk

#define PWM_PHCHGNXT_D2_Msk (0x1ul << PWM_PHCHGNXT_D2_Pos)

PWM_T::PHCHGNXT: D2 Mask

Definition at line 7185 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D2_Pos

#define PWM_PHCHGNXT_D2_Pos (2)

PWM_T::PHCHGNXT: D2 Position

Definition at line 7184 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D3_Msk

#define PWM_PHCHGNXT_D3_Msk (0x1ul << PWM_PHCHGNXT_D3_Pos)

PWM_T::PHCHGNXT: D3 Mask

Definition at line 7188 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D3_Pos

#define PWM_PHCHGNXT_D3_Pos (3)

PWM_T::PHCHGNXT: D3 Position

Definition at line 7187 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D4_Msk

#define PWM_PHCHGNXT_D4_Msk (0x1ul << PWM_PHCHGNXT_D4_Pos)

PWM_T::PHCHGNXT: D4 Mask

Definition at line 7191 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D4_Pos

#define PWM_PHCHGNXT_D4_Pos (4)

PWM_T::PHCHGNXT: D4 Position

Definition at line 7190 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D5_Msk

#define PWM_PHCHGNXT_D5_Msk (0x1ul << PWM_PHCHGNXT_D5_Pos)

PWM_T::PHCHGNXT: D5 Mask

Definition at line 7194 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D5_Pos

#define PWM_PHCHGNXT_D5_Pos (5)

PWM_T::PHCHGNXT: D5 Position

Definition at line 7193 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D6_Msk

#define PWM_PHCHGNXT_D6_Msk (0x1ul << PWM_PHCHGNXT_D6_Pos)

PWM_T::PHCHGNXT: D6 Mask

Definition at line 7197 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D6_Pos

#define PWM_PHCHGNXT_D6_Pos (6)

PWM_T::PHCHGNXT: D6 Position

Definition at line 7196 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D7_Msk

#define PWM_PHCHGNXT_D7_Msk (0x1ul << PWM_PHCHGNXT_D7_Pos)

PWM_T::PHCHGNXT: D7 Mask

Definition at line 7200 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_D7_Pos

#define PWM_PHCHGNXT_D7_Pos (7)

PWM_T::PHCHGNXT: D7 Position

Definition at line 7199 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM0_Msk

#define PWM_PHCHGNXT_PWM0_Msk (0x1ul << PWM_PHCHGNXT_PWM0_Pos)

PWM_T::PHCHGNXT: PWM0 Mask

Definition at line 7203 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM0_Pos

#define PWM_PHCHGNXT_PWM0_Pos (8)

PWM_T::PHCHGNXT: PWM0 Position

Definition at line 7202 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM1_Msk

#define PWM_PHCHGNXT_PWM1_Msk (0x1ul << PWM_PHCHGNXT_PWM1_Pos)

PWM_T::PHCHGNXT: PWM1 Mask

Definition at line 7206 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM1_Pos

#define PWM_PHCHGNXT_PWM1_Pos (9)

PWM_T::PHCHGNXT: PWM1 Position

Definition at line 7205 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM2_Msk

#define PWM_PHCHGNXT_PWM2_Msk (0x1ul << PWM_PHCHGNXT_PWM2_Pos)

PWM_T::PHCHGNXT: PWM2 Mask

Definition at line 7209 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM2_Pos

#define PWM_PHCHGNXT_PWM2_Pos (10)

PWM_T::PHCHGNXT: PWM2 Position

Definition at line 7208 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM3_Msk

#define PWM_PHCHGNXT_PWM3_Msk (0x1ul << PWM_PHCHGNXT_PWM3_Pos)

PWM_T::PHCHGNXT: PWM3 Mask

Definition at line 7212 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM3_Pos

#define PWM_PHCHGNXT_PWM3_Pos (11)

PWM_T::PHCHGNXT: PWM3 Position

Definition at line 7211 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM4_Msk

#define PWM_PHCHGNXT_PWM4_Msk (0x1ul << PWM_PHCHGNXT_PWM4_Pos)

PWM_T::PHCHGNXT: PWM4 Mask

Definition at line 7215 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM4_Pos

#define PWM_PHCHGNXT_PWM4_Pos (12)

PWM_T::PHCHGNXT: PWM4 Position

Definition at line 7214 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM5_Msk

#define PWM_PHCHGNXT_PWM5_Msk (0x1ul << PWM_PHCHGNXT_PWM5_Pos)

PWM_T::PHCHGNXT: PWM5 Mask

Definition at line 7218 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_PWM5_Pos

#define PWM_PHCHGNXT_PWM5_Pos (13)

PWM_T::PHCHGNXT: PWM5 Position

Definition at line 7217 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_T0_Msk

#define PWM_PHCHGNXT_T0_Msk (0x1ul << PWM_PHCHGNXT_T0_Pos)

PWM_T::PHCHGNXT: T0 Mask

Definition at line 7263 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_T0_Pos

#define PWM_PHCHGNXT_T0_Pos (30)

PWM_T::PHCHGNXT: T0 Position

Definition at line 7262 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_T1_Msk

#define PWM_PHCHGNXT_T1_Msk (0x1ul << PWM_PHCHGNXT_T1_Pos)

PWM_T::PHCHGNXT: T1 Mask

Definition at line 7242 of file Mini51Series.h.

## ◆ PWM_PHCHGNXT_T1_Pos

#define PWM_PHCHGNXT_T1_Pos (22)

PWM_T::PHCHGNXT: T1 Position

Definition at line 7241 of file Mini51Series.h.

## ◆ PWM_PIER_BRKIE_Msk

#define PWM_PIER_BRKIE_Msk (0x1ul << PWM_PIER_BRKIE_Pos)

PWM_T::PIER: BRKIE Mask

Definition at line 6831 of file Mini51Series.h.

## ◆ PWM_PIER_BRKIE_Pos

#define PWM_PIER_BRKIE_Pos (16)

PWM_T::PIER: BRKIE Position

Definition at line 6830 of file Mini51Series.h.

## ◆ PWM_PIER_INT_TYPE_Msk

#define PWM_PIER_INT_TYPE_Msk (0x1ul << PWM_PIER_INT_TYPE_Pos)

PWM_T::PIER: INT_TYPE Mask

Definition at line 6834 of file Mini51Series.h.

## ◆ PWM_PIER_INT_TYPE_Pos

#define PWM_PIER_INT_TYPE_Pos (17)

PWM_T::PIER: INT_TYPE Position

Definition at line 6833 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE0_Msk

#define PWM_PIER_PWMDIE0_Msk (0x1ul << PWM_PIER_PWMDIE0_Pos)

PWM_T::PIER: PWMDIE0 Mask

Definition at line 6813 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE0_Pos

#define PWM_PIER_PWMDIE0_Pos (8)

PWM_T::PIER: PWMDIE0 Position

Definition at line 6812 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE1_Msk

#define PWM_PIER_PWMDIE1_Msk (0x1ul << PWM_PIER_PWMDIE1_Pos)

PWM_T::PIER: PWMDIE1 Mask

Definition at line 6816 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE1_Pos

#define PWM_PIER_PWMDIE1_Pos (9)

PWM_T::PIER: PWMDIE1 Position

Definition at line 6815 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE2_Msk

#define PWM_PIER_PWMDIE2_Msk (0x1ul << PWM_PIER_PWMDIE2_Pos)

PWM_T::PIER: PWMDIE2 Mask

Definition at line 6819 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE2_Pos

#define PWM_PIER_PWMDIE2_Pos (10)

PWM_T::PIER: PWMDIE2 Position

Definition at line 6818 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE3_Msk

#define PWM_PIER_PWMDIE3_Msk (0x1ul << PWM_PIER_PWMDIE3_Pos)

PWM_T::PIER: PWMDIE3 Mask

Definition at line 6822 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE3_Pos

#define PWM_PIER_PWMDIE3_Pos (11)

PWM_T::PIER: PWMDIE3 Position

Definition at line 6821 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE4_Msk

#define PWM_PIER_PWMDIE4_Msk (0x1ul << PWM_PIER_PWMDIE4_Pos)

PWM_T::PIER: PWMDIE4 Mask

Definition at line 6825 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE4_Pos

#define PWM_PIER_PWMDIE4_Pos (12)

PWM_T::PIER: PWMDIE4 Position

Definition at line 6824 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE5_Msk

#define PWM_PIER_PWMDIE5_Msk (0x1ul << PWM_PIER_PWMDIE5_Pos)

PWM_T::PIER: PWMDIE5 Mask

Definition at line 6828 of file Mini51Series.h.

## ◆ PWM_PIER_PWMDIE5_Pos

#define PWM_PIER_PWMDIE5_Pos (13)

PWM_T::PIER: PWMDIE5 Position

Definition at line 6827 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE0_Msk

#define PWM_PIER_PWMPIE0_Msk (0x1ul << PWM_PIER_PWMPIE0_Pos)

PWM_T::PIER: PWMPIE0 Mask

Definition at line 6795 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE0_Pos

#define PWM_PIER_PWMPIE0_Pos (0)

PWM_T::PIER: PWMPIE0 Position

Definition at line 6794 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE1_Msk

#define PWM_PIER_PWMPIE1_Msk (0x1ul << PWM_PIER_PWMPIE1_Pos)

PWM_T::PIER: PWMPIE1 Mask

Definition at line 6798 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE1_Pos

#define PWM_PIER_PWMPIE1_Pos (1)

PWM_T::PIER: PWMPIE1 Position

Definition at line 6797 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE2_Msk

#define PWM_PIER_PWMPIE2_Msk (0x1ul << PWM_PIER_PWMPIE2_Pos)

PWM_T::PIER: PWMPIE2 Mask

Definition at line 6801 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE2_Pos

#define PWM_PIER_PWMPIE2_Pos (2)

PWM_T::PIER: PWMPIE2 Position

Definition at line 6800 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE3_Msk

#define PWM_PIER_PWMPIE3_Msk (0x1ul << PWM_PIER_PWMPIE3_Pos)

PWM_T::PIER: PWMPIE3 Mask

Definition at line 6804 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE3_Pos

#define PWM_PIER_PWMPIE3_Pos (3)

PWM_T::PIER: PWMPIE3 Position

Definition at line 6803 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE4_Msk

#define PWM_PIER_PWMPIE4_Msk (0x1ul << PWM_PIER_PWMPIE4_Pos)

PWM_T::PIER: PWMPIE4 Mask

Definition at line 6807 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE4_Pos

#define PWM_PIER_PWMPIE4_Pos (4)

PWM_T::PIER: PWMPIE4 Position

Definition at line 6806 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE5_Msk

#define PWM_PIER_PWMPIE5_Msk (0x1ul << PWM_PIER_PWMPIE5_Pos)

PWM_T::PIER: PWMPIE5 Mask

Definition at line 6810 of file Mini51Series.h.

## ◆ PWM_PIER_PWMPIE5_Pos

#define PWM_PIER_PWMPIE5_Pos (5)

PWM_T::PIER: PWMPIE5 Position

Definition at line 6809 of file Mini51Series.h.

## ◆ PWM_PIIR_BKF0_Msk

#define PWM_PIIR_BKF0_Msk (0x1ul << PWM_PIIR_BKF0_Pos)

PWM_T::PIIR: BKF0 Mask

Definition at line 6873 of file Mini51Series.h.

## ◆ PWM_PIIR_BKF0_Pos

#define PWM_PIIR_BKF0_Pos (16)

PWM_T::PIIR: BKF0 Position

Definition at line 6872 of file Mini51Series.h.

## ◆ PWM_PIIR_BKF1_Msk

#define PWM_PIIR_BKF1_Msk (0x1ul << PWM_PIIR_BKF1_Pos)

PWM_T::PIIR: BKF1 Mask

Definition at line 6876 of file Mini51Series.h.

## ◆ PWM_PIIR_BKF1_Pos

#define PWM_PIIR_BKF1_Pos (17)

PWM_T::PIIR: BKF1 Position

Definition at line 6875 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF0_Msk

#define PWM_PIIR_PWMDIF0_Msk (0x1ul << PWM_PIIR_PWMDIF0_Pos)

PWM_T::PIIR: PWMDIF0 Mask

Definition at line 6855 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF0_Pos

#define PWM_PIIR_PWMDIF0_Pos (8)

PWM_T::PIIR: PWMDIF0 Position

Definition at line 6854 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF1_Msk

#define PWM_PIIR_PWMDIF1_Msk (0x1ul << PWM_PIIR_PWMDIF1_Pos)

PWM_T::PIIR: PWMDIF1 Mask

Definition at line 6858 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF1_Pos

#define PWM_PIIR_PWMDIF1_Pos (9)

PWM_T::PIIR: PWMDIF1 Position

Definition at line 6857 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF2_Msk

#define PWM_PIIR_PWMDIF2_Msk (0x1ul << PWM_PIIR_PWMDIF2_Pos)

PWM_T::PIIR: PWMDIF2 Mask

Definition at line 6861 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF2_Pos

#define PWM_PIIR_PWMDIF2_Pos (10)

PWM_T::PIIR: PWMDIF2 Position

Definition at line 6860 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF3_Msk

#define PWM_PIIR_PWMDIF3_Msk (0x1ul << PWM_PIIR_PWMDIF3_Pos)

PWM_T::PIIR: PWMDIF3 Mask

Definition at line 6864 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF3_Pos

#define PWM_PIIR_PWMDIF3_Pos (11)

PWM_T::PIIR: PWMDIF3 Position

Definition at line 6863 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF4_Msk

#define PWM_PIIR_PWMDIF4_Msk (0x1ul << PWM_PIIR_PWMDIF4_Pos)

PWM_T::PIIR: PWMDIF4 Mask

Definition at line 6867 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF4_Pos

#define PWM_PIIR_PWMDIF4_Pos (12)

PWM_T::PIIR: PWMDIF4 Position

Definition at line 6866 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF5_Msk

#define PWM_PIIR_PWMDIF5_Msk (0x1ul << PWM_PIIR_PWMDIF5_Pos)

PWM_T::PIIR: PWMDIF5 Mask

Definition at line 6870 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMDIF5_Pos

#define PWM_PIIR_PWMDIF5_Pos (13)

PWM_T::PIIR: PWMDIF5 Position

Definition at line 6869 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF0_Msk

#define PWM_PIIR_PWMPIF0_Msk (0x1ul << PWM_PIIR_PWMPIF0_Pos)

PWM_T::PIIR: PWMPIF0 Mask

Definition at line 6837 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF0_Pos

#define PWM_PIIR_PWMPIF0_Pos (0)

PWM_T::PIIR: PWMPIF0 Position

Definition at line 6836 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF1_Msk

#define PWM_PIIR_PWMPIF1_Msk (0x1ul << PWM_PIIR_PWMPIF1_Pos)

PWM_T::PIIR: PWMPIF1 Mask

Definition at line 6840 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF1_Pos

#define PWM_PIIR_PWMPIF1_Pos (1)

PWM_T::PIIR: PWMPIF1 Position

Definition at line 6839 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF2_Msk

#define PWM_PIIR_PWMPIF2_Msk (0x1ul << PWM_PIIR_PWMPIF2_Pos)

PWM_T::PIIR: PWMPIF2 Mask

Definition at line 6843 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF2_Pos

#define PWM_PIIR_PWMPIF2_Pos (2)

PWM_T::PIIR: PWMPIF2 Position

Definition at line 6842 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF3_Msk

#define PWM_PIIR_PWMPIF3_Msk (0x1ul << PWM_PIIR_PWMPIF3_Pos)

PWM_T::PIIR: PWMPIF3 Mask

Definition at line 6846 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF3_Pos

#define PWM_PIIR_PWMPIF3_Pos (3)

PWM_T::PIIR: PWMPIF3 Position

Definition at line 6845 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF4_Msk

#define PWM_PIIR_PWMPIF4_Msk (0x1ul << PWM_PIIR_PWMPIF4_Pos)

PWM_T::PIIR: PWMPIF4 Mask

Definition at line 6849 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF4_Pos

#define PWM_PIIR_PWMPIF4_Pos (4)

PWM_T::PIIR: PWMPIF4 Position

Definition at line 6848 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF5_Msk

#define PWM_PIIR_PWMPIF5_Msk (0x1ul << PWM_PIIR_PWMPIF5_Pos)

PWM_T::PIIR: PWMPIF5 Mask

Definition at line 6852 of file Mini51Series.h.

## ◆ PWM_PIIR_PWMPIF5_Pos

#define PWM_PIIR_PWMPIF5_Pos (5)

PWM_T::PIIR: PWMPIF5 Position

Definition at line 6851 of file Mini51Series.h.

## ◆ PWM_POE_PWM0_Msk

#define PWM_POE_PWM0_Msk (0x1ul << PWM_POE_PWM0_Pos)

PWM_T::POE: PWM0 Mask

Definition at line 6879 of file Mini51Series.h.

## ◆ PWM_POE_PWM0_Pos

#define PWM_POE_PWM0_Pos (0)

PWM_T::POE: PWM0 Position

Definition at line 6878 of file Mini51Series.h.

## ◆ PWM_POE_PWM1_Msk

#define PWM_POE_PWM1_Msk (0x1ul << PWM_POE_PWM1_Pos)

PWM_T::POE: PWM1 Mask

Definition at line 6882 of file Mini51Series.h.

## ◆ PWM_POE_PWM1_Pos

#define PWM_POE_PWM1_Pos (1)

PWM_T::POE: PWM1 Position

Definition at line 6881 of file Mini51Series.h.

## ◆ PWM_POE_PWM2_Msk

#define PWM_POE_PWM2_Msk (0x1ul << PWM_POE_PWM2_Pos)

PWM_T::POE: PWM2 Mask

Definition at line 6885 of file Mini51Series.h.

## ◆ PWM_POE_PWM2_Pos

#define PWM_POE_PWM2_Pos (2)

PWM_T::POE: PWM2 Position

Definition at line 6884 of file Mini51Series.h.

## ◆ PWM_POE_PWM3_Msk

#define PWM_POE_PWM3_Msk (0x1ul << PWM_POE_PWM3_Pos)

PWM_T::POE: PWM3 Mask

Definition at line 6888 of file Mini51Series.h.

## ◆ PWM_POE_PWM3_Pos

#define PWM_POE_PWM3_Pos (3)

PWM_T::POE: PWM3 Position

Definition at line 6887 of file Mini51Series.h.

## ◆ PWM_POE_PWM4_Msk

#define PWM_POE_PWM4_Msk (0x1ul << PWM_POE_PWM4_Pos)

PWM_T::POE: PWM4 Mask

Definition at line 6891 of file Mini51Series.h.

## ◆ PWM_POE_PWM4_Pos

#define PWM_POE_PWM4_Pos (4)

PWM_T::POE: PWM4 Position

Definition at line 6890 of file Mini51Series.h.

## ◆ PWM_POE_PWM5_Msk

#define PWM_POE_PWM5_Msk (0x1ul << PWM_POE_PWM5_Pos)

PWM_T::POE: PWM5 Mask

Definition at line 6894 of file Mini51Series.h.

## ◆ PWM_POE_PWM5_Pos

#define PWM_POE_PWM5_Pos (5)

PWM_T::POE: PWM5 Position

Definition at line 6893 of file Mini51Series.h.

## ◆ PWM_PPR_CP01_Msk

#define PWM_PPR_CP01_Msk (0xfful << PWM_PPR_CP01_Pos)

PWM_T::PPR: CP01 Mask

Definition at line 6684 of file Mini51Series.h.

## ◆ PWM_PPR_CP01_Pos

#define PWM_PPR_CP01_Pos (0)

    @addtogroup PWM_CONST PWM Bit Field Definition
    Constant Definitions for PWM Controller

PWM_T::PPR: CP01 Position

Definition at line 6683 of file Mini51Series.h.

## ◆ PWM_PPR_CP23_Msk

#define PWM_PPR_CP23_Msk (0xfful << PWM_PPR_CP23_Pos)

PWM_T::PPR: CP23 Mask

Definition at line 6687 of file Mini51Series.h.

## ◆ PWM_PPR_CP23_Pos

#define PWM_PPR_CP23_Pos (8)

PWM_T::PPR: CP23 Position

Definition at line 6686 of file Mini51Series.h.

## ◆ PWM_PPR_CP45_Msk

#define PWM_PPR_CP45_Msk (0xfful << PWM_PPR_CP45_Pos)

PWM_T::PPR: CP45 Mask

Definition at line 6690 of file Mini51Series.h.

## ◆ PWM_PPR_CP45_Pos

#define PWM_PPR_CP45_Pos (16)

PWM_T::PPR: CP45 Position

Definition at line 6689 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM0TRGFEN_Msk

#define PWM_TRGCON0_CM0TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM0TRGFEN_Pos)

PWM_T::TRGCON0: CM0TRGFEN Mask

Definition at line 6951 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM0TRGFEN_Pos

#define PWM_TRGCON0_CM0TRGFEN_Pos (2)

PWM_T::TRGCON0: CM0TRGFEN Position

Definition at line 6950 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM0TRGREN_Msk

#define PWM_TRGCON0_CM0TRGREN_Msk (0x1ul << PWM_TRGCON0_CM0TRGREN_Pos)

PWM_T::TRGCON0: CM0TRGREN Mask

Definition at line 6945 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM0TRGREN_Pos

#define PWM_TRGCON0_CM0TRGREN_Pos (0)

PWM_T::TRGCON0: CM0TRGREN Position

Definition at line 6944 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM1TRGFEN_Msk

#define PWM_TRGCON0_CM1TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM1TRGFEN_Pos)

PWM_T::TRGCON0: CM1TRGFEN Mask

Definition at line 6963 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM1TRGFEN_Pos

#define PWM_TRGCON0_CM1TRGFEN_Pos (10)

PWM_T::TRGCON0: CM1TRGFEN Position

Definition at line 6962 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM1TRGREN_Msk

#define PWM_TRGCON0_CM1TRGREN_Msk (0x1ul << PWM_TRGCON0_CM1TRGREN_Pos)

PWM_T::TRGCON0: CM1TRGREN Mask

Definition at line 6957 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM1TRGREN_Pos

#define PWM_TRGCON0_CM1TRGREN_Pos (8)

PWM_T::TRGCON0: CM1TRGREN Position

Definition at line 6956 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM2TRGFEN_Msk

#define PWM_TRGCON0_CM2TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM2TRGFEN_Pos)

PWM_T::TRGCON0: CM2TRGFEN Mask

Definition at line 6975 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM2TRGFEN_Pos

#define PWM_TRGCON0_CM2TRGFEN_Pos (18)

PWM_T::TRGCON0: CM2TRGFEN Position

Definition at line 6974 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM2TRGREN_Msk

#define PWM_TRGCON0_CM2TRGREN_Msk (0x1ul << PWM_TRGCON0_CM2TRGREN_Pos)

PWM_T::TRGCON0: CM2TRGREN Mask

Definition at line 6969 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM2TRGREN_Pos

#define PWM_TRGCON0_CM2TRGREN_Pos (16)

PWM_T::TRGCON0: CM2TRGREN Position

Definition at line 6968 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM3TRGFEN_Msk

#define PWM_TRGCON0_CM3TRGFEN_Msk (0x1ul << PWM_TRGCON0_CM3TRGFEN_Pos)

PWM_T::TRGCON0: CM3TRGFEN Mask

Definition at line 6987 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM3TRGFEN_Pos

#define PWM_TRGCON0_CM3TRGFEN_Pos (26)

PWM_T::TRGCON0: CM3TRGFEN Position

Definition at line 6986 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM3TRGREN_Msk

#define PWM_TRGCON0_CM3TRGREN_Msk (0x1ul << PWM_TRGCON0_CM3TRGREN_Pos)

PWM_T::TRGCON0: CM3TRGREN Mask

Definition at line 6981 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CM3TRGREN_Pos

#define PWM_TRGCON0_CM3TRGREN_Pos (24)

PWM_T::TRGCON0: CM3TRGREN Position

Definition at line 6980 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT0TRGEN_Msk

#define PWM_TRGCON0_CNT0TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT0TRGEN_Pos)

PWM_T::TRGCON0: CNT0TRGEN Mask

Definition at line 6948 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT0TRGEN_Pos

#define PWM_TRGCON0_CNT0TRGEN_Pos (1)

PWM_T::TRGCON0: CNT0TRGEN Position

Definition at line 6947 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT1TRGEN_Msk

#define PWM_TRGCON0_CNT1TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT1TRGEN_Pos)

PWM_T::TRGCON0: CNT1TRGEN Mask

Definition at line 6960 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT1TRGEN_Pos

#define PWM_TRGCON0_CNT1TRGEN_Pos (9)

PWM_T::TRGCON0: CNT1TRGEN Position

Definition at line 6959 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT2TRGEN_Msk

#define PWM_TRGCON0_CNT2TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT2TRGEN_Pos)

PWM_T::TRGCON0: CNT2TRGEN Mask

Definition at line 6972 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT2TRGEN_Pos

#define PWM_TRGCON0_CNT2TRGEN_Pos (17)

PWM_T::TRGCON0: CNT2TRGEN Position

Definition at line 6971 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT3TRGEN_Msk

#define PWM_TRGCON0_CNT3TRGEN_Msk (0x1ul << PWM_TRGCON0_CNT3TRGEN_Pos)

PWM_T::TRGCON0: CNT3TRGEN Mask

Definition at line 6984 of file Mini51Series.h.

## ◆ PWM_TRGCON0_CNT3TRGEN_Pos

#define PWM_TRGCON0_CNT3TRGEN_Pos (25)

PWM_T::TRGCON0: CNT3TRGEN Position

Definition at line 6983 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P0TRGEN_Msk

#define PWM_TRGCON0_P0TRGEN_Msk (0x1ul << PWM_TRGCON0_P0TRGEN_Pos)

PWM_T::TRGCON0: P0TRGEN Mask

Definition at line 6954 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P0TRGEN_Pos

#define PWM_TRGCON0_P0TRGEN_Pos (3)

PWM_T::TRGCON0: P0TRGEN Position

Definition at line 6953 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P1TRGEN_Msk

#define PWM_TRGCON0_P1TRGEN_Msk (0x1ul << PWM_TRGCON0_P1TRGEN_Pos)

PWM_T::TRGCON0: P1TRGEN Mask

Definition at line 6966 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P1TRGEN_Pos

#define PWM_TRGCON0_P1TRGEN_Pos (11)

PWM_T::TRGCON0: P1TRGEN Position

Definition at line 6965 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P2TRGEN_Msk

#define PWM_TRGCON0_P2TRGEN_Msk (0x1ul << PWM_TRGCON0_P2TRGEN_Pos)

PWM_T::TRGCON0: P2TRGEN Mask

Definition at line 6978 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P2TRGEN_Pos

#define PWM_TRGCON0_P2TRGEN_Pos (19)

PWM_T::TRGCON0: P2TRGEN Position

Definition at line 6977 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P3TRGEN_Msk

#define PWM_TRGCON0_P3TRGEN_Msk (0x1ul << PWM_TRGCON0_P3TRGEN_Pos)

PWM_T::TRGCON0: P3TRGEN Mask

Definition at line 6990 of file Mini51Series.h.

## ◆ PWM_TRGCON0_P3TRGEN_Pos

#define PWM_TRGCON0_P3TRGEN_Pos (27)

PWM_T::TRGCON0: P3TRGEN Position

Definition at line 6989 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM4TRGFEN_Msk

#define PWM_TRGCON1_CM4TRGFEN_Msk (0x1ul << PWM_TRGCON1_CM4TRGFEN_Pos)

PWM_T::TRGCON1: CM4TRGFEN Mask

Definition at line 6999 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM4TRGFEN_Pos

#define PWM_TRGCON1_CM4TRGFEN_Pos (2)

PWM_T::TRGCON1: CM4TRGFEN Position

Definition at line 6998 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM4TRGREN_Msk

#define PWM_TRGCON1_CM4TRGREN_Msk (0x1ul << PWM_TRGCON1_CM4TRGREN_Pos)

PWM_T::TRGCON1: CM4TRGREN Mask

Definition at line 6993 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM4TRGREN_Pos

#define PWM_TRGCON1_CM4TRGREN_Pos (0)

PWM_T::TRGCON1: CM4TRGREN Position

Definition at line 6992 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM5TRGFEN_Msk

#define PWM_TRGCON1_CM5TRGFEN_Msk (0x1ul << PWM_TRGCON1_CM5TRGFEN_Pos)

PWM_T::TRGCON1: CM5TRGFEN Mask

Definition at line 7011 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM5TRGFEN_Pos

#define PWM_TRGCON1_CM5TRGFEN_Pos (10)

PWM_T::TRGCON1: CM5TRGFEN Position

Definition at line 7010 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM5TRGREN_Msk

#define PWM_TRGCON1_CM5TRGREN_Msk (0x1ul << PWM_TRGCON1_CM5TRGREN_Pos)

PWM_T::TRGCON1: CM5TRGREN Mask

Definition at line 7005 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CM5TRGREN_Pos

#define PWM_TRGCON1_CM5TRGREN_Pos (8)

PWM_T::TRGCON1: CM5TRGREN Position

Definition at line 7004 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CNT4TRGEN_Msk

#define PWM_TRGCON1_CNT4TRGEN_Msk (0x1ul << PWM_TRGCON1_CNT4TRGEN_Pos)

PWM_T::TRGCON1: CNT4TRGEN Mask

Definition at line 6996 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CNT4TRGEN_Pos

#define PWM_TRGCON1_CNT4TRGEN_Pos (1)

PWM_T::TRGCON1: CNT4TRGEN Position

Definition at line 6995 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CNT5TRGEN_Msk

#define PWM_TRGCON1_CNT5TRGEN_Msk (0x1ul << PWM_TRGCON1_CNT5TRGEN_Pos)

PWM_T::TRGCON1: CNT5TRGEN Mask

Definition at line 7008 of file Mini51Series.h.

## ◆ PWM_TRGCON1_CNT5TRGEN_Pos

#define PWM_TRGCON1_CNT5TRGEN_Pos (9)

PWM_T::TRGCON1: CNT5TRGEN Position

Definition at line 7007 of file Mini51Series.h.

## ◆ PWM_TRGCON1_P4TRGEN_Msk

#define PWM_TRGCON1_P4TRGEN_Msk (0x1ul << PWM_TRGCON1_P4TRGEN_Pos)

PWM_T::TRGCON1: P4TRGEN Mask

Definition at line 7002 of file Mini51Series.h.

## ◆ PWM_TRGCON1_P4TRGEN_Pos

#define PWM_TRGCON1_P4TRGEN_Pos (3)

PWM_T::TRGCON1: P4TRGEN Position

Definition at line 7001 of file Mini51Series.h.

## ◆ PWM_TRGCON1_P5TRGEN_Msk

#define PWM_TRGCON1_P5TRGEN_Msk (0x1ul << PWM_TRGCON1_P5TRGEN_Pos)

PWM_T::TRGCON1: P5TRGEN Mask

Definition at line 7014 of file Mini51Series.h.

## ◆ PWM_TRGCON1_P5TRGEN_Pos

#define PWM_TRGCON1_P5TRGEN_Pos (11)

PWM_T::TRGCON1: P5TRGEN Position

Definition at line 7013 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR0FLAG_F_Msk

#define PWM_TRGSTS0_CMR0FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR0FLAG_F_Pos)

PWM_T::TRGSTS0: CMR0FLAG_F Mask

Definition at line 7023 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR0FLAG_F_Pos

#define PWM_TRGSTS0_CMR0FLAG_F_Pos (2)

PWM_T::TRGSTS0: CMR0FLAG_F Position

Definition at line 7022 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR0FLAG_R_Msk

#define PWM_TRGSTS0_CMR0FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR0FLAG_R_Pos)

PWM_T::TRGSTS0: CMR0FLAG_R Mask

Definition at line 7017 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR0FLAG_R_Pos

#define PWM_TRGSTS0_CMR0FLAG_R_Pos (0)

PWM_T::TRGSTS0: CMR0FLAG_R Position

Definition at line 7016 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR1FLAG_F_Msk

#define PWM_TRGSTS0_CMR1FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR1FLAG_F_Pos)

PWM_T::TRGSTS0: CMR1FLAG_F Mask

Definition at line 7035 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR1FLAG_F_Pos

#define PWM_TRGSTS0_CMR1FLAG_F_Pos (10)

PWM_T::TRGSTS0: CMR1FLAG_F Position

Definition at line 7034 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR1FLAG_R_Msk

#define PWM_TRGSTS0_CMR1FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR1FLAG_R_Pos)

PWM_T::TRGSTS0: CMR1FLAG_R Mask

Definition at line 7029 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR1FLAG_R_Pos

#define PWM_TRGSTS0_CMR1FLAG_R_Pos (8)

PWM_T::TRGSTS0: CMR1FLAG_R Position

Definition at line 7028 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR2FLAG_F_Msk

#define PWM_TRGSTS0_CMR2FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR2FLAG_F_Pos)

PWM_T::TRGSTS0: CMR2FLAG_F Mask

Definition at line 7047 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR2FLAG_F_Pos

#define PWM_TRGSTS0_CMR2FLAG_F_Pos (18)

PWM_T::TRGSTS0: CMR2FLAG_F Position

Definition at line 7046 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR2FLAG_R_Msk

#define PWM_TRGSTS0_CMR2FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR2FLAG_R_Pos)

PWM_T::TRGSTS0: CMR2FLAG_R Mask

Definition at line 7041 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR2FLAG_R_Pos

#define PWM_TRGSTS0_CMR2FLAG_R_Pos (16)

PWM_T::TRGSTS0: CMR2FLAG_R Position

Definition at line 7040 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR3FLAG_F_Msk

#define PWM_TRGSTS0_CMR3FLAG_F_Msk (0x1ul << PWM_TRGSTS0_CMR3FLAG_F_Pos)

PWM_T::TRGSTS0: CMR3FLAG_F Mask

Definition at line 7059 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR3FLAG_F_Pos

#define PWM_TRGSTS0_CMR3FLAG_F_Pos (26)

PWM_T::TRGSTS0: CMR3FLAG_F Position

Definition at line 7058 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR3FLAG_R_Msk

#define PWM_TRGSTS0_CMR3FLAG_R_Msk (0x1ul << PWM_TRGSTS0_CMR3FLAG_R_Pos)

PWM_T::TRGSTS0: CMR3FLAG_R Mask

Definition at line 7053 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CMR3FLAG_R_Pos

#define PWM_TRGSTS0_CMR3FLAG_R_Pos (24)

PWM_T::TRGSTS0: CMR3FLAG_R Position

Definition at line 7052 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT0FLAG_Msk

#define PWM_TRGSTS0_CNT0FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT0FLAG_Pos)

PWM_T::TRGSTS0: CNT0FLAG Mask

Definition at line 7020 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT0FLAG_Pos

#define PWM_TRGSTS0_CNT0FLAG_Pos (1)

PWM_T::TRGSTS0: CNT0FLAG Position

Definition at line 7019 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT1FLAG_Msk

#define PWM_TRGSTS0_CNT1FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT1FLAG_Pos)

PWM_T::TRGSTS0: CNT1FLAG Mask

Definition at line 7032 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT1FLAG_Pos

#define PWM_TRGSTS0_CNT1FLAG_Pos (9)

PWM_T::TRGSTS0: CNT1FLAG Position

Definition at line 7031 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT2FLAG_Msk

#define PWM_TRGSTS0_CNT2FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT2FLAG_Pos)

PWM_T::TRGSTS0: CNT2FLAG Mask

Definition at line 7044 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT2FLAG_Pos

#define PWM_TRGSTS0_CNT2FLAG_Pos (17)

PWM_T::TRGSTS0: CNT2FLAG Position

Definition at line 7043 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT3FLAG_Msk

#define PWM_TRGSTS0_CNT3FLAG_Msk (0x1ul << PWM_TRGSTS0_CNT3FLAG_Pos)

PWM_T::TRGSTS0: CNT3FLAG Mask

Definition at line 7056 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_CNT3FLAG_Pos

#define PWM_TRGSTS0_CNT3FLAG_Pos (25)

PWM_T::TRGSTS0: CNT3FLAG Position

Definition at line 7055 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID0FLAG_Msk

#define PWM_TRGSTS0_PERID0FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID0FLAG_Pos)

PWM_T::TRGSTS0: PERID0FLAG Mask

Definition at line 7026 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID0FLAG_Pos

#define PWM_TRGSTS0_PERID0FLAG_Pos (3)

PWM_T::TRGSTS0: PERID0FLAG Position

Definition at line 7025 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID1FLAG_Msk

#define PWM_TRGSTS0_PERID1FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID1FLAG_Pos)

PWM_T::TRGSTS0: PERID1FLAG Mask

Definition at line 7038 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID1FLAG_Pos

#define PWM_TRGSTS0_PERID1FLAG_Pos (11)

PWM_T::TRGSTS0: PERID1FLAG Position

Definition at line 7037 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID2FLAG_Msk

#define PWM_TRGSTS0_PERID2FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID2FLAG_Pos)

PWM_T::TRGSTS0: PERID2FLAG Mask

Definition at line 7050 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID2FLAG_Pos

#define PWM_TRGSTS0_PERID2FLAG_Pos (19)

PWM_T::TRGSTS0: PERID2FLAG Position

Definition at line 7049 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID3FLAG_Msk

#define PWM_TRGSTS0_PERID3FLAG_Msk (0x1ul << PWM_TRGSTS0_PERID3FLAG_Pos)

PWM_T::TRGSTS0: PERID3FLAG Mask

Definition at line 7062 of file Mini51Series.h.

## ◆ PWM_TRGSTS0_PERID3FLAG_Pos

#define PWM_TRGSTS0_PERID3FLAG_Pos (27)

PWM_T::TRGSTS0: PERID3FLAG Position

Definition at line 7061 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR4FLAG_F_Msk

#define PWM_TRGSTS1_CMR4FLAG_F_Msk (0x1ul << PWM_TRGSTS1_CMR4FLAG_F_Pos)

PWM_T::TRGSTS1: CMR4FLAG_F Mask

Definition at line 7071 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR4FLAG_F_Pos

#define PWM_TRGSTS1_CMR4FLAG_F_Pos (2)

PWM_T::TRGSTS1: CMR4FLAG_F Position

Definition at line 7070 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR4FLAG_R_Msk

#define PWM_TRGSTS1_CMR4FLAG_R_Msk (0x1ul << PWM_TRGSTS1_CMR4FLAG_R_Pos)

PWM_T::TRGSTS1: CMR4FLAG_R Mask

Definition at line 7065 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR4FLAG_R_Pos

#define PWM_TRGSTS1_CMR4FLAG_R_Pos (0)

PWM_T::TRGSTS1: CMR4FLAG_R Position

Definition at line 7064 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR5FLAG_F_Msk

#define PWM_TRGSTS1_CMR5FLAG_F_Msk (0x1ul << PWM_TRGSTS1_CMR5FLAG_F_Pos)

PWM_T::TRGSTS1: CMR5FLAG_F Mask

Definition at line 7083 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR5FLAG_F_Pos

#define PWM_TRGSTS1_CMR5FLAG_F_Pos (10)

PWM_T::TRGSTS1: CMR5FLAG_F Position

Definition at line 7082 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR5FLAG_R_Msk

#define PWM_TRGSTS1_CMR5FLAG_R_Msk (0x1ul << PWM_TRGSTS1_CMR5FLAG_R_Pos)

PWM_T::TRGSTS1: CMR5FLAG_R Mask

Definition at line 7077 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CMR5FLAG_R_Pos

#define PWM_TRGSTS1_CMR5FLAG_R_Pos (8)

PWM_T::TRGSTS1: CMR5FLAG_R Position

Definition at line 7076 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CNT4FLAG_Msk

#define PWM_TRGSTS1_CNT4FLAG_Msk (0x1ul << PWM_TRGSTS1_CNT4FLAG_Pos)

PWM_T::TRGSTS1: CNT4FLAG Mask

Definition at line 7068 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CNT4FLAG_Pos

#define PWM_TRGSTS1_CNT4FLAG_Pos (1)

PWM_T::TRGSTS1: CNT4FLAG Position

Definition at line 7067 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CNT5FLAG_Msk

#define PWM_TRGSTS1_CNT5FLAG_Msk (0x1ul << PWM_TRGSTS1_CNT5FLAG_Pos)

PWM_T::TRGSTS1: CNT5FLAG Mask

Definition at line 7080 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_CNT5FLAG_Pos

#define PWM_TRGSTS1_CNT5FLAG_Pos (9)

PWM_T::TRGSTS1: CNT5FLAG Position

Definition at line 7079 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_PERID4FLAG_Msk

#define PWM_TRGSTS1_PERID4FLAG_Msk (0x1ul << PWM_TRGSTS1_PERID4FLAG_Pos)

PWM_T::TRGSTS1: PERID4FLAG Mask

Definition at line 7074 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_PERID4FLAG_Pos

#define PWM_TRGSTS1_PERID4FLAG_Pos (3)

PWM_T::TRGSTS1: PERID4FLAG Position

Definition at line 7073 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_PERID5FLAG_Msk

#define PWM_TRGSTS1_PERID5FLAG_Msk (0x1ul << PWM_TRGSTS1_PERID5FLAG_Pos)

PWM_T::TRGSTS1: PERID5FLAG Mask

Definition at line 7086 of file Mini51Series.h.

## ◆ PWM_TRGSTS1_PERID5FLAG_Pos

#define PWM_TRGSTS1_PERID5FLAG_Pos (11)

PWM_T::TRGSTS1: PERID5FLAG Position

Definition at line 7085 of file Mini51Series.h.

## ◆ SPI_CNTRL2_BCn_Msk

#define SPI_CNTRL2_BCn_Msk (0x1ul << SPI_CNTRL2_BCn_Pos)

SPI_T::CNTRL2: BCn Mask

Definition at line 8024 of file Mini51Series.h.

## ◆ SPI_CNTRL2_BCn_Pos

#define SPI_CNTRL2_BCn_Pos (31)

SPI_T::CNTRL2: BCn Position

Definition at line 8023 of file Mini51Series.h.

## ◆ SPI_CNTRL2_NOSLVSEL_Msk

#define SPI_CNTRL2_NOSLVSEL_Msk (0x1ul << SPI_CNTRL2_NOSLVSEL_Pos)

SPI_T::CNTRL2: NOSLVSEL Mask

Definition at line 8009 of file Mini51Series.h.

## ◆ SPI_CNTRL2_NOSLVSEL_Pos

#define SPI_CNTRL2_NOSLVSEL_Pos (8)

SPI_T::CNTRL2: NOSLVSEL Position

Definition at line 8008 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SLV_ABORT_Msk

#define SPI_CNTRL2_SLV_ABORT_Msk (0x1ul << SPI_CNTRL2_SLV_ABORT_Pos)

SPI_T::CNTRL2: SLV_ABORT Mask

Definition at line 8012 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SLV_ABORT_Pos

#define SPI_CNTRL2_SLV_ABORT_Pos (9)

SPI_T::CNTRL2: SLV_ABORT Position

Definition at line 8011 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SLV_START_INTSTS_Msk

#define SPI_CNTRL2_SLV_START_INTSTS_Msk (0x1ul << SPI_CNTRL2_SLV_START_INTSTS_Pos)

SPI_T::CNTRL2: SLV_START_INTSTS Mask

Definition at line 8018 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SLV_START_INTSTS_Pos

#define SPI_CNTRL2_SLV_START_INTSTS_Pos (11)

SPI_T::CNTRL2: SLV_START_INTSTS Position

Definition at line 8017 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SS_INT_OPT_Msk

#define SPI_CNTRL2_SS_INT_OPT_Msk (0x1ul << SPI_CNTRL2_SS_INT_OPT_Pos)

SPI_T::CNTRL2: SS_INT_OPT Mask

Definition at line 8021 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SS_INT_OPT_Pos

#define SPI_CNTRL2_SS_INT_OPT_Pos (16)

SPI_T::CNTRL2: SS_INT_OPT Position

Definition at line 8020 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SSTA_INTEN_Msk

#define SPI_CNTRL2_SSTA_INTEN_Msk (0x1ul << SPI_CNTRL2_SSTA_INTEN_Pos)

SPI_T::CNTRL2: SSTA_INTEN Mask

Definition at line 8015 of file Mini51Series.h.

## ◆ SPI_CNTRL2_SSTA_INTEN_Pos

#define SPI_CNTRL2_SSTA_INTEN_Pos (10)

SPI_T::CNTRL2: SSTA_INTEN Position

Definition at line 8014 of file Mini51Series.h.

## ◆ SPI_CNTRL_CLKP_Msk

#define SPI_CNTRL_CLKP_Msk (0x1ul << SPI_CNTRL_CLKP_Pos)

SPI_T::CNTRL: CLKP Mask

Definition at line 7952 of file Mini51Series.h.

## ◆ SPI_CNTRL_CLKP_Pos

#define SPI_CNTRL_CLKP_Pos (11)

SPI_T::CNTRL: CLKP Position

Definition at line 7951 of file Mini51Series.h.

## ◆ SPI_CNTRL_FIFO_Msk

#define SPI_CNTRL_FIFO_Msk (0x1ul << SPI_CNTRL_FIFO_Pos)

SPI_T::CNTRL: FIFO Mask

Definition at line 7970 of file Mini51Series.h.

## ◆ SPI_CNTRL_FIFO_Pos

#define SPI_CNTRL_FIFO_Pos (21)

SPI_T::CNTRL: FIFO Position

Definition at line 7969 of file Mini51Series.h.

## ◆ SPI_CNTRL_GO_BUSY_Msk

#define SPI_CNTRL_GO_BUSY_Msk (0x1ul << SPI_CNTRL_GO_BUSY_Pos)

SPI_T::CNTRL: GO_BUSY Mask

Definition at line 7937 of file Mini51Series.h.

## ◆ SPI_CNTRL_GO_BUSY_Pos

#define SPI_CNTRL_GO_BUSY_Pos (0)

    @addtogroup SPI_CONST SPI Bit Field Definition
    Constant Definitions for SPI Controller

SPI_T::CNTRL: GO_BUSY Position

Definition at line 7936 of file Mini51Series.h.

## ◆ SPI_CNTRL_IE_Msk

#define SPI_CNTRL_IE_Msk (0x1ul << SPI_CNTRL_IE_Pos)

SPI_T::CNTRL: IE Mask

Definition at line 7961 of file Mini51Series.h.

## ◆ SPI_CNTRL_IE_Pos

#define SPI_CNTRL_IE_Pos (17)

SPI_T::CNTRL: IE Position

Definition at line 7960 of file Mini51Series.h.

## ◆ SPI_CNTRL_IF_Msk

#define SPI_CNTRL_IF_Msk (0x1ul << SPI_CNTRL_IF_Pos)

SPI_T::CNTRL: IF Mask

Definition at line 7958 of file Mini51Series.h.

## ◆ SPI_CNTRL_IF_Pos

#define SPI_CNTRL_IF_Pos (16)

SPI_T::CNTRL: IF Position

Definition at line 7957 of file Mini51Series.h.

## ◆ SPI_CNTRL_LSB_Msk

#define SPI_CNTRL_LSB_Msk (0x1ul << SPI_CNTRL_LSB_Pos)

SPI_T::CNTRL: LSB Mask

Definition at line 7949 of file Mini51Series.h.

## ◆ SPI_CNTRL_LSB_Pos

#define SPI_CNTRL_LSB_Pos (10)

SPI_T::CNTRL: LSB Position

Definition at line 7948 of file Mini51Series.h.

## ◆ SPI_CNTRL_REORDER_Msk

#define SPI_CNTRL_REORDER_Msk (0x1ul << SPI_CNTRL_REORDER_Pos)

SPI_T::CNTRL: REORDER Mask

Definition at line 7967 of file Mini51Series.h.

## ◆ SPI_CNTRL_REORDER_Pos

#define SPI_CNTRL_REORDER_Pos (19)

SPI_T::CNTRL: REORDER Position

Definition at line 7966 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_EMPTY_Msk

#define SPI_CNTRL_RX_EMPTY_Msk (0x1ul << SPI_CNTRL_RX_EMPTY_Pos)

SPI_T::CNTRL: RX_EMPTY Mask

Definition at line 7973 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_EMPTY_Pos

#define SPI_CNTRL_RX_EMPTY_Pos (24)

SPI_T::CNTRL: RX_EMPTY Position

Definition at line 7972 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_FULL_Msk

#define SPI_CNTRL_RX_FULL_Msk (0x1ul << SPI_CNTRL_RX_FULL_Pos)

SPI_T::CNTRL: RX_FULL Mask

Definition at line 7976 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_FULL_Pos

#define SPI_CNTRL_RX_FULL_Pos (25)

SPI_T::CNTRL: RX_FULL Position

Definition at line 7975 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_NEG_Msk

#define SPI_CNTRL_RX_NEG_Msk (0x1ul << SPI_CNTRL_RX_NEG_Pos)

SPI_T::CNTRL: RX_NEG Mask

Definition at line 7940 of file Mini51Series.h.

## ◆ SPI_CNTRL_RX_NEG_Pos

#define SPI_CNTRL_RX_NEG_Pos (1)

SPI_T::CNTRL: RX_NEG Position

Definition at line 7939 of file Mini51Series.h.

## ◆ SPI_CNTRL_SLAVE_Msk

#define SPI_CNTRL_SLAVE_Msk (0x1ul << SPI_CNTRL_SLAVE_Pos)

SPI_T::CNTRL: SLAVE Mask

Definition at line 7964 of file Mini51Series.h.

## ◆ SPI_CNTRL_SLAVE_Pos

#define SPI_CNTRL_SLAVE_Pos (18)

SPI_T::CNTRL: SLAVE Position

Definition at line 7963 of file Mini51Series.h.

## ◆ SPI_CNTRL_SP_CYCLE_Msk

#define SPI_CNTRL_SP_CYCLE_Msk (0xful << SPI_CNTRL_SP_CYCLE_Pos)

SPI_T::CNTRL: SP_CYCLE Mask

Definition at line 7955 of file Mini51Series.h.

## ◆ SPI_CNTRL_SP_CYCLE_Pos

#define SPI_CNTRL_SP_CYCLE_Pos (12)

SPI_T::CNTRL: SP_CYCLE Position

Definition at line 7954 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_BIT_LEN_Msk

#define SPI_CNTRL_TX_BIT_LEN_Msk (0x1ful << SPI_CNTRL_TX_BIT_LEN_Pos)

SPI_T::CNTRL: TX_BIT_LEN Mask

Definition at line 7946 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_BIT_LEN_Pos

#define SPI_CNTRL_TX_BIT_LEN_Pos (3)

SPI_T::CNTRL: TX_BIT_LEN Position

Definition at line 7945 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_EMPTY_Msk

#define SPI_CNTRL_TX_EMPTY_Msk (0x1ul << SPI_CNTRL_TX_EMPTY_Pos)

SPI_T::CNTRL: TX_EMPTY Mask

Definition at line 7979 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_EMPTY_Pos

#define SPI_CNTRL_TX_EMPTY_Pos (26)

SPI_T::CNTRL: TX_EMPTY Position

Definition at line 7978 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_FULL_Msk

#define SPI_CNTRL_TX_FULL_Msk (0x1ul << SPI_CNTRL_TX_FULL_Pos)

SPI_T::CNTRL: TX_FULL Mask

Definition at line 7982 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_FULL_Pos

#define SPI_CNTRL_TX_FULL_Pos (27)

SPI_T::CNTRL: TX_FULL Position

Definition at line 7981 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_NEG_Msk

#define SPI_CNTRL_TX_NEG_Msk (0x1ul << SPI_CNTRL_TX_NEG_Pos)

SPI_T::CNTRL: TX_NEG Mask

Definition at line 7943 of file Mini51Series.h.

## ◆ SPI_CNTRL_TX_NEG_Pos

#define SPI_CNTRL_TX_NEG_Pos (2)

SPI_T::CNTRL: TX_NEG Position

Definition at line 7942 of file Mini51Series.h.

## ◆ SPI_DIVIDER_DIVIDER_Msk

#define SPI_DIVIDER_DIVIDER_Msk (0xfful << SPI_DIVIDER_DIVIDER_Pos)

SPI_T::DIVIDER: DIVIDER Mask

Definition at line 7985 of file Mini51Series.h.

## ◆ SPI_DIVIDER_DIVIDER_Pos

#define SPI_DIVIDER_DIVIDER_Pos (0)

SPI_T::DIVIDER: DIVIDER Position

Definition at line 7984 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_CLR_Msk

#define SPI_FIFO_CTL_RX_CLR_Msk (0x1ul << SPI_FIFO_CTL_RX_CLR_Pos)

SPI_T::FIFO_CTL: RX_CLR Mask

Definition at line 8027 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_CLR_Pos

#define SPI_FIFO_CTL_RX_CLR_Pos (0)

SPI_T::FIFO_CTL: RX_CLR Position

Definition at line 8026 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_INTEN_Msk

#define SPI_FIFO_CTL_RX_INTEN_Msk (0x1ul << SPI_FIFO_CTL_RX_INTEN_Pos)

SPI_T::FIFO_CTL: RX_INTEN Mask

Definition at line 8033 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_INTEN_Pos

#define SPI_FIFO_CTL_RX_INTEN_Pos (2)

SPI_T::FIFO_CTL: RX_INTEN Position

Definition at line 8032 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_THRESHOLD_Msk

#define SPI_FIFO_CTL_RX_THRESHOLD_Msk (0x3ul << SPI_FIFO_CTL_RX_THRESHOLD_Pos)

SPI_T::FIFO_CTL: RX_THRESHOLD Mask

Definition at line 8045 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RX_THRESHOLD_Pos

#define SPI_FIFO_CTL_RX_THRESHOLD_Pos (24)

SPI_T::FIFO_CTL: RX_THRESHOLD Position

Definition at line 8044 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RXOV_INTEN_Msk

#define SPI_FIFO_CTL_RXOV_INTEN_Msk (0x1ul << SPI_FIFO_CTL_RXOV_INTEN_Pos)

SPI_T::FIFO_CTL: RXOV_INTEN Mask

Definition at line 8039 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_RXOV_INTEN_Pos

#define SPI_FIFO_CTL_RXOV_INTEN_Pos (6)

SPI_T::FIFO_CTL: RXOV_INTEN Position

Definition at line 8038 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TIMEOUT_INTEN_Msk

#define SPI_FIFO_CTL_TIMEOUT_INTEN_Msk (0x1ul << SPI_FIFO_CTL_TIMEOUT_INTEN_Pos)

SPI_T::FIFO_CTL: TIMEOUT_INTEN Mask

Definition at line 8042 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TIMEOUT_INTEN_Pos

#define SPI_FIFO_CTL_TIMEOUT_INTEN_Pos (21)

SPI_T::FIFO_CTL: TIMEOUT_INTEN Position

Definition at line 8041 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_CLR_Msk

#define SPI_FIFO_CTL_TX_CLR_Msk (0x1ul << SPI_FIFO_CTL_TX_CLR_Pos)

SPI_T::FIFO_CTL: TX_CLR Mask

Definition at line 8030 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_CLR_Pos

#define SPI_FIFO_CTL_TX_CLR_Pos (1)

SPI_T::FIFO_CTL: TX_CLR Position

Definition at line 8029 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_INTEN_Msk

#define SPI_FIFO_CTL_TX_INTEN_Msk (0x1ul << SPI_FIFO_CTL_TX_INTEN_Pos)

SPI_T::FIFO_CTL: TX_INTEN Mask

Definition at line 8036 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_INTEN_Pos

#define SPI_FIFO_CTL_TX_INTEN_Pos (3)

SPI_T::FIFO_CTL: TX_INTEN Position

Definition at line 8035 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_THRESHOLD_Msk

#define SPI_FIFO_CTL_TX_THRESHOLD_Msk (0x3ul << SPI_FIFO_CTL_TX_THRESHOLD_Pos)

SPI_T::FIFO_CTL: TX_THRESHOLD Mask

Definition at line 8048 of file Mini51Series.h.

## ◆ SPI_FIFO_CTL_TX_THRESHOLD_Pos

#define SPI_FIFO_CTL_TX_THRESHOLD_Pos (28)

SPI_T::FIFO_CTL: TX_THRESHOLD Position

Definition at line 8047 of file Mini51Series.h.

## ◆ SPI_RX_RX_Msk

#define SPI_RX_RX_Msk (0xfffffffful << SPI_RX_RX_Pos)

SPI_T::RX: RX Mask

Definition at line 8003 of file Mini51Series.h.

## ◆ SPI_RX_RX_Pos

#define SPI_RX_RX_Pos (0)

SPI_T::RX: RX Position

Definition at line 8002 of file Mini51Series.h.

## ◆ SPI_SSR_AUTOSS_Msk

#define SPI_SSR_AUTOSS_Msk (0x1ul << SPI_SSR_AUTOSS_Pos)

SPI_T::SSR: AUTOSS Mask

Definition at line 7994 of file Mini51Series.h.

## ◆ SPI_SSR_AUTOSS_Pos

#define SPI_SSR_AUTOSS_Pos (3)

SPI_T::SSR: AUTOSS Position

Definition at line 7993 of file Mini51Series.h.

## ◆ SPI_SSR_LTRIG_FLAG_Msk

#define SPI_SSR_LTRIG_FLAG_Msk (0x1ul << SPI_SSR_LTRIG_FLAG_Pos)

SPI_T::SSR: LTRIG_FLAG Mask

Definition at line 8000 of file Mini51Series.h.

## ◆ SPI_SSR_LTRIG_FLAG_Pos

#define SPI_SSR_LTRIG_FLAG_Pos (5)

SPI_T::SSR: LTRIG_FLAG Position

Definition at line 7999 of file Mini51Series.h.

## ◆ SPI_SSR_SS_LTRIG_Msk

#define SPI_SSR_SS_LTRIG_Msk (0x1ul << SPI_SSR_SS_LTRIG_Pos)

SPI_T::SSR: SS_LTRIG Mask

Definition at line 7997 of file Mini51Series.h.

## ◆ SPI_SSR_SS_LTRIG_Pos

#define SPI_SSR_SS_LTRIG_Pos (4)

SPI_T::SSR: SS_LTRIG Position

Definition at line 7996 of file Mini51Series.h.

## ◆ SPI_SSR_SS_LVL_Msk

#define SPI_SSR_SS_LVL_Msk (0x1ul << SPI_SSR_SS_LVL_Pos)

SPI_T::SSR: SS_LVL Mask

Definition at line 7991 of file Mini51Series.h.

## ◆ SPI_SSR_SS_LVL_Pos

#define SPI_SSR_SS_LVL_Pos (2)

SPI_T::SSR: SS_LVL Position

Definition at line 7990 of file Mini51Series.h.

## ◆ SPI_SSR_SSR_Msk

#define SPI_SSR_SSR_Msk (0x1ul << SPI_SSR_SSR_Pos)

SPI_T::SSR: SSR Mask

Definition at line 7988 of file Mini51Series.h.

## ◆ SPI_SSR_SSR_Pos

#define SPI_SSR_SSR_Pos (0)

SPI_T::SSR: SSR Position

Definition at line 7987 of file Mini51Series.h.

## ◆ SPI_STATUS_IF_Msk

#define SPI_STATUS_IF_Msk (0x1ul << SPI_STATUS_IF_Pos)

SPI_T::STATUS: IF Mask

Definition at line 8066 of file Mini51Series.h.

## ◆ SPI_STATUS_IF_Pos

#define SPI_STATUS_IF_Pos (16)

SPI_T::STATUS: IF Position

Definition at line 8065 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_EMPTY_Msk

#define SPI_STATUS_RX_EMPTY_Msk (0x1ul << SPI_STATUS_RX_EMPTY_Pos)

SPI_T::STATUS: RX_EMPTY Mask

Definition at line 8072 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_EMPTY_Pos

#define SPI_STATUS_RX_EMPTY_Pos (24)

SPI_T::STATUS: RX_EMPTY Position

Definition at line 8071 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_FIFO_COUNT_Msk

#define SPI_STATUS_RX_FIFO_COUNT_Msk (0xful << SPI_STATUS_RX_FIFO_COUNT_Pos)

SPI_T::STATUS: RX_FIFO_COUNT Mask

Definition at line 8063 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_FIFO_COUNT_Pos

#define SPI_STATUS_RX_FIFO_COUNT_Pos (12)

SPI_T::STATUS: RX_FIFO_COUNT Position

Definition at line 8062 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_FULL_Msk

#define SPI_STATUS_RX_FULL_Msk (0x1ul << SPI_STATUS_RX_FULL_Pos)

SPI_T::STATUS: RX_FULL Mask

Definition at line 8075 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_FULL_Pos

#define SPI_STATUS_RX_FULL_Pos (25)

SPI_T::STATUS: RX_FULL Position

Definition at line 8074 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_INTSTS_Msk

#define SPI_STATUS_RX_INTSTS_Msk (0x1ul << SPI_STATUS_RX_INTSTS_Pos)

SPI_T::STATUS: RX_INTSTS Mask

Definition at line 8051 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_INTSTS_Pos

#define SPI_STATUS_RX_INTSTS_Pos (0)

SPI_T::STATUS: RX_INTSTS Position

Definition at line 8050 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_OVERRUN_Msk

#define SPI_STATUS_RX_OVERRUN_Msk (0x1ul << SPI_STATUS_RX_OVERRUN_Pos)

SPI_T::STATUS: RX_OVERRUN Mask

Definition at line 8054 of file Mini51Series.h.

## ◆ SPI_STATUS_RX_OVERRUN_Pos

#define SPI_STATUS_RX_OVERRUN_Pos (2)

SPI_T::STATUS: RX_OVERRUN Position

Definition at line 8053 of file Mini51Series.h.

## ◆ SPI_STATUS_SLV_START_INTSTS_Msk

#define SPI_STATUS_SLV_START_INTSTS_Msk (0x1ul << SPI_STATUS_SLV_START_INTSTS_Pos)

SPI_T::STATUS: SLV_START_INTSTS Mask

Definition at line 8060 of file Mini51Series.h.

## ◆ SPI_STATUS_SLV_START_INTSTS_Pos

#define SPI_STATUS_SLV_START_INTSTS_Pos (11)

SPI_T::STATUS: SLV_START_INTSTS Position

Definition at line 8059 of file Mini51Series.h.

## ◆ SPI_STATUS_TIMEOUT_Msk

#define SPI_STATUS_TIMEOUT_Msk (0x1ul << SPI_STATUS_TIMEOUT_Pos)

SPI_T::STATUS: TIMEOUT Mask

Definition at line 8069 of file Mini51Series.h.

## ◆ SPI_STATUS_TIMEOUT_Pos

#define SPI_STATUS_TIMEOUT_Pos (20)

SPI_T::STATUS: TIMEOUT Position

Definition at line 8068 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_EMPTY_Msk

#define SPI_STATUS_TX_EMPTY_Msk (0x1ul << SPI_STATUS_TX_EMPTY_Pos)

SPI_T::STATUS: TX_EMPTY Mask

Definition at line 8078 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_EMPTY_Pos

#define SPI_STATUS_TX_EMPTY_Pos (26)

SPI_T::STATUS: TX_EMPTY Position

Definition at line 8077 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_FIFO_COUNT_Msk

#define SPI_STATUS_TX_FIFO_COUNT_Msk (0xful << SPI_STATUS_TX_FIFO_COUNT_Pos)

SPI_T::STATUS: TX_FIFO_COUNT Mask

Definition at line 8084 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_FIFO_COUNT_Pos

#define SPI_STATUS_TX_FIFO_COUNT_Pos (28)

SPI_T::STATUS: TX_FIFO_COUNT Position

Definition at line 8083 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_FULL_Msk

#define SPI_STATUS_TX_FULL_Msk (0x1ul << SPI_STATUS_TX_FULL_Pos)

SPI_T::STATUS: TX_FULL Mask

Definition at line 8081 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_FULL_Pos

#define SPI_STATUS_TX_FULL_Pos (27)

SPI_T::STATUS: TX_FULL Position

Definition at line 8080 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_INTSTS_Msk

#define SPI_STATUS_TX_INTSTS_Msk (0x1ul << SPI_STATUS_TX_INTSTS_Pos)

SPI_T::STATUS: TX_INTSTS Mask

Definition at line 8057 of file Mini51Series.h.

## ◆ SPI_STATUS_TX_INTSTS_Pos

#define SPI_STATUS_TX_INTSTS_Pos (4)

SPI_T::STATUS: TX_INTSTS Position

Definition at line 8056 of file Mini51Series.h.

## ◆ SPI_TX_TX_Msk

#define SPI_TX_TX_Msk (0xfffffffful << SPI_TX_TX_Pos)

SPI_T::TX: TX Mask

Definition at line 8006 of file Mini51Series.h.

## ◆ SPI_TX_TX_Pos

#define SPI_TX_TX_Pos (0)

SPI_T::TX: TX Position

Definition at line 8005 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_INTF_Msk

#define SYS_BODCR_BOD_INTF_Msk (0x1ul << SYS_BODCR_BOD_INTF_Pos)

GCR_T::BODCTL: BOD_INTF Mask

Definition at line 2781 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_INTF_Pos

#define SYS_BODCR_BOD_INTF_Pos (4)

GCR_T::BODCTL: BOD_INTF Position

Definition at line 2780 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_LPM_Msk

#define SYS_BODCR_BOD_LPM_Msk (0x1ul << SYS_BODCR_BOD_LPM_Pos)

GCR_T::BODCTL: BOD_LPM Mask

Definition at line 2784 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_LPM_Pos

#define SYS_BODCR_BOD_LPM_Pos (5)

GCR_T::BODCTL: BOD_LPM Position

Definition at line 2783 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_OUT_Msk

#define SYS_BODCR_BOD_OUT_Msk (0x1ul << SYS_BODCR_BOD_OUT_Pos)

GCR_T::BODCTL: BOD_OUT Mask

Definition at line 2787 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_OUT_Pos

#define SYS_BODCR_BOD_OUT_Pos (6)

GCR_T::BODCTL: BOD_OUT Position

Definition at line 2786 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_RSTEN_Msk

#define SYS_BODCR_BOD_RSTEN_Msk (0x1ul << SYS_BODCR_BOD_RSTEN_Pos)

GCR_T::BODCTL: BOD_RSTEN Mask

Definition at line 2778 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_RSTEN_Pos

#define SYS_BODCR_BOD_RSTEN_Pos (3)

GCR_T::BODCTL: BOD_RSTEN Position

Definition at line 2777 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_VL_EXT_Msk

#define SYS_BODCR_BOD_VL_EXT_Msk (0x1ul << SYS_BODCR_BOD_VL_EXT_Pos)

GCR_T::BODCTL: BOD_VL_EXT Mask

Definition at line 2772 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_VL_EXT_Pos

#define SYS_BODCR_BOD_VL_EXT_Pos (0)

GCR_T::BODCTL: BOD_VL_EXT Position

Definition at line 2771 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_VL_Msk

#define SYS_BODCR_BOD_VL_Msk (0x3ul << SYS_BODCR_BOD_VL_Pos)

GCR_T::BODCTL: BOD_VL Mask

Definition at line 2775 of file Mini51Series.h.

## ◆ SYS_BODCR_BOD_VL_Pos

#define SYS_BODCR_BOD_VL_Pos (1)

GCR_T::BODCTL: BOD_VL Position

Definition at line 2774 of file Mini51Series.h.

## ◆ SYS_IPRSTC1_CHIP_RST_Msk

#define SYS_IPRSTC1_CHIP_RST_Msk (0x1ul << SYS_IPRSTC1_CHIP_RST_Pos)

GCR_T::IPRSTC1: CHIP_RST Mask

Definition at line 2739 of file Mini51Series.h.

## ◆ SYS_IPRSTC1_CHIP_RST_Pos

#define SYS_IPRSTC1_CHIP_RST_Pos (0)

GCR_T::IPRSTC1: CHIP_RST Position

Definition at line 2738 of file Mini51Series.h.

## ◆ SYS_IPRSTC1_CPU_RST_Msk

#define SYS_IPRSTC1_CPU_RST_Msk (0x1ul << SYS_IPRSTC1_CPU_RST_Pos)

GCR_T::IPRSTC1: CPU_RST Mask

Definition at line 2742 of file Mini51Series.h.

## ◆ SYS_IPRSTC1_CPU_RST_Pos

#define SYS_IPRSTC1_CPU_RST_Pos (1)

GCR_T::IPRSTC1: CPU_RST Position

Definition at line 2741 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_ACMP_RST_Msk

#define SYS_IPRSTC2_ACMP_RST_Msk (0x1ul << SYS_IPRSTC2_ACMP_RST_Pos)

GCR_T::IPRSTC2: ACMP_RST Mask

Definition at line 2766 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_ACMP_RST_Pos

#define SYS_IPRSTC2_ACMP_RST_Pos (22)

GCR_T::IPRSTC2: ACMP_RST Position

Definition at line 2765 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_ADC_RST_Msk

#define SYS_IPRSTC2_ADC_RST_Msk (0x1ul << SYS_IPRSTC2_ADC_RST_Pos)

GCR_T::IPRSTC2: ADC_RST Mask

Definition at line 2769 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_ADC_RST_Pos

#define SYS_IPRSTC2_ADC_RST_Pos (28)

GCR_T::IPRSTC2: ADC_RST Position

Definition at line 2768 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_GPIO_RST_Msk

#define SYS_IPRSTC2_GPIO_RST_Msk (0x1ul << SYS_IPRSTC2_GPIO_RST_Pos)

GCR_T::IPRSTC2: GPIO_RST Mask

Definition at line 2745 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_GPIO_RST_Pos

#define SYS_IPRSTC2_GPIO_RST_Pos (1)

GCR_T::IPRSTC2: GPIO_RST Position

Definition at line 2744 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_I2C_RST_Msk

#define SYS_IPRSTC2_I2C_RST_Msk (0x1ul << SYS_IPRSTC2_I2C_RST_Pos)

GCR_T::IPRSTC2: I2C_RST Mask

Definition at line 2754 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_I2C_RST_Pos

#define SYS_IPRSTC2_I2C_RST_Pos (8)

GCR_T::IPRSTC2: I2C_RST Position

Definition at line 2753 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_PWM_RST_Msk

#define SYS_IPRSTC2_PWM_RST_Msk (0x1ul << SYS_IPRSTC2_PWM_RST_Pos)

GCR_T::IPRSTC2: PWM_RST Mask

Definition at line 2763 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_PWM_RST_Pos

#define SYS_IPRSTC2_PWM_RST_Pos (20)

GCR_T::IPRSTC2: PWM_RST Position

Definition at line 2762 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_SPI_RST_Msk

#define SYS_IPRSTC2_SPI_RST_Msk (0x1ul << SYS_IPRSTC2_SPI_RST_Pos)

GCR_T::IPRSTC2: SPI_RST Mask

Definition at line 2757 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_SPI_RST_Pos

#define SYS_IPRSTC2_SPI_RST_Pos (12)

GCR_T::IPRSTC2: SPI_RST Position

Definition at line 2756 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_TMR0_RST_Msk

#define SYS_IPRSTC2_TMR0_RST_Msk (0x1ul << SYS_IPRSTC2_TMR0_RST_Pos)

GCR_T::IPRSTC2: TMR0_RST Mask

Definition at line 2748 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_TMR0_RST_Pos

#define SYS_IPRSTC2_TMR0_RST_Pos (2)

GCR_T::IPRSTC2: TMR0_RST Position

Definition at line 2747 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_TMR1_RST_Msk

#define SYS_IPRSTC2_TMR1_RST_Msk (0x1ul << SYS_IPRSTC2_TMR1_RST_Pos)

GCR_T::IPRSTC2: TMR1_RST Mask

Definition at line 2751 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_TMR1_RST_Pos

#define SYS_IPRSTC2_TMR1_RST_Pos (3)

GCR_T::IPRSTC2: TMR1_RST Position

Definition at line 2750 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_UART_RST_Msk

#define SYS_IPRSTC2_UART_RST_Msk (0x1ul << SYS_IPRSTC2_UART_RST_Pos)

GCR_T::IPRSTC2: UART_RST Mask

Definition at line 2760 of file Mini51Series.h.

## ◆ SYS_IPRSTC2_UART_RST_Pos

#define SYS_IPRSTC2_UART_RST_Pos (16)

GCR_T::IPRSTC2: UART_RST Position

Definition at line 2759 of file Mini51Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_LOOP_Msk

#define SYS_IRCTRIMCTL_TRIM_LOOP_Msk (0x3ul << SYS_IRCTRIMCTL_TRIM_LOOP_Pos)

GCR_T::IRCTRIMCTL: TRIM_LOOP Mask

Definition at line 2940 of file Mini51Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_LOOP_Pos

#define SYS_IRCTRIMCTL_TRIM_LOOP_Pos (4)

GCR_T::IRCTRIMCTL: TRIM_LOOP Position

Definition at line 2939 of file Mini51Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_SEL_Msk

#define SYS_IRCTRIMCTL_TRIM_SEL_Msk (0x1ul << SYS_IRCTRIMCTL_TRIM_SEL_Pos)

GCR_T::IRCTRIMCTL: TRIM_SEL Mask

Definition at line 2937 of file Mini51Series.h.

## ◆ SYS_IRCTRIMCTL_TRIM_SEL_Pos

#define SYS_IRCTRIMCTL_TRIM_SEL_Pos (0)

GCR_T::IRCTRIMCTL: TRIM_SEL Position

Definition at line 2936 of file Mini51Series.h.

## ◆ SYS_IRCTRIMIEN_32K_ERR_IEN_Msk

#define SYS_IRCTRIMIEN_32K_ERR_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_32K_ERR_IEN_Pos)

GCR_T::IRCTRIMIER: 32K_ERR_IEN Mask

Definition at line 2946 of file Mini51Series.h.

## ◆ SYS_IRCTRIMIEN_32K_ERR_IEN_Pos

#define SYS_IRCTRIMIEN_32K_ERR_IEN_Pos (2)

GCR_T::IRCTRIMIER: 32K_ERR_IEN Position

Definition at line 2945 of file Mini51Series.h.

## ◆ SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk

#define SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Msk (0x1ul << SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos)

GCR_T::IRCTRIMIER: TRIM_FAIL_IEN Mask

Definition at line 2943 of file Mini51Series.h.

## ◆ SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos

#define SYS_IRCTRIMIEN_TRIM_FAIL_IEN_Pos (1)

GCR_T::IRCTRIMIER: TRIM_FAIL_IEN Position

Definition at line 2942 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_32K_ERR_INT_Msk

#define SYS_IRCTRIMINT_32K_ERR_INT_Msk (0x1ul << SYS_IRCTRIMINT_32K_ERR_INT_Pos)

GCR_T::IRCTRIMISR: 32K_ERR_INT Mask

Definition at line 2955 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_32K_ERR_INT_Pos

#define SYS_IRCTRIMINT_32K_ERR_INT_Pos (2)

GCR_T::IRCTRIMISR: 32K_ERR_INT Position

Definition at line 2954 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_FREQ_LOCK_Msk

#define SYS_IRCTRIMINT_FREQ_LOCK_Msk (0x1ul << SYS_IRCTRIMINT_FREQ_LOCK_Pos)

GCR_T::IRCTRIMISR: FREQ_LOCK Mask

Definition at line 2949 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_FREQ_LOCK_Pos

#define SYS_IRCTRIMINT_FREQ_LOCK_Pos (0)

GCR_T::IRCTRIMISR: FREQ_LOCK Position

Definition at line 2948 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk

#define SYS_IRCTRIMINT_TRIM_FAIL_INT_Msk (0x1ul << SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos)

GCR_T::IRCTRIMISR: TRIM_FAIL_INT Mask

Definition at line 2952 of file Mini51Series.h.

## ◆ SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos

#define SYS_IRCTRIMINT_TRIM_FAIL_INT_Pos (1)

GCR_T::IRCTRIMISR: TRIM_FAIL_INT Position

Definition at line 2951 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT0_Msk

#define SYS_P0_MFP_P0_ALT0_Msk (0x1ul << SYS_P0_MFP_P0_ALT0_Pos)

GCR_T::P0_MFP: P0_ALT0 Mask

Definition at line 2796 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT0_Pos

#define SYS_P0_MFP_P0_ALT0_Pos (8)

GCR_T::P0_MFP: P0_ALT0 Position

Definition at line 2795 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT1_Msk

#define SYS_P0_MFP_P0_ALT1_Msk (0x1ul << SYS_P0_MFP_P0_ALT1_Pos)

GCR_T::P0_MFP: P0_ALT1 Mask

Definition at line 2799 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT1_Pos

#define SYS_P0_MFP_P0_ALT1_Pos (9)

GCR_T::P0_MFP: P0_ALT1 Position

Definition at line 2798 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT4_Msk

#define SYS_P0_MFP_P0_ALT4_Msk (0x1ul << SYS_P0_MFP_P0_ALT4_Pos)

GCR_T::P0_MFP: P0_ALT4 Mask

Definition at line 2802 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT4_Pos

#define SYS_P0_MFP_P0_ALT4_Pos (12)

GCR_T::P0_MFP: P0_ALT4 Position

Definition at line 2801 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT5_Msk

#define SYS_P0_MFP_P0_ALT5_Msk (0x1ul << SYS_P0_MFP_P0_ALT5_Pos)

GCR_T::P0_MFP: P0_ALT5 Mask

Definition at line 2805 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT5_Pos

#define SYS_P0_MFP_P0_ALT5_Pos (13)

GCR_T::P0_MFP: P0_ALT5 Position

Definition at line 2804 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT6_Msk

#define SYS_P0_MFP_P0_ALT6_Msk (0x1ul << SYS_P0_MFP_P0_ALT6_Pos)

GCR_T::P0_MFP: P0_ALT6 Mask

Definition at line 2808 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT6_Pos

#define SYS_P0_MFP_P0_ALT6_Pos (14)

GCR_T::P0_MFP: P0_ALT6 Position

Definition at line 2807 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT7_Msk

#define SYS_P0_MFP_P0_ALT7_Msk (0x1ul << SYS_P0_MFP_P0_ALT7_Pos)

GCR_T::P0_MFP: P0_ALT7 Mask

Definition at line 2811 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT7_Pos

#define SYS_P0_MFP_P0_ALT7_Pos (15)

GCR_T::P0_MFP: P0_ALT7 Position

Definition at line 2810 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT_Msk

#define SYS_P0_MFP_P0_ALT_Msk (0xfful << SYS_P0_MFP_P0_ALT_Pos)

GCR_T::P0_MFP: P0_ALT Mask

Definition at line 2793 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_ALT_Pos

#define SYS_P0_MFP_P0_ALT_Pos (8)

GCR_T::P0_MFP: P0_ALT Position

Definition at line 2792 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_MFP_Msk

#define SYS_P0_MFP_P0_MFP_Msk (0xfful << SYS_P0_MFP_P0_MFP_Pos)

GCR_T::P0_MFP: P0_MFP Mask

Definition at line 2790 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_MFP_Pos

#define SYS_P0_MFP_P0_MFP_Pos (0)

GCR_T::P0_MFP: P0_MFP Position

Definition at line 2789 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_TYPE_Msk

#define SYS_P0_MFP_P0_TYPE_Msk (0xfful << SYS_P0_MFP_P0_TYPE_Pos)

GCR_T::P0_MFP: P0_TYPE Mask

Definition at line 2814 of file Mini51Series.h.

## ◆ SYS_P0_MFP_P0_TYPE_Pos

#define SYS_P0_MFP_P0_TYPE_Pos (16)

GCR_T::P0_MFP: P0_TYPE Position

Definition at line 2813 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT0_Msk

#define SYS_P1_MFP_P1_ALT0_Msk (0x1ul << SYS_P1_MFP_P1_ALT0_Pos)

GCR_T::P1_MFP: P1_ALT0 Mask

Definition at line 2823 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT0_Pos

#define SYS_P1_MFP_P1_ALT0_Pos (8)

GCR_T::P1_MFP: P1_ALT0 Position

Definition at line 2822 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT2_Msk

#define SYS_P1_MFP_P1_ALT2_Msk (0x1ul << SYS_P1_MFP_P1_ALT2_Pos)

GCR_T::P1_MFP: P1_ALT2 Mask

Definition at line 2826 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT2_Pos

#define SYS_P1_MFP_P1_ALT2_Pos (10)

GCR_T::P1_MFP: P1_ALT2 Position

Definition at line 2825 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT3_Msk

#define SYS_P1_MFP_P1_ALT3_Msk (0x1ul << SYS_P1_MFP_P1_ALT3_Pos)

GCR_T::P1_MFP: P1_ALT3 Mask

Definition at line 2829 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT3_Pos

#define SYS_P1_MFP_P1_ALT3_Pos (11)

GCR_T::P1_MFP: P1_ALT3 Position

Definition at line 2828 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT4_Msk

#define SYS_P1_MFP_P1_ALT4_Msk (0x1ul << SYS_P1_MFP_P1_ALT4_Pos)

GCR_T::P1_MFP: P1_ALT4 Mask

Definition at line 2832 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT4_Pos

#define SYS_P1_MFP_P1_ALT4_Pos (12)

GCR_T::P1_MFP: P1_ALT4 Position

Definition at line 2831 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT5_Msk

#define SYS_P1_MFP_P1_ALT5_Msk (0x1ul << SYS_P1_MFP_P1_ALT5_Pos)

GCR_T::P1_MFP: P1_ALT5 Mask

Definition at line 2835 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT5_Pos

#define SYS_P1_MFP_P1_ALT5_Pos (13)

GCR_T::P1_MFP: P1_ALT5 Position

Definition at line 2834 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT_Msk

#define SYS_P1_MFP_P1_ALT_Msk (0xfful << SYS_P1_MFP_P1_ALT_Pos)

GCR_T::P1_MFP: P1_ALT Mask

Definition at line 2820 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_ALT_Pos

#define SYS_P1_MFP_P1_ALT_Pos (8)

GCR_T::P1_MFP: P1_ALT Position

Definition at line 2819 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_MFP_Msk

#define SYS_P1_MFP_P1_MFP_Msk (0xfful << SYS_P1_MFP_P1_MFP_Pos)

GCR_T::P1_MFP: P1_MFP Mask

Definition at line 2817 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_MFP_Pos

#define SYS_P1_MFP_P1_MFP_Pos (0)

GCR_T::P1_MFP: P1_MFP Position

Definition at line 2816 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_TYPE_Msk

#define SYS_P1_MFP_P1_TYPE_Msk (0xfful << SYS_P1_MFP_P1_TYPE_Pos)

GCR_T::P1_MFP: P1_TYPE Mask

Definition at line 2838 of file Mini51Series.h.

## ◆ SYS_P1_MFP_P1_TYPE_Pos

#define SYS_P1_MFP_P1_TYPE_Pos (16)

GCR_T::P1_MFP: P1_TYPE Position

Definition at line 2837 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT2_Msk

#define SYS_P2_MFP_P2_ALT2_Msk (0x1ul << SYS_P2_MFP_P2_ALT2_Pos)

GCR_T::P2_MFP: P2_ALT2 Mask

Definition at line 2847 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT2_Pos

#define SYS_P2_MFP_P2_ALT2_Pos (10)

GCR_T::P2_MFP: P2_ALT2 Position

Definition at line 2846 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT3_Msk

#define SYS_P2_MFP_P2_ALT3_Msk (0x1ul << SYS_P2_MFP_P2_ALT3_Pos)

GCR_T::P2_MFP: P2_ALT3 Mask

Definition at line 2850 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT3_Pos

#define SYS_P2_MFP_P2_ALT3_Pos (11)

GCR_T::P2_MFP: P2_ALT3 Position

Definition at line 2849 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT4_Msk

#define SYS_P2_MFP_P2_ALT4_Msk (0x1ul << SYS_P2_MFP_P2_ALT4_Pos)

GCR_T::P2_MFP: P2_ALT4 Mask

Definition at line 2853 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT4_Pos

#define SYS_P2_MFP_P2_ALT4_Pos (12)

GCR_T::P2_MFP: P2_ALT4 Position

Definition at line 2852 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT5_Msk

#define SYS_P2_MFP_P2_ALT5_Msk (0x1ul << SYS_P2_MFP_P2_ALT5_Pos)

GCR_T::P2_MFP: P2_ALT5 Mask

Definition at line 2856 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT5_Pos

#define SYS_P2_MFP_P2_ALT5_Pos (13)

GCR_T::P2_MFP: P2_ALT5 Position

Definition at line 2855 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT6_Msk

#define SYS_P2_MFP_P2_ALT6_Msk (0x1ul << SYS_P2_MFP_P2_ALT6_Pos)

GCR_T::P2_MFP: P2_ALT6 Mask

Definition at line 2859 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT6_Pos

#define SYS_P2_MFP_P2_ALT6_Pos (14)

GCR_T::P2_MFP: P2_ALT6 Position

Definition at line 2858 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT_Msk

#define SYS_P2_MFP_P2_ALT_Msk (0xfful << SYS_P2_MFP_P2_ALT_Pos)

GCR_T::P2_MFP: P2_ALT Mask

Definition at line 2844 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_ALT_Pos

#define SYS_P2_MFP_P2_ALT_Pos (8)

GCR_T::P2_MFP: P2_ALT Position

Definition at line 2843 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_MFP_Msk

#define SYS_P2_MFP_P2_MFP_Msk (0xfful << SYS_P2_MFP_P2_MFP_Pos)

GCR_T::P2_MFP: P2_MFP Mask

Definition at line 2841 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_MFP_Pos

#define SYS_P2_MFP_P2_MFP_Pos (0)

GCR_T::P2_MFP: P2_MFP Position

Definition at line 2840 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_TYPE_Msk

#define SYS_P2_MFP_P2_TYPE_Msk (0xfful << SYS_P2_MFP_P2_TYPE_Pos)

GCR_T::P2_MFP: P2_TYPE Mask

Definition at line 2862 of file Mini51Series.h.

## ◆ SYS_P2_MFP_P2_TYPE_Pos

#define SYS_P2_MFP_P2_TYPE_Pos (16)

GCR_T::P2_MFP: P2_TYPE Position

Definition at line 2861 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P32CPP1_Msk

#define SYS_P3_MFP_P32CPP1_Msk (0x1ul << SYS_P3_MFP_P32CPP1_Pos)

GCR_T::P3_MFP: P32CPP1 Mask

Definition at line 2892 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P32CPP1_Pos

#define SYS_P3_MFP_P32CPP1_Pos (24)

GCR_T::P3_MFP: P32CPP1 Position

Definition at line 2891 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT0_Msk

#define SYS_P3_MFP_P3_ALT0_Msk (0x1ul << SYS_P3_MFP_P3_ALT0_Pos)

GCR_T::P3_MFP: P3_ALT0 Mask

Definition at line 2871 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT0_Pos

#define SYS_P3_MFP_P3_ALT0_Pos (8)

GCR_T::P3_MFP: P3_ALT0 Position

Definition at line 2870 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT1_Msk

#define SYS_P3_MFP_P3_ALT1_Msk (0x1ul << SYS_P3_MFP_P3_ALT1_Pos)

GCR_T::P3_MFP: P3_ALT1 Mask

Definition at line 2874 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT1_Pos

#define SYS_P3_MFP_P3_ALT1_Pos (9)

GCR_T::P3_MFP: P3_ALT1 Position

Definition at line 2873 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT2_Msk

#define SYS_P3_MFP_P3_ALT2_Msk (0x1ul << SYS_P3_MFP_P3_ALT2_Pos)

GCR_T::P3_MFP: P3_ALT2 Mask

Definition at line 2877 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT2_Pos

#define SYS_P3_MFP_P3_ALT2_Pos (10)

GCR_T::P3_MFP: P3_ALT2 Position

Definition at line 2876 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT4_Msk

#define SYS_P3_MFP_P3_ALT4_Msk (0x1ul << SYS_P3_MFP_P3_ALT4_Pos)

GCR_T::P3_MFP: P3_ALT4 Mask

Definition at line 2880 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT4_Pos

#define SYS_P3_MFP_P3_ALT4_Pos (12)

GCR_T::P3_MFP: P3_ALT4 Position

Definition at line 2879 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT5_Msk

#define SYS_P3_MFP_P3_ALT5_Msk (0x1ul << SYS_P3_MFP_P3_ALT5_Pos)

GCR_T::P3_MFP: P3_ALT5 Mask

Definition at line 2883 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT5_Pos

#define SYS_P3_MFP_P3_ALT5_Pos (13)

GCR_T::P3_MFP: P3_ALT5 Position

Definition at line 2882 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT6_Msk

#define SYS_P3_MFP_P3_ALT6_Msk (0x1ul << SYS_P3_MFP_P3_ALT6_Pos)

GCR_T::P3_MFP: P3_ALT6 Mask

Definition at line 2886 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT6_Pos

#define SYS_P3_MFP_P3_ALT6_Pos (14)

GCR_T::P3_MFP: P3_ALT6 Position

Definition at line 2885 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT_Msk

#define SYS_P3_MFP_P3_ALT_Msk (0xfful << SYS_P3_MFP_P3_ALT_Pos)

GCR_T::P3_MFP: P3_ALT Mask

Definition at line 2868 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_ALT_Pos

#define SYS_P3_MFP_P3_ALT_Pos (8)

GCR_T::P3_MFP: P3_ALT Position

Definition at line 2867 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_MFP_Msk

#define SYS_P3_MFP_P3_MFP_Msk (0xfful << SYS_P3_MFP_P3_MFP_Pos)

GCR_T::P3_MFP: P3_MFP Mask

Definition at line 2865 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_MFP_Pos

#define SYS_P3_MFP_P3_MFP_Pos (0)

GCR_T::P3_MFP: P3_MFP Position

Definition at line 2864 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_TYPE_Msk

#define SYS_P3_MFP_P3_TYPE_Msk (0xfful << SYS_P3_MFP_P3_TYPE_Pos)

GCR_T::P3_MFP: P3_TYPE Mask

Definition at line 2889 of file Mini51Series.h.

## ◆ SYS_P3_MFP_P3_TYPE_Pos

#define SYS_P3_MFP_P3_TYPE_Pos (16)

GCR_T::P3_MFP: P3_TYPE Position

Definition at line 2888 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT6_Msk

#define SYS_P4_MFP_P4_ALT6_Msk (0x1ul << SYS_P4_MFP_P4_ALT6_Pos)

GCR_T::P4_MFP: P4_ALT6 Mask

Definition at line 2901 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT6_Pos

#define SYS_P4_MFP_P4_ALT6_Pos (14)

GCR_T::P4_MFP: P4_ALT6 Position

Definition at line 2900 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT7_Msk

#define SYS_P4_MFP_P4_ALT7_Msk (0x1ul << SYS_P4_MFP_P4_ALT7_Pos)

GCR_T::P4_MFP: P4_ALT7 Mask

Definition at line 2904 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT7_Pos

#define SYS_P4_MFP_P4_ALT7_Pos (15)

GCR_T::P4_MFP: P4_ALT7 Position

Definition at line 2903 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT_Msk

#define SYS_P4_MFP_P4_ALT_Msk (0xfful << SYS_P4_MFP_P4_ALT_Pos)

GCR_T::P4_MFP: P4_ALT Mask

Definition at line 2898 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_ALT_Pos

#define SYS_P4_MFP_P4_ALT_Pos (8)

GCR_T::P4_MFP: P4_ALT Position

Definition at line 2897 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_MFP_Msk

#define SYS_P4_MFP_P4_MFP_Msk (0xfful << SYS_P4_MFP_P4_MFP_Pos)

GCR_T::P4_MFP: P4_MFP Mask

Definition at line 2895 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_MFP_Pos

#define SYS_P4_MFP_P4_MFP_Pos (0)

GCR_T::P4_MFP: P4_MFP Position

Definition at line 2894 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_TYPE_Msk

#define SYS_P4_MFP_P4_TYPE_Msk (0xfful << SYS_P4_MFP_P4_TYPE_Pos)

GCR_T::P4_MFP: P4_TYPE Mask

Definition at line 2907 of file Mini51Series.h.

## ◆ SYS_P4_MFP_P4_TYPE_Pos

#define SYS_P4_MFP_P4_TYPE_Pos (16)

GCR_T::P4_MFP: P4_TYPE Position

Definition at line 2906 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT0_Msk

#define SYS_P5_MFP_P5_ALT0_Msk (0x1ul << SYS_P5_MFP_P5_ALT0_Pos)

GCR_T::P5_MFP: P5_ALT0 Mask

Definition at line 2916 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT0_Pos

#define SYS_P5_MFP_P5_ALT0_Pos (8)

GCR_T::P5_MFP: P5_ALT0 Position

Definition at line 2915 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT1_Msk

#define SYS_P5_MFP_P5_ALT1_Msk (0x1ul << SYS_P5_MFP_P5_ALT1_Pos)

GCR_T::P5_MFP: P5_ALT1 Mask

Definition at line 2919 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT1_Pos

#define SYS_P5_MFP_P5_ALT1_Pos (9)

GCR_T::P5_MFP: P5_ALT1 Position

Definition at line 2918 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT2_Msk

#define SYS_P5_MFP_P5_ALT2_Msk (0x1ul << SYS_P5_MFP_P5_ALT2_Pos)

GCR_T::P5_MFP: P5_ALT2 Mask

Definition at line 2922 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT2_Pos

#define SYS_P5_MFP_P5_ALT2_Pos (10)

GCR_T::P5_MFP: P5_ALT2 Position

Definition at line 2921 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT3_Msk

#define SYS_P5_MFP_P5_ALT3_Msk (0x1ul << SYS_P5_MFP_P5_ALT3_Pos)

GCR_T::P5_MFP: P5_ALT3 Mask

Definition at line 2925 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT3_Pos

#define SYS_P5_MFP_P5_ALT3_Pos (11)

GCR_T::P5_MFP: P5_ALT3 Position

Definition at line 2924 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT4_Msk

#define SYS_P5_MFP_P5_ALT4_Msk (0x1ul << SYS_P5_MFP_P5_ALT4_Pos)

GCR_T::P5_MFP: P5_ALT4 Mask

Definition at line 2928 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT4_Pos

#define SYS_P5_MFP_P5_ALT4_Pos (12)

GCR_T::P5_MFP: P5_ALT4 Position

Definition at line 2927 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT5_Msk

#define SYS_P5_MFP_P5_ALT5_Msk (0x1ul << SYS_P5_MFP_P5_ALT5_Pos)

GCR_T::P5_MFP: P5_ALT5 Mask

Definition at line 2931 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT5_Pos

#define SYS_P5_MFP_P5_ALT5_Pos (13)

GCR_T::P5_MFP: P5_ALT5 Position

Definition at line 2930 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT_Msk

#define SYS_P5_MFP_P5_ALT_Msk (0xFFul << SYS_P5_MFP_P5_ALT_Pos)

GCR_T::P5_MFP: P5_ALT Mask

Definition at line 2913 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_ALT_Pos

#define SYS_P5_MFP_P5_ALT_Pos (8)

GCR_T::P5_MFP: P5_ALT Position

Definition at line 2912 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_MFP_Msk

#define SYS_P5_MFP_P5_MFP_Msk (0xfful << SYS_P5_MFP_P5_MFP_Pos)

GCR_T::P5_MFP: P5_MFP Mask

Definition at line 2910 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_MFP_Pos

#define SYS_P5_MFP_P5_MFP_Pos (0)

GCR_T::P5_MFP: P5_MFP Position

Definition at line 2909 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_TYPE_Msk

#define SYS_P5_MFP_P5_TYPE_Msk (0xfful << SYS_P5_MFP_P5_TYPE_Pos)

GCR_T::P5_MFP: P5_TYPE Mask

Definition at line 2934 of file Mini51Series.h.

## ◆ SYS_P5_MFP_P5_TYPE_Pos

#define SYS_P5_MFP_P5_TYPE_Pos (16)

GCR_T::P5_MFP: P5_TYPE Position

Definition at line 2933 of file Mini51Series.h.

## ◆ SYS_PDID_PDID_Msk

#define SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)

GCR_T::PDID: PDID Mask

Definition at line 2718 of file Mini51Series.h.

## ◆ SYS_PDID_PDID_Pos

#define SYS_PDID_PDID_Pos (0)

    @addtogroup GCR_CONST GCR Bit Field Definition
    Constant Definitions for GCR Controller

GCR_T::PDID: PDID Position

Definition at line 2717 of file Mini51Series.h.

## ◆ SYS_RegLockAddr_RegUnLock_Msk

#define SYS_RegLockAddr_RegUnLock_Msk (0x1ul << SYS_RegLockAddr_RegUnLock_Pos)

GCR_T::RegLockAddr: RegUnLock Mask

Definition at line 2958 of file Mini51Series.h.

## ◆ SYS_RegLockAddr_RegUnLock_Pos

#define SYS_RegLockAddr_RegUnLock_Pos 0

GCR_T::RegLockAddr: RegUnLock Position

Definition at line 2957 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_BOD_Msk

#define SYS_RSTSRC_RSTS_BOD_Msk (0x1ul << SYS_RSTSRC_RSTS_BOD_Pos)

GCR_T::RSTSRC: RSTS_BOD Mask

Definition at line 2730 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_BOD_Pos

#define SYS_RSTSRC_RSTS_BOD_Pos (4)

GCR_T::RSTSRC: RSTS_BOD Position

Definition at line 2729 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_CPU_Msk

#define SYS_RSTSRC_RSTS_CPU_Msk (0x1ul << SYS_RSTSRC_RSTS_CPU_Pos)

GCR_T::RSTSRC: RSTS_CPU Mask

Definition at line 2736 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_CPU_Pos

#define SYS_RSTSRC_RSTS_CPU_Pos (7)

GCR_T::RSTSRC: RSTS_CPU Position

Definition at line 2735 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_MCU_Msk

#define SYS_RSTSRC_RSTS_MCU_Msk (0x1ul << SYS_RSTSRC_RSTS_MCU_Pos)

GCR_T::RSTSRC: RSTS_MCU Mask

Definition at line 2733 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_MCU_Pos

#define SYS_RSTSRC_RSTS_MCU_Pos (5)

GCR_T::RSTSRC: RSTS_MCU Position

Definition at line 2732 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_POR_Msk

#define SYS_RSTSRC_RSTS_POR_Msk (0x1ul << SYS_RSTSRC_RSTS_POR_Pos)

GCR_T::RSTSRC: RSTS_POR Mask

Definition at line 2721 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_POR_Pos

#define SYS_RSTSRC_RSTS_POR_Pos (0)

GCR_T::RSTSRC: RSTS_POR Position

Definition at line 2720 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_RESET_Msk

#define SYS_RSTSRC_RSTS_RESET_Msk (0x1ul << SYS_RSTSRC_RSTS_RESET_Pos)

GCR_T::RSTSRC: RSTS_RESET Mask

Definition at line 2724 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_RESET_Pos

#define SYS_RSTSRC_RSTS_RESET_Pos (1)

GCR_T::RSTSRC: RSTS_RESET Position

Definition at line 2723 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_WDT_Msk

#define SYS_RSTSRC_RSTS_WDT_Msk (0x1ul << SYS_RSTSRC_RSTS_WDT_Pos)

GCR_T::RSTSRC: RSTS_WDT Mask

Definition at line 2727 of file Mini51Series.h.

## ◆ SYS_RSTSRC_RSTS_WDT_Pos

#define SYS_RSTSRC_RSTS_WDT_Pos (2)

GCR_T::RSTSRC: RSTS_WDT Position

Definition at line 2726 of file Mini51Series.h.

## ◆ TIMER_TCAP_TCAP_Msk

#define TIMER_TCAP_TCAP_Msk (0xfffffful << TIMER_TCAP_TCAP_Pos)

TIMER_T::TCAP: TCAP Mask

Definition at line 8527 of file Mini51Series.h.

## ◆ TIMER_TCAP_TCAP_Pos

#define TIMER_TCAP_TCAP_Pos (0)

TIMER_T::TCAP: TCAP Position

Definition at line 8526 of file Mini51Series.h.

## ◆ TIMER_TCMP_TCMP_Msk

#define TIMER_TCMP_TCMP_Msk (0xfffffful << TIMER_TCMP_TCMP_Pos)

TIMER_T::TCMPR: TCMP Mask

Definition at line 8515 of file Mini51Series.h.

## ◆ TIMER_TCMP_TCMP_Pos

#define TIMER_TCMP_TCMP_Pos (0)

TIMER_T::TCMPR: TCMP Position

Definition at line 8514 of file Mini51Series.h.

## ◆ TIMER_TCSR_CACT_Msk

#define TIMER_TCSR_CACT_Msk (0x1ul << TIMER_TCSR_CACT_Pos)

TIMER_T::TCSR: CACT Mask

Definition at line 8497 of file Mini51Series.h.

## ◆ TIMER_TCSR_CACT_Pos

#define TIMER_TCSR_CACT_Pos (25)

TIMER_T::TCSR: CACT Position

Definition at line 8496 of file Mini51Series.h.

## ◆ TIMER_TCSR_CAP_SRC_Msk

#define TIMER_TCSR_CAP_SRC_Msk (0x1ul << TIMER_TCSR_CAP_SRC_Pos)

TIMER_T::TCSR: CAP_SRC Mask

Definition at line 8488 of file Mini51Series.h.

## ◆ TIMER_TCSR_CAP_SRC_Pos

#define TIMER_TCSR_CAP_SRC_Pos (19)

TIMER_T::TCSR: CAP_SRC Position

Definition at line 8487 of file Mini51Series.h.

## ◆ TIMER_TCSR_CEN_Msk

#define TIMER_TCSR_CEN_Msk (0x1ul << TIMER_TCSR_CEN_Pos)

TIMER_T::TCSR: CEN Mask

Definition at line 8509 of file Mini51Series.h.

## ◆ TIMER_TCSR_CEN_Pos

#define TIMER_TCSR_CEN_Pos (30)

TIMER_T::TCSR: CEN Position

Definition at line 8508 of file Mini51Series.h.

## ◆ TIMER_TCSR_CRST_Msk

#define TIMER_TCSR_CRST_Msk (0x1ul << TIMER_TCSR_CRST_Pos)

TIMER_T::TCSR: CRST Mask

Definition at line 8500 of file Mini51Series.h.

## ◆ TIMER_TCSR_CRST_Pos

#define TIMER_TCSR_CRST_Pos (26)

TIMER_T::TCSR: CRST Position

Definition at line 8499 of file Mini51Series.h.

## ◆ TIMER_TCSR_CTB_Msk

#define TIMER_TCSR_CTB_Msk (0x1ul << TIMER_TCSR_CTB_Pos)

TIMER_T::TCSR: CTB Mask

Definition at line 8494 of file Mini51Series.h.

## ◆ TIMER_TCSR_CTB_Pos

#define TIMER_TCSR_CTB_Pos (24)

TIMER_T::TCSR: CTB Position

Definition at line 8493 of file Mini51Series.h.

## ◆ TIMER_TCSR_DBGACK_TMR_Msk

#define TIMER_TCSR_DBGACK_TMR_Msk (0x1ul << TIMER_TCSR_DBGACK_TMR_Pos)

TIMER_T::TCSR: DBGACK_TMR Mask

Definition at line 8512 of file Mini51Series.h.

## ◆ TIMER_TCSR_DBGACK_TMR_Pos

#define TIMER_TCSR_DBGACK_TMR_Pos (31)

TIMER_T::TCSR: DBGACK_TMR Position

Definition at line 8511 of file Mini51Series.h.

## ◆ TIMER_TCSR_IE_Msk

#define TIMER_TCSR_IE_Msk (0x1ul << TIMER_TCSR_IE_Pos)

TIMER_T::TCSR: IE Mask

Definition at line 8506 of file Mini51Series.h.

## ◆ TIMER_TCSR_IE_Pos

#define TIMER_TCSR_IE_Pos (29)

TIMER_T::TCSR: IE Position

Definition at line 8505 of file Mini51Series.h.

## ◆ TIMER_TCSR_MODE_Msk

#define TIMER_TCSR_MODE_Msk (0x3ul << TIMER_TCSR_MODE_Pos)

TIMER_T::TCSR: MODE Mask

Definition at line 8503 of file Mini51Series.h.

## ◆ TIMER_TCSR_MODE_Pos

#define TIMER_TCSR_MODE_Pos (27)

TIMER_T::TCSR: MODE Position

Definition at line 8502 of file Mini51Series.h.

## ◆ TIMER_TCSR_PERIODIC_SEL_Msk

#define TIMER_TCSR_PERIODIC_SEL_Msk (0x1ul << TIMER_TCSR_PERIODIC_SEL_Pos)

TIMER_T::TCSR: PERIODIC_SEL Mask

Definition at line 8479 of file Mini51Series.h.

## ◆ TIMER_TCSR_PERIODIC_SEL_Pos

#define TIMER_TCSR_PERIODIC_SEL_Pos (17)

TIMER_T::TCSR: PERIODIC_SEL Position

Definition at line 8478 of file Mini51Series.h.

## ◆ TIMER_TCSR_PRESCALE_Msk

#define TIMER_TCSR_PRESCALE_Msk (0xfful << TIMER_TCSR_PRESCALE_Pos)

TIMER_T::TCSR: PRESCALE Mask

Definition at line 8473 of file Mini51Series.h.

## ◆ TIMER_TCSR_PRESCALE_Pos

#define TIMER_TCSR_PRESCALE_Pos (0)

    @addtogroup TMR_CONST TMR Bit Field Definition
    Constant Definitions for TMR Controller

TIMER_T::TCSR: PRESCALE Position

Definition at line 8472 of file Mini51Series.h.

## ◆ TIMER_TCSR_TDR_EN_Msk

#define TIMER_TCSR_TDR_EN_Msk (0x1ul << TIMER_TCSR_TDR_EN_Pos)

TIMER_T::TCSR: TDR_EN Mask

Definition at line 8476 of file Mini51Series.h.

## ◆ TIMER_TCSR_TDR_EN_Pos

#define TIMER_TCSR_TDR_EN_Pos (16)

TIMER_T::TCSR: TDR_EN Position

Definition at line 8475 of file Mini51Series.h.

## ◆ TIMER_TCSR_TOGGLE_PIN_Msk

#define TIMER_TCSR_TOGGLE_PIN_Msk (0x1ul << TIMER_TCSR_TOGGLE_PIN_Pos)

TIMER TCSR: TOGGLE_PIN Mask

Definition at line 8482 of file Mini51Series.h.

## ◆ TIMER_TCSR_TOGGLE_PIN_Pos

#define TIMER_TCSR_TOGGLE_PIN_Pos (18)

TIMER TCSR: TOGGLE_PIN Position

Definition at line 8481 of file Mini51Series.h.

## ◆ TIMER_TCSR_TOUT_PIN_Msk

#define TIMER_TCSR_TOUT_PIN_Msk (0x1ul << TIMER_TCSR_TOUT_PIN_Pos)

TIMER_T::TCSR: TOUT_PIN Mask

Definition at line 8485 of file Mini51Series.h.

## ◆ TIMER_TCSR_TOUT_PIN_Pos

#define TIMER_TCSR_TOUT_PIN_Pos (18)

TIMER_T::TCSR: TOUT_PIN Position

Definition at line 8484 of file Mini51Series.h.

## ◆ TIMER_TCSR_WAKE_EN_Msk

#define TIMER_TCSR_WAKE_EN_Msk (0x1ul << TIMER_TCSR_WAKE_EN_Pos)

TIMER_T::TCSR: WAKE_EN Mask

Definition at line 8491 of file Mini51Series.h.

## ◆ TIMER_TCSR_WAKE_EN_Pos

#define TIMER_TCSR_WAKE_EN_Pos (23)

TIMER_T::TCSR: WAKE_EN Position

Definition at line 8490 of file Mini51Series.h.

## ◆ TIMER_TDR_TDR_Msk

#define TIMER_TDR_TDR_Msk (0xfffffful << TIMER_TDR_TDR_Pos)

TIMER_T::TDR: TDR Mask

Definition at line 8524 of file Mini51Series.h.

## ◆ TIMER_TDR_TDR_Pos

#define TIMER_TDR_TDR_Pos (0)

TIMER_T::TDR: TDR Position

Definition at line 8523 of file Mini51Series.h.

## ◆ TIMER_TEXCON_CAP_MODE_Msk

#define TIMER_TEXCON_CAP_MODE_Msk (0x1ul << TIMER_TEXCON_CAP_MODE_Pos)

TIMER_T::TEXCON: CAP_MODE Mask

Definition at line 8551 of file Mini51Series.h.

## ◆ TIMER_TEXCON_CAP_MODE_Pos

#define TIMER_TEXCON_CAP_MODE_Pos (8)

TIMER_T::TEXCON: CAP_MODE Position

Definition at line 8550 of file Mini51Series.h.

## ◆ TIMER_TEXCON_RSTCAPSEL_Msk

#define TIMER_TEXCON_RSTCAPSEL_Msk (0x1ul << TIMER_TEXCON_RSTCAPSEL_Pos)

TIMER_T::TEXCON: RSTCAPSEL Mask

Definition at line 8539 of file Mini51Series.h.

## ◆ TIMER_TEXCON_RSTCAPSEL_Pos

#define TIMER_TEXCON_RSTCAPSEL_Pos (4)

TIMER_T::TEXCON: RSTCAPSEL Position

Definition at line 8538 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TCDB_Msk

#define TIMER_TEXCON_TCDB_Msk (0x1ul << TIMER_TEXCON_TCDB_Pos)

TIMER_T::TEXCON: TCDB Mask

Definition at line 8548 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TCDB_Pos

#define TIMER_TEXCON_TCDB_Pos (7)

TIMER_T::TEXCON: TCDB Position

Definition at line 8547 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEX_EDGE_Msk

#define TIMER_TEXCON_TEX_EDGE_Msk (0x3ul << TIMER_TEXCON_TEX_EDGE_Pos)

TIMER_T::TEXCON: TEX_EDGE Mask

Definition at line 8533 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEX_EDGE_Pos

#define TIMER_TEXCON_TEX_EDGE_Pos (1)

TIMER_T::TEXCON: TEX_EDGE Position

Definition at line 8532 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXDB_Msk

#define TIMER_TEXCON_TEXDB_Msk (0x1ul << TIMER_TEXCON_TEXDB_Pos)

TIMER_T::TEXCON: TEXDB Mask

Definition at line 8545 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXDB_Pos

#define TIMER_TEXCON_TEXDB_Pos (6)

TIMER_T::TEXCON: TEXDB Position

Definition at line 8544 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXEN_Msk

#define TIMER_TEXCON_TEXEN_Msk (0x1ul << TIMER_TEXCON_TEXEN_Pos)

TIMER_T::TEXCON: TEXEN Mask

Definition at line 8536 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXEN_Pos

#define TIMER_TEXCON_TEXEN_Pos (3)

TIMER_T::TEXCON: TEXEN Position

Definition at line 8535 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXIEN_Msk

#define TIMER_TEXCON_TEXIEN_Msk (0x1ul << TIMER_TEXCON_TEXIEN_Pos)

TIMER_T::TEXCON: TEXIEN Mask

Definition at line 8542 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TEXIEN_Pos

#define TIMER_TEXCON_TEXIEN_Pos (5)

TIMER_T::TEXCON: TEXIEN Position

Definition at line 8541 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TX_PHASE_Msk

#define TIMER_TEXCON_TX_PHASE_Msk (0x1ul << TIMER_TEXCON_TX_PHASE_Pos)

TIMER_T::TEXCON: TX_PHASE Mask

Definition at line 8530 of file Mini51Series.h.

## ◆ TIMER_TEXCON_TX_PHASE_Pos

#define TIMER_TEXCON_TX_PHASE_Pos (0)

TIMER_T::TEXCON: TX_PHASE Position

Definition at line 8529 of file Mini51Series.h.

## ◆ TIMER_TEXISR_TEXIF_Msk

#define TIMER_TEXISR_TEXIF_Msk (0x1ul << TIMER_TEXISR_TEXIF_Pos)

TIMER_T::TEXISR: TEXIF Mask

Definition at line 8554 of file Mini51Series.h.

## ◆ TIMER_TEXISR_TEXIF_Pos

#define TIMER_TEXISR_TEXIF_Pos (0)

TIMER_T::TEXISR: TEXIF Position

Definition at line 8553 of file Mini51Series.h.

## ◆ TIMER_TISR_TIF_Msk

#define TIMER_TISR_TIF_Msk (0x1ul << TIMER_TISR_TIF_Pos)

TIMER_T::TISR: TIF Mask

Definition at line 8518 of file Mini51Series.h.

## ◆ TIMER_TISR_TIF_Pos

#define TIMER_TISR_TIF_Pos (0)

TIMER_T::TISR: TIF Position

Definition at line 8517 of file Mini51Series.h.

## ◆ TIMER_TISR_TWF_Msk

#define TIMER_TISR_TWF_Msk (0x1ul << TIMER_TISR_TWF_Pos)

TIMER_T::TISR: TWF Mask

Definition at line 8521 of file Mini51Series.h.

## ◆ TIMER_TISR_TWF_Pos

#define TIMER_TISR_TWF_Pos (1)

TIMER_T::TISR: TWF Position

Definition at line 8520 of file Mini51Series.h.

## ◆ UART_ALT_CSR_ADDR_MATCH_Msk

#define UART_ALT_CSR_ADDR_MATCH_Msk (0xfful << UART_ALT_CSR_ADDR_MATCH_Pos)

UART_T::ALT_CSR: ADDR_MATCH Mask

Definition at line 9680 of file Mini51Series.h.

## ◆ UART_ALT_CSR_ADDR_MATCH_Pos

#define UART_ALT_CSR_ADDR_MATCH_Pos (24)

UART_T::ALT_CSR: ADDR_MATCH Position

Definition at line 9679 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_AAD_Msk

#define UART_ALT_CSR_RS485_AAD_Msk (0x1ul << UART_ALT_CSR_RS485_AAD_Pos)

UART_T::ALT_CSR: RS485_AAD Mask

Definition at line 9671 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_AAD_Pos

#define UART_ALT_CSR_RS485_AAD_Pos (9)

UART_T::ALT_CSR: RS485_AAD Position

Definition at line 9670 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_ADD_EN_Msk

#define UART_ALT_CSR_RS485_ADD_EN_Msk (0x1ul << UART_ALT_CSR_RS485_ADD_EN_Pos)

UART_T::ALT_CSR: RS485_ADD_EN Mask

Definition at line 9677 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_ADD_EN_Pos

#define UART_ALT_CSR_RS485_ADD_EN_Pos (15)

UART_T::ALT_CSR: RS485_ADD_EN Position

Definition at line 9676 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_AUD_Msk

#define UART_ALT_CSR_RS485_AUD_Msk (0x1ul << UART_ALT_CSR_RS485_AUD_Pos)

UART_T::ALT_CSR: RS485_AUD Mask

Definition at line 9674 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_AUD_Pos

#define UART_ALT_CSR_RS485_AUD_Pos (10)

UART_T::ALT_CSR: RS485_AUD Position

Definition at line 9673 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_NMM_Msk

#define UART_ALT_CSR_RS485_NMM_Msk (0x1ul << UART_ALT_CSR_RS485_NMM_Pos)

UART_T::ALT_CSR: RS485_NMM Mask

Definition at line 9668 of file Mini51Series.h.

## ◆ UART_ALT_CSR_RS485_NMM_Pos

#define UART_ALT_CSR_RS485_NMM_Pos (8)

UART_T::ALT_CSR: RS485_NMM Position

Definition at line 9667 of file Mini51Series.h.

## ◆ UART_BAUD_BRD_Msk

#define UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)

UART_T::BAUD: BRD Mask

Definition at line 9647 of file Mini51Series.h.

## ◆ UART_BAUD_BRD_Pos

#define UART_BAUD_BRD_Pos (0)

UART_T::BAUD: BRD Position

Definition at line 9646 of file Mini51Series.h.

## ◆ UART_BAUD_DIV_X_EN_Msk

#define UART_BAUD_DIV_X_EN_Msk (0x1ul << UART_BAUD_DIV_X_EN_Pos)

UART_T::BAUD: DIV_X_EN Mask

Definition at line 9656 of file Mini51Series.h.

## ◆ UART_BAUD_DIV_X_EN_Pos

#define UART_BAUD_DIV_X_EN_Pos (29)

UART_T::BAUD: DIV_X_EN Position

Definition at line 9655 of file Mini51Series.h.

## ◆ UART_BAUD_DIV_X_ONE_Msk

#define UART_BAUD_DIV_X_ONE_Msk (0x1ul << UART_BAUD_DIV_X_ONE_Pos)

UART_T::BAUD: DIV_X_ONE Mask

Definition at line 9653 of file Mini51Series.h.

## ◆ UART_BAUD_DIV_X_ONE_Pos

#define UART_BAUD_DIV_X_ONE_Pos (28)

UART_T::BAUD: DIV_X_ONE Position

Definition at line 9652 of file Mini51Series.h.

## ◆ UART_BAUD_DIVIDER_X_Msk

#define UART_BAUD_DIVIDER_X_Msk (0xful << UART_BAUD_DIVIDER_X_Pos)

UART_T::BAUD: DIVIDER_X Mask

Definition at line 9650 of file Mini51Series.h.

## ◆ UART_BAUD_DIVIDER_X_Pos

#define UART_BAUD_DIVIDER_X_Pos (24)

UART_T::BAUD: DIVIDER_X Position

Definition at line 9649 of file Mini51Series.h.

## ◆ UART_FCR_RFITL_Msk

#define UART_FCR_RFITL_Msk (0xful << UART_FCR_RFITL_Pos)

UART_T::FCR: RFITL Mask

Definition at line 9521 of file Mini51Series.h.

## ◆ UART_FCR_RFITL_Pos

#define UART_FCR_RFITL_Pos (4)

UART_T::FCR: RFITL Position

Definition at line 9520 of file Mini51Series.h.

## ◆ UART_FCR_RFR_Msk

#define UART_FCR_RFR_Msk (0x1ul << UART_FCR_RFR_Pos)

UART_T::FCR: RFR Mask

Definition at line 9515 of file Mini51Series.h.

## ◆ UART_FCR_RFR_Pos

#define UART_FCR_RFR_Pos (1)

UART_T::FCR: RFR Position

Definition at line 9514 of file Mini51Series.h.

## ◆ UART_FCR_RTS_TRI_LEV_Msk

#define UART_FCR_RTS_TRI_LEV_Msk (0xful << UART_FCR_RTS_TRI_LEV_Pos)

UART_T::FCR: RTS_TRI_LEV Mask

Definition at line 9527 of file Mini51Series.h.

## ◆ UART_FCR_RTS_TRI_LEV_Pos

#define UART_FCR_RTS_TRI_LEV_Pos (16)

UART_T::FCR: RTS_TRI_LEV Position

Definition at line 9526 of file Mini51Series.h.

## ◆ UART_FCR_RX_DIS_Msk

#define UART_FCR_RX_DIS_Msk (0x1ul << UART_FCR_RX_DIS_Pos)

UART_T::FCR: RX_DIS Mask

Definition at line 9524 of file Mini51Series.h.

## ◆ UART_FCR_RX_DIS_Pos

#define UART_FCR_RX_DIS_Pos (8)

UART_T::FCR: RX_DIS Position

Definition at line 9523 of file Mini51Series.h.

## ◆ UART_FCR_TFR_Msk

#define UART_FCR_TFR_Msk (0x1ul << UART_FCR_TFR_Pos)

UART_T::FCR: TFR Mask

Definition at line 9518 of file Mini51Series.h.

## ◆ UART_FCR_TFR_Pos

#define UART_FCR_TFR_Pos (2)

UART_T::FCR: TFR Position

Definition at line 9517 of file Mini51Series.h.

## ◆ UART_FSR_BIF_Msk

#define UART_FSR_BIF_Msk (0x1ul << UART_FSR_BIF_Pos)

UART_T::FSR: BIF Mask

Definition at line 9578 of file Mini51Series.h.

## ◆ UART_FSR_BIF_Pos

#define UART_FSR_BIF_Pos (6)

UART_T::FSR: BIF Position

Definition at line 9577 of file Mini51Series.h.

## ◆ UART_FSR_FEF_Msk

#define UART_FSR_FEF_Msk (0x1ul << UART_FSR_FEF_Pos)

UART_T::FSR: FEF Mask

Definition at line 9575 of file Mini51Series.h.

## ◆ UART_FSR_FEF_Pos

#define UART_FSR_FEF_Pos (5)

UART_T::FSR: FEF Position

Definition at line 9574 of file Mini51Series.h.

## ◆ UART_FSR_PEF_Msk

#define UART_FSR_PEF_Msk (0x1ul << UART_FSR_PEF_Pos)

UART_T::FSR: PEF Mask

Definition at line 9572 of file Mini51Series.h.

## ◆ UART_FSR_PEF_Pos

#define UART_FSR_PEF_Pos (4)

UART_T::FSR: PEF Position

Definition at line 9571 of file Mini51Series.h.

## ◆ UART_FSR_RS485_ADD_DETF_Msk

#define UART_FSR_RS485_ADD_DETF_Msk (0x1ul << UART_FSR_RS485_ADD_DETF_Pos)

UART_T::FSR: RS485_ADD_DETF Mask

Definition at line 9569 of file Mini51Series.h.

## ◆ UART_FSR_RS485_ADD_DETF_Pos

#define UART_FSR_RS485_ADD_DETF_Pos (3)

UART_T::FSR: RS485_ADD_DETF Position

Definition at line 9568 of file Mini51Series.h.

## ◆ UART_FSR_RX_EMPTY_Msk

#define UART_FSR_RX_EMPTY_Msk (0x1ul << UART_FSR_RX_EMPTY_Pos)

UART_T::FSR: RX_EMPTY Mask

Definition at line 9584 of file Mini51Series.h.

## ◆ UART_FSR_RX_EMPTY_Pos

#define UART_FSR_RX_EMPTY_Pos (14)

UART_T::FSR: RX_EMPTY Position

Definition at line 9583 of file Mini51Series.h.

## ◆ UART_FSR_RX_FULL_Msk

#define UART_FSR_RX_FULL_Msk (0x1ul << UART_FSR_RX_FULL_Pos)

UART_T::FSR: RX_FULL Mask

Definition at line 9587 of file Mini51Series.h.

## ◆ UART_FSR_RX_FULL_Pos

#define UART_FSR_RX_FULL_Pos (15)

UART_T::FSR: RX_FULL Position

Definition at line 9586 of file Mini51Series.h.

## ◆ UART_FSR_RX_OVER_IF_Msk

#define UART_FSR_RX_OVER_IF_Msk (0x1ul << UART_FSR_RX_OVER_IF_Pos)

UART_T::FSR: RX_OVER_IF Mask

Definition at line 9566 of file Mini51Series.h.

## ◆ UART_FSR_RX_OVER_IF_Pos

#define UART_FSR_RX_OVER_IF_Pos (0)

UART_T::FSR: RX_OVER_IF Position

Definition at line 9565 of file Mini51Series.h.

## ◆ UART_FSR_RX_POINTER_Msk

#define UART_FSR_RX_POINTER_Msk (0x3ful << UART_FSR_RX_POINTER_Pos)

UART_T::FSR: RX_POINTER Mask

Definition at line 9581 of file Mini51Series.h.

## ◆ UART_FSR_RX_POINTER_Pos

#define UART_FSR_RX_POINTER_Pos (8)

UART_T::FSR: RX_POINTER Position

Definition at line 9580 of file Mini51Series.h.

## ◆ UART_FSR_TE_FLAG_Msk

#define UART_FSR_TE_FLAG_Msk (0x1ul << UART_FSR_TE_FLAG_Pos)

UART_T::FSR: TE_FLAG Mask

Definition at line 9602 of file Mini51Series.h.

## ◆ UART_FSR_TE_FLAG_Pos

#define UART_FSR_TE_FLAG_Pos (28)

UART_T::FSR: TE_FLAG Position

Definition at line 9601 of file Mini51Series.h.

## ◆ UART_FSR_TX_EMPTY_Msk

#define UART_FSR_TX_EMPTY_Msk (0x1ul << UART_FSR_TX_EMPTY_Pos)

UART_T::FSR: TX_EMPTY Mask

Definition at line 9593 of file Mini51Series.h.

## ◆ UART_FSR_TX_EMPTY_Pos

#define UART_FSR_TX_EMPTY_Pos (22)

UART_T::FSR: TX_EMPTY Position

Definition at line 9592 of file Mini51Series.h.

## ◆ UART_FSR_TX_FULL_Msk

#define UART_FSR_TX_FULL_Msk (0x1ul << UART_FSR_TX_FULL_Pos)

UART_T::FSR: TX_FULL Mask

Definition at line 9596 of file Mini51Series.h.

## ◆ UART_FSR_TX_FULL_Pos

#define UART_FSR_TX_FULL_Pos (23)

UART_T::FSR: TX_FULL Position

Definition at line 9595 of file Mini51Series.h.

## ◆ UART_FSR_TX_OVER_IF_Msk

#define UART_FSR_TX_OVER_IF_Msk (0x1ul << UART_FSR_TX_OVER_IF_Pos)

UART_T::FSR: TX_OVER_IF Mask

Definition at line 9599 of file Mini51Series.h.

## ◆ UART_FSR_TX_OVER_IF_Pos

#define UART_FSR_TX_OVER_IF_Pos (24)

UART_T::FSR: TX_OVER_IF Position

Definition at line 9598 of file Mini51Series.h.

## ◆ UART_FSR_TX_POINTER_Msk

#define UART_FSR_TX_POINTER_Msk (0x3ful << UART_FSR_TX_POINTER_Pos)

UART_T::FSR: TX_POINTER Mask

Definition at line 9590 of file Mini51Series.h.

## ◆ UART_FSR_TX_POINTER_Pos

#define UART_FSR_TX_POINTER_Pos (16)

UART_T::FSR: TX_POINTER Position

Definition at line 9589 of file Mini51Series.h.

## ◆ UART_FUN_SEL_FUN_SEL_Msk

#define UART_FUN_SEL_FUN_SEL_Msk (0x3ul << UART_FUN_SEL_FUN_SEL_Pos)

UART_T::FUN_SEL: FUN_SEL Mask

Definition at line 9683 of file Mini51Series.h.

## ◆ UART_FUN_SEL_FUN_SEL_Pos

#define UART_FUN_SEL_FUN_SEL_Pos (0)

UART_T::FUN_SEL: FUN_SEL Position

Definition at line 9682 of file Mini51Series.h.

## ◆ UART_IER_AUTO_CTS_EN_Msk

#define UART_IER_AUTO_CTS_EN_Msk (0x1ul << UART_IER_AUTO_CTS_EN_Pos)

UART_T::IER: AUTO_CTS_EN Mask

Definition at line 9512 of file Mini51Series.h.

## ◆ UART_IER_AUTO_CTS_EN_Pos

#define UART_IER_AUTO_CTS_EN_Pos (13)

UART_T::IER: AUTO_CTS_EN Position

Definition at line 9511 of file Mini51Series.h.

## ◆ UART_IER_AUTO_RTS_EN_Msk

#define UART_IER_AUTO_RTS_EN_Msk (0x1ul << UART_IER_AUTO_RTS_EN_Pos)

UART_T::IER: AUTO_RTS_EN Mask

Definition at line 9509 of file Mini51Series.h.

## ◆ UART_IER_AUTO_RTS_EN_Pos

#define UART_IER_AUTO_RTS_EN_Pos (12)

UART_T::IER: AUTO_RTS_EN Position

Definition at line 9508 of file Mini51Series.h.

## ◆ UART_IER_BUF_ERR_IEN_Msk

#define UART_IER_BUF_ERR_IEN_Msk (0x1ul << UART_IER_BUF_ERR_IEN_Pos)

UART_T::IER: BUF_ERR_IEN Mask

Definition at line 9500 of file Mini51Series.h.

## ◆ UART_IER_BUF_ERR_IEN_Pos

#define UART_IER_BUF_ERR_IEN_Pos (5)

UART_T::IER: BUF_ERR_IEN Position

Definition at line 9499 of file Mini51Series.h.

## ◆ UART_IER_MODEM_IEN_Msk

#define UART_IER_MODEM_IEN_Msk (0x1ul << UART_IER_MODEM_IEN_Pos)

UART_T::IER: MODEM_IEN Mask

Definition at line 9494 of file Mini51Series.h.

## ◆ UART_IER_MODEM_IEN_Pos

#define UART_IER_MODEM_IEN_Pos (3)

UART_T::IER: MODEM_IEN Position

Definition at line 9493 of file Mini51Series.h.

## ◆ UART_IER_RDA_IEN_Msk

#define UART_IER_RDA_IEN_Msk (0x1ul << UART_IER_RDA_IEN_Pos)

UART_T::IER: RDA_IEN Mask

Definition at line 9485 of file Mini51Series.h.

## ◆ UART_IER_RDA_IEN_Pos

#define UART_IER_RDA_IEN_Pos (0)

UART_T::IER: RDA_IEN Position

Definition at line 9484 of file Mini51Series.h.

## ◆ UART_IER_RLS_IEN_Msk

#define UART_IER_RLS_IEN_Msk (0x1ul << UART_IER_RLS_IEN_Pos)

UART_T::IER: RLS_IEN Mask

Definition at line 9491 of file Mini51Series.h.

## ◆ UART_IER_RLS_IEN_Pos

#define UART_IER_RLS_IEN_Pos (2)

UART_T::IER: RLS_IEN Position

Definition at line 9490 of file Mini51Series.h.

## ◆ UART_IER_RTO_IEN_Msk

#define UART_IER_RTO_IEN_Msk (0x1ul << UART_IER_RTO_IEN_Pos)

UART_T::IER: RTO_IEN Mask

Definition at line 9497 of file Mini51Series.h.

## ◆ UART_IER_RTO_IEN_Pos

#define UART_IER_RTO_IEN_Pos (4)

UART_T::IER: RTO_IEN Position

Definition at line 9496 of file Mini51Series.h.

## ◆ UART_IER_THRE_IEN_Msk

#define UART_IER_THRE_IEN_Msk (0x1ul << UART_IER_THRE_IEN_Pos)

UART_T::IER: THRE_IEN Mask

Definition at line 9488 of file Mini51Series.h.

## ◆ UART_IER_THRE_IEN_Pos

#define UART_IER_THRE_IEN_Pos (1)

UART_T::IER: THRE_IEN Position

Definition at line 9487 of file Mini51Series.h.

## ◆ UART_IER_TIME_OUT_EN_Msk

#define UART_IER_TIME_OUT_EN_Msk (0x1ul << UART_IER_TIME_OUT_EN_Pos)

UART_T::IER: TIME_OUT_EN Mask

Definition at line 9506 of file Mini51Series.h.

## ◆ UART_IER_TIME_OUT_EN_Pos

#define UART_IER_TIME_OUT_EN_Pos (11)

UART_T::IER: TIME_OUT_EN Position

Definition at line 9505 of file Mini51Series.h.

## ◆ UART_IER_WAKE_EN_Msk

#define UART_IER_WAKE_EN_Msk (0x1ul << UART_IER_WAKE_EN_Pos)

UART_T::IER: WAKE_EN Mask

Definition at line 9503 of file Mini51Series.h.

## ◆ UART_IER_WAKE_EN_Pos

#define UART_IER_WAKE_EN_Pos (6)

UART_T::IER: WAKE_EN Position

Definition at line 9502 of file Mini51Series.h.

## ◆ UART_IRCR_INV_RX_Msk

#define UART_IRCR_INV_RX_Msk (0x1ul << UART_IRCR_INV_RX_Pos)

UART_T::IRCR: INV_RX Mask

Definition at line 9665 of file Mini51Series.h.

## ◆ UART_IRCR_INV_RX_Pos

#define UART_IRCR_INV_RX_Pos (6)

UART_T::IRCR: INV_RX Position

Definition at line 9664 of file Mini51Series.h.

## ◆ UART_IRCR_INV_TX_Msk

#define UART_IRCR_INV_TX_Msk (0x1ul << UART_IRCR_INV_TX_Pos)

UART_T::IRCR: INV_TX Mask

Definition at line 9662 of file Mini51Series.h.

## ◆ UART_IRCR_INV_TX_Pos

#define UART_IRCR_INV_TX_Pos (5)

UART_T::IRCR: INV_TX Position

Definition at line 9661 of file Mini51Series.h.

## ◆ UART_IRCR_TX_SELECT_Msk

#define UART_IRCR_TX_SELECT_Msk (0x1ul << UART_IRCR_TX_SELECT_Pos)

UART_T::IRCR: TX_SELECT Mask

Definition at line 9659 of file Mini51Series.h.

## ◆ UART_IRCR_TX_SELECT_Pos

#define UART_IRCR_TX_SELECT_Pos (1)

UART_T::IRCR: TX_SELECT Position

Definition at line 9658 of file Mini51Series.h.

## ◆ UART_ISR_BUF_ERR_IF_Msk

#define UART_ISR_BUF_ERR_IF_Msk (0x1ul << UART_ISR_BUF_ERR_IF_Pos)

UART_T::ISR: BUF_ERR_IF Mask

Definition at line 9620 of file Mini51Series.h.

## ◆ UART_ISR_BUF_ERR_IF_Pos

#define UART_ISR_BUF_ERR_IF_Pos (5)

UART_T::ISR: BUF_ERR_IF Position

Definition at line 9619 of file Mini51Series.h.

## ◆ UART_ISR_BUF_ERR_INT_Msk

#define UART_ISR_BUF_ERR_INT_Msk (0x1ul << UART_ISR_BUF_ERR_INT_Pos)

UART_T::ISR: BUF_ERR_INT Mask

Definition at line 9638 of file Mini51Series.h.

## ◆ UART_ISR_BUF_ERR_INT_Pos

#define UART_ISR_BUF_ERR_INT_Pos (13)

UART_T::ISR: BUF_ERR_INT Position

Definition at line 9637 of file Mini51Series.h.

## ◆ UART_ISR_MODEM_IF_Msk

#define UART_ISR_MODEM_IF_Msk (0x1ul << UART_ISR_MODEM_IF_Pos)

UART_T::ISR: MODEM_IF Mask

Definition at line 9614 of file Mini51Series.h.

## ◆ UART_ISR_MODEM_IF_Pos

#define UART_ISR_MODEM_IF_Pos (3)

UART_T::ISR: MODEM_IF Position

Definition at line 9613 of file Mini51Series.h.

## ◆ UART_ISR_MODEM_INT_Msk

#define UART_ISR_MODEM_INT_Msk (0x1ul << UART_ISR_MODEM_INT_Pos)

UART_T::ISR: MODEM_INT Mask

Definition at line 9632 of file Mini51Series.h.

## ◆ UART_ISR_MODEM_INT_Pos

#define UART_ISR_MODEM_INT_Pos (11)

UART_T::ISR: MODEM_INT Position

Definition at line 9631 of file Mini51Series.h.

## ◆ UART_ISR_RDA_IF_Msk

#define UART_ISR_RDA_IF_Msk (0x1ul << UART_ISR_RDA_IF_Pos)

UART_T::ISR: RDA_IF Mask

Definition at line 9605 of file Mini51Series.h.

## ◆ UART_ISR_RDA_IF_Pos

#define UART_ISR_RDA_IF_Pos (0)

UART_T::ISR: RDA_IF Position

Definition at line 9604 of file Mini51Series.h.

## ◆ UART_ISR_RDA_INT_Msk

#define UART_ISR_RDA_INT_Msk (0x1ul << UART_ISR_RDA_INT_Pos)

UART_T::ISR: RDA_INT Mask

Definition at line 9623 of file Mini51Series.h.

## ◆ UART_ISR_RDA_INT_Pos

#define UART_ISR_RDA_INT_Pos (8)

UART_T::ISR: RDA_INT Position

Definition at line 9622 of file Mini51Series.h.

## ◆ UART_ISR_RLS_IF_Msk

#define UART_ISR_RLS_IF_Msk (0x1ul << UART_ISR_RLS_IF_Pos)

UART_T::ISR: RLS_IF Mask

Definition at line 9611 of file Mini51Series.h.

## ◆ UART_ISR_RLS_IF_Pos

#define UART_ISR_RLS_IF_Pos (2)

UART_T::ISR: RLS_IF Position

Definition at line 9610 of file Mini51Series.h.

## ◆ UART_ISR_RLS_INT_Msk

#define UART_ISR_RLS_INT_Msk (0x1ul << UART_ISR_RLS_INT_Pos)

UART_T::ISR: RLS_INT Mask

Definition at line 9629 of file Mini51Series.h.

## ◆ UART_ISR_RLS_INT_Pos

#define UART_ISR_RLS_INT_Pos (10)

UART_T::ISR: RLS_INT Position

Definition at line 9628 of file Mini51Series.h.

## ◆ UART_ISR_THRE_IF_Msk

#define UART_ISR_THRE_IF_Msk (0x1ul << UART_ISR_THRE_IF_Pos)

UART_T::ISR: THRE_IF Mask

Definition at line 9608 of file Mini51Series.h.

## ◆ UART_ISR_THRE_IF_Pos

#define UART_ISR_THRE_IF_Pos (1)

UART_T::ISR: THRE_IF Position

Definition at line 9607 of file Mini51Series.h.

## ◆ UART_ISR_THRE_INT_Msk

#define UART_ISR_THRE_INT_Msk (0x1ul << UART_ISR_THRE_INT_Pos)

UART_T::ISR: THRE_INT Mask

Definition at line 9626 of file Mini51Series.h.

## ◆ UART_ISR_THRE_INT_Pos

#define UART_ISR_THRE_INT_Pos (9)

UART_T::ISR: THRE_INT Position

Definition at line 9625 of file Mini51Series.h.

## ◆ UART_ISR_TOUT_IF_Msk

#define UART_ISR_TOUT_IF_Msk (0x1ul << UART_ISR_TOUT_IF_Pos)

UART_T::ISR: TOUT_IF Mask

Definition at line 9617 of file Mini51Series.h.

## ◆ UART_ISR_TOUT_IF_Pos

#define UART_ISR_TOUT_IF_Pos (4)

UART_T::ISR: TOUT_IF Position

Definition at line 9616 of file Mini51Series.h.

## ◆ UART_ISR_TOUT_INT_Msk

#define UART_ISR_TOUT_INT_Msk (0x1ul << UART_ISR_TOUT_INT_Pos)

UART_T::ISR: TOUT_INT Mask

Definition at line 9635 of file Mini51Series.h.

## ◆ UART_ISR_TOUT_INT_Pos

#define UART_ISR_TOUT_INT_Pos (12)

UART_T::ISR: TOUT_INT Position

Definition at line 9634 of file Mini51Series.h.

## ◆ UART_LCR_BCB_Msk

#define UART_LCR_BCB_Msk (0x1ul << UART_LCR_BCB_Pos)

UART_T::LCR: BCB Mask

Definition at line 9545 of file Mini51Series.h.

## ◆ UART_LCR_BCB_Pos

#define UART_LCR_BCB_Pos (6)

UART_T::LCR: BCB Position

Definition at line 9544 of file Mini51Series.h.

## ◆ UART_LCR_EPE_Msk

#define UART_LCR_EPE_Msk (0x1ul << UART_LCR_EPE_Pos)

UART_T::LCR: EPE Mask

Definition at line 9539 of file Mini51Series.h.

## ◆ UART_LCR_EPE_Pos

#define UART_LCR_EPE_Pos (4)

UART_T::LCR: EPE Position

Definition at line 9538 of file Mini51Series.h.

## ◆ UART_LCR_NSB_Msk

#define UART_LCR_NSB_Msk (0x1ul << UART_LCR_NSB_Pos)

UART_T::LCR: NSB Mask

Definition at line 9533 of file Mini51Series.h.

## ◆ UART_LCR_NSB_Pos

#define UART_LCR_NSB_Pos (2)

UART_T::LCR: NSB Position

Definition at line 9532 of file Mini51Series.h.

## ◆ UART_LCR_PBE_Msk

#define UART_LCR_PBE_Msk (0x1ul << UART_LCR_PBE_Pos)

UART_T::LCR: PBE Mask

Definition at line 9536 of file Mini51Series.h.

## ◆ UART_LCR_PBE_Pos

#define UART_LCR_PBE_Pos (3)

UART_T::LCR: PBE Position

Definition at line 9535 of file Mini51Series.h.

## ◆ UART_LCR_SPE_Msk

#define UART_LCR_SPE_Msk (0x1ul << UART_LCR_SPE_Pos)

UART_T::LCR: SPE Mask

Definition at line 9542 of file Mini51Series.h.

## ◆ UART_LCR_SPE_Pos

#define UART_LCR_SPE_Pos (5)

UART_T::LCR: SPE Position

Definition at line 9541 of file Mini51Series.h.

## ◆ UART_LCR_WLS_Msk

#define UART_LCR_WLS_Msk (0x3ul << UART_LCR_WLS_Pos)

UART_T::LCR: WLS Mask

Definition at line 9530 of file Mini51Series.h.

## ◆ UART_LCR_WLS_Pos

#define UART_LCR_WLS_Pos (0)

UART_T::LCR: WLS Position

Definition at line 9529 of file Mini51Series.h.

## ◆ UART_MCR_LEV_RTS_Msk

#define UART_MCR_LEV_RTS_Msk (0x1ul << UART_MCR_LEV_RTS_Pos)

UART_T::MCR: LEV_RTS Mask

Definition at line 9551 of file Mini51Series.h.

## ◆ UART_MCR_LEV_RTS_Pos

#define UART_MCR_LEV_RTS_Pos (9)

UART_T::MCR: LEV_RTS Position

Definition at line 9550 of file Mini51Series.h.

## ◆ UART_MCR_RTS_Msk

#define UART_MCR_RTS_Msk (0x1ul << UART_MCR_RTS_Pos)

UART_T::MCR: RTS Mask

Definition at line 9548 of file Mini51Series.h.

## ◆ UART_MCR_RTS_Pos

#define UART_MCR_RTS_Pos (1)

UART_T::MCR: RTS Position

Definition at line 9547 of file Mini51Series.h.

## ◆ UART_MCR_RTS_ST_Msk

#define UART_MCR_RTS_ST_Msk (0x1ul << UART_MCR_RTS_ST_Pos)

UART_T::MCR: RTS_ST Mask

Definition at line 9554 of file Mini51Series.h.

## ◆ UART_MCR_RTS_ST_Pos

#define UART_MCR_RTS_ST_Pos (13)

UART_T::MCR: RTS_ST Position

Definition at line 9553 of file Mini51Series.h.

## ◆ UART_MSR_CTS_ST_Msk

#define UART_MSR_CTS_ST_Msk (0x1ul << UART_MSR_CTS_ST_Pos)

UART_T::MSR: CTS_ST Mask

Definition at line 9560 of file Mini51Series.h.

## ◆ UART_MSR_CTS_ST_Pos

#define UART_MSR_CTS_ST_Pos (4)

UART_T::MSR: CTS_ST Position

Definition at line 9559 of file Mini51Series.h.

## ◆ UART_MSR_DCTSF_Msk

#define UART_MSR_DCTSF_Msk (0x1ul << UART_MSR_DCTSF_Pos)

UART_T::MSR: DCTSF Mask

Definition at line 9557 of file Mini51Series.h.

## ◆ UART_MSR_DCTSF_Pos

#define UART_MSR_DCTSF_Pos (0)

UART_T::MSR: DCTSF Position

Definition at line 9556 of file Mini51Series.h.

## ◆ UART_MSR_LEV_CTS_Msk

#define UART_MSR_LEV_CTS_Msk (0x1ul << UART_MSR_LEV_CTS_Pos)

UART_T::MSR: LEV_CTS Mask

Definition at line 9563 of file Mini51Series.h.

## ◆ UART_MSR_LEV_CTS_Pos

#define UART_MSR_LEV_CTS_Pos (8)

UART_T::MSR: LEV_CTS Position

Definition at line 9562 of file Mini51Series.h.

## ◆ UART_RBR_RBR_Msk

#define UART_RBR_RBR_Msk (0xfful << UART_RBR_RBR_Pos)

UART_T::RBR: RBR Mask

Definition at line 9479 of file Mini51Series.h.

## ◆ UART_RBR_RBR_Pos

#define UART_RBR_RBR_Pos (0)

    @addtogroup UART_CONST UART Bit Field Definition
    Constant Definitions for UART Controller

UART_T::RBR: RBR Position

Definition at line 9478 of file Mini51Series.h.

## ◆ UART_THR_THR_Msk

#define UART_THR_THR_Msk (0xfful << UART_THR_THR_Pos)

UART_T::THR: THR Mask

Definition at line 9482 of file Mini51Series.h.

## ◆ UART_THR_THR_Pos

#define UART_THR_THR_Pos (0)

UART_T::THR: THR Position

Definition at line 9481 of file Mini51Series.h.

## ◆ UART_TOR_DLY_Msk

#define UART_TOR_DLY_Msk (0xfful << UART_TOR_DLY_Pos)

UART_T::TOR: DLY Mask

Definition at line 9644 of file Mini51Series.h.

## ◆ UART_TOR_DLY_Pos

#define UART_TOR_DLY_Pos (8)

UART_T::TOR: DLY Position

Definition at line 9643 of file Mini51Series.h.

## ◆ UART_TOR_TOIC_Msk

#define UART_TOR_TOIC_Msk (0xfful << UART_TOR_TOIC_Pos)

UART_T::TOR: TOIC Mask

Definition at line 9641 of file Mini51Series.h.

## ◆ UART_TOR_TOIC_Pos

#define UART_TOR_TOIC_Pos (0)

UART_T::TOR: TOIC Position

Definition at line 9640 of file Mini51Series.h.

## ◆ WDT_WTCR_DBGACK_WDT_Msk

#define WDT_WTCR_DBGACK_WDT_Msk (0x1ul << WDT_WTCR_DBGACK_WDT_Pos)

WDT_T::WTCR: DBGACK_WDT Mask

Definition at line 9865 of file Mini51Series.h.

## ◆ WDT_WTCR_DBGACK_WDT_Pos

#define WDT_WTCR_DBGACK_WDT_Pos (31)

WDT_T::WTCR: DBGACK_WDT Position

Definition at line 9864 of file Mini51Series.h.

## ◆ WDT_WTCR_WTE_Msk

#define WDT_WTCR_WTE_Msk (0x1ul << WDT_WTCR_WTE_Pos)

WDT_T::WTCR: WTE Mask

Definition at line 9859 of file Mini51Series.h.

## ◆ WDT_WTCR_WTE_Pos

#define WDT_WTCR_WTE_Pos (7)

WDT_T::WTCR: WTE Position

Definition at line 9858 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIE_Msk

#define WDT_WTCR_WTIE_Msk (0x1ul << WDT_WTCR_WTIE_Pos)

WDT_T::WTCR: WTIE Mask

Definition at line 9856 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIE_Pos

#define WDT_WTCR_WTIE_Pos (6)

WDT_T::WTCR: WTIE Position

Definition at line 9855 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIF_Msk

#define WDT_WTCR_WTIF_Msk (0x1ul << WDT_WTCR_WTIF_Pos)

WDT_T::WTCR: WTIF Mask

Definition at line 9847 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIF_Pos

#define WDT_WTCR_WTIF_Pos (3)

WDT_T::WTCR: WTIF Position

Definition at line 9846 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIS_Msk

#define WDT_WTCR_WTIS_Msk (0x7ul << WDT_WTCR_WTIS_Pos)

WDT_T::WTCR: WTIS Mask

Definition at line 9862 of file Mini51Series.h.

## ◆ WDT_WTCR_WTIS_Pos

#define WDT_WTCR_WTIS_Pos (8)

WDT_T::WTCR: WTIS Position

Definition at line 9861 of file Mini51Series.h.

## ◆ WDT_WTCR_WTR_Msk

#define WDT_WTCR_WTR_Msk (0x1ul << WDT_WTCR_WTR_Pos)

WDT_T::WTCR: WTR Mask

Definition at line 9838 of file Mini51Series.h.

## ◆ WDT_WTCR_WTR_Pos

#define WDT_WTCR_WTR_Pos (0)

    @addtogroup WDT_CONST WDT Bit Field Definition
    Constant Definitions for WDT Controller

WDT_T::WTCR: WTR Position

Definition at line 9837 of file Mini51Series.h.

## ◆ WDT_WTCR_WTRE_Msk

#define WDT_WTCR_WTRE_Msk (0x1ul << WDT_WTCR_WTRE_Pos)

WDT_T::WTCR: WTRE Mask

Definition at line 9841 of file Mini51Series.h.

## ◆ WDT_WTCR_WTRE_Pos

#define WDT_WTCR_WTRE_Pos (1)

WDT_T::WTCR: WTRE Position

Definition at line 9840 of file Mini51Series.h.

## ◆ WDT_WTCR_WTRF_Msk

#define WDT_WTCR_WTRF_Msk (0x1ul << WDT_WTCR_WTRF_Pos)

WDT_T::WTCR: WTRF Mask

Definition at line 9844 of file Mini51Series.h.

## ◆ WDT_WTCR_WTRF_Pos

#define WDT_WTCR_WTRF_Pos (2)

WDT_T::WTCR: WTRF Position

Definition at line 9843 of file Mini51Series.h.

## ◆ WDT_WTCR_WTWKE_Msk

#define WDT_WTCR_WTWKE_Msk (0x1ul << WDT_WTCR_WTWKE_Pos)

WDT_T::WTCR: WTWKE Mask

Definition at line 9850 of file Mini51Series.h.

## ◆ WDT_WTCR_WTWKE_Pos

#define WDT_WTCR_WTWKE_Pos (4)

WDT_T::WTCR: WTWKE Position

Definition at line 9849 of file Mini51Series.h.

## ◆ WDT_WTCR_WTWKF_Msk

#define WDT_WTCR_WTWKF_Msk (0x1ul << WDT_WTCR_WTWKF_Pos)

WDT_T::WTCR: WTWKF Mask

Definition at line 9853 of file Mini51Series.h.

## ◆ WDT_WTCR_WTWKF_Pos

#define WDT_WTCR_WTWKF_Pos (5)

WDT_T::WTCR: WTWKF Position

Definition at line 9852 of file Mini51Series.h.