| Mini51 BSP V3.02.002 The Board Support Package for Mini51 Series

timer.h
Go to the documentation of this file.
1 /**************************************************************************/
12 #ifndef __TIMER_H__
13 #define __TIMER_H__
14
15 #ifdef __cplusplus
16 extern "C"
17 {
18 #endif
19
20
33 #define TIMER_ONESHOT_MODE (0UL)
34 #define TIMER_PERIODIC_MODE (1UL << TIMER_TCSR_MODE_Pos)
35 #define TIMER_TOGGLE_MODE (2UL << TIMER_TCSR_MODE_Pos)
36 #define TIMER_CONTINUOUS_MODE (3UL << TIMER_TCSR_MODE_Pos)
37 #define TIMER_CAPTURE_FREE_COUNTING_MODE (0UL)
38 #define TIMER_CAPTURE_TRIGGER_COUNTING_MODE (TIMER_TEXCON_CAP_MODE_Msk)
39 #define TIMER_CAPTURE_COUNTER_RESET_MODE (TIMER_TEXCON_RSTCAPSEL_Msk)
40 #define TIMER_CAPTURE_FALLING_EDGE (0UL)
41 #define TIMER_CAPTURE_RISING_EDGE (1UL << TIMER_TEXCON_TEX_EDGE_Pos)
42 #define TIMER_CAPTURE_FALLING_THEN_RISING_EDGE (2UL << TIMER_TEXCON_TEX_EDGE_Pos)
43 #define TIMER_CAPTURE_RISING_THEN_FALLING_EDGE (3UL << TIMER_TEXCON_TEX_EDGE_Pos)
44 #define TIMER_COUNTER_RISING_EDGE (TIMER_TEXCON_TX_PHASE_Msk)
45 #define TIMER_COUNTER_FALLING_EDGE (0UL)
46 #define TIMER_TOGGLE_TX (0UL)
47 #define TIMER_TOGGLE_TXEX (TIMER_TCSR_TOGGLE_PIN_Msk)
49 /* end of group MINI51_TIMER_EXPORTED_CONSTANTS */
50
51
63 #define TIMER_SET_CMP_VALUE(timer, u32Value) ((timer)->TCMPR = (u32Value))
64
73 #define TIMER_SET_PRESCALE_VALUE(timer, u32Value) ((timer)->TCSR = ((timer)->TCSR & ~TIMER_TCSR_PRESCALE_Msk) | (u32Value))
74
83 #define TIMER_IS_ACTIVE(timer) ((timer)->TCSR & TIMER_TCSR_CACT_Msk ? 1 : 0)
84
94 #define TIMER_SELECT_TOUT_PIN(timer, u32ToutSel) ((timer)->TCSR = ((timer)->TCSR & ~TIMER_TCSR_TOGGLE_PIN_Msk) | (u32ToutSel))
95
96
97
103 __STATIC_INLINE void TIMER_Start(TIMER_T *timer)
104 {
105 timer->TCSR |= TIMER_TCSR_CEN_Msk;
106 }
107
113 __STATIC_INLINE void TIMER_Stop(TIMER_T *timer)
114 {
115 timer->TCSR &= ~TIMER_TCSR_CEN_Msk;
116 }
117
124 __STATIC_INLINE void TIMER_EnableWakeup(TIMER_T *timer)
125 {
126 timer->TCSR |= TIMER_TCSR_WAKE_EN_Msk;
127 }
128
134 __STATIC_INLINE void TIMER_DisableWakeup(TIMER_T *timer)
135 {
136 timer->TCSR &= ~TIMER_TCSR_WAKE_EN_Msk;
137 }
138
139
145 __STATIC_INLINE void TIMER_EnableCaptureDebounce(TIMER_T *timer)
146 {
147 timer->TEXCON |= TIMER_TEXCON_TEXDB_Msk;
148 }
149
155 __STATIC_INLINE void TIMER_DisableCaptureDebounce(TIMER_T *timer)
156 {
157 timer->TEXCON &= ~TIMER_TEXCON_TEXDB_Msk;
158 }
159
160
166 __STATIC_INLINE void TIMER_EnableEventCounterDebounce(TIMER_T *timer)
167 {
168 timer->TEXCON |= TIMER_TEXCON_TCDB_Msk;
169 }
170
176 __STATIC_INLINE void TIMER_DisableEventCounterDebounce(TIMER_T *timer)
177 {
178 timer->TEXCON &= ~TIMER_TEXCON_TCDB_Msk;
179 }
180
186 __STATIC_INLINE void TIMER_EnableInt(TIMER_T *timer)
187 {
188 timer->TCSR |= TIMER_TCSR_IE_Msk;
189 }
190
196 __STATIC_INLINE void TIMER_DisableInt(TIMER_T *timer)
197 {
198 timer->TCSR &= ~TIMER_TCSR_IE_Msk;
199 }
200
206 __STATIC_INLINE void TIMER_EnableCaptureInt(TIMER_T *timer)
207 {
208 timer->TEXCON |= TIMER_TEXCON_TEXIEN_Msk;
209 }
210
216 __STATIC_INLINE void TIMER_DisableCaptureInt(TIMER_T *timer)
217 {
218 timer->TEXCON &= ~TIMER_TEXCON_TEXIEN_Msk;
219 }
220
228 __STATIC_INLINE uint32_t TIMER_GetIntFlag(TIMER_T *timer)
229 {
230 return(timer->TISR & TIMER_TISR_TIF_Msk ? 1 : 0);
231 }
232
238 __STATIC_INLINE void TIMER_ClearIntFlag(TIMER_T *timer)
239 {
240 timer->TISR = TIMER_TISR_TIF_Msk;
241 }
242
250 __STATIC_INLINE uint32_t TIMER_GetCaptureIntFlag(TIMER_T *timer)
251 {
252 return timer->TEXISR;
253 }
254
260 __STATIC_INLINE void TIMER_ClearCaptureIntFlag(TIMER_T *timer)
261 {
262 timer->TEXISR = TIMER_TEXISR_TEXIF_Msk;
263 }
264
272 __STATIC_INLINE uint32_t TIMER_GetWakeupFlag(TIMER_T *timer)
273 {
274 return (timer->TISR & TIMER_TISR_TWF_Msk ? 1 : 0);
275 }
276
282 __STATIC_INLINE void TIMER_ClearWakeupFlag(TIMER_T *timer)
283 {
284 timer->TISR = TIMER_TISR_TWF_Msk;
285 }
286
292 __STATIC_INLINE uint32_t TIMER_GetCaptureData(TIMER_T *timer)
293 {
294 return timer->TCAP;
295 }
296
302 __STATIC_INLINE uint32_t TIMER_GetCounter(TIMER_T *timer)
303 {
304 return timer->TDR;
305 }
306
307 uint32_t TIMER_Open(TIMER_T *timer, uint32_t u32Mode, uint32_t u32Freq);
308 void TIMER_Close(TIMER_T *timer);
309 void TIMER_Delay(TIMER_T *timer, uint32_t u32Usec);
310 void TIMER_EnableCapture(TIMER_T *timer, uint32_t u32CapMode, uint32_t u32Edge);
311 void TIMER_DisableCapture(TIMER_T *timer);
312 void TIMER_EnableEventCounter(TIMER_T *timer, uint32_t u32Edge);
313 void TIMER_DisableEventCounter(TIMER_T *timer);
314 uint32_t TIMER_GetModuleClock(TIMER_T *timer);
315
316 /* end of group MINI51_TIMER_EXPORTED_FUNCTIONS */
318 /* end of group MINI51_TIMER_Driver */
320 /* end of group MINI51_Device_Driver */
322
323 #ifdef __cplusplus
324 }
325 #endif
326
327 #endif //__TIMER_H__
328
329 /*** (C) COPYRIGHT 2013 Nuvoton Technology Corp. ***/
TIMER_TISR_TWF_Msk
#define TIMER_TISR_TWF_Msk
Definition: Mini51Series.h:8521
TIMER_EnableCaptureDebounce
__STATIC_INLINE void TIMER_EnableCaptureDebounce(TIMER_T *timer)
This function is used to enable the capture pin detection de-bounce function.
Definition: timer.h:145
TIMER_EnableEventCounterDebounce
__STATIC_INLINE void TIMER_EnableEventCounterDebounce(TIMER_T *timer)
This function is used to enable the counter pin detection de-bounce function.
Definition: timer.h:166
TIMER_TEXCON_TEXIEN_Msk
#define TIMER_TEXCON_TEXIEN_Msk
Definition: Mini51Series.h:8542
TIMER_TISR_TIF_Msk
#define TIMER_TISR_TIF_Msk
Definition: Mini51Series.h:8518
TIMER_T::TEXCON
__IO uint32_t TEXCON
Definition: Mini51Series.h:8461
TIMER_Close
void TIMER_Close(TIMER_T *timer)
This API stops Timer counting and disable the Timer interrupt function.
Definition: timer.c:73
TIMER_DisableCaptureInt
__STATIC_INLINE void TIMER_DisableCaptureInt(TIMER_T *timer)
This function is used to disable the Timer capture trigger interrupt function.
Definition: timer.h:216
TIMER_GetCounter
__STATIC_INLINE uint32_t TIMER_GetCounter(TIMER_T *timer)
This function reports the current timer counter value.
Definition: timer.h:302
TIMER_DisableInt
__STATIC_INLINE void TIMER_DisableInt(TIMER_T *timer)
This function is used to disable the Timer time-out interrupt function.
Definition: timer.h:196
TIMER_TCSR_CEN_Msk
#define TIMER_TCSR_CEN_Msk
Definition: Mini51Series.h:8509
TIMER_TCSR_IE_Msk
#define TIMER_TCSR_IE_Msk
Definition: Mini51Series.h:8506
TIMER_GetCaptureIntFlag
__STATIC_INLINE uint32_t TIMER_GetCaptureIntFlag(TIMER_T *timer)
This function indicates Timer capture interrupt occurred or not.
Definition: timer.h:250
TIMER_DisableCapture
void TIMER_DisableCapture(TIMER_T *timer)
This API is used to disable the Timer capture function.
Definition: timer.c:159
TIMER_EnableInt
__STATIC_INLINE void TIMER_EnableInt(TIMER_T *timer)
This function is used to enable the Timer time-out interrupt function.
Definition: timer.h:186
TIMER_DisableCaptureDebounce
__STATIC_INLINE void TIMER_DisableCaptureDebounce(TIMER_T *timer)
This function is used to disable the capture pin detection de-bounce function.
Definition: timer.h:155
TIMER_ClearCaptureIntFlag
__STATIC_INLINE void TIMER_ClearCaptureIntFlag(TIMER_T *timer)
This function clears the Timer capture interrupt flag.
Definition: timer.h:260
TIMER_Stop
__STATIC_INLINE void TIMER_Stop(TIMER_T *timer)
This function is used to stop Timer counting.
Definition: timer.h:113
TIMER_TEXCON_TCDB_Msk
#define TIMER_TEXCON_TCDB_Msk
Definition: Mini51Series.h:8548
TIMER_GetModuleClock
uint32_t TIMER_GetModuleClock(TIMER_T *timer)
This API is used to get the clock frequency of Timer.
Definition: timer.c:196
TIMER_EnableCapture
void TIMER_EnableCapture(TIMER_T *timer, uint32_t u32CapMode, uint32_t u32Edge)
This API is used to enable timer capture function with specified mode and capture edge.
Definition: timer.c:145
TIMER_T::TCAP
__I uint32_t TCAP
Definition: Mini51Series.h:8460
TIMER_TCSR_WAKE_EN_Msk
#define TIMER_TCSR_WAKE_EN_Msk
Definition: Mini51Series.h:8491
TIMER_DisableEventCounterDebounce
__STATIC_INLINE void TIMER_DisableEventCounterDebounce(TIMER_T *timer)
This function is used to disable the counter pin detection de-bounce function.
Definition: timer.h:176
TIMER_EnableWakeup
__STATIC_INLINE void TIMER_EnableWakeup(TIMER_T *timer)
This function is used to enable the Timer wake-up function.
Definition: timer.h:124
TIMER_T::TEXISR
__IO uint32_t TEXISR
Definition: Mini51Series.h:8462
TIMER_T::TDR
__I uint32_t TDR
Definition: Mini51Series.h:8459
TIMER_ClearWakeupFlag
__STATIC_INLINE void TIMER_ClearWakeupFlag(TIMER_T *timer)
This function clears the Timer wakeup interrupt flag.
Definition: timer.h:282
TIMER_DisableWakeup
__STATIC_INLINE void TIMER_DisableWakeup(TIMER_T *timer)
This function is used to disable the Timer wake-up function.
Definition: timer.h:134
TIMER_T::TISR
__IO uint32_t TISR
Definition: Mini51Series.h:8458
TIMER_T
Definition: Mini51Series.h:8097
TIMER_T::TCSR
__IO uint32_t TCSR
Definition: Mini51Series.h:8456
TIMER_EnableEventCounter
void TIMER_EnableEventCounter(TIMER_T *timer, uint32_t u32Edge)
This function is used to enable the Timer counter function with specify detection edge.
Definition: timer.c:174
TIMER_Delay
void TIMER_Delay(TIMER_T *timer, uint32_t u32Usec)
This API is used to create a delay loop for u32usec micro seconds.
Definition: timer.c:88
TIMER_GetCaptureData
__STATIC_INLINE uint32_t TIMER_GetCaptureData(TIMER_T *timer)
This function gets the Timer capture data.
Definition: timer.h:292
TIMER_EnableCaptureInt
__STATIC_INLINE void TIMER_EnableCaptureInt(TIMER_T *timer)
This function is used to enable the Timer capture trigger interrupt function.
Definition: timer.h:206
TIMER_Open
uint32_t TIMER_Open(TIMER_T *timer, uint32_t u32Mode, uint32_t u32Freq)
This API is used to configure timer to operate in specified mode and frequency. If timer cannot work ...
Definition: timer.c:42
TIMER_TEXCON_TEXDB_Msk
#define TIMER_TEXCON_TEXDB_Msk
Definition: Mini51Series.h:8545
TIMER_ClearIntFlag
__STATIC_INLINE void TIMER_ClearIntFlag(TIMER_T *timer)
This function clears the Timer time-out interrupt flag.
Definition: timer.h:238
TIMER_TEXISR_TEXIF_Msk
#define TIMER_TEXISR_TEXIF_Msk
Definition: Mini51Series.h:8554
TIMER_GetWakeupFlag
__STATIC_INLINE uint32_t TIMER_GetWakeupFlag(TIMER_T *timer)
This function indicates Timer has waked up system or not.
Definition: timer.h:272
TIMER_Start
__STATIC_INLINE void TIMER_Start(TIMER_T *timer)
This function is used to start Timer counting.
Definition: timer.h:103
TIMER_GetIntFlag
__STATIC_INLINE uint32_t TIMER_GetIntFlag(TIMER_T *timer)
This function indicates Timer time-out interrupt occurred or not.
Definition: timer.h:228
TIMER_DisableEventCounter
void TIMER_DisableEventCounter(TIMER_T *timer)
This API is used to disable the Timer event counter function.
Definition: timer.c:185