| MINI55_BSP V3.02.004 The Board Support Package for Mini55 Series MCU

Data Structures | Macros | Typedefs | Enumerations
Mini55Series.h File Reference

Mini55 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Mini55 series MCU. More...

`#include "core_cm0.h"`
`#include "system_Mini55Series.h"`
`#include <stdint.h>`
`#include "sys.h"`
`#include "clk.h"`
`#include "acmp.h"`
`#include "adc.h"`
`#include "fmc.h"`
`#include "gpio.h"`
`#include "hdiv.h"`
`#include "i2c.h"`
`#include "pwm.h"`
`#include "spi.h"`
`#include "timer.h"`
`#include "uart.h"`
`#include "wdt.h"`
Include dependency graph for Mini55Series.h:
This graph shows which files directly or indirectly include this file:

Go to the source code of this file.

## Data Structures
struct | ACMP_T
struct | ADC_T
struct | CLK_T
struct | FMC_T
struct | GPIO_T
struct | GPIO_DB_T
struct | HDIV_T
struct | I2C_T
struct | INTR_T
struct | PWM_T
struct | SPI_T
struct | SYS_T
struct | TIMER_T
struct | TIMER_AC_T
struct | UART_T
struct | WDT_T

## Macros
#define | __CM0_REV 0x0201
#define | __NVIC_PRIO_BITS 2
#define | __Vendor_SysTickConfig 0
#define | __MPU_PRESENT 0
#define | __FPU_PRESENT 0
#define | FLASH_BASE ((uint32_t)0x00000000)
| Flash base address. More...
#define | SRAM_BASE ((uint32_t)0x20000000)
| SRAM base address. More...
#define | APB1PERIPH_BASE ((uint32_t)0x40000000)
| APB1 base address. More...
#define | APB2PERIPH_BASE ((uint32_t)0x40100000)
| APB2 base address. More...
#define | AHBPERIPH_BASE ((uint32_t)0x50000000)
| AHB base address. More...
#define | WDT_BASE (APB1PERIPH_BASE + 0x04000)
| WDT register base address. More...
#define | TIMER0_BASE (APB1PERIPH_BASE + 0x10000)
| TIMER0 register base address. More...
#define | TIMER1_BASE (APB1PERIPH_BASE + 0x10020)
| TIMER1 register base address. More...
#define | TIMER_AC_BASE (APB1PERIPH_BASE + 0x10040)
| TIMER Advance Capture register base address. More...
#define | I2C_BASE (APB1PERIPH_BASE + 0x20000)
| I2C register base address. More...
#define | SPI_BASE (APB1PERIPH_BASE + 0x30000)
| SPI register base address. More...
#define | PWM_BASE (APB1PERIPH_BASE + 0x40000)
| PWM register base address. More...
#define | UART0_BASE (APB1PERIPH_BASE + 0x50000)
| UART0 register base address. More...
#define | UART1_BASE (APB2PERIPH_BASE + 0x50000)
| UART1 register base address. More...
#define | ACMP_BASE (APB1PERIPH_BASE + 0xD0000)
| ACMP register base address. More...
#define | ADC_BASE (APB1PERIPH_BASE + 0xE0000)
| ADC register base address. More...
#define | SYS_BASE (AHBPERIPH_BASE + 0x00000)
| SYS register base address. More...
#define | CLK_BASE (AHBPERIPH_BASE + 0x00200)
| CLK register base address. More...
#define | INTR_BASE (AHBPERIPH_BASE + 0x00300)
| INT register base address. More...
#define | P0_BASE (AHBPERIPH_BASE + 0x04000)
| GPIO Port 0 register base address. More...
#define | P1_BASE (AHBPERIPH_BASE + 0x04040)
| GPIO Port 1 register base address. More...
#define | P2_BASE (AHBPERIPH_BASE + 0x04080)
| GPIO Port 2 register base address. More...
#define | P3_BASE (AHBPERIPH_BASE + 0x040C0)
| GPIO Port 3 register base address. More...
#define | P4_BASE (AHBPERIPH_BASE + 0x04100)
| GPIO Port 4 register base address. More...
#define | P5_BASE (AHBPERIPH_BASE + 0x04140)
| GPIO Port 5 register base address. More...
#define | GPIO_DBNCECON_BASE (AHBPERIPH_BASE + 0x04180)
| GPIO De-bounce register vase. More...
#define | GPIO_PIN_DATA_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO pin data register base address. More...
#define | GPIOBIT0_BASE (AHBPERIPH_BASE + 0x04200)
| GPIO Port 0 bit access register base address. More...
#define | GPIOBIT1_BASE (AHBPERIPH_BASE + 0x04220)
| GPIO Port 1 bit access register base address. More...
#define | GPIOBIT2_BASE (AHBPERIPH_BASE + 0x04240)
| GPIO Port 2 bit access register base address. More...
#define | GPIOBIT3_BASE (AHBPERIPH_BASE + 0x04260)
| GPIO Port 3 bit access register base address. More...
#define | GPIOBIT4_BASE (AHBPERIPH_BASE + 0x04280)
| GPIO Port 4 bit access register base address. More...
#define | GPIOBIT5_BASE (AHBPERIPH_BASE + 0x042A0)
| GPIO Port 5 bit access register base address. More...
#define | FMC_BASE (AHBPERIPH_BASE + 0x0C000)
| FMC register base address. More...
#define | HDIV_BASE (AHBPERIPH_BASE + 0x14000)
| HDIV register base address. More...
#define | WDT ((WDT_T *) WDT_BASE)
| Pointer to WDT register structure. More...
#define | TIMER0 ((TIMER_T *) TIMER0_BASE)
| Pointer to Timer 0 register structure. More...
#define | TIMER1 ((TIMER_T *) TIMER1_BASE)
| Pointer to Timer 1 register structure. More...
#define | TIMERAC ((TIMER_AC_T *) TIMER_AC_BASE)
| Pointer to Timer Advance Capture register structure. More...
#define | I2C ((I2C_T *) I2C_BASE)
| Pointer to I2C register structure. More...
#define | I2C0 ((I2C_T *) I2C_BASE)
| Pointer to I2C register structure. More...
#define | SPI ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | SPI0 ((SPI_T *) SPI_BASE)
| Pointer to SPI register structure. More...
#define | PWM ((PWM_T *) PWM_BASE)
| Pointer to PWM register structure. More...
#define | UART ((UART_T *) UART0_BASE)
| Pointer to UART0 register structure (compatible with Mini51) More...
#define | UART0 ((UART_T *) UART0_BASE)
| Pointer to UART0 register structure. More...
#define | UART1 ((UART_T *) UART1_BASE)
| Pointer to UART1 register structure. More...
#define | ADC ((ADC_T *) ADC_BASE)
| Pointer to ADC register structure. More...
#define | ACMP ((ACMP_T *) ACMP_BASE)
| Pointer to ACMP register structure. More...
#define | SYS ((SYS_T *) SYS_BASE)
| Pointer to SYS register structure. More...
#define | CLK ((CLK_T *) CLK_BASE)
| Pointer to CLK register structure. More...
#define | INTR ((INTR_T *) INTR_BASE)
| Pointer to INT register structure. More...
#define | P0 ((GPIO_T *) P0_BASE)
| Pointer to GPIO port 0 register structure. More...
#define | P1 ((GPIO_T *) P1_BASE)
| Pointer to GPIO port 1 register structure. More...
#define | P2 ((GPIO_T *) P2_BASE)
| Pointer to GPIO port 2 register structure. More...
#define | P3 ((GPIO_T *) P3_BASE)
| Pointer to GPIO port 3 register structure. More...
#define | P4 ((GPIO_T *) P4_BASE)
| Pointer to GPIO port 4 register structure. More...
#define | P5 ((GPIO_T *) P5_BASE)
| Pointer to GPIO port 5 register structure. More...
#define | GPIO ((GPIO_DB_T *) GPIO_DBNCECON_BASE)
| Pointer to GPIO de-bounce register structure. More...
#define | FMC ((FMC_T *) FMC_BASE)
| Pointer to FMC register structure. More...
#define | HDIV ((HDIV_T *) HDIV_BASE)
| Pointer to HDIV register structure. More...
#define | M8(addr) (*((vu8 *) (addr)))
| Get a 8-bit unsigned value from specified address. More...
#define | M16(addr) (*((vu16 *) (addr)))
| Get a 16-bit unsigned value from specified address. More...
#define | M32(addr) (*((vu32 *) (addr)))
| Get a 32-bit unsigned value from specified address. More...
#define | outpw(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inpw(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outps(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inps(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outpb(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inpb(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | outp32(port, value) *((volatile unsigned int *)(port)) = value
| Set a 32-bit unsigned value to specified I/O port. More...
#define | inp32(port) (*((volatile unsigned int *)(port)))
| Get a 32-bit unsigned value from specified I/O port. More...
#define | outp16(port, value) *((volatile unsigned short *)(port)) = value
| Set a 16-bit unsigned value to specified I/O port. More...
#define | inp16(port) (*((volatile unsigned short *)(port)))
| Get a 16-bit unsigned value from specified I/O port. More...
#define | outp8(port, value) *((volatile unsigned char *)(port)) = value
| Set a 8-bit unsigned value to specified I/O port. More...
#define | inp8(port) (*((volatile unsigned char *)(port)))
| Get a 8-bit unsigned value from specified I/O port. More...
#define | NULL (0)
| NULL pointer. More...
#define | TRUE (1)
| Boolean true, define to use in API parameters or return value. More...
#define | FALSE (0)
| Boolean false, define to use in API parameters or return value. More...
#define | ENABLE (1)
| Enable, define to use in API parameters. More...
#define | DISABLE (0)
| Disable, define to use in API parameters. More...
#define | BIT0 (0x00000001)
| Bit 0 mask of an 32 bit integer. More...
#define | BIT1 (0x00000002)
| Bit 1 mask of an 32 bit integer. More...
#define | BIT2 (0x00000004)
| Bit 2 mask of an 32 bit integer. More...
#define | BIT3 (0x00000008)
| Bit 3 mask of an 32 bit integer. More...
#define | BIT4 (0x00000010)
| Bit 4 mask of an 32 bit integer. More...
#define | BIT5 (0x00000020)
| Bit 5 mask of an 32 bit integer. More...
#define | BIT6 (0x00000040)
| Bit 6 mask of an 32 bit integer. More...
#define | BIT7 (0x00000080)
| Bit 7 mask of an 32 bit integer. More...
#define | BIT8 (0x00000100)
| Bit 8 mask of an 32 bit integer. More...
#define | BIT9 (0x00000200)
| Bit 9 mask of an 32 bit integer. More...
#define | BIT10 (0x00000400)
| Bit 10 mask of an 32 bit integer. More...
#define | BIT11 (0x00000800)
| Bit 11 mask of an 32 bit integer. More...
#define | BIT12 (0x00001000)
| Bit 12 mask of an 32 bit integer. More...
#define | BIT13 (0x00002000)
| Bit 13 mask of an 32 bit integer. More...
#define | BIT14 (0x00004000)
| Bit 14 mask of an 32 bit integer. More...
#define | BIT15 (0x00008000)
| Bit 15 mask of an 32 bit integer. More...
#define | BIT16 (0x00010000)
| Bit 16 mask of an 32 bit integer. More...
#define | BIT17 (0x00020000)
| Bit 17 mask of an 32 bit integer. More...
#define | BIT18 (0x00040000)
| Bit 18 mask of an 32 bit integer. More...
#define | BIT19 (0x00080000)
| Bit 19 mask of an 32 bit integer. More...
#define | BIT20 (0x00100000)
| Bit 20 mask of an 32 bit integer. More...
#define | BIT21 (0x00200000)
| Bit 21 mask of an 32 bit integer. More...
#define | BIT22 (0x00400000)
| Bit 22 mask of an 32 bit integer. More...
#define | BIT23 (0x00800000)
| Bit 23 mask of an 32 bit integer. More...
#define | BIT24 (0x01000000)
| Bit 24 mask of an 32 bit integer. More...
#define | BIT25 (0x02000000)
| Bit 25 mask of an 32 bit integer. More...
#define | BIT26 (0x04000000)
| Bit 26 mask of an 32 bit integer. More...
#define | BIT27 (0x08000000)
| Bit 27 mask of an 32 bit integer. More...
#define | BIT28 (0x10000000)
| Bit 28 mask of an 32 bit integer. More...
#define | BIT29 (0x20000000)
| Bit 29 mask of an 32 bit integer. More...
#define | BIT30 (0x40000000)
| Bit 30 mask of an 32 bit integer. More...
#define | BIT31 (0x80000000)
| Bit 31 mask of an 32 bit integer. More...
#define | BYTE0_Msk (0x000000FF)
| Mask to get bit0~bit7 from a 32 bit integer. More...
#define | BYTE1_Msk (0x0000FF00)
| Mask to get bit8~bit15 from a 32 bit integer. More...
#define | BYTE2_Msk (0x00FF0000)
| Mask to get bit16~bit23 from a 32 bit integer. More...
#define | BYTE3_Msk (0xFF000000)
| Mask to get bit24~bit31 from a 32 bit integer. More...
#define | GET_BYTE0(u32Param) ((u32Param & BYTE0_Msk) )
#define | GET_BYTE1(u32Param) ((u32Param & BYTE1_Msk) >> 8)
#define | GET_BYTE2(u32Param) ((u32Param & BYTE2_Msk) >> 16)
#define | GET_BYTE3(u32Param) ((u32Param & BYTE3_Msk) >> 24)
#define | ACMP_CTL_ACMPEN_Pos (0)
#define | ACMP_CTL_ACMPEN_Msk (0x1ul << ACMP_CTL_ACMPEN_Pos)
#define | ACMP_CTL_ACMPIE_Pos (1)
#define | ACMP_CTL_ACMPIE_Msk (0x1ul << ACMP_CTL_ACMPIE_Pos)
#define | ACMP_CTL_HYSSEL_Pos (2)
#define | ACMP_CTL_HYSSEL_Msk (0x3ul << ACMP_CTL_HYSSEL_Pos)
#define | ACMP_CTL_NEGSEL_Pos (4)
#define | ACMP_CTL_NEGSEL_Msk (0x1ul << ACMP_CTL_NEGSEL_Pos)
#define | ACMP_CTL_RTRGEN_Pos (8)
#define | ACMP_CTL_RTRGEN_Msk (0x1ul << ACMP_CTL_RTRGEN_Pos)
#define | ACMP_CTL_FTRGEN_Pos (9)
#define | ACMP_CTL_FTRGEN_Msk (0x1ul << ACMP_CTL_FTRGEN_Pos)
#define | ACMP_CTL_SMPTSEL_Pos (12)
#define | ACMP_CTL_SMPTSEL_Msk (0x1ul << ACMP_CTL_SMPTSEL_Pos)
#define | ACMP_CTL_POSSEL_Pos (29)
#define | ACMP_CTL_POSSEL_Msk (0x3ul << ACMP_CTL_POSSEL_Pos)
#define | ACMP_STATUS_ACMPIF0_Pos (0)
#define | ACMP_STATUS_ACMPIF0_Msk (0x1ul << ACMP_STATUS_ACMPIF0_Pos)
#define | ACMP_STATUS_ACMPIF1_Pos (1)
#define | ACMP_STATUS_ACMPIF1_Msk (0x1ul << ACMP_STATUS_ACMPIF1_Pos)
#define | ACMP_STATUS_ACMPO0_Pos (2)
#define | ACMP_STATUS_ACMPO0_Msk (0x1ul << ACMP_STATUS_ACMPO0_Pos)
#define | ACMP_STATUS_ACMPO1_Pos (3)
#define | ACMP_STATUS_ACMPO1_Msk (0x1ul << ACMP_STATUS_ACMPO1_Pos)
#define | ACMP_VREF_CRVCTL_Pos (0)
#define | ACMP_VREF_CRVCTL_Msk (0xful << ACMP_VREF_CRVCTL_Pos)
#define | ACMP_VREF_IREFSEL_Pos (7)
#define | ACMP_VREF_IREFSEL_Msk (0x1ul << ACMP_VREF_IREFSEL_Pos)
#define | ADC_DAT_RESULT_Pos (0)
#define | ADC_DAT_RESULT_Msk (0x3fful << ADC_DAT_RESULT_Pos)
#define | ADC_DAT_OV_Pos (16)
#define | ADC_DAT_OV_Msk (0x1ul << ADC_DAT_OV_Pos)
#define | ADC_DAT_VALID_Pos (17)
#define | ADC_DAT_VALID_Msk (0x1ul << ADC_DAT_VALID_Pos)
#define | ADC_CTL_ADCEN_Pos (0)
#define | ADC_CTL_ADCEN_Msk (0x1ul << ADC_CTL_ADCEN_Pos)
#define | ADC_CTL_ADCIEN_Pos (1)
#define | ADC_CTL_ADCIEN_Msk (0x1ul << ADC_CTL_ADCIEN_Pos)
#define | ADC_CTL_HWTRGSEL_Pos (4)
#define | ADC_CTL_HWTRGSEL_Msk (0x3ul << ADC_CTL_HWTRGSEL_Pos)
#define | ADC_CTL_HWTRGCOND_Pos (6)
#define | ADC_CTL_HWTRGCOND_Msk (0x1ul << ADC_CTL_HWTRGCOND_Pos)
#define | ADC_CTL_HWTRGEN_Pos (8)
#define | ADC_CTL_HWTRGEN_Msk (0x1ul << ADC_CTL_HWTRGEN_Pos)
#define | ADC_CTL_SWTRG_Pos (11)
#define | ADC_CTL_SWTRG_Msk (0x1ul << ADC_CTL_SWTRG_Pos)
#define | ADC_CTL_VREFSEL_Pos (12)
#define | ADC_CTL_VREFSEL_Msk (0x1ul << ADC_CTL_VREFSEL_Pos)
#define | ADC_CHEN_CHEN0_Pos (0)
#define | ADC_CHEN_CHEN0_Msk (0x1ul << ADC_CHEN_CHEN0_Pos)
#define | ADC_CHEN_CHEN1_Pos (1)
#define | ADC_CHEN_CHEN1_Msk (0x1ul << ADC_CHEN_CHEN1_Pos)
#define | ADC_CHEN_CHEN2_Pos (2)
#define | ADC_CHEN_CHEN2_Msk (0x1ul << ADC_CHEN_CHEN2_Pos)
#define | ADC_CHEN_CHEN3_Pos (3)
#define | ADC_CHEN_CHEN3_Msk (0x1ul << ADC_CHEN_CHEN3_Pos)
#define | ADC_CHEN_CHEN4_Pos (4)
#define | ADC_CHEN_CHEN4_Msk (0x1ul << ADC_CHEN_CHEN4_Pos)
#define | ADC_CHEN_CHEN5_Pos (5)
#define | ADC_CHEN_CHEN5_Msk (0x1ul << ADC_CHEN_CHEN5_Pos)
#define | ADC_CHEN_CHEN6_Pos (6)
#define | ADC_CHEN_CHEN6_Msk (0x1ul << ADC_CHEN_CHEN6_Pos)
#define | ADC_CHEN_CHEN7_Pos (7)
#define | ADC_CHEN_CHEN7_Msk (0x1ul << ADC_CHEN_CHEN7_Pos)
#define | ADC_CHEN_CH7SEL_Pos (8)
#define | ADC_CHEN_CH7SEL_Msk (0x1ul << ADC_CHEN_CH7SEL_Pos)
#define | ADC_CHEN_CHEN8_Pos (9)
#define | ADC_CHEN_CHEN8_Msk (0x1ul << ADC_CHEN_CHEN8_Pos)
#define | ADC_CHEN_CHEN9_Pos (10)
#define | ADC_CHEN_CHEN9_Msk (0x1ul << ADC_CHEN_CHEN9_Pos)
#define | ADC_CHEN_CHEN10_Pos (11)
#define | ADC_CHEN_CHEN10_Msk (0x1ul << ADC_CHEN_CHEN10_Pos)
#define | ADC_CHEN_CHEN11_Pos (12)
#define | ADC_CHEN_CHEN11_Msk (0x1ul << ADC_CHEN_CHEN11_Pos)
#define | ADC_CHEN_BGEN_Pos (13)
#define | ADC_CHEN_BGEN_Msk (0x1ul << ADC_CHEN_BGEN_Pos)
#define | ADC_CMP_ADCMPEN_Pos (0)
#define | ADC_CMP_ADCMPEN_Msk (0x1ul << ADC_CMP_ADCMPEN_Pos)
#define | ADC_CMP_ADCMPIE_Pos (1)
#define | ADC_CMP_ADCMPIE_Msk (0x1ul << ADC_CMP_ADCMPIE_Pos)
#define | ADC_CMP_CMPCOND_Pos (2)
#define | ADC_CMP_CMPCOND_Msk (0x1ul << ADC_CMP_CMPCOND_Pos)
#define | ADC_CMP_CMPCH_Pos (3)
#define | ADC_CMP_CMPCH_Msk (0xful << ADC_CMP_CMPCH_Pos)
#define | ADC_CMP_CMPMCNT_Pos (8)
#define | ADC_CMP_CMPMCNT_Msk (0xful << ADC_CMP_CMPMCNT_Pos)
#define | ADC_CMP_CMPDAT_Pos (16)
#define | ADC_CMP_CMPDAT_Msk (0x3fful << ADC_CMP_CMPDAT_Pos)
#define | ADC_STATUS_ADIF_Pos (0)
#define | ADC_STATUS_ADIF_Msk (0x1ul << ADC_STATUS_ADIF_Pos)
#define | ADC_STATUS_ADCMPF0_Pos (1)
#define | ADC_STATUS_ADCMPF0_Msk (0x1ul << ADC_STATUS_ADCMPF0_Pos)
#define | ADC_STATUS_ADCMPF1_Pos (2)
#define | ADC_STATUS_ADCMPF1_Msk (0x1ul << ADC_STATUS_ADCMPF1_Pos)
#define | ADC_STATUS_BUSY_Pos (3)
#define | ADC_STATUS_BUSY_Msk (0x1ul << ADC_STATUS_BUSY_Pos)
#define | ADC_STATUS_CHANNEL_Pos (4)
#define | ADC_STATUS_CHANNEL_Msk (0x7ul << ADC_STATUS_CHANNEL_Pos)
#define | ADC_STATUS_VALID_Pos (8)
#define | ADC_STATUS_VALID_Msk (0x1ul << ADC_STATUS_VALID_Pos)
#define | ADC_STATUS_OV_Pos (16)
#define | ADC_STATUS_OV_Msk (0x1ul << ADC_STATUS_OV_Pos)
#define | ADC_TRGDLY_DELAY_Pos (0)
#define | ADC_TRGDLY_DELAY_Msk (0xfful << ADC_TRGDLY_DELAY_Pos)
#define | ADC_EXTSMPT_EXTSMPT_Pos (0)
#define | ADC_EXTSMPT_EXTSMPT_Msk (0xful << ADC_EXTSMPT_EXTSMPT_Pos)
#define | ADC_SEQCTL_SEQEN_Pos (0)
#define | ADC_SEQCTL_SEQEN_Msk (0x1ul << ADC_SEQCTL_SEQEN_Pos)
#define | ADC_SEQCTL_SEQTYPE_Pos (1)
#define | ADC_SEQCTL_SEQTYPE_Msk (0x1ul << ADC_SEQCTL_SEQTYPE_Pos)
#define | ADC_SEQCTL_MODESEL_Pos (2)
#define | ADC_SEQCTL_MODESEL_Msk (0x3ul << ADC_SEQCTL_MODESEL_Pos)
#define | ADC_SEQCTL_TRG1TYPE_Pos (8)
#define | ADC_SEQCTL_TRG1TYPE_Msk (0x3ul << ADC_SEQCTL_TRG1TYPE_Pos)
#define | ADC_SEQCTL_TRG1SRC_Pos (10)
#define | ADC_SEQCTL_TRG1SRC_Msk (0x3ul << ADC_SEQCTL_TRG1SRC_Pos)
#define | ADC_SEQCTL_TRG2TYPE_Pos (16)
#define | ADC_SEQCTL_TRG2TYPE_Msk (0x3ul << ADC_SEQCTL_TRG2TYPE_Pos)
#define | ADC_SEQCTL_TRG2SRC_Pos (18)
#define | ADC_SEQCTL_TRG2SRC_Msk (0x3ul << ADC_SEQCTL_TRG2SRC_Pos)
#define | ADC_SEQDAT0_RESULT_Pos (0)
#define | ADC_SEQDAT0_RESULT_Msk (0x3fful << ADC_SEQDAT0_RESULT_Pos)
#define | ADC_SEQDAT0_OV_Pos (16)
#define | ADC_SEQDAT0_OV_Msk (0x1ul << ADC_SEQDAT0_OV_Pos)
#define | ADC_SEQDAT0_VALID_Pos (17)
#define | ADC_SEQDAT0_VALID_Msk (0x1ul << ADC_SEQDAT0_VALID_Pos)
#define | ADC_SEQDAT1_RESULT_Pos (0)
#define | ADC_SEQDAT1_RESULT_Msk (0x3fful << ADC_SEQDAT1_RESULT_Pos)
#define | ADC_SEQDAT1_OV_Pos (16)
#define | ADC_SEQDAT1_OV_Msk (0x1ul << ADC_SEQDAT1_OV_Pos)
#define | ADC_SEQDAT1_VALID_Pos (17)
#define | ADC_SEQDAT1_VALID_Msk (0x1ul << ADC_SEQDAT1_VALID_Pos)
#define | CLK_PWRCTL_XTLEN_Pos (0)
#define | CLK_PWRCTL_XTLEN_Msk (0x3ul << CLK_PWRCTL_XTLEN_Pos)
#define | CLK_PWRCTL_HIRCEN_Pos (2)
#define | CLK_PWRCTL_HIRCEN_Msk (0x1ul << CLK_PWRCTL_HIRCEN_Pos)
#define | CLK_PWRCTL_LIRCEN_Pos (3)
#define | CLK_PWRCTL_LIRCEN_Msk (0x1ul << CLK_PWRCTL_LIRCEN_Pos)
#define | CLK_PWRCTL_PDWKDLY_Pos (4)
#define | CLK_PWRCTL_PDWKDLY_Msk (0x1ul << CLK_PWRCTL_PDWKDLY_Pos)
#define | CLK_PWRCTL_PDWKIEN_Pos (5)
#define | CLK_PWRCTL_PDWKIEN_Msk (0x1ul << CLK_PWRCTL_PDWKIEN_Pos)
#define | CLK_PWRCTL_PDWKIF_Pos (6)
#define | CLK_PWRCTL_PDWKIF_Msk (0x1ul << CLK_PWRCTL_PDWKIF_Pos)
#define | CLK_PWRCTL_PDEN_Pos (7)
#define | CLK_PWRCTL_PDEN_Msk (0x1ul << CLK_PWRCTL_PDEN_Pos)
#define | CLK_PWRCTL_PDLXT_Pos (9)
#define | CLK_PWRCTL_PDLXT_Msk (0x1ul << CLK_PWRCTL_PDLXT_Pos)
#define | CLK_PWRCTL_HXTGAIN_Pos (10)
#define | CLK_PWRCTL_HXTGAIN_Msk (0x3ul << CLK_PWRCTL_HXTGAIN_Pos)
#define | CLK_AHBCLK_ISPCKEN_Pos (2)
#define | CLK_AHBCLK_ISPCKEN_Msk (0x1ul << CLK_AHBCLK_ISPCKEN_Pos)
#define | CLK_AHBCLK_HDIVCKEN_Pos (4)
#define | CLK_AHBCLK_HDIVCKEN_Msk (0x1ul << CLK_AHBCLK_HDIVCKEN_Pos)
#define | CLK_APBCLK_WDTCKEN_Pos (0)
#define | CLK_APBCLK_WDTCKEN_Msk (0x1ul << CLK_APBCLK_WDTCKEN_Pos)
#define | CLK_APBCLK_TMR0CKEN_Pos (2)
#define | CLK_APBCLK_TMR0CKEN_Msk (0x1ul << CLK_APBCLK_TMR0CKEN_Pos)
#define | CLK_APBCLK_TMR1CKEN_Pos (3)
#define | CLK_APBCLK_TMR1CKEN_Msk (0x1ul << CLK_APBCLK_TMR1CKEN_Pos)
#define | CLK_APBCLK_CLKOCKEN_Pos (6)
#define | CLK_APBCLK_CLKOCKEN_Msk (0x1ul << CLK_APBCLK_CLKOCKEN_Pos)
#define | CLK_APBCLK_I2CCKEN_Pos (8)
#define | CLK_APBCLK_I2CCKEN_Msk (0x1ul << CLK_APBCLK_I2CCKEN_Pos)
#define | CLK_APBCLK_SPICKEN_Pos (12)
#define | CLK_APBCLK_SPICKEN_Msk (0x1ul << CLK_APBCLK_SPICKEN_Pos)
#define | CLK_APBCLK_UART0CKEN_Pos (16)
#define | CLK_APBCLK_UART0CKEN_Msk (0x1ul << CLK_APBCLK_UART0CKEN_Pos)
#define | CLK_APBCLK_UART1CKEN_Pos (17)
#define | CLK_APBCLK_UART1CKEN_Msk (0x1ul << CLK_APBCLK_UART1CKEN_Pos)
#define | CLK_APBCLK_PWMCH01CKEN_Pos (20)
#define | CLK_APBCLK_PWMCH01CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH01CKEN_Pos)
#define | CLK_APBCLK_PWMCH23CKEN_Pos (21)
#define | CLK_APBCLK_PWMCH23CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH23CKEN_Pos)
#define | CLK_APBCLK_PWMCH45CKEN_Pos (22)
#define | CLK_APBCLK_PWMCH45CKEN_Msk (0x1ul << CLK_APBCLK_PWMCH45CKEN_Pos)
#define | CLK_APBCLK_ADCCKEN_Pos (28)
#define | CLK_APBCLK_ADCCKEN_Msk (0x1ul << CLK_APBCLK_ADCCKEN_Pos)
#define | CLK_APBCLK_ACMPCKEN_Pos (30)
#define | CLK_APBCLK_ACMPCKEN_Msk (0x1ul << CLK_APBCLK_ACMPCKEN_Pos)
#define | CLK_STATUS_XTLSTB_Pos (0)
#define | CLK_STATUS_XTLSTB_Msk (0x1ul << CLK_STATUS_XTLSTB_Pos)
#define | CLK_STATUS_LIRCSTB_Pos (3)
#define | CLK_STATUS_LIRCSTB_Msk (0x1ul << CLK_STATUS_LIRCSTB_Pos)
#define | CLK_STATUS_HIRCSTB_Pos (4)
#define | CLK_STATUS_HIRCSTB_Msk (0x1ul << CLK_STATUS_HIRCSTB_Pos)
#define | CLK_STATUS_CLKSFAIL_Pos (7)
#define | CLK_STATUS_CLKSFAIL_Msk (0x1ul << CLK_STATUS_CLKSFAIL_Pos)
#define | CLK_CLKSEL0_HCLKSEL_Pos (0)
#define | CLK_CLKSEL0_HCLKSEL_Msk (0x7ul << CLK_CLKSEL0_HCLKSEL_Pos)
#define | CLK_CLKSEL0_STCLKSEL_Pos (3)
#define | CLK_CLKSEL0_STCLKSEL_Msk (0x7ul << CLK_CLKSEL0_STCLKSEL_Pos)
#define | CLK_CLKSEL1_WDTSEL_Pos (0)
#define | CLK_CLKSEL1_WDTSEL_Msk (0x3ul << CLK_CLKSEL1_WDTSEL_Pos)
#define | CLK_CLKSEL1_ADCSEL_Pos (2)
#define | CLK_CLKSEL1_ADCSEL_Msk (0x3ul << CLK_CLKSEL1_ADCSEL_Pos)
#define | CLK_CLKSEL1_SPISEL_Pos (4)
#define | CLK_CLKSEL1_SPISEL_Msk (0x1ul << CLK_CLKSEL1_SPISEL_Pos)
#define | CLK_CLKSEL1_TMR0SEL_Pos (8)
#define | CLK_CLKSEL1_TMR0SEL_Msk (0x7ul << CLK_CLKSEL1_TMR0SEL_Pos)
#define | CLK_CLKSEL1_TMR1SEL_Pos (12)
#define | CLK_CLKSEL1_TMR1SEL_Msk (0x7ul << CLK_CLKSEL1_TMR1SEL_Pos)
#define | CLK_CLKSEL1_UART0SEL_Pos (24)
#define | CLK_CLKSEL1_UART0SEL_Msk (0x3ul << CLK_CLKSEL1_UART0SEL_Pos)
#define | CLK_CLKSEL1_UART1SEL_Pos (26)
#define | CLK_CLKSEL1_UART1SEL_Msk (0x3ul << CLK_CLKSEL1_UART1SEL_Pos)
#define | CLK_CLKDIV_HCLKDIV_Pos (0)
#define | CLK_CLKDIV_HCLKDIV_Msk (0xful << CLK_CLKDIV_HCLKDIV_Pos)
#define | CLK_CLKDIV_UART0DIV_Pos (8)
#define | CLK_CLKDIV_UART0DIV_Msk (0xful << CLK_CLKDIV_UART0DIV_Pos)
#define | CLK_CLKDIV_UART1DIV_Pos (12)
#define | CLK_CLKDIV_UART1DIV_Msk (0xful << CLK_CLKDIV_UART1DIV_Pos)
#define | CLK_CLKDIV_ADCDIV_Pos (16)
#define | CLK_CLKDIV_ADCDIV_Msk (0xfful << CLK_CLKDIV_ADCDIV_Pos)
#define | CLK_CLKSEL2_FDIVSEL_Pos (2)
#define | CLK_CLKSEL2_FDIVSEL_Msk (0x3ul << CLK_CLKSEL2_FDIVSEL_Pos)
#define | CLK_CLKOCTL_FSEL_Pos (0)
#define | CLK_CLKOCTL_FSEL_Msk (0xful << CLK_CLKOCTL_FSEL_Pos)
#define | CLK_CLKOCTL_CLKOEN_Pos (4)
#define | CLK_CLKOCTL_CLKOEN_Msk (0x1ul << CLK_CLKOCTL_CLKOEN_Pos)
#define | CLK_CLKOCTL_DIV1EN_Pos (5)
#define | CLK_CLKOCTL_DIV1EN_Msk (0x1ul << CLK_CLKOCTL_DIV1EN_Pos)
#define | FMC_ISPCTL_ISPEN_Pos (0)
#define | FMC_ISPCTL_ISPEN_Msk (0x1ul << FMC_ISPCTL_ISPEN_Pos)
#define | FMC_ISPCTL_BS_Pos (1)
#define | FMC_ISPCTL_BS_Msk (0x1ul << FMC_ISPCTL_BS_Pos)
#define | FMC_ISPCTL_APUEN_Pos (3)
#define | FMC_ISPCTL_APUEN_Msk (0x1ul << FMC_ISPCTL_APUEN_Pos)
#define | FMC_ISPCTL_CFGUEN_Pos (4)
#define | FMC_ISPCTL_CFGUEN_Msk (0x1ul << FMC_ISPCTL_CFGUEN_Pos)
#define | FMC_ISPCTL_LDUEN_Pos (5)
#define | FMC_ISPCTL_LDUEN_Msk (0x1ul << FMC_ISPCTL_LDUEN_Pos)
#define | FMC_ISPCTL_ISPFF_Pos (6)
#define | FMC_ISPCTL_ISPFF_Msk (0x1ul << FMC_ISPCTL_ISPFF_Pos)
#define | FMC_ISPADDR_ISPADR_Pos (0)
#define | FMC_ISPADDR_ISPADR_Msk (0xfffffffful << FMC_ISPADDR_ISPADR_Pos)
#define | FMC_ISPDAT_ISPDAT_Pos (0)
#define | FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)
#define | FMC_ISPCMD_CMD_Pos (0)
#define | FMC_ISPCMD_CMD_Msk (0x3ful << FMC_ISPCMD_CMD_Pos)
#define | FMC_ISPTRG_ISPGO_Pos (0)
#define | FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)
#define | FMC_DFBA_DFBA_Pos (0)
#define | FMC_DFBA_DFBA_Msk (0xfffffffful << FMC_DFBA_DFBA_Pos)
#define | FMC_ISPSTS_ISPBUSY_Pos (0)
#define | FMC_ISPSTS_ISPBUSY_Msk (0x1ul << FMC_ISPSTS_ISPBUSY_Pos)
#define | FMC_ISPSTS_CBS_Pos (1)
#define | FMC_ISPSTS_CBS_Msk (0x3ul << FMC_ISPSTS_CBS_Pos)
#define | FMC_ISPSTS_ISPFF_Pos (6)
#define | FMC_ISPSTS_ISPFF_Msk (0x1ul << FMC_ISPSTS_ISPFF_Pos)
#define | FMC_ISPSTS_VECMAP_Pos (9)
#define | FMC_ISPSTS_VECMAP_Msk (0xffful << FMC_ISPSTS_VECMAP_Pos)
#define | GP_MODE_MODE0_Pos (0)
#define | GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)
#define | GP_MODE_MODE1_Pos (2)
#define | GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)
#define | GP_MODE_MODE2_Pos (4)
#define | GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)
#define | GP_MODE_MODE3_Pos (6)
#define | GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)
#define | GP_MODE_MODE4_Pos (8)
#define | GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)
#define | GP_MODE_MODE5_Pos (10)
#define | GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)
#define | GP_DINOFF_DINOFF0_Pos (16)
#define | GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)
#define | GP_DINOFF_DINOFF1_Pos (17)
#define | GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)
#define | GP_DINOFF_DINOFF2_Pos (18)
#define | GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)
#define | GP_DINOFF_DINOFF3_Pos (19)
#define | GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)
#define | GP_DINOFF_DINOFF4_Pos (20)
#define | GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)
#define | GP_DINOFF_DINOFF5_Pos (21)
#define | GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)
#define | GP_DINOFF_DINOFF6_Pos (22)
#define | GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)
#define | GP_DINOFF_DINOFF7_Pos (23)
#define | GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)
#define | GP_DOUT_DOUT0_Pos (0)
#define | GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)
#define | GP_DOUT_DOUT1_Pos (1)
#define | GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)
#define | GP_DOUT_DOUT2_Pos (2)
#define | GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)
#define | GP_DOUT_DOUT3_Pos (3)
#define | GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)
#define | GP_DOUT_DOUT4_Pos (4)
#define | GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)
#define | GP_DOUT_DOUT5_Pos (5)
#define | GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)
#define | GP_DOUT_DOUT6_Pos (6)
#define | GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)
#define | GP_DOUT_DOUT7_Pos (7)
#define | GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)
#define | GP_DATMSK_DATMSK0_Pos (0)
#define | GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)
#define | GP_DATMSK_DATMSK1_Pos (1)
#define | GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)
#define | GP_DATMSK_DATMSK2_Pos (2)
#define | GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)
#define | GP_DATMSK_DATMSK3_Pos (3)
#define | GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)
#define | GP_DATMSK_DATMSK4_Pos (4)
#define | GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)
#define | GP_DATMSK_DATMSK5_Pos (5)
#define | GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)
#define | GP_DATMSK_DATMSK6_Pos (6)
#define | GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)
#define | GP_DATMSK_DATMSK7_Pos (7)
#define | GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)
#define | GP_PIN_PIN0_Pos (0)
#define | GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)
#define | GP_PIN_PIN1_Pos (1)
#define | GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)
#define | GP_PIN_PIN2_Pos (2)
#define | GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)
#define | GP_PIN_PIN3_Pos (3)
#define | GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)
#define | GP_PIN_PIN4_Pos (4)
#define | GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)
#define | GP_PIN_PIN5_Pos (5)
#define | GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)
#define | GP_PIN_PIN6_Pos (6)
#define | GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)
#define | GP_PIN_PIN7_Pos (7)
#define | GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)
#define | GP_DBEN_DBEN0_Pos (0)
#define | GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)
#define | GP_DBEN_DBEN1_Pos (1)
#define | GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)
#define | GP_DBEN_DBEN2_Pos (2)
#define | GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)
#define | GP_DBEN_DBEN3_Pos (3)
#define | GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)
#define | GP_DBEN_DBEN4_Pos (4)
#define | GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)
#define | GP_DBEN_DBEN5_Pos (5)
#define | GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)
#define | GP_DBEN_DBEN6_Pos (6)
#define | GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)
#define | GP_DBEN_DBEN7_Pos (7)
#define | GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)
#define | GP_INTTYPE_TYPE0_Pos (0)
#define | GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)
#define | GP_INTTYPE_TYPE1_Pos (1)
#define | GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)
#define | GP_INTTYPE_TYPE2_Pos (2)
#define | GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)
#define | GP_INTTYPE_TYPE3_Pos (3)
#define | GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)
#define | GP_INTTYPE_TYPE4_Pos (4)
#define | GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)
#define | GP_INTTYPE_TYPE5_Pos (5)
#define | GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)
#define | GP_INTTYPE_TYPE6_Pos (6)
#define | GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)
#define | GP_INTTYPE_TYPE7_Pos (7)
#define | GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)
#define | GP_INTEN_FLIEN0_Pos (0)
#define | GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)
#define | GP_INTEN_FLIEN1_Pos (1)
#define | GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)
#define | GP_INTEN_FLIEN2_Pos (2)
#define | GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)
#define | GP_INTEN_FLIEN3_Pos (3)
#define | GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)
#define | GP_INTEN_FLIEN4_Pos (4)
#define | GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)
#define | GP_INTEN_FLIEN5_Pos (5)
#define | GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)
#define | GP_INTEN_FLIEN6_Pos (6)
#define | GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)
#define | GP_INTEN_FLIEN7_Pos (7)
#define | GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)
#define | GP_INTEN_RHIEN0_Pos (16)
#define | GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)
#define | GP_INTEN_RHIEN1_Pos (17)
#define | GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)
#define | GP_INTEN_RHIEN2_Pos (18)
#define | GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)
#define | GP_INTEN_RHIEN3_Pos (19)
#define | GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)
#define | GP_INTEN_RHIEN4_Pos (20)
#define | GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)
#define | GP_INTEN_RHIEN5_Pos (21)
#define | GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)
#define | GP_INTEN_RHIEN6_Pos (22)
#define | GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)
#define | GP_INTEN_RHIEN7_Pos (23)
#define | GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)
#define | GP_INTSRC_INTSRC0_Pos (0)
#define | GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)
#define | GP_INTSRC_INTSRC1_Pos (1)
#define | GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)
#define | GP_INTSRC_INTSRC2_Pos (2)
#define | GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)
#define | GP_INTSRC_INTSRC3_Pos (3)
#define | GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)
#define | GP_INTSRC_INTSRC4_Pos (4)
#define | GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)
#define | GP_INTSRC_INTSRC5_Pos (5)
#define | GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)
#define | GP_INTSRC_INTSRC6_Pos (6)
#define | GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)
#define | GP_INTSRC_INTSRC7_Pos (7)
#define | GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)
#define | GP_DBCTL_DBCLKSEL_Pos (0)
#define | GP_DBCTL_DBCLKSEL_Msk (0xful << GP_DBCTL_DBCLKSEL_Pos)
#define | GP_DBCTL_DBCLKSRC_Pos (4)
#define | GP_DBCTL_DBCLKSRC_Msk (0x1ul << GP_DBCTL_DBCLKSRC_Pos)
#define | GP_DBCTL_ICLKON_Pos (5)
#define | GP_DBCTL_ICLKON_Msk (0x1ul << GP_DBCTL_ICLKON_Pos)
#define | HDIV_DIVIDEND_DIVIDEND_Pos (0)
#define | HDIV_DIVIDEND_DIVIDEND_Msk (0xfffffffful << HDIV_DIVIDEND_DIVIDEND_Pos)
#define | HDIV_DIVISOR_DIVISOR_Pos (0)
#define | HDIV_DIVISOR_DIVISOR_Msk (0xfffful << HDIV_DIVISOR_DIVISOR_Pos)
#define | HDIV_QUOTIENT_QUOTIENT_Pos (0)
#define | HDIV_QUOTIENT_QUOTIENT_Msk (0xfffffffful << HDIV_QUOTIENT_QUOTIENT_Pos)
#define | HDIV_REM_REM_Pos (0)
#define | HDIV_REM_REM_Msk (0xfffffffful << HDIV_REM_REM_Pos)
#define | HDIV_STATUS_DIVBYZERO_Pos (1)
#define | HDIV_STATUS_DIVBYZERO_Msk (0x1ul << HDIV_STATUS_DIVBYZERO_Pos)
#define | I2C_CTL_AA_Pos (2)
#define | I2C_CTL_AA_Msk (0x1ul << I2C_CTL_AA_Pos)
#define | I2C_CTL_SI_Pos (3)
#define | I2C_CTL_SI_Msk (0x1ul << I2C_CTL_SI_Pos)
#define | I2C_CTL_STO_Pos (4)
#define | I2C_CTL_STO_Msk (0x1ul << I2C_CTL_STO_Pos)
#define | I2C_CTL_STA_Pos (5)
#define | I2C_CTL_STA_Msk (0x1ul << I2C_CTL_STA_Pos)
#define | I2C_CTL_I2CEN_Pos (6)
#define | I2C_CTL_I2CEN_Msk (0x1ul << I2C_CTL_I2CEN_Pos)
#define | I2C_CTL_INTEN_Pos (7)
#define | I2C_CTL_INTEN_Msk (0x1ul << I2C_CTL_INTEN_Pos)
#define | I2C_ADDR0_GC_Pos (0)
#define | I2C_ADDR0_GC_Msk (0x1ul << I2C_ADDR0_GC_Pos)
#define | I2C_ADDR0_ADDR_Pos (1)
#define | I2C_ADDR0_ADDR_Msk (0x7ful << I2C_ADDR0_ADDR_Pos)
#define | I2C_DAT_DAT_Pos (0)
#define | I2C_DAT_DAT_Msk (0xfful << I2C_DAT_DAT_Pos)
#define | I2C_STATUS_STATUS_Pos (0)
#define | I2C_STATUS_STATUS_Msk (0xfful << I2C_STATUS_STATUS_Pos)
#define | I2C_CLKDIV_DIVIDER_Pos (0)
#define | I2C_CLKDIV_DIVIDER_Msk (0xfful << I2C_CLKDIV_DIVIDER_Pos)
#define | I2C_TOCTL_TOIF_Pos (0)
#define | I2C_TOCTL_TOIF_Msk (0x1ul << I2C_TOCTL_TOIF_Pos)
#define | I2C_TOCTL_TOCDIV4_Pos (1)
#define | I2C_TOCTL_TOCDIV4_Msk (0x1ul << I2C_TOCTL_TOCDIV4_Pos)
#define | I2C_TOCTL_TOCEN_Pos (2)
#define | I2C_TOCTL_TOCEN_Msk (0x1ul << I2C_TOCTL_TOCEN_Pos)
#define | I2C_ADDR1_GC_Pos (0)
#define | I2C_ADDR1_GC_Msk (0x1ul << I2C_ADDR1_GC_Pos)
#define | I2C_ADDR1_ADDR_Pos (1)
#define | I2C_ADDR1_ADDR_Msk (0x7ful << I2C_ADDR1_ADDR_Pos)
#define | I2C_ADDR2_GC_Pos (0)
#define | I2C_ADDR2_GC_Msk (0x1ul << I2C_ADDR2_GC_Pos)
#define | I2C_ADDR2_ADDR_Pos (1)
#define | I2C_ADDR2_ADDR_Msk (0x7ful << I2C_ADDR2_ADDR_Pos)
#define | I2C_ADDR3_GC_Pos (0)
#define | I2C_ADDR3_GC_Msk (0x1ul << I2C_ADDR3_GC_Pos)
#define | I2C_ADDR3_ADDR_Pos (1)
#define | I2C_ADDR3_ADDR_Msk (0x7ful << I2C_ADDR3_ADDR_Pos)
#define | I2C_ADDRMSK0_ADDRMSK_Pos (1)
#define | I2C_ADDRMSK0_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK0_ADDRMSK_Pos)
#define | I2C_ADDRMSK1_ADDRMSK_Pos (1)
#define | I2C_ADDRMSK1_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK1_ADDRMSK_Pos)
#define | I2C_ADDRMSK2_ADDRMSK_Pos (1)
#define | I2C_ADDRMSK2_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK2_ADDRMSK_Pos)
#define | I2C_ADDRMSK3_ADDRMSK_Pos (1)
#define | I2C_ADDRMSK3_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK3_ADDRMSK_Pos)
#define | I2C_CTL1_WKEN_Pos (0)
#define | I2C_CTL1_WKEN_Msk (0x1ul << I2C_CTL1_WKEN_Pos)
#define | I2C_CTL1_FIFOEN_Pos (1)
#define | I2C_CTL1_FIFOEN_Msk (0x1ul << I2C_CTL1_FIFOEN_Pos)
#define | I2C_CTL1_NSTRETCH_Pos (2)
#define | I2C_CTL1_NSTRETCH_Msk (0x1ul << I2C_CTL1_NSTRETCH_Pos)
#define | I2C_CTL1_OVIEN_Pos (3)
#define | I2C_CTL1_OVIEN_Msk (0x1ul << I2C_CTL1_OVIEN_Pos)
#define | I2C_CTL1_URIEN_Pos (4)
#define | I2C_CTL1_URIEN_Msk (0x1ul << I2C_CTL1_URIEN_Pos)
#define | I2C_STATUS1_WKIF_Pos (0)
#define | I2C_STATUS1_WKIF_Msk (0x1ul << I2C_STATUS1_WKIF_Pos)
#define | I2C_STATUS1_FULL_Pos (1)
#define | I2C_STATUS1_FULL_Msk (0x1ul << I2C_STATUS1_FULL_Pos)
#define | I2C_STATUS1_EMPTY_Pos (2)
#define | I2C_STATUS1_EMPTY_Msk (0x1ul << I2C_STATUS1_EMPTY_Pos)
#define | I2C_STATUS1_OVIF_Pos (3)
#define | I2C_STATUS1_OVIF_Msk (0x1ul << I2C_STATUS1_OVIF_Pos)
#define | I2C_STATUS1_URIF_Pos (4)
#define | I2C_STATUS1_URIF_Msk (0x1ul << I2C_STATUS1_URIF_Pos)
#define | INT_IRQ0SRC_INT_SRC_Pos (0)
#define | INT_IRQ0SRC_INT_SRC_Msk (0x7ul << INT_IRQ0SRC_INT_SRC_Pos)
#define | INT_IRQ1SRC_INT_SRC_Pos (0)
#define | INT_IRQ1SRC_INT_SRC_Msk (0x7ul << INT_IRQ1SRC_INT_SRC_Pos)
#define | INT_IRQ2SRC_INT_SRC_Pos (0)
#define | INT_IRQ2SRC_INT_SRC_Msk (0x7ul << INT_IRQ2SRC_INT_SRC_Pos)
#define | INT_IRQ3SRC_INT_SRC_Pos (0)
#define | INT_IRQ3SRC_INT_SRC_Msk (0x7ul << INT_IRQ3SRC_INT_SRC_Pos)
#define | INT_IRQ4SRC_INT_SRC_Pos (0)
#define | INT_IRQ4SRC_INT_SRC_Msk (0x7ul << INT_IRQ4SRC_INT_SRC_Pos)
#define | INT_IRQ5SRC_INT_SRC_Pos (0)
#define | INT_IRQ5SRC_INT_SRC_Msk (0x7ul << INT_IRQ5SRC_INT_SRC_Pos)
#define | INT_IRQ6SRC_INT_SRC_Pos (0)
#define | INT_IRQ6SRC_INT_SRC_Msk (0x7ul << INT_IRQ6SRC_INT_SRC_Pos)
#define | INT_IRQ7SRC_INT_SRC_Pos (0)
#define | INT_IRQ7SRC_INT_SRC_Msk (0x7ul << INT_IRQ7SRC_INT_SRC_Pos)
#define | INT_IRQ8SRC_INT_SRC_Pos (0)
#define | INT_IRQ8SRC_INT_SRC_Msk (0x7ul << INT_IRQ8SRC_INT_SRC_Pos)
#define | INT_IRQ9SRC_INT_SRC_Pos (0)
#define | INT_IRQ9SRC_INT_SRC_Msk (0x7ul << INT_IRQ9SRC_INT_SRC_Pos)
#define | INT_IRQ12SRC_INT_SRC_Pos (0)
#define | INT_IRQ12SRC_INT_SRC_Msk (0x7ul << INT_IRQ12SRC_INT_SRC_Pos)
#define | INT_IRQ13SRC_INT_SRC_Pos (0)
#define | INT_IRQ13SRC_INT_SRC_Msk (0x7ul << INT_IRQ13SRC_INT_SRC_Pos)
#define | INT_IRQ14SRC_INT_SRC_Pos (0)
#define | INT_IRQ14SRC_INT_SRC_Msk (0x7ul << INT_IRQ14SRC_INT_SRC_Pos)
#define | INT_IRQ16SRC_INT_SRC_Pos (0)
#define | INT_IRQ16SRC_INT_SRC_Msk (0x7ul << INT_IRQ16SRC_INT_SRC_Pos)
#define | INT_IRQ17SRC_INT_SRC_Pos (0)
#define | INT_IRQ17SRC_INT_SRC_Msk (0x7ul << INT_IRQ17SRC_INT_SRC_Pos)
#define | INT_IRQ18SRC_INT_SRC_Pos (0)
#define | INT_IRQ18SRC_INT_SRC_Msk (0x7ul << INT_IRQ18SRC_INT_SRC_Pos)
#define | INT_IRQ25SRC_INT_SRC_Pos (0)
#define | INT_IRQ25SRC_INT_SRC_Msk (0x7ul << INT_IRQ25SRC_INT_SRC_Pos)
#define | INT_IRQ28SRC_INT_SRC_Pos (0)
#define | INT_IRQ28SRC_INT_SRC_Msk (0x7ul << INT_IRQ28SRC_INT_SRC_Pos)
#define | INT_IRQ29SRC_INT_SRC_Pos (0)
#define | INT_IRQ29SRC_INT_SRC_Msk (0x7ul << INT_IRQ29SRC_INT_SRC_Pos)
#define | INT_NMICTL_NMTSEL_Pos (0)
#define | INT_NMICTL_NMTSEL_Msk (0x1ful << INT_NMICTL_NMTSEL_Pos)
#define | INT_NMICTL_NMISELEN_Pos (8)
#define | INT_NMICTL_NMISELEN_Msk (0x1ul << INT_NMICTL_NMISELEN_Pos)
#define | INT_IRQSTS_IRQ_Pos (0)
#define | INT_IRQSTS_IRQ_Msk (0xfffffffful << INT_IRQSTS_IRQ_Pos)
#define | PWM_CLKPSC_CLKPSC01_Pos (0)
#define | PWM_CLKPSC_CLKPSC01_Msk (0xfful << PWM_CLKPSC_CLKPSC01_Pos)
#define | PWM_CLKPSC_CLKPSC23_Pos (8)
#define | PWM_CLKPSC_CLKPSC23_Msk (0xfful << PWM_CLKPSC_CLKPSC23_Pos)
#define | PWM_CLKPSC_CLKPSC45_Pos (16)
#define | PWM_CLKPSC_CLKPSC45_Msk (0xfful << PWM_CLKPSC_CLKPSC45_Pos)
#define | PWM_CLKDIV_CLKDIV0_Pos (0)
#define | PWM_CLKDIV_CLKDIV0_Msk (0x7ul << PWM_CLKDIV_CLKDIV0_Pos)
#define | PWM_CLKDIV_CLKDIV1_Pos (4)
#define | PWM_CLKDIV_CLKDIV1_Msk (0x7ul << PWM_CLKDIV_CLKDIV1_Pos)
#define | PWM_CLKDIV_CLKDIV2_Pos (8)
#define | PWM_CLKDIV_CLKDIV2_Msk (0x7ul << PWM_CLKDIV_CLKDIV2_Pos)
#define | PWM_CLKDIV_CLKDIV3_Pos (12)
#define | PWM_CLKDIV_CLKDIV3_Msk (0x7ul << PWM_CLKDIV_CLKDIV3_Pos)
#define | PWM_CLKDIV_CLKDIV4_Pos (16)
#define | PWM_CLKDIV_CLKDIV4_Msk (0x7ul << PWM_CLKDIV_CLKDIV4_Pos)
#define | PWM_CLKDIV_CLKDIV5_Pos (20)
#define | PWM_CLKDIV_CLKDIV5_Msk (0x7ul << PWM_CLKDIV_CLKDIV5_Pos)
#define | PWM_CTL_CNTEN0_Pos (0)
#define | PWM_CTL_CNTEN0_Msk (0x1ul << PWM_CTL_CNTEN0_Pos)
#define | PWM_CTL_DBGTRIOFF_Pos (1)
#define | PWM_CTL_DBGTRIOFF_Msk (0x1ul << PWM_CTL_DBGTRIOFF_Pos)
#define | PWM_CTL_PINV0_Pos (2)
#define | PWM_CTL_PINV0_Msk (0x1ul << PWM_CTL_PINV0_Pos)
#define | PWM_CTL_CNTMODE0_Pos (3)
#define | PWM_CTL_CNTMODE0_Msk (0x1ul << PWM_CTL_CNTMODE0_Pos)
#define | PWM_CTL_CNTEN1_Pos (4)
#define | PWM_CTL_CNTEN1_Msk (0x1ul << PWM_CTL_CNTEN1_Pos)
#define | PWM_CTL_HCUPDT_Pos (5)
#define | PWM_CTL_HCUPDT_Msk (0x1ul << PWM_CTL_HCUPDT_Pos)
#define | PWM_CTL_PINV1_Pos (6)
#define | PWM_CTL_PINV1_Msk (0x1ul << PWM_CTL_PINV1_Pos)
#define | PWM_CTL_CNTMODE1_Pos (7)
#define | PWM_CTL_CNTMODE1_Msk (0x1ul << PWM_CTL_CNTMODE1_Pos)
#define | PWM_CTL_CNTEN2_Pos (8)
#define | PWM_CTL_CNTEN2_Msk (0x1ul << PWM_CTL_CNTEN2_Pos)
#define | PWM_CTL_PINV2_Pos (10)
#define | PWM_CTL_PINV2_Msk (0x1ul << PWM_CTL_PINV2_Pos)
#define | PWM_CTL_CNTMODE2_Pos (11)
#define | PWM_CTL_CNTMODE2_Msk (0x1ul << PWM_CTL_CNTMODE2_Pos)
#define | PWM_CTL_CNTEN3_Pos (12)
#define | PWM_CTL_CNTEN3_Msk (0x1ul << PWM_CTL_CNTEN3_Pos)
#define | PWM_CTL_PINV3_Pos (14)
#define | PWM_CTL_PINV3_Msk (0x1ul << PWM_CTL_PINV3_Pos)
#define | PWM_CTL_CNTMODE3_Pos (15)
#define | PWM_CTL_CNTMODE3_Msk (0x1ul << PWM_CTL_CNTMODE3_Pos)
#define | PWM_CTL_CNTEN4_Pos (16)
#define | PWM_CTL_CNTEN4_Msk (0x1ul << PWM_CTL_CNTEN4_Pos)
#define | PWM_CTL_PINV4_Pos (18)
#define | PWM_CTL_PINV4_Msk (0x1ul << PWM_CTL_PINV4_Pos)
#define | PWM_CTL_CNTMODE4_Pos (19)
#define | PWM_CTL_CNTMODE4_Msk (0x1ul << PWM_CTL_CNTMODE4_Pos)
#define | PWM_CTL_CNTEN5_Pos (20)
#define | PWM_CTL_CNTEN5_Msk (0x1ul << PWM_CTL_CNTEN5_Pos)
#define | PWM_CTL_ASYMEN_Pos (21)
#define | PWM_CTL_ASYMEN_Msk (0x1ul << PWM_CTL_ASYMEN_Pos)
#define | PWM_CTL_PINV5_Pos (22)
#define | PWM_CTL_PINV5_Msk (0x1ul << PWM_CTL_PINV5_Pos)
#define | PWM_CTL_CNTMODE5_Pos (23)
#define | PWM_CTL_CNTMODE5_Msk (0x1ul << PWM_CTL_CNTMODE5_Pos)
#define | PWM_CTL_DTCNT01_Pos (24)
#define | PWM_CTL_DTCNT01_Msk (0x1ul << PWM_CTL_DTCNT01_Pos)
#define | PWM_CTL_DTCNT23_Pos (25)
#define | PWM_CTL_DTCNT23_Msk (0x1ul << PWM_CTL_DTCNT23_Pos)
#define | PWM_CTL_DTCNT45_Pos (26)
#define | PWM_CTL_DTCNT45_Msk (0x1ul << PWM_CTL_DTCNT45_Pos)
#define | PWM_CTL_CNTCLR_Pos (27)
#define | PWM_CTL_CNTCLR_Msk (0x1ul << PWM_CTL_CNTCLR_Pos)
#define | PWM_CTL_MODE_Pos (28)
#define | PWM_CTL_MODE_Msk (0x3ul << PWM_CTL_MODE_Pos)
#define | PWM_CTL_GROUPEN_Pos (30)
#define | PWM_CTL_GROUPEN_Msk (0x1ul << PWM_CTL_GROUPEN_Pos)
#define | PWM_CTL_CNTTYPE_Pos (31)
#define | PWM_CTL_CNTTYPE_Msk (0x1ul << PWM_CTL_CNTTYPE_Pos)
#define | PWM_PERIOD_PERIOD_Pos (0)
#define | PWM_PERIOD_PERIOD_Msk (0xfffful << PWM_PERIOD_PERIOD_Pos)
#define | PWM_CMPDAT_CMP_Pos (0)
#define | PWM_CMPDAT_CMP_Msk (0xfffful << PWM_CMPDAT_CMP_Pos)
#define | PWM_CMPDAT_CMPD_Pos (16)
#define | PWM_CMPDAT_CMPD_Msk (0xfffful << PWM_CMPDAT_CMPD_Pos)
#define | PWM_INTEN_ZIEN0_Pos (0)
#define | PWM_INTEN_ZIEN0_Msk (0x1ul << PWM_INTEN_ZIEN0_Pos)
#define | PWM_INTEN_ZIEN1_Pos (1)
#define | PWM_INTEN_ZIEN1_Msk (0x1ul << PWM_INTEN_ZIEN1_Pos)
#define | PWM_INTEN_ZIEN2_Pos (2)
#define | PWM_INTEN_ZIEN2_Msk (0x1ul << PWM_INTEN_ZIEN2_Pos)
#define | PWM_INTEN_ZIEN3_Pos (3)
#define | PWM_INTEN_ZIEN3_Msk (0x1ul << PWM_INTEN_ZIEN3_Pos)
#define | PWM_INTEN_ZIEN4_Pos (4)
#define | PWM_INTEN_ZIEN4_Msk (0x1ul << PWM_INTEN_ZIEN4_Pos)
#define | PWM_INTEN_ZIEN5_Pos (5)
#define | PWM_INTEN_ZIEN5_Msk (0x1ul << PWM_INTEN_ZIEN5_Pos)
#define | PWM_INTEN_CMPDIEN0_Pos (8)
#define | PWM_INTEN_CMPDIEN0_Msk (0x1ul << PWM_INTEN_CMPDIEN0_Pos)
#define | PWM_INTEN_CMPDIEN1_Pos (9)
#define | PWM_INTEN_CMPDIEN1_Msk (0x1ul << PWM_INTEN_CMPDIEN1_Pos)
#define | PWM_INTEN_CMPDIEN2_Pos (10)
#define | PWM_INTEN_CMPDIEN2_Msk (0x1ul << PWM_INTEN_CMPDIEN2_Pos)
#define | PWM_INTEN_CMPDIEN3_Pos (11)
#define | PWM_INTEN_CMPDIEN3_Msk (0x1ul << PWM_INTEN_CMPDIEN3_Pos)
#define | PWM_INTEN_CMPDIEN4_Pos (12)
#define | PWM_INTEN_CMPDIEN4_Msk (0x1ul << PWM_INTEN_CMPDIEN4_Pos)
#define | PWM_INTEN_CMPDIEN5_Pos (13)
#define | PWM_INTEN_CMPDIEN5_Msk (0x1ul << PWM_INTEN_CMPDIEN5_Pos)
#define | PWM_INTEN_BRKIEN_Pos (16)
#define | PWM_INTEN_BRKIEN_Msk (0x1ul << PWM_INTEN_BRKIEN_Pos)
#define | PWM_INTEN_PINTTYPE_Pos (17)
#define | PWM_INTEN_PINTTYPE_Msk (0x1ul << PWM_INTEN_PINTTYPE_Pos)
#define | PWM_INTEN_PIEN0_Pos (18)
#define | PWM_INTEN_PIEN0_Msk (0x1ul << PWM_INTEN_PIEN0_Pos)
#define | PWM_INTEN_PIEN1_Pos (19)
#define | PWM_INTEN_PIEN1_Msk (0x1ul << PWM_INTEN_PIEN1_Pos)
#define | PWM_INTEN_PIEN2_Pos (20)
#define | PWM_INTEN_PIEN2_Msk (0x1ul << PWM_INTEN_PIEN2_Pos)
#define | PWM_INTEN_PIEN3_Pos (21)
#define | PWM_INTEN_PIEN3_Msk (0x1ul << PWM_INTEN_PIEN3_Pos)
#define | PWM_INTEN_PIEN4_Pos (22)
#define | PWM_INTEN_PIEN4_Msk (0x1ul << PWM_INTEN_PIEN4_Pos)
#define | PWM_INTEN_PIEN5_Pos (23)
#define | PWM_INTEN_PIEN5_Msk (0x1ul << PWM_INTEN_PIEN5_Pos)
#define | PWM_INTEN_CMPUIEN0_Pos (24)
#define | PWM_INTEN_CMPUIEN0_Msk (0x1ul << PWM_INTEN_CMPUIEN0_Pos)
#define | PWM_INTEN_CMPUIEN1_Pos (25)
#define | PWM_INTEN_CMPUIEN1_Msk (0x1ul << PWM_INTEN_CMPUIEN1_Pos)
#define | PWM_INTEN_CMPUIEN2_Pos (26)
#define | PWM_INTEN_CMPUIEN2_Msk (0x1ul << PWM_INTEN_CMPUIEN2_Pos)
#define | PWM_INTEN_CMPUIEN3_Pos (27)
#define | PWM_INTEN_CMPUIEN3_Msk (0x1ul << PWM_INTEN_CMPUIEN3_Pos)
#define | PWM_INTEN_CMPUIEN4_Pos (28)
#define | PWM_INTEN_CMPUIEN4_Msk (0x1ul << PWM_INTEN_CMPUIEN4_Pos)
#define | PWM_INTEN_CMPUIEN5_Pos (29)
#define | PWM_INTEN_CMPUIEN5_Msk (0x1ul << PWM_INTEN_CMPUIEN5_Pos)
#define | PWM_INTSTS_ZIF0_Pos (0)
#define | PWM_INTSTS_ZIF0_Msk (0x1ul << PWM_INTSTS_ZIF0_Pos)
#define | PWM_INTSTS_ZIF1_Pos (1)
#define | PWM_INTSTS_ZIF1_Msk (0x1ul << PWM_INTSTS_ZIF1_Pos)
#define | PWM_INTSTS_ZIF2_Pos (2)
#define | PWM_INTSTS_ZIF2_Msk (0x1ul << PWM_INTSTS_ZIF2_Pos)
#define | PWM_INTSTS_ZIF3_Pos (3)
#define | PWM_INTSTS_ZIF3_Msk (0x1ul << PWM_INTSTS_ZIF3_Pos)
#define | PWM_INTSTS_ZIF4_Pos (4)
#define | PWM_INTSTS_ZIF4_Msk (0x1ul << PWM_INTSTS_ZIF4_Pos)
#define | PWM_INTSTS_ZIF5_Pos (5)
#define | PWM_INTSTS_ZIF5_Msk (0x1ul << PWM_INTSTS_ZIF5_Pos)
#define | PWM_INTSTS_CMPDIF0_Pos (8)
#define | PWM_INTSTS_CMPDIF0_Msk (0x1ul << PWM_INTSTS_CMPDIF0_Pos)
#define | PWM_INTSTS_CMPDIF1_Pos (9)
#define | PWM_INTSTS_CMPDIF1_Msk (0x1ul << PWM_INTSTS_CMPDIF1_Pos)
#define | PWM_INTSTS_CMPDIF2_Pos (10)
#define | PWM_INTSTS_CMPDIF2_Msk (0x1ul << PWM_INTSTS_CMPDIF2_Pos)
#define | PWM_INTSTS_CMPDIF3_Pos (11)
#define | PWM_INTSTS_CMPDIF3_Msk (0x1ul << PWM_INTSTS_CMPDIF3_Pos)
#define | PWM_INTSTS_CMPDIF4_Pos (12)
#define | PWM_INTSTS_CMPDIF4_Msk (0x1ul << PWM_INTSTS_CMPDIF4_Pos)
#define | PWM_INTSTS_CMPDIF5_Pos (13)
#define | PWM_INTSTS_CMPDIF5_Msk (0x1ul << PWM_INTSTS_CMPDIF5_Pos)
#define | PWM_INTSTS_BRKIF0_Pos (16)
#define | PWM_INTSTS_BRKIF0_Msk (0x1ul << PWM_INTSTS_BRKIF0_Pos)
#define | PWM_INTSTS_BRKIF1_Pos (17)
#define | PWM_INTSTS_BRKIF1_Msk (0x1ul << PWM_INTSTS_BRKIF1_Pos)
#define | PWM_INTSTS_PIF0_Pos (18)
#define | PWM_INTSTS_PIF0_Msk (0x1ul << PWM_INTSTS_PIF0_Pos)
#define | PWM_INTSTS_PIF1_Pos (19)
#define | PWM_INTSTS_PIF1_Msk (0x1ul << PWM_INTSTS_PIF1_Pos)
#define | PWM_INTSTS_PIF2_Pos (20)
#define | PWM_INTSTS_PIF2_Msk (0x1ul << PWM_INTSTS_PIF2_Pos)
#define | PWM_INTSTS_PIF3_Pos (21)
#define | PWM_INTSTS_PIF3_Msk (0x1ul << PWM_INTSTS_PIF3_Pos)
#define | PWM_INTSTS_PIF4_Pos (22)
#define | PWM_INTSTS_PIF4_Msk (0x1ul << PWM_INTSTS_PIF4_Pos)
#define | PWM_INTSTS_PIF5_Pos (23)
#define | PWM_INTSTS_PIF5_Msk (0x1ul << PWM_INTSTS_PIF5_Pos)
#define | PWM_INTSTS_CMPUIF0_Pos (24)
#define | PWM_INTSTS_CMPUIF0_Msk (0x1ul << PWM_INTSTS_CMPUIF0_Pos)
#define | PWM_INTSTS_CMPUIF1_Pos (25)
#define | PWM_INTSTS_CMPUIF1_Msk (0x1ul << PWM_INTSTS_CMPUIF1_Pos)
#define | PWM_INTSTS_CMPUIF2_Pos (26)
#define | PWM_INTSTS_CMPUIF2_Msk (0x1ul << PWM_INTSTS_CMPUIF2_Pos)
#define | PWM_INTSTS_CMPUIF3_Pos (27)
#define | PWM_INTSTS_CMPUIF3_Msk (0x1ul << PWM_INTSTS_CMPUIF3_Pos)
#define | PWM_INTSTS_CMPUIF4_Pos (28)
#define | PWM_INTSTS_CMPUIF4_Msk (0x1ul << PWM_INTSTS_CMPUIF4_Pos)
#define | PWM_INTSTS_CMPUIF5_Pos (29)
#define | PWM_INTSTS_CMPUIF5_Msk (0x1ul << PWM_INTSTS_CMPUIF5_Pos)
#define | PWM_POEN_POEN0_Pos (0)
#define | PWM_POEN_POEN0_Msk (0x1ul << PWM_POEN_POEN0_Pos)
#define | PWM_POEN_POEN1_Pos (1)
#define | PWM_POEN_POEN1_Msk (0x1ul << PWM_POEN_POEN1_Pos)
#define | PWM_POEN_POEN2_Pos (2)
#define | PWM_POEN_POEN2_Msk (0x1ul << PWM_POEN_POEN2_Pos)
#define | PWM_POEN_POEN3_Pos (3)
#define | PWM_POEN_POEN3_Msk (0x1ul << PWM_POEN_POEN3_Pos)
#define | PWM_POEN_POEN4_Pos (4)
#define | PWM_POEN_POEN4_Msk (0x1ul << PWM_POEN_POEN4_Pos)
#define | PWM_POEN_POEN5_Pos (5)
#define | PWM_POEN_POEN5_Msk (0x1ul << PWM_POEN_POEN5_Pos)
#define | PWM_BRKCTL_BRK0EN_Pos (0)
#define | PWM_BRKCTL_BRK0EN_Msk (0x1ul << PWM_BRKCTL_BRK0EN_Pos)
#define | PWM_BRKCTL_BRK1EN_Pos (1)
#define | PWM_BRKCTL_BRK1EN_Msk (0x1ul << PWM_BRKCTL_BRK1EN_Pos)
#define | PWM_BRKCTL_BRK0SEL_Pos (2)
#define | PWM_BRKCTL_BRK0SEL_Msk (0x1ul << PWM_BRKCTL_BRK0SEL_Pos)
#define | PWM_BRKCTL_BRK1SEL_Pos (3)
#define | PWM_BRKCTL_BRK1SEL_Msk (0x1ul << PWM_BRKCTL_BRK1SEL_Pos)
#define | PWM_BRKCTL_BRKSTS_Pos (7)
#define | PWM_BRKCTL_BRKSTS_Msk (0x1ul << PWM_BRKCTL_BRKSTS_Pos)
#define | PWM_BRKCTL_BRKACT_Pos (8)
#define | PWM_BRKCTL_BRKACT_Msk (0x1ul << PWM_BRKCTL_BRKACT_Pos)
#define | PWM_BRKCTL_SWBRK_Pos (9)
#define | PWM_BRKCTL_SWBRK_Msk (0x1ul << PWM_BRKCTL_SWBRK_Pos)
#define | PWM_BRKCTL_BKOD0_Pos (24)
#define | PWM_BRKCTL_BKOD0_Msk (0x1ul << PWM_BRKCTL_BKOD0_Pos)
#define | PWM_BRKCTL_BKOD1_Pos (25)
#define | PWM_BRKCTL_BKOD1_Msk (0x1ul << PWM_BRKCTL_BKOD1_Pos)
#define | PWM_BRKCTL_BKOD2_Pos (26)
#define | PWM_BRKCTL_BKOD2_Msk (0x1ul << PWM_BRKCTL_BKOD2_Pos)
#define | PWM_BRKCTL_BKOD3_Pos (27)
#define | PWM_BRKCTL_BKOD3_Msk (0x1ul << PWM_BRKCTL_BKOD3_Pos)
#define | PWM_BRKCTL_BKOD4_Pos (28)
#define | PWM_BRKCTL_BKOD4_Msk (0x1ul << PWM_BRKCTL_BKOD4_Pos)
#define | PWM_BRKCTL_BKOD5_Pos (29)
#define | PWM_BRKCTL_BKOD5_Msk (0x1ul << PWM_BRKCTL_BKOD5_Pos)
#define | PWM_BRKCTL_D6BKOD_Pos (30)
#define | PWM_BRKCTL_D6BKOD_Msk (0x1ul << PWM_BRKCTL_D6BKOD_Pos)
#define | PWM_BRKCTL_D7BKOD_Pos (31)
#define | PWM_BRKCTL_D7BKOD_Msk (0x1ul << PWM_BRKCTL_D7BKOD_Pos)
#define | PWM_DTCTL_DTCNT01_Pos (0)
#define | PWM_DTCTL_DTCNT01_Msk (0xfful << PWM_DTCTL_DTCNT01_Pos)
#define | PWM_DTCTL_DTCNT23_Pos (8)
#define | PWM_DTCTL_DTCNT23_Msk (0xfful << PWM_DTCTL_DTCNT23_Pos)
#define | PWM_DTCTL_DTCNT45_Pos (16)
#define | PWM_DTCTL_DTCNT45_Msk (0xfful << PWM_DTCTL_DTCNT45_Pos)
#define | PWM_ADCTCTL0_CUTRGEN0_Pos (0)
#define | PWM_ADCTCTL0_CUTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN0_Pos)
#define | PWM_ADCTCTL0_CPTRGEN0_Pos (1)
#define | PWM_ADCTCTL0_CPTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN0_Pos)
#define | PWM_ADCTCTL0_CDTRGEN0_Pos (2)
#define | PWM_ADCTCTL0_CDTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN0_Pos)
#define | PWM_ADCTCTL0_ZPTRGEN0_Pos (3)
#define | PWM_ADCTCTL0_ZPTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN0_Pos)
#define | PWM_ADCTCTL0_CUTRGEN1_Pos (8)
#define | PWM_ADCTCTL0_CUTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN1_Pos)
#define | PWM_ADCTCTL0_CPTRGEN1_Pos (9)
#define | PWM_ADCTCTL0_CPTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN1_Pos)
#define | PWM_ADCTCTL0_CDTRGEN1_Pos (10)
#define | PWM_ADCTCTL0_CDTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN1_Pos)
#define | PWM_ADCTCTL0_ZPTRGEN1_Pos (11)
#define | PWM_ADCTCTL0_ZPTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN1_Pos)
#define | PWM_ADCTCTL0_CUTRGEN2_Pos (16)
#define | PWM_ADCTCTL0_CUTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN2_Pos)
#define | PWM_ADCTCTL0_CPTRGEN2_Pos (17)
#define | PWM_ADCTCTL0_CPTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN2_Pos)
#define | PWM_ADCTCTL0_CDTRGEN2_Pos (18)
#define | PWM_ADCTCTL0_CDTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN2_Pos)
#define | PWM_ADCTCTL0_ZPTRGEN2_Pos (19)
#define | PWM_ADCTCTL0_ZPTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN2_Pos)
#define | PWM_ADCTCTL0_CUTRGEN3_Pos (24)
#define | PWM_ADCTCTL0_CUTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN3_Pos)
#define | PWM_ADCTCTL0_CPTRGEN3_Pos (25)
#define | PWM_ADCTCTL0_CPTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN3_Pos)
#define | PWM_ADCTCTL0_CDTRGEN3_Pos (26)
#define | PWM_ADCTCTL0_CDTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN3_Pos)
#define | PWM_ADCTCTL0_ZPTRGEN3_Pos (27)
#define | PWM_ADCTCTL0_ZPTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN3_Pos)
#define | PWM_ADCTCTL1_CUTRGEN4_Pos (0)
#define | PWM_ADCTCTL1_CUTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CUTRGEN4_Pos)
#define | PWM_ADCTCTL1_CPTRGEN4_Pos (1)
#define | PWM_ADCTCTL1_CPTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CPTRGEN4_Pos)
#define | PWM_ADCTCTL1_CDTRGEN4_Pos (2)
#define | PWM_ADCTCTL1_CDTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CDTRGEN4_Pos)
#define | PWM_ADCTCTL1_ZPTRGEN4_Pos (3)
#define | PWM_ADCTCTL1_ZPTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_ZPTRGEN4_Pos)
#define | PWM_ADCTCTL1_CUTRGEN5_Pos (8)
#define | PWM_ADCTCTL1_CUTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CUTRGEN5_Pos)
#define | PWM_ADCTCTL1_CPTRGEN5_Pos (9)
#define | PWM_ADCTCTL1_CPTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CPTRGEN5_Pos)
#define | PWM_ADCTCTL1_CDTRGEN5_Pos (10)
#define | PWM_ADCTCTL1_CDTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CDTRGEN5_Pos)
#define | PWM_ADCTCTL1_ZPTRGEN5_Pos (11)
#define | PWM_ADCTCTL1_ZPTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_ZPTRGEN5_Pos)
#define | PWM_ADCTSTS0_CUTRGF0_Pos (0)
#define | PWM_ADCTSTS0_CUTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF0_Pos)
#define | PWM_ADCTSTS0_CPTRGF0_Pos (1)
#define | PWM_ADCTSTS0_CPTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF0_Pos)
#define | PWM_ADCTSTS0_CDTRGF0_Pos (2)
#define | PWM_ADCTSTS0_CDTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF0_Pos)
#define | PWM_ADCTSTS0_ZPTRGF0_Pos (3)
#define | PWM_ADCTSTS0_ZPTRGF0_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF0_Pos)
#define | PWM_ADCTSTS0_CUTRGF1_Pos (8)
#define | PWM_ADCTSTS0_CUTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF1_Pos)
#define | PWM_ADCTSTS0_CPTRGF1_Pos (9)
#define | PWM_ADCTSTS0_CPTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF1_Pos)
#define | PWM_ADCTSTS0_CDTRGF1_Pos (10)
#define | PWM_ADCTSTS0_CDTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF1_Pos)
#define | PWM_ADCTSTS0_ZPTRGF1_Pos (11)
#define | PWM_ADCTSTS0_ZPTRGF1_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF1_Pos)
#define | PWM_ADCTSTS0_CUTRGF2_Pos (16)
#define | PWM_ADCTSTS0_CUTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF2_Pos)
#define | PWM_ADCTSTS0_CPTRGF2_Pos (17)
#define | PWM_ADCTSTS0_CPTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF2_Pos)
#define | PWM_ADCTSTS0_CDTRGF2_Pos (18)
#define | PWM_ADCTSTS0_CDTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF2_Pos)
#define | PWM_ADCTSTS0_ZPTRGF2_Pos (19)
#define | PWM_ADCTSTS0_ZPTRGF2_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF2_Pos)
#define | PWM_ADCTSTS0_CUTRGF3_Pos (24)
#define | PWM_ADCTSTS0_CUTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF3_Pos)
#define | PWM_ADCTSTS0_CPTRGF3_Pos (25)
#define | PWM_ADCTSTS0_CPTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF3_Pos)
#define | PWM_ADCTSTS0_CDTRGF3_Pos (26)
#define | PWM_ADCTSTS0_CDTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF3_Pos)
#define | PWM_ADCTSTS0_ZPTRGF3_Pos (27)
#define | PWM_ADCTSTS0_ZPTRGF3_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF3_Pos)
#define | PWM_ADCTSTS1_CUTRGF4_Pos (0)
#define | PWM_ADCTSTS1_CUTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CUTRGF4_Pos)
#define | PWM_ADCTSTS1_CPTRGF4_Pos (1)
#define | PWM_ADCTSTS1_CPTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CPTRGF4_Pos)
#define | PWM_ADCTSTS1_CDTRGF4_Pos (2)
#define | PWM_ADCTSTS1_CDTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CDTRGF4_Pos)
#define | PWM_ADCTSTS1_ZPTRGF4_Pos (3)
#define | PWM_ADCTSTS1_ZPTRGF4_Msk (0x1ul << PWM_ADCTSTS1_ZPTRGF4_Pos)
#define | PWM_ADCTSTS1_CUTRGF5_Pos (8)
#define | PWM_ADCTSTS1_CUTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CUTRGF5_Pos)
#define | PWM_ADCTSTS1_CPTRGF5_Pos (9)
#define | PWM_ADCTSTS1_CPTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CPTRGF5_Pos)
#define | PWM_ADCTSTS1_CDTRGF5_Pos (10)
#define | PWM_ADCTSTS1_CDTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CDTRGF5_Pos)
#define | PWM_ADCTSTS1_ZPTRGF5_Pos (11)
#define | PWM_ADCTSTS1_ZPTRGF5_Msk (0x1ul << PWM_ADCTSTS1_ZPTRGF5_Pos)
#define | PWM_PHCHG_MSKDAT0_Pos (0)
#define | PWM_PHCHG_MSKDAT0_Msk (0x1ul << PWM_PHCHG_MSKDAT0_Pos)
#define | PWM_PHCHG_MSKDAT1_Pos (1)
#define | PWM_PHCHG_MSKDAT1_Msk (0x1ul << PWM_PHCHG_MSKDAT1_Pos)
#define | PWM_PHCHG_MSKDAT2_Pos (2)
#define | PWM_PHCHG_MSKDAT2_Msk (0x1ul << PWM_PHCHG_MSKDAT2_Pos)
#define | PWM_PHCHG_MSKDAT3_Pos (3)
#define | PWM_PHCHG_MSKDAT3_Msk (0x1ul << PWM_PHCHG_MSKDAT3_Pos)
#define | PWM_PHCHG_MSKDAT4_Pos (4)
#define | PWM_PHCHG_MSKDAT4_Msk (0x1ul << PWM_PHCHG_MSKDAT4_Pos)
#define | PWM_PHCHG_MSKDAT5_Pos (5)
#define | PWM_PHCHG_MSKDAT5_Msk (0x1ul << PWM_PHCHG_MSKDAT5_Pos)
#define | PWM_PHCHG_MSKDAT6_Pos (6)
#define | PWM_PHCHG_MSKDAT6_Msk (0x1ul << PWM_PHCHG_MSKDAT6_Pos)
#define | PWM_PHCHG_MSKDAT7_Pos (7)
#define | PWM_PHCHG_MSKDAT7_Msk (0x1ul << PWM_PHCHG_MSKDAT7_Pos)
#define | PWM_PHCHG_MSKEN0_Pos (8)
#define | PWM_PHCHG_MSKEN0_Msk (0x1ul << PWM_PHCHG_MSKEN0_Pos)
#define | PWM_PHCHG_MSKEN1_Pos (9)
#define | PWM_PHCHG_MSKEN1_Msk (0x1ul << PWM_PHCHG_MSKEN1_Pos)
#define | PWM_PHCHG_MSKEN2_Pos (10)
#define | PWM_PHCHG_MSKEN2_Msk (0x1ul << PWM_PHCHG_MSKEN2_Pos)
#define | PWM_PHCHG_MSKEN3_Pos (11)
#define | PWM_PHCHG_MSKEN3_Msk (0x1ul << PWM_PHCHG_MSKEN3_Pos)
#define | PWM_PHCHG_MSKEN4_Pos (12)
#define | PWM_PHCHG_MSKEN4_Msk (0x1ul << PWM_PHCHG_MSKEN4_Pos)
#define | PWM_PHCHG_MSKEN5_Pos (13)
#define | PWM_PHCHG_MSKEN5_Msk (0x1ul << PWM_PHCHG_MSKEN5_Pos)
#define | PWM_PHCHG_AUTOCLR0_Pos (14)
#define | PWM_PHCHG_AUTOCLR0_Msk (0x1ul << PWM_PHCHG_AUTOCLR0_Pos)
#define | PWM_PHCHG_AUTOCLR1_Pos (15)
#define | PWM_PHCHG_AUTOCLR1_Msk (0x1ul << PWM_PHCHG_AUTOCLR1_Pos)
#define | PWM_PHCHG_OFFEN01_Pos (16)
#define | PWM_PHCHG_OFFEN01_Msk (0x1ul << PWM_PHCHG_OFFEN01_Pos)
#define | PWM_PHCHG_OFFEN11_Pos (17)
#define | PWM_PHCHG_OFFEN11_Msk (0x1ul << PWM_PHCHG_OFFEN11_Pos)
#define | PWM_PHCHG_OFFEN21_Pos (18)
#define | PWM_PHCHG_OFFEN21_Msk (0x1ul << PWM_PHCHG_OFFEN21_Pos)
#define | PWM_PHCHG_OFFEN31_Pos (19)
#define | PWM_PHCHG_OFFEN31_Msk (0x1ul << PWM_PHCHG_OFFEN31_Pos)
#define | PWM_PHCHG_A1POSSEL_Pos (20)
#define | PWM_PHCHG_A1POSSEL_Msk (0x3ul << PWM_PHCHG_A1POSSEL_Pos)
#define | PWM_PHCHG_TMR1TEN_Pos (22)
#define | PWM_PHCHG_TMR1TEN_Msk (0x1ul << PWM_PHCHG_TMR1TEN_Pos)
#define | PWM_PHCHG_ACMP1TEN_Pos (23)
#define | PWM_PHCHG_ACMP1TEN_Msk (0x1ul << PWM_PHCHG_ACMP1TEN_Pos)
#define | PWM_PHCHG_OFFEN00_Pos (24)
#define | PWM_PHCHG_OFFEN00_Msk (0x1ul << PWM_PHCHG_OFFEN00_Pos)
#define | PWM_PHCHG_OFFEN10_Pos (25)
#define | PWM_PHCHG_OFFEN10_Msk (0x1ul << PWM_PHCHG_OFFEN10_Pos)
#define | PWM_PHCHG_OFFEN20_Pos (26)
#define | PWM_PHCHG_OFFEN20_Msk (0x1ul << PWM_PHCHG_OFFEN20_Pos)
#define | PWM_PHCHG_OFFEN30_Pos (27)
#define | PWM_PHCHG_OFFEN30_Msk (0x1ul << PWM_PHCHG_OFFEN30_Pos)
#define | PWM_PHCHG_A0POSSEL_Pos (28)
#define | PWM_PHCHG_A0POSSEL_Msk (0x3ul << PWM_PHCHG_A0POSSEL_Pos)
#define | PWM_PHCHG_T0_Pos (30)
#define | PWM_PHCHG_T0_Msk (0x1ul << PWM_PHCHG_T0_Pos)
#define | PWM_PHCHG_ACMP0TEN_Pos (31)
#define | PWM_PHCHG_ACMP0TEN_Msk (0x1ul << PWM_PHCHG_ACMP0TEN_Pos)
#define | PWM_PHCHGNXT_MSKDAT0_Pos (0)
#define | PWM_PHCHGNXT_MSKDAT0_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT0_Pos)
#define | PWM_PHCHGNXT_MSKDAT1_Pos (1)
#define | PWM_PHCHGNXT_MSKDAT1_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT1_Pos)
#define | PWM_PHCHGNXT_MSKDAT2_Pos (2)
#define | PWM_PHCHGNXT_MSKDAT2_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT2_Pos)
#define | PWM_PHCHGNXT_MSKDAT3_Pos (3)
#define | PWM_PHCHGNXT_MSKDAT3_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT3_Pos)
#define | PWM_PHCHGNXT_MSKDAT4_Pos (4)
#define | PWM_PHCHGNXT_MSKDAT4_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT4_Pos)
#define | PWM_PHCHGNXT_MSKDAT5_Pos (5)
#define | PWM_PHCHGNXT_MSKDAT5_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT5_Pos)
#define | PWM_PHCHGNXT_MSKDAT6_Pos (6)
#define | PWM_PHCHGNXT_MSKDAT6_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT6_Pos)
#define | PWM_PHCHGNXT_MSKDAT7_Pos (7)
#define | PWM_PHCHGNXT_MSKDAT7_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT7_Pos)
#define | PWM_PHCHGNXT_MSKEN0_Pos (8)
#define | PWM_PHCHGNXT_MSKEN0_Msk (0x1ul << PWM_PHCHGNXT_MSKEN0_Pos)
#define | PWM_PHCHGNXT_MSKEN1_Pos (9)
#define | PWM_PHCHGNXT_MSKEN1_Msk (0x1ul << PWM_PHCHGNXT_MSKEN1_Pos)
#define | PWM_PHCHGNXT_MSKEN2_Pos (10)
#define | PWM_PHCHGNXT_MSKEN2_Msk (0x1ul << PWM_PHCHGNXT_MSKEN2_Pos)
#define | PWM_PHCHGNXT_MSKEN3_Pos (11)
#define | PWM_PHCHGNXT_MSKEN3_Msk (0x1ul << PWM_PHCHGNXT_MSKEN3_Pos)
#define | PWM_PHCHGNXT_MSKEN4_Pos (12)
#define | PWM_PHCHGNXT_MSKEN4_Msk (0x1ul << PWM_PHCHGNXT_MSKEN4_Pos)
#define | PWM_PHCHGNXT_MSKEN5_Pos (13)
#define | PWM_PHCHGNXT_MSKEN5_Msk (0x1ul << PWM_PHCHGNXT_MSKEN5_Pos)
#define | PWM_PHCHGNXT_AUTOCLR0_Pos (14)
#define | PWM_PHCHGNXT_AUTOCLR0_Msk (0x1ul << PWM_PHCHGNXT_AUTOCLR0_Pos)
#define | PWM_PHCHGNXT_AUTOCLR1_Pos (15)
#define | PWM_PHCHGNXT_AUTOCLR1_Msk (0x1ul << PWM_PHCHGNXT_AUTOCLR1_Pos)
#define | PWM_PHCHGNXT_OFFEN01_Pos (16)
#define | PWM_PHCHGNXT_OFFEN01_Msk (0x1ul << PWM_PHCHGNXT_OFFEN01_Pos)
#define | PWM_PHCHGNXT_OFFEN11_Pos (17)
#define | PWM_PHCHGNXT_OFFEN11_Msk (0x1ul << PWM_PHCHGNXT_OFFEN11_Pos)
#define | PWM_PHCHGNXT_OFFEN21_Pos (18)
#define | PWM_PHCHGNXT_OFFEN21_Msk (0x1ul << PWM_PHCHGNXT_OFFEN21_Pos)
#define | PWM_PHCHGNXT_OFFEN31_Pos (19)
#define | PWM_PHCHGNXT_OFFEN31_Msk (0x1ul << PWM_PHCHGNXT_OFFEN31_Pos)
#define | PWM_PHCHGNXT_A1POSSEL_Pos (20)
#define | PWM_PHCHGNXT_A1POSSEL_Msk (0x3ul << PWM_PHCHGNXT_A1POSSEL_Pos)
#define | PWM_PHCHGNXT_TMR1TEN_Pos (22)
#define | PWM_PHCHGNXT_TMR1TEN_Msk (0x1ul << PWM_PHCHGNXT_TMR1TEN_Pos)
#define | PWM_PHCHGNXT_ACMP1TEN_Pos (23)
#define | PWM_PHCHGNXT_ACMP1TEN_Msk (0x1ul << PWM_PHCHGNXT_ACMP1TEN_Pos)
#define | PWM_PHCHGNXT_OFFEN00_Pos (24)
#define | PWM_PHCHGNXT_OFFEN00_Msk (0x1ul << PWM_PHCHGNXT_OFFEN00_Pos)
#define | PWM_PHCHGNXT_OFFEN10_Pos (25)
#define | PWM_PHCHGNXT_OFFEN10_Msk (0x1ul << PWM_PHCHGNXT_OFFEN10_Pos)
#define | PWM_PHCHGNXT_OFFEN20_Pos (26)
#define | PWM_PHCHGNXT_OFFEN20_Msk (0x1ul << PWM_PHCHGNXT_OFFEN20_Pos)
#define | PWM_PHCHGNXT_OFFEN30_Pos (27)
#define | PWM_PHCHGNXT_OFFEN30_Msk (0x1ul << PWM_PHCHGNXT_OFFEN30_Pos)
#define | PWM_PHCHGNXT_A0POSSEL_Pos (28)
#define | PWM_PHCHGNXT_A0POSSEL_Msk (0x3ul << PWM_PHCHGNXT_A0POSSEL_Pos)
#define | PWM_PHCHGNXT_TMR0TEN_Pos (30)
#define | PWM_PHCHGNXT_TMR0TEN_Msk (0x1ul << PWM_PHCHGNXT_TMR0TEN_Pos)
#define | PWM_PHCHGNXT_ACMP0TEN_Pos (31)
#define | PWM_PHCHGNXT_ACMP0TEN_Msk (0x1ul << PWM_PHCHGNXT_ACMP0TEN_Pos)
#define | PWM_PHCHGMSK_MASKEND6_Pos (6)
#define | PWM_PHCHGMSK_MASKEND6_Msk (0x1ul << PWM_PHCHGMSK_MASKEND6_Pos)
#define | PWM_PHCHGMSK_MASKEND7_Pos (7)
#define | PWM_PHCHGMSK_MASKEND7_Msk (0x1ul << PWM_PHCHGMSK_MASKEND7_Pos)
#define | PWM_PHCHGMSK_POSCTL0_Pos (8)
#define | PWM_PHCHGMSK_POSCTL0_Msk (0x1ul << PWM_PHCHGMSK_POSCTL0_Pos)
#define | PWM_PHCHGMSK_POSCTL1_Pos (9)
#define | PWM_PHCHGMSK_POSCTL1_Msk (0x1ul << PWM_PHCHGMSK_POSCTL1_Pos)
#define | PWM_IFA_IFAEN_Pos (0)
#define | PWM_IFA_IFAEN_Msk (0x1ul << PWM_IFA_IFAEN_Pos)
#define | PWM_IFA_IFCNT_Pos (4)
#define | PWM_IFA_IFCNT_Msk (0xful << PWM_IFA_IFCNT_Pos)
#define | SPI_CTL_SPIEN_Pos (0)
#define | SPI_CTL_SPIEN_Msk (0x1ul << SPI_CTL_SPIEN_Pos)
#define | SPI_CTL_RXNEG_Pos (1)
#define | SPI_CTL_RXNEG_Msk (0x1ul << SPI_CTL_RXNEG_Pos)
#define | SPI_CTL_TXNEG_Pos (2)
#define | SPI_CTL_TXNEG_Msk (0x1ul << SPI_CTL_TXNEG_Pos)
#define | SPI_CTL_DWIDTH_Pos (3)
#define | SPI_CTL_DWIDTH_Msk (0x1ful << SPI_CTL_DWIDTH_Pos)
#define | SPI_CTL_LSB_Pos (10)
#define | SPI_CTL_LSB_Msk (0x1ul << SPI_CTL_LSB_Pos)
#define | SPI_CTL_CLKPOL_Pos (11)
#define | SPI_CTL_CLKPOL_Msk (0x1ul << SPI_CTL_CLKPOL_Pos)
#define | SPI_CTL_SUSPITV_Pos (12)
#define | SPI_CTL_SUSPITV_Msk (0xful << SPI_CTL_SUSPITV_Pos)
#define | SPI_CTL_UNITIF_Pos (16)
#define | SPI_CTL_UNITIF_Msk (0x1ul << SPI_CTL_UNITIF_Pos)
#define | SPI_CTL_UNITIEN_Pos (17)
#define | SPI_CTL_UNITIEN_Msk (0x1ul << SPI_CTL_UNITIEN_Pos)
#define | SPI_CTL_SLAVE_Pos (18)
#define | SPI_CTL_SLAVE_Msk (0x1ul << SPI_CTL_SLAVE_Pos)
#define | SPI_CTL_REORDER_Pos (19)
#define | SPI_CTL_REORDER_Msk (0x1ul << SPI_CTL_REORDER_Pos)
#define | SPI_CTL_FIFOEN_Pos (21)
#define | SPI_CTL_FIFOEN_Msk (0x1ul << SPI_CTL_FIFOEN_Pos)
#define | SPI_CTL_RXEMPTY_Pos (24)
#define | SPI_CTL_RXEMPTY_Msk (0x1ul << SPI_CTL_RXEMPTY_Pos)
#define | SPI_CTL_RXFULL_Pos (25)
#define | SPI_CTL_RXFULL_Msk (0x1ul << SPI_CTL_RXFULL_Pos)
#define | SPI_CTL_TXEMPTY_Pos (26)
#define | SPI_CTL_TXEMPTY_Msk (0x1ul << SPI_CTL_TXEMPTY_Pos)
#define | SPI_CTL_TXFULL_Pos (27)
#define | SPI_CTL_TXFULL_Msk (0x1ul << SPI_CTL_TXFULL_Pos)
#define | SPI_CLKDIV_DIVIDER_Pos (0)
#define | SPI_CLKDIV_DIVIDER_Msk (0xfful << SPI_CLKDIV_DIVIDER_Pos)
#define | SPI_SSCTL_SS_Pos (0)
#define | SPI_SSCTL_SS_Msk (0x1ul << SPI_SSCTL_SS_Pos)
#define | SPI_SSCTL_SSACTPOL_Pos (2)
#define | SPI_SSCTL_SSACTPOL_Msk (0x1ul << SPI_SSCTL_SSACTPOL_Pos)
#define | SPI_SSCTL_AUTOSS_Pos (3)
#define | SPI_SSCTL_AUTOSS_Msk (0x1ul << SPI_SSCTL_AUTOSS_Pos)
#define | SPI_SSCTL_SSLTEN_Pos (4)
#define | SPI_SSCTL_SSLTEN_Msk (0x1ul << SPI_SSCTL_SSLTEN_Pos)
#define | SPI_SSCTL_LTF_Pos (5)
#define | SPI_SSCTL_LTF_Msk (0x1ul << SPI_SSCTL_LTF_Pos)
#define | SPI_RX_RX_Pos (0)
#define | SPI_RX_RX_Msk (0xfffffffful << SPI_RX_RX_Pos)
#define | SPI_TX_TX_Pos (0)
#define | SPI_TX_TX_Msk (0xfffffffful << SPI_TX_TX_Pos)
#define | SPI_SLVCTL_SLV3WIRE_Pos (8)
#define | SPI_SLVCTL_SLV3WIRE_Msk (0x1ul << SPI_SLVCTL_SLV3WIRE_Pos)
#define | SPI_SLVCTL_SLVABT_Pos (9)
#define | SPI_SLVCTL_SLVABT_Msk (0x1ul << SPI_SLVCTL_SLVABT_Pos)
#define | SPI_SLVCTL_SLVSTIEN_Pos (10)
#define | SPI_SLVCTL_SLVSTIEN_Msk (0x1ul << SPI_SLVCTL_SLVSTIEN_Pos)
#define | SPI_SLVCTL_SLVSTIF_Pos (11)
#define | SPI_SLVCTL_SLVSTIF_Msk (0x1ul << SPI_SLVCTL_SLVSTIF_Pos)
#define | SPI_SLVCTL_SSINAIEN_Pos (16)
#define | SPI_SLVCTL_SSINAIEN_Msk (0x1ul << SPI_SLVCTL_SSINAIEN_Pos)
#define | SPI_SLVCTL_DIVMOD_Pos (31)
#define | SPI_SLVCTL_DIVMOD_Msk (0x1ul << SPI_SLVCTL_DIVMOD_Pos)
#define | SPI_FIFOCTL_RXRST_Pos (0)
#define | SPI_FIFOCTL_RXRST_Msk (0x1ul << SPI_FIFOCTL_RXRST_Pos)
#define | SPI_FIFOCTL_TXRST_Pos (1)
#define | SPI_FIFOCTL_TXRST_Msk (0x1ul << SPI_FIFOCTL_TXRST_Pos)
#define | SPI_FIFOCTL_RXTHIEN_Pos (2)
#define | SPI_FIFOCTL_RXTHIEN_Msk (0x1ul << SPI_FIFOCTL_RXTHIEN_Pos)
#define | SPI_FIFOCTL_TXTHIEN_Pos (3)
#define | SPI_FIFOCTL_TXTHIEN_Msk (0x1ul << SPI_FIFOCTL_TXTHIEN_Pos)
#define | SPI_FIFOCTL_RXOVIEN_Pos (6)
#define | SPI_FIFOCTL_RXOVIEN_Msk (0x1ul << SPI_FIFOCTL_RXOVIEN_Pos)
#define | SPI_FIFOCTL_RXTOIEN_Pos (21)
#define | SPI_FIFOCTL_RXTOIEN_Msk (0x1ul << SPI_FIFOCTL_RXTOIEN_Pos)
#define | SPI_FIFOCTL_RXTH_Pos (24)
#define | SPI_FIFOCTL_RXTH_Msk (0x3ul << SPI_FIFOCTL_RXTH_Pos)
#define | SPI_FIFOCTL_TXTH_Pos (28)
#define | SPI_FIFOCTL_TXTH_Msk (0x3ul << SPI_FIFOCTL_TXTH_Pos)
#define | SPI_STATUS_RXTHIF_Pos (0)
#define | SPI_STATUS_RXTHIF_Msk (0x1ul << SPI_STATUS_RXTHIF_Pos)
#define | SPI_STATUS_RXOVIF_Pos (2)
#define | SPI_STATUS_RXOVIF_Msk (0x1ul << SPI_STATUS_RXOVIF_Pos)
#define | SPI_STATUS_TXTHIF_Pos (4)
#define | SPI_STATUS_TXTHIF_Msk (0x1ul << SPI_STATUS_TXTHIF_Pos)
#define | SPI_STATUS_SLVSTIF_Pos (11)
#define | SPI_STATUS_SLVSTIF_Msk (0x1ul << SPI_STATUS_SLVSTIF_Pos)
#define | SPI_STATUS_RXCNT_Pos (12)
#define | SPI_STATUS_RXCNT_Msk (0xful << SPI_STATUS_RXCNT_Pos)
#define | SPI_STATUS_UNITIF_Pos (16)
#define | SPI_STATUS_UNITIF_Msk (0x1ul << SPI_STATUS_UNITIF_Pos)
#define | SPI_STATUS_SLVTOIF_Pos (20)
#define | SPI_STATUS_SLVTOIF_Msk (0x1ul << SPI_STATUS_SLVTOIF_Pos)
#define | SPI_STATUS_RXEMPTY_Pos (24)
#define | SPI_STATUS_RXEMPTY_Msk (0x1ul << SPI_STATUS_RXEMPTY_Pos)
#define | SPI_STATUS_RXFULL_Pos (25)
#define | SPI_STATUS_RXFULL_Msk (0x1ul << SPI_STATUS_RXFULL_Pos)
#define | SPI_STATUS_TXEMPTY_Pos (26)
#define | SPI_STATUS_TXEMPTY_Msk (0x1ul << SPI_STATUS_TXEMPTY_Pos)
#define | SPI_STATUS_TXFULL_Pos (27)
#define | SPI_STATUS_TXFULL_Msk (0x1ul << SPI_STATUS_TXFULL_Pos)
#define | SPI_STATUS_TXCNT_Pos (28)
#define | SPI_STATUS_TXCNT_Msk (0xful << SPI_STATUS_TXCNT_Pos)
#define | SYS_PDID_PDID_Pos (0)
#define | SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)
#define | SYS_RSTSTS_PORF_Pos (0)
#define | SYS_RSTSTS_PORF_Msk (0x1ul << SYS_RSTSTS_PORF_Pos)
#define | SYS_RSTSTS_PINRF_Pos (1)
#define | SYS_RSTSTS_PINRF_Msk (0x1ul << SYS_RSTSTS_PINRF_Pos)
#define | SYS_RSTSTS_WDTRF_Pos (2)
#define | SYS_RSTSTS_WDTRF_Msk (0x1ul << SYS_RSTSTS_WDTRF_Pos)
#define | SYS_RSTSTS_BODRF_Pos (4)
#define | SYS_RSTSTS_BODRF_Msk (0x1ul << SYS_RSTSTS_BODRF_Pos)
#define | SYS_RSTSTS_SYSRF_Pos (5)
#define | SYS_RSTSTS_SYSRF_Msk (0x1ul << SYS_RSTSTS_SYSRF_Pos)
#define | SYS_RSTSTS_CPURF_Pos (7)
#define | SYS_RSTSTS_CPURF_Msk (0x1ul << SYS_RSTSTS_CPURF_Pos)
#define | SYS_IPRST0_CHIPRST_Pos (0)
#define | SYS_IPRST0_CHIPRST_Msk (0x1ul << SYS_IPRST0_CHIPRST_Pos)
#define | SYS_IPRST0_CPURST_Pos (1)
#define | SYS_IPRST0_CPURST_Msk (0x1ul << SYS_IPRST0_CPURST_Pos)
#define | SYS_IPRST0_CPUWS_Pos (2)
#define | SYS_IPRST0_CPUWS_Msk (0x1ul << SYS_IPRST0_CPUWS_Pos)
#define | SYS_IPRST1_GPIORST_Pos (1)
#define | SYS_IPRST1_GPIORST_Msk (0x1ul << SYS_IPRST1_GPIORST_Pos)
#define | SYS_IPRST1_TMR0RST_Pos (2)
#define | SYS_IPRST1_TMR0RST_Msk (0x1ul << SYS_IPRST1_TMR0RST_Pos)
#define | SYS_IPRST1_TMR1RST_Pos (3)
#define | SYS_IPRST1_TMR1RST_Msk (0x1ul << SYS_IPRST1_TMR1RST_Pos)
#define | SYS_IPRST1_I2C_RST_Pos (8)
#define | SYS_IPRST1_I2C_RST_Msk (0x1ul << SYS_IPRST1_I2C_RST_Pos)
#define | SYS_IPRST1_SPIRST_Pos (12)
#define | SYS_IPRST1_SPIRST_Msk (0x1ul << SYS_IPRST1_SPIRST_Pos)
#define | SYS_IPRST1_UART0RST_Pos (16)
#define | SYS_IPRST1_UART0RST_Msk (0x1ul << SYS_IPRST1_UART0RST_Pos)
#define | SYS_IPRST1_UART1RST_Pos (17)
#define | SYS_IPRST1_UART1RST_Msk (0x1ul << SYS_IPRST1_UART1RST_Pos)
#define | SYS_IPRST1_PWMRST_Pos (20)
#define | SYS_IPRST1_PWMRST_Msk (0x1ul << SYS_IPRST1_PWMRST_Pos)
#define | SYS_IPRST1_ACMPRST_Pos (22)
#define | SYS_IPRST1_ACMPRST_Msk (0x1ul << SYS_IPRST1_ACMPRST_Pos)
#define | SYS_IPRST1_ADCRST_Pos (28)
#define | SYS_IPRST1_ADCRST_Msk (0x1ul << SYS_IPRST1_ADCRST_Pos)
#define | SYS_BODCTL_BODEN_Pos (0)
#define | SYS_BODCTL_BODEN_Msk (0x1ul << SYS_BODCTL_BODEN_Pos)
#define | SYS_BODCTL_BODVL1_0_Pos (1)
#define | SYS_BODCTL_BODVL1_0_Msk (0x3ul << SYS_BODCTL_BODVL1_0_Pos)
#define | SYS_BODCTL_BODRSTEN_Pos (3)
#define | SYS_BODCTL_BODRSTEN_Msk (0x1ul << SYS_BODCTL_BODRSTEN_Pos)
#define | SYS_BODCTL_BODIF_Pos (4)
#define | SYS_BODCTL_BODIF_Msk (0x1ul << SYS_BODCTL_BODIF_Pos)
#define | SYS_BODCTL_BODLPM_Pos (5)
#define | SYS_BODCTL_BODLPM_Msk (0x1ul << SYS_BODCTL_BODLPM_Pos)
#define | SYS_BODCTL_BODOUT_Pos (6)
#define | SYS_BODCTL_BODOUT_Msk (0x1ul << SYS_BODCTL_BODOUT_Pos)
#define | SYS_BODCTL_BODVL2_Pos (7)
#define | SYS_BODCTL_BODVL2_Msk (0x1ul << SYS_BODCTL_BODVL2_Pos)
#define | SYS_BODCTL_BOREN_Pos (8)
#define | SYS_BODCTL_BOREN_Msk (0x1ul << SYS_BODCTL_BOREN_Pos)
#define | SYS_P0_MFP_MFP_Pos (0)
#define | SYS_P0_MFP_MFP_Msk (0xfful << SYS_P0_MFP_MFP_Pos)
#define | SYS_P0_MFP_ALT0_Pos (8)
#define | SYS_P0_MFP_ALT0_Msk (0x1ul << SYS_P0_MFP_ALT0_Pos)
#define | SYS_P0_MFP_ALT1_Pos (9)
#define | SYS_P0_MFP_ALT1_Msk (0x1ul << SYS_P0_MFP_ALT1_Pos)
#define | SYS_P0_MFP_ALT2_Pos (10)
#define | SYS_P0_MFP_ALT2_Msk (0x1ul << SYS_P0_MFP_ALT2_Pos)
#define | SYS_P0_MFP_ALT4_Pos (12)
#define | SYS_P0_MFP_ALT4_Msk (0x1ul << SYS_P0_MFP_ALT4_Pos)
#define | SYS_P0_MFP_ALT5_Pos (13)
#define | SYS_P0_MFP_ALT5_Msk (0x1ul << SYS_P0_MFP_ALT5_Pos)
#define | SYS_P0_MFP_ALT6_Pos (14)
#define | SYS_P0_MFP_ALT6_Msk (0x1ul << SYS_P0_MFP_ALT6_Pos)
#define | SYS_P0_MFP_ALT7_Pos (15)
#define | SYS_P0_MFP_ALT7_Msk (0x1ul << SYS_P0_MFP_ALT7_Pos)
#define | SYS_P0_MFP_TYPE_Pos (16)
#define | SYS_P0_MFP_TYPE_Msk (0xfful << SYS_P0_MFP_TYPE_Pos)
#define | SYS_P0_MFP_HS_Pos (24)
#define | SYS_P0_MFP_HS_Msk (0xfful << SYS_P0_MFP_HS_Pos)
#define | SYS_P1_MFP_MFP_Pos (0)
#define | SYS_P1_MFP_MFP_Msk (0xfful << SYS_P1_MFP_MFP_Pos)
#define | SYS_P1_MFP_ALT0_Pos (8)
#define | SYS_P1_MFP_ALT0_Msk (0x1ul << SYS_P1_MFP_ALT0_Pos)
#define | SYS_P1_MFP_ALT2_Pos (10)
#define | SYS_P1_MFP_ALT2_Msk (0x1ul << SYS_P1_MFP_ALT2_Pos)
#define | SYS_P1_MFP_ALT3_Pos (11)
#define | SYS_P1_MFP_ALT3_Msk (0x1ul << SYS_P1_MFP_ALT3_Pos)
#define | SYS_P1_MFP_ALT4_Pos (12)
#define | SYS_P1_MFP_ALT4_Msk (0x1ul << SYS_P1_MFP_ALT4_Pos)
#define | SYS_P1_MFP_ALT5_Pos (13)
#define | SYS_P1_MFP_ALT5_Msk (0x1ul << SYS_P1_MFP_ALT5_Pos)
#define | SYS_P1_MFP_ALT6_Pos (14)
#define | SYS_P1_MFP_ALT6_Msk (0x1ul << SYS_P1_MFP_ALT6_Pos)
#define | SYS_P1_MFP_TYPE_Pos (16)
#define | SYS_P1_MFP_TYPE_Msk (0xfful << SYS_P1_MFP_TYPE_Pos)
#define | SYS_P1_MFP_HS_Pos (24)
#define | SYS_P1_MFP_HS_Msk (0xfful << SYS_P1_MFP_HS_Pos)
#define | SYS_P2_MFP_MFP_Pos (0)
#define | SYS_P2_MFP_MFP_Msk (0xfful << SYS_P2_MFP_MFP_Pos)
#define | SYS_P2_MFP_ALT2_Pos (10)
#define | SYS_P2_MFP_ALT2_Msk (0x1ul << SYS_P2_MFP_ALT2_Pos)
#define | SYS_P2_MFP_ALT3_Pos (11)
#define | SYS_P2_MFP_ALT3_Msk (0x1ul << SYS_P2_MFP_ALT3_Pos)
#define | SYS_P2_MFP_ALT4_Pos (12)
#define | SYS_P2_MFP_ALT4_Msk (0x1ul << SYS_P2_MFP_ALT4_Pos)
#define | SYS_P2_MFP_ALT5_Pos (13)
#define | SYS_P2_MFP_ALT5_Msk (0x1ul << SYS_P2_MFP_ALT5_Pos)
#define | SYS_P2_MFP_ALT6_Pos (14)
#define | SYS_P2_MFP_ALT6_Msk (0x1ul << SYS_P2_MFP_ALT6_Pos)
#define | SYS_P2_MFP_ALT7_Pos (15)
#define | SYS_P2_MFP_ALT7_Msk (0x1ul << SYS_P2_MFP_ALT7_Pos)
#define | SYS_P2_MFP_TYPE_Pos (16)
#define | SYS_P2_MFP_TYPE_Msk (0xfful << SYS_P2_MFP_TYPE_Pos)
#define | SYS_P2_MFP_HS_Pos (24)
#define | SYS_P2_MFP_HS_Msk (0xfful << SYS_P2_MFP_HS_Pos)
#define | SYS_P3_MFP_MFP_Pos (0)
#define | SYS_P3_MFP_MFP_Msk (0xfful << SYS_P3_MFP_MFP_Pos)
#define | SYS_P3_MFP_ALT0_Pos (8)
#define | SYS_P3_MFP_ALT0_Msk (0x1ul << SYS_P3_MFP_ALT0_Pos)
#define | SYS_P3_MFP_ALT1_Pos (9)
#define | SYS_P3_MFP_ALT1_Msk (0x1ul << SYS_P3_MFP_ALT1_Pos)
#define | SYS_P3_MFP_ALT2_Pos (10)
#define | SYS_P3_MFP_ALT2_Msk (0x1ul << SYS_P3_MFP_ALT2_Pos)
#define | SYS_P3_MFP_ALT4_Pos (12)
#define | SYS_P3_MFP_ALT4_Msk (0x1ul << SYS_P3_MFP_ALT4_Pos)
#define | SYS_P3_MFP_ALT5_Pos (13)
#define | SYS_P3_MFP_ALT5_Msk (0x1ul << SYS_P3_MFP_ALT5_Pos)
#define | SYS_P3_MFP_ALT6_Pos (14)
#define | SYS_P3_MFP_ALT6_Msk (0x1ul << SYS_P3_MFP_ALT6_Pos)
#define | SYS_P3_MFP_ALT7_Pos (15)
#define | SYS_P3_MFP_ALT7_Msk (0x1ul << SYS_P3_MFP_ALT7_Pos)
#define | SYS_P3_MFP_TYPE_Pos (16)
#define | SYS_P3_MFP_TYPE_Msk (0xfful << SYS_P3_MFP_TYPE_Pos)
#define | SYS_P3_MFP_P32CTL_Pos (24)
#define | SYS_P3_MFP_P32CTL_Msk (0x1ul << SYS_P3_MFP_P32CTL_Pos)
#define | SYS_P3_MFP_HS_Pos (25)
#define | SYS_P3_MFP_HS_Msk (0x7ful << SYS_P3_MFP_HS_Pos)
#define | SYS_P4_MFP_MFP_Pos (0)
#define | SYS_P4_MFP_MFP_Msk (0xfful << SYS_P4_MFP_MFP_Pos)
#define | SYS_P4_MFP_ALT6_Pos (14)
#define | SYS_P4_MFP_ALT6_Msk (0x1ul << SYS_P4_MFP_ALT6_Pos)
#define | SYS_P4_MFP_ALT7_Pos (15)
#define | SYS_P4_MFP_ALT7_Msk (0x1ul << SYS_P4_MFP_ALT7_Pos)
#define | SYS_P4_MFP_TYPE_Pos (16)
#define | SYS_P4_MFP_TYPE_Msk (0xfful << SYS_P4_MFP_TYPE_Pos)
#define | SYS_P4_MFP_HS_Pos (24)
#define | SYS_P4_MFP_HS_Msk (0xfful << SYS_P4_MFP_HS_Pos)
#define | SYS_P5_MFP_MFP_Pos (0)
#define | SYS_P5_MFP_MFP_Msk (0xfful << SYS_P5_MFP_MFP_Pos)
#define | SYS_P5_MFP_ALT0_Pos (8)
#define | SYS_P5_MFP_ALT0_Msk (0x1ul << SYS_P5_MFP_ALT0_Pos)
#define | SYS_P5_MFP_ALT1_Pos (9)
#define | SYS_P5_MFP_ALT1_Msk (0x1ul << SYS_P5_MFP_ALT1_Pos)
#define | SYS_P5_MFP_ALT2_Pos (10)
#define | SYS_P5_MFP_ALT2_Msk (0x1ul << SYS_P5_MFP_ALT2_Pos)
#define | SYS_P5_MFP_ALT3_Pos (11)
#define | SYS_P5_MFP_ALT3_Msk (0x1ul << SYS_P5_MFP_ALT3_Pos)
#define | SYS_P5_MFP_ALT4_Pos (12)
#define | SYS_P5_MFP_ALT4_Msk (0x1ul << SYS_P5_MFP_ALT4_Pos)
#define | SYS_P5_MFP_ALT5_Pos (13)
#define | SYS_P5_MFP_ALT5_Msk (0x1ul << SYS_P5_MFP_ALT5_Pos)
#define | SYS_P5_MFP_TYPE_Pos (16)
#define | SYS_P5_MFP_TYPE_Msk (0xfful << SYS_P5_MFP_TYPE_Pos)
#define | SYS_P5_MFP_HS_Pos (24)
#define | SYS_P5_MFP_HS_Msk (0xfful << SYS_P5_MFP_HS_Pos)
#define | SYS_EINT0SEL_SEL_Pos (0)
#define | SYS_EINT0SEL_SEL_Msk (0x1ul << SYS_EINT0SEL_SEL_Pos)
#define | SYS_IRCTCTL_FREQSEL_Pos (0)
#define | SYS_IRCTCTL_FREQSEL_Msk (0x1ul << SYS_IRCTCTL_FREQSEL_Pos)
#define | SYS_IRCTCTL_LOOPSEL_Pos (4)
#define | SYS_IRCTCTL_LOOPSEL_Msk (0x3ul << SYS_IRCTCTL_LOOPSEL_Pos)
#define | SYS_IRCTIEN_TFAILIEN_Pos (1)
#define | SYS_IRCTIEN_TFAILIEN_Msk (0x1ul << SYS_IRCTIEN_TFAILIEN_Pos)
#define | SYS_IRCTIEN_CLKEIEN_Pos (2)
#define | SYS_IRCTIEN_CLKEIEN_Msk (0x1ul << SYS_IRCTIEN_CLKEIEN_Pos)
#define | SYS_IRCTISTS_FREQLOCK_Pos (0)
#define | SYS_IRCTISTS_FREQLOCK_Msk (0x1ul << SYS_IRCTISTS_FREQLOCK_Pos)
#define | SYS_IRCTISTS_TFAILIF_Pos (1)
#define | SYS_IRCTISTS_TFAILIF_Msk (0x1ul << SYS_IRCTISTS_TFAILIF_Pos)
#define | SYS_IRCTISTS_CLKERRIF_Pos (2)
#define | SYS_IRCTISTS_CLKERRIF_Msk (0x1ul << SYS_IRCTISTS_CLKERRIF_Pos)
#define | SYS_REGLCTL_REGWRPROT_Pos (0)
#define | SYS_REGLCTL_REGWRPROT_Msk (0x1ul << SYS_REGLCTL_REGWRPROT_Pos)
#define | SYS_REGLCTL_REGPROTDIS_Pos (0)
#define | SYS_REGLCTL_REGPROTDIS_Msk (0x1ul << SYS_REGLCTL_REGPROTDIS_Pos)
#define | TIMER_CTL_PSC_Pos (0)
#define | TIMER_CTL_PSC_Msk (0xfful << TIMER_CTL_PSC_Pos)
#define | TIMER_CTL_CNTDATEN_Pos (16)
#define | TIMER_CTL_CNTDATEN_Msk (0x1ul << TIMER_CTL_CNTDATEN_Pos)
#define | TIMER_CTL_CMPCTL_Pos (17)
#define | TIMER_CTL_CMPCTL_Msk (0x1ul << TIMER_CTL_CMPCTL_Pos)
#define | TIMER_CTL_TGLPINSEL_Pos (18)
#define | TIMER_CTL_TGLPINSEL_Msk (0x1ul << TIMER_CTL_TGLPINSEL_Pos)
#define | TIMER_CTL_CAPPINSEL_Pos (19)
#define | TIMER_CTL_CAPPINSEL_Msk (0x1ul << TIMER_CTL_CAPPINSEL_Pos)
#define | TIMER_CTL_WKEN_Pos (23)
#define | TIMER_CTL_WKEN_Msk (0x1ul << TIMER_CTL_WKEN_Pos)
#define | TIMER_CTL_EXTCNTEN_Pos (24)
#define | TIMER_CTL_EXTCNTEN_Msk (0x1ul << TIMER_CTL_EXTCNTEN_Pos)
#define | TIMER_CTL_ACTSTS_Pos (25)
#define | TIMER_CTL_ACTSTS_Msk (0x1ul << TIMER_CTL_ACTSTS_Pos)
#define | TIMER_CTL_RSTCNT_Pos (26)
#define | TIMER_CTL_RSTCNT_Msk (0x1ul << TIMER_CTL_RSTCNT_Pos)
#define | TIMER_CTL_OPMODE_Pos (27)
#define | TIMER_CTL_OPMODE_Msk (0x3ul << TIMER_CTL_OPMODE_Pos)
#define | TIMER_CTL_INTEN_Pos (29)
#define | TIMER_CTL_INTEN_Msk (0x1ul << TIMER_CTL_INTEN_Pos)
#define | TIMER_CTL_CNTEN_Pos (30)
#define | TIMER_CTL_CNTEN_Msk (0x1ul << TIMER_CTL_CNTEN_Pos)
#define | TIMER_CTL_ICEDEBUG_Pos (31)
#define | TIMER_CTL_ICEDEBUG_Msk (0x1ul << TIMER_CTL_ICEDEBUG_Pos)
#define | TIMER_CMP_CMPDAT_Pos (0)
#define | TIMER_CMP_CMPDAT_Msk (0xfffffful << TIMER_CMP_CMPDAT_Pos)
#define | TIMER_INTSTS_TIF_Pos (0)
#define | TIMER_INTSTS_TIF_Msk (0x1ul << TIMER_INTSTS_TIF_Pos)
#define | TIMER_INTSTS_TWKF_Pos (1)
#define | TIMER_INTSTS_TWKF_Msk (0x1ul << TIMER_INTSTS_TWKF_Pos)
#define | TIMER_CNT_CNT_Pos (0)
#define | TIMER_CNT_CNT_Msk (0xfffffful << TIMER_CNT_CNT_Pos)
#define | TIMER_CAP_CAPDAT_Pos (0)
#define | TIMER_CAP_CAPDAT_Msk (0xfffffful << TIMER_CAP_CAPDAT_Pos)
#define | TIMER_EXTCTL_CNTPHASE_Pos (0)
#define | TIMER_EXTCTL_CNTPHASE_Msk (0x1ul << TIMER_EXTCTL_CNTPHASE_Pos)
#define | TIMER_EXTCTL_CAPEDGE_Pos (1)
#define | TIMER_EXTCTL_CAPEDGE_Msk (0x3ul << TIMER_EXTCTL_CAPEDGE_Pos)
#define | TIMER_EXTCTL_CAPEN_Pos (3)
#define | TIMER_EXTCTL_CAPEN_Msk (0x1ul << TIMER_EXTCTL_CAPEN_Pos)
#define | TIMER_EXTCTL_CAPFUNCS_Pos (4)
#define | TIMER_EXTCTL_CAPFUNCS_Msk (0x1ul << TIMER_EXTCTL_CAPFUNCS_Pos)
#define | TIMER_EXTCTL_CAPIEN_Pos (5)
#define | TIMER_EXTCTL_CAPIEN_Msk (0x1ul << TIMER_EXTCTL_CAPIEN_Pos)
#define | TIMER_EXTCTL_CAPDBEN_Pos (6)
#define | TIMER_EXTCTL_CAPDBEN_Msk (0x1ul << TIMER_EXTCTL_CAPDBEN_Pos)
#define | TIMER_EXTCTL_ECNTDBEN_Pos (7)
#define | TIMER_EXTCTL_ECNTDBEN_Msk (0x1ul << TIMER_EXTCTL_ECNTDBEN_Pos)
#define | TIMER_EXTCTL_CAPMODE_Pos (8)
#define | TIMER_EXTCTL_CAPMODE_Msk (0x1ul << TIMER_EXTCTL_CAPMODE_Pos)
#define | TIMER_EINTSTS_CAPIF_Pos (0)
#define | TIMER_EINTSTS_CAPIF_Msk (0x1ul << TIMER_EINTSTS_CAPIF_Pos)
#define | TIMER_CCAPCTL_CCAPEN_Pos (0)
#define | TIMER_CCAPCTL_CCAPEN_Msk (0x1ul << TIMER_CCAPCTL_CCAPEN_Pos)
#define | TIMER_CCAPCTL_INV_Pos (1)
#define | TIMER_CCAPCTL_INV_Msk (0x1ul << TIMER_CCAPCTL_INV_Pos)
#define | TIMER_CCAPCTL_TMRSEL_Pos (2)
#define | TIMER_CCAPCTL_TMRSEL_Msk (0x1ul << TIMER_CCAPCTL_TMRSEL_Pos)
#define | TIMER_CCAPCTL_CAPCHSEL_Pos (3)
#define | TIMER_CCAPCTL_CAPCHSEL_Msk (0x7ul << TIMER_CCAPCTL_CAPCHSEL_Pos)
#define | TIMER_CCAPCTL_CAPR1F_Pos (8)
#define | TIMER_CCAPCTL_CAPR1F_Msk (0x1ul << TIMER_CCAPCTL_CAPR1F_Pos)
#define | TIMER_CCAPCTL_CAPF1F_Pos (9)
#define | TIMER_CCAPCTL_CAPF1F_Msk (0x1ul << TIMER_CCAPCTL_CAPF1F_Pos)
#define | TIMER_CCAPCTL_CAPR2F_Pos (10)
#define | TIMER_CCAPCTL_CAPR2F_Msk (0x1ul << TIMER_CCAPCTL_CAPR2F_Pos)
#define | TIMER_CCAPCTL_CAPF2F_Pos (11)
#define | TIMER_CCAPCTL_CAPF2F_Msk (0x1ul << TIMER_CCAPCTL_CAPF2F_Pos)
#define | TIMER_CCAP_CAPDAT_Pos (0)
#define | TIMER_CCAP_CAPDAT_Msk (0xfffffful << TIMER_CCAP_CAPDAT_Pos)
#define | UART_DAT_DAT_Pos (0)
#define | UART_DAT_DAT_Msk (0xfful << UART_DAT_DAT_Pos)
#define | UART_INTEN_RDAIEN_Pos (0)
#define | UART_INTEN_RDAIEN_Msk (0x1ul << UART_INTEN_RDAIEN_Pos)
#define | UART_INTEN_THREIEN_Pos (1)
#define | UART_INTEN_THREIEN_Msk (0x1ul << UART_INTEN_THREIEN_Pos)
#define | UART_INTEN_RLSIEN_Pos (2)
#define | UART_INTEN_RLSIEN_Msk (0x1ul << UART_INTEN_RLSIEN_Pos)
#define | UART_INTEN_MODEMIEN_Pos (3)
#define | UART_INTEN_MODEMIEN_Msk (0x1ul << UART_INTEN_MODEMIEN_Pos)
#define | UART_INTEN_RXTOIEN_Pos (4)
#define | UART_INTEN_RXTOIEN_Msk (0x1ul << UART_INTEN_RXTOIEN_Pos)
#define | UART_INTEN_BUFERRIEN_Pos (5)
#define | UART_INTEN_BUFERRIEN_Msk (0x1ul << UART_INTEN_BUFERRIEN_Pos)
#define | UART_INTEN_WKCTSIEN_Pos (6)
#define | UART_INTEN_WKCTSIEN_Msk (0x1ul << UART_INTEN_WKCTSIEN_Pos)
#define | UART_INTEN_TOCNTEN_Pos (11)
#define | UART_INTEN_TOCNTEN_Msk (0x1ul << UART_INTEN_TOCNTEN_Pos)
#define | UART_INTEN_ATORTSEN_Pos (12)
#define | UART_INTEN_ATORTSEN_Msk (0x1ul << UART_INTEN_ATORTSEN_Pos)
#define | UART_INTEN_ATOCTSEN_Pos (13)
#define | UART_INTEN_ATOCTSEN_Msk (0x1ul << UART_INTEN_ATOCTSEN_Pos)
#define | UART_FIFO_RXRST_Pos (1)
#define | UART_FIFO_RXRST_Msk (0x1ul << UART_FIFO_RXRST_Pos)
#define | UART_FIFO_TXRST_Pos (2)
#define | UART_FIFO_TXRST_Msk (0x1ul << UART_FIFO_TXRST_Pos)
#define | UART_FIFO_RFITL_Pos (4)
#define | UART_FIFO_RFITL_Msk (0xful << UART_FIFO_RFITL_Pos)
#define | UART_FIFO_RXOFF_Pos (8)
#define | UART_FIFO_RXOFF_Msk (0x1ul << UART_FIFO_RXOFF_Pos)
#define | UART_FIFO_RTSTRGLV_Pos (16)
#define | UART_FIFO_RTSTRGLV_Msk (0xful << UART_FIFO_RTSTRGLV_Pos)
#define | UART_LINE_WLS_Pos (0)
#define | UART_LINE_WLS_Msk (0x3ul << UART_LINE_WLS_Pos)
#define | UART_LINE_NSB_Pos (2)
#define | UART_LINE_NSB_Msk (0x1ul << UART_LINE_NSB_Pos)
#define | UART_LINE_PBE_Pos (3)
#define | UART_LINE_PBE_Msk (0x1ul << UART_LINE_PBE_Pos)
#define | UART_LINE_EPE_Pos (4)
#define | UART_LINE_EPE_Msk (0x1ul << UART_LINE_EPE_Pos)
#define | UART_LINE_SPE_Pos (5)
#define | UART_LINE_SPE_Msk (0x1ul << UART_LINE_SPE_Pos)
#define | UART_LINE_BCB_Pos (6)
#define | UART_LINE_BCB_Msk (0x1ul << UART_LINE_BCB_Pos)
#define | UART_MODEM_RTS_Pos (1)
#define | UART_MODEM_RTS_Msk (0x1ul << UART_MODEM_RTS_Pos)
#define | UART_MODEM_RTSACTLV_Pos (9)
#define | UART_MODEM_RTSACTLV_Msk (0x1ul << UART_MODEM_RTSACTLV_Pos)
#define | UART_MODEM_RTSSTS_Pos (13)
#define | UART_MODEM_RTSSTS_Msk (0x1ul << UART_MODEM_RTSSTS_Pos)
#define | UART_MODEMSTS_CTSDETF_Pos (0)
#define | UART_MODEMSTS_CTSDETF_Msk (0x1ul << UART_MODEMSTS_CTSDETF_Pos)
#define | UART_MODEMSTS_CTSSTS_Pos (4)
#define | UART_MODEMSTS_CTSSTS_Msk (0x1ul << UART_MODEMSTS_CTSSTS_Pos)
#define | UART_MODEMSTS_CTSACTLV_Pos (8)
#define | UART_MODEMSTS_CTSACTLV_Msk (0x1ul << UART_MODEMSTS_CTSACTLV_Pos)
#define | UART_FIFOSTS_RXOVIF_Pos (0)
#define | UART_FIFOSTS_RXOVIF_Msk (0x1ul << UART_FIFOSTS_RXOVIF_Pos)
#define | UART_FIFOSTS_ADDRDETF_Pos (3)
#define | UART_FIFOSTS_ADDRDETF_Msk (0x1ul << UART_FIFOSTS_ADDRDETF_Pos)
#define | UART_FIFOSTS_PEF_Pos (4)
#define | UART_FIFOSTS_PEF_Msk (0x1ul << UART_FIFOSTS_PEF_Pos)
#define | UART_FIFOSTS_FEF_Pos (5)
#define | UART_FIFOSTS_FEF_Msk (0x1ul << UART_FIFOSTS_FEF_Pos)
#define | UART_FIFOSTS_BIF_Pos (6)
#define | UART_FIFOSTS_BIF_Msk (0x1ul << UART_FIFOSTS_BIF_Pos)
#define | UART_FIFOSTS_RXPTR_Pos (8)
#define | UART_FIFOSTS_RXPTR_Msk (0x3ful << UART_FIFOSTS_RXPTR_Pos)
#define | UART_FIFOSTS_RXEMPTY_Pos (14)
#define | UART_FIFOSTS_RXEMPTY_Msk (0x1ul << UART_FIFOSTS_RXEMPTY_Pos)
#define | UART_FIFOSTS_RXFULL_Pos (15)
#define | UART_FIFOSTS_RXFULL_Msk (0x1ul << UART_FIFOSTS_RXFULL_Pos)
#define | UART_FIFOSTS_TXPTR_Pos (16)
#define | UART_FIFOSTS_TXPTR_Msk (0x3ful << UART_FIFOSTS_TXPTR_Pos)
#define | UART_FIFOSTS_TXEMPTY_Pos (22)
#define | UART_FIFOSTS_TXEMPTY_Msk (0x1ul << UART_FIFOSTS_TXEMPTY_Pos)
#define | UART_FIFOSTS_TXFULL_Pos (23)
#define | UART_FIFOSTS_TXFULL_Msk (0x1ul << UART_FIFOSTS_TXFULL_Pos)
#define | UART_FIFOSTS_TXOVIF_Pos (24)
#define | UART_FIFOSTS_TXOVIF_Msk (0x1ul << UART_FIFOSTS_TXOVIF_Pos)
#define | UART_FIFOSTS_TXEMPTYF_Pos (28)
#define | UART_FIFOSTS_TXEMPTYF_Msk (0x1ul << UART_FIFOSTS_TXEMPTYF_Pos)
#define | UART_INTSTS_RDAIF_Pos (0)
#define | UART_INTSTS_RDAIF_Msk (0x1ul << UART_INTSTS_RDAIF_Pos)
#define | UART_INTSTS_THREIF_Pos (1)
#define | UART_INTSTS_THREIF_Msk (0x1ul << UART_INTSTS_THREIF_Pos)
#define | UART_INTSTS_RLSIF_Pos (2)
#define | UART_INTSTS_RLSIF_Msk (0x1ul << UART_INTSTS_RLSIF_Pos)
#define | UART_INTSTS_MODEMIF_Pos (3)
#define | UART_INTSTS_MODEMIF_Msk (0x1ul << UART_INTSTS_MODEMIF_Pos)
#define | UART_INTSTS_RXTOIF_Pos (4)
#define | UART_INTSTS_RXTOIF_Msk (0x1ul << UART_INTSTS_RXTOIF_Pos)
#define | UART_INTSTS_BUFERRIF_Pos (5)
#define | UART_INTSTS_BUFERRIF_Msk (0x1ul << UART_INTSTS_BUFERRIF_Pos)
#define | UART_INTSTS_RDAINT_Pos (8)
#define | UART_INTSTS_RDAINT_Msk (0x1ul << UART_INTSTS_RDAINT_Pos)
#define | UART_INTSTS_THREINT_Pos (9)
#define | UART_INTSTS_THREINT_Msk (0x1ul << UART_INTSTS_THREINT_Pos)
#define | UART_INTSTS_RLSINT_Pos (10)
#define | UART_INTSTS_RLSINT_Msk (0x1ul << UART_INTSTS_RLSINT_Pos)
#define | UART_INTSTS_MODEMINT_Pos (11)
#define | UART_INTSTS_MODEMINT_Msk (0x1ul << UART_INTSTS_MODEMINT_Pos)
#define | UART_INTSTS_RXTOINT_Pos (12)
#define | UART_INTSTS_RXTOINT_Msk (0x1ul << UART_INTSTS_RXTOINT_Pos)
#define | UART_INTSTS_BUFERRINT_Pos (13)
#define | UART_INTSTS_BUFERRINT_Msk (0x1ul << UART_INTSTS_BUFERRINT_Pos)
#define | UART_TOUT_TOIC_Pos (0)
#define | UART_TOUT_TOIC_Msk (0xfful << UART_TOUT_TOIC_Pos)
#define | UART_TOUT_DLY_Pos (8)
#define | UART_TOUT_DLY_Msk (0xfful << UART_TOUT_DLY_Pos)
#define | UART_BAUD_BRD_Pos (0)
#define | UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)
#define | UART_BAUD_EDIVM1_Pos (24)
#define | UART_BAUD_EDIVM1_Msk (0xful << UART_BAUD_EDIVM1_Pos)
#define | UART_BAUD_BAUDM0_Pos (28)
#define | UART_BAUD_BAUDM0_Msk (0x1ul << UART_BAUD_BAUDM0_Pos)
#define | UART_BAUD_BAUDM1_Pos (29)
#define | UART_BAUD_BAUDM1_Msk (0x1ul << UART_BAUD_BAUDM1_Pos)
#define | UART_IRDA_TXEN_Pos (1)
#define | UART_IRDA_TXEN_Msk (0x1ul << UART_IRDA_TXEN_Pos)
#define | UART_IRDA_TXINV_Pos (5)
#define | UART_IRDA_TXINV_Msk (0x1ul << UART_IRDA_TXINV_Pos)
#define | UART_IRDA_RXINV_Pos (6)
#define | UART_IRDA_RXINV_Msk (0x1ul << UART_IRDA_RXINV_Pos)
#define | UART_ALTCTL_RS485NMM_Pos (8)
#define | UART_ALTCTL_RS485NMM_Msk (0x1ul << UART_ALTCTL_RS485NMM_Pos)
#define | UART_ALTCTL_RS485AAD_Pos (9)
#define | UART_ALTCTL_RS485AAD_Msk (0x1ul << UART_ALTCTL_RS485AAD_Pos)
#define | UART_ALTCTL_RS485AUD_Pos (10)
#define | UART_ALTCTL_RS485AUD_Msk (0x1ul << UART_ALTCTL_RS485AUD_Pos)
#define | UART_ALTCTL_ADDRDEN_Pos (15)
#define | UART_ALTCTL_ADDRDEN_Msk (0x1ul << UART_ALTCTL_ADDRDEN_Pos)
#define | UART_ALTCTL_ADDRMV_Pos (24)
#define | UART_ALTCTL_ADDRMV_Msk (0xfful << UART_ALTCTL_ADDRMV_Pos)
#define | UART_FUNCSEL_FUNCSEL_Pos (0)
#define | UART_FUNCSEL_FUNCSEL_Msk (0x3ul << UART_FUNCSEL_FUNCSEL_Pos)
#define | WDT_CTL_RSTCNT_Pos (0)
#define | WDT_CTL_RSTCNT_Msk (0x1ul << WDT_CTL_RSTCNT_Pos)
#define | WDT_CTL_RSTEN_Pos (1)
#define | WDT_CTL_RSTEN_Msk (0x1ul << WDT_CTL_RSTEN_Pos)
#define | WDT_CTL_RSTF_Pos (2)
#define | WDT_CTL_RSTF_Msk (0x1ul << WDT_CTL_RSTF_Pos)
#define | WDT_CTL_IF_Pos (3)
#define | WDT_CTL_IF_Msk (0x1ul << WDT_CTL_IF_Pos)
#define | WDT_CTL_WKEN_Pos (4)
#define | WDT_CTL_WKEN_Msk (0x1ul << WDT_CTL_WKEN_Pos)
#define | WDT_CTL_WKF_Pos (5)
#define | WDT_CTL_WKF_Msk (0x1ul << WDT_CTL_WKF_Pos)
#define | WDT_CTL_INTEN_Pos (6)
#define | WDT_CTL_INTEN_Msk (0x1ul << WDT_CTL_INTEN_Pos)
#define | WDT_CTL_WDTEN_Pos (7)
#define | WDT_CTL_WDTEN_Msk (0x1ul << WDT_CTL_WDTEN_Pos)
#define | WDT_CTL_TOUTSEL_Pos (8)
#define | WDT_CTL_TOUTSEL_Msk (0x7ul << WDT_CTL_TOUTSEL_Pos)
#define | WDT_CTL_ICEDEBUG_Pos (31)
#define | WDT_CTL_ICEDEBUG_Msk (0x1ul << WDT_CTL_ICEDEBUG_Pos)

## Typedefs
typedef enum IRQn | IRQn_Type
typedef volatile unsigned char | vu8
| Define 8-bit unsigned volatile data type. More...
typedef volatile unsigned short | vu16
| Define 16-bit unsigned volatile data type. More...
typedef volatile unsigned long | vu32
| Define 32-bit unsigned volatile data type. More...

## Enumerations
enum | IRQn { NonMaskableInt_IRQn = -14 , HardFault_IRQn = -13 , SVCall_IRQn = -5 , PendSV_IRQn = -2 , SysTick_IRQn = -1 , BOD_IRQn = 0 , WDT_IRQn = 1 , EINT0_IRQn = 2 , EINT1_IRQn = 3 , GPIO01_IRQn = 4 , GPIO234_IRQn = 5 , PWM_IRQn = 6 , FB_IRQn = 7 , TMR0_IRQn = 8 , TMR1_IRQn = 9 , UART0_IRQn = 12 , UART1_IRQn = 13 , SPI_IRQn = 14 , GPIO5_IRQn = 16 , HIRC_IRQn = 17 , I2C_IRQn = 18 , ACMP_IRQn = 25 , PDWU_IRQn = 28 , ADC_IRQn = 29 }

## Detailed Description

Mini55 series peripheral access layer header file. This file contains all the peripheral register's definitions, bits definitions and memory mapping for NuMicro Mini55 series MCU.

Version
  V1.00

Revision
  26

Date
  15/07/17 3:25p

Note
  Copyright (C) 2022 Nuvoton Technology Corp. All rights reserved.

Definition in file Mini55Series.h.

## Macro Definition Documentation

## ◆ FMC_DFBA_DFBA_Msk

#define FMC_DFBA_DFBA_Msk (0xfffffffful << FMC_DFBA_DFBA_Pos)

FMC_T::DFBA: DFBA Mask

Definition at line 1454 of file Mini55Series.h.

## ◆ FMC_DFBA_DFBA_Pos

#define FMC_DFBA_DFBA_Pos (0)

FMC_T::DFBA: DFBA Position

Definition at line 1453 of file Mini55Series.h.

## ◆ FMC_ISPADDR_ISPADR_Msk

#define FMC_ISPADDR_ISPADR_Msk (0xfffffffful << FMC_ISPADDR_ISPADR_Pos)

FMC_T::ISPADDR: ISPADR Mask

Definition at line 1442 of file Mini55Series.h.

## ◆ FMC_ISPADDR_ISPADR_Pos

#define FMC_ISPADDR_ISPADR_Pos (0)

FMC_T::ISPADDR: ISPADR Position

Definition at line 1441 of file Mini55Series.h.

## ◆ FMC_ISPCMD_CMD_Msk

#define FMC_ISPCMD_CMD_Msk (0x3ful << FMC_ISPCMD_CMD_Pos)

FMC_T::ISPCMD: CMD Mask

Definition at line 1448 of file Mini55Series.h.

## ◆ FMC_ISPCMD_CMD_Pos

#define FMC_ISPCMD_CMD_Pos (0)

FMC_T::ISPCMD: CMD Position

Definition at line 1447 of file Mini55Series.h.

## ◆ FMC_ISPCTL_APUEN_Msk

#define FMC_ISPCTL_APUEN_Msk (0x1ul << FMC_ISPCTL_APUEN_Pos)

FMC_T::ISPCTL: APUEN Mask

Definition at line 1430 of file Mini55Series.h.

## ◆ FMC_ISPCTL_APUEN_Pos

#define FMC_ISPCTL_APUEN_Pos (3)

FMC_T::ISPCTL: APUEN Position

Definition at line 1429 of file Mini55Series.h.

## ◆ FMC_ISPCTL_BS_Msk

#define FMC_ISPCTL_BS_Msk (0x1ul << FMC_ISPCTL_BS_Pos)

FMC_T::ISPCTL: BS Mask

Definition at line 1427 of file Mini55Series.h.

## ◆ FMC_ISPCTL_BS_Pos

#define FMC_ISPCTL_BS_Pos (1)

FMC_T::ISPCTL: BS Position

Definition at line 1426 of file Mini55Series.h.

## ◆ FMC_ISPCTL_CFGUEN_Msk

#define FMC_ISPCTL_CFGUEN_Msk (0x1ul << FMC_ISPCTL_CFGUEN_Pos)

FMC_T::ISPCTL: CFGUEN Mask

Definition at line 1433 of file Mini55Series.h.

## ◆ FMC_ISPCTL_CFGUEN_Pos

#define FMC_ISPCTL_CFGUEN_Pos (4)

FMC_T::ISPCTL: CFGUEN Position

Definition at line 1432 of file Mini55Series.h.

## ◆ FMC_ISPCTL_ISPEN_Msk

#define FMC_ISPCTL_ISPEN_Msk (0x1ul << FMC_ISPCTL_ISPEN_Pos)

FMC_T::ISPCTL: ISPEN Mask

Definition at line 1424 of file Mini55Series.h.

## ◆ FMC_ISPCTL_ISPEN_Pos

#define FMC_ISPCTL_ISPEN_Pos (0)

    @addtogroup FMC_CONST FMC Bit Field Definition
    Constant Definitions for FMC Controller

FMC_T::ISPCTL: ISPEN Position

Definition at line 1423 of file Mini55Series.h.

## ◆ FMC_ISPCTL_ISPFF_Msk

#define FMC_ISPCTL_ISPFF_Msk (0x1ul << FMC_ISPCTL_ISPFF_Pos)

FMC_T::ISPCTL: ISPFF Mask

Definition at line 1439 of file Mini55Series.h.

## ◆ FMC_ISPCTL_ISPFF_Pos

#define FMC_ISPCTL_ISPFF_Pos (6)

FMC_T::ISPCTL: ISPFF Position

Definition at line 1438 of file Mini55Series.h.

## ◆ FMC_ISPCTL_LDUEN_Msk

#define FMC_ISPCTL_LDUEN_Msk (0x1ul << FMC_ISPCTL_LDUEN_Pos)

FMC_T::ISPCTL: LDUEN Mask

Definition at line 1436 of file Mini55Series.h.

## ◆ FMC_ISPCTL_LDUEN_Pos

#define FMC_ISPCTL_LDUEN_Pos (5)

FMC_T::ISPCTL: LDUEN Position

Definition at line 1435 of file Mini55Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Msk

#define FMC_ISPDAT_ISPDAT_Msk (0xfffffffful << FMC_ISPDAT_ISPDAT_Pos)

FMC_T::ISPDAT: ISPDAT Mask

Definition at line 1445 of file Mini55Series.h.

## ◆ FMC_ISPDAT_ISPDAT_Pos

#define FMC_ISPDAT_ISPDAT_Pos (0)

FMC_T::ISPDAT: ISPDAT Position

Definition at line 1444 of file Mini55Series.h.

## ◆ FMC_ISPSTS_CBS_Msk

#define FMC_ISPSTS_CBS_Msk (0x3ul << FMC_ISPSTS_CBS_Pos)

FMC_T::ISPSTS: CBS Mask

Definition at line 1460 of file Mini55Series.h.

## ◆ FMC_ISPSTS_CBS_Pos

#define FMC_ISPSTS_CBS_Pos (1)

FMC_T::ISPSTS: CBS Position

Definition at line 1459 of file Mini55Series.h.

## ◆ FMC_ISPSTS_ISPBUSY_Msk

#define FMC_ISPSTS_ISPBUSY_Msk (0x1ul << FMC_ISPSTS_ISPBUSY_Pos)

FMC_T::ISPSTS: ISPBUSY Mask

Definition at line 1457 of file Mini55Series.h.

## ◆ FMC_ISPSTS_ISPBUSY_Pos

#define FMC_ISPSTS_ISPBUSY_Pos (0)

FMC_T::ISPSTS: ISPBUSY Position

Definition at line 1456 of file Mini55Series.h.

## ◆ FMC_ISPSTS_ISPFF_Msk

#define FMC_ISPSTS_ISPFF_Msk (0x1ul << FMC_ISPSTS_ISPFF_Pos)

FMC_T::ISPSTS: ISPFF Mask

Definition at line 1463 of file Mini55Series.h.

## ◆ FMC_ISPSTS_ISPFF_Pos

#define FMC_ISPSTS_ISPFF_Pos (6)

FMC_T::ISPSTS: ISPFF Position

Definition at line 1462 of file Mini55Series.h.

## ◆ FMC_ISPSTS_VECMAP_Msk

#define FMC_ISPSTS_VECMAP_Msk (0xffful << FMC_ISPSTS_VECMAP_Pos)

FMC_T::ISPSTS: VECMAP Mask

Definition at line 1466 of file Mini55Series.h.

## ◆ FMC_ISPSTS_VECMAP_Pos

#define FMC_ISPSTS_VECMAP_Pos (9)

FMC_T::ISPSTS: VECMAP Position

Definition at line 1465 of file Mini55Series.h.

## ◆ FMC_ISPTRG_ISPGO_Msk

#define FMC_ISPTRG_ISPGO_Msk (0x1ul << FMC_ISPTRG_ISPGO_Pos)

FMC_T::ISPTRG: ISPGO Mask

Definition at line 1451 of file Mini55Series.h.

## ◆ FMC_ISPTRG_ISPGO_Pos

#define FMC_ISPTRG_ISPGO_Pos (0)

FMC_T::ISPTRG: ISPGO Position

Definition at line 1450 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK0_Msk

#define GP_DATMSK_DATMSK0_Msk (0x1ul << GP_DATMSK_DATMSK0_Pos)

GPIO_T::DATMSK: DATMSK0 Mask

Definition at line 1820 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK0_Pos

#define GP_DATMSK_DATMSK0_Pos (0)

GPIO_T::DATMSK: DATMSK0 Position

Definition at line 1819 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK1_Msk

#define GP_DATMSK_DATMSK1_Msk (0x1ul << GP_DATMSK_DATMSK1_Pos)

GPIO_T::DATMSK: DATMSK1 Mask

Definition at line 1823 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK1_Pos

#define GP_DATMSK_DATMSK1_Pos (1)

GPIO_T::DATMSK: DATMSK1 Position

Definition at line 1822 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK2_Msk

#define GP_DATMSK_DATMSK2_Msk (0x1ul << GP_DATMSK_DATMSK2_Pos)

GPIO_T::DATMSK: DATMSK2 Mask

Definition at line 1826 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK2_Pos

#define GP_DATMSK_DATMSK2_Pos (2)

GPIO_T::DATMSK: DATMSK2 Position

Definition at line 1825 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK3_Msk

#define GP_DATMSK_DATMSK3_Msk (0x1ul << GP_DATMSK_DATMSK3_Pos)

GPIO_T::DATMSK: DATMSK3 Mask

Definition at line 1829 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK3_Pos

#define GP_DATMSK_DATMSK3_Pos (3)

GPIO_T::DATMSK: DATMSK3 Position

Definition at line 1828 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK4_Msk

#define GP_DATMSK_DATMSK4_Msk (0x1ul << GP_DATMSK_DATMSK4_Pos)

GPIO_T::DATMSK: DATMSK4 Mask

Definition at line 1832 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK4_Pos

#define GP_DATMSK_DATMSK4_Pos (4)

GPIO_T::DATMSK: DATMSK4 Position

Definition at line 1831 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK5_Msk

#define GP_DATMSK_DATMSK5_Msk (0x1ul << GP_DATMSK_DATMSK5_Pos)

GPIO_T::DATMSK: DATMSK5 Mask

Definition at line 1835 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK5_Pos

#define GP_DATMSK_DATMSK5_Pos (5)

GPIO_T::DATMSK: DATMSK5 Position

Definition at line 1834 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK6_Msk

#define GP_DATMSK_DATMSK6_Msk (0x1ul << GP_DATMSK_DATMSK6_Pos)

GPIO_T::DATMSK: DATMSK6 Mask

Definition at line 1838 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK6_Pos

#define GP_DATMSK_DATMSK6_Pos (6)

GPIO_T::DATMSK: DATMSK6 Position

Definition at line 1837 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK7_Msk

#define GP_DATMSK_DATMSK7_Msk (0x1ul << GP_DATMSK_DATMSK7_Pos)

GPIO_T::DATMSK: DATMSK7 Mask

Definition at line 1841 of file Mini55Series.h.

## ◆ GP_DATMSK_DATMSK7_Pos

#define GP_DATMSK_DATMSK7_Pos (7)

GPIO_T::DATMSK: DATMSK7 Position

Definition at line 1840 of file Mini55Series.h.

## ◆ GP_DBCTL_DBCLKSEL_Msk

#define GP_DBCTL_DBCLKSEL_Msk (0xful << GP_DBCTL_DBCLKSEL_Pos)

GPIO_DB_T::DBCTL: DBCLKSEL Mask

Definition at line 1988 of file Mini55Series.h.

## ◆ GP_DBCTL_DBCLKSEL_Pos

#define GP_DBCTL_DBCLKSEL_Pos (0)

GPIO_DB_T::DBCTL: DBCLKSEL Position

Definition at line 1987 of file Mini55Series.h.

## ◆ GP_DBCTL_DBCLKSRC_Msk

#define GP_DBCTL_DBCLKSRC_Msk (0x1ul << GP_DBCTL_DBCLKSRC_Pos)

GPIO_DB_T::DBCTL: DBCLKSRC Mask

Definition at line 1991 of file Mini55Series.h.

## ◆ GP_DBCTL_DBCLKSRC_Pos

#define GP_DBCTL_DBCLKSRC_Pos (4)

GPIO_DB_T::DBCTL: DBCLKSRC Position

Definition at line 1990 of file Mini55Series.h.

## ◆ GP_DBCTL_ICLKON_Msk

#define GP_DBCTL_ICLKON_Msk (0x1ul << GP_DBCTL_ICLKON_Pos)

GPIO_DB_T::DBCTL: ICLKON Mask

Definition at line 1994 of file Mini55Series.h.

## ◆ GP_DBCTL_ICLKON_Pos

#define GP_DBCTL_ICLKON_Pos (5)

GPIO_DB_T::DBCTL: ICLKON Position

Definition at line 1993 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN0_Msk

#define GP_DBEN_DBEN0_Msk (0x1ul << GP_DBEN_DBEN0_Pos)

GPIO_T::DBEN: DBEN0 Mask

Definition at line 1868 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN0_Pos

#define GP_DBEN_DBEN0_Pos (0)

GPIO_T::DBEN: DBEN0 Position

Definition at line 1867 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN1_Msk

#define GP_DBEN_DBEN1_Msk (0x1ul << GP_DBEN_DBEN1_Pos)

GPIO_T::DBEN: DBEN1 Mask

Definition at line 1871 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN1_Pos

#define GP_DBEN_DBEN1_Pos (1)

GPIO_T::DBEN: DBEN1 Position

Definition at line 1870 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN2_Msk

#define GP_DBEN_DBEN2_Msk (0x1ul << GP_DBEN_DBEN2_Pos)

GPIO_T::DBEN: DBEN2 Mask

Definition at line 1874 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN2_Pos

#define GP_DBEN_DBEN2_Pos (2)

GPIO_T::DBEN: DBEN2 Position

Definition at line 1873 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN3_Msk

#define GP_DBEN_DBEN3_Msk (0x1ul << GP_DBEN_DBEN3_Pos)

GPIO_T::DBEN: DBEN3 Mask

Definition at line 1877 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN3_Pos

#define GP_DBEN_DBEN3_Pos (3)

GPIO_T::DBEN: DBEN3 Position

Definition at line 1876 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN4_Msk

#define GP_DBEN_DBEN4_Msk (0x1ul << GP_DBEN_DBEN4_Pos)

GPIO_T::DBEN: DBEN4 Mask

Definition at line 1880 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN4_Pos

#define GP_DBEN_DBEN4_Pos (4)

GPIO_T::DBEN: DBEN4 Position

Definition at line 1879 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN5_Msk

#define GP_DBEN_DBEN5_Msk (0x1ul << GP_DBEN_DBEN5_Pos)

GPIO_T::DBEN: DBEN5 Mask

Definition at line 1883 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN5_Pos

#define GP_DBEN_DBEN5_Pos (5)

GPIO_T::DBEN: DBEN5 Position

Definition at line 1882 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN6_Msk

#define GP_DBEN_DBEN6_Msk (0x1ul << GP_DBEN_DBEN6_Pos)

GPIO_T::DBEN: DBEN6 Mask

Definition at line 1886 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN6_Pos

#define GP_DBEN_DBEN6_Pos (6)

GPIO_T::DBEN: DBEN6 Position

Definition at line 1885 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN7_Msk

#define GP_DBEN_DBEN7_Msk (0x1ul << GP_DBEN_DBEN7_Pos)

GPIO_T::DBEN: DBEN7 Mask

Definition at line 1889 of file Mini55Series.h.

## ◆ GP_DBEN_DBEN7_Pos

#define GP_DBEN_DBEN7_Pos (7)

GPIO_T::DBEN: DBEN7 Position

Definition at line 1888 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF0_Msk

#define GP_DINOFF_DINOFF0_Msk (0x1ul << GP_DINOFF_DINOFF0_Pos)

GPIO_T::DINOFF: DINOFF0 Mask

Definition at line 1772 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF0_Pos

#define GP_DINOFF_DINOFF0_Pos (16)

GPIO_T::DINOFF: DINOFF0 Position

Definition at line 1771 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF1_Msk

#define GP_DINOFF_DINOFF1_Msk (0x1ul << GP_DINOFF_DINOFF1_Pos)

GPIO_T::DINOFF: DINOFF1 Mask

Definition at line 1775 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF1_Pos

#define GP_DINOFF_DINOFF1_Pos (17)

GPIO_T::DINOFF: DINOFF1 Position

Definition at line 1774 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF2_Msk

#define GP_DINOFF_DINOFF2_Msk (0x1ul << GP_DINOFF_DINOFF2_Pos)

GPIO_T::DINOFF: DINOFF2 Mask

Definition at line 1778 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF2_Pos

#define GP_DINOFF_DINOFF2_Pos (18)

GPIO_T::DINOFF: DINOFF2 Position

Definition at line 1777 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF3_Msk

#define GP_DINOFF_DINOFF3_Msk (0x1ul << GP_DINOFF_DINOFF3_Pos)

GPIO_T::DINOFF: DINOFF3 Mask

Definition at line 1781 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF3_Pos

#define GP_DINOFF_DINOFF3_Pos (19)

GPIO_T::DINOFF: DINOFF3 Position

Definition at line 1780 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF4_Msk

#define GP_DINOFF_DINOFF4_Msk (0x1ul << GP_DINOFF_DINOFF4_Pos)

GPIO_T::DINOFF: DINOFF4 Mask

Definition at line 1784 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF4_Pos

#define GP_DINOFF_DINOFF4_Pos (20)

GPIO_T::DINOFF: DINOFF4 Position

Definition at line 1783 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF5_Msk

#define GP_DINOFF_DINOFF5_Msk (0x1ul << GP_DINOFF_DINOFF5_Pos)

GPIO_T::DINOFF: DINOFF5 Mask

Definition at line 1787 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF5_Pos

#define GP_DINOFF_DINOFF5_Pos (21)

GPIO_T::DINOFF: DINOFF5 Position

Definition at line 1786 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF6_Msk

#define GP_DINOFF_DINOFF6_Msk (0x1ul << GP_DINOFF_DINOFF6_Pos)

GPIO_T::DINOFF: DINOFF6 Mask

Definition at line 1790 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF6_Pos

#define GP_DINOFF_DINOFF6_Pos (22)

GPIO_T::DINOFF: DINOFF6 Position

Definition at line 1789 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF7_Msk

#define GP_DINOFF_DINOFF7_Msk (0x1ul << GP_DINOFF_DINOFF7_Pos)

GPIO_T::DINOFF: DINOFF7 Mask

Definition at line 1793 of file Mini55Series.h.

## ◆ GP_DINOFF_DINOFF7_Pos

#define GP_DINOFF_DINOFF7_Pos (23)

GPIO_T::DINOFF: DINOFF7 Position

Definition at line 1792 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT0_Msk

#define GP_DOUT_DOUT0_Msk (0x1ul << GP_DOUT_DOUT0_Pos)

GPIO_T::DOUT: DOUT0 Mask

Definition at line 1796 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT0_Pos

#define GP_DOUT_DOUT0_Pos (0)

GPIO_T::DOUT: DOUT0 Position

Definition at line 1795 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT1_Msk

#define GP_DOUT_DOUT1_Msk (0x1ul << GP_DOUT_DOUT1_Pos)

GPIO_T::DOUT: DOUT1 Mask

Definition at line 1799 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT1_Pos

#define GP_DOUT_DOUT1_Pos (1)

GPIO_T::DOUT: DOUT1 Position

Definition at line 1798 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT2_Msk

#define GP_DOUT_DOUT2_Msk (0x1ul << GP_DOUT_DOUT2_Pos)

GPIO_T::DOUT: DOUT2 Mask

Definition at line 1802 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT2_Pos

#define GP_DOUT_DOUT2_Pos (2)

GPIO_T::DOUT: DOUT2 Position

Definition at line 1801 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT3_Msk

#define GP_DOUT_DOUT3_Msk (0x1ul << GP_DOUT_DOUT3_Pos)

GPIO_T::DOUT: DOUT3 Mask

Definition at line 1805 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT3_Pos

#define GP_DOUT_DOUT3_Pos (3)

GPIO_T::DOUT: DOUT3 Position

Definition at line 1804 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT4_Msk

#define GP_DOUT_DOUT4_Msk (0x1ul << GP_DOUT_DOUT4_Pos)

GPIO_T::DOUT: DOUT4 Mask

Definition at line 1808 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT4_Pos

#define GP_DOUT_DOUT4_Pos (4)

GPIO_T::DOUT: DOUT4 Position

Definition at line 1807 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT5_Msk

#define GP_DOUT_DOUT5_Msk (0x1ul << GP_DOUT_DOUT5_Pos)

GPIO_T::DOUT: DOUT5 Mask

Definition at line 1811 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT5_Pos

#define GP_DOUT_DOUT5_Pos (5)

GPIO_T::DOUT: DOUT5 Position

Definition at line 1810 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT6_Msk

#define GP_DOUT_DOUT6_Msk (0x1ul << GP_DOUT_DOUT6_Pos)

GPIO_T::DOUT: DOUT6 Mask

Definition at line 1814 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT6_Pos

#define GP_DOUT_DOUT6_Pos (6)

GPIO_T::DOUT: DOUT6 Position

Definition at line 1813 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT7_Msk

#define GP_DOUT_DOUT7_Msk (0x1ul << GP_DOUT_DOUT7_Pos)

GPIO_T::DOUT: DOUT7 Mask

Definition at line 1817 of file Mini55Series.h.

## ◆ GP_DOUT_DOUT7_Pos

#define GP_DOUT_DOUT7_Pos (7)

GPIO_T::DOUT: DOUT7 Position

Definition at line 1816 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN0_Msk

#define GP_INTEN_FLIEN0_Msk (0x1ul << GP_INTEN_FLIEN0_Pos)

GPIO_T::INTEN: FLIEN0 Mask

Definition at line 1916 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN0_Pos

#define GP_INTEN_FLIEN0_Pos (0)

GPIO_T::INTEN: FLIEN0 Position

Definition at line 1915 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN1_Msk

#define GP_INTEN_FLIEN1_Msk (0x1ul << GP_INTEN_FLIEN1_Pos)

GPIO_T::INTEN: FLIEN1 Mask

Definition at line 1919 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN1_Pos

#define GP_INTEN_FLIEN1_Pos (1)

GPIO_T::INTEN: FLIEN1 Position

Definition at line 1918 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN2_Msk

#define GP_INTEN_FLIEN2_Msk (0x1ul << GP_INTEN_FLIEN2_Pos)

GPIO_T::INTEN: FLIEN2 Mask

Definition at line 1922 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN2_Pos

#define GP_INTEN_FLIEN2_Pos (2)

GPIO_T::INTEN: FLIEN2 Position

Definition at line 1921 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN3_Msk

#define GP_INTEN_FLIEN3_Msk (0x1ul << GP_INTEN_FLIEN3_Pos)

GPIO_T::INTEN: FLIEN3 Mask

Definition at line 1925 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN3_Pos

#define GP_INTEN_FLIEN3_Pos (3)

GPIO_T::INTEN: FLIEN3 Position

Definition at line 1924 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN4_Msk

#define GP_INTEN_FLIEN4_Msk (0x1ul << GP_INTEN_FLIEN4_Pos)

GPIO_T::INTEN: FLIEN4 Mask

Definition at line 1928 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN4_Pos

#define GP_INTEN_FLIEN4_Pos (4)

GPIO_T::INTEN: FLIEN4 Position

Definition at line 1927 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN5_Msk

#define GP_INTEN_FLIEN5_Msk (0x1ul << GP_INTEN_FLIEN5_Pos)

GPIO_T::INTEN: FLIEN5 Mask

Definition at line 1931 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN5_Pos

#define GP_INTEN_FLIEN5_Pos (5)

GPIO_T::INTEN: FLIEN5 Position

Definition at line 1930 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN6_Msk

#define GP_INTEN_FLIEN6_Msk (0x1ul << GP_INTEN_FLIEN6_Pos)

GPIO_T::INTEN: FLIEN6 Mask

Definition at line 1934 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN6_Pos

#define GP_INTEN_FLIEN6_Pos (6)

GPIO_T::INTEN: FLIEN6 Position

Definition at line 1933 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN7_Msk

#define GP_INTEN_FLIEN7_Msk (0x1ul << GP_INTEN_FLIEN7_Pos)

GPIO_T::INTEN: FLIEN7 Mask

Definition at line 1937 of file Mini55Series.h.

## ◆ GP_INTEN_FLIEN7_Pos

#define GP_INTEN_FLIEN7_Pos (7)

GPIO_T::INTEN: FLIEN7 Position

Definition at line 1936 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN0_Msk

#define GP_INTEN_RHIEN0_Msk (0x1ul << GP_INTEN_RHIEN0_Pos)

GPIO_T::INTEN: RHIEN0 Mask

Definition at line 1940 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN0_Pos

#define GP_INTEN_RHIEN0_Pos (16)

GPIO_T::INTEN: RHIEN0 Position

Definition at line 1939 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN1_Msk

#define GP_INTEN_RHIEN1_Msk (0x1ul << GP_INTEN_RHIEN1_Pos)

GPIO_T::INTEN: RHIEN1 Mask

Definition at line 1943 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN1_Pos

#define GP_INTEN_RHIEN1_Pos (17)

GPIO_T::INTEN: RHIEN1 Position

Definition at line 1942 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN2_Msk

#define GP_INTEN_RHIEN2_Msk (0x1ul << GP_INTEN_RHIEN2_Pos)

GPIO_T::INTEN: RHIEN2 Mask

Definition at line 1946 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN2_Pos

#define GP_INTEN_RHIEN2_Pos (18)

GPIO_T::INTEN: RHIEN2 Position

Definition at line 1945 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN3_Msk

#define GP_INTEN_RHIEN3_Msk (0x1ul << GP_INTEN_RHIEN3_Pos)

GPIO_T::INTEN: RHIEN3 Mask

Definition at line 1949 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN3_Pos

#define GP_INTEN_RHIEN3_Pos (19)

GPIO_T::INTEN: RHIEN3 Position

Definition at line 1948 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN4_Msk

#define GP_INTEN_RHIEN4_Msk (0x1ul << GP_INTEN_RHIEN4_Pos)

GPIO_T::INTEN: RHIEN4 Mask

Definition at line 1952 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN4_Pos

#define GP_INTEN_RHIEN4_Pos (20)

GPIO_T::INTEN: RHIEN4 Position

Definition at line 1951 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN5_Msk

#define GP_INTEN_RHIEN5_Msk (0x1ul << GP_INTEN_RHIEN5_Pos)

GPIO_T::INTEN: RHIEN5 Mask

Definition at line 1955 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN5_Pos

#define GP_INTEN_RHIEN5_Pos (21)

GPIO_T::INTEN: RHIEN5 Position

Definition at line 1954 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN6_Msk

#define GP_INTEN_RHIEN6_Msk (0x1ul << GP_INTEN_RHIEN6_Pos)

GPIO_T::INTEN: RHIEN6 Mask

Definition at line 1958 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN6_Pos

#define GP_INTEN_RHIEN6_Pos (22)

GPIO_T::INTEN: RHIEN6 Position

Definition at line 1957 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN7_Msk

#define GP_INTEN_RHIEN7_Msk (0x1ul << GP_INTEN_RHIEN7_Pos)

GPIO_T::INTEN: RHIEN7 Mask

Definition at line 1961 of file Mini55Series.h.

## ◆ GP_INTEN_RHIEN7_Pos

#define GP_INTEN_RHIEN7_Pos (23)

GPIO_T::INTEN: RHIEN7 Position

Definition at line 1960 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC0_Msk

#define GP_INTSRC_INTSRC0_Msk (0x1ul << GP_INTSRC_INTSRC0_Pos)

GPIO_T::INTSRC: INTSRC0 Mask

Definition at line 1964 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC0_Pos

#define GP_INTSRC_INTSRC0_Pos (0)

GPIO_T::INTSRC: INTSRC0 Position

Definition at line 1963 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC1_Msk

#define GP_INTSRC_INTSRC1_Msk (0x1ul << GP_INTSRC_INTSRC1_Pos)

GPIO_T::INTSRC: INTSRC1 Mask

Definition at line 1967 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC1_Pos

#define GP_INTSRC_INTSRC1_Pos (1)

GPIO_T::INTSRC: INTSRC1 Position

Definition at line 1966 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC2_Msk

#define GP_INTSRC_INTSRC2_Msk (0x1ul << GP_INTSRC_INTSRC2_Pos)

GPIO_T::INTSRC: INTSRC2 Mask

Definition at line 1970 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC2_Pos

#define GP_INTSRC_INTSRC2_Pos (2)

GPIO_T::INTSRC: INTSRC2 Position

Definition at line 1969 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC3_Msk

#define GP_INTSRC_INTSRC3_Msk (0x1ul << GP_INTSRC_INTSRC3_Pos)

GPIO_T::INTSRC: INTSRC3 Mask

Definition at line 1973 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC3_Pos

#define GP_INTSRC_INTSRC3_Pos (3)

GPIO_T::INTSRC: INTSRC3 Position

Definition at line 1972 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC4_Msk

#define GP_INTSRC_INTSRC4_Msk (0x1ul << GP_INTSRC_INTSRC4_Pos)

GPIO_T::INTSRC: INTSRC4 Mask

Definition at line 1976 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC4_Pos

#define GP_INTSRC_INTSRC4_Pos (4)

GPIO_T::INTSRC: INTSRC4 Position

Definition at line 1975 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC5_Msk

#define GP_INTSRC_INTSRC5_Msk (0x1ul << GP_INTSRC_INTSRC5_Pos)

GPIO_T::INTSRC: INTSRC5 Mask

Definition at line 1979 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC5_Pos

#define GP_INTSRC_INTSRC5_Pos (5)

GPIO_T::INTSRC: INTSRC5 Position

Definition at line 1978 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC6_Msk

#define GP_INTSRC_INTSRC6_Msk (0x1ul << GP_INTSRC_INTSRC6_Pos)

GPIO_T::INTSRC: INTSRC6 Mask

Definition at line 1982 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC6_Pos

#define GP_INTSRC_INTSRC6_Pos (6)

GPIO_T::INTSRC: INTSRC6 Position

Definition at line 1981 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC7_Msk

#define GP_INTSRC_INTSRC7_Msk (0x1ul << GP_INTSRC_INTSRC7_Pos)

GPIO_T::INTSRC: INTSRC7 Mask

Definition at line 1985 of file Mini55Series.h.

## ◆ GP_INTSRC_INTSRC7_Pos

#define GP_INTSRC_INTSRC7_Pos (7)

GPIO_T::INTSRC: INTSRC7 Position

Definition at line 1984 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE0_Msk

#define GP_INTTYPE_TYPE0_Msk (0x1ul << GP_INTTYPE_TYPE0_Pos)

GPIO_T::INTTYPE: TYPE0 Mask

Definition at line 1892 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE0_Pos

#define GP_INTTYPE_TYPE0_Pos (0)

GPIO_T::INTTYPE: TYPE0 Position

Definition at line 1891 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE1_Msk

#define GP_INTTYPE_TYPE1_Msk (0x1ul << GP_INTTYPE_TYPE1_Pos)

GPIO_T::INTTYPE: TYPE1 Mask

Definition at line 1895 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE1_Pos

#define GP_INTTYPE_TYPE1_Pos (1)

GPIO_T::INTTYPE: TYPE1 Position

Definition at line 1894 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE2_Msk

#define GP_INTTYPE_TYPE2_Msk (0x1ul << GP_INTTYPE_TYPE2_Pos)

GPIO_T::INTTYPE: TYPE2 Mask

Definition at line 1898 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE2_Pos

#define GP_INTTYPE_TYPE2_Pos (2)

GPIO_T::INTTYPE: TYPE2 Position

Definition at line 1897 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE3_Msk

#define GP_INTTYPE_TYPE3_Msk (0x1ul << GP_INTTYPE_TYPE3_Pos)

GPIO_T::INTTYPE: TYPE3 Mask

Definition at line 1901 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE3_Pos

#define GP_INTTYPE_TYPE3_Pos (3)

GPIO_T::INTTYPE: TYPE3 Position

Definition at line 1900 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE4_Msk

#define GP_INTTYPE_TYPE4_Msk (0x1ul << GP_INTTYPE_TYPE4_Pos)

GPIO_T::INTTYPE: TYPE4 Mask

Definition at line 1904 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE4_Pos

#define GP_INTTYPE_TYPE4_Pos (4)

GPIO_T::INTTYPE: TYPE4 Position

Definition at line 1903 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE5_Msk

#define GP_INTTYPE_TYPE5_Msk (0x1ul << GP_INTTYPE_TYPE5_Pos)

GPIO_T::INTTYPE: TYPE5 Mask

Definition at line 1907 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE5_Pos

#define GP_INTTYPE_TYPE5_Pos (5)

GPIO_T::INTTYPE: TYPE5 Position

Definition at line 1906 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE6_Msk

#define GP_INTTYPE_TYPE6_Msk (0x1ul << GP_INTTYPE_TYPE6_Pos)

GPIO_T::INTTYPE: TYPE6 Mask

Definition at line 1910 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE6_Pos

#define GP_INTTYPE_TYPE6_Pos (6)

GPIO_T::INTTYPE: TYPE6 Position

Definition at line 1909 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE7_Msk

#define GP_INTTYPE_TYPE7_Msk (0x1ul << GP_INTTYPE_TYPE7_Pos)

GPIO_T::INTTYPE: TYPE7 Mask

Definition at line 1913 of file Mini55Series.h.

## ◆ GP_INTTYPE_TYPE7_Pos

#define GP_INTTYPE_TYPE7_Pos (7)

GPIO_T::INTTYPE: TYPE7 Position

Definition at line 1912 of file Mini55Series.h.

## ◆ GP_MODE_MODE0_Msk

#define GP_MODE_MODE0_Msk (0x3ul << GP_MODE_MODE0_Pos)

GPIO_T::MODE: MODE0 Mask

Definition at line 1754 of file Mini55Series.h.

## ◆ GP_MODE_MODE0_Pos

#define GP_MODE_MODE0_Pos (0)

    @addtogroup GP_CONST GP Bit Field Definition
    Constant Definitions for GP Controller

GPIO_T::MODE: MODE0 Position

Definition at line 1753 of file Mini55Series.h.

## ◆ GP_MODE_MODE1_Msk

#define GP_MODE_MODE1_Msk (0x3ul << GP_MODE_MODE1_Pos)

GPIO_T::MODE: MODE1 Mask

Definition at line 1757 of file Mini55Series.h.

## ◆ GP_MODE_MODE1_Pos

#define GP_MODE_MODE1_Pos (2)

GPIO_T::MODE: MODE1 Position

Definition at line 1756 of file Mini55Series.h.

## ◆ GP_MODE_MODE2_Msk

#define GP_MODE_MODE2_Msk (0x3ul << GP_MODE_MODE2_Pos)

GPIO_T::MODE: MODE2 Mask

Definition at line 1760 of file Mini55Series.h.

## ◆ GP_MODE_MODE2_Pos

#define GP_MODE_MODE2_Pos (4)

GPIO_T::MODE: MODE2 Position

Definition at line 1759 of file Mini55Series.h.

## ◆ GP_MODE_MODE3_Msk

#define GP_MODE_MODE3_Msk (0x3ul << GP_MODE_MODE3_Pos)

GPIO_T::MODE: MODE3 Mask

Definition at line 1763 of file Mini55Series.h.

## ◆ GP_MODE_MODE3_Pos

#define GP_MODE_MODE3_Pos (6)

GPIO_T::MODE: MODE3 Position

Definition at line 1762 of file Mini55Series.h.

## ◆ GP_MODE_MODE4_Msk

#define GP_MODE_MODE4_Msk (0x3ul << GP_MODE_MODE4_Pos)

GPIO_T::MODE: MODE4 Mask

Definition at line 1766 of file Mini55Series.h.

## ◆ GP_MODE_MODE4_Pos

#define GP_MODE_MODE4_Pos (8)

GPIO_T::MODE: MODE4 Position

Definition at line 1765 of file Mini55Series.h.

## ◆ GP_MODE_MODE5_Msk

#define GP_MODE_MODE5_Msk (0x3ul << GP_MODE_MODE5_Pos)

GPIO_T::MODE: MODE5 Mask

Definition at line 1769 of file Mini55Series.h.

## ◆ GP_MODE_MODE5_Pos

#define GP_MODE_MODE5_Pos (10)

GPIO_T::MODE: MODE5 Position

Definition at line 1768 of file Mini55Series.h.

## ◆ GP_PIN_PIN0_Msk

#define GP_PIN_PIN0_Msk (0x1ul << GP_PIN_PIN0_Pos)

GPIO_T::PIN: PIN0 Mask

Definition at line 1844 of file Mini55Series.h.

## ◆ GP_PIN_PIN0_Pos

#define GP_PIN_PIN0_Pos (0)

GPIO_T::PIN: PIN0 Position

Definition at line 1843 of file Mini55Series.h.

## ◆ GP_PIN_PIN1_Msk

#define GP_PIN_PIN1_Msk (0x1ul << GP_PIN_PIN1_Pos)

GPIO_T::PIN: PIN1 Mask

Definition at line 1847 of file Mini55Series.h.

## ◆ GP_PIN_PIN1_Pos

#define GP_PIN_PIN1_Pos (1)

GPIO_T::PIN: PIN1 Position

Definition at line 1846 of file Mini55Series.h.

## ◆ GP_PIN_PIN2_Msk

#define GP_PIN_PIN2_Msk (0x1ul << GP_PIN_PIN2_Pos)

GPIO_T::PIN: PIN2 Mask

Definition at line 1850 of file Mini55Series.h.

## ◆ GP_PIN_PIN2_Pos

#define GP_PIN_PIN2_Pos (2)

GPIO_T::PIN: PIN2 Position

Definition at line 1849 of file Mini55Series.h.

## ◆ GP_PIN_PIN3_Msk

#define GP_PIN_PIN3_Msk (0x1ul << GP_PIN_PIN3_Pos)

GPIO_T::PIN: PIN3 Mask

Definition at line 1853 of file Mini55Series.h.

## ◆ GP_PIN_PIN3_Pos

#define GP_PIN_PIN3_Pos (3)

GPIO_T::PIN: PIN3 Position

Definition at line 1852 of file Mini55Series.h.

## ◆ GP_PIN_PIN4_Msk

#define GP_PIN_PIN4_Msk (0x1ul << GP_PIN_PIN4_Pos)

GPIO_T::PIN: PIN4 Mask

Definition at line 1856 of file Mini55Series.h.

## ◆ GP_PIN_PIN4_Pos

#define GP_PIN_PIN4_Pos (4)

GPIO_T::PIN: PIN4 Position

Definition at line 1855 of file Mini55Series.h.

## ◆ GP_PIN_PIN5_Msk

#define GP_PIN_PIN5_Msk (0x1ul << GP_PIN_PIN5_Pos)

GPIO_T::PIN: PIN5 Mask

Definition at line 1859 of file Mini55Series.h.

## ◆ GP_PIN_PIN5_Pos

#define GP_PIN_PIN5_Pos (5)

GPIO_T::PIN: PIN5 Position

Definition at line 1858 of file Mini55Series.h.

## ◆ GP_PIN_PIN6_Msk

#define GP_PIN_PIN6_Msk (0x1ul << GP_PIN_PIN6_Pos)

GPIO_T::PIN: PIN6 Mask

Definition at line 1862 of file Mini55Series.h.

## ◆ GP_PIN_PIN6_Pos

#define GP_PIN_PIN6_Pos (6)

GPIO_T::PIN: PIN6 Position

Definition at line 1861 of file Mini55Series.h.

## ◆ GP_PIN_PIN7_Msk

#define GP_PIN_PIN7_Msk (0x1ul << GP_PIN_PIN7_Pos)

GPIO_T::PIN: PIN7 Mask

Definition at line 1865 of file Mini55Series.h.

## ◆ GP_PIN_PIN7_Pos

#define GP_PIN_PIN7_Pos (7)

GPIO_T::PIN: PIN7 Position

Definition at line 1864 of file Mini55Series.h.

## ◆ HDIV_DIVIDEND_DIVIDEND_Msk

#define HDIV_DIVIDEND_DIVIDEND_Msk (0xfffffffful << HDIV_DIVIDEND_DIVIDEND_Pos)

HDIV_T::DIVIDEND: DIVIDEND Mask

Definition at line 2083 of file Mini55Series.h.

## ◆ HDIV_DIVIDEND_DIVIDEND_Pos

#define HDIV_DIVIDEND_DIVIDEND_Pos (0)

    @addtogroup HDIV_CONST HDIV Bit Field Definition
    Constant Definitions for HDIV Controller

HDIV_T::DIVIDEND: DIVIDEND Position

Definition at line 2082 of file Mini55Series.h.

## ◆ HDIV_DIVISOR_DIVISOR_Msk

#define HDIV_DIVISOR_DIVISOR_Msk (0xfffful << HDIV_DIVISOR_DIVISOR_Pos)

HDIV_T::DIVISOR: DIVISOR Mask

Definition at line 2086 of file Mini55Series.h.

## ◆ HDIV_DIVISOR_DIVISOR_Pos

#define HDIV_DIVISOR_DIVISOR_Pos (0)

HDIV_T::DIVISOR: DIVISOR Position

Definition at line 2085 of file Mini55Series.h.

## ◆ HDIV_QUOTIENT_QUOTIENT_Msk

#define HDIV_QUOTIENT_QUOTIENT_Msk (0xfffffffful << HDIV_QUOTIENT_QUOTIENT_Pos)

HDIV_T::QUOTIENT: QUOTIENT Mask

Definition at line 2089 of file Mini55Series.h.

## ◆ HDIV_QUOTIENT_QUOTIENT_Pos

#define HDIV_QUOTIENT_QUOTIENT_Pos (0)

HDIV_T::QUOTIENT: QUOTIENT Position

Definition at line 2088 of file Mini55Series.h.

## ◆ HDIV_REM_REM_Msk

#define HDIV_REM_REM_Msk (0xfffffffful << HDIV_REM_REM_Pos)

HDIV_T::REM: REM Mask

Definition at line 2092 of file Mini55Series.h.

## ◆ HDIV_REM_REM_Pos

#define HDIV_REM_REM_Pos (0)

HDIV_T::REM: REM Position

Definition at line 2091 of file Mini55Series.h.

## ◆ HDIV_STATUS_DIVBYZERO_Msk

#define HDIV_STATUS_DIVBYZERO_Msk (0x1ul << HDIV_STATUS_DIVBYZERO_Pos)

HDIV_T::STATUS: DIVBYZERO Mask

Definition at line 2095 of file Mini55Series.h.

## ◆ HDIV_STATUS_DIVBYZERO_Pos

#define HDIV_STATUS_DIVBYZERO_Pos (1)

HDIV_T::STATUS: DIVBYZERO Position

Definition at line 2094 of file Mini55Series.h.

## ◆ I2C_ADDR0_ADDR_Msk

#define I2C_ADDR0_ADDR_Msk (0x7ful << I2C_ADDR0_ADDR_Pos)

I2C_T::ADDR0: ADDR Mask

Definition at line 2420 of file Mini55Series.h.

## ◆ I2C_ADDR0_ADDR_Pos

#define I2C_ADDR0_ADDR_Pos (1)

I2C_T::ADDR0: ADDR Position

Definition at line 2419 of file Mini55Series.h.

## ◆ I2C_ADDR0_GC_Msk

#define I2C_ADDR0_GC_Msk (0x1ul << I2C_ADDR0_GC_Pos)

I2C_T::ADDR0: GC Mask

Definition at line 2417 of file Mini55Series.h.

## ◆ I2C_ADDR0_GC_Pos

#define I2C_ADDR0_GC_Pos (0)

I2C_T::ADDR0: GC Position

Definition at line 2416 of file Mini55Series.h.

## ◆ I2C_ADDR1_ADDR_Msk

#define I2C_ADDR1_ADDR_Msk (0x7ful << I2C_ADDR1_ADDR_Pos)

I2C_T::ADDR1: ADDR Mask

Definition at line 2444 of file Mini55Series.h.

## ◆ I2C_ADDR1_ADDR_Pos

#define I2C_ADDR1_ADDR_Pos (1)

I2C_T::ADDR1: ADDR Position

Definition at line 2443 of file Mini55Series.h.

## ◆ I2C_ADDR1_GC_Msk

#define I2C_ADDR1_GC_Msk (0x1ul << I2C_ADDR1_GC_Pos)

I2C_T::ADDR1: GC Mask

Definition at line 2441 of file Mini55Series.h.

## ◆ I2C_ADDR1_GC_Pos

#define I2C_ADDR1_GC_Pos (0)

I2C_T::ADDR1: GC Position

Definition at line 2440 of file Mini55Series.h.

## ◆ I2C_ADDR2_ADDR_Msk

#define I2C_ADDR2_ADDR_Msk (0x7ful << I2C_ADDR2_ADDR_Pos)

I2C_T::ADDR2: ADDR Mask

Definition at line 2450 of file Mini55Series.h.

## ◆ I2C_ADDR2_ADDR_Pos

#define I2C_ADDR2_ADDR_Pos (1)

I2C_T::ADDR2: ADDR Position

Definition at line 2449 of file Mini55Series.h.

## ◆ I2C_ADDR2_GC_Msk

#define I2C_ADDR2_GC_Msk (0x1ul << I2C_ADDR2_GC_Pos)

I2C_T::ADDR2: GC Mask

Definition at line 2447 of file Mini55Series.h.

## ◆ I2C_ADDR2_GC_Pos

#define I2C_ADDR2_GC_Pos (0)

I2C_T::ADDR2: GC Position

Definition at line 2446 of file Mini55Series.h.

## ◆ I2C_ADDR3_ADDR_Msk

#define I2C_ADDR3_ADDR_Msk (0x7ful << I2C_ADDR3_ADDR_Pos)

I2C_T::ADDR3: ADDR Mask

Definition at line 2456 of file Mini55Series.h.

## ◆ I2C_ADDR3_ADDR_Pos

#define I2C_ADDR3_ADDR_Pos (1)

I2C_T::ADDR3: ADDR Position

Definition at line 2455 of file Mini55Series.h.

## ◆ I2C_ADDR3_GC_Msk

#define I2C_ADDR3_GC_Msk (0x1ul << I2C_ADDR3_GC_Pos)

I2C_T::ADDR3: GC Mask

Definition at line 2453 of file Mini55Series.h.

## ◆ I2C_ADDR3_GC_Pos

#define I2C_ADDR3_GC_Pos (0)

I2C_T::ADDR3: GC Position

Definition at line 2452 of file Mini55Series.h.

## ◆ I2C_ADDRMSK0_ADDRMSK_Msk

#define I2C_ADDRMSK0_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK0_ADDRMSK_Pos)

I2C_T::ADDRMSK0: ADDRMSK Mask

Definition at line 2459 of file Mini55Series.h.

## ◆ I2C_ADDRMSK0_ADDRMSK_Pos

#define I2C_ADDRMSK0_ADDRMSK_Pos (1)

I2C_T::ADDRMSK0: ADDRMSK Position

Definition at line 2458 of file Mini55Series.h.

## ◆ I2C_ADDRMSK1_ADDRMSK_Msk

#define I2C_ADDRMSK1_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK1_ADDRMSK_Pos)

I2C_T::ADDRMSK1: ADDRMSK Mask

Definition at line 2462 of file Mini55Series.h.

## ◆ I2C_ADDRMSK1_ADDRMSK_Pos

#define I2C_ADDRMSK1_ADDRMSK_Pos (1)

I2C_T::ADDRMSK1: ADDRMSK Position

Definition at line 2461 of file Mini55Series.h.

## ◆ I2C_ADDRMSK2_ADDRMSK_Msk

#define I2C_ADDRMSK2_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK2_ADDRMSK_Pos)

I2C_T::ADDRMSK2: ADDRMSK Mask

Definition at line 2465 of file Mini55Series.h.

## ◆ I2C_ADDRMSK2_ADDRMSK_Pos

#define I2C_ADDRMSK2_ADDRMSK_Pos (1)

I2C_T::ADDRMSK2: ADDRMSK Position

Definition at line 2464 of file Mini55Series.h.

## ◆ I2C_ADDRMSK3_ADDRMSK_Msk

#define I2C_ADDRMSK3_ADDRMSK_Msk (0x7ful << I2C_ADDRMSK3_ADDRMSK_Pos)

I2C_T::ADDRMSK3: ADDRMSK Mask

Definition at line 2468 of file Mini55Series.h.

## ◆ I2C_ADDRMSK3_ADDRMSK_Pos

#define I2C_ADDRMSK3_ADDRMSK_Pos (1)

I2C_T::ADDRMSK3: ADDRMSK Position

Definition at line 2467 of file Mini55Series.h.

## ◆ I2C_CLKDIV_DIVIDER_Msk

#define I2C_CLKDIV_DIVIDER_Msk (0xfful << I2C_CLKDIV_DIVIDER_Pos)

I2C_T::CLKDIV: DIVIDER Mask

Definition at line 2429 of file Mini55Series.h.

## ◆ I2C_CLKDIV_DIVIDER_Pos

#define I2C_CLKDIV_DIVIDER_Pos (0)

I2C_T::CLKDIV: DIVIDER Position

Definition at line 2428 of file Mini55Series.h.

## ◆ I2C_CTL1_FIFOEN_Msk

#define I2C_CTL1_FIFOEN_Msk (0x1ul << I2C_CTL1_FIFOEN_Pos)

I2C_T::CTL1: FIFOEN Mask

Definition at line 2474 of file Mini55Series.h.

## ◆ I2C_CTL1_FIFOEN_Pos

#define I2C_CTL1_FIFOEN_Pos (1)

I2C_T::CTL1: FIFOEN Position

Definition at line 2473 of file Mini55Series.h.

## ◆ I2C_CTL1_NSTRETCH_Msk

#define I2C_CTL1_NSTRETCH_Msk (0x1ul << I2C_CTL1_NSTRETCH_Pos)

I2C_T::CTL1: NSTRETCH Mask

Definition at line 2477 of file Mini55Series.h.

## ◆ I2C_CTL1_NSTRETCH_Pos

#define I2C_CTL1_NSTRETCH_Pos (2)

I2C_T::CTL1: NSTRETCH Position

Definition at line 2476 of file Mini55Series.h.

## ◆ I2C_CTL1_OVIEN_Msk

#define I2C_CTL1_OVIEN_Msk (0x1ul << I2C_CTL1_OVIEN_Pos)

I2C_T::CTL1: OVIEN Mask

Definition at line 2480 of file Mini55Series.h.

## ◆ I2C_CTL1_OVIEN_Pos

#define I2C_CTL1_OVIEN_Pos (3)

I2C_T::CTL1: OVIEN Position

Definition at line 2479 of file Mini55Series.h.

## ◆ I2C_CTL1_URIEN_Msk

#define I2C_CTL1_URIEN_Msk (0x1ul << I2C_CTL1_URIEN_Pos)

I2C_T::CTL1: URIEN Mask

Definition at line 2483 of file Mini55Series.h.

## ◆ I2C_CTL1_URIEN_Pos

#define I2C_CTL1_URIEN_Pos (4)

I2C_T::CTL1: URIEN Position

Definition at line 2482 of file Mini55Series.h.

## ◆ I2C_CTL1_WKEN_Msk

#define I2C_CTL1_WKEN_Msk (0x1ul << I2C_CTL1_WKEN_Pos)

I2C_T::CTL1: WKEN Mask

Definition at line 2471 of file Mini55Series.h.

## ◆ I2C_CTL1_WKEN_Pos

#define I2C_CTL1_WKEN_Pos (0)

I2C_T::CTL1: WKEN Position

Definition at line 2470 of file Mini55Series.h.

## ◆ I2C_CTL_AA_Msk

#define I2C_CTL_AA_Msk (0x1ul << I2C_CTL_AA_Pos)

I2C_T::CTL: AA Mask

Definition at line 2399 of file Mini55Series.h.

## ◆ I2C_CTL_AA_Pos

#define I2C_CTL_AA_Pos (2)

    @addtogroup I2C_CONST I2C Bit Field Definition
    Constant Definitions for I2C Controller

I2C_T::CTL: AA Position

Definition at line 2398 of file Mini55Series.h.

## ◆ I2C_CTL_I2CEN_Msk

#define I2C_CTL_I2CEN_Msk (0x1ul << I2C_CTL_I2CEN_Pos)

I2C_T::CTL: I2CEN Mask

Definition at line 2411 of file Mini55Series.h.

## ◆ I2C_CTL_I2CEN_Pos

#define I2C_CTL_I2CEN_Pos (6)

I2C_T::CTL: I2CEN Position

Definition at line 2410 of file Mini55Series.h.

## ◆ I2C_CTL_INTEN_Msk

#define I2C_CTL_INTEN_Msk (0x1ul << I2C_CTL_INTEN_Pos)

I2C_T::CTL: INTEN Mask

Definition at line 2414 of file Mini55Series.h.

## ◆ I2C_CTL_INTEN_Pos

#define I2C_CTL_INTEN_Pos (7)

I2C_T::CTL: INTEN Position

Definition at line 2413 of file Mini55Series.h.

## ◆ I2C_CTL_SI_Msk

#define I2C_CTL_SI_Msk (0x1ul << I2C_CTL_SI_Pos)

I2C_T::CTL: SI Mask

Definition at line 2402 of file Mini55Series.h.

## ◆ I2C_CTL_SI_Pos

#define I2C_CTL_SI_Pos (3)

I2C_T::CTL: SI Position

Definition at line 2401 of file Mini55Series.h.

## ◆ I2C_CTL_STA_Msk

#define I2C_CTL_STA_Msk (0x1ul << I2C_CTL_STA_Pos)

I2C_T::CTL: STA Mask

Definition at line 2408 of file Mini55Series.h.

## ◆ I2C_CTL_STA_Pos

#define I2C_CTL_STA_Pos (5)

I2C_T::CTL: STA Position

Definition at line 2407 of file Mini55Series.h.

## ◆ I2C_CTL_STO_Msk

#define I2C_CTL_STO_Msk (0x1ul << I2C_CTL_STO_Pos)

I2C_T::CTL: STO Mask

Definition at line 2405 of file Mini55Series.h.

## ◆ I2C_CTL_STO_Pos

#define I2C_CTL_STO_Pos (4)

I2C_T::CTL: STO Position

Definition at line 2404 of file Mini55Series.h.

## ◆ I2C_DAT_DAT_Msk

#define I2C_DAT_DAT_Msk (0xfful << I2C_DAT_DAT_Pos)

I2C_T::DAT: DAT Mask

Definition at line 2423 of file Mini55Series.h.

## ◆ I2C_DAT_DAT_Pos

#define I2C_DAT_DAT_Pos (0)

I2C_T::DAT: DAT Position

Definition at line 2422 of file Mini55Series.h.

## ◆ I2C_STATUS1_EMPTY_Msk

#define I2C_STATUS1_EMPTY_Msk (0x1ul << I2C_STATUS1_EMPTY_Pos)

I2C_T::STATUS1: EMPTY Mask

Definition at line 2492 of file Mini55Series.h.

## ◆ I2C_STATUS1_EMPTY_Pos

#define I2C_STATUS1_EMPTY_Pos (2)

I2C_T::STATUS1: EMPTY Position

Definition at line 2491 of file Mini55Series.h.

## ◆ I2C_STATUS1_FULL_Msk

#define I2C_STATUS1_FULL_Msk (0x1ul << I2C_STATUS1_FULL_Pos)

I2C_T::STATUS1: FULL Mask

Definition at line 2489 of file Mini55Series.h.

## ◆ I2C_STATUS1_FULL_Pos

#define I2C_STATUS1_FULL_Pos (1)

I2C_T::STATUS1: FULL Position

Definition at line 2488 of file Mini55Series.h.

## ◆ I2C_STATUS1_OVIF_Msk

#define I2C_STATUS1_OVIF_Msk (0x1ul << I2C_STATUS1_OVIF_Pos)

I2C_T::STATUS1: OVIF Mask

Definition at line 2495 of file Mini55Series.h.

## ◆ I2C_STATUS1_OVIF_Pos

#define I2C_STATUS1_OVIF_Pos (3)

I2C_T::STATUS1: OVIF Position

Definition at line 2494 of file Mini55Series.h.

## ◆ I2C_STATUS1_URIF_Msk

#define I2C_STATUS1_URIF_Msk (0x1ul << I2C_STATUS1_URIF_Pos)

I2C_T::STATUS1: URIF Mask

Definition at line 2498 of file Mini55Series.h.

## ◆ I2C_STATUS1_URIF_Pos

#define I2C_STATUS1_URIF_Pos (4)

I2C_T::STATUS1: URIF Position

Definition at line 2497 of file Mini55Series.h.

## ◆ I2C_STATUS1_WKIF_Msk

#define I2C_STATUS1_WKIF_Msk (0x1ul << I2C_STATUS1_WKIF_Pos)

I2C_T::STATUS1: WKIF Mask

Definition at line 2486 of file Mini55Series.h.

## ◆ I2C_STATUS1_WKIF_Pos

#define I2C_STATUS1_WKIF_Pos (0)

I2C_T::STATUS1: WKIF Position

Definition at line 2485 of file Mini55Series.h.

## ◆ I2C_STATUS_STATUS_Msk

#define I2C_STATUS_STATUS_Msk (0xfful << I2C_STATUS_STATUS_Pos)

I2C_T::STATUS: STATUS Mask

Definition at line 2426 of file Mini55Series.h.

## ◆ I2C_STATUS_STATUS_Pos

#define I2C_STATUS_STATUS_Pos (0)

I2C_T::STATUS: STATUS Position

Definition at line 2425 of file Mini55Series.h.

## ◆ I2C_TOCTL_TOCDIV4_Msk

#define I2C_TOCTL_TOCDIV4_Msk (0x1ul << I2C_TOCTL_TOCDIV4_Pos)

I2C_T::TOCTL: TOCDIV4 Mask

Definition at line 2435 of file Mini55Series.h.

## ◆ I2C_TOCTL_TOCDIV4_Pos

#define I2C_TOCTL_TOCDIV4_Pos (1)

I2C_T::TOCTL: TOCDIV4 Position

Definition at line 2434 of file Mini55Series.h.

## ◆ I2C_TOCTL_TOCEN_Msk

#define I2C_TOCTL_TOCEN_Msk (0x1ul << I2C_TOCTL_TOCEN_Pos)

I2C_T::TOCTL: TOCEN Mask

Definition at line 2438 of file Mini55Series.h.

## ◆ I2C_TOCTL_TOCEN_Pos

#define I2C_TOCTL_TOCEN_Pos (2)

I2C_T::TOCTL: TOCEN Position

Definition at line 2437 of file Mini55Series.h.

## ◆ I2C_TOCTL_TOIF_Msk

#define I2C_TOCTL_TOIF_Msk (0x1ul << I2C_TOCTL_TOIF_Pos)

I2C_T::TOCTL: TOIF Mask

Definition at line 2432 of file Mini55Series.h.

## ◆ I2C_TOCTL_TOIF_Pos

#define I2C_TOCTL_TOIF_Pos (0)

I2C_T::TOCTL: TOIF Position

Definition at line 2431 of file Mini55Series.h.

## ◆ INT_IRQ0SRC_INT_SRC_Msk

#define INT_IRQ0SRC_INT_SRC_Msk (0x7ul << INT_IRQ0SRC_INT_SRC_Pos)

INTR_T::IRQ0SRC: INT_SRC Mask

Definition at line 2802 of file Mini55Series.h.

## ◆ INT_IRQ0SRC_INT_SRC_Pos

#define INT_IRQ0SRC_INT_SRC_Pos (0)

    @addtogroup INT_CONST INT Bit Field Definition
    Constant Definitions for INT Controller

INTR_T::IRQ0SRC: INT_SRC Position

Definition at line 2801 of file Mini55Series.h.

## ◆ INT_IRQ12SRC_INT_SRC_Msk

#define INT_IRQ12SRC_INT_SRC_Msk (0x7ul << INT_IRQ12SRC_INT_SRC_Pos)

INTR_T::IRQ12SRC: INT_SRC Mask

Definition at line 2832 of file Mini55Series.h.

## ◆ INT_IRQ12SRC_INT_SRC_Pos

#define INT_IRQ12SRC_INT_SRC_Pos (0)

INTR_T::IRQ12SRC: INT_SRC Position

Definition at line 2831 of file Mini55Series.h.

## ◆ INT_IRQ13SRC_INT_SRC_Msk

#define INT_IRQ13SRC_INT_SRC_Msk (0x7ul << INT_IRQ13SRC_INT_SRC_Pos)

INTR_T::IRQ13SRC: INT_SRC Mask

Definition at line 2835 of file Mini55Series.h.

## ◆ INT_IRQ13SRC_INT_SRC_Pos

#define INT_IRQ13SRC_INT_SRC_Pos (0)

INTR_T::IRQ13SRC: INT_SRC Position

Definition at line 2834 of file Mini55Series.h.

## ◆ INT_IRQ14SRC_INT_SRC_Msk

#define INT_IRQ14SRC_INT_SRC_Msk (0x7ul << INT_IRQ14SRC_INT_SRC_Pos)

INTR_T::IRQ14SRC: INT_SRC Mask

Definition at line 2838 of file Mini55Series.h.

## ◆ INT_IRQ14SRC_INT_SRC_Pos

#define INT_IRQ14SRC_INT_SRC_Pos (0)

INTR_T::IRQ14SRC: INT_SRC Position

Definition at line 2837 of file Mini55Series.h.

## ◆ INT_IRQ16SRC_INT_SRC_Msk

#define INT_IRQ16SRC_INT_SRC_Msk (0x7ul << INT_IRQ16SRC_INT_SRC_Pos)

INTR_T::IRQ16SRC: INT_SRC Mask

Definition at line 2841 of file Mini55Series.h.

## ◆ INT_IRQ16SRC_INT_SRC_Pos

#define INT_IRQ16SRC_INT_SRC_Pos (0)

INTR_T::IRQ16SRC: INT_SRC Position

Definition at line 2840 of file Mini55Series.h.

## ◆ INT_IRQ17SRC_INT_SRC_Msk

#define INT_IRQ17SRC_INT_SRC_Msk (0x7ul << INT_IRQ17SRC_INT_SRC_Pos)

INTR_T::IRQ17SRC: INT_SRC Mask

Definition at line 2844 of file Mini55Series.h.

## ◆ INT_IRQ17SRC_INT_SRC_Pos

#define INT_IRQ17SRC_INT_SRC_Pos (0)

INTR_T::IRQ17SRC: INT_SRC Position

Definition at line 2843 of file Mini55Series.h.

## ◆ INT_IRQ18SRC_INT_SRC_Msk

#define INT_IRQ18SRC_INT_SRC_Msk (0x7ul << INT_IRQ18SRC_INT_SRC_Pos)

INTR_T::IRQ18SRC: INT_SRC Mask

Definition at line 2847 of file Mini55Series.h.

## ◆ INT_IRQ18SRC_INT_SRC_Pos

#define INT_IRQ18SRC_INT_SRC_Pos (0)

INTR_T::IRQ18SRC: INT_SRC Position

Definition at line 2846 of file Mini55Series.h.

## ◆ INT_IRQ1SRC_INT_SRC_Msk

#define INT_IRQ1SRC_INT_SRC_Msk (0x7ul << INT_IRQ1SRC_INT_SRC_Pos)

INTR_T::IRQ1SRC: INT_SRC Mask

Definition at line 2805 of file Mini55Series.h.

## ◆ INT_IRQ1SRC_INT_SRC_Pos

#define INT_IRQ1SRC_INT_SRC_Pos (0)

INTR_T::IRQ1SRC: INT_SRC Position

Definition at line 2804 of file Mini55Series.h.

## ◆ INT_IRQ25SRC_INT_SRC_Msk

#define INT_IRQ25SRC_INT_SRC_Msk (0x7ul << INT_IRQ25SRC_INT_SRC_Pos)

INTR_T::IRQ25SRC: INT_SRC Mask

Definition at line 2850 of file Mini55Series.h.

## ◆ INT_IRQ25SRC_INT_SRC_Pos

#define INT_IRQ25SRC_INT_SRC_Pos (0)

INTR_T::IRQ25SRC: INT_SRC Position

Definition at line 2849 of file Mini55Series.h.

## ◆ INT_IRQ28SRC_INT_SRC_Msk

#define INT_IRQ28SRC_INT_SRC_Msk (0x7ul << INT_IRQ28SRC_INT_SRC_Pos)

INTR_T::IRQ28SRC: INT_SRC Mask

Definition at line 2853 of file Mini55Series.h.

## ◆ INT_IRQ28SRC_INT_SRC_Pos

#define INT_IRQ28SRC_INT_SRC_Pos (0)

INTR_T::IRQ28SRC: INT_SRC Position

Definition at line 2852 of file Mini55Series.h.

## ◆ INT_IRQ29SRC_INT_SRC_Msk

#define INT_IRQ29SRC_INT_SRC_Msk (0x7ul << INT_IRQ29SRC_INT_SRC_Pos)

INTR_T::IRQ29SRC: INT_SRC Mask

Definition at line 2856 of file Mini55Series.h.

## ◆ INT_IRQ29SRC_INT_SRC_Pos

#define INT_IRQ29SRC_INT_SRC_Pos (0)

INTR_T::IRQ29SRC: INT_SRC Position

Definition at line 2855 of file Mini55Series.h.

## ◆ INT_IRQ2SRC_INT_SRC_Msk

#define INT_IRQ2SRC_INT_SRC_Msk (0x7ul << INT_IRQ2SRC_INT_SRC_Pos)

INTR_T::IRQ2SRC: INT_SRC Mask

Definition at line 2808 of file Mini55Series.h.

## ◆ INT_IRQ2SRC_INT_SRC_Pos

#define INT_IRQ2SRC_INT_SRC_Pos (0)

INTR_T::IRQ2SRC: INT_SRC Position

Definition at line 2807 of file Mini55Series.h.

## ◆ INT_IRQ3SRC_INT_SRC_Msk

#define INT_IRQ3SRC_INT_SRC_Msk (0x7ul << INT_IRQ3SRC_INT_SRC_Pos)

INTR_T::IRQ3SRC: INT_SRC Mask

Definition at line 2811 of file Mini55Series.h.

## ◆ INT_IRQ3SRC_INT_SRC_Pos

#define INT_IRQ3SRC_INT_SRC_Pos (0)

INTR_T::IRQ3SRC: INT_SRC Position

Definition at line 2810 of file Mini55Series.h.

## ◆ INT_IRQ4SRC_INT_SRC_Msk

#define INT_IRQ4SRC_INT_SRC_Msk (0x7ul << INT_IRQ4SRC_INT_SRC_Pos)

INTR_T::IRQ4SRC: INT_SRC Mask

Definition at line 2814 of file Mini55Series.h.

## ◆ INT_IRQ4SRC_INT_SRC_Pos

#define INT_IRQ4SRC_INT_SRC_Pos (0)

INTR_T::IRQ4SRC: INT_SRC Position

Definition at line 2813 of file Mini55Series.h.

## ◆ INT_IRQ5SRC_INT_SRC_Msk

#define INT_IRQ5SRC_INT_SRC_Msk (0x7ul << INT_IRQ5SRC_INT_SRC_Pos)

INTR_T::IRQ5SRC: INT_SRC Mask

Definition at line 2817 of file Mini55Series.h.

## ◆ INT_IRQ5SRC_INT_SRC_Pos

#define INT_IRQ5SRC_INT_SRC_Pos (0)

INTR_T::IRQ5SRC: INT_SRC Position

Definition at line 2816 of file Mini55Series.h.

## ◆ INT_IRQ6SRC_INT_SRC_Msk

#define INT_IRQ6SRC_INT_SRC_Msk (0x7ul << INT_IRQ6SRC_INT_SRC_Pos)

INTR_T::IRQ6SRC: INT_SRC Mask

Definition at line 2820 of file Mini55Series.h.

## ◆ INT_IRQ6SRC_INT_SRC_Pos

#define INT_IRQ6SRC_INT_SRC_Pos (0)

INTR_T::IRQ6SRC: INT_SRC Position

Definition at line 2819 of file Mini55Series.h.

## ◆ INT_IRQ7SRC_INT_SRC_Msk

#define INT_IRQ7SRC_INT_SRC_Msk (0x7ul << INT_IRQ7SRC_INT_SRC_Pos)

INTR_T::IRQ7SRC: INT_SRC Mask

Definition at line 2823 of file Mini55Series.h.

## ◆ INT_IRQ7SRC_INT_SRC_Pos

#define INT_IRQ7SRC_INT_SRC_Pos (0)

INTR_T::IRQ7SRC: INT_SRC Position

Definition at line 2822 of file Mini55Series.h.

## ◆ INT_IRQ8SRC_INT_SRC_Msk

#define INT_IRQ8SRC_INT_SRC_Msk (0x7ul << INT_IRQ8SRC_INT_SRC_Pos)

INTR_T::IRQ8SRC: INT_SRC Mask

Definition at line 2826 of file Mini55Series.h.

## ◆ INT_IRQ8SRC_INT_SRC_Pos

#define INT_IRQ8SRC_INT_SRC_Pos (0)

INTR_T::IRQ8SRC: INT_SRC Position

Definition at line 2825 of file Mini55Series.h.

## ◆ INT_IRQ9SRC_INT_SRC_Msk

#define INT_IRQ9SRC_INT_SRC_Msk (0x7ul << INT_IRQ9SRC_INT_SRC_Pos)

INTR_T::IRQ9SRC: INT_SRC Mask

Definition at line 2829 of file Mini55Series.h.

## ◆ INT_IRQ9SRC_INT_SRC_Pos

#define INT_IRQ9SRC_INT_SRC_Pos (0)

INTR_T::IRQ9SRC: INT_SRC Position

Definition at line 2828 of file Mini55Series.h.

## ◆ INT_IRQSTS_IRQ_Msk

#define INT_IRQSTS_IRQ_Msk (0xfffffffful << INT_IRQSTS_IRQ_Pos)

INTR_T::IRQSTS: IRQ Mask

Definition at line 2865 of file Mini55Series.h.

## ◆ INT_IRQSTS_IRQ_Pos

#define INT_IRQSTS_IRQ_Pos (0)

INTR_T::IRQSTS: IRQ Position

Definition at line 2864 of file Mini55Series.h.

## ◆ INT_NMICTL_NMISELEN_Msk

#define INT_NMICTL_NMISELEN_Msk (0x1ul << INT_NMICTL_NMISELEN_Pos)

INTR_T::NMICTL: NMISELEN Mask

Definition at line 2862 of file Mini55Series.h.

## ◆ INT_NMICTL_NMISELEN_Pos

#define INT_NMICTL_NMISELEN_Pos (8)

INTR_T::NMICTL: NMISELEN Position

Definition at line 2861 of file Mini55Series.h.

## ◆ INT_NMICTL_NMTSEL_Msk

#define INT_NMICTL_NMTSEL_Msk (0x1ful << INT_NMICTL_NMTSEL_Pos)

INTR_T::NMICTL: NMTSEL Mask

Definition at line 2859 of file Mini55Series.h.

## ◆ INT_NMICTL_NMTSEL_Pos

#define INT_NMICTL_NMTSEL_Pos (0)

INTR_T::NMICTL: NMTSEL Position

Definition at line 2858 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN0_Msk

#define PWM_ADCTCTL0_CDTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN0_Pos)

PWM_T::ADCTCTL0: CDTRGEN0 Mask

Definition at line 4224 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN0_Pos

#define PWM_ADCTCTL0_CDTRGEN0_Pos (2)

PWM_T::ADCTCTL0: CDTRGEN0 Position

Definition at line 4223 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN1_Msk

#define PWM_ADCTCTL0_CDTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN1_Pos)

PWM_T::ADCTCTL0: CDTRGEN1 Mask

Definition at line 4236 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN1_Pos

#define PWM_ADCTCTL0_CDTRGEN1_Pos (10)

PWM_T::ADCTCTL0: CDTRGEN1 Position

Definition at line 4235 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN2_Msk

#define PWM_ADCTCTL0_CDTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN2_Pos)

PWM_T::ADCTCTL0: CDTRGEN2 Mask

Definition at line 4248 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN2_Pos

#define PWM_ADCTCTL0_CDTRGEN2_Pos (18)

PWM_T::ADCTCTL0: CDTRGEN2 Position

Definition at line 4247 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN3_Msk

#define PWM_ADCTCTL0_CDTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CDTRGEN3_Pos)

PWM_T::ADCTCTL0: CDTRGEN3 Mask

Definition at line 4260 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CDTRGEN3_Pos

#define PWM_ADCTCTL0_CDTRGEN3_Pos (26)

PWM_T::ADCTCTL0: CDTRGEN3 Position

Definition at line 4259 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN0_Msk

#define PWM_ADCTCTL0_CPTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN0_Pos)

PWM_T::ADCTCTL0: CPTRGEN0 Mask

Definition at line 4221 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN0_Pos

#define PWM_ADCTCTL0_CPTRGEN0_Pos (1)

PWM_T::ADCTCTL0: CPTRGEN0 Position

Definition at line 4220 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN1_Msk

#define PWM_ADCTCTL0_CPTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN1_Pos)

PWM_T::ADCTCTL0: CPTRGEN1 Mask

Definition at line 4233 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN1_Pos

#define PWM_ADCTCTL0_CPTRGEN1_Pos (9)

PWM_T::ADCTCTL0: CPTRGEN1 Position

Definition at line 4232 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN2_Msk

#define PWM_ADCTCTL0_CPTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN2_Pos)

PWM_T::ADCTCTL0: CPTRGEN2 Mask

Definition at line 4245 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN2_Pos

#define PWM_ADCTCTL0_CPTRGEN2_Pos (17)

PWM_T::ADCTCTL0: CPTRGEN2 Position

Definition at line 4244 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN3_Msk

#define PWM_ADCTCTL0_CPTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CPTRGEN3_Pos)

PWM_T::ADCTCTL0: CPTRGEN3 Mask

Definition at line 4257 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CPTRGEN3_Pos

#define PWM_ADCTCTL0_CPTRGEN3_Pos (25)

PWM_T::ADCTCTL0: CPTRGEN3 Position

Definition at line 4256 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN0_Msk

#define PWM_ADCTCTL0_CUTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN0_Pos)

PWM_T::ADCTCTL0: CUTRGEN0 Mask

Definition at line 4218 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN0_Pos

#define PWM_ADCTCTL0_CUTRGEN0_Pos (0)

PWM_T::ADCTCTL0: CUTRGEN0 Position

Definition at line 4217 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN1_Msk

#define PWM_ADCTCTL0_CUTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN1_Pos)

PWM_T::ADCTCTL0: CUTRGEN1 Mask

Definition at line 4230 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN1_Pos

#define PWM_ADCTCTL0_CUTRGEN1_Pos (8)

PWM_T::ADCTCTL0: CUTRGEN1 Position

Definition at line 4229 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN2_Msk

#define PWM_ADCTCTL0_CUTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN2_Pos)

PWM_T::ADCTCTL0: CUTRGEN2 Mask

Definition at line 4242 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN2_Pos

#define PWM_ADCTCTL0_CUTRGEN2_Pos (16)

PWM_T::ADCTCTL0: CUTRGEN2 Position

Definition at line 4241 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN3_Msk

#define PWM_ADCTCTL0_CUTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_CUTRGEN3_Pos)

PWM_T::ADCTCTL0: CUTRGEN3 Mask

Definition at line 4254 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_CUTRGEN3_Pos

#define PWM_ADCTCTL0_CUTRGEN3_Pos (24)

PWM_T::ADCTCTL0: CUTRGEN3 Position

Definition at line 4253 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN0_Msk

#define PWM_ADCTCTL0_ZPTRGEN0_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN0_Pos)

PWM_T::ADCTCTL0: ZPTRGEN0 Mask

Definition at line 4227 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN0_Pos

#define PWM_ADCTCTL0_ZPTRGEN0_Pos (3)

PWM_T::ADCTCTL0: ZPTRGEN0 Position

Definition at line 4226 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN1_Msk

#define PWM_ADCTCTL0_ZPTRGEN1_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN1_Pos)

PWM_T::ADCTCTL0: ZPTRGEN1 Mask

Definition at line 4239 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN1_Pos

#define PWM_ADCTCTL0_ZPTRGEN1_Pos (11)

PWM_T::ADCTCTL0: ZPTRGEN1 Position

Definition at line 4238 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN2_Msk

#define PWM_ADCTCTL0_ZPTRGEN2_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN2_Pos)

PWM_T::ADCTCTL0: ZPTRGEN2 Mask

Definition at line 4251 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN2_Pos

#define PWM_ADCTCTL0_ZPTRGEN2_Pos (19)

PWM_T::ADCTCTL0: ZPTRGEN2 Position

Definition at line 4250 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN3_Msk

#define PWM_ADCTCTL0_ZPTRGEN3_Msk (0x1ul << PWM_ADCTCTL0_ZPTRGEN3_Pos)

PWM_T::ADCTCTL0: ZPTRGEN3 Mask

Definition at line 4263 of file Mini55Series.h.

## ◆ PWM_ADCTCTL0_ZPTRGEN3_Pos

#define PWM_ADCTCTL0_ZPTRGEN3_Pos (27)

PWM_T::ADCTCTL0: ZPTRGEN3 Position

Definition at line 4262 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CDTRGEN4_Msk

#define PWM_ADCTCTL1_CDTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CDTRGEN4_Pos)

PWM_T::ADCTCTL1: CDTRGEN4 Mask

Definition at line 4272 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CDTRGEN4_Pos

#define PWM_ADCTCTL1_CDTRGEN4_Pos (2)

PWM_T::ADCTCTL1: CDTRGEN4 Position

Definition at line 4271 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CDTRGEN5_Msk

#define PWM_ADCTCTL1_CDTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CDTRGEN5_Pos)

PWM_T::ADCTCTL1: CDTRGEN5 Mask

Definition at line 4284 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CDTRGEN5_Pos

#define PWM_ADCTCTL1_CDTRGEN5_Pos (10)

PWM_T::ADCTCTL1: CDTRGEN5 Position

Definition at line 4283 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CPTRGEN4_Msk

#define PWM_ADCTCTL1_CPTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CPTRGEN4_Pos)

PWM_T::ADCTCTL1: CPTRGEN4 Mask

Definition at line 4269 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CPTRGEN4_Pos

#define PWM_ADCTCTL1_CPTRGEN4_Pos (1)

PWM_T::ADCTCTL1: CPTRGEN4 Position

Definition at line 4268 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CPTRGEN5_Msk

#define PWM_ADCTCTL1_CPTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CPTRGEN5_Pos)

PWM_T::ADCTCTL1: CPTRGEN5 Mask

Definition at line 4281 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CPTRGEN5_Pos

#define PWM_ADCTCTL1_CPTRGEN5_Pos (9)

PWM_T::ADCTCTL1: CPTRGEN5 Position

Definition at line 4280 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CUTRGEN4_Msk

#define PWM_ADCTCTL1_CUTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_CUTRGEN4_Pos)

PWM_T::ADCTCTL1: CUTRGEN4 Mask

Definition at line 4266 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CUTRGEN4_Pos

#define PWM_ADCTCTL1_CUTRGEN4_Pos (0)

PWM_T::ADCTCTL1: CUTRGEN4 Position

Definition at line 4265 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CUTRGEN5_Msk

#define PWM_ADCTCTL1_CUTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_CUTRGEN5_Pos)

PWM_T::ADCTCTL1: CUTRGEN5 Mask

Definition at line 4278 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_CUTRGEN5_Pos

#define PWM_ADCTCTL1_CUTRGEN5_Pos (8)

PWM_T::ADCTCTL1: CUTRGEN5 Position

Definition at line 4277 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_ZPTRGEN4_Msk

#define PWM_ADCTCTL1_ZPTRGEN4_Msk (0x1ul << PWM_ADCTCTL1_ZPTRGEN4_Pos)

PWM_T::ADCTCTL1: ZPTRGEN4 Mask

Definition at line 4275 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_ZPTRGEN4_Pos

#define PWM_ADCTCTL1_ZPTRGEN4_Pos (3)

PWM_T::ADCTCTL1: ZPTRGEN4 Position

Definition at line 4274 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_ZPTRGEN5_Msk

#define PWM_ADCTCTL1_ZPTRGEN5_Msk (0x1ul << PWM_ADCTCTL1_ZPTRGEN5_Pos)

PWM_T::ADCTCTL1: ZPTRGEN5 Mask

Definition at line 4287 of file Mini55Series.h.

## ◆ PWM_ADCTCTL1_ZPTRGEN5_Pos

#define PWM_ADCTCTL1_ZPTRGEN5_Pos (11)

PWM_T::ADCTCTL1: ZPTRGEN5 Position

Definition at line 4286 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF0_Msk

#define PWM_ADCTSTS0_CDTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF0_Pos)

PWM_T::ADCTSTS0: CDTRGF0 Mask

Definition at line 4296 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF0_Pos

#define PWM_ADCTSTS0_CDTRGF0_Pos (2)

PWM_T::ADCTSTS0: CDTRGF0 Position

Definition at line 4295 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF1_Msk

#define PWM_ADCTSTS0_CDTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF1_Pos)

PWM_T::ADCTSTS0: CDTRGF1 Mask

Definition at line 4308 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF1_Pos

#define PWM_ADCTSTS0_CDTRGF1_Pos (10)

PWM_T::ADCTSTS0: CDTRGF1 Position

Definition at line 4307 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF2_Msk

#define PWM_ADCTSTS0_CDTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF2_Pos)

PWM_T::ADCTSTS0: CDTRGF2 Mask

Definition at line 4320 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF2_Pos

#define PWM_ADCTSTS0_CDTRGF2_Pos (18)

PWM_T::ADCTSTS0: CDTRGF2 Position

Definition at line 4319 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF3_Msk

#define PWM_ADCTSTS0_CDTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CDTRGF3_Pos)

PWM_T::ADCTSTS0: CDTRGF3 Mask

Definition at line 4332 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CDTRGF3_Pos

#define PWM_ADCTSTS0_CDTRGF3_Pos (26)

PWM_T::ADCTSTS0: CDTRGF3 Position

Definition at line 4331 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF0_Msk

#define PWM_ADCTSTS0_CPTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF0_Pos)

PWM_T::ADCTSTS0: CPTRGF0 Mask

Definition at line 4293 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF0_Pos

#define PWM_ADCTSTS0_CPTRGF0_Pos (1)

PWM_T::ADCTSTS0: CPTRGF0 Position

Definition at line 4292 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF1_Msk

#define PWM_ADCTSTS0_CPTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF1_Pos)

PWM_T::ADCTSTS0: CPTRGF1 Mask

Definition at line 4305 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF1_Pos

#define PWM_ADCTSTS0_CPTRGF1_Pos (9)

PWM_T::ADCTSTS0: CPTRGF1 Position

Definition at line 4304 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF2_Msk

#define PWM_ADCTSTS0_CPTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF2_Pos)

PWM_T::ADCTSTS0: CPTRGF2 Mask

Definition at line 4317 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF2_Pos

#define PWM_ADCTSTS0_CPTRGF2_Pos (17)

PWM_T::ADCTSTS0: CPTRGF2 Position

Definition at line 4316 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF3_Msk

#define PWM_ADCTSTS0_CPTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CPTRGF3_Pos)

PWM_T::ADCTSTS0: CPTRGF3 Mask

Definition at line 4329 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CPTRGF3_Pos

#define PWM_ADCTSTS0_CPTRGF3_Pos (25)

PWM_T::ADCTSTS0: CPTRGF3 Position

Definition at line 4328 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF0_Msk

#define PWM_ADCTSTS0_CUTRGF0_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF0_Pos)

PWM_T::ADCTSTS0: CUTRGF0 Mask

Definition at line 4290 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF0_Pos

#define PWM_ADCTSTS0_CUTRGF0_Pos (0)

PWM_T::ADCTSTS0: CUTRGF0 Position

Definition at line 4289 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF1_Msk

#define PWM_ADCTSTS0_CUTRGF1_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF1_Pos)

PWM_T::ADCTSTS0: CUTRGF1 Mask

Definition at line 4302 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF1_Pos

#define PWM_ADCTSTS0_CUTRGF1_Pos (8)

PWM_T::ADCTSTS0: CUTRGF1 Position

Definition at line 4301 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF2_Msk

#define PWM_ADCTSTS0_CUTRGF2_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF2_Pos)

PWM_T::ADCTSTS0: CUTRGF2 Mask

Definition at line 4314 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF2_Pos

#define PWM_ADCTSTS0_CUTRGF2_Pos (16)

PWM_T::ADCTSTS0: CUTRGF2 Position

Definition at line 4313 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF3_Msk

#define PWM_ADCTSTS0_CUTRGF3_Msk (0x1ul << PWM_ADCTSTS0_CUTRGF3_Pos)

PWM_T::ADCTSTS0: CUTRGF3 Mask

Definition at line 4326 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_CUTRGF3_Pos

#define PWM_ADCTSTS0_CUTRGF3_Pos (24)

PWM_T::ADCTSTS0: CUTRGF3 Position

Definition at line 4325 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF0_Msk

#define PWM_ADCTSTS0_ZPTRGF0_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF0_Pos)

PWM_T::ADCTSTS0: ZPTRGF0 Mask

Definition at line 4299 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF0_Pos

#define PWM_ADCTSTS0_ZPTRGF0_Pos (3)

PWM_T::ADCTSTS0: ZPTRGF0 Position

Definition at line 4298 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF1_Msk

#define PWM_ADCTSTS0_ZPTRGF1_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF1_Pos)

PWM_T::ADCTSTS0: ZPTRGF1 Mask

Definition at line 4311 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF1_Pos

#define PWM_ADCTSTS0_ZPTRGF1_Pos (11)

PWM_T::ADCTSTS0: ZPTRGF1 Position

Definition at line 4310 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF2_Msk

#define PWM_ADCTSTS0_ZPTRGF2_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF2_Pos)

PWM_T::ADCTSTS0: ZPTRGF2 Mask

Definition at line 4323 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF2_Pos

#define PWM_ADCTSTS0_ZPTRGF2_Pos (19)

PWM_T::ADCTSTS0: ZPTRGF2 Position

Definition at line 4322 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF3_Msk

#define PWM_ADCTSTS0_ZPTRGF3_Msk (0x1ul << PWM_ADCTSTS0_ZPTRGF3_Pos)

PWM_T::ADCTSTS0: ZPTRGF3 Mask

Definition at line 4335 of file Mini55Series.h.

## ◆ PWM_ADCTSTS0_ZPTRGF3_Pos

#define PWM_ADCTSTS0_ZPTRGF3_Pos (27)

PWM_T::ADCTSTS0: ZPTRGF3 Position

Definition at line 4334 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CDTRGF4_Msk

#define PWM_ADCTSTS1_CDTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CDTRGF4_Pos)

PWM_T::ADCTSTS1: CDTRGF4 Mask

Definition at line 4344 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CDTRGF4_Pos

#define PWM_ADCTSTS1_CDTRGF4_Pos (2)

PWM_T::ADCTSTS1: CDTRGF4 Position

Definition at line 4343 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CDTRGF5_Msk

#define PWM_ADCTSTS1_CDTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CDTRGF5_Pos)

PWM_T::ADCTSTS1: CDTRGF5 Mask

Definition at line 4356 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CDTRGF5_Pos

#define PWM_ADCTSTS1_CDTRGF5_Pos (10)

PWM_T::ADCTSTS1: CDTRGF5 Position

Definition at line 4355 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CPTRGF4_Msk

#define PWM_ADCTSTS1_CPTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CPTRGF4_Pos)

PWM_T::ADCTSTS1: CPTRGF4 Mask

Definition at line 4341 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CPTRGF4_Pos

#define PWM_ADCTSTS1_CPTRGF4_Pos (1)

PWM_T::ADCTSTS1: CPTRGF4 Position

Definition at line 4340 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CPTRGF5_Msk

#define PWM_ADCTSTS1_CPTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CPTRGF5_Pos)

PWM_T::ADCTSTS1: CPTRGF5 Mask

Definition at line 4353 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CPTRGF5_Pos

#define PWM_ADCTSTS1_CPTRGF5_Pos (9)

PWM_T::ADCTSTS1: CPTRGF5 Position

Definition at line 4352 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CUTRGF4_Msk

#define PWM_ADCTSTS1_CUTRGF4_Msk (0x1ul << PWM_ADCTSTS1_CUTRGF4_Pos)

PWM_T::ADCTSTS1: CUTRGF4 Mask

Definition at line 4338 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CUTRGF4_Pos

#define PWM_ADCTSTS1_CUTRGF4_Pos (0)

PWM_T::ADCTSTS1: CUTRGF4 Position

Definition at line 4337 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CUTRGF5_Msk

#define PWM_ADCTSTS1_CUTRGF5_Msk (0x1ul << PWM_ADCTSTS1_CUTRGF5_Pos)

PWM_T::ADCTSTS1: CUTRGF5 Mask

Definition at line 4350 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_CUTRGF5_Pos

#define PWM_ADCTSTS1_CUTRGF5_Pos (8)

PWM_T::ADCTSTS1: CUTRGF5 Position

Definition at line 4349 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_ZPTRGF4_Msk

#define PWM_ADCTSTS1_ZPTRGF4_Msk (0x1ul << PWM_ADCTSTS1_ZPTRGF4_Pos)

PWM_T::ADCTSTS1: ZPTRGF4 Mask

Definition at line 4347 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_ZPTRGF4_Pos

#define PWM_ADCTSTS1_ZPTRGF4_Pos (3)

PWM_T::ADCTSTS1: ZPTRGF4 Position

Definition at line 4346 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_ZPTRGF5_Msk

#define PWM_ADCTSTS1_ZPTRGF5_Msk (0x1ul << PWM_ADCTSTS1_ZPTRGF5_Pos)

PWM_T::ADCTSTS1: ZPTRGF5 Mask

Definition at line 4359 of file Mini55Series.h.

## ◆ PWM_ADCTSTS1_ZPTRGF5_Pos

#define PWM_ADCTSTS1_ZPTRGF5_Pos (11)

PWM_T::ADCTSTS1: ZPTRGF5 Position

Definition at line 4358 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD0_Msk

#define PWM_BRKCTL_BKOD0_Msk (0x1ul << PWM_BRKCTL_BKOD0_Pos)

PWM_T::BRKCTL: BKOD0 Mask

Definition at line 4185 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD0_Pos

#define PWM_BRKCTL_BKOD0_Pos (24)

PWM_T::BRKCTL: BKOD0 Position

Definition at line 4184 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD1_Msk

#define PWM_BRKCTL_BKOD1_Msk (0x1ul << PWM_BRKCTL_BKOD1_Pos)

PWM_T::BRKCTL: BKOD1 Mask

Definition at line 4188 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD1_Pos

#define PWM_BRKCTL_BKOD1_Pos (25)

PWM_T::BRKCTL: BKOD1 Position

Definition at line 4187 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD2_Msk

#define PWM_BRKCTL_BKOD2_Msk (0x1ul << PWM_BRKCTL_BKOD2_Pos)

PWM_T::BRKCTL: BKOD2 Mask

Definition at line 4191 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD2_Pos

#define PWM_BRKCTL_BKOD2_Pos (26)

PWM_T::BRKCTL: BKOD2 Position

Definition at line 4190 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD3_Msk

#define PWM_BRKCTL_BKOD3_Msk (0x1ul << PWM_BRKCTL_BKOD3_Pos)

PWM_T::BRKCTL: BKOD3 Mask

Definition at line 4194 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD3_Pos

#define PWM_BRKCTL_BKOD3_Pos (27)

PWM_T::BRKCTL: BKOD3 Position

Definition at line 4193 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD4_Msk

#define PWM_BRKCTL_BKOD4_Msk (0x1ul << PWM_BRKCTL_BKOD4_Pos)

PWM_T::BRKCTL: BKOD4 Mask

Definition at line 4197 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD4_Pos

#define PWM_BRKCTL_BKOD4_Pos (28)

PWM_T::BRKCTL: BKOD4 Position

Definition at line 4196 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD5_Msk

#define PWM_BRKCTL_BKOD5_Msk (0x1ul << PWM_BRKCTL_BKOD5_Pos)

PWM_T::BRKCTL: BKOD5 Mask

Definition at line 4200 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BKOD5_Pos

#define PWM_BRKCTL_BKOD5_Pos (29)

PWM_T::BRKCTL: BKOD5 Position

Definition at line 4199 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRK0EN_Msk

#define PWM_BRKCTL_BRK0EN_Msk (0x1ul << PWM_BRKCTL_BRK0EN_Pos)

PWM_T::BRKCTL: BRK0EN Mask

Definition at line 4164 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRK0EN_Pos

#define PWM_BRKCTL_BRK0EN_Pos (0)

PWM_T::BRKCTL: BRK0EN Position

Definition at line 4163 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRK0SEL_Msk

#define PWM_BRKCTL_BRK0SEL_Msk (0x1ul << PWM_BRKCTL_BRK0SEL_Pos)

PWM_T::BRKCTL: BRK0SEL Mask

Definition at line 4170 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRK0SEL_Pos

#define PWM_BRKCTL_BRK0SEL_Pos (2)

PWM_T::BRKCTL: BRK0SEL Position

Definition at line 4169 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRK1EN_Msk

#define PWM_BRKCTL_BRK1EN_Msk (0x1ul << PWM_BRKCTL_BRK1EN_Pos)

PWM_T::BRKCTL: BRK1EN Mask

Definition at line 4167 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRK1EN_Pos

#define PWM_BRKCTL_BRK1EN_Pos (1)

PWM_T::BRKCTL: BRK1EN Position

Definition at line 4166 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRK1SEL_Msk

#define PWM_BRKCTL_BRK1SEL_Msk (0x1ul << PWM_BRKCTL_BRK1SEL_Pos)

PWM_T::BRKCTL: BRK1SEL Mask

Definition at line 4173 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRK1SEL_Pos

#define PWM_BRKCTL_BRK1SEL_Pos (3)

PWM_T::BRKCTL: BRK1SEL Position

Definition at line 4172 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRKACT_Msk

#define PWM_BRKCTL_BRKACT_Msk (0x1ul << PWM_BRKCTL_BRKACT_Pos)

PWM_T::BRKCTL: BRKACT Mask

Definition at line 4179 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRKACT_Pos

#define PWM_BRKCTL_BRKACT_Pos (8)

PWM_T::BRKCTL: BRKACT Position

Definition at line 4178 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRKSTS_Msk

#define PWM_BRKCTL_BRKSTS_Msk (0x1ul << PWM_BRKCTL_BRKSTS_Pos)

PWM_T::BRKCTL: BRKSTS Mask

Definition at line 4176 of file Mini55Series.h.

## ◆ PWM_BRKCTL_BRKSTS_Pos

#define PWM_BRKCTL_BRKSTS_Pos (7)

PWM_T::BRKCTL: BRKSTS Position

Definition at line 4175 of file Mini55Series.h.

## ◆ PWM_BRKCTL_D6BKOD_Msk

#define PWM_BRKCTL_D6BKOD_Msk (0x1ul << PWM_BRKCTL_D6BKOD_Pos)

PWM_T::BRKCTL: D6BKOD Mask

Definition at line 4203 of file Mini55Series.h.

## ◆ PWM_BRKCTL_D6BKOD_Pos

#define PWM_BRKCTL_D6BKOD_Pos (30)

PWM_T::BRKCTL: D6BKOD Position

Definition at line 4202 of file Mini55Series.h.

## ◆ PWM_BRKCTL_D7BKOD_Msk

#define PWM_BRKCTL_D7BKOD_Msk (0x1ul << PWM_BRKCTL_D7BKOD_Pos)

PWM_T::BRKCTL: D7BKOD Mask

Definition at line 4206 of file Mini55Series.h.

## ◆ PWM_BRKCTL_D7BKOD_Pos

#define PWM_BRKCTL_D7BKOD_Pos (31)

PWM_T::BRKCTL: D7BKOD Position

Definition at line 4205 of file Mini55Series.h.

## ◆ PWM_BRKCTL_SWBRK_Msk

#define PWM_BRKCTL_SWBRK_Msk (0x1ul << PWM_BRKCTL_SWBRK_Pos)

PWM_T::BRKCTL: SWBRK Mask

Definition at line 4182 of file Mini55Series.h.

## ◆ PWM_BRKCTL_SWBRK_Pos

#define PWM_BRKCTL_SWBRK_Pos (9)

PWM_T::BRKCTL: SWBRK Position

Definition at line 4181 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV0_Msk

#define PWM_CLKDIV_CLKDIV0_Msk (0x7ul << PWM_CLKDIV_CLKDIV0_Pos)

PWM_T::CLKDIV: CLKDIV0 Mask

Definition at line 3879 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV0_Pos

#define PWM_CLKDIV_CLKDIV0_Pos (0)

PWM_T::CLKDIV: CLKDIV0 Position

Definition at line 3878 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV1_Msk

#define PWM_CLKDIV_CLKDIV1_Msk (0x7ul << PWM_CLKDIV_CLKDIV1_Pos)

PWM_T::CLKDIV: CLKDIV1 Mask

Definition at line 3882 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV1_Pos

#define PWM_CLKDIV_CLKDIV1_Pos (4)

PWM_T::CLKDIV: CLKDIV1 Position

Definition at line 3881 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV2_Msk

#define PWM_CLKDIV_CLKDIV2_Msk (0x7ul << PWM_CLKDIV_CLKDIV2_Pos)

PWM_T::CLKDIV: CLKDIV2 Mask

Definition at line 3885 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV2_Pos

#define PWM_CLKDIV_CLKDIV2_Pos (8)

PWM_T::CLKDIV: CLKDIV2 Position

Definition at line 3884 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV3_Msk

#define PWM_CLKDIV_CLKDIV3_Msk (0x7ul << PWM_CLKDIV_CLKDIV3_Pos)

PWM_T::CLKDIV: CLKDIV3 Mask

Definition at line 3888 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV3_Pos

#define PWM_CLKDIV_CLKDIV3_Pos (12)

PWM_T::CLKDIV: CLKDIV3 Position

Definition at line 3887 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV4_Msk

#define PWM_CLKDIV_CLKDIV4_Msk (0x7ul << PWM_CLKDIV_CLKDIV4_Pos)

PWM_T::CLKDIV: CLKDIV4 Mask

Definition at line 3891 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV4_Pos

#define PWM_CLKDIV_CLKDIV4_Pos (16)

PWM_T::CLKDIV: CLKDIV4 Position

Definition at line 3890 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV5_Msk

#define PWM_CLKDIV_CLKDIV5_Msk (0x7ul << PWM_CLKDIV_CLKDIV5_Pos)

PWM_T::CLKDIV: CLKDIV5 Mask

Definition at line 3894 of file Mini55Series.h.

## ◆ PWM_CLKDIV_CLKDIV5_Pos

#define PWM_CLKDIV_CLKDIV5_Pos (20)

PWM_T::CLKDIV: CLKDIV5 Position

Definition at line 3893 of file Mini55Series.h.

## ◆ PWM_CLKPSC_CLKPSC01_Msk

#define PWM_CLKPSC_CLKPSC01_Msk (0xfful << PWM_CLKPSC_CLKPSC01_Pos)

PWM_T::CLKPSC: CLKPSC01 Mask

Definition at line 3870 of file Mini55Series.h.

## ◆ PWM_CLKPSC_CLKPSC01_Pos

#define PWM_CLKPSC_CLKPSC01_Pos (0)

    @addtogroup PWM_CONST PWM Bit Field Definition
    Constant Definitions for PWM Controller

PWM_T::CLKPSC: CLKPSC01 Position

Definition at line 3869 of file Mini55Series.h.

## ◆ PWM_CLKPSC_CLKPSC23_Msk

#define PWM_CLKPSC_CLKPSC23_Msk (0xfful << PWM_CLKPSC_CLKPSC23_Pos)

PWM_T::CLKPSC: CLKPSC23 Mask

Definition at line 3873 of file Mini55Series.h.

## ◆ PWM_CLKPSC_CLKPSC23_Pos

#define PWM_CLKPSC_CLKPSC23_Pos (8)

PWM_T::CLKPSC: CLKPSC23 Position

Definition at line 3872 of file Mini55Series.h.

## ◆ PWM_CLKPSC_CLKPSC45_Msk

#define PWM_CLKPSC_CLKPSC45_Msk (0xfful << PWM_CLKPSC_CLKPSC45_Pos)

PWM_T::CLKPSC: CLKPSC45 Mask

Definition at line 3876 of file Mini55Series.h.

## ◆ PWM_CLKPSC_CLKPSC45_Pos

#define PWM_CLKPSC_CLKPSC45_Pos (16)

PWM_T::CLKPSC: CLKPSC45 Position

Definition at line 3875 of file Mini55Series.h.

## ◆ PWM_CMPDAT_CMP_Msk

#define PWM_CMPDAT_CMP_Msk (0xfffful << PWM_CMPDAT_CMP_Pos)

PWM_T::CMPDAT: CMP Mask

Definition at line 3984 of file Mini55Series.h.

## ◆ PWM_CMPDAT_CMP_Pos

#define PWM_CMPDAT_CMP_Pos (0)

PWM_T::CMPDAT: CMP Position

Definition at line 3983 of file Mini55Series.h.

## ◆ PWM_CMPDAT_CMPD_Msk

#define PWM_CMPDAT_CMPD_Msk (0xfffful << PWM_CMPDAT_CMPD_Pos)

PWM_T::CMPDAT: CMPD Mask

Definition at line 3987 of file Mini55Series.h.

## ◆ PWM_CMPDAT_CMPD_Pos

#define PWM_CMPDAT_CMPD_Pos (16)

PWM_T::CMPDAT: CMPD Position

Definition at line 3986 of file Mini55Series.h.

## ◆ PWM_CTL_ASYMEN_Msk

#define PWM_CTL_ASYMEN_Msk (0x1ul << PWM_CTL_ASYMEN_Pos)

PWM_T::CTL: ASYMEN Mask

Definition at line 3951 of file Mini55Series.h.

## ◆ PWM_CTL_ASYMEN_Pos

#define PWM_CTL_ASYMEN_Pos (21)

PWM_T::CTL: ASYMEN Position

Definition at line 3950 of file Mini55Series.h.

## ◆ PWM_CTL_CNTCLR_Msk

#define PWM_CTL_CNTCLR_Msk (0x1ul << PWM_CTL_CNTCLR_Pos)

PWM_T::CTL: CNTCLR Mask

Definition at line 3969 of file Mini55Series.h.

## ◆ PWM_CTL_CNTCLR_Pos

#define PWM_CTL_CNTCLR_Pos (27)

PWM_T::CTL: CNTCLR Position

Definition at line 3968 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN0_Msk

#define PWM_CTL_CNTEN0_Msk (0x1ul << PWM_CTL_CNTEN0_Pos)

PWM_T::CTL: CNTEN0 Mask

Definition at line 3897 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN0_Pos

#define PWM_CTL_CNTEN0_Pos (0)

PWM_T::CTL: CNTEN0 Position

Definition at line 3896 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN1_Msk

#define PWM_CTL_CNTEN1_Msk (0x1ul << PWM_CTL_CNTEN1_Pos)

PWM_T::CTL: CNTEN1 Mask

Definition at line 3909 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN1_Pos

#define PWM_CTL_CNTEN1_Pos (4)

PWM_T::CTL: CNTEN1 Position

Definition at line 3908 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN2_Msk

#define PWM_CTL_CNTEN2_Msk (0x1ul << PWM_CTL_CNTEN2_Pos)

PWM_T::CTL: CNTEN2 Mask

Definition at line 3921 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN2_Pos

#define PWM_CTL_CNTEN2_Pos (8)

PWM_T::CTL: CNTEN2 Position

Definition at line 3920 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN3_Msk

#define PWM_CTL_CNTEN3_Msk (0x1ul << PWM_CTL_CNTEN3_Pos)

PWM_T::CTL: CNTEN3 Mask

Definition at line 3930 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN3_Pos

#define PWM_CTL_CNTEN3_Pos (12)

PWM_T::CTL: CNTEN3 Position

Definition at line 3929 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN4_Msk

#define PWM_CTL_CNTEN4_Msk (0x1ul << PWM_CTL_CNTEN4_Pos)

PWM_T::CTL: CNTEN4 Mask

Definition at line 3939 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN4_Pos

#define PWM_CTL_CNTEN4_Pos (16)

PWM_T::CTL: CNTEN4 Position

Definition at line 3938 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN5_Msk

#define PWM_CTL_CNTEN5_Msk (0x1ul << PWM_CTL_CNTEN5_Pos)

PWM_T::CTL: CNTEN5 Mask

Definition at line 3948 of file Mini55Series.h.

## ◆ PWM_CTL_CNTEN5_Pos

#define PWM_CTL_CNTEN5_Pos (20)

PWM_T::CTL: CNTEN5 Position

Definition at line 3947 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE0_Msk

#define PWM_CTL_CNTMODE0_Msk (0x1ul << PWM_CTL_CNTMODE0_Pos)

PWM_T::CTL: CNTMODE0 Mask

Definition at line 3906 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE0_Pos

#define PWM_CTL_CNTMODE0_Pos (3)

PWM_T::CTL: CNTMODE0 Position

Definition at line 3905 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE1_Msk

#define PWM_CTL_CNTMODE1_Msk (0x1ul << PWM_CTL_CNTMODE1_Pos)

PWM_T::CTL: CNTMODE1 Mask

Definition at line 3918 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE1_Pos

#define PWM_CTL_CNTMODE1_Pos (7)

PWM_T::CTL: CNTMODE1 Position

Definition at line 3917 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE2_Msk

#define PWM_CTL_CNTMODE2_Msk (0x1ul << PWM_CTL_CNTMODE2_Pos)

PWM_T::CTL: CNTMODE2 Mask

Definition at line 3927 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE2_Pos

#define PWM_CTL_CNTMODE2_Pos (11)

PWM_T::CTL: CNTMODE2 Position

Definition at line 3926 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE3_Msk

#define PWM_CTL_CNTMODE3_Msk (0x1ul << PWM_CTL_CNTMODE3_Pos)

PWM_T::CTL: CNTMODE3 Mask

Definition at line 3936 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE3_Pos

#define PWM_CTL_CNTMODE3_Pos (15)

PWM_T::CTL: CNTMODE3 Position

Definition at line 3935 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE4_Msk

#define PWM_CTL_CNTMODE4_Msk (0x1ul << PWM_CTL_CNTMODE4_Pos)

PWM_T::CTL: CNTMODE4 Mask

Definition at line 3945 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE4_Pos

#define PWM_CTL_CNTMODE4_Pos (19)

PWM_T::CTL: CNTMODE4 Position

Definition at line 3944 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE5_Msk

#define PWM_CTL_CNTMODE5_Msk (0x1ul << PWM_CTL_CNTMODE5_Pos)

PWM_T::CTL: CNTMODE5 Mask

Definition at line 3957 of file Mini55Series.h.

## ◆ PWM_CTL_CNTMODE5_Pos

#define PWM_CTL_CNTMODE5_Pos (23)

PWM_T::CTL: CNTMODE5 Position

Definition at line 3956 of file Mini55Series.h.

## ◆ PWM_CTL_CNTTYPE_Msk

#define PWM_CTL_CNTTYPE_Msk (0x1ul << PWM_CTL_CNTTYPE_Pos)

PWM_T::CTL: CNTTYPE Mask

Definition at line 3978 of file Mini55Series.h.

## ◆ PWM_CTL_CNTTYPE_Pos

#define PWM_CTL_CNTTYPE_Pos (31)

PWM_T::CTL: CNTTYPE Position

Definition at line 3977 of file Mini55Series.h.

## ◆ PWM_CTL_DBGTRIOFF_Msk

#define PWM_CTL_DBGTRIOFF_Msk (0x1ul << PWM_CTL_DBGTRIOFF_Pos)

PWM_T::CTL: DBGTRIOFF Mask

Definition at line 3900 of file Mini55Series.h.

## ◆ PWM_CTL_DBGTRIOFF_Pos

#define PWM_CTL_DBGTRIOFF_Pos (1)

PWM_T::CTL: DBGTRIOFF Position

Definition at line 3899 of file Mini55Series.h.

## ◆ PWM_CTL_DTCNT01_Msk

#define PWM_CTL_DTCNT01_Msk (0x1ul << PWM_CTL_DTCNT01_Pos)

PWM_T::CTL: DTCNT01 Mask

Definition at line 3960 of file Mini55Series.h.

## ◆ PWM_CTL_DTCNT01_Pos

#define PWM_CTL_DTCNT01_Pos (24)

PWM_T::CTL: DTCNT01 Position

Definition at line 3959 of file Mini55Series.h.

## ◆ PWM_CTL_DTCNT23_Msk

#define PWM_CTL_DTCNT23_Msk (0x1ul << PWM_CTL_DTCNT23_Pos)

PWM_T::CTL: DTCNT23 Mask

Definition at line 3963 of file Mini55Series.h.

## ◆ PWM_CTL_DTCNT23_Pos

#define PWM_CTL_DTCNT23_Pos (25)

PWM_T::CTL: DTCNT23 Position

Definition at line 3962 of file Mini55Series.h.

## ◆ PWM_CTL_DTCNT45_Msk

#define PWM_CTL_DTCNT45_Msk (0x1ul << PWM_CTL_DTCNT45_Pos)

PWM_T::CTL: DTCNT45 Mask

Definition at line 3966 of file Mini55Series.h.

## ◆ PWM_CTL_DTCNT45_Pos

#define PWM_CTL_DTCNT45_Pos (26)

PWM_T::CTL: DTCNT45 Position

Definition at line 3965 of file Mini55Series.h.

## ◆ PWM_CTL_GROUPEN_Msk

#define PWM_CTL_GROUPEN_Msk (0x1ul << PWM_CTL_GROUPEN_Pos)

PWM_T::CTL: GROUPEN Mask

Definition at line 3975 of file Mini55Series.h.

## ◆ PWM_CTL_GROUPEN_Pos

#define PWM_CTL_GROUPEN_Pos (30)

PWM_T::CTL: GROUPEN Position

Definition at line 3974 of file Mini55Series.h.

## ◆ PWM_CTL_HCUPDT_Msk

#define PWM_CTL_HCUPDT_Msk (0x1ul << PWM_CTL_HCUPDT_Pos)

PWM_T::CTL: HCUPDT Mask

Definition at line 3912 of file Mini55Series.h.

## ◆ PWM_CTL_HCUPDT_Pos

#define PWM_CTL_HCUPDT_Pos (5)

PWM_T::CTL: HCUPDT Position

Definition at line 3911 of file Mini55Series.h.

## ◆ PWM_CTL_MODE_Msk

#define PWM_CTL_MODE_Msk (0x3ul << PWM_CTL_MODE_Pos)

PWM_T::CTL: MODE Mask

Definition at line 3972 of file Mini55Series.h.

## ◆ PWM_CTL_MODE_Pos

#define PWM_CTL_MODE_Pos (28)

PWM_T::CTL: MODE Position

Definition at line 3971 of file Mini55Series.h.

## ◆ PWM_CTL_PINV0_Msk

#define PWM_CTL_PINV0_Msk (0x1ul << PWM_CTL_PINV0_Pos)

PWM_T::CTL: PINV0 Mask

Definition at line 3903 of file Mini55Series.h.

## ◆ PWM_CTL_PINV0_Pos

#define PWM_CTL_PINV0_Pos (2)

PWM_T::CTL: PINV0 Position

Definition at line 3902 of file Mini55Series.h.

## ◆ PWM_CTL_PINV1_Msk

#define PWM_CTL_PINV1_Msk (0x1ul << PWM_CTL_PINV1_Pos)

PWM_T::CTL: PINV1 Mask

Definition at line 3915 of file Mini55Series.h.

## ◆ PWM_CTL_PINV1_Pos

#define PWM_CTL_PINV1_Pos (6)

PWM_T::CTL: PINV1 Position

Definition at line 3914 of file Mini55Series.h.

## ◆ PWM_CTL_PINV2_Msk

#define PWM_CTL_PINV2_Msk (0x1ul << PWM_CTL_PINV2_Pos)

PWM_T::CTL: PINV2 Mask

Definition at line 3924 of file Mini55Series.h.

## ◆ PWM_CTL_PINV2_Pos

#define PWM_CTL_PINV2_Pos (10)

PWM_T::CTL: PINV2 Position

Definition at line 3923 of file Mini55Series.h.

## ◆ PWM_CTL_PINV3_Msk

#define PWM_CTL_PINV3_Msk (0x1ul << PWM_CTL_PINV3_Pos)

PWM_T::CTL: PINV3 Mask

Definition at line 3933 of file Mini55Series.h.

## ◆ PWM_CTL_PINV3_Pos

#define PWM_CTL_PINV3_Pos (14)

PWM_T::CTL: PINV3 Position

Definition at line 3932 of file Mini55Series.h.

## ◆ PWM_CTL_PINV4_Msk

#define PWM_CTL_PINV4_Msk (0x1ul << PWM_CTL_PINV4_Pos)

PWM_T::CTL: PINV4 Mask

Definition at line 3942 of file Mini55Series.h.

## ◆ PWM_CTL_PINV4_Pos

#define PWM_CTL_PINV4_Pos (18)

PWM_T::CTL: PINV4 Position

Definition at line 3941 of file Mini55Series.h.

## ◆ PWM_CTL_PINV5_Msk

#define PWM_CTL_PINV5_Msk (0x1ul << PWM_CTL_PINV5_Pos)

PWM_T::CTL: PINV5 Mask

Definition at line 3954 of file Mini55Series.h.

## ◆ PWM_CTL_PINV5_Pos

#define PWM_CTL_PINV5_Pos (22)

PWM_T::CTL: PINV5 Position

Definition at line 3953 of file Mini55Series.h.

## ◆ PWM_DTCTL_DTCNT01_Msk

#define PWM_DTCTL_DTCNT01_Msk (0xfful << PWM_DTCTL_DTCNT01_Pos)

PWM_T::DTCTL: DTCNT01 Mask

Definition at line 4209 of file Mini55Series.h.

## ◆ PWM_DTCTL_DTCNT01_Pos

#define PWM_DTCTL_DTCNT01_Pos (0)

PWM_T::DTCTL: DTCNT01 Position

Definition at line 4208 of file Mini55Series.h.

## ◆ PWM_DTCTL_DTCNT23_Msk

#define PWM_DTCTL_DTCNT23_Msk (0xfful << PWM_DTCTL_DTCNT23_Pos)

PWM_T::DTCTL: DTCNT23 Mask

Definition at line 4212 of file Mini55Series.h.

## ◆ PWM_DTCTL_DTCNT23_Pos

#define PWM_DTCTL_DTCNT23_Pos (8)

PWM_T::DTCTL: DTCNT23 Position

Definition at line 4211 of file Mini55Series.h.

## ◆ PWM_DTCTL_DTCNT45_Msk

#define PWM_DTCTL_DTCNT45_Msk (0xfful << PWM_DTCTL_DTCNT45_Pos)

PWM_T::DTCTL: DTCNT45 Mask

Definition at line 4215 of file Mini55Series.h.

## ◆ PWM_DTCTL_DTCNT45_Pos

#define PWM_DTCTL_DTCNT45_Pos (16)

PWM_T::DTCTL: DTCNT45 Position

Definition at line 4214 of file Mini55Series.h.

## ◆ PWM_IFA_IFAEN_Msk

#define PWM_IFA_IFAEN_Msk (0x1ul << PWM_IFA_IFAEN_Pos)

PWM_T::IFA: IFAEN Mask

Definition at line 4554 of file Mini55Series.h.

## ◆ PWM_IFA_IFAEN_Pos

#define PWM_IFA_IFAEN_Pos (0)

PWM_T::IFA: IFAEN Position

Definition at line 4553 of file Mini55Series.h.

## ◆ PWM_IFA_IFCNT_Msk

#define PWM_IFA_IFCNT_Msk (0xful << PWM_IFA_IFCNT_Pos)

PWM_T::IFA: IFCNT Mask

Definition at line 4557 of file Mini55Series.h.

## ◆ PWM_IFA_IFCNT_Pos

#define PWM_IFA_IFCNT_Pos (4)

PWM_T::IFA: IFCNT Position

Definition at line 4556 of file Mini55Series.h.

## ◆ PWM_INTEN_BRKIEN_Msk

#define PWM_INTEN_BRKIEN_Msk (0x1ul << PWM_INTEN_BRKIEN_Pos)

PWM_T::INTEN: BRKIEN Mask

Definition at line 4026 of file Mini55Series.h.

## ◆ PWM_INTEN_BRKIEN_Pos

#define PWM_INTEN_BRKIEN_Pos (16)

PWM_T::INTEN: BRKIEN Position

Definition at line 4025 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN0_Msk

#define PWM_INTEN_CMPDIEN0_Msk (0x1ul << PWM_INTEN_CMPDIEN0_Pos)

PWM_T::INTEN: CMPDIEN0 Mask

Definition at line 4008 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN0_Pos

#define PWM_INTEN_CMPDIEN0_Pos (8)

PWM_T::INTEN: CMPDIEN0 Position

Definition at line 4007 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN1_Msk

#define PWM_INTEN_CMPDIEN1_Msk (0x1ul << PWM_INTEN_CMPDIEN1_Pos)

PWM_T::INTEN: CMPDIEN1 Mask

Definition at line 4011 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN1_Pos

#define PWM_INTEN_CMPDIEN1_Pos (9)

PWM_T::INTEN: CMPDIEN1 Position

Definition at line 4010 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN2_Msk

#define PWM_INTEN_CMPDIEN2_Msk (0x1ul << PWM_INTEN_CMPDIEN2_Pos)

PWM_T::INTEN: CMPDIEN2 Mask

Definition at line 4014 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN2_Pos

#define PWM_INTEN_CMPDIEN2_Pos (10)

PWM_T::INTEN: CMPDIEN2 Position

Definition at line 4013 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN3_Msk

#define PWM_INTEN_CMPDIEN3_Msk (0x1ul << PWM_INTEN_CMPDIEN3_Pos)

PWM_T::INTEN: CMPDIEN3 Mask

Definition at line 4017 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN3_Pos

#define PWM_INTEN_CMPDIEN3_Pos (11)

PWM_T::INTEN: CMPDIEN3 Position

Definition at line 4016 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN4_Msk

#define PWM_INTEN_CMPDIEN4_Msk (0x1ul << PWM_INTEN_CMPDIEN4_Pos)

PWM_T::INTEN: CMPDIEN4 Mask

Definition at line 4020 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN4_Pos

#define PWM_INTEN_CMPDIEN4_Pos (12)

PWM_T::INTEN: CMPDIEN4 Position

Definition at line 4019 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN5_Msk

#define PWM_INTEN_CMPDIEN5_Msk (0x1ul << PWM_INTEN_CMPDIEN5_Pos)

PWM_T::INTEN: CMPDIEN5 Mask

Definition at line 4023 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPDIEN5_Pos

#define PWM_INTEN_CMPDIEN5_Pos (13)

PWM_T::INTEN: CMPDIEN5 Position

Definition at line 4022 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN0_Msk

#define PWM_INTEN_CMPUIEN0_Msk (0x1ul << PWM_INTEN_CMPUIEN0_Pos)

PWM_T::INTEN: CMPUIEN0 Mask

Definition at line 4050 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN0_Pos

#define PWM_INTEN_CMPUIEN0_Pos (24)

PWM_T::INTEN: CMPUIEN0 Position

Definition at line 4049 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN1_Msk

#define PWM_INTEN_CMPUIEN1_Msk (0x1ul << PWM_INTEN_CMPUIEN1_Pos)

PWM_T::INTEN: CMPUIEN1 Mask

Definition at line 4053 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN1_Pos

#define PWM_INTEN_CMPUIEN1_Pos (25)

PWM_T::INTEN: CMPUIEN1 Position

Definition at line 4052 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN2_Msk

#define PWM_INTEN_CMPUIEN2_Msk (0x1ul << PWM_INTEN_CMPUIEN2_Pos)

PWM_T::INTEN: CMPUIEN2 Mask

Definition at line 4056 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN2_Pos

#define PWM_INTEN_CMPUIEN2_Pos (26)

PWM_T::INTEN: CMPUIEN2 Position

Definition at line 4055 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN3_Msk

#define PWM_INTEN_CMPUIEN3_Msk (0x1ul << PWM_INTEN_CMPUIEN3_Pos)

PWM_T::INTEN: CMPUIEN3 Mask

Definition at line 4059 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN3_Pos

#define PWM_INTEN_CMPUIEN3_Pos (27)

PWM_T::INTEN: CMPUIEN3 Position

Definition at line 4058 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN4_Msk

#define PWM_INTEN_CMPUIEN4_Msk (0x1ul << PWM_INTEN_CMPUIEN4_Pos)

PWM_T::INTEN: CMPUIEN4 Mask

Definition at line 4062 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN4_Pos

#define PWM_INTEN_CMPUIEN4_Pos (28)

PWM_T::INTEN: CMPUIEN4 Position

Definition at line 4061 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN5_Msk

#define PWM_INTEN_CMPUIEN5_Msk (0x1ul << PWM_INTEN_CMPUIEN5_Pos)

PWM_T::INTEN: CMPUIEN5 Mask

Definition at line 4065 of file Mini55Series.h.

## ◆ PWM_INTEN_CMPUIEN5_Pos

#define PWM_INTEN_CMPUIEN5_Pos (29)

PWM_T::INTEN: CMPUIEN5 Position

Definition at line 4064 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN0_Msk

#define PWM_INTEN_PIEN0_Msk (0x1ul << PWM_INTEN_PIEN0_Pos)

PWM_T::INTEN: PIEN0 Mask

Definition at line 4032 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN0_Pos

#define PWM_INTEN_PIEN0_Pos (18)

PWM_T::INTEN: PIEN0 Position

Definition at line 4031 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN1_Msk

#define PWM_INTEN_PIEN1_Msk (0x1ul << PWM_INTEN_PIEN1_Pos)

PWM_T::INTEN: PIEN1 Mask

Definition at line 4035 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN1_Pos

#define PWM_INTEN_PIEN1_Pos (19)

PWM_T::INTEN: PIEN1 Position

Definition at line 4034 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN2_Msk

#define PWM_INTEN_PIEN2_Msk (0x1ul << PWM_INTEN_PIEN2_Pos)

PWM_T::INTEN: PIEN2 Mask

Definition at line 4038 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN2_Pos

#define PWM_INTEN_PIEN2_Pos (20)

PWM_T::INTEN: PIEN2 Position

Definition at line 4037 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN3_Msk

#define PWM_INTEN_PIEN3_Msk (0x1ul << PWM_INTEN_PIEN3_Pos)

PWM_T::INTEN: PIEN3 Mask

Definition at line 4041 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN3_Pos

#define PWM_INTEN_PIEN3_Pos (21)

PWM_T::INTEN: PIEN3 Position

Definition at line 4040 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN4_Msk

#define PWM_INTEN_PIEN4_Msk (0x1ul << PWM_INTEN_PIEN4_Pos)

PWM_T::INTEN: PIEN4 Mask

Definition at line 4044 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN4_Pos

#define PWM_INTEN_PIEN4_Pos (22)

PWM_T::INTEN: PIEN4 Position

Definition at line 4043 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN5_Msk

#define PWM_INTEN_PIEN5_Msk (0x1ul << PWM_INTEN_PIEN5_Pos)

PWM_T::INTEN: PIEN5 Mask

Definition at line 4047 of file Mini55Series.h.

## ◆ PWM_INTEN_PIEN5_Pos

#define PWM_INTEN_PIEN5_Pos (23)

PWM_T::INTEN: PIEN5 Position

Definition at line 4046 of file Mini55Series.h.

## ◆ PWM_INTEN_PINTTYPE_Msk

#define PWM_INTEN_PINTTYPE_Msk (0x1ul << PWM_INTEN_PINTTYPE_Pos)

PWM_T::INTEN: PINTTYPE Mask

Definition at line 4029 of file Mini55Series.h.

## ◆ PWM_INTEN_PINTTYPE_Pos

#define PWM_INTEN_PINTTYPE_Pos (17)

PWM_T::INTEN: PINTTYPE Position

Definition at line 4028 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN0_Msk

#define PWM_INTEN_ZIEN0_Msk (0x1ul << PWM_INTEN_ZIEN0_Pos)

PWM_T::INTEN: ZIEN0 Mask

Definition at line 3990 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN0_Pos

#define PWM_INTEN_ZIEN0_Pos (0)

PWM_T::INTEN: ZIEN0 Position

Definition at line 3989 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN1_Msk

#define PWM_INTEN_ZIEN1_Msk (0x1ul << PWM_INTEN_ZIEN1_Pos)

PWM_T::INTEN: ZIEN1 Mask

Definition at line 3993 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN1_Pos

#define PWM_INTEN_ZIEN1_Pos (1)

PWM_T::INTEN: ZIEN1 Position

Definition at line 3992 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN2_Msk

#define PWM_INTEN_ZIEN2_Msk (0x1ul << PWM_INTEN_ZIEN2_Pos)

PWM_T::INTEN: ZIEN2 Mask

Definition at line 3996 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN2_Pos

#define PWM_INTEN_ZIEN2_Pos (2)

PWM_T::INTEN: ZIEN2 Position

Definition at line 3995 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN3_Msk

#define PWM_INTEN_ZIEN3_Msk (0x1ul << PWM_INTEN_ZIEN3_Pos)

PWM_T::INTEN: ZIEN3 Mask

Definition at line 3999 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN3_Pos

#define PWM_INTEN_ZIEN3_Pos (3)

PWM_T::INTEN: ZIEN3 Position

Definition at line 3998 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN4_Msk

#define PWM_INTEN_ZIEN4_Msk (0x1ul << PWM_INTEN_ZIEN4_Pos)

PWM_T::INTEN: ZIEN4 Mask

Definition at line 4002 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN4_Pos

#define PWM_INTEN_ZIEN4_Pos (4)

PWM_T::INTEN: ZIEN4 Position

Definition at line 4001 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN5_Msk

#define PWM_INTEN_ZIEN5_Msk (0x1ul << PWM_INTEN_ZIEN5_Pos)

PWM_T::INTEN: ZIEN5 Mask

Definition at line 4005 of file Mini55Series.h.

## ◆ PWM_INTEN_ZIEN5_Pos

#define PWM_INTEN_ZIEN5_Pos (5)

PWM_T::INTEN: ZIEN5 Position

Definition at line 4004 of file Mini55Series.h.

## ◆ PWM_INTSTS_BRKIF0_Msk

#define PWM_INTSTS_BRKIF0_Msk (0x1ul << PWM_INTSTS_BRKIF0_Pos)

PWM_T::INTSTS: BRKIF0 Mask

Definition at line 4104 of file Mini55Series.h.

## ◆ PWM_INTSTS_BRKIF0_Pos

#define PWM_INTSTS_BRKIF0_Pos (16)

PWM_T::INTSTS: BRKIF0 Position

Definition at line 4103 of file Mini55Series.h.

## ◆ PWM_INTSTS_BRKIF1_Msk

#define PWM_INTSTS_BRKIF1_Msk (0x1ul << PWM_INTSTS_BRKIF1_Pos)

PWM_T::INTSTS: BRKIF1 Mask

Definition at line 4107 of file Mini55Series.h.

## ◆ PWM_INTSTS_BRKIF1_Pos

#define PWM_INTSTS_BRKIF1_Pos (17)

PWM_T::INTSTS: BRKIF1 Position

Definition at line 4106 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF0_Msk

#define PWM_INTSTS_CMPDIF0_Msk (0x1ul << PWM_INTSTS_CMPDIF0_Pos)

PWM_T::INTSTS: CMPDIF0 Mask

Definition at line 4086 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF0_Pos

#define PWM_INTSTS_CMPDIF0_Pos (8)

PWM_T::INTSTS: CMPDIF0 Position

Definition at line 4085 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF1_Msk

#define PWM_INTSTS_CMPDIF1_Msk (0x1ul << PWM_INTSTS_CMPDIF1_Pos)

PWM_T::INTSTS: CMPDIF1 Mask

Definition at line 4089 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF1_Pos

#define PWM_INTSTS_CMPDIF1_Pos (9)

PWM_T::INTSTS: CMPDIF1 Position

Definition at line 4088 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF2_Msk

#define PWM_INTSTS_CMPDIF2_Msk (0x1ul << PWM_INTSTS_CMPDIF2_Pos)

PWM_T::INTSTS: CMPDIF2 Mask

Definition at line 4092 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF2_Pos

#define PWM_INTSTS_CMPDIF2_Pos (10)

PWM_T::INTSTS: CMPDIF2 Position

Definition at line 4091 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF3_Msk

#define PWM_INTSTS_CMPDIF3_Msk (0x1ul << PWM_INTSTS_CMPDIF3_Pos)

PWM_T::INTSTS: CMPDIF3 Mask

Definition at line 4095 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF3_Pos

#define PWM_INTSTS_CMPDIF3_Pos (11)

PWM_T::INTSTS: CMPDIF3 Position

Definition at line 4094 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF4_Msk

#define PWM_INTSTS_CMPDIF4_Msk (0x1ul << PWM_INTSTS_CMPDIF4_Pos)

PWM_T::INTSTS: CMPDIF4 Mask

Definition at line 4098 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF4_Pos

#define PWM_INTSTS_CMPDIF4_Pos (12)

PWM_T::INTSTS: CMPDIF4 Position

Definition at line 4097 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF5_Msk

#define PWM_INTSTS_CMPDIF5_Msk (0x1ul << PWM_INTSTS_CMPDIF5_Pos)

PWM_T::INTSTS: CMPDIF5 Mask

Definition at line 4101 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPDIF5_Pos

#define PWM_INTSTS_CMPDIF5_Pos (13)

PWM_T::INTSTS: CMPDIF5 Position

Definition at line 4100 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF0_Msk

#define PWM_INTSTS_CMPUIF0_Msk (0x1ul << PWM_INTSTS_CMPUIF0_Pos)

PWM_T::INTSTS: CMPUIF0 Mask

Definition at line 4128 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF0_Pos

#define PWM_INTSTS_CMPUIF0_Pos (24)

PWM_T::INTSTS: CMPUIF0 Position

Definition at line 4127 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF1_Msk

#define PWM_INTSTS_CMPUIF1_Msk (0x1ul << PWM_INTSTS_CMPUIF1_Pos)

PWM_T::INTSTS: CMPUIF1 Mask

Definition at line 4131 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF1_Pos

#define PWM_INTSTS_CMPUIF1_Pos (25)

PWM_T::INTSTS: CMPUIF1 Position

Definition at line 4130 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF2_Msk

#define PWM_INTSTS_CMPUIF2_Msk (0x1ul << PWM_INTSTS_CMPUIF2_Pos)

PWM_T::INTSTS: CMPUIF2 Mask

Definition at line 4134 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF2_Pos

#define PWM_INTSTS_CMPUIF2_Pos (26)

PWM_T::INTSTS: CMPUIF2 Position

Definition at line 4133 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF3_Msk

#define PWM_INTSTS_CMPUIF3_Msk (0x1ul << PWM_INTSTS_CMPUIF3_Pos)

PWM_T::INTSTS: CMPUIF3 Mask

Definition at line 4137 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF3_Pos

#define PWM_INTSTS_CMPUIF3_Pos (27)

PWM_T::INTSTS: CMPUIF3 Position

Definition at line 4136 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF4_Msk

#define PWM_INTSTS_CMPUIF4_Msk (0x1ul << PWM_INTSTS_CMPUIF4_Pos)

PWM_T::INTSTS: CMPUIF4 Mask

Definition at line 4140 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF4_Pos

#define PWM_INTSTS_CMPUIF4_Pos (28)

PWM_T::INTSTS: CMPUIF4 Position

Definition at line 4139 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF5_Msk

#define PWM_INTSTS_CMPUIF5_Msk (0x1ul << PWM_INTSTS_CMPUIF5_Pos)

PWM_T::INTSTS: CMPUIF5 Mask

Definition at line 4143 of file Mini55Series.h.

## ◆ PWM_INTSTS_CMPUIF5_Pos

#define PWM_INTSTS_CMPUIF5_Pos (29)

PWM_T::INTSTS: CMPUIF5 Position

Definition at line 4142 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF0_Msk

#define PWM_INTSTS_PIF0_Msk (0x1ul << PWM_INTSTS_PIF0_Pos)

PWM_T::INTSTS: PIF0 Mask

Definition at line 4110 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF0_Pos

#define PWM_INTSTS_PIF0_Pos (18)

PWM_T::INTSTS: PIF0 Position

Definition at line 4109 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF1_Msk

#define PWM_INTSTS_PIF1_Msk (0x1ul << PWM_INTSTS_PIF1_Pos)

PWM_T::INTSTS: PIF1 Mask

Definition at line 4113 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF1_Pos

#define PWM_INTSTS_PIF1_Pos (19)

PWM_T::INTSTS: PIF1 Position

Definition at line 4112 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF2_Msk

#define PWM_INTSTS_PIF2_Msk (0x1ul << PWM_INTSTS_PIF2_Pos)

PWM_T::INTSTS: PIF2 Mask

Definition at line 4116 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF2_Pos

#define PWM_INTSTS_PIF2_Pos (20)

PWM_T::INTSTS: PIF2 Position

Definition at line 4115 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF3_Msk

#define PWM_INTSTS_PIF3_Msk (0x1ul << PWM_INTSTS_PIF3_Pos)

PWM_T::INTSTS: PIF3 Mask

Definition at line 4119 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF3_Pos

#define PWM_INTSTS_PIF3_Pos (21)

PWM_T::INTSTS: PIF3 Position

Definition at line 4118 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF4_Msk

#define PWM_INTSTS_PIF4_Msk (0x1ul << PWM_INTSTS_PIF4_Pos)

PWM_T::INTSTS: PIF4 Mask

Definition at line 4122 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF4_Pos

#define PWM_INTSTS_PIF4_Pos (22)

PWM_T::INTSTS: PIF4 Position

Definition at line 4121 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF5_Msk

#define PWM_INTSTS_PIF5_Msk (0x1ul << PWM_INTSTS_PIF5_Pos)

PWM_T::INTSTS: PIF5 Mask

Definition at line 4125 of file Mini55Series.h.

## ◆ PWM_INTSTS_PIF5_Pos

#define PWM_INTSTS_PIF5_Pos (23)

PWM_T::INTSTS: PIF5 Position

Definition at line 4124 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF0_Msk

#define PWM_INTSTS_ZIF0_Msk (0x1ul << PWM_INTSTS_ZIF0_Pos)

PWM_T::INTSTS: ZIF0 Mask

Definition at line 4068 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF0_Pos

#define PWM_INTSTS_ZIF0_Pos (0)

PWM_T::INTSTS: ZIF0 Position

Definition at line 4067 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF1_Msk

#define PWM_INTSTS_ZIF1_Msk (0x1ul << PWM_INTSTS_ZIF1_Pos)

PWM_T::INTSTS: ZIF1 Mask

Definition at line 4071 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF1_Pos

#define PWM_INTSTS_ZIF1_Pos (1)

PWM_T::INTSTS: ZIF1 Position

Definition at line 4070 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF2_Msk

#define PWM_INTSTS_ZIF2_Msk (0x1ul << PWM_INTSTS_ZIF2_Pos)

PWM_T::INTSTS: ZIF2 Mask

Definition at line 4074 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF2_Pos

#define PWM_INTSTS_ZIF2_Pos (2)

PWM_T::INTSTS: ZIF2 Position

Definition at line 4073 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF3_Msk

#define PWM_INTSTS_ZIF3_Msk (0x1ul << PWM_INTSTS_ZIF3_Pos)

PWM_T::INTSTS: ZIF3 Mask

Definition at line 4077 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF3_Pos

#define PWM_INTSTS_ZIF3_Pos (3)

PWM_T::INTSTS: ZIF3 Position

Definition at line 4076 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF4_Msk

#define PWM_INTSTS_ZIF4_Msk (0x1ul << PWM_INTSTS_ZIF4_Pos)

PWM_T::INTSTS: ZIF4 Mask

Definition at line 4080 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF4_Pos

#define PWM_INTSTS_ZIF4_Pos (4)

PWM_T::INTSTS: ZIF4 Position

Definition at line 4079 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF5_Msk

#define PWM_INTSTS_ZIF5_Msk (0x1ul << PWM_INTSTS_ZIF5_Pos)

PWM_T::INTSTS: ZIF5 Mask

Definition at line 4083 of file Mini55Series.h.

## ◆ PWM_INTSTS_ZIF5_Pos

#define PWM_INTSTS_ZIF5_Pos (5)

PWM_T::INTSTS: ZIF5 Position

Definition at line 4082 of file Mini55Series.h.

## ◆ PWM_PERIOD_PERIOD_Msk

#define PWM_PERIOD_PERIOD_Msk (0xfffful << PWM_PERIOD_PERIOD_Pos)

PWM_T::PERIOD: PERIOD Mask

Definition at line 3981 of file Mini55Series.h.

## ◆ PWM_PERIOD_PERIOD_Pos

#define PWM_PERIOD_PERIOD_Pos (0)

PWM_T::PERIOD: PERIOD Position

Definition at line 3980 of file Mini55Series.h.

## ◆ PWM_PHCHG_A0POSSEL_Msk

#define PWM_PHCHG_A0POSSEL_Msk (0x3ul << PWM_PHCHG_A0POSSEL_Pos)

PWM_T::PHCHG: A0POSSEL Mask

Definition at line 4443 of file Mini55Series.h.

## ◆ PWM_PHCHG_A0POSSEL_Pos

#define PWM_PHCHG_A0POSSEL_Pos (28)

PWM_T::PHCHG: A0POSSEL Position

Definition at line 4442 of file Mini55Series.h.

## ◆ PWM_PHCHG_A1POSSEL_Msk

#define PWM_PHCHG_A1POSSEL_Msk (0x3ul << PWM_PHCHG_A1POSSEL_Pos)

PWM_T::PHCHG: A1POSSEL Mask

Definition at line 4422 of file Mini55Series.h.

## ◆ PWM_PHCHG_A1POSSEL_Pos

#define PWM_PHCHG_A1POSSEL_Pos (20)

PWM_T::PHCHG: A1POSSEL Position

Definition at line 4421 of file Mini55Series.h.

## ◆ PWM_PHCHG_ACMP0TEN_Msk

#define PWM_PHCHG_ACMP0TEN_Msk (0x1ul << PWM_PHCHG_ACMP0TEN_Pos)

PWM_T::PHCHG: ACMP0TEN Mask

Definition at line 4449 of file Mini55Series.h.

## ◆ PWM_PHCHG_ACMP0TEN_Pos

#define PWM_PHCHG_ACMP0TEN_Pos (31)

PWM_T::PHCHG: ACMP0TEN Position

Definition at line 4448 of file Mini55Series.h.

## ◆ PWM_PHCHG_ACMP1TEN_Msk

#define PWM_PHCHG_ACMP1TEN_Msk (0x1ul << PWM_PHCHG_ACMP1TEN_Pos)

PWM_T::PHCHG: ACMP1TEN Mask

Definition at line 4428 of file Mini55Series.h.

## ◆ PWM_PHCHG_ACMP1TEN_Pos

#define PWM_PHCHG_ACMP1TEN_Pos (23)

PWM_T::PHCHG: ACMP1TEN Position

Definition at line 4427 of file Mini55Series.h.

## ◆ PWM_PHCHG_AUTOCLR0_Msk

#define PWM_PHCHG_AUTOCLR0_Msk (0x1ul << PWM_PHCHG_AUTOCLR0_Pos)

PWM_T::PHCHG: AUTOCLR0 Mask

Definition at line 4404 of file Mini55Series.h.

## ◆ PWM_PHCHG_AUTOCLR0_Pos

#define PWM_PHCHG_AUTOCLR0_Pos (14)

PWM_T::PHCHG: AUTOCLR0 Position

Definition at line 4403 of file Mini55Series.h.

## ◆ PWM_PHCHG_AUTOCLR1_Msk

#define PWM_PHCHG_AUTOCLR1_Msk (0x1ul << PWM_PHCHG_AUTOCLR1_Pos)

PWM_T::PHCHG: AUTOCLR1 Mask

Definition at line 4407 of file Mini55Series.h.

## ◆ PWM_PHCHG_AUTOCLR1_Pos

#define PWM_PHCHG_AUTOCLR1_Pos (15)

PWM_T::PHCHG: AUTOCLR1 Position

Definition at line 4406 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT0_Msk

#define PWM_PHCHG_MSKDAT0_Msk (0x1ul << PWM_PHCHG_MSKDAT0_Pos)

PWM_T::PHCHG: MSKDAT0 Mask

Definition at line 4362 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT0_Pos

#define PWM_PHCHG_MSKDAT0_Pos (0)

PWM_T::PHCHG: MSKDAT0 Position

Definition at line 4361 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT1_Msk

#define PWM_PHCHG_MSKDAT1_Msk (0x1ul << PWM_PHCHG_MSKDAT1_Pos)

PWM_T::PHCHG: MSKDAT1 Mask

Definition at line 4365 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT1_Pos

#define PWM_PHCHG_MSKDAT1_Pos (1)

PWM_T::PHCHG: MSKDAT1 Position

Definition at line 4364 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT2_Msk

#define PWM_PHCHG_MSKDAT2_Msk (0x1ul << PWM_PHCHG_MSKDAT2_Pos)

PWM_T::PHCHG: MSKDAT2 Mask

Definition at line 4368 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT2_Pos

#define PWM_PHCHG_MSKDAT2_Pos (2)

PWM_T::PHCHG: MSKDAT2 Position

Definition at line 4367 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT3_Msk

#define PWM_PHCHG_MSKDAT3_Msk (0x1ul << PWM_PHCHG_MSKDAT3_Pos)

PWM_T::PHCHG: MSKDAT3 Mask

Definition at line 4371 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT3_Pos

#define PWM_PHCHG_MSKDAT3_Pos (3)

PWM_T::PHCHG: MSKDAT3 Position

Definition at line 4370 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT4_Msk

#define PWM_PHCHG_MSKDAT4_Msk (0x1ul << PWM_PHCHG_MSKDAT4_Pos)

PWM_T::PHCHG: MSKDAT4 Mask

Definition at line 4374 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT4_Pos

#define PWM_PHCHG_MSKDAT4_Pos (4)

PWM_T::PHCHG: MSKDAT4 Position

Definition at line 4373 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT5_Msk

#define PWM_PHCHG_MSKDAT5_Msk (0x1ul << PWM_PHCHG_MSKDAT5_Pos)

PWM_T::PHCHG: MSKDAT5 Mask

Definition at line 4377 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT5_Pos

#define PWM_PHCHG_MSKDAT5_Pos (5)

PWM_T::PHCHG: MSKDAT5 Position

Definition at line 4376 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT6_Msk

#define PWM_PHCHG_MSKDAT6_Msk (0x1ul << PWM_PHCHG_MSKDAT6_Pos)

PWM_T::PHCHG: MSKDAT6 Mask

Definition at line 4380 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT6_Pos

#define PWM_PHCHG_MSKDAT6_Pos (6)

PWM_T::PHCHG: MSKDAT6 Position

Definition at line 4379 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT7_Msk

#define PWM_PHCHG_MSKDAT7_Msk (0x1ul << PWM_PHCHG_MSKDAT7_Pos)

PWM_T::PHCHG: MSKDAT7 Mask

Definition at line 4383 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKDAT7_Pos

#define PWM_PHCHG_MSKDAT7_Pos (7)

PWM_T::PHCHG: MSKDAT7 Position

Definition at line 4382 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN0_Msk

#define PWM_PHCHG_MSKEN0_Msk (0x1ul << PWM_PHCHG_MSKEN0_Pos)

PWM_T::PHCHG: MSKEN0 Mask

Definition at line 4386 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN0_Pos

#define PWM_PHCHG_MSKEN0_Pos (8)

PWM_T::PHCHG: MSKEN0 Position

Definition at line 4385 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN1_Msk

#define PWM_PHCHG_MSKEN1_Msk (0x1ul << PWM_PHCHG_MSKEN1_Pos)

PWM_T::PHCHG: MSKEN1 Mask

Definition at line 4389 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN1_Pos

#define PWM_PHCHG_MSKEN1_Pos (9)

PWM_T::PHCHG: MSKEN1 Position

Definition at line 4388 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN2_Msk

#define PWM_PHCHG_MSKEN2_Msk (0x1ul << PWM_PHCHG_MSKEN2_Pos)

PWM_T::PHCHG: MSKEN2 Mask

Definition at line 4392 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN2_Pos

#define PWM_PHCHG_MSKEN2_Pos (10)

PWM_T::PHCHG: MSKEN2 Position

Definition at line 4391 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN3_Msk

#define PWM_PHCHG_MSKEN3_Msk (0x1ul << PWM_PHCHG_MSKEN3_Pos)

PWM_T::PHCHG: MSKEN3 Mask

Definition at line 4395 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN3_Pos

#define PWM_PHCHG_MSKEN3_Pos (11)

PWM_T::PHCHG: MSKEN3 Position

Definition at line 4394 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN4_Msk

#define PWM_PHCHG_MSKEN4_Msk (0x1ul << PWM_PHCHG_MSKEN4_Pos)

PWM_T::PHCHG: MSKEN4 Mask

Definition at line 4398 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN4_Pos

#define PWM_PHCHG_MSKEN4_Pos (12)

PWM_T::PHCHG: MSKEN4 Position

Definition at line 4397 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN5_Msk

#define PWM_PHCHG_MSKEN5_Msk (0x1ul << PWM_PHCHG_MSKEN5_Pos)

PWM_T::PHCHG: MSKEN5 Mask

Definition at line 4401 of file Mini55Series.h.

## ◆ PWM_PHCHG_MSKEN5_Pos

#define PWM_PHCHG_MSKEN5_Pos (13)

PWM_T::PHCHG: MSKEN5 Position

Definition at line 4400 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN00_Msk

#define PWM_PHCHG_OFFEN00_Msk (0x1ul << PWM_PHCHG_OFFEN00_Pos)

PWM_T::PHCHG: OFFEN00 Mask

Definition at line 4431 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN00_Pos

#define PWM_PHCHG_OFFEN00_Pos (24)

PWM_T::PHCHG: OFFEN00 Position

Definition at line 4430 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN01_Msk

#define PWM_PHCHG_OFFEN01_Msk (0x1ul << PWM_PHCHG_OFFEN01_Pos)

PWM_T::PHCHG: OFFEN01 Mask

Definition at line 4410 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN01_Pos

#define PWM_PHCHG_OFFEN01_Pos (16)

PWM_T::PHCHG: OFFEN01 Position

Definition at line 4409 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN10_Msk

#define PWM_PHCHG_OFFEN10_Msk (0x1ul << PWM_PHCHG_OFFEN10_Pos)

PWM_T::PHCHG: OFFEN10 Mask

Definition at line 4434 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN10_Pos

#define PWM_PHCHG_OFFEN10_Pos (25)

PWM_T::PHCHG: OFFEN10 Position

Definition at line 4433 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN11_Msk

#define PWM_PHCHG_OFFEN11_Msk (0x1ul << PWM_PHCHG_OFFEN11_Pos)

PWM_T::PHCHG: OFFEN11 Mask

Definition at line 4413 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN11_Pos

#define PWM_PHCHG_OFFEN11_Pos (17)

PWM_T::PHCHG: OFFEN11 Position

Definition at line 4412 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN20_Msk

#define PWM_PHCHG_OFFEN20_Msk (0x1ul << PWM_PHCHG_OFFEN20_Pos)

PWM_T::PHCHG: OFFEN20 Mask

Definition at line 4437 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN20_Pos

#define PWM_PHCHG_OFFEN20_Pos (26)

PWM_T::PHCHG: OFFEN20 Position

Definition at line 4436 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN21_Msk

#define PWM_PHCHG_OFFEN21_Msk (0x1ul << PWM_PHCHG_OFFEN21_Pos)

PWM_T::PHCHG: OFFEN21 Mask

Definition at line 4416 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN21_Pos

#define PWM_PHCHG_OFFEN21_Pos (18)

PWM_T::PHCHG: OFFEN21 Position

Definition at line 4415 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN30_Msk

#define PWM_PHCHG_OFFEN30_Msk (0x1ul << PWM_PHCHG_OFFEN30_Pos)

PWM_T::PHCHG: OFFEN30 Mask

Definition at line 4440 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN30_Pos

#define PWM_PHCHG_OFFEN30_Pos (27)

PWM_T::PHCHG: OFFEN30 Position

Definition at line 4439 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN31_Msk

#define PWM_PHCHG_OFFEN31_Msk (0x1ul << PWM_PHCHG_OFFEN31_Pos)

PWM_T::PHCHG: OFFEN31 Mask

Definition at line 4419 of file Mini55Series.h.

## ◆ PWM_PHCHG_OFFEN31_Pos

#define PWM_PHCHG_OFFEN31_Pos (19)

PWM_T::PHCHG: OFFEN31 Position

Definition at line 4418 of file Mini55Series.h.

## ◆ PWM_PHCHG_T0_Msk

#define PWM_PHCHG_T0_Msk (0x1ul << PWM_PHCHG_T0_Pos)

PWM_T::PHCHG: T0 Mask

Definition at line 4446 of file Mini55Series.h.

## ◆ PWM_PHCHG_T0_Pos

#define PWM_PHCHG_T0_Pos (30)

PWM_T::PHCHG: T0 Position

Definition at line 4445 of file Mini55Series.h.

## ◆ PWM_PHCHG_TMR1TEN_Msk

#define PWM_PHCHG_TMR1TEN_Msk (0x1ul << PWM_PHCHG_TMR1TEN_Pos)

PWM_T::PHCHG: TMR1TEN Mask

Definition at line 4425 of file Mini55Series.h.

## ◆ PWM_PHCHG_TMR1TEN_Pos

#define PWM_PHCHG_TMR1TEN_Pos (22)

PWM_T::PHCHG: TMR1TEN Position

Definition at line 4424 of file Mini55Series.h.

## ◆ PWM_PHCHGMSK_MASKEND6_Msk

#define PWM_PHCHGMSK_MASKEND6_Msk (0x1ul << PWM_PHCHGMSK_MASKEND6_Pos)

PWM_T::PHCHGMSK: MASKEND6 Mask

Definition at line 4542 of file Mini55Series.h.

## ◆ PWM_PHCHGMSK_MASKEND6_Pos

#define PWM_PHCHGMSK_MASKEND6_Pos (6)

PWM_T::PHCHGMSK: MASKEND6 Position

Definition at line 4541 of file Mini55Series.h.

## ◆ PWM_PHCHGMSK_MASKEND7_Msk

#define PWM_PHCHGMSK_MASKEND7_Msk (0x1ul << PWM_PHCHGMSK_MASKEND7_Pos)

PWM_T::PHCHGMSK: MASKEND7 Mask

Definition at line 4545 of file Mini55Series.h.

## ◆ PWM_PHCHGMSK_MASKEND7_Pos

#define PWM_PHCHGMSK_MASKEND7_Pos (7)

PWM_T::PHCHGMSK: MASKEND7 Position

Definition at line 4544 of file Mini55Series.h.

## ◆ PWM_PHCHGMSK_POSCTL0_Msk

#define PWM_PHCHGMSK_POSCTL0_Msk (0x1ul << PWM_PHCHGMSK_POSCTL0_Pos)

PWM_T::PHCHGMSK: POSCTL0 Mask

Definition at line 4548 of file Mini55Series.h.

## ◆ PWM_PHCHGMSK_POSCTL0_Pos

#define PWM_PHCHGMSK_POSCTL0_Pos (8)

PWM_T::PHCHGMSK: POSCTL0 Position

Definition at line 4547 of file Mini55Series.h.

## ◆ PWM_PHCHGMSK_POSCTL1_Msk

#define PWM_PHCHGMSK_POSCTL1_Msk (0x1ul << PWM_PHCHGMSK_POSCTL1_Pos)

PWM_T::PHCHGMSK: POSCTL1 Mask

Definition at line 4551 of file Mini55Series.h.

## ◆ PWM_PHCHGMSK_POSCTL1_Pos

#define PWM_PHCHGMSK_POSCTL1_Pos (9)

PWM_T::PHCHGMSK: POSCTL1 Position

Definition at line 4550 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_A0POSSEL_Msk

#define PWM_PHCHGNXT_A0POSSEL_Msk (0x3ul << PWM_PHCHGNXT_A0POSSEL_Pos)

PWM_T::PHCHGNXT: A0POSSEL Mask

Definition at line 4533 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_A0POSSEL_Pos

#define PWM_PHCHGNXT_A0POSSEL_Pos (28)

PWM_T::PHCHGNXT: A0POSSEL Position

Definition at line 4532 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_A1POSSEL_Msk

#define PWM_PHCHGNXT_A1POSSEL_Msk (0x3ul << PWM_PHCHGNXT_A1POSSEL_Pos)

PWM_T::PHCHGNXT: A1POSSEL Mask

Definition at line 4512 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_A1POSSEL_Pos

#define PWM_PHCHGNXT_A1POSSEL_Pos (20)

PWM_T::PHCHGNXT: A1POSSEL Position

Definition at line 4511 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_ACMP0TEN_Msk

#define PWM_PHCHGNXT_ACMP0TEN_Msk (0x1ul << PWM_PHCHGNXT_ACMP0TEN_Pos)

PWM_T::PHCHGNXT: ACMP0TEN Mask

Definition at line 4539 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_ACMP0TEN_Pos

#define PWM_PHCHGNXT_ACMP0TEN_Pos (31)

PWM_T::PHCHGNXT: ACMP0TEN Position

Definition at line 4538 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_ACMP1TEN_Msk

#define PWM_PHCHGNXT_ACMP1TEN_Msk (0x1ul << PWM_PHCHGNXT_ACMP1TEN_Pos)

PWM_T::PHCHGNXT: ACMP1TEN Mask

Definition at line 4518 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_ACMP1TEN_Pos

#define PWM_PHCHGNXT_ACMP1TEN_Pos (23)

PWM_T::PHCHGNXT: ACMP1TEN Position

Definition at line 4517 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_AUTOCLR0_Msk

#define PWM_PHCHGNXT_AUTOCLR0_Msk (0x1ul << PWM_PHCHGNXT_AUTOCLR0_Pos)

PWM_T::PHCHGNXT: AUTOCLR0 Mask

Definition at line 4494 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_AUTOCLR0_Pos

#define PWM_PHCHGNXT_AUTOCLR0_Pos (14)

PWM_T::PHCHGNXT: AUTOCLR0 Position

Definition at line 4493 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_AUTOCLR1_Msk

#define PWM_PHCHGNXT_AUTOCLR1_Msk (0x1ul << PWM_PHCHGNXT_AUTOCLR1_Pos)

PWM_T::PHCHGNXT: AUTOCLR1 Mask

Definition at line 4497 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_AUTOCLR1_Pos

#define PWM_PHCHGNXT_AUTOCLR1_Pos (15)

PWM_T::PHCHGNXT: AUTOCLR1 Position

Definition at line 4496 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT0_Msk

#define PWM_PHCHGNXT_MSKDAT0_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT0_Pos)

PWM_T::PHCHGNXT: MSKDAT0 Mask

Definition at line 4452 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT0_Pos

#define PWM_PHCHGNXT_MSKDAT0_Pos (0)

PWM_T::PHCHGNXT: MSKDAT0 Position

Definition at line 4451 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT1_Msk

#define PWM_PHCHGNXT_MSKDAT1_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT1_Pos)

PWM_T::PHCHGNXT: MSKDAT1 Mask

Definition at line 4455 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT1_Pos

#define PWM_PHCHGNXT_MSKDAT1_Pos (1)

PWM_T::PHCHGNXT: MSKDAT1 Position

Definition at line 4454 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT2_Msk

#define PWM_PHCHGNXT_MSKDAT2_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT2_Pos)

PWM_T::PHCHGNXT: MSKDAT2 Mask

Definition at line 4458 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT2_Pos

#define PWM_PHCHGNXT_MSKDAT2_Pos (2)

PWM_T::PHCHGNXT: MSKDAT2 Position

Definition at line 4457 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT3_Msk

#define PWM_PHCHGNXT_MSKDAT3_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT3_Pos)

PWM_T::PHCHGNXT: MSKDAT3 Mask

Definition at line 4461 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT3_Pos

#define PWM_PHCHGNXT_MSKDAT3_Pos (3)

PWM_T::PHCHGNXT: MSKDAT3 Position

Definition at line 4460 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT4_Msk

#define PWM_PHCHGNXT_MSKDAT4_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT4_Pos)

PWM_T::PHCHGNXT: MSKDAT4 Mask

Definition at line 4464 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT4_Pos

#define PWM_PHCHGNXT_MSKDAT4_Pos (4)

PWM_T::PHCHGNXT: MSKDAT4 Position

Definition at line 4463 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT5_Msk

#define PWM_PHCHGNXT_MSKDAT5_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT5_Pos)

PWM_T::PHCHGNXT: MSKDAT5 Mask

Definition at line 4467 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT5_Pos

#define PWM_PHCHGNXT_MSKDAT5_Pos (5)

PWM_T::PHCHGNXT: MSKDAT5 Position

Definition at line 4466 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT6_Msk

#define PWM_PHCHGNXT_MSKDAT6_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT6_Pos)

PWM_T::PHCHGNXT: MSKDAT6 Mask

Definition at line 4470 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT6_Pos

#define PWM_PHCHGNXT_MSKDAT6_Pos (6)

PWM_T::PHCHGNXT: MSKDAT6 Position

Definition at line 4469 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT7_Msk

#define PWM_PHCHGNXT_MSKDAT7_Msk (0x1ul << PWM_PHCHGNXT_MSKDAT7_Pos)

PWM_T::PHCHGNXT: MSKDAT7 Mask

Definition at line 4473 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKDAT7_Pos

#define PWM_PHCHGNXT_MSKDAT7_Pos (7)

PWM_T::PHCHGNXT: MSKDAT7 Position

Definition at line 4472 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN0_Msk

#define PWM_PHCHGNXT_MSKEN0_Msk (0x1ul << PWM_PHCHGNXT_MSKEN0_Pos)

PWM_T::PHCHGNXT: MSKEN0 Mask

Definition at line 4476 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN0_Pos

#define PWM_PHCHGNXT_MSKEN0_Pos (8)

PWM_T::PHCHGNXT: MSKEN0 Position

Definition at line 4475 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN1_Msk

#define PWM_PHCHGNXT_MSKEN1_Msk (0x1ul << PWM_PHCHGNXT_MSKEN1_Pos)

PWM_T::PHCHGNXT: MSKEN1 Mask

Definition at line 4479 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN1_Pos

#define PWM_PHCHGNXT_MSKEN1_Pos (9)

PWM_T::PHCHGNXT: MSKEN1 Position

Definition at line 4478 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN2_Msk

#define PWM_PHCHGNXT_MSKEN2_Msk (0x1ul << PWM_PHCHGNXT_MSKEN2_Pos)

PWM_T::PHCHGNXT: MSKEN2 Mask

Definition at line 4482 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN2_Pos

#define PWM_PHCHGNXT_MSKEN2_Pos (10)

PWM_T::PHCHGNXT: MSKEN2 Position

Definition at line 4481 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN3_Msk

#define PWM_PHCHGNXT_MSKEN3_Msk (0x1ul << PWM_PHCHGNXT_MSKEN3_Pos)

PWM_T::PHCHGNXT: MSKEN3 Mask

Definition at line 4485 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN3_Pos

#define PWM_PHCHGNXT_MSKEN3_Pos (11)

PWM_T::PHCHGNXT: MSKEN3 Position

Definition at line 4484 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN4_Msk

#define PWM_PHCHGNXT_MSKEN4_Msk (0x1ul << PWM_PHCHGNXT_MSKEN4_Pos)

PWM_T::PHCHGNXT: MSKEN4 Mask

Definition at line 4488 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN4_Pos

#define PWM_PHCHGNXT_MSKEN4_Pos (12)

PWM_T::PHCHGNXT: MSKEN4 Position

Definition at line 4487 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN5_Msk

#define PWM_PHCHGNXT_MSKEN5_Msk (0x1ul << PWM_PHCHGNXT_MSKEN5_Pos)

PWM_T::PHCHGNXT: MSKEN5 Mask

Definition at line 4491 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_MSKEN5_Pos

#define PWM_PHCHGNXT_MSKEN5_Pos (13)

PWM_T::PHCHGNXT: MSKEN5 Position

Definition at line 4490 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN00_Msk

#define PWM_PHCHGNXT_OFFEN00_Msk (0x1ul << PWM_PHCHGNXT_OFFEN00_Pos)

PWM_T::PHCHGNXT: OFFEN00 Mask

Definition at line 4521 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN00_Pos

#define PWM_PHCHGNXT_OFFEN00_Pos (24)

PWM_T::PHCHGNXT: OFFEN00 Position

Definition at line 4520 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN01_Msk

#define PWM_PHCHGNXT_OFFEN01_Msk (0x1ul << PWM_PHCHGNXT_OFFEN01_Pos)

PWM_T::PHCHGNXT: OFFEN01 Mask

Definition at line 4500 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN01_Pos

#define PWM_PHCHGNXT_OFFEN01_Pos (16)

PWM_T::PHCHGNXT: OFFEN01 Position

Definition at line 4499 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN10_Msk

#define PWM_PHCHGNXT_OFFEN10_Msk (0x1ul << PWM_PHCHGNXT_OFFEN10_Pos)

PWM_T::PHCHGNXT: OFFEN10 Mask

Definition at line 4524 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN10_Pos

#define PWM_PHCHGNXT_OFFEN10_Pos (25)

PWM_T::PHCHGNXT: OFFEN10 Position

Definition at line 4523 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN11_Msk

#define PWM_PHCHGNXT_OFFEN11_Msk (0x1ul << PWM_PHCHGNXT_OFFEN11_Pos)

PWM_T::PHCHGNXT: OFFEN11 Mask

Definition at line 4503 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN11_Pos

#define PWM_PHCHGNXT_OFFEN11_Pos (17)

PWM_T::PHCHGNXT: OFFEN11 Position

Definition at line 4502 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN20_Msk

#define PWM_PHCHGNXT_OFFEN20_Msk (0x1ul << PWM_PHCHGNXT_OFFEN20_Pos)

PWM_T::PHCHGNXT: OFFEN20 Mask

Definition at line 4527 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN20_Pos

#define PWM_PHCHGNXT_OFFEN20_Pos (26)

PWM_T::PHCHGNXT: OFFEN20 Position

Definition at line 4526 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN21_Msk

#define PWM_PHCHGNXT_OFFEN21_Msk (0x1ul << PWM_PHCHGNXT_OFFEN21_Pos)

PWM_T::PHCHGNXT: OFFEN21 Mask

Definition at line 4506 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN21_Pos

#define PWM_PHCHGNXT_OFFEN21_Pos (18)

PWM_T::PHCHGNXT: OFFEN21 Position

Definition at line 4505 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN30_Msk

#define PWM_PHCHGNXT_OFFEN30_Msk (0x1ul << PWM_PHCHGNXT_OFFEN30_Pos)

PWM_T::PHCHGNXT: OFFEN30 Mask

Definition at line 4530 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN30_Pos

#define PWM_PHCHGNXT_OFFEN30_Pos (27)

PWM_T::PHCHGNXT: OFFEN30 Position

Definition at line 4529 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN31_Msk

#define PWM_PHCHGNXT_OFFEN31_Msk (0x1ul << PWM_PHCHGNXT_OFFEN31_Pos)

PWM_T::PHCHGNXT: OFFEN31 Mask

Definition at line 4509 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_OFFEN31_Pos

#define PWM_PHCHGNXT_OFFEN31_Pos (19)

PWM_T::PHCHGNXT: OFFEN31 Position

Definition at line 4508 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_TMR0TEN_Msk

#define PWM_PHCHGNXT_TMR0TEN_Msk (0x1ul << PWM_PHCHGNXT_TMR0TEN_Pos)

PWM_T::PHCHGNXT: TMR0TEN Mask

Definition at line 4536 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_TMR0TEN_Pos

#define PWM_PHCHGNXT_TMR0TEN_Pos (30)

PWM_T::PHCHGNXT: TMR0TEN Position

Definition at line 4535 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_TMR1TEN_Msk

#define PWM_PHCHGNXT_TMR1TEN_Msk (0x1ul << PWM_PHCHGNXT_TMR1TEN_Pos)

PWM_T::PHCHGNXT: TMR1TEN Mask

Definition at line 4515 of file Mini55Series.h.

## ◆ PWM_PHCHGNXT_TMR1TEN_Pos

#define PWM_PHCHGNXT_TMR1TEN_Pos (22)

PWM_T::PHCHGNXT: TMR1TEN Position

Definition at line 4514 of file Mini55Series.h.

## ◆ PWM_POEN_POEN0_Msk

#define PWM_POEN_POEN0_Msk (0x1ul << PWM_POEN_POEN0_Pos)

PWM_T::POEN: POEN0 Mask

Definition at line 4146 of file Mini55Series.h.

## ◆ PWM_POEN_POEN0_Pos

#define PWM_POEN_POEN0_Pos (0)

PWM_T::POEN: POEN0 Position

Definition at line 4145 of file Mini55Series.h.

## ◆ PWM_POEN_POEN1_Msk

#define PWM_POEN_POEN1_Msk (0x1ul << PWM_POEN_POEN1_Pos)

PWM_T::POEN: POEN1 Mask

Definition at line 4149 of file Mini55Series.h.

## ◆ PWM_POEN_POEN1_Pos

#define PWM_POEN_POEN1_Pos (1)

PWM_T::POEN: POEN1 Position

Definition at line 4148 of file Mini55Series.h.

## ◆ PWM_POEN_POEN2_Msk

#define PWM_POEN_POEN2_Msk (0x1ul << PWM_POEN_POEN2_Pos)

PWM_T::POEN: POEN2 Mask

Definition at line 4152 of file Mini55Series.h.

## ◆ PWM_POEN_POEN2_Pos

#define PWM_POEN_POEN2_Pos (2)

PWM_T::POEN: POEN2 Position

Definition at line 4151 of file Mini55Series.h.

## ◆ PWM_POEN_POEN3_Msk

#define PWM_POEN_POEN3_Msk (0x1ul << PWM_POEN_POEN3_Pos)

PWM_T::POEN: POEN3 Mask

Definition at line 4155 of file Mini55Series.h.

## ◆ PWM_POEN_POEN3_Pos

#define PWM_POEN_POEN3_Pos (3)

PWM_T::POEN: POEN3 Position

Definition at line 4154 of file Mini55Series.h.

## ◆ PWM_POEN_POEN4_Msk

#define PWM_POEN_POEN4_Msk (0x1ul << PWM_POEN_POEN4_Pos)

PWM_T::POEN: POEN4 Mask

Definition at line 4158 of file Mini55Series.h.

## ◆ PWM_POEN_POEN4_Pos

#define PWM_POEN_POEN4_Pos (4)

PWM_T::POEN: POEN4 Position

Definition at line 4157 of file Mini55Series.h.

## ◆ PWM_POEN_POEN5_Msk

#define PWM_POEN_POEN5_Msk (0x1ul << PWM_POEN_POEN5_Pos)

PWM_T::POEN: POEN5 Mask

Definition at line 4161 of file Mini55Series.h.

## ◆ PWM_POEN_POEN5_Pos

#define PWM_POEN_POEN5_Pos (5)

PWM_T::POEN: POEN5 Position

Definition at line 4160 of file Mini55Series.h.

## ◆ SPI_CLKDIV_DIVIDER_Msk

#define SPI_CLKDIV_DIVIDER_Msk (0xfful << SPI_CLKDIV_DIVIDER_Pos)

SPI_T::CLKDIV: DIVIDER Mask

Definition at line 4947 of file Mini55Series.h.

## ◆ SPI_CLKDIV_DIVIDER_Pos

#define SPI_CLKDIV_DIVIDER_Pos (0)

SPI_T::CLKDIV: DIVIDER Position

Definition at line 4946 of file Mini55Series.h.

## ◆ SPI_CTL_CLKPOL_Msk

#define SPI_CTL_CLKPOL_Msk (0x1ul << SPI_CTL_CLKPOL_Pos)

SPI_T::CTL: CLKPOL Mask

Definition at line 4914 of file Mini55Series.h.

## ◆ SPI_CTL_CLKPOL_Pos

#define SPI_CTL_CLKPOL_Pos (11)

SPI_T::CTL: CLKPOL Position

Definition at line 4913 of file Mini55Series.h.

## ◆ SPI_CTL_DWIDTH_Msk

#define SPI_CTL_DWIDTH_Msk (0x1ful << SPI_CTL_DWIDTH_Pos)

SPI_T::CTL: DWIDTH Mask

Definition at line 4908 of file Mini55Series.h.

## ◆ SPI_CTL_DWIDTH_Pos

#define SPI_CTL_DWIDTH_Pos (3)

SPI_T::CTL: DWIDTH Position

Definition at line 4907 of file Mini55Series.h.

## ◆ SPI_CTL_FIFOEN_Msk

#define SPI_CTL_FIFOEN_Msk (0x1ul << SPI_CTL_FIFOEN_Pos)

SPI_T::CTL: FIFOEN Mask

Definition at line 4932 of file Mini55Series.h.

## ◆ SPI_CTL_FIFOEN_Pos

#define SPI_CTL_FIFOEN_Pos (21)

SPI_T::CTL: FIFOEN Position

Definition at line 4931 of file Mini55Series.h.

## ◆ SPI_CTL_LSB_Msk

#define SPI_CTL_LSB_Msk (0x1ul << SPI_CTL_LSB_Pos)

SPI_T::CTL: LSB Mask

Definition at line 4911 of file Mini55Series.h.

## ◆ SPI_CTL_LSB_Pos

#define SPI_CTL_LSB_Pos (10)

SPI_T::CTL: LSB Position

Definition at line 4910 of file Mini55Series.h.

## ◆ SPI_CTL_REORDER_Msk

#define SPI_CTL_REORDER_Msk (0x1ul << SPI_CTL_REORDER_Pos)

SPI_T::CTL: REORDER Mask

Definition at line 4929 of file Mini55Series.h.

## ◆ SPI_CTL_REORDER_Pos

#define SPI_CTL_REORDER_Pos (19)

SPI_T::CTL: REORDER Position

Definition at line 4928 of file Mini55Series.h.

## ◆ SPI_CTL_RXEMPTY_Msk

#define SPI_CTL_RXEMPTY_Msk (0x1ul << SPI_CTL_RXEMPTY_Pos)

SPI_T::CTL: RXEMPTY Mask

Definition at line 4935 of file Mini55Series.h.

## ◆ SPI_CTL_RXEMPTY_Pos

#define SPI_CTL_RXEMPTY_Pos (24)

SPI_T::CTL: RXEMPTY Position

Definition at line 4934 of file Mini55Series.h.

## ◆ SPI_CTL_RXFULL_Msk

#define SPI_CTL_RXFULL_Msk (0x1ul << SPI_CTL_RXFULL_Pos)

SPI_T::CTL: RXFULL Mask

Definition at line 4938 of file Mini55Series.h.

## ◆ SPI_CTL_RXFULL_Pos

#define SPI_CTL_RXFULL_Pos (25)

SPI_T::CTL: RXFULL Position

Definition at line 4937 of file Mini55Series.h.

## ◆ SPI_CTL_RXNEG_Msk

#define SPI_CTL_RXNEG_Msk (0x1ul << SPI_CTL_RXNEG_Pos)

SPI_T::CTL: RXNEG Mask

Definition at line 4902 of file Mini55Series.h.

## ◆ SPI_CTL_RXNEG_Pos

#define SPI_CTL_RXNEG_Pos (1)

SPI_T::CTL: RXNEG Position

Definition at line 4901 of file Mini55Series.h.

## ◆ SPI_CTL_SLAVE_Msk

#define SPI_CTL_SLAVE_Msk (0x1ul << SPI_CTL_SLAVE_Pos)

SPI_T::CTL: SLAVE Mask

Definition at line 4926 of file Mini55Series.h.

## ◆ SPI_CTL_SLAVE_Pos

#define SPI_CTL_SLAVE_Pos (18)

SPI_T::CTL: SLAVE Position

Definition at line 4925 of file Mini55Series.h.

## ◆ SPI_CTL_SPIEN_Msk

#define SPI_CTL_SPIEN_Msk (0x1ul << SPI_CTL_SPIEN_Pos)

SPI_T::CTL: SPIEN Mask

Definition at line 4899 of file Mini55Series.h.

## ◆ SPI_CTL_SPIEN_Pos

#define SPI_CTL_SPIEN_Pos (0)

    @addtogroup SPI_CONST SPI Bit Field Definition
    Constant Definitions for SPI Controller

SPI_T::CTL: SPIEN Position

Definition at line 4898 of file Mini55Series.h.

## ◆ SPI_CTL_SUSPITV_Msk

#define SPI_CTL_SUSPITV_Msk (0xful << SPI_CTL_SUSPITV_Pos)

SPI_T::CTL: SUSPITV Mask

Definition at line 4917 of file Mini55Series.h.

## ◆ SPI_CTL_SUSPITV_Pos

#define SPI_CTL_SUSPITV_Pos (12)

SPI_T::CTL: SUSPITV Position

Definition at line 4916 of file Mini55Series.h.

## ◆ SPI_CTL_TXEMPTY_Msk

#define SPI_CTL_TXEMPTY_Msk (0x1ul << SPI_CTL_TXEMPTY_Pos)

SPI_T::CTL: TXEMPTY Mask

Definition at line 4941 of file Mini55Series.h.

## ◆ SPI_CTL_TXEMPTY_Pos

#define SPI_CTL_TXEMPTY_Pos (26)

SPI_T::CTL: TXEMPTY Position

Definition at line 4940 of file Mini55Series.h.

## ◆ SPI_CTL_TXFULL_Msk

#define SPI_CTL_TXFULL_Msk (0x1ul << SPI_CTL_TXFULL_Pos)

SPI_T::CTL: TXFULL Mask

Definition at line 4944 of file Mini55Series.h.

## ◆ SPI_CTL_TXFULL_Pos

#define SPI_CTL_TXFULL_Pos (27)

SPI_T::CTL: TXFULL Position

Definition at line 4943 of file Mini55Series.h.

## ◆ SPI_CTL_TXNEG_Msk

#define SPI_CTL_TXNEG_Msk (0x1ul << SPI_CTL_TXNEG_Pos)

SPI_T::CTL: TXNEG Mask

Definition at line 4905 of file Mini55Series.h.

## ◆ SPI_CTL_TXNEG_Pos

#define SPI_CTL_TXNEG_Pos (2)

SPI_T::CTL: TXNEG Position

Definition at line 4904 of file Mini55Series.h.

## ◆ SPI_CTL_UNITIEN_Msk

#define SPI_CTL_UNITIEN_Msk (0x1ul << SPI_CTL_UNITIEN_Pos)

SPI_T::CTL: UNITIEN Mask

Definition at line 4923 of file Mini55Series.h.

## ◆ SPI_CTL_UNITIEN_Pos

#define SPI_CTL_UNITIEN_Pos (17)

SPI_T::CTL: UNITIEN Position

Definition at line 4922 of file Mini55Series.h.

## ◆ SPI_CTL_UNITIF_Msk

#define SPI_CTL_UNITIF_Msk (0x1ul << SPI_CTL_UNITIF_Pos)

SPI_T::CTL: UNITIF Mask

Definition at line 4920 of file Mini55Series.h.

## ◆ SPI_CTL_UNITIF_Pos

#define SPI_CTL_UNITIF_Pos (16)

SPI_T::CTL: UNITIF Position

Definition at line 4919 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXOVIEN_Msk

#define SPI_FIFOCTL_RXOVIEN_Msk (0x1ul << SPI_FIFOCTL_RXOVIEN_Pos)

SPI_T::FIFOCTL: RXOVIEN Mask

Definition at line 5001 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXOVIEN_Pos

#define SPI_FIFOCTL_RXOVIEN_Pos (6)

SPI_T::FIFOCTL: RXOVIEN Position

Definition at line 5000 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXRST_Msk

#define SPI_FIFOCTL_RXRST_Msk (0x1ul << SPI_FIFOCTL_RXRST_Pos)

SPI_T::FIFOCTL: RXRST Mask

Definition at line 4989 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXRST_Pos

#define SPI_FIFOCTL_RXRST_Pos (0)

SPI_T::FIFOCTL: RXRST Position

Definition at line 4988 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXTH_Msk

#define SPI_FIFOCTL_RXTH_Msk (0x3ul << SPI_FIFOCTL_RXTH_Pos)

SPI_T::FIFOCTL: RXTH Mask

Definition at line 5007 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXTH_Pos

#define SPI_FIFOCTL_RXTH_Pos (24)

SPI_T::FIFOCTL: RXTH Position

Definition at line 5006 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXTHIEN_Msk

#define SPI_FIFOCTL_RXTHIEN_Msk (0x1ul << SPI_FIFOCTL_RXTHIEN_Pos)

SPI_T::FIFOCTL: RXTHIEN Mask

Definition at line 4995 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXTHIEN_Pos

#define SPI_FIFOCTL_RXTHIEN_Pos (2)

SPI_T::FIFOCTL: RXTHIEN Position

Definition at line 4994 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXTOIEN_Msk

#define SPI_FIFOCTL_RXTOIEN_Msk (0x1ul << SPI_FIFOCTL_RXTOIEN_Pos)

SPI_T::FIFOCTL: RXTOIEN Mask

Definition at line 5004 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_RXTOIEN_Pos

#define SPI_FIFOCTL_RXTOIEN_Pos (21)

SPI_T::FIFOCTL: RXTOIEN Position

Definition at line 5003 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_TXRST_Msk

#define SPI_FIFOCTL_TXRST_Msk (0x1ul << SPI_FIFOCTL_TXRST_Pos)

SPI_T::FIFOCTL: TXRST Mask

Definition at line 4992 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_TXRST_Pos

#define SPI_FIFOCTL_TXRST_Pos (1)

SPI_T::FIFOCTL: TXRST Position

Definition at line 4991 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_TXTH_Msk

#define SPI_FIFOCTL_TXTH_Msk (0x3ul << SPI_FIFOCTL_TXTH_Pos)

SPI_T::FIFOCTL: TXTH Mask

Definition at line 5010 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_TXTH_Pos

#define SPI_FIFOCTL_TXTH_Pos (28)

SPI_T::FIFOCTL: TXTH Position

Definition at line 5009 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_TXTHIEN_Msk

#define SPI_FIFOCTL_TXTHIEN_Msk (0x1ul << SPI_FIFOCTL_TXTHIEN_Pos)

SPI_T::FIFOCTL: TXTHIEN Mask

Definition at line 4998 of file Mini55Series.h.

## ◆ SPI_FIFOCTL_TXTHIEN_Pos

#define SPI_FIFOCTL_TXTHIEN_Pos (3)

SPI_T::FIFOCTL: TXTHIEN Position

Definition at line 4997 of file Mini55Series.h.

## ◆ SPI_RX_RX_Msk

#define SPI_RX_RX_Msk (0xfffffffful << SPI_RX_RX_Pos)

SPI_T::RX: RX Mask

Definition at line 4965 of file Mini55Series.h.

## ◆ SPI_RX_RX_Pos

#define SPI_RX_RX_Pos (0)

SPI_T::RX: RX Position

Definition at line 4964 of file Mini55Series.h.

## ◆ SPI_SLVCTL_DIVMOD_Msk

#define SPI_SLVCTL_DIVMOD_Msk (0x1ul << SPI_SLVCTL_DIVMOD_Pos)

SPI_T::SLVCTL: DIVMOD Mask

Definition at line 4986 of file Mini55Series.h.

## ◆ SPI_SLVCTL_DIVMOD_Pos

#define SPI_SLVCTL_DIVMOD_Pos (31)

SPI_T::SLVCTL: DIVMOD Position

Definition at line 4985 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SLV3WIRE_Msk

#define SPI_SLVCTL_SLV3WIRE_Msk (0x1ul << SPI_SLVCTL_SLV3WIRE_Pos)

SPI_T::SLVCTL: SLV3WIRE Mask

Definition at line 4971 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SLV3WIRE_Pos

#define SPI_SLVCTL_SLV3WIRE_Pos (8)

SPI_T::SLVCTL: SLV3WIRE Position

Definition at line 4970 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SLVABT_Msk

#define SPI_SLVCTL_SLVABT_Msk (0x1ul << SPI_SLVCTL_SLVABT_Pos)

SPI_T::SLVCTL: SLVABT Mask

Definition at line 4974 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SLVABT_Pos

#define SPI_SLVCTL_SLVABT_Pos (9)

SPI_T::SLVCTL: SLVABT Position

Definition at line 4973 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SLVSTIEN_Msk

#define SPI_SLVCTL_SLVSTIEN_Msk (0x1ul << SPI_SLVCTL_SLVSTIEN_Pos)

SPI_T::SLVCTL: SLVSTIEN Mask

Definition at line 4977 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SLVSTIEN_Pos

#define SPI_SLVCTL_SLVSTIEN_Pos (10)

SPI_T::SLVCTL: SLVSTIEN Position

Definition at line 4976 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SLVSTIF_Msk

#define SPI_SLVCTL_SLVSTIF_Msk (0x1ul << SPI_SLVCTL_SLVSTIF_Pos)

SPI_T::SLVCTL: SLVSTIF Mask

Definition at line 4980 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SLVSTIF_Pos

#define SPI_SLVCTL_SLVSTIF_Pos (11)

SPI_T::SLVCTL: SLVSTIF Position

Definition at line 4979 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SSINAIEN_Msk

#define SPI_SLVCTL_SSINAIEN_Msk (0x1ul << SPI_SLVCTL_SSINAIEN_Pos)

SPI_T::SLVCTL: SSINAIEN Mask

Definition at line 4983 of file Mini55Series.h.

## ◆ SPI_SLVCTL_SSINAIEN_Pos

#define SPI_SLVCTL_SSINAIEN_Pos (16)

SPI_T::SLVCTL: SSINAIEN Position

Definition at line 4982 of file Mini55Series.h.

## ◆ SPI_SSCTL_AUTOSS_Msk

#define SPI_SSCTL_AUTOSS_Msk (0x1ul << SPI_SSCTL_AUTOSS_Pos)

SPI_T::SSCTL: AUTOSS Mask

Definition at line 4956 of file Mini55Series.h.

## ◆ SPI_SSCTL_AUTOSS_Pos

#define SPI_SSCTL_AUTOSS_Pos (3)

SPI_T::SSCTL: AUTOSS Position

Definition at line 4955 of file Mini55Series.h.

## ◆ SPI_SSCTL_LTF_Msk

#define SPI_SSCTL_LTF_Msk (0x1ul << SPI_SSCTL_LTF_Pos)

SPI_T::SSCTL: LTF Mask

Definition at line 4962 of file Mini55Series.h.

## ◆ SPI_SSCTL_LTF_Pos

#define SPI_SSCTL_LTF_Pos (5)

SPI_T::SSCTL: LTF Position

Definition at line 4961 of file Mini55Series.h.

## ◆ SPI_SSCTL_SS_Msk

#define SPI_SSCTL_SS_Msk (0x1ul << SPI_SSCTL_SS_Pos)

SPI_T::SSCTL: SS Mask

Definition at line 4950 of file Mini55Series.h.

## ◆ SPI_SSCTL_SS_Pos

#define SPI_SSCTL_SS_Pos (0)

SPI_T::SSCTL: SS Position

Definition at line 4949 of file Mini55Series.h.

## ◆ SPI_SSCTL_SSACTPOL_Msk

#define SPI_SSCTL_SSACTPOL_Msk (0x1ul << SPI_SSCTL_SSACTPOL_Pos)

SPI_T::SSCTL: SSACTPOL Mask

Definition at line 4953 of file Mini55Series.h.

## ◆ SPI_SSCTL_SSACTPOL_Pos

#define SPI_SSCTL_SSACTPOL_Pos (2)

SPI_T::SSCTL: SSACTPOL Position

Definition at line 4952 of file Mini55Series.h.

## ◆ SPI_SSCTL_SSLTEN_Msk

#define SPI_SSCTL_SSLTEN_Msk (0x1ul << SPI_SSCTL_SSLTEN_Pos)

SPI_T::SSCTL: SSLTEN Mask

Definition at line 4959 of file Mini55Series.h.

## ◆ SPI_SSCTL_SSLTEN_Pos

#define SPI_SSCTL_SSLTEN_Pos (4)

SPI_T::SSCTL: SSLTEN Position

Definition at line 4958 of file Mini55Series.h.

## ◆ SPI_STATUS_RXCNT_Msk

#define SPI_STATUS_RXCNT_Msk (0xful << SPI_STATUS_RXCNT_Pos)

SPI_T::STATUS: RXCNT Mask

Definition at line 5025 of file Mini55Series.h.

## ◆ SPI_STATUS_RXCNT_Pos

#define SPI_STATUS_RXCNT_Pos (12)

SPI_T::STATUS: RXCNT Position

Definition at line 5024 of file Mini55Series.h.

## ◆ SPI_STATUS_RXEMPTY_Msk

#define SPI_STATUS_RXEMPTY_Msk (0x1ul << SPI_STATUS_RXEMPTY_Pos)

SPI_T::STATUS: RXEMPTY Mask

Definition at line 5034 of file Mini55Series.h.

## ◆ SPI_STATUS_RXEMPTY_Pos

#define SPI_STATUS_RXEMPTY_Pos (24)

SPI_T::STATUS: RXEMPTY Position

Definition at line 5033 of file Mini55Series.h.

## ◆ SPI_STATUS_RXFULL_Msk

#define SPI_STATUS_RXFULL_Msk (0x1ul << SPI_STATUS_RXFULL_Pos)

SPI_T::STATUS: RXFULL Mask

Definition at line 5037 of file Mini55Series.h.

## ◆ SPI_STATUS_RXFULL_Pos

#define SPI_STATUS_RXFULL_Pos (25)

SPI_T::STATUS: RXFULL Position

Definition at line 5036 of file Mini55Series.h.

## ◆ SPI_STATUS_RXOVIF_Msk

#define SPI_STATUS_RXOVIF_Msk (0x1ul << SPI_STATUS_RXOVIF_Pos)

SPI_T::STATUS: RXOVIF Mask

Definition at line 5016 of file Mini55Series.h.

## ◆ SPI_STATUS_RXOVIF_Pos

#define SPI_STATUS_RXOVIF_Pos (2)

SPI_T::STATUS: RXOVIF Position

Definition at line 5015 of file Mini55Series.h.

## ◆ SPI_STATUS_RXTHIF_Msk

#define SPI_STATUS_RXTHIF_Msk (0x1ul << SPI_STATUS_RXTHIF_Pos)

SPI_T::STATUS: RXTHIF Mask

Definition at line 5013 of file Mini55Series.h.

## ◆ SPI_STATUS_RXTHIF_Pos

#define SPI_STATUS_RXTHIF_Pos (0)

SPI_T::STATUS: RXTHIF Position

Definition at line 5012 of file Mini55Series.h.

## ◆ SPI_STATUS_SLVSTIF_Msk

#define SPI_STATUS_SLVSTIF_Msk (0x1ul << SPI_STATUS_SLVSTIF_Pos)

SPI_T::STATUS: SLVSTIF Mask

Definition at line 5022 of file Mini55Series.h.

## ◆ SPI_STATUS_SLVSTIF_Pos

#define SPI_STATUS_SLVSTIF_Pos (11)

SPI_T::STATUS: SLVSTIF Position

Definition at line 5021 of file Mini55Series.h.

## ◆ SPI_STATUS_SLVTOIF_Msk

#define SPI_STATUS_SLVTOIF_Msk (0x1ul << SPI_STATUS_SLVTOIF_Pos)

SPI_T::STATUS: SLVTOIF Mask

Definition at line 5031 of file Mini55Series.h.

## ◆ SPI_STATUS_SLVTOIF_Pos

#define SPI_STATUS_SLVTOIF_Pos (20)

SPI_T::STATUS: SLVTOIF Position

Definition at line 5030 of file Mini55Series.h.

## ◆ SPI_STATUS_TXCNT_Msk

#define SPI_STATUS_TXCNT_Msk (0xful << SPI_STATUS_TXCNT_Pos)

SPI_T::STATUS: TXCNT Mask

Definition at line 5046 of file Mini55Series.h.

## ◆ SPI_STATUS_TXCNT_Pos

#define SPI_STATUS_TXCNT_Pos (28)

SPI_T::STATUS: TXCNT Position

Definition at line 5045 of file Mini55Series.h.

## ◆ SPI_STATUS_TXEMPTY_Msk

#define SPI_STATUS_TXEMPTY_Msk (0x1ul << SPI_STATUS_TXEMPTY_Pos)

SPI_T::STATUS: TXEMPTY Mask

Definition at line 5040 of file Mini55Series.h.

## ◆ SPI_STATUS_TXEMPTY_Pos

#define SPI_STATUS_TXEMPTY_Pos (26)

SPI_T::STATUS: TXEMPTY Position

Definition at line 5039 of file Mini55Series.h.

## ◆ SPI_STATUS_TXFULL_Msk

#define SPI_STATUS_TXFULL_Msk (0x1ul << SPI_STATUS_TXFULL_Pos)

SPI_T::STATUS: TXFULL Mask

Definition at line 5043 of file Mini55Series.h.

## ◆ SPI_STATUS_TXFULL_Pos

#define SPI_STATUS_TXFULL_Pos (27)

SPI_T::STATUS: TXFULL Position

Definition at line 5042 of file Mini55Series.h.

## ◆ SPI_STATUS_TXTHIF_Msk

#define SPI_STATUS_TXTHIF_Msk (0x1ul << SPI_STATUS_TXTHIF_Pos)

SPI_T::STATUS: TXTHIF Mask

Definition at line 5019 of file Mini55Series.h.

## ◆ SPI_STATUS_TXTHIF_Pos

#define SPI_STATUS_TXTHIF_Pos (4)

SPI_T::STATUS: TXTHIF Position

Definition at line 5018 of file Mini55Series.h.

## ◆ SPI_STATUS_UNITIF_Msk

#define SPI_STATUS_UNITIF_Msk (0x1ul << SPI_STATUS_UNITIF_Pos)

SPI_T::STATUS: UNITIF Mask

Definition at line 5028 of file Mini55Series.h.

## ◆ SPI_STATUS_UNITIF_Pos

#define SPI_STATUS_UNITIF_Pos (16)

SPI_T::STATUS: UNITIF Position

Definition at line 5027 of file Mini55Series.h.

## ◆ SPI_TX_TX_Msk

#define SPI_TX_TX_Msk (0xfffffffful << SPI_TX_TX_Pos)

SPI_T::TX: TX Mask

Definition at line 4968 of file Mini55Series.h.

## ◆ SPI_TX_TX_Pos

#define SPI_TX_TX_Pos (0)

SPI_T::TX: TX Position

Definition at line 4967 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODEN_Msk

#define SYS_BODCTL_BODEN_Msk (0x1ul << SYS_BODCTL_BODEN_Pos)

SYS_T::BODCTL: BODEN Mask

Definition at line 5556 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODEN_Pos

#define SYS_BODCTL_BODEN_Pos (0)

SYS_T::BODCTL: BODEN Position

Definition at line 5555 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODIF_Msk

#define SYS_BODCTL_BODIF_Msk (0x1ul << SYS_BODCTL_BODIF_Pos)

SYS_T::BODCTL: BODIF Mask

Definition at line 5565 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODIF_Pos

#define SYS_BODCTL_BODIF_Pos (4)

SYS_T::BODCTL: BODIF Position

Definition at line 5564 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODLPM_Msk

#define SYS_BODCTL_BODLPM_Msk (0x1ul << SYS_BODCTL_BODLPM_Pos)

SYS_T::BODCTL: BODLPM Mask

Definition at line 5568 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODLPM_Pos

#define SYS_BODCTL_BODLPM_Pos (5)

SYS_T::BODCTL: BODLPM Position

Definition at line 5567 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODOUT_Msk

#define SYS_BODCTL_BODOUT_Msk (0x1ul << SYS_BODCTL_BODOUT_Pos)

SYS_T::BODCTL: BODOUT Mask

Definition at line 5571 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODOUT_Pos

#define SYS_BODCTL_BODOUT_Pos (6)

SYS_T::BODCTL: BODOUT Position

Definition at line 5570 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODRSTEN_Msk

#define SYS_BODCTL_BODRSTEN_Msk (0x1ul << SYS_BODCTL_BODRSTEN_Pos)

SYS_T::BODCTL: BODRSTEN Mask

Definition at line 5562 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODRSTEN_Pos

#define SYS_BODCTL_BODRSTEN_Pos (3)

SYS_T::BODCTL: BODRSTEN Position

Definition at line 5561 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODVL1_0_Msk

#define SYS_BODCTL_BODVL1_0_Msk (0x3ul << SYS_BODCTL_BODVL1_0_Pos)

SYS_T::BODCTL: BODVL1_0 Mask

Definition at line 5559 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODVL1_0_Pos

#define SYS_BODCTL_BODVL1_0_Pos (1)

SYS_T::BODCTL: BODVL1_0 Position

Definition at line 5558 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODVL2_Msk

#define SYS_BODCTL_BODVL2_Msk (0x1ul << SYS_BODCTL_BODVL2_Pos)

SYS_T::BODCTL: BODVL2 Mask

Definition at line 5574 of file Mini55Series.h.

## ◆ SYS_BODCTL_BODVL2_Pos

#define SYS_BODCTL_BODVL2_Pos (7)

SYS_T::BODCTL: BODVL2 Position

Definition at line 5573 of file Mini55Series.h.

## ◆ SYS_BODCTL_BOREN_Msk

#define SYS_BODCTL_BOREN_Msk (0x1ul << SYS_BODCTL_BOREN_Pos)

SYS_T::BODCTL: BOREN Mask

Definition at line 5577 of file Mini55Series.h.

## ◆ SYS_BODCTL_BOREN_Pos

#define SYS_BODCTL_BOREN_Pos (8)

SYS_T::BODCTL: BOREN Position

Definition at line 5576 of file Mini55Series.h.

## ◆ SYS_EINT0SEL_SEL_Msk

#define SYS_EINT0SEL_SEL_Msk (0x1ul << SYS_EINT0SEL_SEL_Pos)

SYS_T::EINT0SEL: SEL Mask

Definition at line 5739 of file Mini55Series.h.

## ◆ SYS_EINT0SEL_SEL_Pos

#define SYS_EINT0SEL_SEL_Pos (0)

SYS_T::EINT0SEL: SEL Position

Definition at line 5738 of file Mini55Series.h.

## ◆ SYS_IPRST0_CHIPRST_Msk

#define SYS_IPRST0_CHIPRST_Msk (0x1ul << SYS_IPRST0_CHIPRST_Pos)

SYS_T::IPRST0: CHIPRST Mask

Definition at line 5517 of file Mini55Series.h.

## ◆ SYS_IPRST0_CHIPRST_Pos

#define SYS_IPRST0_CHIPRST_Pos (0)

SYS_T::IPRST0: CHIPRST Position

Definition at line 5516 of file Mini55Series.h.

## ◆ SYS_IPRST0_CPURST_Msk

#define SYS_IPRST0_CPURST_Msk (0x1ul << SYS_IPRST0_CPURST_Pos)

SYS_T::IPRST0: CPURST Mask

Definition at line 5520 of file Mini55Series.h.

## ◆ SYS_IPRST0_CPURST_Pos

#define SYS_IPRST0_CPURST_Pos (1)

SYS_T::IPRST0: CPURST Position

Definition at line 5519 of file Mini55Series.h.

## ◆ SYS_IPRST0_CPUWS_Msk

#define SYS_IPRST0_CPUWS_Msk (0x1ul << SYS_IPRST0_CPUWS_Pos)

SYS_T::IPRST0: CPUWS Mask

Definition at line 5523 of file Mini55Series.h.

## ◆ SYS_IPRST0_CPUWS_Pos

#define SYS_IPRST0_CPUWS_Pos (2)

SYS_T::IPRST0: CPUWS Position

Definition at line 5522 of file Mini55Series.h.

## ◆ SYS_IPRST1_ACMPRST_Msk

#define SYS_IPRST1_ACMPRST_Msk (0x1ul << SYS_IPRST1_ACMPRST_Pos)

SYS_T::IPRST1: ACMPRST Mask

Definition at line 5550 of file Mini55Series.h.

## ◆ SYS_IPRST1_ACMPRST_Pos

#define SYS_IPRST1_ACMPRST_Pos (22)

SYS_T::IPRST1: ACMPRST Position

Definition at line 5549 of file Mini55Series.h.

## ◆ SYS_IPRST1_ADCRST_Msk

#define SYS_IPRST1_ADCRST_Msk (0x1ul << SYS_IPRST1_ADCRST_Pos)

SYS_T::IPRST1: ADCRST Mask

Definition at line 5553 of file Mini55Series.h.

## ◆ SYS_IPRST1_ADCRST_Pos

#define SYS_IPRST1_ADCRST_Pos (28)

SYS_T::IPRST1: ADCRST Position

Definition at line 5552 of file Mini55Series.h.

## ◆ SYS_IPRST1_GPIORST_Msk

#define SYS_IPRST1_GPIORST_Msk (0x1ul << SYS_IPRST1_GPIORST_Pos)

SYS_T::IPRST1: GPIORST Mask

Definition at line 5526 of file Mini55Series.h.

## ◆ SYS_IPRST1_GPIORST_Pos

#define SYS_IPRST1_GPIORST_Pos (1)

SYS_T::IPRST1: GPIORST Position

Definition at line 5525 of file Mini55Series.h.

## ◆ SYS_IPRST1_I2C_RST_Msk

#define SYS_IPRST1_I2C_RST_Msk (0x1ul << SYS_IPRST1_I2C_RST_Pos)

SYS_T::IPRST1: I2C_RST Mask

Definition at line 5535 of file Mini55Series.h.

## ◆ SYS_IPRST1_I2C_RST_Pos

#define SYS_IPRST1_I2C_RST_Pos (8)

SYS_T::IPRST1: I2C_RST Position

Definition at line 5534 of file Mini55Series.h.

## ◆ SYS_IPRST1_PWMRST_Msk

#define SYS_IPRST1_PWMRST_Msk (0x1ul << SYS_IPRST1_PWMRST_Pos)

SYS_T::IPRST1: PWMRST Mask

Definition at line 5547 of file Mini55Series.h.

## ◆ SYS_IPRST1_PWMRST_Pos

#define SYS_IPRST1_PWMRST_Pos (20)

SYS_T::IPRST1: PWMRST Position

Definition at line 5546 of file Mini55Series.h.

## ◆ SYS_IPRST1_SPIRST_Msk

#define SYS_IPRST1_SPIRST_Msk (0x1ul << SYS_IPRST1_SPIRST_Pos)

SYS_T::IPRST1: SPIRST Mask

Definition at line 5538 of file Mini55Series.h.

## ◆ SYS_IPRST1_SPIRST_Pos

#define SYS_IPRST1_SPIRST_Pos (12)

SYS_T::IPRST1: SPIRST Position

Definition at line 5537 of file Mini55Series.h.

## ◆ SYS_IPRST1_TMR0RST_Msk

#define SYS_IPRST1_TMR0RST_Msk (0x1ul << SYS_IPRST1_TMR0RST_Pos)

SYS_T::IPRST1: TMR0RST Mask

Definition at line 5529 of file Mini55Series.h.

## ◆ SYS_IPRST1_TMR0RST_Pos

#define SYS_IPRST1_TMR0RST_Pos (2)

SYS_T::IPRST1: TMR0RST Position

Definition at line 5528 of file Mini55Series.h.

## ◆ SYS_IPRST1_TMR1RST_Msk

#define SYS_IPRST1_TMR1RST_Msk (0x1ul << SYS_IPRST1_TMR1RST_Pos)

SYS_T::IPRST1: TMR1RST Mask

Definition at line 5532 of file Mini55Series.h.

## ◆ SYS_IPRST1_TMR1RST_Pos

#define SYS_IPRST1_TMR1RST_Pos (3)

SYS_T::IPRST1: TMR1RST Position

Definition at line 5531 of file Mini55Series.h.

## ◆ SYS_IPRST1_UART0RST_Msk

#define SYS_IPRST1_UART0RST_Msk (0x1ul << SYS_IPRST1_UART0RST_Pos)

SYS_T::IPRST1: UART0RST Mask

Definition at line 5541 of file Mini55Series.h.

## ◆ SYS_IPRST1_UART0RST_Pos

#define SYS_IPRST1_UART0RST_Pos (16)

SYS_T::IPRST1: UART0RST Position

Definition at line 5540 of file Mini55Series.h.

## ◆ SYS_IPRST1_UART1RST_Msk

#define SYS_IPRST1_UART1RST_Msk (0x1ul << SYS_IPRST1_UART1RST_Pos)

SYS_T::IPRST1: UART1RST Mask

Definition at line 5544 of file Mini55Series.h.

## ◆ SYS_IPRST1_UART1RST_Pos

#define SYS_IPRST1_UART1RST_Pos (17)

SYS_T::IPRST1: UART1RST Position

Definition at line 5543 of file Mini55Series.h.

## ◆ SYS_IRCTCTL_FREQSEL_Msk

#define SYS_IRCTCTL_FREQSEL_Msk (0x1ul << SYS_IRCTCTL_FREQSEL_Pos)

SYS_T::IRCTCTL: FREQSEL Mask

Definition at line 5742 of file Mini55Series.h.

## ◆ SYS_IRCTCTL_FREQSEL_Pos

#define SYS_IRCTCTL_FREQSEL_Pos (0)

SYS_T::IRCTCTL: FREQSEL Position

Definition at line 5741 of file Mini55Series.h.

## ◆ SYS_IRCTCTL_LOOPSEL_Msk

#define SYS_IRCTCTL_LOOPSEL_Msk (0x3ul << SYS_IRCTCTL_LOOPSEL_Pos)

SYS_T::IRCTCTL: LOOPSEL Mask

Definition at line 5745 of file Mini55Series.h.

## ◆ SYS_IRCTCTL_LOOPSEL_Pos

#define SYS_IRCTCTL_LOOPSEL_Pos (4)

SYS_T::IRCTCTL: LOOPSEL Position

Definition at line 5744 of file Mini55Series.h.

## ◆ SYS_IRCTIEN_CLKEIEN_Msk

#define SYS_IRCTIEN_CLKEIEN_Msk (0x1ul << SYS_IRCTIEN_CLKEIEN_Pos)

SYS_T::IRCTIEN: CLKEIEN Mask

Definition at line 5751 of file Mini55Series.h.

## ◆ SYS_IRCTIEN_CLKEIEN_Pos

#define SYS_IRCTIEN_CLKEIEN_Pos (2)

SYS_T::IRCTIEN: CLKEIEN Position

Definition at line 5750 of file Mini55Series.h.

## ◆ SYS_IRCTIEN_TFAILIEN_Msk

#define SYS_IRCTIEN_TFAILIEN_Msk (0x1ul << SYS_IRCTIEN_TFAILIEN_Pos)

SYS_T::IRCTIEN: TFAILIEN Mask

Definition at line 5748 of file Mini55Series.h.

## ◆ SYS_IRCTIEN_TFAILIEN_Pos

#define SYS_IRCTIEN_TFAILIEN_Pos (1)

SYS_T::IRCTIEN: TFAILIEN Position

Definition at line 5747 of file Mini55Series.h.

## ◆ SYS_IRCTISTS_CLKERRIF_Msk

#define SYS_IRCTISTS_CLKERRIF_Msk (0x1ul << SYS_IRCTISTS_CLKERRIF_Pos)

SYS_T::IRCTISTS: CLKERRIF Mask

Definition at line 5760 of file Mini55Series.h.

## ◆ SYS_IRCTISTS_CLKERRIF_Pos

#define SYS_IRCTISTS_CLKERRIF_Pos (2)

SYS_T::IRCTISTS: CLKERRIF Position

Definition at line 5759 of file Mini55Series.h.

## ◆ SYS_IRCTISTS_FREQLOCK_Msk

#define SYS_IRCTISTS_FREQLOCK_Msk (0x1ul << SYS_IRCTISTS_FREQLOCK_Pos)

SYS_T::IRCTISTS: FREQLOCK Mask

Definition at line 5754 of file Mini55Series.h.

## ◆ SYS_IRCTISTS_FREQLOCK_Pos

#define SYS_IRCTISTS_FREQLOCK_Pos (0)

SYS_T::IRCTISTS: FREQLOCK Position

Definition at line 5753 of file Mini55Series.h.

## ◆ SYS_IRCTISTS_TFAILIF_Msk

#define SYS_IRCTISTS_TFAILIF_Msk (0x1ul << SYS_IRCTISTS_TFAILIF_Pos)

SYS_T::IRCTISTS: TFAILIF Mask

Definition at line 5757 of file Mini55Series.h.

## ◆ SYS_IRCTISTS_TFAILIF_Pos

#define SYS_IRCTISTS_TFAILIF_Pos (1)

SYS_T::IRCTISTS: TFAILIF Position

Definition at line 5756 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT0_Msk

#define SYS_P0_MFP_ALT0_Msk (0x1ul << SYS_P0_MFP_ALT0_Pos)

SYS_T::P0_MFP: ALT0 Mask

Definition at line 5583 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT0_Pos

#define SYS_P0_MFP_ALT0_Pos (8)

SYS_T::P0_MFP: ALT0 Position

Definition at line 5582 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT1_Msk

#define SYS_P0_MFP_ALT1_Msk (0x1ul << SYS_P0_MFP_ALT1_Pos)

SYS_T::P0_MFP: ALT1 Mask

Definition at line 5586 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT1_Pos

#define SYS_P0_MFP_ALT1_Pos (9)

SYS_T::P0_MFP: ALT1 Position

Definition at line 5585 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT2_Msk

#define SYS_P0_MFP_ALT2_Msk (0x1ul << SYS_P0_MFP_ALT2_Pos)

SYS_T::P0_MFP: ALT2 Mask

Definition at line 5589 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT2_Pos

#define SYS_P0_MFP_ALT2_Pos (10)

SYS_T::P0_MFP: ALT2 Position

Definition at line 5588 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT4_Msk

#define SYS_P0_MFP_ALT4_Msk (0x1ul << SYS_P0_MFP_ALT4_Pos)

SYS_T::P0_MFP: ALT4 Mask

Definition at line 5592 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT4_Pos

#define SYS_P0_MFP_ALT4_Pos (12)

SYS_T::P0_MFP: ALT4 Position

Definition at line 5591 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT5_Msk

#define SYS_P0_MFP_ALT5_Msk (0x1ul << SYS_P0_MFP_ALT5_Pos)

SYS_T::P0_MFP: ALT5 Mask

Definition at line 5595 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT5_Pos

#define SYS_P0_MFP_ALT5_Pos (13)

SYS_T::P0_MFP: ALT5 Position

Definition at line 5594 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT6_Msk

#define SYS_P0_MFP_ALT6_Msk (0x1ul << SYS_P0_MFP_ALT6_Pos)

SYS_T::P0_MFP: ALT6 Mask

Definition at line 5598 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT6_Pos

#define SYS_P0_MFP_ALT6_Pos (14)

SYS_T::P0_MFP: ALT6 Position

Definition at line 5597 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT7_Msk

#define SYS_P0_MFP_ALT7_Msk (0x1ul << SYS_P0_MFP_ALT7_Pos)

SYS_T::P0_MFP: ALT7 Mask

Definition at line 5601 of file Mini55Series.h.

## ◆ SYS_P0_MFP_ALT7_Pos

#define SYS_P0_MFP_ALT7_Pos (15)

SYS_T::P0_MFP: ALT7 Position

Definition at line 5600 of file Mini55Series.h.

## ◆ SYS_P0_MFP_HS_Msk

#define SYS_P0_MFP_HS_Msk (0xfful << SYS_P0_MFP_HS_Pos)

SYS_T::P0_MFP: HS Mask

Definition at line 5607 of file Mini55Series.h.

## ◆ SYS_P0_MFP_HS_Pos

#define SYS_P0_MFP_HS_Pos (24)

SYS_T::P0_MFP: HS Position

Definition at line 5606 of file Mini55Series.h.

## ◆ SYS_P0_MFP_MFP_Msk

#define SYS_P0_MFP_MFP_Msk (0xfful << SYS_P0_MFP_MFP_Pos)

SYS_T::P0_MFP: MFP Mask

Definition at line 5580 of file Mini55Series.h.

## ◆ SYS_P0_MFP_MFP_Pos

#define SYS_P0_MFP_MFP_Pos (0)

SYS_T::P0_MFP: MFP Position

Definition at line 5579 of file Mini55Series.h.

## ◆ SYS_P0_MFP_TYPE_Msk

#define SYS_P0_MFP_TYPE_Msk (0xfful << SYS_P0_MFP_TYPE_Pos)

SYS_T::P0_MFP: TYPE Mask

Definition at line 5604 of file Mini55Series.h.

## ◆ SYS_P0_MFP_TYPE_Pos

#define SYS_P0_MFP_TYPE_Pos (16)

SYS_T::P0_MFP: TYPE Position

Definition at line 5603 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT0_Msk

#define SYS_P1_MFP_ALT0_Msk (0x1ul << SYS_P1_MFP_ALT0_Pos)

SYS_T::P1_MFP: ALT0 Mask

Definition at line 5613 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT0_Pos

#define SYS_P1_MFP_ALT0_Pos (8)

SYS_T::P1_MFP: ALT0 Position

Definition at line 5612 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT2_Msk

#define SYS_P1_MFP_ALT2_Msk (0x1ul << SYS_P1_MFP_ALT2_Pos)

SYS_T::P1_MFP: ALT2 Mask

Definition at line 5616 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT2_Pos

#define SYS_P1_MFP_ALT2_Pos (10)

SYS_T::P1_MFP: ALT2 Position

Definition at line 5615 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT3_Msk

#define SYS_P1_MFP_ALT3_Msk (0x1ul << SYS_P1_MFP_ALT3_Pos)

SYS_T::P1_MFP: ALT3 Mask

Definition at line 5619 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT3_Pos

#define SYS_P1_MFP_ALT3_Pos (11)

SYS_T::P1_MFP: ALT3 Position

Definition at line 5618 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT4_Msk

#define SYS_P1_MFP_ALT4_Msk (0x1ul << SYS_P1_MFP_ALT4_Pos)

SYS_T::P1_MFP: ALT4 Mask

Definition at line 5622 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT4_Pos

#define SYS_P1_MFP_ALT4_Pos (12)

SYS_T::P1_MFP: ALT4 Position

Definition at line 5621 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT5_Msk

#define SYS_P1_MFP_ALT5_Msk (0x1ul << SYS_P1_MFP_ALT5_Pos)

SYS_T::P1_MFP: ALT5 Mask

Definition at line 5625 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT5_Pos

#define SYS_P1_MFP_ALT5_Pos (13)

SYS_T::P1_MFP: ALT5 Position

Definition at line 5624 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT6_Msk

#define SYS_P1_MFP_ALT6_Msk (0x1ul << SYS_P1_MFP_ALT6_Pos)

SYS_T::P1_MFP: ALT6 Mask

Definition at line 5628 of file Mini55Series.h.

## ◆ SYS_P1_MFP_ALT6_Pos

#define SYS_P1_MFP_ALT6_Pos (14)

SYS_T::P1_MFP: ALT6 Position

Definition at line 5627 of file Mini55Series.h.

## ◆ SYS_P1_MFP_HS_Msk

#define SYS_P1_MFP_HS_Msk (0xfful << SYS_P1_MFP_HS_Pos)

SYS_T::P1_MFP: HS Mask

Definition at line 5634 of file Mini55Series.h.

## ◆ SYS_P1_MFP_HS_Pos

#define SYS_P1_MFP_HS_Pos (24)

SYS_T::P1_MFP: HS Position

Definition at line 5633 of file Mini55Series.h.

## ◆ SYS_P1_MFP_MFP_Msk

#define SYS_P1_MFP_MFP_Msk (0xfful << SYS_P1_MFP_MFP_Pos)

SYS_T::P1_MFP: MFP Mask

Definition at line 5610 of file Mini55Series.h.

## ◆ SYS_P1_MFP_MFP_Pos

#define SYS_P1_MFP_MFP_Pos (0)

SYS_T::P1_MFP: MFP Position

Definition at line 5609 of file Mini55Series.h.

## ◆ SYS_P1_MFP_TYPE_Msk

#define SYS_P1_MFP_TYPE_Msk (0xfful << SYS_P1_MFP_TYPE_Pos)

SYS_T::P1_MFP: TYPE Mask

Definition at line 5631 of file Mini55Series.h.

## ◆ SYS_P1_MFP_TYPE_Pos

#define SYS_P1_MFP_TYPE_Pos (16)

SYS_T::P1_MFP: TYPE Position

Definition at line 5630 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT2_Msk

#define SYS_P2_MFP_ALT2_Msk (0x1ul << SYS_P2_MFP_ALT2_Pos)

SYS_T::P2_MFP: ALT2 Mask

Definition at line 5640 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT2_Pos

#define SYS_P2_MFP_ALT2_Pos (10)

SYS_T::P2_MFP: ALT2 Position

Definition at line 5639 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT3_Msk

#define SYS_P2_MFP_ALT3_Msk (0x1ul << SYS_P2_MFP_ALT3_Pos)

SYS_T::P2_MFP: ALT3 Mask

Definition at line 5643 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT3_Pos

#define SYS_P2_MFP_ALT3_Pos (11)

SYS_T::P2_MFP: ALT3 Position

Definition at line 5642 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT4_Msk

#define SYS_P2_MFP_ALT4_Msk (0x1ul << SYS_P2_MFP_ALT4_Pos)

SYS_T::P2_MFP: ALT4 Mask

Definition at line 5646 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT4_Pos

#define SYS_P2_MFP_ALT4_Pos (12)

SYS_T::P2_MFP: ALT4 Position

Definition at line 5645 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT5_Msk

#define SYS_P2_MFP_ALT5_Msk (0x1ul << SYS_P2_MFP_ALT5_Pos)

SYS_T::P2_MFP: ALT5 Mask

Definition at line 5649 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT5_Pos

#define SYS_P2_MFP_ALT5_Pos (13)

SYS_T::P2_MFP: ALT5 Position

Definition at line 5648 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT6_Msk

#define SYS_P2_MFP_ALT6_Msk (0x1ul << SYS_P2_MFP_ALT6_Pos)

SYS_T::P2_MFP: ALT6 Mask

Definition at line 5652 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT6_Pos

#define SYS_P2_MFP_ALT6_Pos (14)

SYS_T::P2_MFP: ALT6 Position

Definition at line 5651 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT7_Msk

#define SYS_P2_MFP_ALT7_Msk (0x1ul << SYS_P2_MFP_ALT7_Pos)

SYS_T::P2_MFP: ALT7 Mask

Definition at line 5655 of file Mini55Series.h.

## ◆ SYS_P2_MFP_ALT7_Pos

#define SYS_P2_MFP_ALT7_Pos (15)

SYS_T::P2_MFP: ALT7 Position

Definition at line 5654 of file Mini55Series.h.

## ◆ SYS_P2_MFP_HS_Msk

#define SYS_P2_MFP_HS_Msk (0xfful << SYS_P2_MFP_HS_Pos)

SYS_T::P2_MFP: HS Mask

Definition at line 5661 of file Mini55Series.h.

## ◆ SYS_P2_MFP_HS_Pos

#define SYS_P2_MFP_HS_Pos (24)

SYS_T::P2_MFP: HS Position

Definition at line 5660 of file Mini55Series.h.

## ◆ SYS_P2_MFP_MFP_Msk

#define SYS_P2_MFP_MFP_Msk (0xfful << SYS_P2_MFP_MFP_Pos)

SYS_T::P2_MFP: MFP Mask

Definition at line 5637 of file Mini55Series.h.

## ◆ SYS_P2_MFP_MFP_Pos

#define SYS_P2_MFP_MFP_Pos (0)

SYS_T::P2_MFP: MFP Position

Definition at line 5636 of file Mini55Series.h.

## ◆ SYS_P2_MFP_TYPE_Msk

#define SYS_P2_MFP_TYPE_Msk (0xfful << SYS_P2_MFP_TYPE_Pos)

SYS_T::P2_MFP: TYPE Mask

Definition at line 5658 of file Mini55Series.h.

## ◆ SYS_P2_MFP_TYPE_Pos

#define SYS_P2_MFP_TYPE_Pos (16)

SYS_T::P2_MFP: TYPE Position

Definition at line 5657 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT0_Msk

#define SYS_P3_MFP_ALT0_Msk (0x1ul << SYS_P3_MFP_ALT0_Pos)

SYS_T::P3_MFP: ALT0 Mask

Definition at line 5667 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT0_Pos

#define SYS_P3_MFP_ALT0_Pos (8)

SYS_T::P3_MFP: ALT0 Position

Definition at line 5666 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT1_Msk

#define SYS_P3_MFP_ALT1_Msk (0x1ul << SYS_P3_MFP_ALT1_Pos)

SYS_T::P3_MFP: ALT1 Mask

Definition at line 5670 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT1_Pos

#define SYS_P3_MFP_ALT1_Pos (9)

SYS_T::P3_MFP: ALT1 Position

Definition at line 5669 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT2_Msk

#define SYS_P3_MFP_ALT2_Msk (0x1ul << SYS_P3_MFP_ALT2_Pos)

SYS_T::P3_MFP: ALT2 Mask

Definition at line 5673 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT2_Pos

#define SYS_P3_MFP_ALT2_Pos (10)

SYS_T::P3_MFP: ALT2 Position

Definition at line 5672 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT4_Msk

#define SYS_P3_MFP_ALT4_Msk (0x1ul << SYS_P3_MFP_ALT4_Pos)

SYS_T::P3_MFP: ALT4 Mask

Definition at line 5676 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT4_Pos

#define SYS_P3_MFP_ALT4_Pos (12)

SYS_T::P3_MFP: ALT4 Position

Definition at line 5675 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT5_Msk

#define SYS_P3_MFP_ALT5_Msk (0x1ul << SYS_P3_MFP_ALT5_Pos)

SYS_T::P3_MFP: ALT5 Mask

Definition at line 5679 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT5_Pos

#define SYS_P3_MFP_ALT5_Pos (13)

SYS_T::P3_MFP: ALT5 Position

Definition at line 5678 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT6_Msk

#define SYS_P3_MFP_ALT6_Msk (0x1ul << SYS_P3_MFP_ALT6_Pos)

SYS_T::P3_MFP: ALT6 Mask

Definition at line 5682 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT6_Pos

#define SYS_P3_MFP_ALT6_Pos (14)

SYS_T::P3_MFP: ALT6 Position

Definition at line 5681 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT7_Msk

#define SYS_P3_MFP_ALT7_Msk (0x1ul << SYS_P3_MFP_ALT7_Pos)

SYS_T::P3_MFP: ALT7 Mask

Definition at line 5685 of file Mini55Series.h.

## ◆ SYS_P3_MFP_ALT7_Pos

#define SYS_P3_MFP_ALT7_Pos (15)

SYS_T::P3_MFP: ALT7 Position

Definition at line 5684 of file Mini55Series.h.

## ◆ SYS_P3_MFP_HS_Msk

#define SYS_P3_MFP_HS_Msk (0x7ful << SYS_P3_MFP_HS_Pos)

SYS_T::P3_MFP: HS Mask

Definition at line 5694 of file Mini55Series.h.

## ◆ SYS_P3_MFP_HS_Pos

#define SYS_P3_MFP_HS_Pos (25)

SYS_T::P3_MFP: HS Position

Definition at line 5693 of file Mini55Series.h.

## ◆ SYS_P3_MFP_MFP_Msk

#define SYS_P3_MFP_MFP_Msk (0xfful << SYS_P3_MFP_MFP_Pos)

SYS_T::P3_MFP: MFP Mask

Definition at line 5664 of file Mini55Series.h.

## ◆ SYS_P3_MFP_MFP_Pos

#define SYS_P3_MFP_MFP_Pos (0)

SYS_T::P3_MFP: MFP Position

Definition at line 5663 of file Mini55Series.h.

## ◆ SYS_P3_MFP_P32CTL_Msk

#define SYS_P3_MFP_P32CTL_Msk (0x1ul << SYS_P3_MFP_P32CTL_Pos)

SYS_T::P3_MFP: P32CTL Mask

Definition at line 5691 of file Mini55Series.h.

## ◆ SYS_P3_MFP_P32CTL_Pos

#define SYS_P3_MFP_P32CTL_Pos (24)

SYS_T::P3_MFP: P32CTL Position

Definition at line 5690 of file Mini55Series.h.

## ◆ SYS_P3_MFP_TYPE_Msk

#define SYS_P3_MFP_TYPE_Msk (0xfful << SYS_P3_MFP_TYPE_Pos)

SYS_T::P3_MFP: TYPE Mask

Definition at line 5688 of file Mini55Series.h.

## ◆ SYS_P3_MFP_TYPE_Pos

#define SYS_P3_MFP_TYPE_Pos (16)

SYS_T::P3_MFP: TYPE Position

Definition at line 5687 of file Mini55Series.h.

## ◆ SYS_P4_MFP_ALT6_Msk

#define SYS_P4_MFP_ALT6_Msk (0x1ul << SYS_P4_MFP_ALT6_Pos)

SYS_T::P4_MFP: ALT6 Mask

Definition at line 5700 of file Mini55Series.h.

## ◆ SYS_P4_MFP_ALT6_Pos

#define SYS_P4_MFP_ALT6_Pos (14)

SYS_T::P4_MFP: ALT6 Position

Definition at line 5699 of file Mini55Series.h.

## ◆ SYS_P4_MFP_ALT7_Msk

#define SYS_P4_MFP_ALT7_Msk (0x1ul << SYS_P4_MFP_ALT7_Pos)

SYS_T::P4_MFP: ALT7 Mask

Definition at line 5703 of file Mini55Series.h.

## ◆ SYS_P4_MFP_ALT7_Pos

#define SYS_P4_MFP_ALT7_Pos (15)

SYS_T::P4_MFP: ALT7 Position

Definition at line 5702 of file Mini55Series.h.

## ◆ SYS_P4_MFP_HS_Msk

#define SYS_P4_MFP_HS_Msk (0xfful << SYS_P4_MFP_HS_Pos)

SYS_T::P4_MFP: HS Mask

Definition at line 5709 of file Mini55Series.h.

## ◆ SYS_P4_MFP_HS_Pos

#define SYS_P4_MFP_HS_Pos (24)

SYS_T::P4_MFP: HS Position

Definition at line 5708 of file Mini55Series.h.

## ◆ SYS_P4_MFP_MFP_Msk

#define SYS_P4_MFP_MFP_Msk (0xfful << SYS_P4_MFP_MFP_Pos)

SYS_T::P4_MFP: MFP Mask

Definition at line 5697 of file Mini55Series.h.

## ◆ SYS_P4_MFP_MFP_Pos

#define SYS_P4_MFP_MFP_Pos (0)

SYS_T::P4_MFP: MFP Position

Definition at line 5696 of file Mini55Series.h.

## ◆ SYS_P4_MFP_TYPE_Msk

#define SYS_P4_MFP_TYPE_Msk (0xfful << SYS_P4_MFP_TYPE_Pos)

SYS_T::P4_MFP: TYPE Mask

Definition at line 5706 of file Mini55Series.h.

## ◆ SYS_P4_MFP_TYPE_Pos

#define SYS_P4_MFP_TYPE_Pos (16)

SYS_T::P4_MFP: TYPE Position

Definition at line 5705 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT0_Msk

#define SYS_P5_MFP_ALT0_Msk (0x1ul << SYS_P5_MFP_ALT0_Pos)

SYS_T::P5_MFP: ALT0 Mask

Definition at line 5715 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT0_Pos

#define SYS_P5_MFP_ALT0_Pos (8)

SYS_T::P5_MFP: ALT0 Position

Definition at line 5714 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT1_Msk

#define SYS_P5_MFP_ALT1_Msk (0x1ul << SYS_P5_MFP_ALT1_Pos)

SYS_T::P5_MFP: ALT1 Mask

Definition at line 5718 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT1_Pos

#define SYS_P5_MFP_ALT1_Pos (9)

SYS_T::P5_MFP: ALT1 Position

Definition at line 5717 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT2_Msk

#define SYS_P5_MFP_ALT2_Msk (0x1ul << SYS_P5_MFP_ALT2_Pos)

SYS_T::P5_MFP: ALT2 Mask

Definition at line 5721 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT2_Pos

#define SYS_P5_MFP_ALT2_Pos (10)

SYS_T::P5_MFP: ALT2 Position

Definition at line 5720 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT3_Msk

#define SYS_P5_MFP_ALT3_Msk (0x1ul << SYS_P5_MFP_ALT3_Pos)

SYS_T::P5_MFP: ALT3 Mask

Definition at line 5724 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT3_Pos

#define SYS_P5_MFP_ALT3_Pos (11)

SYS_T::P5_MFP: ALT3 Position

Definition at line 5723 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT4_Msk

#define SYS_P5_MFP_ALT4_Msk (0x1ul << SYS_P5_MFP_ALT4_Pos)

SYS_T::P5_MFP: ALT4 Mask

Definition at line 5727 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT4_Pos

#define SYS_P5_MFP_ALT4_Pos (12)

SYS_T::P5_MFP: ALT4 Position

Definition at line 5726 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT5_Msk

#define SYS_P5_MFP_ALT5_Msk (0x1ul << SYS_P5_MFP_ALT5_Pos)

SYS_T::P5_MFP: ALT5 Mask

Definition at line 5730 of file Mini55Series.h.

## ◆ SYS_P5_MFP_ALT5_Pos

#define SYS_P5_MFP_ALT5_Pos (13)

SYS_T::P5_MFP: ALT5 Position

Definition at line 5729 of file Mini55Series.h.

## ◆ SYS_P5_MFP_HS_Msk

#define SYS_P5_MFP_HS_Msk (0xfful << SYS_P5_MFP_HS_Pos)

SYS_T::P5_MFP: HS Mask

Definition at line 5736 of file Mini55Series.h.

## ◆ SYS_P5_MFP_HS_Pos

#define SYS_P5_MFP_HS_Pos (24)

SYS_T::P5_MFP: HS Position

Definition at line 5735 of file Mini55Series.h.

## ◆ SYS_P5_MFP_MFP_Msk

#define SYS_P5_MFP_MFP_Msk (0xfful << SYS_P5_MFP_MFP_Pos)

SYS_T::P5_MFP: MFP Mask

Definition at line 5712 of file Mini55Series.h.

## ◆ SYS_P5_MFP_MFP_Pos

#define SYS_P5_MFP_MFP_Pos (0)

SYS_T::P5_MFP: MFP Position

Definition at line 5711 of file Mini55Series.h.

## ◆ SYS_P5_MFP_TYPE_Msk

#define SYS_P5_MFP_TYPE_Msk (0xfful << SYS_P5_MFP_TYPE_Pos)

SYS_T::P5_MFP: TYPE Mask

Definition at line 5733 of file Mini55Series.h.

## ◆ SYS_P5_MFP_TYPE_Pos

#define SYS_P5_MFP_TYPE_Pos (16)

SYS_T::P5_MFP: TYPE Position

Definition at line 5732 of file Mini55Series.h.

## ◆ SYS_PDID_PDID_Msk

#define SYS_PDID_PDID_Msk (0xfffffffful << SYS_PDID_PDID_Pos)

SYS_T::PDID: PDID Mask

Definition at line 5496 of file Mini55Series.h.

## ◆ SYS_PDID_PDID_Pos

#define SYS_PDID_PDID_Pos (0)

    @addtogroup SYS_CONST SYS Bit Field Definition
    Constant Definitions for SYS Controller

SYS_T::PDID: PDID Position

Definition at line 5495 of file Mini55Series.h.

## ◆ SYS_REGLCTL_REGPROTDIS_Msk

#define SYS_REGLCTL_REGPROTDIS_Msk (0x1ul << SYS_REGLCTL_REGPROTDIS_Pos)

SYS_T::REGLCTL: REGPROTDIS Mask

Definition at line 5766 of file Mini55Series.h.

## ◆ SYS_REGLCTL_REGPROTDIS_Pos

#define SYS_REGLCTL_REGPROTDIS_Pos (0)

SYS_T::REGLCTL: REGPROTDIS Position

Definition at line 5765 of file Mini55Series.h.

## ◆ SYS_REGLCTL_REGWRPROT_Msk

#define SYS_REGLCTL_REGWRPROT_Msk (0x1ul << SYS_REGLCTL_REGWRPROT_Pos)

SYS_T::REGLCTL: REGWRPROT Mask

Definition at line 5763 of file Mini55Series.h.

## ◆ SYS_REGLCTL_REGWRPROT_Pos

#define SYS_REGLCTL_REGWRPROT_Pos (0)

SYS_T::REGLCTL: REGWRPROT Position

Definition at line 5762 of file Mini55Series.h.

## ◆ SYS_RSTSTS_BODRF_Msk

#define SYS_RSTSTS_BODRF_Msk (0x1ul << SYS_RSTSTS_BODRF_Pos)

SYS_T::RSTSTS: BODRF Mask

Definition at line 5508 of file Mini55Series.h.

## ◆ SYS_RSTSTS_BODRF_Pos

#define SYS_RSTSTS_BODRF_Pos (4)

SYS_T::RSTSTS: BODRF Position

Definition at line 5507 of file Mini55Series.h.

## ◆ SYS_RSTSTS_CPURF_Msk

#define SYS_RSTSTS_CPURF_Msk (0x1ul << SYS_RSTSTS_CPURF_Pos)

SYS_T::RSTSTS: CPURF Mask

Definition at line 5514 of file Mini55Series.h.

## ◆ SYS_RSTSTS_CPURF_Pos

#define SYS_RSTSTS_CPURF_Pos (7)

SYS_T::RSTSTS: CPURF Position

Definition at line 5513 of file Mini55Series.h.

## ◆ SYS_RSTSTS_PINRF_Msk

#define SYS_RSTSTS_PINRF_Msk (0x1ul << SYS_RSTSTS_PINRF_Pos)

SYS_T::RSTSTS: PINRF Mask

Definition at line 5502 of file Mini55Series.h.

## ◆ SYS_RSTSTS_PINRF_Pos

#define SYS_RSTSTS_PINRF_Pos (1)

SYS_T::RSTSTS: PINRF Position

Definition at line 5501 of file Mini55Series.h.

## ◆ SYS_RSTSTS_PORF_Msk

#define SYS_RSTSTS_PORF_Msk (0x1ul << SYS_RSTSTS_PORF_Pos)

SYS_T::RSTSTS: PORF Mask

Definition at line 5499 of file Mini55Series.h.

## ◆ SYS_RSTSTS_PORF_Pos

#define SYS_RSTSTS_PORF_Pos (0)

SYS_T::RSTSTS: PORF Position

Definition at line 5498 of file Mini55Series.h.

## ◆ SYS_RSTSTS_SYSRF_Msk

#define SYS_RSTSTS_SYSRF_Msk (0x1ul << SYS_RSTSTS_SYSRF_Pos)

SYS_T::RSTSTS: SYSRF Mask

Definition at line 5511 of file Mini55Series.h.

## ◆ SYS_RSTSTS_SYSRF_Pos

#define SYS_RSTSTS_SYSRF_Pos (5)

SYS_T::RSTSTS: SYSRF Position

Definition at line 5510 of file Mini55Series.h.

## ◆ SYS_RSTSTS_WDTRF_Msk

#define SYS_RSTSTS_WDTRF_Msk (0x1ul << SYS_RSTSTS_WDTRF_Pos)

SYS_T::RSTSTS: WDTRF Mask

Definition at line 5505 of file Mini55Series.h.

## ◆ SYS_RSTSTS_WDTRF_Pos

#define SYS_RSTSTS_WDTRF_Pos (2)

SYS_T::RSTSTS: WDTRF Position

Definition at line 5504 of file Mini55Series.h.

## ◆ TIMER_CAP_CAPDAT_Msk

#define TIMER_CAP_CAPDAT_Msk (0xfffffful << TIMER_CAP_CAPDAT_Pos)

TIMER_T::CAP: CAPDAT Mask

Definition at line 6103 of file Mini55Series.h.

## ◆ TIMER_CAP_CAPDAT_Pos

#define TIMER_CAP_CAPDAT_Pos (0)

TIMER_T::CAP: CAPDAT Position

Definition at line 6102 of file Mini55Series.h.

## ◆ TIMER_CCAP_CAPDAT_Msk

#define TIMER_CCAP_CAPDAT_Msk (0xfffffful << TIMER_CCAP_CAPDAT_Pos)

TIMER_AC_T::CCAP: CAPDAT Mask

Definition at line 6157 of file Mini55Series.h.

## ◆ TIMER_CCAP_CAPDAT_Pos

#define TIMER_CCAP_CAPDAT_Pos (0)

TIMER_AC_T::CCAP: CAPDAT Position

Definition at line 6156 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPCHSEL_Msk

#define TIMER_CCAPCTL_CAPCHSEL_Msk (0x7ul << TIMER_CCAPCTL_CAPCHSEL_Pos)

TIMER_AC_T::CCAPCTL: CAPCHSEL Mask

Definition at line 6142 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPCHSEL_Pos

#define TIMER_CCAPCTL_CAPCHSEL_Pos (3)

TIMER_AC_T::CCAPCTL: CAPCHSEL Position

Definition at line 6141 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPF1F_Msk

#define TIMER_CCAPCTL_CAPF1F_Msk (0x1ul << TIMER_CCAPCTL_CAPF1F_Pos)

TIMER_AC_T::CCAPCTL: CAPF1F Mask

Definition at line 6148 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPF1F_Pos

#define TIMER_CCAPCTL_CAPF1F_Pos (9)

TIMER_AC_T::CCAPCTL: CAPF1F Position

Definition at line 6147 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPF2F_Msk

#define TIMER_CCAPCTL_CAPF2F_Msk (0x1ul << TIMER_CCAPCTL_CAPF2F_Pos)

TIMER_AC_T::CCAPCTL: CAPF2F Mask

Definition at line 6154 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPF2F_Pos

#define TIMER_CCAPCTL_CAPF2F_Pos (11)

TIMER_AC_T::CCAPCTL: CAPF2F Position

Definition at line 6153 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPR1F_Msk

#define TIMER_CCAPCTL_CAPR1F_Msk (0x1ul << TIMER_CCAPCTL_CAPR1F_Pos)

TIMER_AC_T::CCAPCTL: CAPR1F Mask

Definition at line 6145 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPR1F_Pos

#define TIMER_CCAPCTL_CAPR1F_Pos (8)

TIMER_AC_T::CCAPCTL: CAPR1F Position

Definition at line 6144 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPR2F_Msk

#define TIMER_CCAPCTL_CAPR2F_Msk (0x1ul << TIMER_CCAPCTL_CAPR2F_Pos)

TIMER_AC_T::CCAPCTL: CAPR2F Mask

Definition at line 6151 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CAPR2F_Pos

#define TIMER_CCAPCTL_CAPR2F_Pos (10)

TIMER_AC_T::CCAPCTL: CAPR2F Position

Definition at line 6150 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CCAPEN_Msk

#define TIMER_CCAPCTL_CCAPEN_Msk (0x1ul << TIMER_CCAPCTL_CCAPEN_Pos)

TIMER_AC_T::CCAPCTL: CCAPEN Mask

Definition at line 6133 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_CCAPEN_Pos

#define TIMER_CCAPCTL_CCAPEN_Pos (0)

TIMER_AC_T::CCAPCTL: CCAPEN Position

Definition at line 6132 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_INV_Msk

#define TIMER_CCAPCTL_INV_Msk (0x1ul << TIMER_CCAPCTL_INV_Pos)

TIMER_AC_T::CCAPCTL: INV Mask

Definition at line 6136 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_INV_Pos

#define TIMER_CCAPCTL_INV_Pos (1)

TIMER_AC_T::CCAPCTL: INV Position

Definition at line 6135 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_TMRSEL_Msk

#define TIMER_CCAPCTL_TMRSEL_Msk (0x1ul << TIMER_CCAPCTL_TMRSEL_Pos)

TMR CCAPCTL: TMRSEL Mask

Definition at line 6139 of file Mini55Series.h.

## ◆ TIMER_CCAPCTL_TMRSEL_Pos

#define TIMER_CCAPCTL_TMRSEL_Pos (2)

TIMER_AC_T::CCAPCTL: TMRSEL Position

Definition at line 6138 of file Mini55Series.h.

## ◆ TIMER_CMP_CMPDAT_Msk

#define TIMER_CMP_CMPDAT_Msk (0xfffffful << TIMER_CMP_CMPDAT_Pos)

TIMER_T::CMP: CMPDAT Mask

Definition at line 6091 of file Mini55Series.h.

## ◆ TIMER_CMP_CMPDAT_Pos

#define TIMER_CMP_CMPDAT_Pos (0)

TIMER_T::CMP: CMPDAT Position

Definition at line 6090 of file Mini55Series.h.

## ◆ TIMER_CNT_CNT_Msk

#define TIMER_CNT_CNT_Msk (0xfffffful << TIMER_CNT_CNT_Pos)

TIMER_T::CNT: CNT Mask

Definition at line 6100 of file Mini55Series.h.

## ◆ TIMER_CNT_CNT_Pos

#define TIMER_CNT_CNT_Pos (0)

TIMER_T::CNT: CNT Position

Definition at line 6099 of file Mini55Series.h.

## ◆ TIMER_CTL_ACTSTS_Msk

#define TIMER_CTL_ACTSTS_Msk (0x1ul << TIMER_CTL_ACTSTS_Pos)

TIMER_T::CTL: ACTSTS Mask

Definition at line 6073 of file Mini55Series.h.

## ◆ TIMER_CTL_ACTSTS_Pos

#define TIMER_CTL_ACTSTS_Pos (25)

TIMER_T::CTL: ACTSTS Position

Definition at line 6072 of file Mini55Series.h.

## ◆ TIMER_CTL_CAPPINSEL_Msk

#define TIMER_CTL_CAPPINSEL_Msk (0x1ul << TIMER_CTL_CAPPINSEL_Pos)

TIMER_T::CTL: CAPPINSEL Mask

Definition at line 6064 of file Mini55Series.h.

## ◆ TIMER_CTL_CAPPINSEL_Pos

#define TIMER_CTL_CAPPINSEL_Pos (19)

TIMER_T::CTL: CAPPINSEL Position

Definition at line 6063 of file Mini55Series.h.

## ◆ TIMER_CTL_CMPCTL_Msk

#define TIMER_CTL_CMPCTL_Msk (0x1ul << TIMER_CTL_CMPCTL_Pos)

TIMER_T::CTL: CMPCTL Mask

Definition at line 6058 of file Mini55Series.h.

## ◆ TIMER_CTL_CMPCTL_Pos

#define TIMER_CTL_CMPCTL_Pos (17)

TIMER_T::CTL: CMPCTL Position

Definition at line 6057 of file Mini55Series.h.

## ◆ TIMER_CTL_CNTDATEN_Msk

#define TIMER_CTL_CNTDATEN_Msk (0x1ul << TIMER_CTL_CNTDATEN_Pos)

TIMER_T::CTL: CNTDATEN Mask

Definition at line 6055 of file Mini55Series.h.

## ◆ TIMER_CTL_CNTDATEN_Pos

#define TIMER_CTL_CNTDATEN_Pos (16)

TIMER_T::CTL: CNTDATEN Position

Definition at line 6054 of file Mini55Series.h.

## ◆ TIMER_CTL_CNTEN_Msk

#define TIMER_CTL_CNTEN_Msk (0x1ul << TIMER_CTL_CNTEN_Pos)

TIMER_T::CTL: CNTEN Mask

Definition at line 6085 of file Mini55Series.h.

## ◆ TIMER_CTL_CNTEN_Pos

#define TIMER_CTL_CNTEN_Pos (30)

TIMER_T::CTL: CNTEN Position

Definition at line 6084 of file Mini55Series.h.

## ◆ TIMER_CTL_EXTCNTEN_Msk

#define TIMER_CTL_EXTCNTEN_Msk (0x1ul << TIMER_CTL_EXTCNTEN_Pos)

TIMER_T::CTL: EXTCNTEN Mask

Definition at line 6070 of file Mini55Series.h.

## ◆ TIMER_CTL_EXTCNTEN_Pos

#define TIMER_CTL_EXTCNTEN_Pos (24)

TIMER_T::CTL: EXTCNTEN Position

Definition at line 6069 of file Mini55Series.h.

## ◆ TIMER_CTL_ICEDEBUG_Msk

#define TIMER_CTL_ICEDEBUG_Msk (0x1ul << TIMER_CTL_ICEDEBUG_Pos)

TIMER_T::CTL: ICEDEBUG Mask

Definition at line 6088 of file Mini55Series.h.

## ◆ TIMER_CTL_ICEDEBUG_Pos

#define TIMER_CTL_ICEDEBUG_Pos (31)

TIMER_T::CTL: ICEDEBUG Position

Definition at line 6087 of file Mini55Series.h.

## ◆ TIMER_CTL_INTEN_Msk

#define TIMER_CTL_INTEN_Msk (0x1ul << TIMER_CTL_INTEN_Pos)

TIMER_T::CTL: INTEN Mask

Definition at line 6082 of file Mini55Series.h.

## ◆ TIMER_CTL_INTEN_Pos

#define TIMER_CTL_INTEN_Pos (29)

TIMER_T::CTL: INTEN Position

Definition at line 6081 of file Mini55Series.h.

## ◆ TIMER_CTL_OPMODE_Msk

#define TIMER_CTL_OPMODE_Msk (0x3ul << TIMER_CTL_OPMODE_Pos)

TIMER_T::CTL: OPMODE Mask

Definition at line 6079 of file Mini55Series.h.

## ◆ TIMER_CTL_OPMODE_Pos

#define TIMER_CTL_OPMODE_Pos (27)

TIMER_T::CTL: OPMODE Position

Definition at line 6078 of file Mini55Series.h.

## ◆ TIMER_CTL_PSC_Msk

#define TIMER_CTL_PSC_Msk (0xfful << TIMER_CTL_PSC_Pos)

TIMER_T::CTL: PSC Mask

Definition at line 6052 of file Mini55Series.h.

## ◆ TIMER_CTL_PSC_Pos

#define TIMER_CTL_PSC_Pos (0)

    @addtogroup TIMER_CONST TIMER Bit Field Definition
    Constant Definitions for TIMER Controller

TIMER_T::CTL: PSC Position

Definition at line 6051 of file Mini55Series.h.

## ◆ TIMER_CTL_RSTCNT_Msk

#define TIMER_CTL_RSTCNT_Msk (0x1ul << TIMER_CTL_RSTCNT_Pos)

TIMER_T::CTL: RSTCNT Mask

Definition at line 6076 of file Mini55Series.h.

## ◆ TIMER_CTL_RSTCNT_Pos

#define TIMER_CTL_RSTCNT_Pos (26)

TIMER_T::CTL: RSTCNT Position

Definition at line 6075 of file Mini55Series.h.

## ◆ TIMER_CTL_TGLPINSEL_Msk

#define TIMER_CTL_TGLPINSEL_Msk (0x1ul << TIMER_CTL_TGLPINSEL_Pos)

TIMER_T::CTL: TGLPINSEL Mask

Definition at line 6061 of file Mini55Series.h.

## ◆ TIMER_CTL_TGLPINSEL_Pos

#define TIMER_CTL_TGLPINSEL_Pos (18)

TIMER_T::CTL: TGLPINSEL Position

Definition at line 6060 of file Mini55Series.h.

## ◆ TIMER_CTL_WKEN_Msk

#define TIMER_CTL_WKEN_Msk (0x1ul << TIMER_CTL_WKEN_Pos)

TIMER_T::CTL: WKEN Mask

Definition at line 6067 of file Mini55Series.h.

## ◆ TIMER_CTL_WKEN_Pos

#define TIMER_CTL_WKEN_Pos (23)

TIMER_T::CTL: WKEN Position

Definition at line 6066 of file Mini55Series.h.

## ◆ TIMER_EINTSTS_CAPIF_Msk

#define TIMER_EINTSTS_CAPIF_Msk (0x1ul << TIMER_EINTSTS_CAPIF_Pos)

TIMER_T::EINTSTS: CAPIF Mask

Definition at line 6130 of file Mini55Series.h.

## ◆ TIMER_EINTSTS_CAPIF_Pos

#define TIMER_EINTSTS_CAPIF_Pos (0)

TIMER_T::EINTSTS: CAPIF Position

Definition at line 6129 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPDBEN_Msk

#define TIMER_EXTCTL_CAPDBEN_Msk (0x1ul << TIMER_EXTCTL_CAPDBEN_Pos)

TIMER_T::EXTCTL: CAPDBEN Mask

Definition at line 6121 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPDBEN_Pos

#define TIMER_EXTCTL_CAPDBEN_Pos (6)

TIMER_T::EXTCTL: CAPDBEN Position

Definition at line 6120 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPEDGE_Msk

#define TIMER_EXTCTL_CAPEDGE_Msk (0x3ul << TIMER_EXTCTL_CAPEDGE_Pos)

TIMER_T::EXTCTL: CAPEDGE Mask

Definition at line 6109 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPEDGE_Pos

#define TIMER_EXTCTL_CAPEDGE_Pos (1)

TIMER_T::EXTCTL: CAPEDGE Position

Definition at line 6108 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPEN_Msk

#define TIMER_EXTCTL_CAPEN_Msk (0x1ul << TIMER_EXTCTL_CAPEN_Pos)

TIMER_T::EXTCTL: CAPEN Mask

Definition at line 6112 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPEN_Pos

#define TIMER_EXTCTL_CAPEN_Pos (3)

TIMER_T::EXTCTL: CAPEN Position

Definition at line 6111 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPFUNCS_Msk

#define TIMER_EXTCTL_CAPFUNCS_Msk (0x1ul << TIMER_EXTCTL_CAPFUNCS_Pos)

TIMER_T::EXTCTL: CAPFUNCS Mask

Definition at line 6115 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPFUNCS_Pos

#define TIMER_EXTCTL_CAPFUNCS_Pos (4)

TIMER_T::EXTCTL: CAPFUNCS Position

Definition at line 6114 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPIEN_Msk

#define TIMER_EXTCTL_CAPIEN_Msk (0x1ul << TIMER_EXTCTL_CAPIEN_Pos)

TIMER_T::EXTCTL: CAPIEN Mask

Definition at line 6118 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPIEN_Pos

#define TIMER_EXTCTL_CAPIEN_Pos (5)

TIMER_T::EXTCTL: CAPIEN Position

Definition at line 6117 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPMODE_Msk

#define TIMER_EXTCTL_CAPMODE_Msk (0x1ul << TIMER_EXTCTL_CAPMODE_Pos)

TIMER_T::EXTCTL: CAPMODE Mask

Definition at line 6127 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CAPMODE_Pos

#define TIMER_EXTCTL_CAPMODE_Pos (8)

TIMER_T::EXTCTL: CAPMODE Position

Definition at line 6126 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CNTPHASE_Msk

#define TIMER_EXTCTL_CNTPHASE_Msk (0x1ul << TIMER_EXTCTL_CNTPHASE_Pos)

TIMER_T::EXTCTL: CNTPHASE Mask

Definition at line 6106 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_CNTPHASE_Pos

#define TIMER_EXTCTL_CNTPHASE_Pos (0)

TIMER_T::EXTCTL: CNTPHASE Position

Definition at line 6105 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_ECNTDBEN_Msk

#define TIMER_EXTCTL_ECNTDBEN_Msk (0x1ul << TIMER_EXTCTL_ECNTDBEN_Pos)

TIMER_T::EXTCTL: ECNTDBEN Mask

Definition at line 6124 of file Mini55Series.h.

## ◆ TIMER_EXTCTL_ECNTDBEN_Pos

#define TIMER_EXTCTL_ECNTDBEN_Pos (7)

TIMER_T::EXTCTL: ECNTDBEN Position

Definition at line 6123 of file Mini55Series.h.

## ◆ TIMER_INTSTS_TIF_Msk

#define TIMER_INTSTS_TIF_Msk (0x1ul << TIMER_INTSTS_TIF_Pos)

TIMER_T::INTSTS: TIF Mask

Definition at line 6094 of file Mini55Series.h.

## ◆ TIMER_INTSTS_TIF_Pos

#define TIMER_INTSTS_TIF_Pos (0)

TIMER_T::INTSTS: TIF Position

Definition at line 6093 of file Mini55Series.h.

## ◆ TIMER_INTSTS_TWKF_Msk

#define TIMER_INTSTS_TWKF_Msk (0x1ul << TIMER_INTSTS_TWKF_Pos)

TIMER_T::INTSTS: TWKF Mask

Definition at line 6097 of file Mini55Series.h.

## ◆ TIMER_INTSTS_TWKF_Pos

#define TIMER_INTSTS_TWKF_Pos (1)

TIMER_T::INTSTS: TWKF Position

Definition at line 6096 of file Mini55Series.h.

## ◆ UART_ALTCTL_ADDRDEN_Msk

#define UART_ALTCTL_ADDRDEN_Msk (0x1ul << UART_ALTCTL_ADDRDEN_Pos)

UART_T::ALTCTL: ADDRDEN Mask

Definition at line 6816 of file Mini55Series.h.

## ◆ UART_ALTCTL_ADDRDEN_Pos

#define UART_ALTCTL_ADDRDEN_Pos (15)

UART_T::ALTCTL: ADDRDEN Position

Definition at line 6815 of file Mini55Series.h.

## ◆ UART_ALTCTL_ADDRMV_Msk

#define UART_ALTCTL_ADDRMV_Msk (0xfful << UART_ALTCTL_ADDRMV_Pos)

UART_T::ALTCTL: ADDRMV Mask

Definition at line 6819 of file Mini55Series.h.

## ◆ UART_ALTCTL_ADDRMV_Pos

#define UART_ALTCTL_ADDRMV_Pos (24)

UART_T::ALTCTL: ADDRMV Position

Definition at line 6818 of file Mini55Series.h.

## ◆ UART_ALTCTL_RS485AAD_Msk

#define UART_ALTCTL_RS485AAD_Msk (0x1ul << UART_ALTCTL_RS485AAD_Pos)

UART_T::ALTCTL: RS485AAD Mask

Definition at line 6810 of file Mini55Series.h.

## ◆ UART_ALTCTL_RS485AAD_Pos

#define UART_ALTCTL_RS485AAD_Pos (9)

UART_T::ALTCTL: RS485AAD Position

Definition at line 6809 of file Mini55Series.h.

## ◆ UART_ALTCTL_RS485AUD_Msk

#define UART_ALTCTL_RS485AUD_Msk (0x1ul << UART_ALTCTL_RS485AUD_Pos)

UART_T::ALTCTL: RS485AUD Mask

Definition at line 6813 of file Mini55Series.h.

## ◆ UART_ALTCTL_RS485AUD_Pos

#define UART_ALTCTL_RS485AUD_Pos (10)

UART_T::ALTCTL: RS485AUD Position

Definition at line 6812 of file Mini55Series.h.

## ◆ UART_ALTCTL_RS485NMM_Msk

#define UART_ALTCTL_RS485NMM_Msk (0x1ul << UART_ALTCTL_RS485NMM_Pos)

UART_T::ALTCTL: RS485NMM Mask

Definition at line 6807 of file Mini55Series.h.

## ◆ UART_ALTCTL_RS485NMM_Pos

#define UART_ALTCTL_RS485NMM_Pos (8)

UART_T::ALTCTL: RS485NMM Position

Definition at line 6806 of file Mini55Series.h.

## ◆ UART_BAUD_BAUDM0_Msk

#define UART_BAUD_BAUDM0_Msk (0x1ul << UART_BAUD_BAUDM0_Pos)

UART_T::BAUD: BAUDM0 Mask

Definition at line 6792 of file Mini55Series.h.

## ◆ UART_BAUD_BAUDM0_Pos

#define UART_BAUD_BAUDM0_Pos (28)

UART_T::BAUD: BAUDM0 Position

Definition at line 6791 of file Mini55Series.h.

## ◆ UART_BAUD_BAUDM1_Msk

#define UART_BAUD_BAUDM1_Msk (0x1ul << UART_BAUD_BAUDM1_Pos)

UART_T::BAUD: BAUDM1 Mask

Definition at line 6795 of file Mini55Series.h.

## ◆ UART_BAUD_BAUDM1_Pos

#define UART_BAUD_BAUDM1_Pos (29)

UART_T::BAUD: BAUDM1 Position

Definition at line 6794 of file Mini55Series.h.

## ◆ UART_BAUD_BRD_Msk

#define UART_BAUD_BRD_Msk (0xfffful << UART_BAUD_BRD_Pos)

UART_T::BAUD: BRD Mask

Definition at line 6786 of file Mini55Series.h.

## ◆ UART_BAUD_BRD_Pos

#define UART_BAUD_BRD_Pos (0)

UART_T::BAUD: BRD Position

Definition at line 6785 of file Mini55Series.h.

## ◆ UART_BAUD_EDIVM1_Msk

#define UART_BAUD_EDIVM1_Msk (0xful << UART_BAUD_EDIVM1_Pos)

UART_T::BAUD: EDIVM1 Mask

Definition at line 6789 of file Mini55Series.h.

## ◆ UART_BAUD_EDIVM1_Pos

#define UART_BAUD_EDIVM1_Pos (24)

UART_T::BAUD: EDIVM1 Position

Definition at line 6788 of file Mini55Series.h.

## ◆ UART_DAT_DAT_Msk

#define UART_DAT_DAT_Msk (0xfful << UART_DAT_DAT_Pos)

UART_T::DAT: DAT Mask

Definition at line 6621 of file Mini55Series.h.

## ◆ UART_DAT_DAT_Pos

#define UART_DAT_DAT_Pos (0)

    @addtogroup UART_CONST UART Bit Field Definition
    Constant Definitions for UART Controller

UART_T::DAT: DAT Position

Definition at line 6620 of file Mini55Series.h.

## ◆ UART_FIFO_RFITL_Msk

#define UART_FIFO_RFITL_Msk (0xful << UART_FIFO_RFITL_Pos)

UART_T::FIFO: RFITL Mask

Definition at line 6660 of file Mini55Series.h.

## ◆ UART_FIFO_RFITL_Pos

#define UART_FIFO_RFITL_Pos (4)

UART_T::FIFO: RFITL Position

Definition at line 6659 of file Mini55Series.h.

## ◆ UART_FIFO_RTSTRGLV_Msk

#define UART_FIFO_RTSTRGLV_Msk (0xful << UART_FIFO_RTSTRGLV_Pos)

UART_T::FIFO: RTSTRGLV Mask

Definition at line 6666 of file Mini55Series.h.

## ◆ UART_FIFO_RTSTRGLV_Pos

#define UART_FIFO_RTSTRGLV_Pos (16)

UART_T::FIFO: RTSTRGLV Position

Definition at line 6665 of file Mini55Series.h.

## ◆ UART_FIFO_RXOFF_Msk

#define UART_FIFO_RXOFF_Msk (0x1ul << UART_FIFO_RXOFF_Pos)

UART_T::FIFO: RXOFF Mask

Definition at line 6663 of file Mini55Series.h.

## ◆ UART_FIFO_RXOFF_Pos

#define UART_FIFO_RXOFF_Pos (8)

UART_T::FIFO: RXOFF Position

Definition at line 6662 of file Mini55Series.h.

## ◆ UART_FIFO_RXRST_Msk

#define UART_FIFO_RXRST_Msk (0x1ul << UART_FIFO_RXRST_Pos)

UART_T::FIFO: RXRST Mask

Definition at line 6654 of file Mini55Series.h.

## ◆ UART_FIFO_RXRST_Pos

#define UART_FIFO_RXRST_Pos (1)

UART_T::FIFO: RXRST Position

Definition at line 6653 of file Mini55Series.h.

## ◆ UART_FIFO_TXRST_Msk

#define UART_FIFO_TXRST_Msk (0x1ul << UART_FIFO_TXRST_Pos)

UART_T::FIFO: TXRST Mask

Definition at line 6657 of file Mini55Series.h.

## ◆ UART_FIFO_TXRST_Pos

#define UART_FIFO_TXRST_Pos (2)

UART_T::FIFO: TXRST Position

Definition at line 6656 of file Mini55Series.h.

## ◆ UART_FIFOSTS_ADDRDETF_Msk

#define UART_FIFOSTS_ADDRDETF_Msk (0x1ul << UART_FIFOSTS_ADDRDETF_Pos)

UART_T::FIFOSTS: ADDRDETF Mask

Definition at line 6708 of file Mini55Series.h.

## ◆ UART_FIFOSTS_ADDRDETF_Pos

#define UART_FIFOSTS_ADDRDETF_Pos (3)

UART_T::FIFOSTS: ADDRDETF Position

Definition at line 6707 of file Mini55Series.h.

## ◆ UART_FIFOSTS_BIF_Msk

#define UART_FIFOSTS_BIF_Msk (0x1ul << UART_FIFOSTS_BIF_Pos)

UART_T::FIFOSTS: BIF Mask

Definition at line 6717 of file Mini55Series.h.

## ◆ UART_FIFOSTS_BIF_Pos

#define UART_FIFOSTS_BIF_Pos (6)

UART_T::FIFOSTS: BIF Position

Definition at line 6716 of file Mini55Series.h.

## ◆ UART_FIFOSTS_FEF_Msk

#define UART_FIFOSTS_FEF_Msk (0x1ul << UART_FIFOSTS_FEF_Pos)

UART_T::FIFOSTS: FEF Mask

Definition at line 6714 of file Mini55Series.h.

## ◆ UART_FIFOSTS_FEF_Pos

#define UART_FIFOSTS_FEF_Pos (5)

UART_T::FIFOSTS: FEF Position

Definition at line 6713 of file Mini55Series.h.

## ◆ UART_FIFOSTS_PEF_Msk

#define UART_FIFOSTS_PEF_Msk (0x1ul << UART_FIFOSTS_PEF_Pos)

UART_T::FIFOSTS: PEF Mask

Definition at line 6711 of file Mini55Series.h.

## ◆ UART_FIFOSTS_PEF_Pos

#define UART_FIFOSTS_PEF_Pos (4)

UART_T::FIFOSTS: PEF Position

Definition at line 6710 of file Mini55Series.h.

## ◆ UART_FIFOSTS_RXEMPTY_Msk

#define UART_FIFOSTS_RXEMPTY_Msk (0x1ul << UART_FIFOSTS_RXEMPTY_Pos)

UART_T::FIFOSTS: RXEMPTY Mask

Definition at line 6723 of file Mini55Series.h.

## ◆ UART_FIFOSTS_RXEMPTY_Pos

#define UART_FIFOSTS_RXEMPTY_Pos (14)

UART_T::FIFOSTS: RXEMPTY Position

Definition at line 6722 of file Mini55Series.h.

## ◆ UART_FIFOSTS_RXFULL_Msk

#define UART_FIFOSTS_RXFULL_Msk (0x1ul << UART_FIFOSTS_RXFULL_Pos)

UART_T::FIFOSTS: RXFULL Mask

Definition at line 6726 of file Mini55Series.h.

## ◆ UART_FIFOSTS_RXFULL_Pos

#define UART_FIFOSTS_RXFULL_Pos (15)

UART_T::FIFOSTS: RXFULL Position

Definition at line 6725 of file Mini55Series.h.

## ◆ UART_FIFOSTS_RXOVIF_Msk

#define UART_FIFOSTS_RXOVIF_Msk (0x1ul << UART_FIFOSTS_RXOVIF_Pos)

UART_T::FIFOSTS: RXOVIF Mask

Definition at line 6705 of file Mini55Series.h.

## ◆ UART_FIFOSTS_RXOVIF_Pos

#define UART_FIFOSTS_RXOVIF_Pos (0)

UART_T::FIFOSTS: RXOVIF Position

Definition at line 6704 of file Mini55Series.h.

## ◆ UART_FIFOSTS_RXPTR_Msk

#define UART_FIFOSTS_RXPTR_Msk (0x3ful << UART_FIFOSTS_RXPTR_Pos)

UART_T::FIFOSTS: RXPTR Mask

Definition at line 6720 of file Mini55Series.h.

## ◆ UART_FIFOSTS_RXPTR_Pos

#define UART_FIFOSTS_RXPTR_Pos (8)

UART_T::FIFOSTS: RXPTR Position

Definition at line 6719 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXEMPTY_Msk

#define UART_FIFOSTS_TXEMPTY_Msk (0x1ul << UART_FIFOSTS_TXEMPTY_Pos)

UART_T::FIFOSTS: TXEMPTY Mask

Definition at line 6732 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXEMPTY_Pos

#define UART_FIFOSTS_TXEMPTY_Pos (22)

UART_T::FIFOSTS: TXEMPTY Position

Definition at line 6731 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXEMPTYF_Msk

#define UART_FIFOSTS_TXEMPTYF_Msk (0x1ul << UART_FIFOSTS_TXEMPTYF_Pos)

UART_T::FIFOSTS: TXEMPTYF Mask

Definition at line 6741 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXEMPTYF_Pos

#define UART_FIFOSTS_TXEMPTYF_Pos (28)

UART_T::FIFOSTS: TXEMPTYF Position

Definition at line 6740 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXFULL_Msk

#define UART_FIFOSTS_TXFULL_Msk (0x1ul << UART_FIFOSTS_TXFULL_Pos)

UART_T::FIFOSTS: TXFULL Mask

Definition at line 6735 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXFULL_Pos

#define UART_FIFOSTS_TXFULL_Pos (23)

UART_T::FIFOSTS: TXFULL Position

Definition at line 6734 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXOVIF_Msk

#define UART_FIFOSTS_TXOVIF_Msk (0x1ul << UART_FIFOSTS_TXOVIF_Pos)

UART_T::FIFOSTS: TXOVIF Mask

Definition at line 6738 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXOVIF_Pos

#define UART_FIFOSTS_TXOVIF_Pos (24)

UART_T::FIFOSTS: TXOVIF Position

Definition at line 6737 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXPTR_Msk

#define UART_FIFOSTS_TXPTR_Msk (0x3ful << UART_FIFOSTS_TXPTR_Pos)

UART_T::FIFOSTS: TXPTR Mask

Definition at line 6729 of file Mini55Series.h.

## ◆ UART_FIFOSTS_TXPTR_Pos

#define UART_FIFOSTS_TXPTR_Pos (16)

UART_T::FIFOSTS: TXPTR Position

Definition at line 6728 of file Mini55Series.h.

## ◆ UART_FUNCSEL_FUNCSEL_Msk

#define UART_FUNCSEL_FUNCSEL_Msk (0x3ul << UART_FUNCSEL_FUNCSEL_Pos)

UART_T::FUNCSEL: FUNCSEL Mask

Definition at line 6822 of file Mini55Series.h.

## ◆ UART_FUNCSEL_FUNCSEL_Pos

#define UART_FUNCSEL_FUNCSEL_Pos (0)

UART_T::FUNCSEL: FUNCSEL Position

Definition at line 6821 of file Mini55Series.h.

## ◆ UART_INTEN_ATOCTSEN_Msk

#define UART_INTEN_ATOCTSEN_Msk (0x1ul << UART_INTEN_ATOCTSEN_Pos)

UART_T::INTEN: ATOCTSEN Mask

Definition at line 6651 of file Mini55Series.h.

## ◆ UART_INTEN_ATOCTSEN_Pos

#define UART_INTEN_ATOCTSEN_Pos (13)

UART_T::INTEN: ATOCTSEN Position

Definition at line 6650 of file Mini55Series.h.

## ◆ UART_INTEN_ATORTSEN_Msk

#define UART_INTEN_ATORTSEN_Msk (0x1ul << UART_INTEN_ATORTSEN_Pos)

UART_T::INTEN: ATORTSEN Mask

Definition at line 6648 of file Mini55Series.h.

## ◆ UART_INTEN_ATORTSEN_Pos

#define UART_INTEN_ATORTSEN_Pos (12)

UART_T::INTEN: ATORTSEN Position

Definition at line 6647 of file Mini55Series.h.

## ◆ UART_INTEN_BUFERRIEN_Msk

#define UART_INTEN_BUFERRIEN_Msk (0x1ul << UART_INTEN_BUFERRIEN_Pos)

UART_T::INTEN: BUFERRIEN Mask

Definition at line 6639 of file Mini55Series.h.

## ◆ UART_INTEN_BUFERRIEN_Pos

#define UART_INTEN_BUFERRIEN_Pos (5)

UART_T::INTEN: BUFERRIEN Position

Definition at line 6638 of file Mini55Series.h.

## ◆ UART_INTEN_MODEMIEN_Msk

#define UART_INTEN_MODEMIEN_Msk (0x1ul << UART_INTEN_MODEMIEN_Pos)

UART_T::INTEN: MODEMIEN Mask

Definition at line 6633 of file Mini55Series.h.

## ◆ UART_INTEN_MODEMIEN_Pos

#define UART_INTEN_MODEMIEN_Pos (3)

UART_T::INTEN: MODEMIEN Position

Definition at line 6632 of file Mini55Series.h.

## ◆ UART_INTEN_RDAIEN_Msk

#define UART_INTEN_RDAIEN_Msk (0x1ul << UART_INTEN_RDAIEN_Pos)

UART_T::INTEN: RDAIEN Mask

Definition at line 6624 of file Mini55Series.h.

## ◆ UART_INTEN_RDAIEN_Pos

#define UART_INTEN_RDAIEN_Pos (0)

UART_T::INTEN: RDAIEN Position

Definition at line 6623 of file Mini55Series.h.

## ◆ UART_INTEN_RLSIEN_Msk

#define UART_INTEN_RLSIEN_Msk (0x1ul << UART_INTEN_RLSIEN_Pos)

UART_T::INTEN: RLSIEN Mask

Definition at line 6630 of file Mini55Series.h.

## ◆ UART_INTEN_RLSIEN_Pos

#define UART_INTEN_RLSIEN_Pos (2)

UART_T::INTEN: RLSIEN Position

Definition at line 6629 of file Mini55Series.h.

## ◆ UART_INTEN_RXTOIEN_Msk

#define UART_INTEN_RXTOIEN_Msk (0x1ul << UART_INTEN_RXTOIEN_Pos)

UART_T::INTEN: RXTOIEN Mask

Definition at line 6636 of file Mini55Series.h.

## ◆ UART_INTEN_RXTOIEN_Pos

#define UART_INTEN_RXTOIEN_Pos (4)

UART_T::INTEN: RXTOIEN Position

Definition at line 6635 of file Mini55Series.h.

## ◆ UART_INTEN_THREIEN_Msk

#define UART_INTEN_THREIEN_Msk (0x1ul << UART_INTEN_THREIEN_Pos)

UART_T::INTEN: THREIEN Mask

Definition at line 6627 of file Mini55Series.h.

## ◆ UART_INTEN_THREIEN_Pos

#define UART_INTEN_THREIEN_Pos (1)

UART_T::INTEN: THREIEN Position

Definition at line 6626 of file Mini55Series.h.

## ◆ UART_INTEN_TOCNTEN_Msk

#define UART_INTEN_TOCNTEN_Msk (0x1ul << UART_INTEN_TOCNTEN_Pos)

UART_T::INTEN: TOCNTEN Mask

Definition at line 6645 of file Mini55Series.h.

## ◆ UART_INTEN_TOCNTEN_Pos

#define UART_INTEN_TOCNTEN_Pos (11)

UART_T::INTEN: TOCNTEN Position

Definition at line 6644 of file Mini55Series.h.

## ◆ UART_INTEN_WKCTSIEN_Msk

#define UART_INTEN_WKCTSIEN_Msk (0x1ul << UART_INTEN_WKCTSIEN_Pos)

UART_T::INTEN: WKCTSIEN Mask

Definition at line 6642 of file Mini55Series.h.

## ◆ UART_INTEN_WKCTSIEN_Pos

#define UART_INTEN_WKCTSIEN_Pos (6)

UART_T::INTEN: WKCTSIEN Position

Definition at line 6641 of file Mini55Series.h.

## ◆ UART_INTSTS_BUFERRIF_Msk

#define UART_INTSTS_BUFERRIF_Msk (0x1ul << UART_INTSTS_BUFERRIF_Pos)

UART_T::INTSTS: BUFERRIF Mask

Definition at line 6759 of file Mini55Series.h.

## ◆ UART_INTSTS_BUFERRIF_Pos

#define UART_INTSTS_BUFERRIF_Pos (5)

UART_T::INTSTS: BUFERRIF Position

Definition at line 6758 of file Mini55Series.h.

## ◆ UART_INTSTS_BUFERRINT_Msk

#define UART_INTSTS_BUFERRINT_Msk (0x1ul << UART_INTSTS_BUFERRINT_Pos)

UART_T::INTSTS: BUFERRINT Mask

Definition at line 6777 of file Mini55Series.h.

## ◆ UART_INTSTS_BUFERRINT_Pos

#define UART_INTSTS_BUFERRINT_Pos (13)

UART_T::INTSTS: BUFERRINT Position

Definition at line 6776 of file Mini55Series.h.

## ◆ UART_INTSTS_MODEMIF_Msk

#define UART_INTSTS_MODEMIF_Msk (0x1ul << UART_INTSTS_MODEMIF_Pos)

UART_T::INTSTS: MODENIF Mask

Definition at line 6753 of file Mini55Series.h.

## ◆ UART_INTSTS_MODEMIF_Pos

#define UART_INTSTS_MODEMIF_Pos (3)

UART_T::INTSTS: MODENIF Position

Definition at line 6752 of file Mini55Series.h.

## ◆ UART_INTSTS_MODEMINT_Msk

#define UART_INTSTS_MODEMINT_Msk (0x1ul << UART_INTSTS_MODEMINT_Pos)

UART_T::INTSTS: MODEMINT Mask

Definition at line 6771 of file Mini55Series.h.

## ◆ UART_INTSTS_MODEMINT_Pos

#define UART_INTSTS_MODEMINT_Pos (11)

UART_T::INTSTS: MODEMINT Position

Definition at line 6770 of file Mini55Series.h.

## ◆ UART_INTSTS_RDAIF_Msk

#define UART_INTSTS_RDAIF_Msk (0x1ul << UART_INTSTS_RDAIF_Pos)

UART_T::INTSTS: RDAIF Mask

Definition at line 6744 of file Mini55Series.h.

## ◆ UART_INTSTS_RDAIF_Pos

#define UART_INTSTS_RDAIF_Pos (0)

UART_T::INTSTS: RDAIF Position

Definition at line 6743 of file Mini55Series.h.

## ◆ UART_INTSTS_RDAINT_Msk

#define UART_INTSTS_RDAINT_Msk (0x1ul << UART_INTSTS_RDAINT_Pos)

UART_T::INTSTS: RDAINT Mask

Definition at line 6762 of file Mini55Series.h.

## ◆ UART_INTSTS_RDAINT_Pos

#define UART_INTSTS_RDAINT_Pos (8)

UART_T::INTSTS: RDAINT Position

Definition at line 6761 of file Mini55Series.h.

## ◆ UART_INTSTS_RLSIF_Msk

#define UART_INTSTS_RLSIF_Msk (0x1ul << UART_INTSTS_RLSIF_Pos)

UART_T::INTSTS: RLSIF Mask

Definition at line 6750 of file Mini55Series.h.

## ◆ UART_INTSTS_RLSIF_Pos

#define UART_INTSTS_RLSIF_Pos (2)

UART_T::INTSTS: RLSIF Position

Definition at line 6749 of file Mini55Series.h.

## ◆ UART_INTSTS_RLSINT_Msk

#define UART_INTSTS_RLSINT_Msk (0x1ul << UART_INTSTS_RLSINT_Pos)

UART_T::INTSTS: RLSINT Mask

Definition at line 6768 of file Mini55Series.h.

## ◆ UART_INTSTS_RLSINT_Pos

#define UART_INTSTS_RLSINT_Pos (10)

UART_T::INTSTS: RLSINT Position

Definition at line 6767 of file Mini55Series.h.

## ◆ UART_INTSTS_RXTOIF_Msk

#define UART_INTSTS_RXTOIF_Msk (0x1ul << UART_INTSTS_RXTOIF_Pos)

UART_T::INTSTS: RXTOIF Mask

Definition at line 6756 of file Mini55Series.h.

## ◆ UART_INTSTS_RXTOIF_Pos

#define UART_INTSTS_RXTOIF_Pos (4)

UART_T::INTSTS: RXTOIF Position

Definition at line 6755 of file Mini55Series.h.

## ◆ UART_INTSTS_RXTOINT_Msk

#define UART_INTSTS_RXTOINT_Msk (0x1ul << UART_INTSTS_RXTOINT_Pos)

UART_T::INTSTS: RXTOINT Mask

Definition at line 6774 of file Mini55Series.h.

## ◆ UART_INTSTS_RXTOINT_Pos

#define UART_INTSTS_RXTOINT_Pos (12)

UART_T::INTSTS: RXTOINT Position

Definition at line 6773 of file Mini55Series.h.

## ◆ UART_INTSTS_THREIF_Msk

#define UART_INTSTS_THREIF_Msk (0x1ul << UART_INTSTS_THREIF_Pos)

UART_T::INTSTS: THREIF Mask

Definition at line 6747 of file Mini55Series.h.

## ◆ UART_INTSTS_THREIF_Pos

#define UART_INTSTS_THREIF_Pos (1)

UART_T::INTSTS: THREIF Position

Definition at line 6746 of file Mini55Series.h.

## ◆ UART_INTSTS_THREINT_Msk

#define UART_INTSTS_THREINT_Msk (0x1ul << UART_INTSTS_THREINT_Pos)

UART_T::INTSTS: THREINT Mask

Definition at line 6765 of file Mini55Series.h.

## ◆ UART_INTSTS_THREINT_Pos

#define UART_INTSTS_THREINT_Pos (9)

UART_T::INTSTS: THREINT Position

Definition at line 6764 of file Mini55Series.h.

## ◆ UART_IRDA_RXINV_Msk

#define UART_IRDA_RXINV_Msk (0x1ul << UART_IRDA_RXINV_Pos)

UART_T::IRDA: RXINV Mask

Definition at line 6804 of file Mini55Series.h.

## ◆ UART_IRDA_RXINV_Pos

#define UART_IRDA_RXINV_Pos (6)

UART_T::IRDA: RXINV Position

Definition at line 6803 of file Mini55Series.h.

## ◆ UART_IRDA_TXEN_Msk

#define UART_IRDA_TXEN_Msk (0x1ul << UART_IRDA_TXEN_Pos)

UART_T::IRDA: TXEN Mask

Definition at line 6798 of file Mini55Series.h.

## ◆ UART_IRDA_TXEN_Pos

#define UART_IRDA_TXEN_Pos (1)

UART_T::IRDA: TXEN Position

Definition at line 6797 of file Mini55Series.h.

## ◆ UART_IRDA_TXINV_Msk

#define UART_IRDA_TXINV_Msk (0x1ul << UART_IRDA_TXINV_Pos)

UART_T::IRDA: TXINV Mask

Definition at line 6801 of file Mini55Series.h.

## ◆ UART_IRDA_TXINV_Pos

#define UART_IRDA_TXINV_Pos (5)

UART_T::IRDA: TXINV Position

Definition at line 6800 of file Mini55Series.h.

## ◆ UART_LINE_BCB_Msk

#define UART_LINE_BCB_Msk (0x1ul << UART_LINE_BCB_Pos)

UART_T::LINE: BCB Mask

Definition at line 6684 of file Mini55Series.h.

## ◆ UART_LINE_BCB_Pos

#define UART_LINE_BCB_Pos (6)

UART_T::LINE: BCB Position

Definition at line 6683 of file Mini55Series.h.

## ◆ UART_LINE_EPE_Msk

#define UART_LINE_EPE_Msk (0x1ul << UART_LINE_EPE_Pos)

UART_T::LINE: EPE Mask

Definition at line 6678 of file Mini55Series.h.

## ◆ UART_LINE_EPE_Pos

#define UART_LINE_EPE_Pos (4)

UART_T::LINE: EPE Position

Definition at line 6677 of file Mini55Series.h.

## ◆ UART_LINE_NSB_Msk

#define UART_LINE_NSB_Msk (0x1ul << UART_LINE_NSB_Pos)

UART_T::LINE: NSB Mask

Definition at line 6672 of file Mini55Series.h.

## ◆ UART_LINE_NSB_Pos

#define UART_LINE_NSB_Pos (2)

UART_T::LINE: NSB Position

Definition at line 6671 of file Mini55Series.h.

## ◆ UART_LINE_PBE_Msk

#define UART_LINE_PBE_Msk (0x1ul << UART_LINE_PBE_Pos)

UART_T::LINE: PBE Mask

Definition at line 6675 of file Mini55Series.h.

## ◆ UART_LINE_PBE_Pos

#define UART_LINE_PBE_Pos (3)

UART_T::LINE: PBE Position

Definition at line 6674 of file Mini55Series.h.

## ◆ UART_LINE_SPE_Msk

#define UART_LINE_SPE_Msk (0x1ul << UART_LINE_SPE_Pos)

UART_T::LINE: SPE Mask

Definition at line 6681 of file Mini55Series.h.

## ◆ UART_LINE_SPE_Pos

#define UART_LINE_SPE_Pos (5)

UART_T::LINE: SPE Position

Definition at line 6680 of file Mini55Series.h.

## ◆ UART_LINE_WLS_Msk

#define UART_LINE_WLS_Msk (0x3ul << UART_LINE_WLS_Pos)

UART_T::LINE: WLS Mask

Definition at line 6669 of file Mini55Series.h.

## ◆ UART_LINE_WLS_Pos

#define UART_LINE_WLS_Pos (0)

UART_T::LINE: WLS Position

Definition at line 6668 of file Mini55Series.h.

## ◆ UART_MODEM_RTS_Msk

#define UART_MODEM_RTS_Msk (0x1ul << UART_MODEM_RTS_Pos)

UART_T::MODEM: RTS Mask

Definition at line 6687 of file Mini55Series.h.

## ◆ UART_MODEM_RTS_Pos

#define UART_MODEM_RTS_Pos (1)

UART_T::MODEM: RTS Position

Definition at line 6686 of file Mini55Series.h.

## ◆ UART_MODEM_RTSACTLV_Msk

#define UART_MODEM_RTSACTLV_Msk (0x1ul << UART_MODEM_RTSACTLV_Pos)

UART_T::MODEM: RTSACTLV Mask

Definition at line 6690 of file Mini55Series.h.

## ◆ UART_MODEM_RTSACTLV_Pos

#define UART_MODEM_RTSACTLV_Pos (9)

UART_T::MODEM: RTSACTLV Position

Definition at line 6689 of file Mini55Series.h.

## ◆ UART_MODEM_RTSSTS_Msk

#define UART_MODEM_RTSSTS_Msk (0x1ul << UART_MODEM_RTSSTS_Pos)

UART_T::MODEM: RTSSTS Mask

Definition at line 6693 of file Mini55Series.h.

## ◆ UART_MODEM_RTSSTS_Pos

#define UART_MODEM_RTSSTS_Pos (13)

UART_T::MODEM: RTSSTS Position

Definition at line 6692 of file Mini55Series.h.

## ◆ UART_MODEMSTS_CTSACTLV_Msk

#define UART_MODEMSTS_CTSACTLV_Msk (0x1ul << UART_MODEMSTS_CTSACTLV_Pos)

UART_T::MODEMSTS: CTSACTLV Mask

Definition at line 6702 of file Mini55Series.h.

## ◆ UART_MODEMSTS_CTSACTLV_Pos

#define UART_MODEMSTS_CTSACTLV_Pos (8)

UART_T::MODEMSTS: CTSACTLV Position

Definition at line 6701 of file Mini55Series.h.

## ◆ UART_MODEMSTS_CTSDETF_Msk

#define UART_MODEMSTS_CTSDETF_Msk (0x1ul << UART_MODEMSTS_CTSDETF_Pos)

UART_T::MODEMSTS: CTSDETF Mask

Definition at line 6696 of file Mini55Series.h.

## ◆ UART_MODEMSTS_CTSDETF_Pos

#define UART_MODEMSTS_CTSDETF_Pos (0)

UART_T::MODEMSTS: CTSDETF Position

Definition at line 6695 of file Mini55Series.h.

## ◆ UART_MODEMSTS_CTSSTS_Msk

#define UART_MODEMSTS_CTSSTS_Msk (0x1ul << UART_MODEMSTS_CTSSTS_Pos)

UART_T::MODEMSTS: CTSSTS Mask

Definition at line 6699 of file Mini55Series.h.

## ◆ UART_MODEMSTS_CTSSTS_Pos

#define UART_MODEMSTS_CTSSTS_Pos (4)

UART_T::MODEMSTS: CTSSTS Position

Definition at line 6698 of file Mini55Series.h.

## ◆ UART_TOUT_DLY_Msk

#define UART_TOUT_DLY_Msk (0xfful << UART_TOUT_DLY_Pos)

UART_T::TOUT: DLY Mask

Definition at line 6783 of file Mini55Series.h.

## ◆ UART_TOUT_DLY_Pos

#define UART_TOUT_DLY_Pos (8)

UART_T::TOUT: DLY Position

Definition at line 6782 of file Mini55Series.h.

## ◆ UART_TOUT_TOIC_Msk

#define UART_TOUT_TOIC_Msk (0xfful << UART_TOUT_TOIC_Pos)

UART_T::TOUT: TOIC Mask

Definition at line 6780 of file Mini55Series.h.

## ◆ UART_TOUT_TOIC_Pos

#define UART_TOUT_TOIC_Pos (0)

UART_T::TOUT: TOIC Position

Definition at line 6779 of file Mini55Series.h.

## ◆ WDT_CTL_ICEDEBUG_Msk

#define WDT_CTL_ICEDEBUG_Msk (0x1ul << WDT_CTL_ICEDEBUG_Pos)

WDT_T::CTL: ICEDEBUG Mask

Definition at line 6933 of file Mini55Series.h.

## ◆ WDT_CTL_ICEDEBUG_Pos

#define WDT_CTL_ICEDEBUG_Pos (31)

WDT_T::CTL: ICEDEBUG Position

Definition at line 6932 of file Mini55Series.h.

## ◆ WDT_CTL_IF_Msk

#define WDT_CTL_IF_Msk (0x1ul << WDT_CTL_IF_Pos)

WDT_T::CTL: IF Mask

Definition at line 6915 of file Mini55Series.h.

## ◆ WDT_CTL_IF_Pos

#define WDT_CTL_IF_Pos (3)

WDT_T::CTL: IF Position

Definition at line 6914 of file Mini55Series.h.

## ◆ WDT_CTL_INTEN_Msk

#define WDT_CTL_INTEN_Msk (0x1ul << WDT_CTL_INTEN_Pos)

WDT_T::CTL: INTEN Mask

Definition at line 6924 of file Mini55Series.h.

## ◆ WDT_CTL_INTEN_Pos

#define WDT_CTL_INTEN_Pos (6)

WDT_T::CTL: INTEN Position

Definition at line 6923 of file Mini55Series.h.

## ◆ WDT_CTL_RSTCNT_Msk

#define WDT_CTL_RSTCNT_Msk (0x1ul << WDT_CTL_RSTCNT_Pos)

WDT_T::CTL: RSTCNT Mask

Definition at line 6906 of file Mini55Series.h.

## ◆ WDT_CTL_RSTCNT_Pos

#define WDT_CTL_RSTCNT_Pos (0)

    @addtogroup WDT_CONST WDT Bit Field Definition
    Constant Definitions for WDT Controller

WDT_T::CTL: RSTCNT Position

Definition at line 6905 of file Mini55Series.h.

## ◆ WDT_CTL_RSTEN_Msk

#define WDT_CTL_RSTEN_Msk (0x1ul << WDT_CTL_RSTEN_Pos)

WDT_T::CTL: RSTEN Mask

Definition at line 6909 of file Mini55Series.h.

## ◆ WDT_CTL_RSTEN_Pos

#define WDT_CTL_RSTEN_Pos (1)

WDT_T::CTL: RSTEN Position

Definition at line 6908 of file Mini55Series.h.

## ◆ WDT_CTL_RSTF_Msk

#define WDT_CTL_RSTF_Msk (0x1ul << WDT_CTL_RSTF_Pos)

WDT_T::CTL: RSTF Mask

Definition at line 6912 of file Mini55Series.h.

## ◆ WDT_CTL_RSTF_Pos

#define WDT_CTL_RSTF_Pos (2)

WDT_T::CTL: RSTF Position

Definition at line 6911 of file Mini55Series.h.

## ◆ WDT_CTL_TOUTSEL_Msk

#define WDT_CTL_TOUTSEL_Msk (0x7ul << WDT_CTL_TOUTSEL_Pos)

WDT_T::CTL: TOUTSEL Mask

Definition at line 6930 of file Mini55Series.h.

## ◆ WDT_CTL_TOUTSEL_Pos

#define WDT_CTL_TOUTSEL_Pos (8)

WDT_T::CTL: TOUTSEL Position

Definition at line 6929 of file Mini55Series.h.

## ◆ WDT_CTL_WDTEN_Msk

#define WDT_CTL_WDTEN_Msk (0x1ul << WDT_CTL_WDTEN_Pos)

WDT_T::CTL: WDTEN Mask

Definition at line 6927 of file Mini55Series.h.

## ◆ WDT_CTL_WDTEN_Pos

#define WDT_CTL_WDTEN_Pos (7)

WDT_T::CTL: WDTEN Position

Definition at line 6926 of file Mini55Series.h.

## ◆ WDT_CTL_WKEN_Msk

#define WDT_CTL_WKEN_Msk (0x1ul << WDT_CTL_WKEN_Pos)

WDT_T::CTL: WKEN Mask

Definition at line 6918 of file Mini55Series.h.

## ◆ WDT_CTL_WKEN_Pos

#define WDT_CTL_WKEN_Pos (4)

WDT_T::CTL: WKEN Position

Definition at line 6917 of file Mini55Series.h.

## ◆ WDT_CTL_WKF_Msk

#define WDT_CTL_WKF_Msk (0x1ul << WDT_CTL_WKF_Pos)

WDT_T::CTL: WKF Mask

Definition at line 6921 of file Mini55Series.h.

## ◆ WDT_CTL_WKF_Pos

#define WDT_CTL_WKF_Pos (5)

WDT_T::CTL: WKF Position

Definition at line 6920 of file Mini55Series.h.