| MINI55_BSP V3.02.004 The Board Support Package for Mini55 Series MCU

Data Fields
PWM_T Struct Reference

`#include <Mini55Series.h>`

## Data Fields
__IO uint32_t | CLKPSC
__IO uint32_t | CLKDIV
__IO uint32_t | CTL
__IO uint32_t | PERIOD [6]
__IO uint32_t | CMPDAT [6]
__IO uint32_t | INTEN
__IO uint32_t | INTSTS
__IO uint32_t | POEN
__IO uint32_t | BRKCTL
__IO uint32_t | DTCTL
__IO uint32_t | ADCTCTL0
__IO uint32_t | ADCTCTL1
__IO uint32_t | ADCTSTS0
__IO uint32_t | ADCTSTS1
__IO uint32_t | PHCHG
__IO uint32_t | PHCHGNXT
__IO uint32_t | PHCHGMSK
__IO uint32_t | IFA

## Detailed Description

    @addtogroup PWM Pulse Width Modulation Controller(PWM)
    Memory Mapped Structure for PWM Controller

Definition at line 2877 of file Mini55Series.h.

The documentation for this struct was generated from the following file:

- Device/Nuvoton/Mini55Series/Include/Mini55Series.h