| MINI55_BSP V3.03.000 The Board Support Package for Mini55 Series MCU

Functions
fmc.c File Reference

MINI55 series FMC driver source file. More...

`#include <stdio.h>`
`#include "Mini55Series.h"`
Include dependency graph for fmc.c:

Go to the source code of this file.

## Functions
void | FMC_Close (void)
| Disable all FMC functions. More...
int32_t | FMC_Erase (uint32_t u32PageAddr)
| Execute ISP command to erase a flash page. The page size is 512 bytes. More...
int32_t | FMC_GetBootSource (void)
| Get the current boot source. More...
void | FMC_Open (void)
| Enable FMC ISP function. More...
uint32_t | FMC_Read (uint32_t u32Addr)
| Execute ISP command to read a word from flash. More...
uint32_t | FMC_ReadCID (void)
| Read company ID. More...
uint32_t | FMC_ReadPID (void)
| Read product ID. More...
uint32_t | FMC_ReadUCID (uint32_t u32Index)
| This function reads one of the four UCID. More...
uint32_t | FMC_ReadUID (uint32_t u32Index)
| This function reads one of the three UID. More...
uint32_t | FMC_ReadDataFlashBaseAddr (void)
| Get the base address of Data Flash if enabled. More...
void | FMC_SetVectorPageAddr (uint32_t u32PageAddr)
| This function will force re-map assigned flash page to CPU address 0x0. More...
uint32_t | FMC_GetVectorPageAddr (void)
| Obtain the current vector page address setting. More...
void | FMC_Write (uint32_t u32Addr, uint32_t u32Data)
| Writes a word data to specified flash address. More...
int32_t | FMC_ReadConfig (uint32_t *u32Config, uint32_t u32Count)
| Execute ISP command to read User Configuration. More...
int32_t | FMC_WriteConfig (uint32_t *u32Config, uint32_t u32Count)
| Execute ISP command to write User Configuration. More...

## Detailed Description

MINI55 series FMC driver source file.

Version
  V1.00

Revision
  7

Date
  15/07/07 5:48p

Note
  SPDX-License-Identifier: Apache-2.0 Copyright (C) 2014 Nuvoton Technology Corp. All rights reserved.

Definition in file fmc.c.